(footprint "Transformer_ED8_4-Lead_10.5x8mm_P5mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Isolated audio transformer, ED8, 4-lead, body 10.5x8mm body, pitch 5mm, height 5mm, https://gitlab.com/kicad/libraries/kicad-footprints/-/merge_requests/3626")
	(tags "permalloy core ")
	(property "Reference" "REF**"
		(at -5 1.5 90)
		(layer "F.SilkS")
	)
	(property "Value" "Transformer_ED8_4-Lead_10.5x8mm_P5mm"
		(at 0 8.8 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -2.5 -6.325 180)
		(size 1.25 2.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at 2.5 -6.325 180)
		(size 1.25 2.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at 2.5 6.325 180)
		(size 1.25 2.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -2.5 6.325 180)
		(size 1.25 2.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Transformer_SMD.3dshapes/Transformer_ED8_4-Lead_10.5x8mm_P5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
