(footprint "Transformer_Ethernet_Bel_S558-5999-T7-F"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Ethernet Transformer, Bel S558-5999-T7-F, https://www.belfuse.com/resources/ICMs/lan-/S558-5999-T7-F.pdf")
	(tags "Ethernet Transformer")
	(property "Reference" "REF**"
		(at 0 -7.3 0)
		(layer "F.SilkS")
	)
	(property "Value" "Transformer_Ethernet_Bel_S558-5999-T7-F"
		(at 0 7.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 -7.3 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -4.51 -4.445)
		(size 1.78 0.62)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -4.51 -3.175)
		(size 1.78 0.62)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -4.51 -1.905)
		(size 1.78 0.62)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -4.51 -0.635)
		(size 1.78 0.62)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -4.51 0.635)
		(size 1.78 0.62)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -4.51 1.905)
		(size 1.78 0.62)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -4.51 3.175)
		(size 1.78 0.62)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -4.51 4.445)
		(size 1.78 0.62)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 4.51 4.445)
		(size 1.78 0.62)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 4.51 3.175)
		(size 1.78 0.62)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 4.51 1.905)
		(size 1.78 0.62)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 4.51 0.635)
		(size 1.78 0.62)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 4.51 -0.635)
		(size 1.78 0.62)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 4.51 -1.905)
		(size 1.78 0.62)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at 4.51 -3.175)
		(size 1.78 0.62)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 4.51 -4.445)
		(size 1.78 0.62)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Transformer_SMD.3dshapes/Transformer_Ethernet_Bel_S558-5999-T7-F.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
