(footprint "Transformer_Wuerth_750315371"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Power Transformer, horizontal core with bobbin, 6 pin, 2.54mm pitch, 11.24mm row spacing, 12.6x8.3x4.1mm")
	(tags "transformer flyback")
	(property "Reference" "REF**"
		(at -5.5 -5.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Transformer_Wuerth_750315371"
		(at 0 5.2 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -5.62 -2.54)
		(size 1.83 1.09)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd roundrect
		(at -5.62 0)
		(size 1.83 1.09)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "3" smd roundrect
		(at -5.62 2.54)
		(size 1.83 1.09)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "4" smd roundrect
		(at 5.62 2.54)
		(size 1.83 1.09)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "5" smd roundrect
		(at 5.62 0)
		(size 1.83 1.09)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "6" smd roundrect
		(at 5.62 -2.54)
		(size 1.83 1.09)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Transformer_SMD.3dshapes/Transformer_Wuerth_750315371.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
