(footprint "Transformer_Breve_TEZ-38x45"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "http://www.breve.pl/pdf/ANG/TEZ_ang.pdf")
	(tags "TEZ PCB Transformer")
	(property "Reference" "REF**"
		(at 12.5 -33 0)
		(layer "F.SilkS")
	)
	(property "Value" "Transformer_Breve_TEZ-38x45"
		(at 12.25 -11 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "3"
		(at 12.5 5 0)
		(layer "F.SilkS")
	)
	(fp_text user "10"
		(at 0 -29.5 0)
		(layer "F.SilkS")
	)
	(fp_text user "5"
		(at 25 5 0)
		(layer "F.SilkS")
	)
	(fp_text user "9"
		(at 5 -29.5 0)
		(layer "F.SilkS")
	)
	(fp_text user "8"
		(at 12.5 -29.5 0)
		(layer "F.SilkS")
	)
	(fp_text user "6"
		(at 25 -29.5 0)
		(layer "F.SilkS")
	)
	(fp_text user "7"
		(at 20 -29.5 0)
		(layer "F.SilkS")
	)
	(fp_text user "1"
		(at 0 5 0)
		(layer "F.SilkS")
	)
	(fp_text user "4"
		(at 20 5 0)
		(layer "F.SilkS")
	)
	(fp_text user "2"
		(at 5 5 0)
		(layer "F.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at 12.5 -12.5 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 2 2)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 5 0)
		(size 2 2)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 20 0)
		(size 2 2)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 25 0)
		(size 2 2)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 25 -25)
		(size 2 2)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 20 -25)
		(size 2 2)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 12.5 -25)
		(size 2 2)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 5 -25)
		(size 2 2)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole circle
		(at 0 -25)
		(size 2 2)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Transformer_THT.3dshapes/Transformer_Breve_TEZ-38x45.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
