(footprint "Transformer_CHK_EI30-2VA_Neutral"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Trafo, Printtrafo, CHK, EI30, 2VA, neutral,")
	(tags "Trafo Printtrafo CHK EI30 2VA neutral ")
	(property "Reference" "REF**"
		(at 10 -27.78 0)
		(layer "F.SilkS")
	)
	(property "Value" "Transformer_CHK_EI30-2VA_Neutral"
		(at 10 -10 90)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "1"
		(at 3.65 0.16 90)
		(layer "F.SilkS")
	)
	(fp_text user "5"
		(at 3.65 -20.16 90)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at 8 -10 90)
		(layer "F.Fab")
	)
	(fp_text user "6"
		(at 16.35 -20.16 90)
		(layer "F.Fab")
	)
	(fp_text user "10"
		(at 16.35 0.16 90)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0 -5)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 0 -10)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 0 -15)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 0 -20)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 20 -20)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 20 -15)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 20 -10)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 20 -5)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole circle
		(at 20 0)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Transformer_THT.3dshapes/Transformer_CHK_EI30-2VA_Neutral.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
