(footprint "Transformer_CHK_EI42-5VA_2xSec"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Trafo, Printtrafo, CHK, EI42, 5VA, 2x Sec,")
	(tags "Trafo Printtrafo CHK EI42 5VA 2x Sec ")
	(property "Reference" "REF**"
		(at 12.5 -34.13 0)
		(layer "F.SilkS")
	)
	(property "Value" "Transformer_CHK_EI42-5VA_2xSec"
		(at 14 -10.5 90)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "Pri"
		(at -3.5 -10 90)
		(layer "F.SilkS")
	)
	(fp_text user "1"
		(at 0 4 0)
		(layer "F.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at 12 -10 90)
		(layer "F.Fab")
	)
	(fp_text user "7"
		(at 20.5 -13 0)
		(layer "F.Fab")
	)
	(fp_text user "6"
		(at 20.5 -21 0)
		(layer "F.Fab")
	)
	(fp_text user "5"
		(at 0 -23 0)
		(layer "F.Fab")
	)
	(fp_text user "Sec-I"
		(at 28.5 -18 90)
		(layer "F.Fab")
	)
	(fp_text user "Sec-II"
		(at 28.5 -2 90)
		(layer "F.Fab")
	)
	(fp_text user "10"
		(at 20.5 2 0)
		(layer "F.Fab")
	)
	(fp_text user "9"
		(at 20.5 -6 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0 -5)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 0 -10)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 0 -15)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 0 -20)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 25 -20)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 25 -15)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 25 -10)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 25 -5)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole circle
		(at 25 0)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Transformer_THT.3dshapes/Transformer_CHK_EI42-5VA_2xSec.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
