(footprint "Transformer_CHK_EI54-16VA_2xSec"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Trafo, Printtrafo, CHK, EI54, 16VA, 2x Sec,http://www.eratransformers.com/product-detail/19")
	(tags "Trafo Printtrafo CHK EI54 16VA 2x Sec ")
	(property "Reference" "REF**"
		(at 14.5 -54.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Transformer_CHK_EI54-16VA_2xSec"
		(at 15 -15 90)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "Pri"
		(at -5 -15 90)
		(layer "F.SilkS")
	)
	(fp_text user "1"
		(at 1 3 0)
		(layer "F.SilkS")
	)
	(fp_text user "9"
		(at 26 -23 0)
		(layer "F.Fab")
	)
	(fp_text user "8"
		(at 26 -31 0)
		(layer "F.Fab")
	)
	(fp_text user "13"
		(at 26 -6 0)
		(layer "F.Fab")
	)
	(fp_text user "Sec-I"
		(at 35 -27 90)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at 13 -15 90)
		(layer "F.Fab")
	)
	(fp_text user "14"
		(at 26 2 0)
		(layer "F.Fab")
	)
	(fp_text user "Sec-II"
		(at 35 -1 90)
		(layer "F.Fab")
	)
	(fp_text user "7"
		(at 1 -33 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -3.5 -47.5)
		(size 4.5 4.5)
		(drill 4.5)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -3.5 17.5)
		(size 4.5 4.5)
		(drill 4.5)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 33.5 -47.5)
		(size 4.5 4.5)
		(drill 4.5)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 33.5 17.5)
		(size 4.5 4.5)
		(drill 4.5)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 3 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0 -5)
		(size 3 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 0 -10)
		(size 3 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 0 -15)
		(size 3 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 0 -20)
		(size 3 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 0 -25)
		(size 3 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 0 -30)
		(size 3 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 30 -30)
		(size 3 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 30 -25)
		(size 3 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole circle
		(at 30 -20)
		(size 3 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 30 -15)
		(size 3 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole circle
		(at 30 -10)
		(size 3 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at 30 -5)
		(size 3 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole circle
		(at 30 0)
		(size 3 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Transformer_THT.3dshapes/Transformer_CHK_EI54-16VA_2xSec.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
