(footprint "Transformer_CHK_UI30-4VA_Flat"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Trafo, Flattrafo, CHK, UI30, 4VA,")
	(tags "Trafo Flattrafo CHK UI30 4VA ")
	(property "Reference" "REF**"
		(at 17.5 -41 0)
		(layer "F.SilkS")
	)
	(property "Value" "Transformer_CHK_UI30-4VA_Flat"
		(at 17.5 -17.5 90)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "1"
		(at 3 2 0)
		(layer "F.SilkS")
	)
	(fp_text user "Sec"
		(at 27.5 -17.5 0)
		(layer "F.SilkS")
	)
	(fp_text user "Pri"
		(at 5.5 -17.5 0)
		(layer "F.SilkS")
	)
	(fp_text user "3"
		(at 3 -12 0)
		(layer "F.Fab")
	)
	(fp_text user "16"
		(at 32 1.5 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at 15.5 -17.5 90)
		(layer "F.Fab")
	)
	(fp_text user "9"
		(at 32 -36.5 0)
		(layer "F.Fab")
	)
	(fp_text user "15"
		(at 31 -6.5 0)
		(layer "F.Fab")
	)
	(fp_text user "6"
		(at 2.5 -23.5 0)
		(layer "F.Fab")
	)
	(fp_text user "8"
		(at 2.5 -36.5 0)
		(layer "F.Fab")
	)
	(fp_text user "10"
		(at 32 -28.5 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -6.25 -36.25)
		(size 3 3)
		(drill 3)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -6.25 1.25)
		(size 3 3)
		(drill 3)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 41.25 -36.25)
		(size 3 3)
		(drill 3)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 41.25 1.25)
		(size 3 3)
		(drill 3)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 3 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0 -5)
		(size 3 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 0 -10)
		(size 3 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 0 -15)
		(size 3 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 0 -20)
		(size 3 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 0 -25)
		(size 3 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 0 -30)
		(size 3 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 0 -35)
		(size 3 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 35 -35)
		(size 3 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole circle
		(at 35 -30)
		(size 3 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 35 -25)
		(size 3 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole circle
		(at 35 -20)
		(size 3 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at 35 -15)
		(size 3 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole circle
		(at 35 -10)
		(size 3 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "15" thru_hole circle
		(at 35 -5)
		(size 3 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "16" thru_hole circle
		(at 35 0)
		(size 3 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Transformer_THT.3dshapes/Transformer_CHK_UI30-4VA_Flat.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
