(footprint "Transformer_CHK_UI39-10VA_Flat"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Trafo, Flattrafo, CHK, UI39, 10VA,")
	(tags "Trafo Flattrafo CHK UI39 10VA ")
	(property "Reference" "REF**"
		(at 22.5 -53 0)
		(layer "F.SilkS")
	)
	(property "Value" "Transformer_CHK_UI39-10VA_Flat"
		(at 22.5 -23 90)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "1"
		(at 3.5 2 0)
		(layer "F.SilkS")
	)
	(fp_text user "Sec"
		(at 34.5 -23 0)
		(layer "F.SilkS")
	)
	(fp_text user "Pri"
		(at 7.5 -23 0)
		(layer "F.SilkS")
	)
	(fp_text user "4"
		(at 3.5 -17 0)
		(layer "F.Fab")
	)
	(fp_text user "13"
		(at 41.5 -34 0)
		(layer "F.Fab")
	)
	(fp_text user "18"
		(at 41.5 -12 0)
		(layer "F.Fab")
	)
	(fp_text user "10"
		(at 3.5 -48 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at 20.5 -23 90)
		(layer "F.Fab")
	)
	(fp_text user "11"
		(at 41.5 -48 0)
		(layer "F.Fab")
	)
	(fp_text user "20"
		(at 41.5 2 0)
		(layer "F.Fab")
	)
	(fp_text user "7"
		(at 3.5 -29 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -8.75 -48)
		(size 3 3)
		(drill 3)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -8.75 2)
		(size 3 3)
		(drill 3)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 53.75 -48)
		(size 3 3)
		(drill 3)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 53.75 2)
		(size 3 3)
		(drill 3)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 2.5 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0 -5)
		(size 2.5 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 0 -10)
		(size 2.5 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 0 -15)
		(size 2.5 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 0 -20.33)
		(size 2.5 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 0 -25.66)
		(size 2.5 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 0 -30.99)
		(size 2.5 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 0 -36)
		(size 2.5 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 0 -41)
		(size 2.5 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole circle
		(at 0 -46)
		(size 2.5 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 45 -46)
		(size 2.5 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole circle
		(at 45 -41)
		(size 2.5 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at 45 -36)
		(size 2.5 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole circle
		(at 45 -31)
		(size 2.5 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "15" thru_hole circle
		(at 45 -25.66)
		(size 2.5 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "16" thru_hole circle
		(at 45 -20.33)
		(size 2.5 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "17" thru_hole circle
		(at 45 -15)
		(size 2.5 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "18" thru_hole circle
		(at 45 -10)
		(size 2.5 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "19" thru_hole circle
		(at 45 -5)
		(size 2.5 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "20" thru_hole circle
		(at 45 0)
		(size 2.5 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Transformer_THT.3dshapes/Transformer_CHK_UI39-10VA_Flat.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
