(footprint "Transformer_EPCOS_B66359A1013T_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Transformer, Transformator, ETD29, 13 Pin, Horizontal, EPCOS-B66359A1013T,")
	(tags "Transformer Transformator ETD29 13 Pin Horizontal EPCOS-B66359A1013T ")
	(property "Reference" "REF**"
		(at 15.24 -33.02 0)
		(layer "F.SilkS")
	)
	(property "Value" "Transformer_EPCOS_B66359A1013T_Horizontal"
		(at 15.24 7.62 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "1"
		(at 0 3.81 0)
		(layer "F.SilkS")
	)
	(fp_text user "8"
		(at 30.48 -29.21 0)
		(layer "F.Fab")
	)
	(fp_text user "7"
		(at 30.48 3.81 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at 15.245 -12.7 0)
		(layer "F.Fab")
	)
	(fp_text user "14"
		(at 0 -29.21 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 2.5 2.5)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 5.08 0)
		(size 2.5 2.5)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 10.16 0)
		(size 2.5 2.5)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 20.32 0)
		(size 2.5 2.5)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 25.4 0)
		(size 2.5 2.5)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 30.48 0)
		(size 2.5 2.5)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 30.48 -25.4)
		(size 2.5 2.5)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 25.4 -25.4)
		(size 2.5 2.5)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole circle
		(at 20.32 -25.4)
		(size 2.5 2.5)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 15.24 -25.4)
		(size 2.5 2.5)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole circle
		(at 10.16 -25.4)
		(size 2.5 2.5)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at 5.08 -25.4)
		(size 2.5 2.5)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole circle
		(at 0 -25.4)
		(size 2.5 2.5)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Transformer_THT.3dshapes/Transformer_EPCOS_B66359A1013T_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
