(footprint "Transformer_Microphone_Lundahl_LL1587"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "AUDIO TRAFO LUNDAHL, https://www.lundahltransformers.com/wp-content/uploads/datasheets/1587.pdf")
	(tags "AUDIO TRAFO LUNDAHL")
	(property "Reference" "REF**"
		(at 10.35 -15.55 0)
		(layer "F.SilkS")
	)
	(property "Value" "Transformer_Microphone_Lundahl_LL1587"
		(at 10.16 -1.9 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 10.16 -5.715 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 2.29 2.29)
		(drill 1.52)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0 -3.81)
		(size 2.29 2.29)
		(drill 1.52)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 0 -7.62)
		(size 2.29 2.29)
		(drill 1.52)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 0 -11.43)
		(size 2.29 2.29)
		(drill 1.52)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 20.32 0)
		(size 2.29 2.29)
		(drill 1.52)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 20.32 -3.81)
		(size 2.29 2.29)
		(drill 1.52)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 20.32 -11.43)
		(size 2.29 2.29)
		(drill 1.52)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Transformer_THT.3dshapes/Transformer_Microphone_Lundahl_LL1587.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
