(footprint "GaN_Systems_GaNPX-3_5x6.6mm_Drain2.93x0.6mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "GaN Systems GaNPX GS66502B Package, https://gansystems.com/wp-content/uploads/2020/04/GS66502B-DS-Rev-200402.pdf")
	(tags "ganpx gs66502b")
	(property "Reference" "REF**"
		(at 0 -4.21 0)
		(layer "F.SilkS")
	)
	(property "Value" "GaN_Systems_GaNPX-3_5x6.6mm_Drain2.93x0.6mm"
		(at 0 6.6 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.34 0.9525)
		(size 1.58 1.235)
		(layers "F.Paste")
		(roundrect_rratio 0.2024291498)
	)
	(pad "" smd roundrect
		(at -0.34 2.3875)
		(size 1.58 1.235)
		(layers "F.Paste")
		(roundrect_rratio 0.2024291498)
	)
	(pad "" smd roundrect
		(at 1.44 0.9525)
		(size 1.58 1.235)
		(layers "F.Paste")
		(roundrect_rratio 0.2024291498)
	)
	(pad "" smd roundrect
		(at 1.44 2.3875)
		(size 1.58 1.235)
		(layers "F.Paste")
		(roundrect_rratio 0.2024291498)
	)
	(pad "1" smd roundrect
		(at 0.41 -2.91)
		(size 2.93 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -2.13 1.81)
		(size 0.6 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at 0.55 1.67)
		(size 3.76 3.07)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.08143322476)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Transistor_Power.3dshapes/GaN_Systems_GaNPX-3_5x6.6mm_Drain2.93x0.6mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
