(footprint "GaN_Systems_GaNPX-4_7x8.4mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "GaN Systems GaNPX GS66508B Package, https://gansystems.com/wp-content/uploads/2020/04/GS66508B-DS-Rev-200402.pdf")
	(tags "ganpx gs66508b")
	(property "Reference" "REF**"
		(at 0 -5.2 0)
		(layer "F.SilkS")
	)
	(property "Value" "GaN_Systems_GaNPX-4_7x8.4mm"
		(at 0 5.5 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -2.575 0.3875)
		(size 1.3 1.225)
		(layers "F.Paste")
		(roundrect_rratio 0.2)
		(chamfer_ratio 0.2)
		(chamfer)
	)
	(pad "" smd roundrect
		(at -2.575 1.8125)
		(size 1.3 1.225)
		(layers "F.Paste")
		(roundrect_rratio 0.2)
		(chamfer_ratio 0.2)
		(chamfer)
	)
	(pad "" smd roundrect
		(at -1.075 0.3875)
		(size 1.3 1.225)
		(layers "F.Paste")
		(roundrect_rratio 0.2)
		(chamfer_ratio 0.2)
		(chamfer)
	)
	(pad "" smd roundrect
		(at -1.075 1.8125)
		(size 1.3 1.225)
		(layers "F.Paste")
		(roundrect_rratio 0.2)
		(chamfer_ratio 0.2)
		(chamfer)
	)
	(pad "" smd roundrect
		(at 0.5875 0.3875)
		(size 1.625 1.225)
		(layers "F.Paste")
		(roundrect_rratio 0.2)
		(chamfer_ratio 0.2)
		(chamfer)
	)
	(pad "" smd roundrect
		(at 0.5875 1.8125)
		(size 1.625 1.225)
		(layers "F.Paste")
		(roundrect_rratio 0.2)
		(chamfer_ratio 0.2)
		(chamfer)
	)
	(pad "" smd roundrect
		(at 0.5875 3.275)
		(size 1.625 1.3)
		(layers "F.Paste")
		(roundrect_rratio 0.2)
		(chamfer_ratio 0.2)
		(chamfer)
	)
	(pad "" smd roundrect
		(at 2.4125 0.3875)
		(size 1.625 1.225)
		(layers "F.Paste")
		(roundrect_rratio 0.2)
		(chamfer_ratio 0.2)
		(chamfer)
	)
	(pad "" smd roundrect
		(at 2.4125 1.8125)
		(size 1.625 1.225)
		(layers "F.Paste")
		(roundrect_rratio 0.2)
		(chamfer_ratio 0.2)
		(chamfer)
	)
	(pad "" smd roundrect
		(at 2.4125 3.275)
		(size 1.625 1.3)
		(layers "F.Paste")
		(roundrect_rratio 0.2)
		(chamfer_ratio 0.2)
		(chamfer)
	)
	(pad "1" smd roundrect
		(at 0 -3.63)
		(size 6 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd custom
		(at 0 1.1)
		(size 3.05 3.05)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(arc
						(start -3.425 1.275)
						(mid -3.351777 1.451777)
						(end -3.175 1.525)
					)
					(xy 3.425 1.525)
					(arc
						(start 3.425 -1.275)
						(mid 3.351777 -1.451777)
						(end 3.175 -1.525)
					)
					(arc
						(start -3.175 -1.525)
						(mid -3.351777 -1.451777)
						(end -3.425 -1.275)
					)
				)
				(width 0.0001)
				(fill yes)
			)
		)
	)
	(pad "2" smd custom
		(at 1.5 3.38)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(arc
						(start 1.675 0.745)
						(mid 1.851777 0.671777)
						(end 1.925 0.495)
					)
					(xy 1.925 -1.93) (xy -2.175 -1.93)
					(arc
						(start -2.175 -0.755)
						(mid -1.998223 -0.681777)
						(end -1.925 -0.505)
					)
					(arc
						(start -1.925 0.495)
						(mid -1.851777 0.671777)
						(end -1.675 0.745)
					)
				)
				(width 0.0001)
				(fill yes)
			)
		)
	)
	(pad "3" smd roundrect
		(at -2.93 3.63)
		(size 1 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -1.43 3.63)
		(size 1 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Transistor_Power.3dshapes/GaN_Systems_GaNPX-4_7x8.4mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
