(footprint "Infineon_AG-ECONO2"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "28-lead TH, EconoPACK 2, same as Littelfuse_Package_H_XN2MM, https://www.infineon.com/dgdl/Infineon-FS75R07N2E4-DS-v02_00-en_de.pdf?fileId=db3a30432f5008fe012f52f916333979")
	(tags "igbt diode module")
	(property "Reference" "REF**"
		(at -20.8 -3.9 0)
		(layer "F.SilkS")
	)
	(property "Value" "Infineon_AG-ECONO2"
		(at 28.48 20.95 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 30.1 19.3 180)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -16.02 4.95)
		(size 2.6 2.6)
		(drill 2.6)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -16.02 36.95)
		(size 2.6 2.6)
		(drill 2.6)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 76.98 4.95)
		(size 2.6 2.6)
		(drill 2.6)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 76.98 36.95)
		(size 2.6 2.6)
		(drill 2.6)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 3.81 0)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 11.43 0)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 15.24 0)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 22.86 0)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 26.67 0)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 34.29 0)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 38.1 0)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 45.72 0)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole circle
		(at 49.53 0)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 57.15 0)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole circle
		(at 60.96 0)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at 70.08 9.52)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole circle
		(at 70.08 13.33)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "15" thru_hole circle
		(at 70.08 28.57)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "16" thru_hole circle
		(at 70.08 32.38)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "17" thru_hole circle
		(at 60.96 41.9)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "18" thru_hole circle
		(at 57.15 41.9)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "19" thru_hole circle
		(at 45.72 41.9)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "20" thru_hole circle
		(at 41.91 41.9)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 26.67 41.9)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "22" thru_hole circle
		(at 22.86 41.9)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "23" thru_hole circle
		(at 7.62 41.9)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "24" thru_hole circle
		(at 3.81 41.9)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "25" thru_hole circle
		(at -9.12 32.38)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "26" thru_hole circle
		(at -9.12 28.57)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "27" thru_hole circle
		(at -9.12 13.33)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "28" thru_hole circle
		(at -9.12 9.52)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
			"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
			"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
			"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
			"In29.Cu" "In30.Cu"
		)
		(name "MH")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -10.51413 20.95) (xy -10.53344 20.489281) (xy -10.591234 20.031793) (xy -10.687107 19.580746)
				(xy -10.820386 19.139303) (xy -10.990137 18.710561) (xy -11.195169 18.297527) (xy -11.434044 17.903098)
				(xy -11.705086 17.530041) (xy -12.006394 17.180973) (xy -12.335854 16.858341) (xy -12.691156 16.56441)
				(xy -13.069807 16.30124) (xy -13.469152 16.070678) (xy -13.88639 15.874341) (xy -14.318593 15.713606)
				(xy -14.76273 15.589601) (xy -15.215686 15.503195) (xy -15.674284 15.454995) (xy -16.135306 15.445338)
				(xy -16.59552 15.474292) (xy -17.051697 15.541654) (xy -17.500638 15.646952) (xy -17.939192 15.789447)
				(xy -18.364285 15.96814) (xy -18.772935 16.181777) (xy -19.162275 16.428859) (xy -19.529574 16.707654)
				(xy -19.872255 17.016206) (xy -20.187916 17.352351) (xy -20.474342 17.713731) (xy -20.729524 18.097811)
				(xy -20.951673 18.501897) (xy -21.139228 18.923154) (xy -21.290877 19.358629) (xy -21.405554 19.805265)
				(xy -21.482455 20.259932) (xy -21.52104 20.719438) (xy -21.52104 21.180562) (xy -21.482455 21.640068)
				(xy -21.405554 22.094735) (xy -21.290877 22.541371) (xy -21.139228 22.976846) (xy -20.951673 23.398103)
				(xy -20.729524 23.802189) (xy -20.474342 24.186269) (xy -20.187916 24.547649) (xy -19.872255 24.883794)
				(xy -19.529574 25.192346) (xy -19.162275 25.471141) (xy -18.772935 25.718223) (xy -18.364285 25.93186)
				(xy -17.939192 26.110553) (xy -17.500638 26.253048) (xy -17.051697 26.358346) (xy -16.59552 26.425708)
				(xy -16.135306 26.454662) (xy -15.674284 26.445005) (xy -15.215686 26.396805) (xy -14.76273 26.310399)
				(xy -14.318593 26.186394) (xy -13.88639 26.025659) (xy -13.469152 25.829322) (xy -13.069807 25.59876)
				(xy -12.691156 25.33559) (xy -12.335854 25.041659) (xy -12.006394 24.719027) (xy -11.705086 24.369959)
				(xy -11.434044 23.996902) (xy -11.195169 23.602473) (xy -10.990137 23.189439) (xy -10.820386 22.760697)
				(xy -10.687107 22.319254) (xy -10.591234 21.868207) (xy -10.53344 21.410719)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
			"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
			"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
			"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
			"In29.Cu" "In30.Cu"
		)
		(name "MH")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 82.48587 20.95) (xy 82.46656 20.489281) (xy 82.408766 20.031793) (xy 82.312893 19.580746) (xy 82.179614 19.139303)
				(xy 82.009863 18.710561) (xy 81.804831 18.297527) (xy 81.565956 17.903098) (xy 81.294914 17.530041)
				(xy 80.993606 17.180973) (xy 80.664146 16.858341) (xy 80.308844 16.56441) (xy 79.930193 16.30124)
				(xy 79.530848 16.070678) (xy 79.11361 15.874341) (xy 78.681407 15.713606) (xy 78.23727 15.589601)
				(xy 77.784314 15.503195) (xy 77.325716 15.454995) (xy 76.864694 15.445338) (xy 76.40448 15.474292)
				(xy 75.948303 15.541654) (xy 75.499362 15.646952) (xy 75.060808 15.789447) (xy 74.635715 15.96814)
				(xy 74.227065 16.181777) (xy 73.837725 16.428859) (xy 73.470426 16.707654) (xy 73.127745 17.016206)
				(xy 72.812084 17.352351) (xy 72.525658 17.713731) (xy 72.270476 18.097811) (xy 72.048327 18.501897)
				(xy 71.860772 18.923154) (xy 71.709123 19.358629) (xy 71.594446 19.805265) (xy 71.517545 20.259932)
				(xy 71.47896 20.719438) (xy 71.47896 21.180562) (xy 71.517545 21.640068) (xy 71.594446 22.094735)
				(xy 71.709123 22.541371) (xy 71.860772 22.976846) (xy 72.048327 23.398103) (xy 72.270476 23.802189)
				(xy 72.525658 24.186269) (xy 72.812084 24.547649) (xy 73.127745 24.883794) (xy 73.470426 25.192346)
				(xy 73.837725 25.471141) (xy 74.227065 25.718223) (xy 74.635715 25.93186) (xy 75.060808 26.110553)
				(xy 75.499362 26.253048) (xy 75.948303 26.358346) (xy 76.40448 26.425708) (xy 76.864694 26.454662)
				(xy 77.325716 26.445005) (xy 77.784314 26.396805) (xy 78.23727 26.310399) (xy 78.681407 26.186394)
				(xy 79.11361 26.025659) (xy 79.530848 25.829322) (xy 79.930193 25.59876) (xy 80.308844 25.33559)
				(xy 80.664146 25.041659) (xy 80.993606 24.719027) (xy 81.294914 24.369959) (xy 81.565956 23.996902)
				(xy 81.804831 23.602473) (xy 82.009863 23.189439) (xy 82.179614 22.760697) (xy 82.312893 22.319254)
				(xy 82.408766 21.868207) (xy 82.46656 21.410719)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Transistor_Power_Module.3dshapes/Infineon_AG-ECONO2.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
