(footprint "Infineon_AG-ECONO3B"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "41-lead TH, EconoPACK 3B, https://www.infineon.com/dgdl/Infineon-FS300R12N3E7-DataSheet-v01_00-EN.pdf?fileId=8ac78c8c8900bb57018901d6e6f6124b")
	(tags "igbt diode module")
	(property "Reference" "REF**"
		(at -20.8 -3.9 0)
		(layer "F.SilkS")
	)
	(property "Value" "Infineon_AG-ECONO3B"
		(at 36.362 33.655 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 36.362 29.595 180)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -14.995 4.21)
		(size 5.8 5.8)
		(drill 5.8)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -14.995 54.21)
		(size 5.8 5.8)
		(drill 5.8)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -7.245 0.46)
		(size 2.5 2.5)
		(drill 2.5)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -7.245 57.96)
		(size 2.5 2.5)
		(drill 2.5)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 87.255 0.46)
		(size 2.5 2.5)
		(drill 2.5)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 87.255 57.96)
		(size 2.5 2.5)
		(drill 2.5)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 95.005 4.21)
		(size 5.8 5.8)
		(drill 5.8)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 95.005 54.21)
		(size 5.8 5.8)
		(drill 5.8)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 2.46 2.46)
		(drill 1.64)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 45)
	)
	(pad "2" thru_hole circle
		(at 3.81 0)
		(size 2.46 2.46)
		(drill 1.64)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 15.23951 0)
		(size 2.46 2.46)
		(drill 1.64)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 19.04951 0)
		(size 2.46 2.46)
		(drill 1.64)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 30.47951 0)
		(size 2.46 2.46)
		(drill 1.64)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 34.28951 0)
		(size 2.46 2.46)
		(drill 1.64)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 45.71951 0)
		(size 2.46 2.46)
		(drill 1.64)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 49.52951 0)
		(size 2.46 2.46)
		(drill 1.64)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 60.95951 0)
		(size 2.46 2.46)
		(drill 1.64)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole circle
		(at 64.76951 0)
		(size 2.46 2.46)
		(drill 1.64)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 76.19951 0)
		(size 2.46 2.46)
		(drill 1.64)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole circle
		(at 80.00951 0)
		(size 2.46 2.46)
		(drill 1.64)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at 99.06 15.875)
		(size 2.46 2.46)
		(drill 1.64)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole circle
		(at 99.06 19.685)
		(size 2.46 2.46)
		(drill 1.64)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "15" thru_hole circle
		(at 99.06 23.495)
		(size 2.46 2.46)
		(drill 1.64)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "16" thru_hole circle
		(at 99.06 34.925)
		(size 2.46 2.46)
		(drill 1.64)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "17" thru_hole circle
		(at 99.06 38.735)
		(size 2.46 2.46)
		(drill 1.64)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "18" thru_hole circle
		(at 99.06 42.545)
		(size 2.46 2.46)
		(drill 1.64)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "19" thru_hole circle
		(at 81.91451 58.42)
		(size 2.46 2.46)
		(drill 1.64)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "20" thru_hole circle
		(at 78.10451 58.42)
		(size 2.46 2.46)
		(drill 1.64)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 66.675 58.42)
		(size 2.46 2.46)
		(drill 1.64)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "22" thru_hole circle
		(at 62.86451 58.42)
		(size 2.46 2.46)
		(drill 1.64)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "23" thru_hole circle
		(at 59.05451 58.42)
		(size 2.46 2.46)
		(drill 1.64)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "24" thru_hole circle
		(at 55.24451 58.42)
		(size 2.46 2.46)
		(drill 1.64)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "25" thru_hole circle
		(at 51.435 58.42)
		(size 2.46 2.46)
		(drill 1.64)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "26" thru_hole circle
		(at 40.00451 58.42)
		(size 2.46 2.46)
		(drill 1.64)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "27" thru_hole circle
		(at 36.19451 58.42)
		(size 2.46 2.46)
		(drill 1.64)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "28" thru_hole circle
		(at 32.38451 58.42)
		(size 2.46 2.46)
		(drill 1.64)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "29" thru_hole circle
		(at 28.57451 58.42)
		(size 2.46 2.46)
		(drill 1.64)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "30" thru_hole circle
		(at 24.76451 58.42)
		(size 2.46 2.46)
		(drill 1.64)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "31" thru_hole circle
		(at 13.33451 58.42)
		(size 2.46 2.46)
		(drill 1.64)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "32" thru_hole circle
		(at 9.52451 58.42)
		(size 2.46 2.46)
		(drill 1.64)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at 5.71451 58.42)
		(size 2.46 2.46)
		(drill 1.64)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "34" thru_hole circle
		(at 1.90451 58.42)
		(size 2.46 2.46)
		(drill 1.64)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "35" thru_hole circle
		(at -1.90549 58.42)
		(size 2.46 2.46)
		(drill 1.64)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "36" thru_hole circle
		(at -19.05 42.545)
		(size 2.46 2.46)
		(drill 1.64)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "37" thru_hole circle
		(at -19.05 38.735)
		(size 2.46 2.46)
		(drill 1.64)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "38" thru_hole circle
		(at -19.05 34.925)
		(size 2.46 2.46)
		(drill 1.64)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "39" thru_hole circle
		(at -19.05 23.495)
		(size 2.46 2.46)
		(drill 1.64)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "40" thru_hole circle
		(at -19.05 19.685)
		(size 2.46 2.46)
		(drill 1.64)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at -19.05 15.875)
		(size 2.46 2.46)
		(drill 1.64)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
			"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
			"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
			"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
			"In29.Cu" "In30.Cu"
		)
		(name "MH")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -9.50084 4.202) (xy -9.520147 3.741357) (xy -9.577931 3.283945) (xy -9.673788 2.832972) (xy -9.807046 2.391602)
				(xy -9.976769 1.962931) (xy -10.181767 1.549965) (xy -10.420602 1.155602) (xy -10.691599 0.782606)
				(xy -10.992857 0.433596) (xy -11.322263 0.111017) (xy -11.677506 -0.182865) (xy -12.056095 -0.445991)
				(xy -12.455374 -0.676515) (xy -12.872542 -0.87282) (xy -13.304674 -1.033528) (xy -13.748738 -1.157513)
				(xy -14.201619 -1.243905) (xy -14.660141 -1.292097) (xy -15.121087 -1.301753) (xy -15.581225 -1.272803)
				(xy -16.037327 -1.205452) (xy -16.486193 -1.100171) (xy -16.924675 -0.9577) (xy -17.349698 -0.779037)
				(xy -17.75828 -0.565435) (xy -18.147555 -0.318394) (xy -18.514794 -0.039645) (xy -18.857419 0.268856)
				(xy -19.173028 0.604946) (xy -19.459406 0.966266) (xy -19.714546 1.350282) (xy -19.936657 1.754301)
				(xy -20.124182 2.175489) (xy -20.275806 2.610892) (xy -20.390463 3.057454) (xy -20.467352 3.512046)
				(xy -20.505931 3.971476) (xy -20.505931 4.432524) (xy -20.467352 4.891954) (xy -20.390463 5.346546)
				(xy -20.275806 5.793108) (xy -20.124182 6.228511) (xy -19.936657 6.649699) (xy -19.714546 7.053718)
				(xy -19.459406 7.437734) (xy -19.173028 7.799054) (xy -18.857419 8.135144) (xy -18.514794 8.443645)
				(xy -18.147555 8.722394) (xy -17.75828 8.969435) (xy -17.349698 9.183037) (xy -16.924675 9.3617)
				(xy -16.486193 9.504171) (xy -16.037327 9.609452) (xy -15.581225 9.676803) (xy -15.121087 9.705753)
				(xy -14.660141 9.696097) (xy -14.201619 9.647905) (xy -13.748738 9.561513) (xy -13.304674 9.437528)
				(xy -12.872542 9.27682) (xy -12.455374 9.080515) (xy -12.056095 8.849991) (xy -11.677506 8.586865)
				(xy -11.322263 8.292983) (xy -10.992857 7.970404) (xy -10.691599 7.621394) (xy -10.420602 7.248398)
				(xy -10.181767 6.854035) (xy -9.976769 6.441069) (xy -9.807046 6.012398) (xy -9.673788 5.571028)
				(xy -9.577931 5.120055) (xy -9.520147 4.662643)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
			"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
			"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
			"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
			"In29.Cu" "In30.Cu"
		)
		(name "MH")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -9.50084 54.202) (xy -9.520147 53.741357) (xy -9.577931 53.283945) (xy -9.673788 52.832972)
				(xy -9.807046 52.391602) (xy -9.976769 51.962931) (xy -10.181767 51.549965) (xy -10.420602 51.155602)
				(xy -10.691599 50.782606) (xy -10.992857 50.433596) (xy -11.322263 50.111017) (xy -11.677506 49.817135)
				(xy -12.056095 49.554009) (xy -12.455374 49.323485) (xy -12.872542 49.12718) (xy -13.304674 48.966472)
				(xy -13.748738 48.842487) (xy -14.201619 48.756095) (xy -14.660141 48.707903) (xy -15.121087 48.698247)
				(xy -15.581225 48.727197) (xy -16.037327 48.794548) (xy -16.486193 48.899829) (xy -16.924675 49.0423)
				(xy -17.349698 49.220963) (xy -17.75828 49.434565) (xy -18.147555 49.681606) (xy -18.514794 49.960355)
				(xy -18.857419 50.268856) (xy -19.173028 50.604946) (xy -19.459406 50.966266) (xy -19.714546 51.350282)
				(xy -19.936657 51.754301) (xy -20.124182 52.175489) (xy -20.275806 52.610892) (xy -20.390463 53.057454)
				(xy -20.467352 53.512046) (xy -20.505931 53.971476) (xy -20.505931 54.432524) (xy -20.467352 54.891954)
				(xy -20.390463 55.346546) (xy -20.275806 55.793108) (xy -20.124182 56.228511) (xy -19.936657 56.649699)
				(xy -19.714546 57.053718) (xy -19.459406 57.437734) (xy -19.173028 57.799054) (xy -18.857419 58.135144)
				(xy -18.514794 58.443645) (xy -18.147555 58.722394) (xy -17.75828 58.969435) (xy -17.349698 59.183037)
				(xy -16.924675 59.3617) (xy -16.486193 59.504171) (xy -16.037327 59.609452) (xy -15.581225 59.676803)
				(xy -15.121087 59.705753) (xy -14.660141 59.696097) (xy -14.201619 59.647905) (xy -13.748738 59.561513)
				(xy -13.304674 59.437528) (xy -12.872542 59.27682) (xy -12.455374 59.080515) (xy -12.056095 58.849991)
				(xy -11.677506 58.586865) (xy -11.322263 58.292983) (xy -10.992857 57.970404) (xy -10.691599 57.621394)
				(xy -10.420602 57.248398) (xy -10.181767 56.854035) (xy -9.976769 56.441069) (xy -9.807046 56.012398)
				(xy -9.673788 55.571028) (xy -9.577931 55.120055) (xy -9.520147 54.662643)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
			"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
			"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
			"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
			"In29.Cu" "In30.Cu"
		)
		(name "MH")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 100.49916 4.202) (xy 100.479853 3.741357) (xy 100.422069 3.283945) (xy 100.326212 2.832972)
				(xy 100.192954 2.391602) (xy 100.023231 1.962931) (xy 99.818233 1.549965) (xy 99.579398 1.155602)
				(xy 99.308401 0.782606) (xy 99.007143 0.433596) (xy 98.677737 0.111017) (xy 98.322494 -0.182865)
				(xy 97.943905 -0.445991) (xy 97.544626 -0.676515) (xy 97.127458 -0.87282) (xy 96.695326 -1.033528)
				(xy 96.251262 -1.157513) (xy 95.798381 -1.243905) (xy 95.339859 -1.292097) (xy 94.878913 -1.301753)
				(xy 94.418775 -1.272803) (xy 93.962673 -1.205452) (xy 93.513807 -1.100171) (xy 93.075325 -0.9577)
				(xy 92.650302 -0.779037) (xy 92.24172 -0.565435) (xy 91.852445 -0.318394) (xy 91.485206 -0.039645)
				(xy 91.142581 0.268856) (xy 90.826972 0.604946) (xy 90.540594 0.966266) (xy 90.285454 1.350282)
				(xy 90.063343 1.754301) (xy 89.875818 2.175489) (xy 89.724194 2.610892) (xy 89.609537 3.057454)
				(xy 89.532648 3.512046) (xy 89.494069 3.971476) (xy 89.494069 4.432524) (xy 89.532648 4.891954)
				(xy 89.609537 5.346546) (xy 89.724194 5.793108) (xy 89.875818 6.228511) (xy 90.063343 6.649699)
				(xy 90.285454 7.053718) (xy 90.540594 7.437734) (xy 90.826972 7.799054) (xy 91.142581 8.135144)
				(xy 91.485206 8.443645) (xy 91.852445 8.722394) (xy 92.24172 8.969435) (xy 92.650302 9.183037) (xy 93.075325 9.3617)
				(xy 93.513807 9.504171) (xy 93.962673 9.609452) (xy 94.418775 9.676803) (xy 94.878913 9.705753)
				(xy 95.339859 9.696097) (xy 95.798381 9.647905) (xy 96.251262 9.561513) (xy 96.695326 9.437528)
				(xy 97.127458 9.27682) (xy 97.544626 9.080515) (xy 97.943905 8.849991) (xy 98.322494 8.586865) (xy 98.677737 8.292983)
				(xy 99.007143 7.970404) (xy 99.308401 7.621394) (xy 99.579398 7.248398) (xy 99.818233 6.854035)
				(xy 100.023231 6.441069) (xy 100.192954 6.012398) (xy 100.326212 5.571028) (xy 100.422069 5.120055)
				(xy 100.479853 4.662643)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
			"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
			"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
			"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
			"In29.Cu" "In30.Cu"
		)
		(name "MH")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 100.49916 54.202) (xy 100.479853 53.741357) (xy 100.422069 53.283945) (xy 100.326212 52.832972)
				(xy 100.192954 52.391602) (xy 100.023231 51.962931) (xy 99.818233 51.549965) (xy 99.579398 51.155602)
				(xy 99.308401 50.782606) (xy 99.007143 50.433596) (xy 98.677737 50.111017) (xy 98.322494 49.817135)
				(xy 97.943905 49.554009) (xy 97.544626 49.323485) (xy 97.127458 49.12718) (xy 96.695326 48.966472)
				(xy 96.251262 48.842487) (xy 95.798381 48.756095) (xy 95.339859 48.707903) (xy 94.878913 48.698247)
				(xy 94.418775 48.727197) (xy 93.962673 48.794548) (xy 93.513807 48.899829) (xy 93.075325 49.0423)
				(xy 92.650302 49.220963) (xy 92.24172 49.434565) (xy 91.852445 49.681606) (xy 91.485206 49.960355)
				(xy 91.142581 50.268856) (xy 90.826972 50.604946) (xy 90.540594 50.966266) (xy 90.285454 51.350282)
				(xy 90.063343 51.754301) (xy 89.875818 52.175489) (xy 89.724194 52.610892) (xy 89.609537 53.057454)
				(xy 89.532648 53.512046) (xy 89.494069 53.971476) (xy 89.494069 54.432524) (xy 89.532648 54.891954)
				(xy 89.609537 55.346546) (xy 89.724194 55.793108) (xy 89.875818 56.228511) (xy 90.063343 56.649699)
				(xy 90.285454 57.053718) (xy 90.540594 57.437734) (xy 90.826972 57.799054) (xy 91.142581 58.135144)
				(xy 91.485206 58.443645) (xy 91.852445 58.722394) (xy 92.24172 58.969435) (xy 92.650302 59.183037)
				(xy 93.075325 59.3617) (xy 93.513807 59.504171) (xy 93.962673 59.609452) (xy 94.418775 59.676803)
				(xy 94.878913 59.705753) (xy 95.339859 59.696097) (xy 95.798381 59.647905) (xy 96.251262 59.561513)
				(xy 96.695326 59.437528) (xy 97.127458 59.27682) (xy 97.544626 59.080515) (xy 97.943905 58.849991)
				(xy 98.322494 58.586865) (xy 98.677737 58.292983) (xy 99.007143 57.970404) (xy 99.308401 57.621394)
				(xy 99.579398 57.248398) (xy 99.818233 56.854035) (xy 100.023231 56.441069) (xy 100.192954 56.012398)
				(xy 100.326212 55.571028) (xy 100.422069 55.120055) (xy 100.479853 54.662643)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD7_3DMODEL_DIR}/Transistor_Power_Module.3dshapes/Infineon_AG-ECONO3B.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
