(footprint "Infineon_EasyPACK-1B"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "22-lead TH, EasyPACK 1B, https://www.infineon.com/dgdl/Infineon-FS30R06W1E3-DataSheet-v02_01-EN.pdf?fileId=db3a304313b8b5a60113cecd4c3102c1")
	(tags "igbt diode module")
	(property "Reference" "REF**"
		(at -11.43 0 0)
		(layer "F.SilkS")
	)
	(property "Value" "Infineon_EasyPACK-1B"
		(at 15.4 12.6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 16 14.1 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -5.25 -1.2 180)
		(size 2.3 2.3)
		(drill 2.3)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -5.25 26.8 180)
		(size 2.3 2.3)
		(drill 2.3)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 6.4 12.8 180)
		(size 6 6)
		(drill 6)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 37.25 -1.2 180)
		(size 2.3 2.3)
		(drill 2.3)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 37.25 26.8 180)
		(size 2.3 2.3)
		(drill 2.3)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "EU" thru_hole circle
		(at 32 0 180)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "EU" thru_hole circle
		(at 32 3.2 180)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "EV" thru_hole circle
		(at 32 6.4 180)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "EV" thru_hole circle
		(at 32 9.6 180)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "EW" thru_hole circle
		(at 32 22.4 180)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "EW" thru_hole circle
		(at 32 25.6 180)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "G1" thru_hole circle
		(at 0 0 180)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "G2" thru_hole circle
		(at 28.8 0 180)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "G3" thru_hole circle
		(at 0 6.4 180)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "G4" thru_hole circle
		(at 32 16 180)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "G5" thru_hole circle
		(at 0 25.6 180)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "G6" thru_hole circle
		(at 28.8 25.6 180)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "P" thru_hole circle
		(at 12.8 9.6 180)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "P" thru_hole circle
		(at 16 9.6 180)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "T1" thru_hole circle
		(at 22.4 9.6 180)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "T2" thru_hole circle
		(at 25.6 9.6 180)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "U" thru_hole circle
		(at 3.2 0 180)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "U" thru_hole circle
		(at 6.4 0 180)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "V" thru_hole circle
		(at 0 16 180)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "V" thru_hole circle
		(at 0 19.2 180)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "W" thru_hole circle
		(at 3.2 25.6 180)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "W" thru_hole circle
		(at 6.4 25.6 180)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
			"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
			"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
			"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
			"In29.Cu" "In30.Cu"
		)
		(name "MH")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -5.754926 12.8) (xy -5.774496 13.230965) (xy -5.833045 13.658382) (xy -5.930091 14.078734) (xy -6.064835 14.48856)
				(xy -6.236168 14.884487) (xy -6.44268 15.263257) (xy -6.68267 15.621751) (xy -6.954165 15.957018)
				(xy -7.254928 16.2663) (xy -7.582484 16.547049) (xy -7.934137 16.796956) (xy -8.306993 17.013964)
				(xy -8.697982 17.196285) (xy -9.103886 17.342419) (xy -9.521365 17.451164) (xy -9.94698 17.521624)
				(xy -10.377231 17.55322) (xy -10.808574 17.545691) (xy -11.237459 17.499099) (xy -11.660357 17.413828)
				(xy -12.073785 17.29058) (xy -12.474342 17.130368) (xy -12.85873 16.934513) (xy -13.223785 16.704625)
				(xy -13.566503 16.442598) (xy -13.884061 16.150588) (xy -14.173847 15.830998) (xy -14.433476 15.48646)
				(xy -14.660809 15.119809) (xy -14.853976 14.734063) (xy -15.011387 14.332397) (xy -15.131746 13.918118)
				(xy -15.214063 13.494636) (xy -15.25766 13.065435) (xy -15.262177 12.63405) (xy -15.227579 12.204031)
				(xy -15.154149 11.778918) (xy -15.042492 11.362209) (xy -14.893528 10.957335) (xy -14.708481 10.567628)
				(xy -14.488876 10.196296) (xy -14.23652 9.846396) (xy -13.953491 9.520808) (xy -13.642117 9.222211)
				(xy -13.304962 8.953064) (xy -12.944802 8.715582) (xy -12.5646 8.51172) (xy -12.167486 8.343155)
				(xy -11.756729 8.211275) (xy -11.33571 8.117166) (xy -10.907894 8.061603) (xy -10.476804 8.045042)
				(xy -10.045986 8.06762) (xy -9.618988 8.129151) (xy -9.199324 8.22913) (xy -8.790448 8.366731) (xy -8.395727 8.540824)
				(xy -8.018408 8.749975) (xy -7.661598 8.992463) (xy -7.328234 9.266291) (xy -7.02106 9.569206) (xy -6.742604 9.898715)
				(xy -6.495158 10.252104) (xy -6.280759 10.626466) (xy -6.101172 11.018718) (xy -5.957875 11.425632)
				(xy -5.852047 11.84386) (xy -5.78456 12.269957) (xy -5.755969 12.700417)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
			"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
			"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
			"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
			"In29.Cu" "In30.Cu"
		)
		(name "MH")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 47.245074 12.8) (xy 47.225504 13.230965) (xy 47.166955 13.658382) (xy 47.069909 14.078734) (xy 46.935165 14.48856)
				(xy 46.763832 14.884487) (xy 46.55732 15.263257) (xy 46.31733 15.621751) (xy 46.045835 15.957018)
				(xy 45.745072 16.2663) (xy 45.417516 16.547049) (xy 45.065863 16.796956) (xy 44.693007 17.013964)
				(xy 44.302018 17.196285) (xy 43.896114 17.342419) (xy 43.478635 17.451164) (xy 43.05302 17.521624)
				(xy 42.622769 17.55322) (xy 42.191426 17.545691) (xy 41.762541 17.499099) (xy 41.339643 17.413828)
				(xy 40.926215 17.29058) (xy 40.525658 17.130368) (xy 40.14127 16.934513) (xy 39.776215 16.704625)
				(xy 39.433497 16.442598) (xy 39.115939 16.150588) (xy 38.826153 15.830998) (xy 38.566524 15.48646)
				(xy 38.339191 15.119809) (xy 38.146024 14.734063) (xy 37.988613 14.332397) (xy 37.868254 13.918118)
				(xy 37.785937 13.494636) (xy 37.74234 13.065435) (xy 37.737823 12.63405) (xy 37.772421 12.204031)
				(xy 37.845851 11.778918) (xy 37.957508 11.362209) (xy 38.106472 10.957335) (xy 38.291519 10.567628)
				(xy 38.511124 10.196296) (xy 38.76348 9.846396) (xy 39.046509 9.520808) (xy 39.357883 9.222211)
				(xy 39.695038 8.953064) (xy 40.055198 8.715582) (xy 40.4354 8.51172) (xy 40.832514 8.343155) (xy 41.243271 8.211275)
				(xy 41.66429 8.117166) (xy 42.092106 8.061603) (xy 42.523196 8.045042) (xy 42.954014 8.06762) (xy 43.381012 8.129151)
				(xy 43.800676 8.22913) (xy 44.209552 8.366731) (xy 44.604273 8.540824) (xy 44.981592 8.749975) (xy 45.338402 8.992463)
				(xy 45.671766 9.266291) (xy 45.97894 9.569206) (xy 46.257396 9.898715) (xy 46.504842 10.252104)
				(xy 46.719241 10.626466) (xy 46.898828 11.018718) (xy 47.042125 11.425632) (xy 47.147953 11.84386)
				(xy 47.21544 12.269957) (xy 47.244031 12.700417)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD7_3DMODEL_DIR}/Transistor_Power_Module.3dshapes/Infineon_EasyPACK-1B.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
