(footprint "Infineon_EasyPIM-1B"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "35-lead TH, EasyPIM 1B, https://www.infineon.com/dgdl/Infineon-FP10R06W1E3-DS-v02_01-en_de.pdf?fileId=db3a304412b407950112b43312285a63")
	(tags "brifge rectifier igbt diode module")
	(property "Reference" "REF**"
		(at -11.4 2.4 0)
		(layer "F.SilkS")
	)
	(property "Value" "Infineon_EasyPIM-1B"
		(at 15.4 13 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 16 11.5 180)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -5.25 -1.2)
		(size 2.3 2.3)
		(drill 2.3)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -5.25 26.8)
		(size 2.3 2.3)
		(drill 2.3)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 25.6 12.8)
		(size 6 6)
		(drill 6)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 37.25 -1.2)
		(size 2.3 2.3)
		(drill 2.3)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 37.25 26.8)
		(size 2.3 2.3)
		(drill 2.3)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "B" thru_hole circle
		(at 0 25.6)
		(size 1.06 1.06)
		(drill 0.66)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "EU" thru_hole circle
		(at 32 25.6)
		(size 1.06 1.06)
		(drill 0.66)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "EV" thru_hole circle
		(at 25.6 25.6)
		(size 1.06 1.06)
		(drill 0.66)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "EW" thru_hole circle
		(at 19.2 25.6)
		(size 1.06 1.06)
		(drill 0.66)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "G1" thru_hole circle
		(at 28.8 0)
		(size 1.06 1.06)
		(drill 0.66)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "G2" thru_hole circle
		(at 28.8 25.6)
		(size 1.06 1.06)
		(drill 0.66)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "G3" thru_hole circle
		(at 19.2 0)
		(size 1.06 1.06)
		(drill 0.66)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "G4" thru_hole circle
		(at 22.4 25.6)
		(size 1.06 1.06)
		(drill 0.66)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "G5" thru_hole circle
		(at 9.6 0)
		(size 1.06 1.06)
		(drill 0.66)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "G6" thru_hole circle
		(at 16 25.6)
		(size 1.06 1.06)
		(drill 0.66)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "GB" thru_hole circle
		(at 9.6 25.6)
		(size 1.06 1.06)
		(drill 0.66)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "L1" thru_hole rect
		(at 0 0)
		(size 1.06 1.06)
		(drill 0.66)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "L2" thru_hole circle
		(at 6.4 6.6)
		(size 1.06 1.06)
		(drill 0.66)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "L3" thru_hole circle
		(at 6.4 12.8)
		(size 1.06 1.06)
		(drill 0.66)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "N" thru_hole circle
		(at 12.8 25.6)
		(size 1.06 1.06)
		(drill 0.66)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "NB" thru_hole circle
		(at 6.4 25.6)
		(size 1.06 1.06)
		(drill 0.66)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "P" thru_hole circle
		(at 6.4 19.2)
		(size 1.06 1.06)
		(drill 0.66)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "P1" thru_hole circle
		(at 9.6 19.2)
		(size 1.06 1.06)
		(drill 0.66)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "T1" thru_hole circle
		(at 12.8 9.6)
		(size 1.06 1.06)
		(drill 0.66)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "T2" thru_hole circle
		(at 16 9.6)
		(size 1.06 1.06)
		(drill 0.66)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "U" thru_hole circle
		(at 32 0)
		(size 1.06 1.06)
		(drill 0.66)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "V" thru_hole circle
		(at 22.4 0)
		(size 1.06 1.06)
		(drill 0.66)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "W" thru_hole circle
		(at 12.8 0)
		(size 1.06 1.06)
		(drill 0.66)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
			"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
			"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
			"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
			"In29.Cu" "In30.Cu"
		)
		(name "MH")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -5.754926 12.8) (xy -5.774496 12.369035) (xy -5.833045 11.941618) (xy -5.930091 11.521266) (xy -6.064835 11.11144)
				(xy -6.236168 10.715513) (xy -6.44268 10.336743) (xy -6.68267 9.978249) (xy -6.954165 9.642982)
				(xy -7.254928 9.3337) (xy -7.582484 9.052951) (xy -7.934137 8.803044) (xy -8.306993 8.586036) (xy -8.697982 8.403715)
				(xy -9.103886 8.257581) (xy -9.521365 8.148836) (xy -9.94698 8.078376) (xy -10.377231 8.04678) (xy -10.808574 8.054309)
				(xy -11.237459 8.100901) (xy -11.660357 8.186172) (xy -12.073785 8.30942) (xy -12.474342 8.469632)
				(xy -12.85873 8.665487) (xy -13.223785 8.895375) (xy -13.566503 9.157402) (xy -13.884061 9.449412)
				(xy -14.173847 9.769002) (xy -14.433476 10.11354) (xy -14.660809 10.480191) (xy -14.853976 10.865937)
				(xy -15.011387 11.267603) (xy -15.131746 11.681882) (xy -15.214063 12.105364) (xy -15.25766 12.534565)
				(xy -15.262177 12.96595) (xy -15.227579 13.395969) (xy -15.154149 13.821082) (xy -15.042492 14.237791)
				(xy -14.893528 14.642665) (xy -14.708481 15.032372) (xy -14.488876 15.403704) (xy -14.23652 15.753604)
				(xy -13.953491 16.079192) (xy -13.642117 16.377789) (xy -13.304962 16.646936) (xy -12.944802 16.884418)
				(xy -12.5646 17.08828) (xy -12.167486 17.256845) (xy -11.756729 17.388725) (xy -11.33571 17.482834)
				(xy -10.907894 17.538397) (xy -10.476804 17.554958) (xy -10.045986 17.53238) (xy -9.618988 17.470849)
				(xy -9.199324 17.37087) (xy -8.790448 17.233269) (xy -8.395727 17.059176) (xy -8.018408 16.850025)
				(xy -7.661598 16.607537) (xy -7.328234 16.333709) (xy -7.02106 16.030794) (xy -6.742604 15.701285)
				(xy -6.495158 15.347896) (xy -6.280759 14.973534) (xy -6.101172 14.581282) (xy -5.957875 14.174368)
				(xy -5.852047 13.75614) (xy -5.78456 13.330043) (xy -5.755969 12.899583)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
			"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
			"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
			"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
			"In29.Cu" "In30.Cu"
		)
		(name "MH")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 47.245074 12.8) (xy 47.225504 12.369035) (xy 47.166955 11.941618) (xy 47.069909 11.521266) (xy 46.935165 11.11144)
				(xy 46.763832 10.715513) (xy 46.55732 10.336743) (xy 46.31733 9.978249) (xy 46.045835 9.642982)
				(xy 45.745072 9.3337) (xy 45.417516 9.052951) (xy 45.065863 8.803044) (xy 44.693007 8.586036) (xy 44.302018 8.403715)
				(xy 43.896114 8.257581) (xy 43.478635 8.148836) (xy 43.05302 8.078376) (xy 42.622769 8.04678) (xy 42.191426 8.054309)
				(xy 41.762541 8.100901) (xy 41.339643 8.186172) (xy 40.926215 8.30942) (xy 40.525658 8.469632) (xy 40.14127 8.665487)
				(xy 39.776215 8.895375) (xy 39.433497 9.157402) (xy 39.115939 9.449412) (xy 38.826153 9.769002)
				(xy 38.566524 10.11354) (xy 38.339191 10.480191) (xy 38.146024 10.865937) (xy 37.988613 11.267603)
				(xy 37.868254 11.681882) (xy 37.785937 12.105364) (xy 37.74234 12.534565) (xy 37.737823 12.96595)
				(xy 37.772421 13.395969) (xy 37.845851 13.821082) (xy 37.957508 14.237791) (xy 38.106472 14.642665)
				(xy 38.291519 15.032372) (xy 38.511124 15.403704) (xy 38.76348 15.753604) (xy 39.046509 16.079192)
				(xy 39.357883 16.377789) (xy 39.695038 16.646936) (xy 40.055198 16.884418) (xy 40.4354 17.08828)
				(xy 40.832514 17.256845) (xy 41.243271 17.388725) (xy 41.66429 17.482834) (xy 42.092106 17.538397)
				(xy 42.523196 17.554958) (xy 42.954014 17.53238) (xy 43.381012 17.470849) (xy 43.800676 17.37087)
				(xy 44.209552 17.233269) (xy 44.604273 17.059176) (xy 44.981592 16.850025) (xy 45.338402 16.607537)
				(xy 45.671766 16.333709) (xy 45.97894 16.030794) (xy 46.257396 15.701285) (xy 46.504842 15.347896)
				(xy 46.719241 14.973534) (xy 46.898828 14.581282) (xy 47.042125 14.174368) (xy 47.147953 13.75614)
				(xy 47.21544 13.330043) (xy 47.244031 12.899583)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Transistor_Power_Module.3dshapes/Infineon_EasyPIM-1B.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
