(footprint "Infineon_EasyPIM-2B"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "35-lead TH, EasyPIM 2B, same as ST_ACEPACK-2-CIB, https://www.infineon.com/dgdl/Infineon-FP50R06W2E3-DS-v02_02-EN.pdf?fileId=db3a30431b3e89eb011b455c99987d24")
	(tags "brifge rectifier igbt diode module")
	(property "Reference" "REF**"
		(at 0 -6 180)
		(layer "F.SilkS")
	)
	(property "Value" "Infineon_EasyPIM-2B"
		(at 16 23.5 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 16 22 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -5.25 -1.5)
		(size 2.3 2.3)
		(drill 2.3)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -5.25 49.5)
		(size 2.3 2.3)
		(drill 2.3)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 16 12.8)
		(size 6 6)
		(drill 6)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 37.25 -1.5)
		(size 2.3 2.3)
		(drill 2.3)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 37.25 49.5)
		(size 2.3 2.3)
		(drill 2.3)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "B" thru_hole circle
		(at 22.4 28.8)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "EU" thru_hole circle
		(at 32 19.2)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "EU" thru_hole circle
		(at 32 22.4)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "EV" thru_hole circle
		(at 32 9.6)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "EV" thru_hole circle
		(at 32 12.8)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "EW" thru_hole circle
		(at 32 0)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "EW" thru_hole circle
		(at 32 3.2)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "G1" thru_hole circle
		(at 0 28.8)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "G2" thru_hole circle
		(at 32 25.6)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "G3" thru_hole circle
		(at 0 12.8)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "G4" thru_hole circle
		(at 32 16)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "G5" thru_hole circle
		(at 3.2 0)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "G6" thru_hole circle
		(at 32 6.4)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "GB" thru_hole circle
		(at 32 32)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "L1" thru_hole circle
		(at 16 38.4)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "L1" thru_hole circle
		(at 19.2 38.4)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "L2" thru_hole circle
		(at 6.4 41.6)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "L2" thru_hole circle
		(at 9.6 41.6)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "L3" thru_hole circle
		(at 0 44.8)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "L3" thru_hole circle
		(at 0 48)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "N" thru_hole circle
		(at 32 44.8)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "N" thru_hole circle
		(at 32 48)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "NB" thru_hole circle
		(at 32 28.8)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "P" thru_hole circle
		(at 22.4 44.8)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "P" thru_hole circle
		(at 22.4 48)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "P1" thru_hole circle
		(at 9.6 28.8)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "P1" thru_hole circle
		(at 9.6 32)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "T1" thru_hole circle
		(at 22.4 0)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "T2" thru_hole circle
		(at 12.8 0)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "U" thru_hole circle
		(at 0 32)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "U" thru_hole circle
		(at 0 35.2)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "V" thru_hole circle
		(at 0 16)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "V" thru_hole circle
		(at 0 19.2)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "W" thru_hole rect
		(at 0 0)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "W" thru_hole circle
		(at 0 3.2)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
			"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
			"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
			"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
			"In29.Cu" "In30.Cu"
		)
		(name "MH")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -5.754926 24) (xy -5.774496 23.569035) (xy -5.833045 23.141618) (xy -5.930091 22.721266) (xy -6.064835 22.31144)
				(xy -6.236168 21.915513) (xy -6.44268 21.536743) (xy -6.68267 21.178249) (xy -6.954165 20.842982)
				(xy -7.254928 20.5337) (xy -7.582484 20.252951) (xy -7.934137 20.003044) (xy -8.306993 19.786036)
				(xy -8.697982 19.603715) (xy -9.103886 19.457581) (xy -9.521365 19.348836) (xy -9.94698 19.278376)
				(xy -10.377231 19.24678) (xy -10.808574 19.254309) (xy -11.237459 19.300901) (xy -11.660357 19.386172)
				(xy -12.073785 19.50942) (xy -12.474342 19.669632) (xy -12.85873 19.865487) (xy -13.223785 20.095375)
				(xy -13.566503 20.357402) (xy -13.884061 20.649412) (xy -14.173847 20.969002) (xy -14.433476 21.31354)
				(xy -14.660809 21.680191) (xy -14.853976 22.065937) (xy -15.011387 22.467603) (xy -15.131746 22.881882)
				(xy -15.214063 23.305364) (xy -15.25766 23.734565) (xy -15.262177 24.16595) (xy -15.227579 24.595969)
				(xy -15.154149 25.021082) (xy -15.042492 25.437791) (xy -14.893528 25.842665) (xy -14.708481 26.232372)
				(xy -14.488876 26.603704) (xy -14.23652 26.953604) (xy -13.953491 27.279192) (xy -13.642117 27.577789)
				(xy -13.304962 27.846936) (xy -12.944802 28.084418) (xy -12.5646 28.28828) (xy -12.167486 28.456845)
				(xy -11.756729 28.588725) (xy -11.33571 28.682834) (xy -10.907894 28.738397) (xy -10.476804 28.754958)
				(xy -10.045986 28.73238) (xy -9.618988 28.670849) (xy -9.199324 28.57087) (xy -8.790448 28.433269)
				(xy -8.395727 28.259176) (xy -8.018408 28.050025) (xy -7.661598 27.807537) (xy -7.328234 27.533709)
				(xy -7.02106 27.230794) (xy -6.742604 26.901285) (xy -6.495158 26.547896) (xy -6.280759 26.173534)
				(xy -6.101172 25.781282) (xy -5.957875 25.374368) (xy -5.852047 24.95614) (xy -5.78456 24.530043)
				(xy -5.755969 24.099583)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
			"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
			"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
			"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
			"In29.Cu" "In30.Cu"
		)
		(name "MH")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 47.245074 24) (xy 47.225504 23.569035) (xy 47.166955 23.141618) (xy 47.069909 22.721266) (xy 46.935165 22.31144)
				(xy 46.763832 21.915513) (xy 46.55732 21.536743) (xy 46.31733 21.178249) (xy 46.045835 20.842982)
				(xy 45.745072 20.5337) (xy 45.417516 20.252951) (xy 45.065863 20.003044) (xy 44.693007 19.786036)
				(xy 44.302018 19.603715) (xy 43.896114 19.457581) (xy 43.478635 19.348836) (xy 43.05302 19.278376)
				(xy 42.622769 19.24678) (xy 42.191426 19.254309) (xy 41.762541 19.300901) (xy 41.339643 19.386172)
				(xy 40.926215 19.50942) (xy 40.525658 19.669632) (xy 40.14127 19.865487) (xy 39.776215 20.095375)
				(xy 39.433497 20.357402) (xy 39.115939 20.649412) (xy 38.826153 20.969002) (xy 38.566524 21.31354)
				(xy 38.339191 21.680191) (xy 38.146024 22.065937) (xy 37.988613 22.467603) (xy 37.868254 22.881882)
				(xy 37.785937 23.305364) (xy 37.74234 23.734565) (xy 37.737823 24.16595) (xy 37.772421 24.595969)
				(xy 37.845851 25.021082) (xy 37.957508 25.437791) (xy 38.106472 25.842665) (xy 38.291519 26.232372)
				(xy 38.511124 26.603704) (xy 38.76348 26.953604) (xy 39.046509 27.279192) (xy 39.357883 27.577789)
				(xy 39.695038 27.846936) (xy 40.055198 28.084418) (xy 40.4354 28.28828) (xy 40.832514 28.456845)
				(xy 41.243271 28.588725) (xy 41.66429 28.682834) (xy 42.092106 28.738397) (xy 42.523196 28.754958)
				(xy 42.954014 28.73238) (xy 43.381012 28.670849) (xy 43.800676 28.57087) (xy 44.209552 28.433269)
				(xy 44.604273 28.259176) (xy 44.981592 28.050025) (xy 45.338402 27.807537) (xy 45.671766 27.533709)
				(xy 45.97894 27.230794) (xy 46.257396 26.901285) (xy 46.504842 26.547896) (xy 46.719241 26.173534)
				(xy 46.898828 25.781282) (xy 47.042125 25.374368) (xy 47.147953 24.95614) (xy 47.21544 24.530043)
				(xy 47.244031 24.099583)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Transistor_Power_Module.3dshapes/Infineon_EasyPIM-2B.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
