(footprint "Littelfuse_Package_H_XBN2MM"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "24-lead TH, Package H, https://www.littelfuse.com/~/media/electronics/datasheets/power_semiconductors/littelfuse_power_semiconductor_igbt_module_mg1215h_xbn2mm_datasheet.pdf.pdf")
	(tags "brifge rectifier igbt diode module")
	(property "Reference" "REF**"
		(at -20.85 -3 0)
		(layer "F.SilkS")
	)
	(property "Value" "Littelfuse_Package_H_XBN2MM"
		(at 28.48 20.95 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 28.5 19.05 180)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -16.02 4.95)
		(size 2.6 2.6)
		(drill 2.6)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -16.02 36.95)
		(size 2.6 2.6)
		(drill 2.6)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 76.98 4.95)
		(size 2.6 2.6)
		(drill 2.6)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 76.98 36.95)
		(size 2.6 2.6)
		(drill 2.6)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 11.43 0)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 22.86 0)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 34.29 0)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 45.72 0)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 57.15 0)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 70.08 13.33)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 70.08 28.57)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 70.08 32.38)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole circle
		(at 64.77 41.9)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 60.96 41.9)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole circle
		(at 57.15 41.9)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at 53.34 41.9)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole circle
		(at 49.53 41.9)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "15" thru_hole circle
		(at 41.91 41.9)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "16" thru_hole circle
		(at 38.1 41.9)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "17" thru_hole circle
		(at 30.48 41.9)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "18" thru_hole circle
		(at 26.67 41.9)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "19" thru_hole circle
		(at 19.05 41.9)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "20" thru_hole circle
		(at 15.24 41.9)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at -9.12 36.19)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "22" thru_hole circle
		(at -9.12 28.57)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "23" thru_hole circle
		(at -9.12 13.33)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "24" thru_hole circle
		(at -9.12 5.71)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
			"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
			"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
			"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
			"In29.Cu" "In30.Cu"
		)
		(name "MH")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -10.51504 20.95) (xy -10.534347 20.489357) (xy -10.592131 20.031945) (xy -10.687988 19.580972)
				(xy -10.821246 19.139602) (xy -10.990969 18.710931) (xy -11.195967 18.297965) (xy -11.434802 17.903602)
				(xy -11.705799 17.530606) (xy -12.007057 17.181596) (xy -12.336463 16.859017) (xy -12.691706 16.565135)
				(xy -13.070295 16.302009) (xy -13.469574 16.071485) (xy -13.886742 15.87518) (xy -14.318874 15.714472)
				(xy -14.762938 15.590487) (xy -15.215819 15.504095) (xy -15.674341 15.455903) (xy -16.135287 15.446247)
				(xy -16.595425 15.475197) (xy -17.051527 15.542548) (xy -17.500393 15.647829) (xy -17.938875 15.7903)
				(xy -18.363898 15.968963) (xy -18.77248 16.182565) (xy -19.161755 16.429606) (xy -19.528994 16.708355)
				(xy -19.871619 17.016856) (xy -20.187228 17.352946) (xy -20.473606 17.714266) (xy -20.728746 18.098282)
				(xy -20.950857 18.502301) (xy -21.138382 18.923489) (xy -21.290006 19.358892) (xy -21.404663 19.805454)
				(xy -21.481552 20.260046) (xy -21.520131 20.719476) (xy -21.520131 21.180524) (xy -21.481552 21.639954)
				(xy -21.404663 22.094546) (xy -21.290006 22.541108) (xy -21.138382 22.976511) (xy -20.950857 23.397699)
				(xy -20.728746 23.801718) (xy -20.473606 24.185734) (xy -20.187228 24.547054) (xy -19.871619 24.883144)
				(xy -19.528994 25.191645) (xy -19.161755 25.470394) (xy -18.77248 25.717435) (xy -18.363898 25.931037)
				(xy -17.938875 26.1097) (xy -17.500393 26.252171) (xy -17.051527 26.357452) (xy -16.595425 26.424803)
				(xy -16.135287 26.453753) (xy -15.674341 26.444097) (xy -15.215819 26.395905) (xy -14.762938 26.309513)
				(xy -14.318874 26.185528) (xy -13.886742 26.02482) (xy -13.469574 25.828515) (xy -13.070295 25.597991)
				(xy -12.691706 25.334865) (xy -12.336463 25.040983) (xy -12.007057 24.718404) (xy -11.705799 24.369394)
				(xy -11.434802 23.996398) (xy -11.195967 23.602035) (xy -10.990969 23.189069) (xy -10.821246 22.760398)
				(xy -10.687988 22.319028) (xy -10.592131 21.868055) (xy -10.534347 21.410643)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
			"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
			"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
			"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
			"In29.Cu" "In30.Cu"
		)
		(name "MH")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 82.48496 20.95) (xy 82.465653 20.489357) (xy 82.407869 20.031945) (xy 82.312012 19.580972) (xy 82.178754 19.139602)
				(xy 82.009031 18.710931) (xy 81.804033 18.297965) (xy 81.565198 17.903602) (xy 81.294201 17.530606)
				(xy 80.992943 17.181596) (xy 80.663537 16.859017) (xy 80.308294 16.565135) (xy 79.929705 16.302009)
				(xy 79.530426 16.071485) (xy 79.113258 15.87518) (xy 78.681126 15.714472) (xy 78.237062 15.590487)
				(xy 77.784181 15.504095) (xy 77.325659 15.455903) (xy 76.864713 15.446247) (xy 76.404575 15.475197)
				(xy 75.948473 15.542548) (xy 75.499607 15.647829) (xy 75.061125 15.7903) (xy 74.636102 15.968963)
				(xy 74.22752 16.182565) (xy 73.838245 16.429606) (xy 73.471006 16.708355) (xy 73.128381 17.016856)
				(xy 72.812772 17.352946) (xy 72.526394 17.714266) (xy 72.271254 18.098282) (xy 72.049143 18.502301)
				(xy 71.861618 18.923489) (xy 71.709994 19.358892) (xy 71.595337 19.805454) (xy 71.518448 20.260046)
				(xy 71.479869 20.719476) (xy 71.479869 21.180524) (xy 71.518448 21.639954) (xy 71.595337 22.094546)
				(xy 71.709994 22.541108) (xy 71.861618 22.976511) (xy 72.049143 23.397699) (xy 72.271254 23.801718)
				(xy 72.526394 24.185734) (xy 72.812772 24.547054) (xy 73.128381 24.883144) (xy 73.471006 25.191645)
				(xy 73.838245 25.470394) (xy 74.22752 25.717435) (xy 74.636102 25.931037) (xy 75.061125 26.1097)
				(xy 75.499607 26.252171) (xy 75.948473 26.357452) (xy 76.404575 26.424803) (xy 76.864713 26.453753)
				(xy 77.325659 26.444097) (xy 77.784181 26.395905) (xy 78.237062 26.309513) (xy 78.681126 26.185528)
				(xy 79.113258 26.02482) (xy 79.530426 25.828515) (xy 79.929705 25.597991) (xy 80.308294 25.334865)
				(xy 80.663537 25.040983) (xy 80.992943 24.718404) (xy 81.294201 24.369394) (xy 81.565198 23.996398)
				(xy 81.804033 23.602035) (xy 82.009031 23.189069) (xy 82.178754 22.760398) (xy 82.312012 22.319028)
				(xy 82.407869 21.868055) (xy 82.465653 21.410643)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Transistor_Power_Module.3dshapes/Littelfuse_Package_H_XBN2MM.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
