(footprint "Littelfuse_Package_W_XN2MM"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "35-lead TH, Package W, https://www.littelfuse.com/~/media/electronics/datasheets/power_semiconductors/littelfuse_power_semiconductor_igbt_module_mg1275w_xn2mm_datasheet.pdf.pdf")
	(tags "igbt diode module")
	(property "Reference" "REF**"
		(at -15.1 -3.9 180)
		(layer "F.SilkS")
	)
	(property "Value" "Littelfuse_Package_W_XN2MM"
		(at 44.9 29.2 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 44.8 27.2 180)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -7.24 0.45)
		(size 2.5 2.5)
		(drill 2.5)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -7.24 57.91)
		(size 2.5 2.5)
		(drill 2.5)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 87.26 0.45)
		(size 2.5 2.5)
		(drill 2.5)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 87.26 57.91)
		(size 2.5 2.5)
		(drill 2.5)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 3.81 0)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 15.24 0)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 19.05 0)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 30.48 0)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 34.29 0)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 45.72 0)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 49.53 0)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 60.96 0)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole circle
		(at 64.77 0)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 76.2 0)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole circle
		(at 80.01 0)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at 99.07 15.86)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole circle
		(at 99.07 19.67)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "15" thru_hole circle
		(at 99.07 23.48)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "16" thru_hole circle
		(at 99.07 34.91)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "17" thru_hole circle
		(at 99.07 38.72)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "18" thru_hole circle
		(at 99.07 42.53)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "19" thru_hole circle
		(at 81.92 58.4)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "20" thru_hole circle
		(at 78.11 58.4)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 62.91 58.4)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "22" thru_hole circle
		(at 59.11 58.4)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "23" thru_hole circle
		(at 55.25 58.4)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "24" thru_hole circle
		(at 40.01 58.4)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "25" thru_hole circle
		(at 36.21 58.4)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "26" thru_hole circle
		(at 32.39 58.4)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "27" thru_hole circle
		(at 17.15 58.4)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "28" thru_hole circle
		(at 13.34 58.4)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "29" thru_hole circle
		(at 9.51 58.4)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "30" thru_hole circle
		(at -19.05 42.53)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "31" thru_hole circle
		(at -19.05 38.72)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "32" thru_hole circle
		(at -19.05 34.91)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at -19.05 23.48)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "34" thru_hole circle
		(at -19.05 19.67)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "35" thru_hole circle
		(at -19.05 15.8)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
			"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
			"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
			"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
			"In29.Cu" "In30.Cu"
		)
		(name "MH")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -9.48504 4.2) (xy -9.504347 3.739357) (xy -9.562131 3.281945) (xy -9.657988 2.830972) (xy -9.791246 2.389602)
				(xy -9.960969 1.960931) (xy -10.165967 1.547965) (xy -10.404802 1.153602) (xy -10.675799 0.780606)
				(xy -10.977057 0.431596) (xy -11.306463 0.109017) (xy -11.661706 -0.184865) (xy -12.040295 -0.447991)
				(xy -12.439574 -0.678515) (xy -12.856742 -0.87482) (xy -13.288874 -1.035528) (xy -13.732938 -1.159513)
				(xy -14.185819 -1.245905) (xy -14.644341 -1.294097) (xy -15.105287 -1.303753) (xy -15.565425 -1.274803)
				(xy -16.021527 -1.207452) (xy -16.470393 -1.102171) (xy -16.908875 -0.9597) (xy -17.333898 -0.781037)
				(xy -17.74248 -0.567435) (xy -18.131755 -0.320394) (xy -18.498994 -0.041645) (xy -18.841619 0.266856)
				(xy -19.157228 0.602946) (xy -19.443606 0.964266) (xy -19.698746 1.348282) (xy -19.920857 1.752301)
				(xy -20.108382 2.173489) (xy -20.260006 2.608892) (xy -20.374663 3.055454) (xy -20.451552 3.510046)
				(xy -20.490131 3.969476) (xy -20.490131 4.430524) (xy -20.451552 4.889954) (xy -20.374663 5.344546)
				(xy -20.260006 5.791108) (xy -20.108382 6.226511) (xy -19.920857 6.647699) (xy -19.698746 7.051718)
				(xy -19.443606 7.435734) (xy -19.157228 7.797054) (xy -18.841619 8.133144) (xy -18.498994 8.441645)
				(xy -18.131755 8.720394) (xy -17.74248 8.967435) (xy -17.333898 9.181037) (xy -16.908875 9.3597)
				(xy -16.470393 9.502171) (xy -16.021527 9.607452) (xy -15.565425 9.674803) (xy -15.105287 9.703753)
				(xy -14.644341 9.694097) (xy -14.185819 9.645905) (xy -13.732938 9.559513) (xy -13.288874 9.435528)
				(xy -12.856742 9.27482) (xy -12.439574 9.078515) (xy -12.040295 8.847991) (xy -11.661706 8.584865)
				(xy -11.306463 8.290983) (xy -10.977057 7.968404) (xy -10.675799 7.619394) (xy -10.404802 7.246398)
				(xy -10.165967 6.852035) (xy -9.960969 6.439069) (xy -9.791246 6.010398) (xy -9.657988 5.569028)
				(xy -9.562131 5.118055) (xy -9.504347 4.660643)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
			"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
			"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
			"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
			"In29.Cu" "In30.Cu"
		)
		(name "MH")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -9.48504 54.2) (xy -9.504347 53.739357) (xy -9.562131 53.281945) (xy -9.657988 52.830972) (xy -9.791246 52.389602)
				(xy -9.960969 51.960931) (xy -10.165967 51.547965) (xy -10.404802 51.153602) (xy -10.675799 50.780606)
				(xy -10.977057 50.431596) (xy -11.306463 50.109017) (xy -11.661706 49.815135) (xy -12.040295 49.552009)
				(xy -12.439574 49.321485) (xy -12.856742 49.12518) (xy -13.288874 48.964472) (xy -13.732938 48.840487)
				(xy -14.185819 48.754095) (xy -14.644341 48.705903) (xy -15.105287 48.696247) (xy -15.565425 48.725197)
				(xy -16.021527 48.792548) (xy -16.470393 48.897829) (xy -16.908875 49.0403) (xy -17.333898 49.218963)
				(xy -17.74248 49.432565) (xy -18.131755 49.679606) (xy -18.498994 49.958355) (xy -18.841619 50.266856)
				(xy -19.157228 50.602946) (xy -19.443606 50.964266) (xy -19.698746 51.348282) (xy -19.920857 51.752301)
				(xy -20.108382 52.173489) (xy -20.260006 52.608892) (xy -20.374663 53.055454) (xy -20.451552 53.510046)
				(xy -20.490131 53.969476) (xy -20.490131 54.430524) (xy -20.451552 54.889954) (xy -20.374663 55.344546)
				(xy -20.260006 55.791108) (xy -20.108382 56.226511) (xy -19.920857 56.647699) (xy -19.698746 57.051718)
				(xy -19.443606 57.435734) (xy -19.157228 57.797054) (xy -18.841619 58.133144) (xy -18.498994 58.441645)
				(xy -18.131755 58.720394) (xy -17.74248 58.967435) (xy -17.333898 59.181037) (xy -16.908875 59.3597)
				(xy -16.470393 59.502171) (xy -16.021527 59.607452) (xy -15.565425 59.674803) (xy -15.105287 59.703753)
				(xy -14.644341 59.694097) (xy -14.185819 59.645905) (xy -13.732938 59.559513) (xy -13.288874 59.435528)
				(xy -12.856742 59.27482) (xy -12.439574 59.078515) (xy -12.040295 58.847991) (xy -11.661706 58.584865)
				(xy -11.306463 58.290983) (xy -10.977057 57.968404) (xy -10.675799 57.619394) (xy -10.404802 57.246398)
				(xy -10.165967 56.852035) (xy -9.960969 56.439069) (xy -9.791246 56.010398) (xy -9.657988 55.569028)
				(xy -9.562131 55.118055) (xy -9.504347 54.660643)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
			"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
			"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
			"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
			"In29.Cu" "In30.Cu"
		)
		(name "MH")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 100.51496 4.2) (xy 100.495653 3.739357) (xy 100.437869 3.281945) (xy 100.342012 2.830972) (xy 100.208754 2.389602)
				(xy 100.039031 1.960931) (xy 99.834033 1.547965) (xy 99.595198 1.153602) (xy 99.324201 0.780606)
				(xy 99.022943 0.431596) (xy 98.693537 0.109017) (xy 98.338294 -0.184865) (xy 97.959705 -0.447991)
				(xy 97.560426 -0.678515) (xy 97.143258 -0.87482) (xy 96.711126 -1.035528) (xy 96.267062 -1.159513)
				(xy 95.814181 -1.245905) (xy 95.355659 -1.294097) (xy 94.894713 -1.303753) (xy 94.434575 -1.274803)
				(xy 93.978473 -1.207452) (xy 93.529607 -1.102171) (xy 93.091125 -0.9597) (xy 92.666102 -0.781037)
				(xy 92.25752 -0.567435) (xy 91.868245 -0.320394) (xy 91.501006 -0.041645) (xy 91.158381 0.266856)
				(xy 90.842772 0.602946) (xy 90.556394 0.964266) (xy 90.301254 1.348282) (xy 90.079143 1.752301)
				(xy 89.891618 2.173489) (xy 89.739994 2.608892) (xy 89.625337 3.055454) (xy 89.548448 3.510046)
				(xy 89.509869 3.969476) (xy 89.509869 4.430524) (xy 89.548448 4.889954) (xy 89.625337 5.344546)
				(xy 89.739994 5.791108) (xy 89.891618 6.226511) (xy 90.079143 6.647699) (xy 90.301254 7.051718)
				(xy 90.556394 7.435734) (xy 90.842772 7.797054) (xy 91.158381 8.133144) (xy 91.501006 8.441645)
				(xy 91.868245 8.720394) (xy 92.25752 8.967435) (xy 92.666102 9.181037) (xy 93.091125 9.3597) (xy 93.529607 9.502171)
				(xy 93.978473 9.607452) (xy 94.434575 9.674803) (xy 94.894713 9.703753) (xy 95.355659 9.694097)
				(xy 95.814181 9.645905) (xy 96.267062 9.559513) (xy 96.711126 9.435528) (xy 97.143258 9.27482) (xy 97.560426 9.078515)
				(xy 97.959705 8.847991) (xy 98.338294 8.584865) (xy 98.693537 8.290983) (xy 99.022943 7.968404)
				(xy 99.324201 7.619394) (xy 99.595198 7.246398) (xy 99.834033 6.852035) (xy 100.039031 6.439069)
				(xy 100.208754 6.010398) (xy 100.342012 5.569028) (xy 100.437869 5.118055) (xy 100.495653 4.660643)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
			"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
			"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
			"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
			"In29.Cu" "In30.Cu"
		)
		(name "MH")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 100.51496 54.2) (xy 100.495653 53.739357) (xy 100.437869 53.281945) (xy 100.342012 52.830972)
				(xy 100.208754 52.389602) (xy 100.039031 51.960931) (xy 99.834033 51.547965) (xy 99.595198 51.153602)
				(xy 99.324201 50.780606) (xy 99.022943 50.431596) (xy 98.693537 50.109017) (xy 98.338294 49.815135)
				(xy 97.959705 49.552009) (xy 97.560426 49.321485) (xy 97.143258 49.12518) (xy 96.711126 48.964472)
				(xy 96.267062 48.840487) (xy 95.814181 48.754095) (xy 95.355659 48.705903) (xy 94.894713 48.696247)
				(xy 94.434575 48.725197) (xy 93.978473 48.792548) (xy 93.529607 48.897829) (xy 93.091125 49.0403)
				(xy 92.666102 49.218963) (xy 92.25752 49.432565) (xy 91.868245 49.679606) (xy 91.501006 49.958355)
				(xy 91.158381 50.266856) (xy 90.842772 50.602946) (xy 90.556394 50.964266) (xy 90.301254 51.348282)
				(xy 90.079143 51.752301) (xy 89.891618 52.173489) (xy 89.739994 52.608892) (xy 89.625337 53.055454)
				(xy 89.548448 53.510046) (xy 89.509869 53.969476) (xy 89.509869 54.430524) (xy 89.548448 54.889954)
				(xy 89.625337 55.344546) (xy 89.739994 55.791108) (xy 89.891618 56.226511) (xy 90.079143 56.647699)
				(xy 90.301254 57.051718) (xy 90.556394 57.435734) (xy 90.842772 57.797054) (xy 91.158381 58.133144)
				(xy 91.501006 58.441645) (xy 91.868245 58.720394) (xy 92.25752 58.967435) (xy 92.666102 59.181037)
				(xy 93.091125 59.3597) (xy 93.529607 59.502171) (xy 93.978473 59.607452) (xy 94.434575 59.674803)
				(xy 94.894713 59.703753) (xy 95.355659 59.694097) (xy 95.814181 59.645905) (xy 96.267062 59.559513)
				(xy 96.711126 59.435528) (xy 97.143258 59.27482) (xy 97.560426 59.078515) (xy 97.959705 58.847991)
				(xy 98.338294 58.584865) (xy 98.693537 58.290983) (xy 99.022943 57.968404) (xy 99.324201 57.619394)
				(xy 99.595198 57.246398) (xy 99.834033 56.852035) (xy 100.039031 56.439069) (xy 100.208754 56.010398)
				(xy 100.342012 55.569028) (xy 100.437869 55.118055) (xy 100.495653 54.660643)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Transistor_Power_Module.3dshapes/Littelfuse_Package_W_XN2MM.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
