(footprint "ST_ACEPACK-2-CIB"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "35-lead TH, ACEPACK 2 CIB, same as Infineon_EasyPIM-2B, https://www.st.com/resource/en/datasheet/a2c25s12m3.pdf")
	(tags "brifge rectifier igbt diode module")
	(property "Reference" "REF**"
		(at 0 -6 180)
		(layer "F.SilkS")
	)
	(property "Value" "ST_ACEPACK-2-CIB"
		(at 16 23.5 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 16 22 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -5.25 -1.5)
		(size 2.3 2.3)
		(drill 2.3)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -5.25 49.5 90)
		(size 2.3 2.3)
		(drill 2.3)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 16 12.8 90)
		(size 6 6)
		(drill 6)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 37.25 -1.5 270)
		(size 2.3 2.3)
		(drill 2.3)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 37.25 49.5 270)
		(size 2.3 2.3)
		(drill 2.3)
		(layers "*.Cu" "*.Mask")
	)
	(pad "B" thru_hole circle
		(at 22.4 28.8)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "EU" thru_hole circle
		(at 32 19.2)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "EU" thru_hole circle
		(at 32 22.4)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "EV" thru_hole circle
		(at 32 9.6)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "EV" thru_hole circle
		(at 32 12.8)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "EW" thru_hole circle
		(at 32 0)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "EW" thru_hole circle
		(at 32 3.2)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "G1" thru_hole circle
		(at 0 28.8)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "G2" thru_hole circle
		(at 32 25.6)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "G3" thru_hole circle
		(at 0 12.8)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "G4" thru_hole circle
		(at 32 16)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "G5" thru_hole circle
		(at 3.2 0)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "G6" thru_hole circle
		(at 32 6.4)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "GB" thru_hole circle
		(at 32 32)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "L1" thru_hole circle
		(at 16 38.4)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "L1" thru_hole circle
		(at 19.2 38.4)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "L2" thru_hole circle
		(at 6.4 41.6)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "L2" thru_hole circle
		(at 9.6 41.6)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "L3" thru_hole circle
		(at 0 44.8)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "L3" thru_hole circle
		(at 0 48)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "N" thru_hole circle
		(at 32 44.8)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "N" thru_hole circle
		(at 32 48)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "NB" thru_hole circle
		(at 32 28.8)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "P" thru_hole circle
		(at 22.4 44.8)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "P" thru_hole circle
		(at 22.4 48)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "P1" thru_hole circle
		(at 9.6 28.8)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "P1" thru_hole circle
		(at 9.6 32)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "T1" thru_hole circle
		(at 22.4 0)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "T2" thru_hole circle
		(at 12.8 0)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "U" thru_hole circle
		(at 0 32)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "U" thru_hole circle
		(at 0 35.2)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "V" thru_hole circle
		(at 0 16)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "V" thru_hole circle
		(at 0 19.2)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "W" thru_hole rect
		(at 0 0)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "W" thru_hole circle
		(at 0 3.2)
		(size 2 2)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
			"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
			"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
			"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
			"In29.Cu" "In30.Cu"
		)
		(name "MH")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -5.79498 24) (xy -5.814344 23.573572) (xy -5.872277 23.150654) (xy -5.968301 22.734727) (xy -6.101626 22.329215)
				(xy -6.271156 21.937455) (xy -6.475494 21.562673) (xy -6.712959 21.207952) (xy -6.981595 20.876214)
				(xy -7.279192 20.570188) (xy -7.6033 20.292394) (xy -7.951252 20.045117) (xy -8.320183 19.830394)
				(xy -8.707056 19.649992) (xy -9.108688 19.505396) (xy -9.521771 19.397796) (xy -9.942907 19.328077)
				(xy -10.368628 19.296814) (xy -10.795431 19.304264) (xy -11.219801 19.350366) (xy -11.638247 19.434739)
				(xy -12.047324 19.55669) (xy -12.443665 19.715215) (xy -12.824006 19.909009) (xy -13.185219 20.136477)
				(xy -13.524329 20.395746) (xy -13.838545 20.684682) (xy -14.12528 21.000907) (xy -14.382176 21.341819)
				(xy -14.607116 21.704611) (xy -14.79825 22.086296) (xy -14.954004 22.483733) (xy -15.073096 22.893652)
				(xy -15.154546 23.312676) (xy -15.197684 23.737359) (xy -15.202154 24.164203) (xy -15.16792 24.589695)
				(xy -15.095263 25.010334) (xy -14.984781 25.422656) (xy -14.837385 25.823269) (xy -14.654286 26.208873)
				(xy -14.436993 26.576296) (xy -14.187293 26.922513) (xy -13.907243 27.244674) (xy -13.599147 27.540127)
				(xy -13.265541 27.806441) (xy -12.909172 28.041423) (xy -12.532972 28.24314) (xy -12.140038 28.409931)
				(xy -11.733605 28.540422) (xy -11.317018 28.63354) (xy -10.893706 28.688519) (xy -10.467153 28.704905)
				(xy -10.040871 28.682565) (xy -9.618367 28.621681) (xy -9.203121 28.522756) (xy -8.798549 28.386602)
				(xy -8.407983 28.214342) (xy -8.034636 28.007392) (xy -7.681582 27.767457) (xy -7.351727 27.496511)
				(xy -7.047786 27.196785) (xy -6.772261 26.870745) (xy -6.52742 26.521076) (xy -6.315278 26.150655)
				(xy -6.137581 25.762532) (xy -5.995793 25.3599) (xy -5.891079 24.946076) (xy -5.824302 24.524464)
				(xy -5.796012 24.098535)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
			"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
			"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
			"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
			"In29.Cu" "In30.Cu"
		)
		(name "MH")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 47.20502 24) (xy 47.185656 23.573572) (xy 47.127723 23.150654) (xy 47.031699 22.734727) (xy 46.898374 22.329215)
				(xy 46.728844 21.937455) (xy 46.524506 21.562673) (xy 46.287041 21.207952) (xy 46.018405 20.876214)
				(xy 45.720808 20.570188) (xy 45.3967 20.292394) (xy 45.048748 20.045117) (xy 44.679817 19.830394)
				(xy 44.292944 19.649992) (xy 43.891312 19.505396) (xy 43.478229 19.397796) (xy 43.057093 19.328077)
				(xy 42.631372 19.296814) (xy 42.204569 19.304264) (xy 41.780199 19.350366) (xy 41.361753 19.434739)
				(xy 40.952676 19.55669) (xy 40.556335 19.715215) (xy 40.175994 19.909009) (xy 39.814781 20.136477)
				(xy 39.475671 20.395746) (xy 39.161455 20.684682) (xy 38.87472 21.000907) (xy 38.617824 21.341819)
				(xy 38.392884 21.704611) (xy 38.20175 22.086296) (xy 38.045996 22.483733) (xy 37.926904 22.893652)
				(xy 37.845454 23.312676) (xy 37.802316 23.737359) (xy 37.797846 24.164203) (xy 37.83208 24.589695)
				(xy 37.904737 25.010334) (xy 38.015219 25.422656) (xy 38.162615 25.823269) (xy 38.345714 26.208873)
				(xy 38.563007 26.576296) (xy 38.812707 26.922513) (xy 39.092757 27.244674) (xy 39.400853 27.540127)
				(xy 39.734459 27.806441) (xy 40.090828 28.041423) (xy 40.467028 28.24314) (xy 40.859962 28.409931)
				(xy 41.266395 28.540422) (xy 41.682982 28.63354) (xy 42.106294 28.688519) (xy 42.532847 28.704905)
				(xy 42.959129 28.682565) (xy 43.381633 28.621681) (xy 43.796879 28.522756) (xy 44.201451 28.386602)
				(xy 44.592017 28.214342) (xy 44.965364 28.007392) (xy 45.318418 27.767457) (xy 45.648273 27.496511)
				(xy 45.952214 27.196785) (xy 46.227739 26.870745) (xy 46.47258 26.521076) (xy 46.684722 26.150655)
				(xy 46.862419 25.762532) (xy 47.004207 25.3599) (xy 47.108921 24.946076) (xy 47.175698 24.524464)
				(xy 47.203988 24.098535)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Transistor_Power_Module.3dshapes/ST_ACEPACK-2-CIB.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
