(footprint "ST_SDIP-25L"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "25-lead TH, SDIP-25L, https://www.st.com/resource/en/datasheet/stgips20k60.pdf")
	(tags "igbt diode module")
	(property "Reference" "REF**"
		(at 0 -2.6 0)
		(layer "F.SilkS")
	)
	(property "Value" "ST_SDIP-25L"
		(at 22.85 12.615 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 22.6 10.8 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 2.35 0)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 5.95 0)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 8.3 0)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 10.65 0)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 14.25 0)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 16.6 0)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 20.2 0)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 22.55 0)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole circle
		(at 24.9 0)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 28.5 0)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole circle
		(at 30.85 0)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at 34.45 0)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole circle
		(at 36.8 0)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "15" thru_hole circle
		(at 39.15 0)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "16" thru_hole circle
		(at 41.5 0)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "17" thru_hole circle
		(at 41.45 25.23)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "18" thru_hole circle
		(at 36.75 25.23)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "19" thru_hole circle
		(at 32.05 25.23)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "20" thru_hole circle
		(at 27.35 25.23)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 20.85 25.23)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "22" thru_hole circle
		(at 14.35 25.23)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "23" thru_hole circle
		(at 9.65 25.23)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "24" thru_hole circle
		(at 4.95 25.23)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "25" thru_hole circle
		(at 0.25 25.23)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
			"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
			"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
			"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
			"In29.Cu" "In30.Cu"
		)
		(name "MH")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 4.454773 11.77) (xy 4.435736 11.418487) (xy 4.378847 11.071085) (xy 4.284771 10.73186) (xy 4.15461 10.404779)
				(xy 3.989885 10.093668) (xy 3.792524 9.802167) (xy 3.564836 9.533686) (xy 3.309483 9.291366) (xy 3.029454 9.07804)
				(xy 2.728023 8.896206) (xy 2.408718 8.747989) (xy 2.075273 8.635124) (xy 1.731589 8.558932) (xy 1.381686 8.520302)
				(xy 1.029658 8.519688) (xy 0.679623 8.557096) (xy 0.335675 8.632088) (xy 0.001838 8.743789) (xy -0.317983 8.89089)
				(xy -0.620046 9.071671) (xy -0.900818 9.284017) (xy -1.157015 9.525445) (xy -1.385639 9.79313) (xy -1.584016 10.08394)
				(xy -1.749826 10.394473) (xy -1.881128 10.721098) (xy -1.976388 11.059993) (xy -2.034489 11.407194)
				(xy -2.054753 11.758639) (xy -2.036943 12.110216) (xy -1.981267 12.457814) (xy -1.888376 12.797366)
				(xy -1.759357 13.124899) (xy -1.595719 13.436583) (xy -1.399377 13.728771) (xy -1.172627 13.998045)
				(xy -0.918122 14.241256) (xy -0.638839 14.455557) (xy -0.338045 14.638443) (xy -0.019259 14.787773)
				(xy 0.31379 14.901801) (xy 0.657206 14.979193) (xy 1.006971 15.019044) (xy 1.358995 15.020887) (xy 1.709159 14.984701)
				(xy 2.053366 14.91091) (xy 2.387591 14.800375) (xy 2.707923 14.654391) (xy 3.010616 14.474666) (xy 3.292128 14.263301)
				(xy 3.549166 14.022769) (xy 3.778723 13.755884) (xy 3.978114 13.465768) (xy 4.145007 13.155815)
				(xy 4.277448 12.82965) (xy 4.37389 12.49109) (xy 4.433203 12.144094) (xy 4.454694 11.792722)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
			"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
			"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
			"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
			"In29.Cu" "In30.Cu"
		)
		(name "MH")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 43.754773 11.77) (xy 43.735736 11.418487) (xy 43.678847 11.071085) (xy 43.584771 10.73186) (xy 43.45461 10.404779)
				(xy 43.289885 10.093668) (xy 43.092524 9.802167) (xy 42.864836 9.533686) (xy 42.609483 9.291366)
				(xy 42.329454 9.07804) (xy 42.028023 8.896206) (xy 41.708718 8.747989) (xy 41.375273 8.635124) (xy 41.031589 8.558932)
				(xy 40.681686 8.520302) (xy 40.329658 8.519688) (xy 39.979623 8.557096) (xy 39.635675 8.632088)
				(xy 39.301838 8.743789) (xy 38.982017 8.89089) (xy 38.679954 9.071671) (xy 38.399182 9.284017) (xy 38.142985 9.525445)
				(xy 37.914361 9.79313) (xy 37.715984 10.08394) (xy 37.550174 10.394473) (xy 37.418872 10.721098)
				(xy 37.323612 11.059993) (xy 37.265511 11.407194) (xy 37.245247 11.758639) (xy 37.263057 12.110216)
				(xy 37.318733 12.457814) (xy 37.411624 12.797366) (xy 37.540643 13.124899) (xy 37.704281 13.436583)
				(xy 37.900623 13.728771) (xy 38.127373 13.998045) (xy 38.381878 14.241256) (xy 38.661161 14.455557)
				(xy 38.961955 14.638443) (xy 39.280741 14.787773) (xy 39.61379 14.901801) (xy 39.957206 14.979193)
				(xy 40.306971 15.019044) (xy 40.658995 15.020887) (xy 41.009159 14.984701) (xy 41.353366 14.91091)
				(xy 41.687591 14.800375) (xy 42.007923 14.654391) (xy 42.310616 14.474666) (xy 42.592128 14.263301)
				(xy 42.849166 14.022769) (xy 43.078723 13.755884) (xy 43.278114 13.465768) (xy 43.445007 13.155815)
				(xy 43.577448 12.82965) (xy 43.67389 12.49109) (xy 43.733203 12.144094) (xy 43.754694 11.792722)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Transistor_Power_Module.3dshapes/ST_SDIP-25L.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
