(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "14529"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 19.05 0)
		)
		(property "Value" "14529"
			(at -7.62 -21.59 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.alldatasheet.com/datasheet-pdf/pdf/97272/HITACHI/HD14529B.html"
			(at 0 0 0)
		)
		(property "Description" "Dual 4 to 1 Multiplexer"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS MUX MUX4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "14529_1_0"
			(pin input line
				(at -12.7 15.24 0)
				(length 5.08)
				(name "X0")
				(number "2")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "X1")
				(number "3")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "X2")
				(number "4")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "X3")
				(number "5")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "Y0")
				(number "14")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "Y1")
				(number "13")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "Y2")
				(number "12")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "Y3")
				(number "11")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "A")
				(number "6")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "B")
				(number "7")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 5.08)
				(name "STX")
				(number "1")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 5.08)
				(name "STY")
				(number "15")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 5.08)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin tri_state line
				(at 12.7 15.24 180)
				(length 5.08)
				(name "Z")
				(number "9")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "W")
				(number "10")
			)
		)
		(symbol "14529_1_1")
		(embedded_fonts no)
	)
	(symbol "4001"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "4001"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/cd40/cd4000bms-01bms-02bms-25bms.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad Nor 2 inputs"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Nor2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?14*"
			(at 0 0 0)
		)
		(symbol "4001_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "2")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "3")
			)
		)
		(symbol "4001_1_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "3")
			)
		)
		(symbol "4001_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "6")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "4")
			)
		)
		(symbol "4001_2_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "4")
			)
		)
		(symbol "4001_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "8")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "9")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "10")
			)
		)
		(symbol "4001_3_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "8")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "10")
			)
		)
		(symbol "4001_4_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "12")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "13")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "11")
			)
		)
		(symbol "4001_4_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "12")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "13")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "11")
			)
		)
		(symbol "4001_5_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "VSS")
				(number "7")
			)
		)
		(symbol "4001_5_1")
		(embedded_fonts no)
	)
	(symbol "4002"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "4002"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/cd40/cd4000bms-01bms-02bms-25bms.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual  4 input NOR gate"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Nor4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?14*"
			(at 0 0 0)
		)
		(symbol "4002_1_1"
			(pin input line
				(at -7.62 3.81 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin input line
				(at -7.62 1.27 0)
				(length 4.826)
				(name "~")
				(number "3")
			)
			(pin input line
				(at -7.62 -1.27 0)
				(length 4.826)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -7.62 -3.81 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "1")
			)
		)
		(symbol "4002_1_2"
			(pin input inverted
				(at -7.62 3.81 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin input inverted
				(at -7.62 1.27 0)
				(length 3.81)
				(name "~")
				(number "3")
			)
			(pin input inverted
				(at -7.62 -1.27 0)
				(length 3.81)
				(name "~")
				(number "4")
			)
			(pin input inverted
				(at -7.62 -3.81 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "1")
			)
		)
		(symbol "4002_2_1"
			(pin input line
				(at -7.62 3.81 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin input line
				(at -7.62 1.27 0)
				(length 4.826)
				(name "~")
				(number "10")
			)
			(pin input line
				(at -7.62 -1.27 0)
				(length 4.826)
				(name "~")
				(number "11")
			)
			(pin input line
				(at -7.62 -3.81 0)
				(length 3.81)
				(name "~")
				(number "12")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "13")
			)
		)
		(symbol "4002_2_2"
			(pin input inverted
				(at -7.62 3.81 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin input inverted
				(at -7.62 1.27 0)
				(length 3.81)
				(name "~")
				(number "10")
			)
			(pin input inverted
				(at -7.62 -1.27 0)
				(length 3.81)
				(name "~")
				(number "11")
			)
			(pin input inverted
				(at -7.62 -3.81 0)
				(length 3.81)
				(name "~")
				(number "12")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "13")
			)
		)
		(symbol "4002_3_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "VSS")
				(number "7")
			)
		)
		(symbol "4002_3_1")
		(embedded_fonts no)
	)
	(symbol "4009"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "4009"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.sycelectronica.com.ar/semiconductores/CD4009.pdf"
			(at 0 0 0)
		)
		(property "Description" "Hex Buffer Inverter"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS INV BUFFER high sink, VCC and VDD sep. VDD>VI>VCC!"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "4009_1_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "3")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "2")
			)
		)
		(symbol "4009_2_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "4")
			)
		)
		(symbol "4009_3_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "7")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "4009_4_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "10")
			)
		)
		(symbol "4009_5_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "11")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "12")
			)
		)
		(symbol "4009_6_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "14")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "15")
			)
		)
		(symbol "4009_7_0"
			(pin power_in line
				(at -2.54 12.7 270)
				(length 5.08)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "1")
			)
		)
		(symbol "4009_7_1")
		(embedded_fonts no)
	)
	(symbol "4010"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "4010"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/cd4010b-q1.pdf"
			(at 0 0 0)
		)
		(property "Description" "Hex Buffer"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS BUFFER high sink, VCC and VDD sep. VDD>VI>VCC!"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "4010_1_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "3")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "2")
			)
		)
		(symbol "4010_2_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "4")
			)
		)
		(symbol "4010_3_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "7")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "4010_4_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "10")
			)
		)
		(symbol "4010_5_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "11")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "12")
			)
		)
		(symbol "4010_6_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "14")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "15")
			)
		)
		(symbol "4010_7_0"
			(pin power_in line
				(at -2.54 12.7 270)
				(length 5.08)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "1")
			)
		)
		(symbol "4010_7_1")
		(embedded_fonts no)
	)
	(symbol "40106"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "40106"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/HEF40106B.pdf"
			(at 0 0 0)
		)
		(property "Description" "Hex Schmitt trigger inverter"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?14*"
			(at 0 0 0)
		)
		(symbol "40106_1_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "2")
			)
		)
		(symbol "40106_2_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "3")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "4")
			)
		)
		(symbol "40106_3_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "40106_4_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "40106_5_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "11")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "10")
			)
		)
		(symbol "40106_6_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "13")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "12")
			)
		)
		(symbol "40106_7_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "VSS")
				(number "7")
			)
		)
		(symbol "40106_7_1")
		(embedded_fonts no)
	)
	(symbol "4011"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "4011"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/cd40/cd4011bms-12bms-23bms.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad Nand 2 inputs"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Nand2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?14*"
			(at 0 0 0)
		)
		(symbol "4011_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "3")
			)
		)
		(symbol "4011_1_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "1")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "3")
			)
		)
		(symbol "4011_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "6")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "4")
			)
		)
		(symbol "4011_2_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "5")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "4")
			)
		)
		(symbol "4011_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "8")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "10")
			)
		)
		(symbol "4011_3_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "8")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "9")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "10")
			)
		)
		(symbol "4011_4_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "12")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "13")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "11")
			)
		)
		(symbol "4011_4_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "12")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "13")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "11")
			)
		)
		(symbol "4011_5_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "VSS")
				(number "7")
			)
		)
		(symbol "4011_5_1")
		(embedded_fonts no)
	)
	(symbol "4012"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "4012"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/cd40/cd4011bms-12bms-23bms.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual 4 inputs Nand"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Nand4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?14*"
			(at 0 0 0)
		)
		(symbol "4012_1_1"
			(pin input line
				(at -7.62 3.81 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin input line
				(at -7.62 1.27 0)
				(length 3.81)
				(name "~")
				(number "3")
			)
			(pin input line
				(at -7.62 -1.27 0)
				(length 3.81)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -7.62 -3.81 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "1")
			)
		)
		(symbol "4012_1_2"
			(pin input inverted
				(at -7.62 3.81 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin input inverted
				(at -7.62 1.27 0)
				(length 4.826)
				(name "~")
				(number "3")
			)
			(pin input inverted
				(at -7.62 -1.27 0)
				(length 4.826)
				(name "~")
				(number "4")
			)
			(pin input inverted
				(at -7.62 -3.81 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "1")
			)
		)
		(symbol "4012_2_1"
			(pin input line
				(at -7.62 3.81 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin input line
				(at -7.62 1.27 0)
				(length 3.81)
				(name "~")
				(number "10")
			)
			(pin input line
				(at -7.62 -1.27 0)
				(length 3.81)
				(name "~")
				(number "11")
			)
			(pin input line
				(at -7.62 -3.81 0)
				(length 3.81)
				(name "~")
				(number "12")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "13")
			)
		)
		(symbol "4012_2_2"
			(pin input inverted
				(at -7.62 3.81 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin input inverted
				(at -7.62 1.27 0)
				(length 4.826)
				(name "~")
				(number "10")
			)
			(pin input inverted
				(at -7.62 -1.27 0)
				(length 4.826)
				(name "~")
				(number "11")
			)
			(pin input inverted
				(at -7.62 -3.81 0)
				(length 3.81)
				(name "~")
				(number "12")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "13")
			)
		)
		(symbol "4012_3_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "VSS")
				(number "7")
			)
		)
		(symbol "4012_3_1")
		(embedded_fonts no)
	)
	(symbol "4013"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "4013"
			(at -7.62 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/MC14013B-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Dual D  FlipFlop, Set & reset"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS DFF"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "4013_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin input clock
				(at -7.62 0 0)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin input line
				(at 0 7.62 270)
				(length 2.54)
				(name "S")
				(number "6")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "R")
				(number "4")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "Q")
				(number "1")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~{Q}")
				(number "2")
			)
		)
		(symbol "4013_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "D")
				(number "9")
			)
			(pin input clock
				(at -7.62 0 0)
				(length 2.54)
				(name "C")
				(number "11")
			)
			(pin input line
				(at 0 7.62 270)
				(length 2.54)
				(name "S")
				(number "8")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "R")
				(number "10")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "Q")
				(number "13")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~{Q}")
				(number "12")
			)
		)
		(symbol "4013_3_0"
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
		)
		(symbol "4013_3_1")
		(embedded_fonts no)
	)
	(symbol "4016"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "4016"
			(at -7.62 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/cd4016b.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad Analog Switches"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS SWITCH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?14*"
			(at 0 0 0)
		)
		(symbol "4016_1_0"
			(pin passive line
				(at -7.62 0 0)
				(length 5.08)
				(name "~")
				(number "1")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "~")
				(number "13")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 5.08)
				(name "~")
				(number "2")
			)
		)
		(symbol "4016_2_0"
			(pin passive line
				(at -7.62 0 0)
				(length 5.08)
				(name "~")
				(number "4")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 5.08)
				(name "~")
				(number "3")
			)
		)
		(symbol "4016_3_0"
			(pin passive line
				(at -7.62 0 0)
				(length 5.08)
				(name "~")
				(number "8")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 5.08)
				(name "~")
				(number "9")
			)
		)
		(symbol "4016_4_0"
			(pin passive line
				(at -7.62 0 0)
				(length 5.08)
				(name "~")
				(number "11")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 5.08)
				(name "~")
				(number "10")
			)
		)
		(symbol "4016_5_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "VSS")
				(number "7")
			)
		)
		(symbol "4016_5_1")
		(embedded_fonts no)
	)
	(symbol "4017"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "4017"
			(at -7.62 -19.05 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/cd40/cd4017bms-22bms.pdf"
			(at 0 0 0)
		)
		(property "Description" "Johnson Counter ( 10 outputs )"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "CNT CNT10"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "4017_1_0"
			(pin input clock
				(at -12.7 12.7 0)
				(length 5.08)
				(name "CLK")
				(number "14")
			)
			(pin input inverted
				(at -12.7 10.16 0)
				(length 5.08)
				(name "CKEN")
				(number "13")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "Reset")
				(number "15")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 5.08)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "Q0")
				(number "3")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "Q1")
				(number "2")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Q2")
				(number "4")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q3")
				(number "7")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "Q4")
				(number "10")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "Q5")
				(number "1")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "Q6")
				(number "5")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "Q7")
				(number "6")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "Q8")
				(number "9")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 5.08)
				(name "Q9")
				(number "11")
			)
			(pin output line
				(at 12.7 -15.24 180)
				(length 5.08)
				(name "Cout")
				(number "12")
			)
		)
		(symbol "4017_1_1")
		(embedded_fonts no)
	)
	(symbol "4020"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "4020"
			(at -7.62 -19.05 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/cd40/cd4020bms-24bms-40bms.pdf"
			(at 0 0 0)
		)
		(property "Description" "Binary counter 14 stages (asynchronous)"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS CNT CNT14"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "4020_1_0"
			(pin input inverted_clock
				(at -12.7 12.7 0)
				(length 5.08)
				(name "CLK")
				(number "10")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "Reset")
				(number "11")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 5.08)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "Q0")
				(number "9")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "Q3")
				(number "7")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Q4")
				(number "5")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q5")
				(number "4")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "Q6")
				(number "6")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "Q7")
				(number "13")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "Q8")
				(number "12")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "Q9")
				(number "14")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "Q10")
				(number "15")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 5.08)
				(name "Q11")
				(number "1")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 5.08)
				(name "Q12")
				(number "2")
			)
			(pin output line
				(at 12.7 -15.24 180)
				(length 5.08)
				(name "Q13")
				(number "3")
			)
		)
		(symbol "4020_1_1")
		(embedded_fonts no)
	)
	(symbol "4021"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 19.05 0)
		)
		(property "Value" "4021"
			(at 3.81 19.05 0)
		)
		(property "Footprint" ""
			(at 0 3.81 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/HEF4021B.pdf"
			(at 0 3.81 0)
		)
		(property "Description" "8-bit static shift register"
			(at 0 0 0)
		)
		(property "ki_keywords" "shift register SR PISO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm* SOIC*5.3x10.2mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "4021_0_1")
		(symbol "4021_1_1"
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "CP")
				(number "10")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "PL")
				(number "9")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "DS")
				(number "11")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "D0")
				(number "7")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "D1")
				(number "6")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "D2")
				(number "5")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "D3")
				(number "4")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "D4")
				(number "13")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "D5")
				(number "14")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "D6")
				(number "15")
			)
			(pin input line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "D7")
				(number "1")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "VSS")
				(number "8")
			)
			(pin output line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "Q5")
				(number "2")
			)
			(pin output line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "Q6")
				(number "12")
			)
			(pin output line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "Q7")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4022"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "4022"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/cd40/cd4017bms-22bms.pdf"
			(at 0 0 0)
		)
		(property "Description" "Johnson Counter (8 states)"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS CNT CNT8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "4022_1_0"
			(pin input clock
				(at -12.7 10.16 0)
				(length 5.08)
				(name "CLK")
				(number "14")
			)
			(pin input inverted
				(at -12.7 7.62 0)
				(length 5.08)
				(name "CKEN")
				(number "13")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "Reset")
				(number "15")
			)
			(pin no_connect line
				(at -12.7 -5.08 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -12.7 -7.62 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 5.08)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "Q0")
				(number "2")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Q1")
				(number "1")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q2")
				(number "3")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "Q3")
				(number "7")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "Q4")
				(number "11")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "Q5")
				(number "4")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "Q6")
				(number "5")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "Q7")
				(number "10")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 5.08)
				(name "Cout")
				(number "12")
			)
		)
		(symbol "4022_1_1")
		(embedded_fonts no)
	)
	(symbol "4023"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "4023"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/cd40/cd4011bms-12bms-23bms.pdf"
			(at 0 0 0)
		)
		(property "Description" "Triple Nand 3 inputs"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Nand3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?14*"
			(at 0 0 0)
		)
		(symbol "4023_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "8")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "9")
			)
		)
		(symbol "4023_1_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "1")
			)
			(pin input inverted
				(at -7.62 0 0)
				(length 4.953)
				(name "~")
				(number "2")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "8")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "9")
			)
		)
		(symbol "4023_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "3")
			)
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "4023_2_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "3")
			)
			(pin input inverted
				(at -7.62 0 0)
				(length 4.953)
				(name "~")
				(number "4")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "4023_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "11")
			)
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "12")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "13")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "10")
			)
		)
		(symbol "4023_3_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "11")
			)
			(pin input inverted
				(at -7.62 0 0)
				(length 4.953)
				(name "~")
				(number "12")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "13")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "10")
			)
		)
		(symbol "4023_4_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "VSS")
				(number "7")
			)
		)
		(symbol "4023_4_1")
		(embedded_fonts no)
	)
	(symbol "4025"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "4025"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/cd40/cd4000bms-01bms-02bms-25bms.pdf"
			(at 0 0 0)
		)
		(property "Description" "Triple Nor 3 inputs"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Nor3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?14*"
			(at 0 0 0)
		)
		(symbol "4025_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -7.62 0 0)
				(length 4.953)
				(name "~")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "8")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "9")
			)
		)
		(symbol "4025_1_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin input inverted
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "8")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "9")
			)
		)
		(symbol "4025_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "3")
			)
			(pin input line
				(at -7.62 0 0)
				(length 4.953)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "5")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "4025_2_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "3")
			)
			(pin input inverted
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "4")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "4025_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "11")
			)
			(pin input line
				(at -7.62 0 0)
				(length 4.953)
				(name "~")
				(number "12")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "13")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "10")
			)
		)
		(symbol "4025_3_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "11")
			)
			(pin input inverted
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "12")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "13")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "10")
			)
		)
		(symbol "4025_4_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "VSS")
				(number "7")
			)
		)
		(symbol "4025_4_1")
		(embedded_fonts no)
	)
	(symbol "4027"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "4027"
			(at -7.62 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/cd40/cd4027bms.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual JK FlipFlop, set & reset"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS JK JKFF"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "4027_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "J")
				(number "6")
			)
			(pin input clock
				(at -7.62 0 0)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "K")
				(number "5")
			)
			(pin input line
				(at 0 7.62 270)
				(length 2.54)
				(name "S")
				(number "7")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "R")
				(number "4")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "Q")
				(number "1")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~{Q}")
				(number "2")
			)
		)
		(symbol "4027_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "J")
				(number "10")
			)
			(pin input clock
				(at -7.62 0 0)
				(length 2.54)
				(name "C")
				(number "13")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "K")
				(number "11")
			)
			(pin input line
				(at 0 7.62 270)
				(length 2.54)
				(name "S")
				(number "9")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "R")
				(number "12")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "Q")
				(number "15")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~{Q}")
				(number "14")
			)
		)
		(symbol "4027_3_0"
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "8")
			)
		)
		(symbol "4027_3_1")
		(embedded_fonts no)
	)
	(symbol "4028"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "4028"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/cd40/cd4028bms.pdf"
			(at 0 0 0)
		)
		(property "Description" "Decoder 4 to 10 lines"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS DECOD DECOD10"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "4028_1_0"
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "A")
				(number "10")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "B")
				(number "13")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "C")
				(number "12")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "D")
				(number "11")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 5.08)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "S0")
				(number "3")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "S1")
				(number "14")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "S2")
				(number "2")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "S3")
				(number "15")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "S4")
				(number "1")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "S5")
				(number "6")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "S6")
				(number "7")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "S7")
				(number "4")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 5.08)
				(name "S8")
				(number "9")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 5.08)
				(name "S9")
				(number "5")
			)
		)
		(symbol "4028_1_1")
		(embedded_fonts no)
	)
	(symbol "4029"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "4029"
			(at -7.62 -19.05 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/cd40/cd4029bms.pdf"
			(at 0 0 0)
		)
		(property "Description" "Up/Down Counter"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS COUNTER"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "4029_1_0"
			(pin input inverted_clock
				(at -12.7 12.7 0)
				(length 5.08)
				(name "CK")
				(number "15")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "J1")
				(number "4")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "J2")
				(number "12")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "J3")
				(number "13")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "J4")
				(number "3")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "Cin")
				(number "5")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 5.08)
				(name "PE")
				(number "1")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 5.08)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "Q1")
				(number "6")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "Q2")
				(number "11")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Q3")
				(number "14")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q4")
				(number "2")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "U/D")
				(number "10")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "B/D")
				(number "9")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "Cout")
				(number "7")
			)
		)
		(symbol "4029_1_1")
		(embedded_fonts no)
	)
	(symbol "4040"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "4040"
			(at -7.62 -19.05 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/cd40/cd4020bms-24bms-40bms.pdf"
			(at 0 0 0)
		)
		(property "Description" "Binary Counter 12 stages (Asynchronous)"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS CNT CNT12"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "4040_1_0"
			(pin input inverted_clock
				(at -12.7 12.7 0)
				(length 5.08)
				(name "CLK")
				(number "10")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "Reset")
				(number "11")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 5.08)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "Q0")
				(number "9")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "Q1")
				(number "7")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Q2")
				(number "6")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q3")
				(number "5")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "Q4")
				(number "3")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "Q5")
				(number "2")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "Q6")
				(number "4")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "Q7")
				(number "13")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "Q8")
				(number "12")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 5.08)
				(name "Q9")
				(number "14")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 5.08)
				(name "Q10")
				(number "15")
			)
			(pin output line
				(at 12.7 -15.24 180)
				(length 5.08)
				(name "Q11")
				(number "1")
			)
		)
		(symbol "4040_1_1")
		(embedded_fonts no)
	)
	(symbol "4046"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "4046"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/HEF4046B.pdf"
			(at 0 0 0)
		)
		(property "Description" "Phase Comp & VCO"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS PLL"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "4046_1_0"
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "RefIn")
				(number "3")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "SigIn")
				(number "14")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "C1")
				(number "6")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "C2")
				(number "7")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "R1")
				(number "11")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "R2")
				(number "12")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "Inh")
				(number "5")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 5.08)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "FOUT")
				(number "4")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "PC1")
				(number "2")
			)
			(pin tri_state line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "PC2")
				(number "13")
			)
			(pin input line
				(at 12.7 0 180)
				(length 5.08)
				(name "VCOin")
				(number "9")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "PCP")
				(number "1")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "SFout")
				(number "10")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 5.08)
				(name "ZOUT")
				(number "15")
			)
		)
		(symbol "4046_1_1")
		(embedded_fonts no)
	)
	(symbol "4047"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 24.13 0)
		)
		(property "Value" "4047"
			(at -7.62 -24.13 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/cd4047b.pdf"
			(at 0 0 0)
		)
		(property "Description" "Monostable/Astable Multivibrator"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS monostable astable multivibrator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "4047_1_0"
			(pin input line
				(at -15.24 17.78 0)
				(length 5.08)
				(name "ASTABLE")
				(number "5")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 5.08)
				(name "~{ASTABLE}")
				(number "4")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 5.08)
				(name "-TRIGGER")
				(number "6")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 5.08)
				(name "+TRIGGER")
				(number "8")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "RETRIGGER")
				(number "12")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "EXT_RESET")
				(number "9")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 5.08)
				(name "R")
				(number "2")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 5.08)
				(name "C")
				(number "1")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 5.08)
				(name "RC_COMMON")
				(number "3")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 5.08)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 5.08)
				(name "VSS")
				(number "7")
			)
			(pin output line
				(at 15.24 17.78 180)
				(length 5.08)
				(name "OSC_OUT")
				(number "13")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 5.08)
				(name "Q")
				(number "10")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "~{Q}")
				(number "11")
			)
		)
		(symbol "4047_1_1")
		(embedded_fonts no)
	)
	(symbol "4049"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "4049"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/intersil/documents/cd40/cd4049ubms.pdf"
			(at 0 0 0)
		)
		(property "Description" "Hex Buffer Inverter"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS BUFFER"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "4049_1_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "3")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "2")
			)
		)
		(symbol "4049_2_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "4")
			)
		)
		(symbol "4049_3_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "7")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "4049_4_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "10")
			)
		)
		(symbol "4049_5_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "11")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "12")
			)
		)
		(symbol "4049_6_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "14")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "15")
			)
		)
		(symbol "4049_7_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
		)
		(symbol "4049_7_1")
		(embedded_fonts no)
	)
	(symbol "4050"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "4050"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/intersil/documents/cd40/cd4050bms.pdf"
			(at 0 0 0)
		)
		(property "Description" "Hex Buffer"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS BUFFER"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "4050_1_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "3")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "2")
			)
		)
		(symbol "4050_2_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "4")
			)
		)
		(symbol "4050_3_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "7")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "4050_4_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "10")
			)
		)
		(symbol "4050_5_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "11")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "12")
			)
		)
		(symbol "4050_6_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "14")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "15")
			)
		)
		(symbol "4050_7_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
		)
		(symbol "4050_7_1")
		(embedded_fonts no)
	)
	(symbol "4051"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 19.05 0)
		)
		(property "Value" "4051"
			(at -7.62 -19.05 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/cd40/cd4051bms-52bms-53bms.pdf"
			(at 0 0 0)
		)
		(property "Description" "Analog Multiplexer 8 to 1 lins"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS MUX MUX8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "4051_1_0"
			(pin passive line
				(at -12.7 15.24 0)
				(length 5.08)
				(name "X0")
				(number "13")
			)
			(pin passive line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "X1")
				(number "14")
			)
			(pin passive line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "X2")
				(number "15")
			)
			(pin passive line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "X3")
				(number "12")
			)
			(pin passive line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "X4")
				(number "1")
			)
			(pin passive line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "X5")
				(number "5")
			)
			(pin passive line
				(at -12.7 0 0)
				(length 5.08)
				(name "X6")
				(number "2")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "X7")
				(number "4")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "Inh")
				(number "6")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "A")
				(number "11")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "B")
				(number "10")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 5.08)
				(name "C")
				(number "9")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 5.08)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -22.86 90)
				(length 5.08)
				(name "VEE")
				(number "7")
			)
			(pin passive line
				(at 12.7 15.24 180)
				(length 5.08)
				(name "X")
				(number "3")
			)
		)
		(symbol "4051_1_1")
		(embedded_fonts no)
	)
	(symbol "4052"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 19.05 0)
		)
		(property "Value" "4052"
			(at -7.62 -19.05 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/cd40/cd4051bms-52bms-53bms.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Analog Multiplexer 4 to 1 line"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS MUX MUX4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "4052_1_0"
			(pin passive line
				(at -12.7 15.24 0)
				(length 5.08)
				(name "X0")
				(number "12")
			)
			(pin passive line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "X1")
				(number "14")
			)
			(pin passive line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "X2")
				(number "15")
			)
			(pin passive line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "X3")
				(number "11")
			)
			(pin passive line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "Y0")
				(number "1")
			)
			(pin passive line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "Y1")
				(number "5")
			)
			(pin passive line
				(at -12.7 0 0)
				(length 5.08)
				(name "Y2")
				(number "2")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "Y3")
				(number "4")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "Inh")
				(number "6")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "A")
				(number "10")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 5.08)
				(name "B")
				(number "9")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 5.08)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -22.86 90)
				(length 5.08)
				(name "VEE")
				(number "7")
			)
			(pin passive line
				(at 12.7 15.24 180)
				(length 5.08)
				(name "X")
				(number "13")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Y")
				(number "3")
			)
		)
		(symbol "4052_1_1")
		(embedded_fonts no)
	)
	(symbol "4053"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 19.05 0)
		)
		(property "Value" "4053"
			(at -7.62 -19.05 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/cd40/cd4051bms-52bms-53bms.pdf"
			(at 0 0 0)
		)
		(property "Description" "Triple analog Multiplexer 2 to 1 line"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS MUX MUX2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "4053_1_0"
			(pin passive line
				(at -12.7 15.24 0)
				(length 5.08)
				(name "X0")
				(number "12")
			)
			(pin passive line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "X1")
				(number "13")
			)
			(pin passive line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "Y0")
				(number "2")
			)
			(pin passive line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "Y1")
				(number "1")
			)
			(pin passive line
				(at -12.7 0 0)
				(length 5.08)
				(name "Z0")
				(number "5")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "Z1")
				(number "3")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "Inh")
				(number "6")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "A")
				(number "11")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "B")
				(number "10")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 5.08)
				(name "C")
				(number "9")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 5.08)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -22.86 90)
				(length 5.08)
				(name "VEE")
				(number "7")
			)
			(pin passive line
				(at 12.7 15.24 180)
				(length 5.08)
				(name "X")
				(number "14")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Y")
				(number "15")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 5.08)
				(name "Z")
				(number "4")
			)
		)
		(symbol "4053_1_1")
		(embedded_fonts no)
	)
	(symbol "4056"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "4056"
			(at -7.62 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/cd4056b.pdf"
			(at 0 0 0)
		)
		(property "Description" "BCD to 7-Segment Decoder/Driver, Strobed-Latch Function"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS LCD 7-segment decoder driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "4056_1_0"
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "2^0")
				(number "5")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "2^1")
				(number "3")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "2^2")
				(number "2")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "2^3")
				(number "4")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "STROBE")
				(number "1")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "FREQ.IN")
				(number "6")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 5.08)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 5.08)
				(name "VEE")
				(number "7")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "a")
				(number "9")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "b")
				(number "10")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "c")
				(number "11")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "d")
				(number "12")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "e")
				(number "13")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "f")
				(number "15")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "g")
				(number "14")
			)
		)
		(symbol "4056_1_1")
		(embedded_fonts no)
	)
	(symbol "4060"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 16.51 0)
		)
		(property "Value" "4060"
			(at 6.35 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/m74hc4060.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "Binary counter (14-stages) and oscillator"
			(at 0 0 0)
		)
		(property "ki_keywords" "binary counter oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*7.62* TSSOP*16*4.4x5* SOIC*16*3.9x9.9*"
			(at 0 0 0)
		)
		(symbol "4060_1_0"
			(pin input inverted_clock
				(at -12.7 12.7 0)
				(length 5.08)
				(name "~{Φ0}")
				(number "9")
			)
			(pin input clock
				(at -12.7 10.16 0)
				(length 5.08)
				(name "Φ0")
				(number "10")
			)
			(pin input inverted_clock
				(at -12.7 7.62 0)
				(length 5.08)
				(name "~{Φ1}")
				(number "11")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "CLR")
				(number "12")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 5.08)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "Q4")
				(number "7")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "Q5")
				(number "5")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Q6")
				(number "4")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q7")
				(number "6")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "Q8")
				(number "14")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "Q9")
				(number "13")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "Q10")
				(number "15")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "Q12")
				(number "1")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 5.08)
				(name "Q13")
				(number "2")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 5.08)
				(name "Q14")
				(number "3")
			)
		)
		(symbol "4060_1_1")
		(embedded_fonts no)
	)
	(symbol "4069"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "4069"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/cd40/cd4069ubms.pdf"
			(at 0 0 0)
		)
		(property "Description" "Hex inverter"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS NOT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?14*"
			(at 0 0 0)
		)
		(symbol "4069_1_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "2")
			)
		)
		(symbol "4069_2_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "3")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "4")
			)
		)
		(symbol "4069_3_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "4069_4_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "4069_5_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "11")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "10")
			)
		)
		(symbol "4069_6_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "13")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "12")
			)
		)
		(symbol "4069_7_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "VSS")
				(number "7")
			)
		)
		(symbol "4069_7_1")
		(embedded_fonts no)
	)
	(symbol "4070"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "4070"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/cd40/cd4070bms-77bms.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad Xor 2 inputs"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS XOR2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?14*"
			(at 0 0 0)
		)
		(symbol "4070_1_0"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.445)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.445)
				(name "~")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "3")
			)
		)
		(symbol "4070_1_1")
		(symbol "4070_2_0"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.445)
				(name "~")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.445)
				(name "~")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "4")
			)
		)
		(symbol "4070_2_1")
		(symbol "4070_3_0"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.445)
				(name "~")
				(number "8")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.445)
				(name "~")
				(number "9")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "10")
			)
		)
		(symbol "4070_3_1")
		(symbol "4070_4_0"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.445)
				(name "~")
				(number "12")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.445)
				(name "~")
				(number "13")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "11")
			)
		)
		(symbol "4070_4_1")
		(symbol "4070_5_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "VSS")
				(number "7")
			)
		)
		(symbol "4070_5_1")
		(embedded_fonts no)
	)
	(symbol "4071"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "4071"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/cd40/cd4071bms-72bms-75bms.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad Or 2 inputs"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS OR2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?14*"
			(at 0 0 0)
		)
		(symbol "4071_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "3")
			)
		)
		(symbol "4071_1_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "3")
			)
		)
		(symbol "4071_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "4")
			)
		)
		(symbol "4071_2_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "6")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "4")
			)
		)
		(symbol "4071_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "8")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "9")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "10")
			)
		)
		(symbol "4071_3_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "8")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "10")
			)
		)
		(symbol "4071_4_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "12")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "13")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "11")
			)
		)
		(symbol "4071_4_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "12")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "13")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "11")
			)
		)
		(symbol "4071_5_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "VSS")
				(number "7")
			)
		)
		(symbol "4071_5_1")
		(embedded_fonts no)
	)
	(symbol "4072"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "4072"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/cd40/cd4071bms-72bms-75bms.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual 4 input OR gate"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS OR4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?14*"
			(at 0 0 0)
		)
		(symbol "4072_1_1"
			(pin input line
				(at -7.62 3.81 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin input line
				(at -7.62 1.27 0)
				(length 4.826)
				(name "~")
				(number "3")
			)
			(pin input line
				(at -7.62 -1.27 0)
				(length 4.826)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -7.62 -3.81 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "1")
			)
		)
		(symbol "4072_1_2"
			(pin input inverted
				(at -7.62 3.81 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin input inverted
				(at -7.62 1.27 0)
				(length 3.81)
				(name "~")
				(number "3")
			)
			(pin input inverted
				(at -7.62 -1.27 0)
				(length 3.81)
				(name "~")
				(number "4")
			)
			(pin input inverted
				(at -7.62 -3.81 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "1")
			)
		)
		(symbol "4072_2_1"
			(pin input line
				(at -7.62 3.81 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin input line
				(at -7.62 1.27 0)
				(length 4.826)
				(name "~")
				(number "10")
			)
			(pin input line
				(at -7.62 -1.27 0)
				(length 4.826)
				(name "~")
				(number "11")
			)
			(pin input line
				(at -7.62 -3.81 0)
				(length 3.81)
				(name "~")
				(number "12")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "13")
			)
		)
		(symbol "4072_2_2"
			(pin input inverted
				(at -7.62 3.81 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin input inverted
				(at -7.62 1.27 0)
				(length 3.81)
				(name "~")
				(number "10")
			)
			(pin input inverted
				(at -7.62 -1.27 0)
				(length 3.81)
				(name "~")
				(number "11")
			)
			(pin input inverted
				(at -7.62 -3.81 0)
				(length 3.81)
				(name "~")
				(number "12")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "13")
			)
		)
		(symbol "4072_3_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "VSS")
				(number "7")
			)
		)
		(symbol "4072_3_1")
		(embedded_fonts no)
	)
	(symbol "4073"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "4073"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/cd40/cd4073bms-81bms-82bms.pdf"
			(at 0 0 0)
		)
		(property "Description" "Triple And 3 inputs"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS And3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?14*"
			(at 0 0 0)
		)
		(symbol "4073_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "8")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "9")
			)
		)
		(symbol "4073_1_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "1")
			)
			(pin input inverted
				(at -7.62 0 0)
				(length 4.953)
				(name "~")
				(number "2")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "8")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "9")
			)
		)
		(symbol "4073_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "3")
			)
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "4073_2_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "3")
			)
			(pin input inverted
				(at -7.62 0 0)
				(length 4.953)
				(name "~")
				(number "4")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "5")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "4073_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "11")
			)
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "12")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "13")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "10")
			)
		)
		(symbol "4073_3_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "11")
			)
			(pin input inverted
				(at -7.62 0 0)
				(length 4.953)
				(name "~")
				(number "12")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "13")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "10")
			)
		)
		(symbol "4073_4_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "VSS")
				(number "7")
			)
		)
		(symbol "4073_4_1")
		(embedded_fonts no)
	)
	(symbol "4075"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "4075"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/cd40/cd4071bms-72bms-75bms.pdf"
			(at 0 0 0)
		)
		(property "Description" "Triple Or 3 inputs"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Or3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?14*"
			(at 0 0 0)
		)
		(symbol "4075_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -7.62 0 0)
				(length 4.953)
				(name "~")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "8")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "9")
			)
		)
		(symbol "4075_1_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin input inverted
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "8")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "9")
			)
		)
		(symbol "4075_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "3")
			)
			(pin input line
				(at -7.62 0 0)
				(length 4.953)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "4075_2_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "3")
			)
			(pin input inverted
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "4")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "4075_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "11")
			)
			(pin input line
				(at -7.62 0 0)
				(length 4.953)
				(name "~")
				(number "12")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "13")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "10")
			)
		)
		(symbol "4075_3_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "11")
			)
			(pin input inverted
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "12")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "13")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "10")
			)
		)
		(symbol "4075_4_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "VSS")
				(number "7")
			)
		)
		(symbol "4075_4_1")
		(embedded_fonts no)
	)
	(symbol "4077"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "4077"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/cd40/cd4076bms.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad Xnor 2 inputs"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS XOR XNOR XNOR2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?14*"
			(at 0 0 0)
		)
		(symbol "4077_1_0"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.445)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.445)
				(name "~")
				(number "2")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "3")
			)
		)
		(symbol "4077_1_1")
		(symbol "4077_2_0"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.445)
				(name "~")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.445)
				(name "~")
				(number "6")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "4")
			)
		)
		(symbol "4077_2_1")
		(symbol "4077_3_0"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.445)
				(name "~")
				(number "8")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.445)
				(name "~")
				(number "9")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "10")
			)
		)
		(symbol "4077_3_1")
		(symbol "4077_4_0"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.445)
				(name "~")
				(number "12")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.445)
				(name "~")
				(number "13")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "11")
			)
		)
		(symbol "4077_4_1")
		(symbol "4077_5_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "VSS")
				(number "7")
			)
		)
		(symbol "4077_5_1")
		(embedded_fonts no)
	)
	(symbol "4081"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "4081"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/cd40/cd4073bms-81bms-82bms.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad And 2 inputs"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS And2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?14*"
			(at 0 0 0)
		)
		(symbol "4081_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "3")
			)
		)
		(symbol "4081_1_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "1")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "2")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "3")
			)
		)
		(symbol "4081_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "4")
			)
		)
		(symbol "4081_2_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "5")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "6")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "4")
			)
		)
		(symbol "4081_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "8")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "10")
			)
		)
		(symbol "4081_3_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "8")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "9")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "10")
			)
		)
		(symbol "4081_4_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "12")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "13")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "11")
			)
		)
		(symbol "4081_4_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "12")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "13")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "11")
			)
		)
		(symbol "4081_5_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "VSS")
				(number "7")
			)
		)
		(symbol "4081_5_1")
		(embedded_fonts no)
	)
	(symbol "4098"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 11.43 0)
		)
		(property "Value" "4098"
			(at -5.08 -11.43 0)
		)
		(property "Footprint" ""
			(at -5.08 11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/cd4098b.pdf"
			(at -5.08 11.43 0)
		)
		(property "Description" "Dual Monostable Multivibrator"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS monostable multivibrator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "4098_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "Cx1")
				(number "1")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "Rx1_Cx1")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{Reset1}")
				(number "3")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "+TR1")
				(number "4")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "-TR1")
				(number "5")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "Q1")
				(number "6")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{Q1}")
				(number "7")
			)
		)
		(symbol "4098_2_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "Cx2")
				(number "15")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "Rx2_Cx2")
				(number "14")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{Reset2}")
				(number "13")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "+TR2")
				(number "12")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "-TR2")
				(number "11")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "Q2")
				(number "10")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{Q2}")
				(number "9")
			)
		)
		(symbol "4098_3_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4504"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 21.59 0)
		)
		(property "Value" "4504"
			(at 6.35 21.59 0)
		)
		(property "Footprint" ""
			(at 0 -33.02 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/cd4504b.pdf"
			(at -16.51 -8.89 0)
		)
		(property "Description" "CMOS Hex Voltage-Level Shifter for TTL-to-CMOS or CMOS-to-CMOS, DIP-16/SOIC-16/TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Level-shifter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "4504_0_1")
		(symbol "4504_1_1"
			(pin input line
				(at -11.43 12.7 0)
				(length 2.54)
				(name "Ain")
				(number "3")
			)
			(pin input line
				(at -11.43 7.62 0)
				(length 2.54)
				(name "Bin")
				(number "5")
			)
			(pin input line
				(at -11.43 2.54 0)
				(length 2.54)
				(name "Cin")
				(number "7")
			)
			(pin input line
				(at -11.43 -2.54 0)
				(length 2.54)
				(name "Din")
				(number "9")
			)
			(pin input line
				(at -11.43 -7.62 0)
				(length 2.54)
				(name "Ein")
				(number "11")
			)
			(pin input line
				(at -11.43 -12.7 0)
				(length 2.54)
				(name "Fin")
				(number "14")
			)
			(pin input line
				(at -11.43 -17.78 0)
				(length 2.54)
				(name "Select")
				(number "13")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin output line
				(at 11.43 12.7 180)
				(length 2.54)
				(name "Aout")
				(number "2")
			)
			(pin output line
				(at 11.43 7.62 180)
				(length 2.54)
				(name "Bout")
				(number "4")
			)
			(pin output line
				(at 11.43 2.54 180)
				(length 2.54)
				(name "Cout")
				(number "6")
			)
			(pin output line
				(at 11.43 -2.54 180)
				(length 2.54)
				(name "Dout")
				(number "10")
			)
			(pin output line
				(at 11.43 -7.62 180)
				(length 2.54)
				(name "Eout")
				(number "12")
			)
			(pin output line
				(at 11.43 -12.7 180)
				(length 2.54)
				(name "Fout")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4510"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "4510"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheets/150/109581_DS.pdf"
			(at 0 0 0)
		)
		(property "Description" "4 bits programmable counter"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS CNT CNT4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "4510_1_0"
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "A1")
				(number "4")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "A2")
				(number "12")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "A3")
				(number "13")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "A4")
				(number "3")
			)
			(pin input inverted
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "CI")
				(number "5")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "U/D")
				(number "10")
			)
			(pin input clock
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "CLK")
				(number "15")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "PE")
				(number "1")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "RST")
				(number "9")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 5.08)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "Q1")
				(number "6")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Q2")
				(number "11")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q3")
				(number "14")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "Q4")
				(number "2")
			)
			(pin output inverted
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "CO")
				(number "7")
			)
		)
		(symbol "4510_1_1")
		(embedded_fonts no)
	)
	(symbol "4518"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "4518"
			(at -7.62 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/cd45/cd4518bms-20bms.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual BCD Up-Counter"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "4518_1_0"
			(pin input clock
				(at -12.7 0 0)
				(length 5.08)
				(name "CK")
				(number "1")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "Reset")
				(number "7")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "Enable")
				(number "2")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "Q1")
				(number "3")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "Q2")
				(number "4")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "Q3")
				(number "5")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "Q4")
				(number "6")
			)
		)
		(symbol "4518_1_1")
		(symbol "4518_2_0"
			(pin input clock
				(at -12.7 0 0)
				(length 5.08)
				(name "CK")
				(number "9")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "Reset")
				(number "15")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "Enable")
				(number "10")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "Q1")
				(number "11")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "Q2")
				(number "12")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "Q3")
				(number "13")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "Q4")
				(number "14")
			)
		)
		(symbol "4518_2_1")
		(symbol "4518_3_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
		)
		(symbol "4518_3_1")
		(embedded_fonts no)
	)
	(symbol "4520"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "4520"
			(at -7.62 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/cd45/cd4518bms-20bms.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Binary Up-Counter"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "4520_1_0"
			(pin input clock
				(at -12.7 0 0)
				(length 5.08)
				(name "CK")
				(number "1")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "Reset")
				(number "7")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "Enable")
				(number "2")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "Q1")
				(number "3")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "Q2")
				(number "4")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "Q3")
				(number "5")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "Q4")
				(number "6")
			)
		)
		(symbol "4520_1_1")
		(symbol "4520_2_0"
			(pin input clock
				(at -12.7 0 0)
				(length 5.08)
				(name "CK")
				(number "9")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "Reset")
				(number "15")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "Enable")
				(number "10")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "Q1")
				(number "11")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "Q2")
				(number "12")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "Q3")
				(number "13")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "Q4")
				(number "14")
			)
		)
		(symbol "4520_2_1")
		(symbol "4520_3_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
		)
		(symbol "4520_3_1")
		(embedded_fonts no)
	)
	(symbol "4538"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 11.43 0)
		)
		(property "Value" "4538"
			(at 0 -11.43 0)
		)
		(property "Footprint" ""
			(at 0 1.27 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/HEF4538B.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "Monostable"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "4538_1_0"
			(pin input clock
				(at -12.7 2.54 0)
				(length 5.08)
				(name "Clk+")
				(number "4")
			)
			(pin input inverted_clock
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "Clk-")
				(number "5")
			)
			(pin input inverted
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "R")
				(number "3")
			)
			(pin input line
				(at -5.08 15.24 270)
				(length 5.08)
				(name "Cx")
				(number "1")
			)
			(pin input line
				(at 5.08 15.24 270)
				(length 5.08)
				(name "RxCx")
				(number "2")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "Q")
				(number "6")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "~{Q}")
				(number "7")
			)
		)
		(symbol "4538_1_1")
		(symbol "4538_2_0"
			(pin input clock
				(at -12.7 2.54 0)
				(length 5.08)
				(name "Clk+")
				(number "12")
			)
			(pin input inverted_clock
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "Clk-")
				(number "11")
			)
			(pin input inverted
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "R")
				(number "13")
			)
			(pin input line
				(at -5.08 15.24 270)
				(length 5.08)
				(name "Cx")
				(number "15")
			)
			(pin input line
				(at 5.08 15.24 270)
				(length 5.08)
				(name "RxCx")
				(number "14")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "Q")
				(number "10")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "~{Q}")
				(number "9")
			)
		)
		(symbol "4538_2_1")
		(symbol "4538_3_0"
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
		)
		(symbol "4538_3_1")
		(embedded_fonts no)
	)
	(symbol "4543"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "4543"
			(at -7.62 -11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/cd4543b.pdf"
			(at 0 0 0)
		)
		(property "Description" "BCD to 7-segment latch/decoder/driver"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS 7-segment latch decoder driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "4543_1_0"
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "D0")
				(number "5")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "D1")
				(number "3")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "D2")
				(number "2")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "D3")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "~{LE}")
				(number "1")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "BL")
				(number "7")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "PH")
				(number "6")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Qa")
				(number "9")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Qb")
				(number "10")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "Qc")
				(number "11")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "Qd")
				(number "12")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "Qe")
				(number "13")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "Qf")
				(number "15")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "Qg")
				(number "14")
			)
		)
		(symbol "4543_1_1")
		(embedded_fonts no)
	)
	(symbol "CD4033B"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 17.78 0)
		)
		(property "Value" "CD4033B"
			(at 7.62 17.78 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/cd4033b.pdf"
			(at 0 0 0)
		)
		(property "Description" "20V, CMOS Decade Counter/Divider, 7 Segment Decoder, Ripple Blanking, Lamp Test, 100mW/Output, DIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "schmitt triggered"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "CD4033B_1_1"
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "RIPPLE_BLANKING_IN")
				(number "3")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "CLOCK")
				(number "1")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "CLOCK_INHIBIT")
				(number "2")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "RESET")
				(number "15")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "LAMP_TEST")
				(number "14")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "V_{DD}")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "V_{SS}")
				(number "8")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "RIPPLE_BLANKING_OUT")
				(number "4")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "CARRY_OUT")
				(number "5")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "a")
				(number "10")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "b")
				(number "12")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "c")
				(number "13")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "d")
				(number "9")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "e")
				(number "11")
			)
			(pin output line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "f")
				(number "6")
			)
			(pin output line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "g")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HEF4093B"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "HEF4093B"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/HEF4093B.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad 2-Input NAND Schmitt Trigger, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "NAND2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "HEF4093B_1_0")
		(symbol "HEF4093B_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "3")
			)
		)
		(symbol "HEF4093B_1_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "1")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "3")
			)
		)
		(symbol "HEF4093B_2_0")
		(symbol "HEF4093B_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "6")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "4")
			)
		)
		(symbol "HEF4093B_2_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "5")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "4")
			)
		)
		(symbol "HEF4093B_3_0")
		(symbol "HEF4093B_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "8")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "10")
			)
		)
		(symbol "HEF4093B_3_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "8")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "9")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "10")
			)
		)
		(symbol "HEF4093B_4_0")
		(symbol "HEF4093B_4_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "12")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "13")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "11")
			)
		)
		(symbol "HEF4093B_4_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "12")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "13")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "11")
			)
		)
		(symbol "HEF4093B_5_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
		)
		(symbol "HEF4093B_5_1")
		(embedded_fonts no)
	)
	(symbol "HEF4094B"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.858 17.018 0)
		)
		(property "Value" "HEF4094B"
			(at 6.858 16.764 0)
		)
		(property "Footprint" ""
			(at 0 3.81 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/HEF4094B.pdf"
			(at 0.254 -30.48 0)
		)
		(property "Description" "8-bit serial-in parallel-out shift register, 3..15V"
			(at 0.254 -28.448 0)
		)
		(property "ki_keywords" "shift-store store logic shift-and-store 8-stage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*16*3.9x9.9mm*P1.27mm* TSSOP*16*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "HEF4094B_1_0"
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "OE")
				(number "15")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "V_{DD}")
				(number "16")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "V_{SS}")
				(number "8")
			)
			(pin output line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "QS1")
				(number "9")
			)
			(pin output line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "QS2")
				(number "10")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "QP1")
				(number "5")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "QP2")
				(number "6")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "QP3")
				(number "7")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "QP4")
				(number "14")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "QP5")
				(number "13")
			)
			(pin output line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "QP6")
				(number "12")
			)
			(pin output line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "QP7")
				(number "11")
			)
		)
		(symbol "HEF4094B_1_1"
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "D")
				(number "2")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "CP")
				(number "3")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "STR")
				(number "1")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "QP0")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "14528"
		(extends "4538")
		(property "Reference" "U"
			(at 0 11.43 0)
		)
		(property "Value" "14528"
			(at 0 -11.43 0)
		)
		(property "Footprint" ""
			(at 0 1.27 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC14528B-D.PDF"
			(at 0 1.27 0)
		)
		(property "Description" "Monostable"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
	)
	(symbol "14538"
		(extends "4538")
		(property "Reference" "U"
			(at 0 11.43 0)
		)
		(property "Value" "14538"
			(at 0 -11.43 0)
		)
		(property "Footprint" ""
			(at 0 1.27 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC14538B-D.PDF"
			(at 0 1.27 0)
		)
		(property "Description" "Monostable"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
	)
	(symbol "4066"
		(extends "4016")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "4066"
			(at -7.62 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/cd4066b.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad Analog Switches"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS SWITCH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?14*"
			(at 0 0 0)
		)
	)
	(symbol "4528"
		(extends "4538")
		(property "Reference" "U"
			(at 0 11.43 0)
		)
		(property "Value" "4528"
			(at 0 -11.43 0)
		)
		(property "Footprint" ""
			(at 0 1.27 0)
		)
		(property "Datasheet" "http://datasheet.octopart.com/CD4528BCN-Fairchild-datasheet-143503.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "Monostable"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
	)
)
