(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "4001"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "4001"
			(at 3.81 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4001_0_0"
			(text "1"
				(at 1.524 0 0)
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "Vdd")
				(number "14")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "Vss")
				(number "7")
			)
		)
		(symbol "4001_0_1")
		(symbol "4001_1_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "3")
			)
		)
		(symbol "4001_2_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "5")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "6")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "4")
			)
		)
		(symbol "4001_3_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "8")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "9")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "10")
			)
		)
		(symbol "4001_4_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "12")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "13")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4002"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 7.62 0)
		)
		(property "Value" "4002"
			(at 5.08 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4002_0_0"
			(text "1"
				(at 0 0 0)
			)
		)
		(symbol "4002_0_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 3.81)
				(name "Vdd")
				(number "14")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 3.81)
				(name "Vss")
				(number "7")
			)
		)
		(symbol "4002_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "3")
			)
			(pin input line
				(at -12.7 0 0)
				(length 7.62)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "12")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "1")
			)
		)
		(symbol "4002_2_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 7.62)
				(name "~")
				(number "9")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "10")
			)
			(pin input line
				(at -12.7 0 0)
				(length 7.62)
				(name "~")
				(number "11")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "12")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4006"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 8.89 0)
		)
		(property "Value" "4006"
			(at 6.35 -15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4006_0_0")
		(symbol "4006_0_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "Vdd")
				(number "14")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 3.81)
				(name "Vss")
				(number "7")
			)
		)
		(symbol "4006_1_1"
			(pin input clock
				(at -10.16 5.08 0)
				(length 3.81)
				(name "~{CP}")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 3.81)
				(name "DA")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 3.81)
				(name "DC")
				(number "4")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 3.81)
				(name "DB")
				(number "5")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 3.81)
				(name "DD")
				(number "6")
			)
			(pin output line
				(at 10.16 0 180)
				(length 3.81)
				(name "Q3A")
				(number "13")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 3.81)
				(name "Q3B")
				(number "11")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 3.81)
				(name "Q4C")
				(number "12")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 3.81)
				(name "Q3B")
				(number "10")
			)
			(pin output line
				(at 10.16 -10.16 180)
				(length 3.81)
				(name "Q3D")
				(number "8")
			)
			(pin output line
				(at 10.16 -12.7 180)
				(length 3.81)
				(name "Q4D")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4008"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 12.7 0)
		)
		(property "Value" "4008"
			(at 7.62 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4008_0_0"
			(text "P"
				(at 0 6.35 0)
			)
			(text "Q"
				(at 0 -3.81 0)
			)
		)
		(symbol "4008_0_1")
		(symbol "4008_1_1"
			(pin input line
				(at -10.16 10.16 0)
				(length 3.81)
				(name "A0")
				(number "7")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 3.81)
				(name "A1")
				(number "5")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 3.81)
				(name "A2")
				(number "3")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 3.81)
				(name "A3")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 3.81)
				(name "B0")
				(number "6")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 3.81)
				(name "B1")
				(number "4")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 3.81)
				(name "B2")
				(number "2")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 3.81)
				(name "B3")
				(number "15")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 3.81)
				(name "Cin")
				(number "9")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 3.81)
				(name "Vdd")
				(number "16")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 3.81)
				(name "Vss")
				(number "8")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 3.81)
				(name "S0")
				(number "10")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 3.81)
				(name "S1")
				(number "11")
			)
			(pin output line
				(at 10.16 0 180)
				(length 3.81)
				(name "S2")
				(number "12")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 3.81)
				(name "S3")
				(number "13")
			)
			(pin output line
				(at 10.16 -10.16 180)
				(length 3.81)
				(name "Cout")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4009"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 6.35 0)
		)
		(property "Value" "4009"
			(at 5.08 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4009_0_0")
		(symbol "4009_0_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "Vdd")
				(number "16")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "Vss")
				(number "8")
			)
			(pin power_in line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "Vcc")
				(number "1")
			)
		)
		(symbol "4009_1_1"
			(pin input line
				(at -12.7 0 0)
				(length 7.62)
				(name "~")
				(number "3")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "2")
			)
		)
		(symbol "4009_2_1"
			(pin input line
				(at -12.7 0 0)
				(length 7.62)
				(name "~")
				(number "5")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "4")
			)
		)
		(symbol "4009_3_1"
			(pin input line
				(at -12.7 0 0)
				(length 7.62)
				(name "~")
				(number "7")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "6")
			)
		)
		(symbol "4009_4_1"
			(pin input line
				(at -12.7 0 0)
				(length 7.62)
				(name "~")
				(number "9")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "10")
			)
		)
		(symbol "4009_5_1"
			(pin input line
				(at -12.7 0 0)
				(length 7.62)
				(name "~")
				(number "11")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "12")
			)
		)
		(symbol "4009_6_1"
			(pin input line
				(at -12.7 0 0)
				(length 7.62)
				(name "~")
				(number "14")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4010"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 6.35 0)
		)
		(property "Value" "4010"
			(at 5.08 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4010_0_0")
		(symbol "4010_0_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "Vdd")
				(number "16")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "Vss")
				(number "8")
			)
			(pin power_in line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "Vcc")
				(number "1")
			)
		)
		(symbol "4010_1_1"
			(pin input line
				(at -12.7 0 0)
				(length 7.62)
				(name "~")
				(number "3")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "2")
			)
		)
		(symbol "4010_2_1"
			(pin input line
				(at -12.7 0 0)
				(length 7.62)
				(name "~")
				(number "5")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "4")
			)
		)
		(symbol "4010_3_1"
			(pin input line
				(at -12.7 0 0)
				(length 7.62)
				(name "~")
				(number "7")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "6")
			)
		)
		(symbol "4010_4_1"
			(pin input line
				(at -12.7 0 0)
				(length 7.62)
				(name "~")
				(number "9")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "10")
			)
		)
		(symbol "4010_5_1"
			(pin input line
				(at -12.7 0 0)
				(length 7.62)
				(name "~")
				(number "11")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "12")
			)
		)
		(symbol "4010_6_1"
			(pin input line
				(at -12.7 0 0)
				(length 7.62)
				(name "~")
				(number "14")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "40104"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 8.89 0)
		)
		(property "Value" "40104"
			(at 6.35 -15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "40104_0_0")
		(symbol "40104_0_1")
		(symbol "40104_1_1"
			(pin input line
				(at -10.16 12.7 0)
				(length 3.81)
				(name "S0")
				(number "9")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 3.81)
				(name "S1")
				(number "10")
			)
			(pin input clock
				(at -10.16 7.62 0)
				(length 3.81)
				(name "CK")
				(number "11")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 3.81)
				(name "EN")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 3.81)
				(name "SRin")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 3.81)
				(name "D0")
				(number "3")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 3.81)
				(name "D1")
				(number "4")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 3.81)
				(name "D2")
				(number "5")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 3.81)
				(name "D3")
				(number "6")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 3.81)
				(name "SLin")
				(number "7")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "Vdd")
				(number "16")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 3.81)
				(name "Vss")
				(number "8")
			)
			(pin output line
				(at 10.16 0 180)
				(length 3.81)
				(name "Q0")
				(number "15")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 3.81)
				(name "Q1")
				(number "14")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 3.81)
				(name "Q2")
				(number "13")
			)
			(pin output line
				(at 10.16 -10.16 180)
				(length 3.81)
				(name "Q3")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "40106"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 5.08 0)
		)
		(property "Value" "40106"
			(at 1.27 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "40106_0_0")
		(symbol "40106_0_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 3.81)
				(name "Vdd")
				(number "14")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 3.81)
				(name "Vss")
				(number "7")
			)
		)
		(symbol "40106_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "2")
			)
		)
		(symbol "40106_2_1"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "3")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "4")
			)
		)
		(symbol "40106_3_1"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "40106_4_1"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "40106_5_1"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "11")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "10")
			)
		)
		(symbol "40106_6_1"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "13")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4011"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "4011"
			(at 5.08 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4011_0_0"
			(text "&"
				(at 0.508 0 0)
			)
		)
		(symbol "4011_0_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "Vdd")
				(number "14")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "Vss")
				(number "7")
			)
		)
		(symbol "4011_1_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "3")
			)
		)
		(symbol "4011_2_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "5")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "6")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "4")
			)
		)
		(symbol "4011_3_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "8")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "9")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "10")
			)
		)
		(symbol "4011_4_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "12")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "13")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "40110"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 13.97 0)
		)
		(property "Value" "40110"
			(at 7.62 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "40110_0_1")
		(symbol "40110_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 3.81)
				(name "LE")
				(number "6")
			)
			(pin input clock
				(at -10.16 2.54 0)
				(length 3.81)
				(name "CKd")
				(number "7")
			)
			(pin input clock
				(at -10.16 0 0)
				(length 3.81)
				(name "CKu")
				(number "9")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 3.81)
				(name "CLR")
				(number "5")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 3.81)
				(name "~{TE}")
				(number "4")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 3.81)
				(name "Vdd")
				(number "16")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 3.81)
				(name "Vss")
				(number "8")
			)
			(pin output line
				(at 10.16 10.16 180)
				(length 3.81)
				(name "Qa")
				(number "1")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 3.81)
				(name "Qb")
				(number "15")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 3.81)
				(name "Qc")
				(number "14")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 3.81)
				(name "Qd")
				(number "13")
			)
			(pin output line
				(at 10.16 0 180)
				(length 3.81)
				(name "Qe")
				(number "12")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 3.81)
				(name "Qf")
				(number "3")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 3.81)
				(name "Qg")
				(number "2")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 3.81)
				(name "B")
				(number "11")
			)
			(pin output line
				(at 10.16 -10.16 180)
				(length 3.81)
				(name "C")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4012"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 7.62 0)
		)
		(property "Value" "4012"
			(at 5.08 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4012_0_0"
			(text "&"
				(at 0 0 0)
			)
		)
		(symbol "4012_0_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 3.81)
				(name "Vdd")
				(number "14")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 3.81)
				(name "Vss")
				(number "7")
			)
		)
		(symbol "4012_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "3")
			)
			(pin input line
				(at -12.7 0 0)
				(length 7.62)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "12")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "1")
			)
		)
		(symbol "4012_2_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 7.62)
				(name "~")
				(number "9")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "10")
			)
			(pin input line
				(at -12.7 0 0)
				(length 7.62)
				(name "~")
				(number "11")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "12")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4013"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 8.89 0)
		)
		(property "Value" "4013"
			(at 7.62 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4013_0_0"
			(pin power_in line
				(at 0 10.16 270)
				(length 3.81)
				(name "Vdd")
				(number "14")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 3.81)
				(name "Vss")
				(number "7")
			)
		)
		(symbol "4013_0_1")
		(symbol "4013_1_1"
			(pin input line
				(at -15.24 5.08 0)
				(length 7.62)
				(name "D")
				(number "5")
			)
			(pin input clock
				(at -15.24 2.54 0)
				(length 7.62)
				(name "Cp")
				(number "3")
			)
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "R")
				(number "4")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 7.62)
				(name "S")
				(number "6")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 7.62)
				(name "Q")
				(number "1")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 7.62)
				(name "~{Q}")
				(number "2")
			)
		)
		(symbol "4013_2_1"
			(pin input line
				(at -15.24 5.08 0)
				(length 7.62)
				(name "D")
				(number "9")
			)
			(pin input clock
				(at -15.24 2.54 0)
				(length 7.62)
				(name "Cp")
				(number "11")
			)
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "R")
				(number "10")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 7.62)
				(name "S")
				(number "8")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 7.62)
				(name "Q")
				(number "13")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 7.62)
				(name "~{Q}")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4014"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 11.43 0)
		)
		(property "Value" "4014"
			(at 7.62 -17.78 0)
		)
		(property "Footprint" ""
			(at 0 3.81 0)
		)
		(property "Datasheet" ""
			(at 0 3.81 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4014_0_1")
		(symbol "4014_1_1"
			(pin input line
				(at -10.16 12.7 0)
				(length 3.81)
				(name "PL")
				(number "9")
			)
			(pin input clock
				(at -10.16 10.16 0)
				(length 3.81)
				(name "CP")
				(number "10")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 3.81)
				(name "DS")
				(number "11")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 3.81)
				(name "P0")
				(number "7")
			)
			(pin input line
				(at -10.16 0 0)
				(length 3.81)
				(name "P1")
				(number "6")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 3.81)
				(name "P2")
				(number "5")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 3.81)
				(name "P3")
				(number "4")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 3.81)
				(name "P4")
				(number "13")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 3.81)
				(name "P5")
				(number "14")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 3.81)
				(name "P6")
				(number "15")
			)
			(pin input line
				(at -10.16 -15.24 0)
				(length 3.81)
				(name "P7")
				(number "1")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "Vdd")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "Vss")
				(number "8")
			)
			(pin output line
				(at 10.16 -10.16 180)
				(length 3.81)
				(name "Q5")
				(number "2")
			)
			(pin output line
				(at 10.16 -12.7 180)
				(length 3.81)
				(name "Q6")
				(number "12")
			)
			(pin output line
				(at 10.16 -15.24 180)
				(length 3.81)
				(name "Q7")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4015"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 7.62 0)
		)
		(property "Value" "4015"
			(at 6.35 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4015_0_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 3.81)
				(name "Vdd")
				(number "16")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 3.81)
				(name "Vss")
				(number "8")
			)
		)
		(symbol "4015_1_1"
			(pin input clock
				(at -10.16 5.08 0)
				(length 3.81)
				(name "CP")
				(number "9")
			)
			(pin input line
				(at -10.16 0 0)
				(length 3.81)
				(name "D")
				(number "7")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 3.81)
				(name "MR")
				(number "6")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 3.81)
				(name "Q1")
				(number "5")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 3.81)
				(name "Q2")
				(number "4")
			)
			(pin output line
				(at 10.16 0 180)
				(length 3.81)
				(name "Q3")
				(number "3")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 3.81)
				(name "Q4")
				(number "10")
			)
		)
		(symbol "4015_2_1"
			(pin input clock
				(at -10.16 5.08 0)
				(length 3.81)
				(name "CP")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 3.81)
				(name "D")
				(number "15")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 3.81)
				(name "MR")
				(number "14")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 3.81)
				(name "Q1")
				(number "13")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 3.81)
				(name "Q2")
				(number "12")
			)
			(pin output line
				(at 10.16 0 180)
				(length 3.81)
				(name "Q3")
				(number "11")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 3.81)
				(name "Q4")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4016"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 5.08 0)
		)
		(property "Value" "4016"
			(at 5.08 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4016_0_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vdd")
				(number "14")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "Vss")
				(number "7")
			)
		)
		(symbol "4016_1_1"
			(pin passive line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "I/O")
				(number "1")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "ON")
				(number "13")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 7.62)
				(name "O/I")
				(number "2")
			)
		)
		(symbol "4016_2_1"
			(pin passive line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "I/O")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "ON")
				(number "5")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 7.62)
				(name "O/I")
				(number "3")
			)
		)
		(symbol "4016_3_1"
			(pin passive line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "I/O")
				(number "8")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "ON")
				(number "6")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 7.62)
				(name "O/I")
				(number "9")
			)
		)
		(symbol "4016_4_1"
			(pin passive line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "I/O")
				(number "11")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "ON")
				(number "12")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 7.62)
				(name "O/I")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4017"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 17.78 0)
		)
		(property "Value" "4017"
			(at 10.16 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4017_0_0"
			(text "&"
				(at -2.032 11.43 0)
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "8")
			)
		)
		(symbol "4017_0_1")
		(symbol "4017_1_1"
			(pin input line
				(at -10.16 15.24 0)
				(length 3.81)
				(name "CP0")
				(number "14")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 3.81)
				(name "~{CP1}")
				(number "13")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 3.81)
				(name "MR")
				(number "15")
			)
			(pin output line
				(at 10.16 15.24 180)
				(length 3.81)
				(name "Q0")
				(number "3")
			)
			(pin output line
				(at 10.16 12.7 180)
				(length 3.81)
				(name "Q1")
				(number "2")
			)
			(pin output line
				(at 10.16 10.16 180)
				(length 3.81)
				(name "Q2")
				(number "4")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 3.81)
				(name "Q3")
				(number "7")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 3.81)
				(name "Q4")
				(number "10")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 3.81)
				(name "Q5")
				(number "1")
			)
			(pin output line
				(at 10.16 0 180)
				(length 3.81)
				(name "Q6")
				(number "5")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 3.81)
				(name "Q7")
				(number "6")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 3.81)
				(name "Q8")
				(number "9")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 3.81)
				(name "Q9")
				(number "11")
			)
			(pin output line
				(at 10.16 -12.7 180)
				(length 3.81)
				(name "Co")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "40174"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 7.62 0)
		)
		(property "Value" "40174"
			(at 7.62 -12.7 0)
		)
		(property "Footprint" ""
			(at 0 -1.27 0)
		)
		(property "Datasheet" ""
			(at 0 -1.27 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "40174_0_0"
			(pin input line
				(at -12.7 10.16 0)
				(length 7.62)
				(name "~{R}")
				(number "1")
			)
			(pin input clock
				(at -12.7 7.62 0)
				(length 7.62)
				(name "Ck")
				(number "9")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 5.08)
				(name "Vdd")
				(number "16")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 3.81)
				(name "Vss")
				(number "8")
			)
		)
		(symbol "40174_0_1")
		(symbol "40174_1_0"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "3")
			)
			(pin input line
				(at -12.7 0 0)
				(length 7.62)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "6")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 7.62)
				(name "~")
				(number "11")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 7.62)
				(name "~")
				(number "13")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 7.62)
				(name "~")
				(number "14")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "5")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 7.62)
				(name "~")
				(number "7")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 7.62)
				(name "~")
				(number "10")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 7.62)
				(name "~")
				(number "12")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 7.62)
				(name "~")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "40175"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 11.43 0)
		)
		(property "Value" "40175"
			(at 7.62 -15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "40175_0_1")
		(symbol "40175_1_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 7.62)
				(name "~{R}")
				(number "1")
			)
			(pin input clock
				(at -12.7 10.16 0)
				(length 7.62)
				(name "Ck")
				(number "9")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 7.62)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -12.7 0 0)
				(length 7.62)
				(name "~")
				(number "5")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 7.62)
				(name "~")
				(number "12")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 7.62)
				(name "~")
				(number "13")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 5.08)
				(name "Vdd")
				(number "16")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 3.81)
				(name "Vss")
				(number "8")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin output inverted
				(at 12.7 2.54 180)
				(length 7.62)
				(name "~")
				(number "3")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "7")
			)
			(pin output inverted
				(at 12.7 -2.54 180)
				(length 7.62)
				(name "~")
				(number "6")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 7.62)
				(name "~")
				(number "10")
			)
			(pin output inverted
				(at 12.7 -7.62 180)
				(length 7.62)
				(name "~")
				(number "11")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 7.62)
				(name "~")
				(number "15")
			)
			(pin output inverted
				(at 12.7 -12.7 180)
				(length 7.62)
				(name "~")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4018"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 15.24 0)
		)
		(property "Value" "4018"
			(at 5.08 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 2.54 0)
		)
		(property "Datasheet" ""
			(at 0 2.54 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4018_0_1")
		(symbol "4018_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 7.62)
				(name "MR")
				(number "15")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 7.62)
				(name "D")
				(number "1")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 7.62)
				(name "PL")
				(number "10")
			)
			(pin input clock
				(at -12.7 2.54 0)
				(length 7.62)
				(name "CP")
				(number "14")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "P0")
				(number "2")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 7.62)
				(name "P1")
				(number "3")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 7.62)
				(name "P2")
				(number "7")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 7.62)
				(name "P3")
				(number "9")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 7.62)
				(name "P4")
				(number "12")
			)
			(pin power_in line
				(at 0 16.51 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -16.51 90)
				(length 2.54)
				(name "VSS")
				(number "8")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 7.62)
				(name "~{Q0}")
				(number "5")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 7.62)
				(name "~{Q1}")
				(number "4")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 7.62)
				(name "~{Q2}")
				(number "6")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 7.62)
				(name "~{Q3}")
				(number "11")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 7.62)
				(name "~{Q4}")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4019"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.89 11.43 0)
		)
		(property "Value" "4019"
			(at 8.89 -15.24 0)
		)
		(property "Footprint" ""
			(at 0 1.27 0)
		)
		(property "Datasheet" ""
			(at 0 1.27 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4019_0_1"
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "Vdd")
				(number "16")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 3.81)
				(name "Vss")
				(number "8")
			)
		)
		(symbol "4019_1_1"
			(pin input line
				(at -10.16 12.7 0)
				(length 3.81)
				(name "SA")
				(number "9")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 3.81)
				(name "SB")
				(number "14")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 3.81)
				(name "A0")
				(number "6")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 3.81)
				(name "B0")
				(number "7")
			)
			(pin input line
				(at -10.16 0 0)
				(length 3.81)
				(name "A1")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 3.81)
				(name "B1")
				(number "5")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 3.81)
				(name "A2")
				(number "2")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 3.81)
				(name "B2")
				(number "3")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 3.81)
				(name "A3")
				(number "15")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 3.81)
				(name "B3")
				(number "1")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 3.81)
				(name "Q0")
				(number "10")
			)
			(pin output line
				(at 10.16 0 180)
				(length 3.81)
				(name "Q1")
				(number "11")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 3.81)
				(name "Q2")
				(number "12")
			)
			(pin output line
				(at 10.16 -10.16 180)
				(length 3.81)
				(name "Q3")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "40192"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 12.7 0)
		)
		(property "Value" "40192"
			(at 8.89 -19.05 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "40192_0_0"
			(text "1"
				(at 1.27 -7.62 0)
			)
			(text "2"
				(at 1.27 -10.16 0)
			)
			(text "4"
				(at 1.27 -12.7 0)
			)
			(text "8"
				(at 1.27 -15.24 0)
			)
		)
		(symbol "40192_0_1")
		(symbol "40192_1_1"
			(pin input line
				(at -12.7 8.89 0)
				(length 7.62)
				(name "MR")
				(number "14")
			)
			(pin input clock
				(at -12.7 5.08 0)
				(length 7.62)
				(name "UP")
				(number "5")
			)
			(pin input clock
				(at -12.7 1.27 0)
				(length 7.62)
				(name "DOWN")
				(number "4")
			)
			(pin input input_low
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "LOAD")
				(number "11")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 7.62)
				(name "P0")
				(number "15")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 7.62)
				(name "P1")
				(number "1")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 7.62)
				(name "P2")
				(number "10")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 7.62)
				(name "P3")
				(number "9")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "8")
			)
			(pin output output_low
				(at 12.7 3.81 180)
				(length 7.62)
				(name "CO")
				(number "12")
			)
			(pin output output_low
				(at 12.7 0 180)
				(length 7.62)
				(name "BO")
				(number "13")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 7.62)
				(name "Q0")
				(number "3")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 7.62)
				(name "Q1")
				(number "2")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 7.62)
				(name "Q2")
				(number "6")
			)
			(pin output line
				(at 12.7 -15.24 180)
				(length 7.62)
				(name "Q3")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "40193"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 12.7 0)
		)
		(property "Value" "40193"
			(at 8.89 -19.05 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "40193_0_0"
			(text "1"
				(at 1.27 -7.62 0)
			)
			(text "2"
				(at 1.27 -10.16 0)
			)
			(text "4"
				(at 1.27 -12.7 0)
			)
			(text "8"
				(at 1.27 -15.24 0)
			)
		)
		(symbol "40193_0_1")
		(symbol "40193_1_1"
			(pin input line
				(at -12.7 8.89 0)
				(length 7.62)
				(name "MR")
				(number "14")
			)
			(pin input clock
				(at -12.7 5.08 0)
				(length 7.62)
				(name "UP")
				(number "5")
			)
			(pin input clock
				(at -12.7 1.27 0)
				(length 7.62)
				(name "DOWN")
				(number "4")
			)
			(pin input input_low
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "LOAD")
				(number "11")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 7.62)
				(name "P0")
				(number "15")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 7.62)
				(name "P1")
				(number "1")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 7.62)
				(name "P2")
				(number "10")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 7.62)
				(name "P3")
				(number "9")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "8")
			)
			(pin output output_low
				(at 12.7 3.81 180)
				(length 7.62)
				(name "CO")
				(number "12")
			)
			(pin output output_low
				(at 12.7 0 180)
				(length 7.62)
				(name "BO")
				(number "13")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 7.62)
				(name "Q0")
				(number "3")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 7.62)
				(name "Q1")
				(number "2")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 7.62)
				(name "Q2")
				(number "6")
			)
			(pin output line
				(at 12.7 -15.24 180)
				(length 7.62)
				(name "Q3")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "40194"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 13.97 0)
		)
		(property "Value" "40194"
			(at 0 -15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "40194_0_0")
		(symbol "40194_0_1"
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "Vdd")
				(number "16")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 3.81)
				(name "Vss")
				(number "8")
			)
		)
		(symbol "40194_1_1"
			(pin input line
				(at -10.16 11.43 0)
				(length 3.81)
				(name "S0")
				(number "9")
			)
			(pin input line
				(at -10.16 8.89 0)
				(length 3.81)
				(name "S1")
				(number "10")
			)
			(pin input clock
				(at -10.16 6.35 0)
				(length 3.81)
				(name "CK")
				(number "11")
			)
			(pin input input_low
				(at -10.16 3.81 0)
				(length 3.81)
				(name "MR")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 3.81)
				(name "DSr")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 3.81)
				(name "D0")
				(number "3")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 3.81)
				(name "D1")
				(number "4")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 3.81)
				(name "D2")
				(number "5")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 3.81)
				(name "D3")
				(number "6")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 3.81)
				(name "DSl")
				(number "7")
			)
			(pin output line
				(at 10.16 -1.27 180)
				(length 3.81)
				(name "Q0")
				(number "15")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 3.81)
				(name "Q1")
				(number "14")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 3.81)
				(name "Q2")
				(number "13")
			)
			(pin output line
				(at 10.16 -11.43 180)
				(length 3.81)
				(name "Q3")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4020"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 17.78 0)
		)
		(property "Value" "4020"
			(at 5.08 -17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4020_0_0"
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "8")
			)
		)
		(symbol "4020_1_1"
			(pin input clock
				(at -10.16 10.16 0)
				(length 3.81)
				(name "~{CLK}")
				(number "10")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 3.81)
				(name "MR")
				(number "11")
			)
			(pin output line
				(at 10.16 15.24 180)
				(length 3.81)
				(name "Q0")
				(number "9")
			)
			(pin output line
				(at 10.16 12.7 180)
				(length 3.81)
				(name "Q3")
				(number "7")
			)
			(pin output line
				(at 10.16 10.16 180)
				(length 3.81)
				(name "Q4")
				(number "5")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 3.81)
				(name "Q5")
				(number "4")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 3.81)
				(name "Q6")
				(number "6")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 3.81)
				(name "Q7")
				(number "13")
			)
			(pin output line
				(at 10.16 0 180)
				(length 3.81)
				(name "Q8")
				(number "12")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 3.81)
				(name "Q9")
				(number "14")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 3.81)
				(name "Q10")
				(number "15")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 3.81)
				(name "Q11")
				(number "1")
			)
			(pin output line
				(at 10.16 -10.16 180)
				(length 3.81)
				(name "Q12")
				(number "2")
			)
			(pin output line
				(at 10.16 -12.7 180)
				(length 3.81)
				(name "Q13")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4021"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 7.62 0)
		)
		(property "Value" "4021"
			(at 7.62 -21.59 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4021_0_0"
			(text "1"
				(at -1.016 6.604 0)
			)
		)
		(symbol "4021_0_1"
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "Vss")
				(number "8")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 3.81)
				(name "Vdd")
				(number "16")
			)
		)
		(symbol "4021_1_1"
			(pin output line
				(at -10.16 7.62 0)
				(length 3.81)
				(name "PL")
				(number "9")
			)
			(pin output line
				(at -10.16 5.08 0)
				(length 3.81)
				(name "CP")
				(number "10")
			)
			(pin output line
				(at -10.16 1.27 0)
				(length 3.81)
				(name "DS")
				(number "11")
			)
			(pin input line
				(at -10.16 -1.27 0)
				(length 3.81)
				(name "P0")
				(number "7")
			)
			(pin input line
				(at -10.16 -3.81 0)
				(length 3.81)
				(name "P1")
				(number "6")
			)
			(pin input line
				(at -10.16 -6.35 0)
				(length 3.81)
				(name "P2")
				(number "5")
			)
			(pin input line
				(at -10.16 -8.89 0)
				(length 3.81)
				(name "P3")
				(number "4")
			)
			(pin input line
				(at -10.16 -11.43 0)
				(length 3.81)
				(name "P4")
				(number "13")
			)
			(pin input line
				(at -10.16 -13.97 0)
				(length 3.81)
				(name "P5")
				(number "14")
			)
			(pin input line
				(at -10.16 -16.51 0)
				(length 3.81)
				(name "P6")
				(number "15")
			)
			(pin input line
				(at -10.16 -19.05 0)
				(length 3.81)
				(name "P7")
				(number "1")
			)
			(pin output line
				(at 10.16 -13.97 180)
				(length 3.81)
				(name "Q5")
				(number "2")
			)
			(pin output line
				(at 10.16 -16.51 180)
				(length 3.81)
				(name "Q6")
				(number "12")
			)
			(pin output line
				(at 10.16 -19.05 180)
				(length 3.81)
				(name "Q7")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4022"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 15.24 0)
		)
		(property "Value" "4022"
			(at 8.89 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4022_0_0"
			(text "&"
				(at -3.048 8.636 0)
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "VSS")
				(number "8")
			)
		)
		(symbol "4022_0_1")
		(symbol "4022_1_1"
			(pin output line
				(at -10.16 10.16 0)
				(length 3.81)
				(name "CP0")
				(number "14")
			)
			(pin input line
				(at -10.16 6.35 0)
				(length 3.81)
				(name "~{CP1}")
				(number "13")
			)
			(pin input line
				(at -10.16 -8.89 0)
				(length 3.81)
				(name "MR")
				(number "15")
			)
			(pin output line
				(at 10.16 11.43 180)
				(length 3.81)
				(name "Q0")
				(number "2")
			)
			(pin output line
				(at 10.16 8.89 180)
				(length 3.81)
				(name "Q1")
				(number "1")
			)
			(pin output line
				(at 10.16 6.35 180)
				(length 3.81)
				(name "Q2")
				(number "3")
			)
			(pin output line
				(at 10.16 3.81 180)
				(length 3.81)
				(name "Q3")
				(number "7")
			)
			(pin output line
				(at 10.16 1.27 180)
				(length 3.81)
				(name "Q4")
				(number "11")
			)
			(pin output line
				(at 10.16 -1.27 180)
				(length 3.81)
				(name "Q5")
				(number "4")
			)
			(pin output line
				(at 10.16 -3.81 180)
				(length 3.81)
				(name "Q6")
				(number "5")
			)
			(pin output line
				(at 10.16 -6.35 180)
				(length 3.81)
				(name "Q7")
				(number "10")
			)
			(pin output line
				(at 10.16 -10.16 180)
				(length 3.81)
				(name "Co")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4023"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "4023"
			(at 6.35 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4023_0_0"
			(text "&"
				(at 0.762 0 0)
			)
		)
		(symbol "4023_0_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "Vdd")
				(number "14")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "Vss")
				(number "7")
			)
		)
		(symbol "4023_1_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -12.7 0 0)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "8")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "9")
			)
		)
		(symbol "4023_2_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "3")
			)
			(pin input line
				(at -12.7 0 0)
				(length 7.62)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "5")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "6")
			)
		)
		(symbol "4023_3_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "11")
			)
			(pin input line
				(at -12.7 0 0)
				(length 7.62)
				(name "~")
				(number "12")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "13")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4024"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 11.43 0)
		)
		(property "Value" "4024"
			(at 10.16 -10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4024_0_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
		)
		(symbol "4024_1_1"
			(pin input clock
				(at -10.16 5.08 0)
				(length 3.81)
				(name "~{CLK}")
				(number "1")
			)
			(pin input line
				(at -10.16 1.27 0)
				(length 3.81)
				(name "MR")
				(number "2")
			)
			(pin output line
				(at 10.16 8.89 180)
				(length 3.81)
				(name "Q0")
				(number "12")
			)
			(pin output line
				(at 10.16 6.35 180)
				(length 3.81)
				(name "Q1")
				(number "11")
			)
			(pin output line
				(at 10.16 3.81 180)
				(length 3.81)
				(name "Q2")
				(number "9")
			)
			(pin output line
				(at 10.16 1.27 180)
				(length 3.81)
				(name "Q3")
				(number "6")
			)
			(pin output line
				(at 10.16 -1.27 180)
				(length 3.81)
				(name "Q4")
				(number "5")
			)
			(pin output line
				(at 10.16 -3.81 180)
				(length 3.81)
				(name "Q5")
				(number "4")
			)
			(pin output line
				(at 10.16 -6.35 180)
				(length 3.81)
				(name "Q6")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "40240"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 8.89 0)
		)
		(property "Value" "40240"
			(at 8.89 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "40240_0_0")
		(symbol "40240_0_1"
			(pin power_in line
				(at 0 12.7 270)
				(length 3.81)
				(name "Vdd")
				(number "20")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 3.81)
				(name "Vss")
				(number "10")
			)
		)
		(symbol "40240_1_0"
			(pin input line
				(at -12.7 0 0)
				(length 7.62)
				(name "~")
				(number "4")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 7.62)
				(name "~")
				(number "18")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "16")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 7.62)
				(name "~")
				(number "14")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 7.62)
				(name "~")
				(number "12")
			)
		)
		(symbol "40240_1_1"
			(pin input line
				(at -12.7 6.35 0)
				(length 7.62)
				(name "~{EN}")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "6")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 7.62)
				(name "~")
				(number "8")
			)
		)
		(symbol "40240_2_0"
			(pin input line
				(at -12.7 6.35 0)
				(length 7.62)
				(name "~{EN}")
				(number "19")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "11")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "15")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 7.62)
				(name "~")
				(number "17")
			)
		)
		(symbol "40240_2_1"
			(pin input line
				(at -12.7 0 0)
				(length 7.62)
				(name "~")
				(number "13")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 7.62)
				(name "~")
				(number "9")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "7")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 7.62)
				(name "~")
				(number "5")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 7.62)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "40245"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 16.51 0)
		)
		(property "Value" "40245"
			(at 8.636 -15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "40245_0_0")
		(symbol "40245_0_1")
		(symbol "40245_1_0"
			(pin output line
				(at -10.16 12.7 0)
				(length 3.81)
				(name "~{G}")
				(number "19")
			)
			(pin output inverted
				(at -10.16 10.16 0)
				(length 3.81)
				(name "Dir")
				(number "1")
			)
			(pin output line
				(at -10.16 6.35 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin output line
				(at -10.16 3.81 0)
				(length 3.81)
				(name "~")
				(number "3")
			)
			(pin output line
				(at -10.16 1.27 0)
				(length 3.81)
				(name "~")
				(number "4")
			)
			(pin output line
				(at -10.16 -1.27 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin output line
				(at -10.16 -3.81 0)
				(length 3.81)
				(name "~")
				(number "6")
			)
			(pin output line
				(at -10.16 -6.35 0)
				(length 3.81)
				(name "~")
				(number "7")
			)
			(pin output line
				(at -10.16 -8.89 0)
				(length 3.81)
				(name "~")
				(number "8")
			)
			(pin output line
				(at -10.16 -11.43 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "Vdd")
				(number "20")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "Vss")
				(number "10")
			)
			(pin bidirectional line
				(at 10.16 6.35 180)
				(length 3.81)
				(name "~")
				(number "18")
			)
			(pin bidirectional line
				(at 10.16 3.81 180)
				(length 3.81)
				(name "~")
				(number "17")
			)
			(pin bidirectional line
				(at 10.16 1.27 180)
				(length 3.81)
				(name "~")
				(number "16")
			)
			(pin bidirectional line
				(at 10.16 -1.27 180)
				(length 3.81)
				(name "~")
				(number "15")
			)
			(pin bidirectional line
				(at 10.16 -3.81 180)
				(length 3.81)
				(name "~")
				(number "14")
			)
			(pin bidirectional line
				(at 10.16 -6.35 180)
				(length 3.81)
				(name "~")
				(number "13")
			)
			(pin bidirectional line
				(at 10.16 -8.89 180)
				(length 3.81)
				(name "~")
				(number "12")
			)
			(pin bidirectional line
				(at 10.16 -11.43 180)
				(length 3.81)
				(name "~")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4025"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "4025"
			(at 6.35 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4025_0_0"
			(text "1"
				(at 0.762 0 0)
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vdd")
				(number "14")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "Vss")
				(number "7")
			)
		)
		(symbol "4025_1_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -12.7 0 0)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "8")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "9")
			)
		)
		(symbol "4025_2_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "3")
			)
			(pin input line
				(at -12.7 0 0)
				(length 7.62)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "5")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "6")
			)
		)
		(symbol "4025_3_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "11")
			)
			(pin input line
				(at -12.7 0 0)
				(length 7.62)
				(name "~")
				(number "12")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "13")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4027"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 7.62 0)
		)
		(property "Value" "4027"
			(at 6.35 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4027_0_0"
			(pin power_in line
				(at 0 10.16 270)
				(length 3.81)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 3.81)
				(name "VSS")
				(number "8")
			)
		)
		(symbol "4027_0_1")
		(symbol "4027_1_1"
			(pin input line
				(at -15.24 5.08 0)
				(length 7.62)
				(name "S")
				(number "7")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 7.62)
				(name "J")
				(number "6")
			)
			(pin input clock
				(at -15.24 0 0)
				(length 7.62)
				(name "CK")
				(number "3")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 7.62)
				(name "K")
				(number "5")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 7.62)
				(name "R")
				(number "4")
			)
			(pin output line
				(at 15.24 3.81 180)
				(length 7.62)
				(name "Q")
				(number "1")
			)
			(pin output line
				(at 15.24 -3.81 180)
				(length 7.62)
				(name "~{Q}")
				(number "2")
			)
		)
		(symbol "4027_2_1"
			(pin input line
				(at -15.24 5.08 0)
				(length 7.62)
				(name "S")
				(number "9")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 7.62)
				(name "J")
				(number "10")
			)
			(pin input clock
				(at -15.24 0 0)
				(length 7.62)
				(name "CK")
				(number "13")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 7.62)
				(name "K")
				(number "11")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 7.62)
				(name "R")
				(number "12")
			)
			(pin output line
				(at 15.24 3.81 180)
				(length 7.62)
				(name "Q")
				(number "15")
			)
			(pin output line
				(at 15.24 -3.81 180)
				(length 7.62)
				(name "~{Q}")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4028"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 16.51 0)
		)
		(property "Value" "4028"
			(at 6.35 -15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4028_0_0"
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VDD")
				(number "16")
			)
		)
		(symbol "4028_0_1"
			(pin power_in line
				(at 0 -17.78 90)
				(length 3.81)
				(name "VSS")
				(number "8")
			)
		)
		(symbol "4028_1_1"
			(pin input line
				(at -15.24 3.81 0)
				(length 7.62)
				(name "A")
				(number "10")
			)
			(pin input line
				(at -15.24 1.27 0)
				(length 7.62)
				(name "B")
				(number "13")
			)
			(pin input line
				(at -15.24 -1.27 0)
				(length 7.62)
				(name "C")
				(number "12")
			)
			(pin input line
				(at -15.24 -3.81 0)
				(length 7.62)
				(name "D")
				(number "11")
			)
			(pin output line
				(at 15.24 11.43 180)
				(length 7.62)
				(name "S0")
				(number "3")
			)
			(pin output line
				(at 15.24 8.89 180)
				(length 7.62)
				(name "S1")
				(number "14")
			)
			(pin output line
				(at 15.24 6.35 180)
				(length 7.62)
				(name "S2")
				(number "2")
			)
			(pin output line
				(at 15.24 3.81 180)
				(length 7.62)
				(name "S3")
				(number "15")
			)
			(pin output line
				(at 15.24 1.27 180)
				(length 7.62)
				(name "S4")
				(number "1")
			)
			(pin output line
				(at 15.24 -1.27 180)
				(length 7.62)
				(name "S5")
				(number "6")
			)
			(pin output line
				(at 15.24 -3.81 180)
				(length 7.62)
				(name "S6")
				(number "7")
			)
			(pin output line
				(at 15.24 -6.35 180)
				(length 7.62)
				(name "S7")
				(number "4")
			)
			(pin output line
				(at 15.24 -8.89 180)
				(length 7.62)
				(name "S8")
				(number "9")
			)
			(pin output line
				(at 15.24 -11.43 180)
				(length 7.62)
				(name "S9")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4029"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.89 8.89 0)
		)
		(property "Value" "4029"
			(at 8.89 -19.05 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4029_0_0"
			(text "1"
				(at 1.27 -7.62 0)
			)
			(text "2"
				(at 1.27 -10.16 0)
			)
			(text "3"
				(at 1.27 -12.7 0)
			)
			(text "4"
				(at 1.27 -15.24 0)
			)
		)
		(symbol "4029_1_1"
			(pin input line
				(at -12.7 8.89 0)
				(length 7.62)
				(name "B/D")
				(number "9")
			)
			(pin input line
				(at -12.7 6.35 0)
				(length 7.62)
				(name "U/D")
				(number "10")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~{CE}")
				(number "5")
			)
			(pin input line
				(at -12.7 -1.27 0)
				(length 7.62)
				(name "PL")
				(number "1")
			)
			(pin input clock
				(at -12.7 -3.81 0)
				(length 7.62)
				(name "CK")
				(number "15")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 7.62)
				(name "P0")
				(number "4")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 7.62)
				(name "P1")
				(number "12")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 7.62)
				(name "P2")
				(number "13")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 7.62)
				(name "P3")
				(number "3")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "8")
			)
			(pin output line
				(at 12.7 1.27 180)
				(length 7.62)
				(name "~{TC}")
				(number "7")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 7.62)
				(name "Q0")
				(number "6")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 7.62)
				(name "Q1")
				(number "11")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 7.62)
				(name "Q2")
				(number "14")
			)
			(pin output line
				(at 12.7 -15.24 180)
				(length 7.62)
				(name "Q3")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4030"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "4030"
			(at 6.35 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4030_0_0"
			(text "=1"
				(at 0.254 0 0)
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vdd")
				(number "14")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "Vss")
				(number "7")
			)
		)
		(symbol "4030_1_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "3")
			)
		)
		(symbol "4030_2_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "5")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "6")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "4")
			)
		)
		(symbol "4030_3_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "8")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "9")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "10")
			)
		)
		(symbol "4030_4_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "12")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "13")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "40373"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 13.97 0)
		)
		(property "Value" "40373"
			(at 8.89 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "40373_0_0"
			(pin input line
				(at -12.7 10.16 0)
				(length 7.62)
				(name "~{EN}")
				(number "1")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 7.62)
				(name "ST")
				(number "11")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "Vdd")
				(number "20")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "Vss")
				(number "10")
			)
		)
		(symbol "40373_0_1")
		(symbol "40373_1_0"
			(pin input line
				(at -12.7 3.81 0)
				(length 7.62)
				(name "~")
				(number "3")
			)
			(pin input line
				(at -12.7 1.27 0)
				(length 7.62)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -12.7 -1.27 0)
				(length 7.62)
				(name "~")
				(number "7")
			)
			(pin input line
				(at -12.7 -3.81 0)
				(length 7.62)
				(name "~")
				(number "8")
			)
			(pin input line
				(at -12.7 -6.35 0)
				(length 7.62)
				(name "~")
				(number "13")
			)
			(pin input line
				(at -12.7 -8.89 0)
				(length 7.62)
				(name "~")
				(number "14")
			)
			(pin input line
				(at -12.7 -11.43 0)
				(length 7.62)
				(name "~")
				(number "17")
			)
			(pin input line
				(at -12.7 -13.97 0)
				(length 7.62)
				(name "~")
				(number "18")
			)
			(pin output line
				(at 12.7 3.81 180)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin output line
				(at 12.7 1.27 180)
				(length 7.62)
				(name "~")
				(number "5")
			)
			(pin output line
				(at 12.7 -1.27 180)
				(length 7.62)
				(name "~")
				(number "6")
			)
			(pin output line
				(at 12.7 -3.81 180)
				(length 7.62)
				(name "~")
				(number "9")
			)
			(pin output line
				(at 12.7 -6.35 180)
				(length 7.62)
				(name "~")
				(number "12")
			)
			(pin output line
				(at 12.7 -8.89 180)
				(length 7.62)
				(name "~")
				(number "15")
			)
			(pin output line
				(at 12.7 -11.43 180)
				(length 7.62)
				(name "~")
				(number "16")
			)
			(pin output line
				(at 12.7 -13.97 180)
				(length 7.62)
				(name "~")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "40374"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 13.97 0)
		)
		(property "Value" "40374"
			(at 8.89 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.digchip.com/datasheets/download_datasheet.php?id=369790&part-number=HEF40374BDB"
			(at 0 0 0)
		)
		(property "Description" "8-bit D-flip-flop with 3-State outputs"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS BUFFER 3State"
			(at 0 0 0)
		)
		(symbol "40374_0_0"
			(pin input line
				(at -12.7 10.16 0)
				(length 7.62)
				(name "~{E}")
				(number "1")
			)
			(pin input clock
				(at -12.7 7.62 0)
				(length 7.62)
				(name "Ck")
				(number "11")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "Vdd")
				(number "20")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "Vss")
				(number "10")
			)
		)
		(symbol "40374_0_1")
		(symbol "40374_1_0"
			(pin input line
				(at -12.7 3.81 0)
				(length 7.62)
				(name "~")
				(number "3")
			)
			(pin input line
				(at -12.7 1.27 0)
				(length 7.62)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -12.7 -1.27 0)
				(length 7.62)
				(name "~")
				(number "7")
			)
			(pin input line
				(at -12.7 -3.81 0)
				(length 7.62)
				(name "~")
				(number "8")
			)
			(pin input line
				(at -12.7 -6.35 0)
				(length 7.62)
				(name "~")
				(number "13")
			)
			(pin input line
				(at -12.7 -8.89 0)
				(length 7.62)
				(name "~")
				(number "14")
			)
			(pin input line
				(at -12.7 -11.43 0)
				(length 7.62)
				(name "~")
				(number "17")
			)
			(pin input line
				(at -12.7 -13.97 0)
				(length 7.62)
				(name "~")
				(number "18")
			)
			(pin tri_state line
				(at 12.7 3.81 180)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin tri_state line
				(at 12.7 1.27 180)
				(length 7.62)
				(name "~")
				(number "5")
			)
			(pin tri_state line
				(at 12.7 -1.27 180)
				(length 7.62)
				(name "~")
				(number "6")
			)
			(pin tri_state line
				(at 12.7 -3.81 180)
				(length 7.62)
				(name "~")
				(number "9")
			)
			(pin tri_state line
				(at 12.7 -6.35 180)
				(length 7.62)
				(name "~")
				(number "12")
			)
			(pin tri_state line
				(at 12.7 -8.89 180)
				(length 7.62)
				(name "~")
				(number "15")
			)
			(pin tri_state line
				(at 12.7 -11.43 180)
				(length 7.62)
				(name "~")
				(number "16")
			)
			(pin tri_state line
				(at 12.7 -13.97 180)
				(length 7.62)
				(name "~")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4040"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 16.51 0)
		)
		(property "Value" "4040"
			(at 5.08 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4040_0_0"
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VSS")
				(number "8")
			)
		)
		(symbol "4040_1_1"
			(pin input clock_low
				(at -10.16 10.16 0)
				(length 3.81)
				(name "CLK")
				(number "10")
			)
			(pin input line
				(at -10.16 6.35 0)
				(length 3.81)
				(name "MR")
				(number "11")
			)
			(pin output line
				(at 10.16 13.97 180)
				(length 3.81)
				(name "Q0")
				(number "9")
			)
			(pin output line
				(at 10.16 11.43 180)
				(length 3.81)
				(name "Q3")
				(number "7")
			)
			(pin output line
				(at 10.16 8.89 180)
				(length 3.81)
				(name "Q4")
				(number "6")
			)
			(pin output line
				(at 10.16 6.35 180)
				(length 3.81)
				(name "Q5")
				(number "5")
			)
			(pin output line
				(at 10.16 3.81 180)
				(length 3.81)
				(name "Q6")
				(number "3")
			)
			(pin output line
				(at 10.16 1.27 180)
				(length 3.81)
				(name "Q7")
				(number "2")
			)
			(pin output line
				(at 10.16 -1.27 180)
				(length 3.81)
				(name "Q8")
				(number "4")
			)
			(pin output line
				(at 10.16 -3.81 180)
				(length 3.81)
				(name "Q9")
				(number "13")
			)
			(pin output line
				(at 10.16 -6.35 180)
				(length 3.81)
				(name "Q10")
				(number "12")
			)
			(pin output line
				(at 10.16 -8.89 180)
				(length 3.81)
				(name "Q11")
				(number "14")
			)
			(pin output line
				(at 10.16 -11.43 180)
				(length 3.81)
				(name "Q12")
				(number "15")
			)
			(pin output line
				(at 10.16 -13.97 180)
				(length 3.81)
				(name "Q13")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4041"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 6.35 0)
		)
		(property "Value" "4041"
			(at 6.35 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4041_0_0")
		(symbol "4041_0_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "Vdd")
				(number "14")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "Vss")
				(number "7")
			)
		)
		(symbol "4041_1_1"
			(pin output line
				(at -12.7 0 0)
				(length 7.62)
				(name "~")
				(number "3")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin output inverted
				(at 12.7 -2.54 180)
				(length 7.62)
				(name "~")
				(number "2")
			)
		)
		(symbol "4041_2_1"
			(pin output line
				(at -12.7 0 0)
				(length 7.62)
				(name "~")
				(number "6")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 7.62)
				(name "~")
				(number "4")
			)
			(pin output inverted
				(at 12.7 -2.54 180)
				(length 7.62)
				(name "~")
				(number "5")
			)
		)
		(symbol "4041_3_1"
			(pin output line
				(at -12.7 0 0)
				(length 7.62)
				(name "~")
				(number "10")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 7.62)
				(name "~")
				(number "8")
			)
			(pin output inverted
				(at 12.7 -2.54 180)
				(length 7.62)
				(name "~")
				(number "9")
			)
		)
		(symbol "4041_4_1"
			(pin output line
				(at -12.7 0 0)
				(length 7.62)
				(name "~")
				(number "13")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 7.62)
				(name "~")
				(number "11")
			)
			(pin output inverted
				(at 12.7 -2.54 180)
				(length 7.62)
				(name "~")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4042"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 11.43 0)
		)
		(property "Value" "4042"
			(at 7.62 -15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4042_0_0"
			(text "=1"
				(at -2.54 10.16 0)
			)
		)
		(symbol "4042_0_1")
		(symbol "4042_1_0"
			(pin input clock
				(at -12.7 11.43 0)
				(length 7.62)
				(name "E0")
				(number "5")
			)
			(pin input line
				(at -12.7 8.89 0)
				(length 7.62)
				(name "E1")
				(number "6")
			)
			(pin input line
				(at -12.7 3.81 0)
				(length 7.62)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -12.7 -1.27 0)
				(length 7.62)
				(name "~")
				(number "7")
			)
			(pin input line
				(at -12.7 -6.35 0)
				(length 7.62)
				(name "~")
				(number "13")
			)
			(pin input line
				(at -12.7 -11.43 0)
				(length 7.62)
				(name "~")
				(number "14")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 3.81)
				(name "Vss")
				(number "8")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "Vdd")
				(number "16")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin output inverted
				(at 12.7 2.54 180)
				(length 7.62)
				(name "~")
				(number "3")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "10")
			)
			(pin output inverted
				(at 12.7 -2.54 180)
				(length 7.62)
				(name "~")
				(number "9")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 7.62)
				(name "~")
				(number "11")
			)
			(pin output inverted
				(at 12.7 -7.62 180)
				(length 7.62)
				(name "~")
				(number "12")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin output inverted
				(at 12.7 -12.7 180)
				(length 7.62)
				(name "~")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4043"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 12.7 0)
		)
		(property "Value" "4043"
			(at 7.62 -20.32 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4043_0_0"
			(text "1"
				(at -1.27 -1.27 0)
			)
		)
		(symbol "4043_1_0"
			(pin input line
				(at -12.7 6.35 0)
				(length 7.62)
				(name "EN")
				(number "5")
			)
			(pin input line
				(at -12.7 0 0)
				(length 7.62)
				(name "~")
				(number "3")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 7.62)
				(name "~")
				(number "7")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 7.62)
				(name "~")
				(number "6")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 7.62)
				(name "~")
				(number "11")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 7.62)
				(name "~")
				(number "12")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 7.62)
				(name "~")
				(number "15")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 7.62)
				(name "~")
				(number "14")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "Vdd")
				(number "16")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 3.81)
				(name "Vss")
				(number "8")
			)
			(pin output line
				(at 12.7 -1.27 180)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin output line
				(at 12.7 -6.35 180)
				(length 7.62)
				(name "~")
				(number "9")
			)
			(pin output line
				(at 12.7 -11.43 180)
				(length 7.62)
				(name "~")
				(number "10")
			)
			(pin output line
				(at 12.7 -16.51 180)
				(length 7.62)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4044"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 6.35 0)
		)
		(property "Value" "4044"
			(at 7.62 -20.32 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4044_0_0"
			(text "&"
				(at -2.54 -1.27 0)
			)
		)
		(symbol "4044_1_0"
			(pin input line
				(at -12.7 6.35 0)
				(length 7.62)
				(name "EN")
				(number "5")
			)
			(pin input line
				(at -12.7 0 0)
				(length 7.62)
				(name "~")
				(number "3")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 7.62)
				(name "~")
				(number "7")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 7.62)
				(name "~")
				(number "6")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 7.62)
				(name "~")
				(number "11")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 7.62)
				(name "~")
				(number "12")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 7.62)
				(name "~")
				(number "15")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 7.62)
				(name "~")
				(number "14")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "Vdd")
				(number "16")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 3.81)
				(name "Vss")
				(number "8")
			)
			(pin output line
				(at 12.7 -1.27 180)
				(length 7.62)
				(name "~")
				(number "13")
			)
			(pin output line
				(at 12.7 -6.35 180)
				(length 7.62)
				(name "~")
				(number "9")
			)
			(pin output line
				(at 12.7 -11.43 180)
				(length 7.62)
				(name "~")
				(number "10")
			)
			(pin output line
				(at 12.7 -16.51 180)
				(length 7.62)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4046"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.89 12.7 0)
		)
		(property "Value" "4046"
			(at 8.89 -15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4046_0_1"
			(pin power_in line
				(at 0 15.24 270)
				(length 3.81)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "VSS")
				(number "8")
			)
		)
		(symbol "4046_1_1"
			(pin input line
				(at -15.24 10.16 0)
				(length 7.62)
				(name "RefIn")
				(number "3")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 7.62)
				(name "SigIn")
				(number "14")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 7.62)
				(name "C1")
				(number "6")
			)
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "C2")
				(number "7")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 7.62)
				(name "R1")
				(number "11")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 7.62)
				(name "R2")
				(number "12")
			)
			(pin input line
				(at -15.24 -11.43 0)
				(length 7.62)
				(name "Inh")
				(number "5")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 7.62)
				(name "FOUT")
				(number "4")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 7.62)
				(name "PC1")
				(number "2")
			)
			(pin tri_state line
				(at 15.24 5.08 180)
				(length 7.62)
				(name "PC2")
				(number "13")
			)
			(pin input line
				(at 15.24 0 180)
				(length 7.62)
				(name "VCOin")
				(number "9")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 7.62)
				(name "PCP")
				(number "1")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 7.62)
				(name "SFout")
				(number "10")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 7.62)
				(name "ZOUT")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4048"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 17.78 0)
		)
		(property "Value" "4048"
			(at 8.89 -21.59 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4048_0_1")
		(symbol "4048_1_1"
			(pin input line
				(at -15.24 15.24 0)
				(length 7.62)
				(name "EN")
				(number "2")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 7.62)
				(name "Ka")
				(number "10")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 7.62)
				(name "Kb")
				(number "7")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 7.62)
				(name "Kc")
				(number "9")
			)
			(pin input line
				(at -15.24 3.81 0)
				(length 7.62)
				(name "Ex")
				(number "15")
			)
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "A")
				(number "14")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 7.62)
				(name "B")
				(number "13")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 7.62)
				(name "C")
				(number "12")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 7.62)
				(name "D")
				(number "11")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 7.62)
				(name "E")
				(number "6")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 7.62)
				(name "F")
				(number "5")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 7.62)
				(name "G")
				(number "4")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 7.62)
				(name "H")
				(number "3")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "Vdd")
				(number "16")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 3.81)
				(name "Vss")
				(number "8")
			)
			(pin output line
				(at 15.24 0 180)
				(length 7.62)
				(name "J")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4049"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 7.62 0)
		)
		(property "Value" "4049"
			(at 8.89 -11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4049_0_0"
			(pin power_in line
				(at 0 10.16 270)
				(length 3.81)
				(name "Vdd")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 3.81)
				(name "Vss")
				(number "8")
			)
		)
		(symbol "4049_0_1")
		(symbol "4049_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 3.81)
				(name "~")
				(number "3")
			)
			(pin output inverted
				(at 10.16 0 180)
				(length 3.81)
				(name "~")
				(number "2")
			)
		)
		(symbol "4049_2_1"
			(pin input line
				(at -10.16 0 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin output inverted
				(at 10.16 0 180)
				(length 3.81)
				(name "~")
				(number "4")
			)
		)
		(symbol "4049_3_1"
			(pin input line
				(at -10.16 0 0)
				(length 3.81)
				(name "~")
				(number "7")
			)
			(pin output inverted
				(at 10.16 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "4049_4_1"
			(pin input line
				(at -10.16 0 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin output inverted
				(at 10.16 0 180)
				(length 3.81)
				(name "~")
				(number "10")
			)
		)
		(symbol "4049_5_1"
			(pin input line
				(at -10.16 0 0)
				(length 3.81)
				(name "~")
				(number "11")
			)
			(pin output inverted
				(at 10.16 0 180)
				(length 3.81)
				(name "~")
				(number "12")
			)
		)
		(symbol "4049_6_1"
			(pin input line
				(at -10.16 0 0)
				(length 3.81)
				(name "~")
				(number "14")
			)
			(pin output inverted
				(at 10.16 0 180)
				(length 3.81)
				(name "~")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4050"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 6.35 0)
		)
		(property "Value" "4050"
			(at 7.62 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4050_0_0"
			(pin power_in line
				(at 0 10.16 270)
				(length 3.81)
				(name "Vdd")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 3.81)
				(name "Vss")
				(number "8")
			)
		)
		(symbol "4050_0_1")
		(symbol "4050_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 3.81)
				(name "~")
				(number "3")
			)
			(pin output line
				(at 10.16 0 180)
				(length 3.81)
				(name "~")
				(number "2")
			)
		)
		(symbol "4050_2_1"
			(pin input line
				(at -10.16 0 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin output line
				(at 10.16 0 180)
				(length 3.81)
				(name "~")
				(number "4")
			)
		)
		(symbol "4050_3_1"
			(pin input line
				(at -10.16 0 0)
				(length 3.81)
				(name "~")
				(number "7")
			)
			(pin output line
				(at 10.16 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "4050_4_1"
			(pin input line
				(at -10.16 0 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin output line
				(at 10.16 0 180)
				(length 3.81)
				(name "~")
				(number "10")
			)
		)
		(symbol "4050_5_1"
			(pin input line
				(at -10.16 0 0)
				(length 3.81)
				(name "~")
				(number "11")
			)
			(pin output line
				(at 10.16 0 180)
				(length 3.81)
				(name "~")
				(number "12")
			)
		)
		(symbol "4050_6_1"
			(pin input line
				(at -10.16 0 0)
				(length 3.81)
				(name "~")
				(number "14")
			)
			(pin output line
				(at 10.16 0 180)
				(length 3.81)
				(name "~")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4051"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.89 17.78 0)
		)
		(property "Value" "4051"
			(at 6.35 -17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4051_0_0"
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "Vdd")
				(number "16")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 3.81)
				(name "Vss")
				(number "8")
			)
		)
		(symbol "4051_0_1")
		(symbol "4051_1_1"
			(pin passive line
				(at -15.24 15.24 0)
				(length 7.62)
				(name "X0")
				(number "13")
			)
			(pin passive line
				(at -15.24 12.7 0)
				(length 7.62)
				(name "X1")
				(number "14")
			)
			(pin passive line
				(at -15.24 10.16 0)
				(length 7.62)
				(name "X2")
				(number "15")
			)
			(pin passive line
				(at -15.24 7.62 0)
				(length 7.62)
				(name "X3")
				(number "12")
			)
			(pin passive line
				(at -15.24 5.08 0)
				(length 7.62)
				(name "X4")
				(number "1")
			)
			(pin passive line
				(at -15.24 2.54 0)
				(length 7.62)
				(name "X5")
				(number "5")
			)
			(pin passive line
				(at -15.24 0 0)
				(length 7.62)
				(name "X6")
				(number "2")
			)
			(pin passive line
				(at -15.24 -2.54 0)
				(length 7.62)
				(name "X7")
				(number "4")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 7.62)
				(name "~{E}")
				(number "6")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 7.62)
				(name "A")
				(number "11")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 7.62)
				(name "B")
				(number "10")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 7.62)
				(name "C")
				(number "9")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 3.81)
				(name "VEE")
				(number "7")
			)
			(pin passive line
				(at 15.24 7.62 180)
				(length 7.62)
				(name "X")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4052"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 11.43 15.24 0)
		)
		(property "Value" "4052"
			(at 10.16 -19.05 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4052_0_0"
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "Vdd")
				(number "16")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "Vss")
				(number "8")
			)
		)
		(symbol "4052_0_1")
		(symbol "4052_1_1"
			(pin input line
				(at -15.24 15.24 0)
				(length 7.62)
				(name "A0")
				(number "10")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 7.62)
				(name "A1")
				(number "9")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 7.62)
				(name "~{E}")
				(number "6")
			)
			(pin passive line
				(at -15.24 5.08 0)
				(length 7.62)
				(name "X0")
				(number "12")
			)
			(pin passive line
				(at -15.24 2.54 0)
				(length 7.62)
				(name "X1")
				(number "14")
			)
			(pin passive line
				(at -15.24 0 0)
				(length 7.62)
				(name "X2")
				(number "15")
			)
			(pin passive line
				(at -15.24 -2.54 0)
				(length 7.62)
				(name "X3")
				(number "11")
			)
			(pin passive line
				(at -15.24 -7.62 0)
				(length 7.62)
				(name "Y0")
				(number "1")
			)
			(pin passive line
				(at -15.24 -10.16 0)
				(length 7.62)
				(name "Y1")
				(number "5")
			)
			(pin passive line
				(at -15.24 -12.7 0)
				(length 7.62)
				(name "Y2")
				(number "2")
			)
			(pin passive line
				(at -15.24 -15.24 0)
				(length 7.62)
				(name "Y3")
				(number "4")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 2.54)
				(name "VEE")
				(number "7")
			)
			(pin passive line
				(at 15.24 1.27 180)
				(length 7.62)
				(name "X")
				(number "13")
			)
			(pin passive line
				(at 15.24 -11.43 180)
				(length 7.62)
				(name "Y")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4053"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 11.43 13.97 0)
		)
		(property "Value" "4053"
			(at 8.89 -17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4053_0_0"
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "8")
			)
		)
		(symbol "4053_0_1")
		(symbol "4053_1_1"
			(pin input line
				(at -15.24 11.43 0)
				(length 7.62)
				(name "~{E}")
				(number "6")
			)
			(pin passive line
				(at -15.24 3.81 0)
				(length 7.62)
				(name "X0")
				(number "12")
			)
			(pin passive line
				(at -15.24 1.27 0)
				(length 7.62)
				(name "X1")
				(number "13")
			)
			(pin passive line
				(at -15.24 -3.81 0)
				(length 7.62)
				(name "Y0")
				(number "2")
			)
			(pin passive line
				(at -15.24 -6.35 0)
				(length 7.62)
				(name "Y1")
				(number "1")
			)
			(pin passive line
				(at -15.24 -11.43 0)
				(length 7.62)
				(name "Z0")
				(number "5")
			)
			(pin passive line
				(at -15.24 -13.97 0)
				(length 7.62)
				(name "Z0")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 3.81)
				(name "VEE")
				(number "7")
			)
			(pin passive line
				(at 15.24 3.81 180)
				(length 7.62)
				(name "X")
				(number "14")
			)
			(pin input line
				(at 15.24 1.27 180)
				(length 7.62)
				(name "A")
				(number "11")
			)
			(pin passive line
				(at 15.24 -3.81 180)
				(length 7.62)
				(name "Y")
				(number "15")
			)
			(pin input line
				(at 15.24 -6.35 180)
				(length 7.62)
				(name "B")
				(number "10")
			)
			(pin passive line
				(at 15.24 -11.43 180)
				(length 7.62)
				(name "Z")
				(number "4")
			)
			(pin input line
				(at 15.24 -13.97 180)
				(length 7.62)
				(name "C")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4060"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 16.51 0)
		)
		(property "Value" "4060"
			(at 6.35 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/m74hc4060.pdf"
			(at 0 0 0)
		)
		(property "Description" "Binary counter (14-stages) and oscillator"
			(at 0 0 0)
		)
		(property "ki_keywords" "binary counter oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*7.62* TSSOP*16*4.4x5* SOIC*16*3.9x9.9*"
			(at 0 0 0)
		)
		(symbol "4060_1_0"
			(pin input clock_low
				(at -15.24 12.7 0)
				(length 7.62)
				(name "~{Φ0}")
				(number "9")
			)
			(pin input clock
				(at -15.24 10.16 0)
				(length 7.62)
				(name "Φ0")
				(number "10")
			)
			(pin input clock_low
				(at -15.24 7.62 0)
				(length 7.62)
				(name "~{Φ1}")
				(number "11")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 7.62)
				(name "CLR")
				(number "12")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 7.62)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 7.62)
				(name "VSS")
				(number "8")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 7.62)
				(name "Q4")
				(number "7")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 7.62)
				(name "Q5")
				(number "5")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 7.62)
				(name "Q6")
				(number "4")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 7.62)
				(name "Q7")
				(number "6")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 7.62)
				(name "Q8")
				(number "14")
			)
			(pin output line
				(at 15.24 0 180)
				(length 7.62)
				(name "Q9")
				(number "13")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 7.62)
				(name "Q10")
				(number "15")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 7.62)
				(name "Q12")
				(number "1")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 7.62)
				(name "Q13")
				(number "2")
			)
			(pin output line
				(at 15.24 -12.7 180)
				(length 7.62)
				(name "Q14")
				(number "3")
			)
		)
		(symbol "4060_1_1")
		(embedded_fonts no)
	)
	(symbol "4068"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 11.176 0)
		)
		(property "Value" "4068"
			(at 3.81 11.176 0)
		)
		(property "Footprint" ""
			(at 0 -1.27 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/cd4068b.pdf"
			(at 0 0 0)
		)
		(property "Description" "CMOS 8-input NAND/AND Gate"
			(at 0 0 0)
		)
		(property "ki_keywords" "cmos nand and 8-input"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SO*5.3x10.2mm*P1.27mm* SO*3.9x8.65mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "4068_0_0"
			(text "&"
				(at 0 -1.27 0)
			)
		)
		(symbol "4068_0_1"
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "Vdd")
				(number "14")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 5.08)
				(name "Vss")
				(number "7")
			)
		)
		(symbol "4068_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 5.08)
				(name "A")
				(number "2")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 5.08)
				(name "B")
				(number "3")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 5.08)
				(name "C")
				(number "4")
			)
			(pin input line
				(at -10.16 0 0)
				(length 5.08)
				(name "D")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 5.08)
				(name "E")
				(number "9")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 5.08)
				(name "F")
				(number "10")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 5.08)
				(name "G")
				(number "11")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 5.08)
				(name "H")
				(number "12")
			)
			(pin no_connect line
				(at 5.08 -5.08 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at 5.08 -7.62 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 5.08)
				(name "K")
				(number "1")
			)
			(pin output inverted
				(at 10.16 0 180)
				(length 5.08)
				(name "J")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4069"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "4069"
			(at 7.62 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4069_0_0"
			(text "1"
				(at -1.27 0 0)
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 3.81)
				(name "Vdd")
				(number "14")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 3.81)
				(name "Vss")
				(number "7")
			)
		)
		(symbol "4069_0_1")
		(symbol "4069_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin output inverted
				(at 10.16 0 180)
				(length 3.81)
				(name "~")
				(number "2")
			)
		)
		(symbol "4069_2_1"
			(pin input line
				(at -10.16 0 0)
				(length 3.81)
				(name "~")
				(number "3")
			)
			(pin output inverted
				(at 10.16 0 180)
				(length 3.81)
				(name "~")
				(number "4")
			)
		)
		(symbol "4069_3_1"
			(pin input line
				(at -10.16 0 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin output inverted
				(at 10.16 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "4069_4_1"
			(pin input line
				(at -10.16 0 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin output inverted
				(at 10.16 0 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "4069_5_1"
			(pin input line
				(at -10.16 0 0)
				(length 3.81)
				(name "~")
				(number "11")
			)
			(pin output inverted
				(at 10.16 0 180)
				(length 3.81)
				(name "~")
				(number "10")
			)
		)
		(symbol "4069_6_1"
			(pin input line
				(at -10.16 0 0)
				(length 3.81)
				(name "~")
				(number "13")
			)
			(pin output inverted
				(at 10.16 0 180)
				(length 3.81)
				(name "~")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4070"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "4070"
			(at 6.35 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4070_0_0"
			(text "=1"
				(at 0.254 0 0)
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "Vdd")
				(number "14")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "Vss")
				(number "7")
			)
		)
		(symbol "4070_1_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "3")
			)
		)
		(symbol "4070_2_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "5")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "6")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "4")
			)
		)
		(symbol "4070_3_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "8")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "9")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "10")
			)
		)
		(symbol "4070_4_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "12")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "13")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4071"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "4071"
			(at 6.35 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4071_0_0"
			(text "1"
				(at 0.254 0 0)
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "Vdd")
				(number "14")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "Vss")
				(number "7")
			)
		)
		(symbol "4071_1_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "3")
			)
		)
		(symbol "4071_2_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "5")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "6")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "4")
			)
		)
		(symbol "4071_3_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "8")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "9")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "10")
			)
		)
		(symbol "4071_4_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "12")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "13")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4072"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 6.35 0)
		)
		(property "Value" "4072"
			(at 5.08 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4072_0_0"
			(text "1"
				(at 0 0 0)
			)
		)
		(symbol "4072_0_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "Vdd")
				(number "14")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "Vss")
				(number "7")
			)
		)
		(symbol "4072_1_1"
			(pin input line
				(at -12.7 3.81 0)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin input line
				(at -12.7 1.27 0)
				(length 7.62)
				(name "~")
				(number "3")
			)
			(pin input line
				(at -12.7 -1.27 0)
				(length 7.62)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -12.7 -3.81 0)
				(length 7.62)
				(name "~")
				(number "12")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "1")
			)
		)
		(symbol "4072_2_1"
			(pin input line
				(at -12.7 3.81 0)
				(length 7.62)
				(name "~")
				(number "9")
			)
			(pin input line
				(at -12.7 1.27 0)
				(length 7.62)
				(name "~")
				(number "10")
			)
			(pin input line
				(at -12.7 -1.27 0)
				(length 7.62)
				(name "~")
				(number "11")
			)
			(pin input line
				(at -12.7 -3.81 0)
				(length 7.62)
				(name "~")
				(number "12")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4073"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "4073"
			(at 6.35 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4073_0_0"
			(text "&"
				(at 0.762 0 0)
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "Vdd")
				(number "14")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "Vss")
				(number "7")
			)
		)
		(symbol "4073_1_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -12.7 0 0)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "8")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "9")
			)
		)
		(symbol "4073_2_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "3")
			)
			(pin input line
				(at -12.7 0 0)
				(length 7.62)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "5")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "6")
			)
		)
		(symbol "4073_3_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "11")
			)
			(pin input line
				(at -12.7 0 0)
				(length 7.62)
				(name "~")
				(number "12")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "13")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4075"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "4075"
			(at 6.35 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4075_0_0"
			(text "1"
				(at 0.762 0 0)
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "Vdd")
				(number "14")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "Vss")
				(number "7")
			)
		)
		(symbol "4075_1_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -12.7 0 0)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "8")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "9")
			)
		)
		(symbol "4075_2_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "3")
			)
			(pin input line
				(at -12.7 0 0)
				(length 7.62)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "5")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "6")
			)
		)
		(symbol "4075_3_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "11")
			)
			(pin input line
				(at -12.7 0 0)
				(length 7.62)
				(name "~")
				(number "12")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "13")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4077"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "4077"
			(at 3.81 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4077_0_0"
			(text "=1"
				(at 1.524 0 0)
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "Vdd")
				(number "14")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "Vss")
				(number "7")
			)
		)
		(symbol "4077_1_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "3")
			)
		)
		(symbol "4077_2_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "5")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "6")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "4")
			)
		)
		(symbol "4077_3_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "8")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "9")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "10")
			)
		)
		(symbol "4077_4_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "12")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "13")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4078"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 10.16 0)
		)
		(property "Value" "4078"
			(at 5.08 -12.7 0)
		)
		(property "Footprint" ""
			(at 0 -1.27 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/cd4078b.pdf"
			(at 0 -22.86 0)
		)
		(property "Description" "8-input OR/NOR gate"
			(at 0 -20.32 0)
		)
		(property "ki_keywords" "cmos"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DIP*W7.62mm* TSSOP*4.4x5mm* SOIC*3.9x8.7mm*"
			(at 0 0 0)
		)
		(symbol "4078_0_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 3.81)
				(name "Vdd")
				(number "14")
			)
		)
		(symbol "4078_1_0"
			(text "≥1"
				(at 0 -1.27 0)
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 3.81)
				(name "Vss")
				(number "7")
			)
		)
		(symbol "4078_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 5.08)
				(name "~")
				(number "2")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 5.08)
				(name "~")
				(number "3")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 5.08)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -10.16 0 0)
				(length 5.08)
				(name "~")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 5.08)
				(name "~")
				(number "9")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 5.08)
				(name "~")
				(number "10")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 5.08)
				(name "~")
				(number "11")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 5.08)
				(name "~")
				(number "12")
			)
			(pin no_connect line
				(at 5.08 5.08 180)
				(length 3.81)
				(hide yes)
				(name "~")
				(number "8")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 3.81)
				(hide yes)
				(name "~")
				(number "6")
			)
			(pin output line
				(at 10.16 0 180)
				(length 5.08)
				(name "~")
				(number "1")
			)
			(pin output inverted
				(at 10.16 -2.54 180)
				(length 5.08)
				(name "~")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4081"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "4081"
			(at 6.35 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4081_0_0"
			(text "&"
				(at 0.254 0 0)
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "Vdd")
				(number "14")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "Vss")
				(number "7")
			)
		)
		(symbol "4081_1_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "3")
			)
		)
		(symbol "4081_2_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "5")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "6")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "4")
			)
		)
		(symbol "4081_3_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "8")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "9")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "10")
			)
		)
		(symbol "4081_4_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "12")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "13")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4082"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 6.35 0)
		)
		(property "Value" "4082"
			(at 5.08 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4082_0_0"
			(text "&"
				(at 0 0 0)
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vdd")
				(number "14")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "Vss")
				(number "7")
			)
		)
		(symbol "4082_0_1")
		(symbol "4082_1_1"
			(pin input line
				(at -12.7 3.81 0)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin input line
				(at -12.7 1.27 0)
				(length 7.62)
				(name "~")
				(number "3")
			)
			(pin input line
				(at -12.7 -1.27 0)
				(length 7.62)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -12.7 -3.81 0)
				(length 7.62)
				(name "~")
				(number "5")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "1")
			)
		)
		(symbol "4082_2_1"
			(pin input line
				(at -12.7 3.81 0)
				(length 7.62)
				(name "~")
				(number "9")
			)
			(pin input line
				(at -12.7 1.27 0)
				(length 7.62)
				(name "~")
				(number "10")
			)
			(pin input line
				(at -12.7 -1.27 0)
				(length 7.62)
				(name "~")
				(number "11")
			)
			(pin input line
				(at -12.7 -3.81 0)
				(length 7.62)
				(name "~")
				(number "12")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4093"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "4093"
			(at 5.08 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4093_0_0"
			(text "&"
				(at 0.508 0 0)
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vdd")
				(number "14")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "Vss")
				(number "7")
			)
		)
		(symbol "4093_1_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "3")
			)
		)
		(symbol "4093_2_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "5")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "6")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "4")
			)
		)
		(symbol "4093_3_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "8")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "9")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "10")
			)
		)
		(symbol "4093_4_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "12")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "13")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4095"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 13.97 0)
		)
		(property "Value" "4095"
			(at 7.62 -12.7 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4095_0_0"
			(text "&"
				(at -2.54 0 0)
			)
			(text "&"
				(at -2.54 -7.62 0)
			)
			(text "J"
				(at 0 0 0)
			)
			(text "K"
				(at 0 -7.62 0)
			)
		)
		(symbol "4095_0_1")
		(symbol "4095_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 7.62)
				(name "S")
				(number "13")
			)
			(pin input clock
				(at -12.7 7.62 0)
				(length 7.62)
				(name "CK")
				(number "12")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 7.62)
				(name "R")
				(number "2")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "J1")
				(number "3")
			)
			(pin input line
				(at -12.7 0 0)
				(length 7.62)
				(name "J2")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "J3")
				(number "5")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 7.62)
				(name "K1")
				(number "11")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 7.62)
				(name "K2")
				(number "10")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 7.62)
				(name "K3")
				(number "9")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 3.81)
				(name "Vdd")
				(number "14")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 3.81)
				(name "Vss")
				(number "7")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 7.62)
				(name "Q")
				(number "8")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 7.62)
				(name "~{Q}")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4096"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 12.7 0)
		)
		(property "Value" "4096"
			(at 8.89 -12.7 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4096_0_0"
			(text "&"
				(at -1.27 0 0)
			)
			(text "&"
				(at -1.27 -7.62 0)
			)
			(text "J"
				(at 1.27 0 0)
			)
			(text "K"
				(at 1.27 -7.62 0)
			)
		)
		(symbol "4096_0_1")
		(symbol "4096_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 7.62)
				(name "S")
				(number "13")
			)
			(pin input clock
				(at -12.7 7.62 0)
				(length 7.62)
				(name "CK")
				(number "12")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 7.62)
				(name "R")
				(number "2")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "J1")
				(number "3")
			)
			(pin input line
				(at -12.7 0 0)
				(length 7.62)
				(name "J2")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~{J3}")
				(number "5")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 7.62)
				(name "K1")
				(number "11")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 7.62)
				(name "K2")
				(number "10")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 7.62)
				(name "~{K3}")
				(number "9")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 3.81)
				(name "Vdd")
				(number "14")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 3.81)
				(name "Vss")
				(number "7")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 7.62)
				(name "Q")
				(number "8")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 7.62)
				(name "~{Q}")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4099"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 19.05 0)
		)
		(property "Value" "4099"
			(at 7.62 -17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4099_0_1")
		(symbol "4099_1_1"
			(pin input line
				(at -12.7 16.51 0)
				(length 7.62)
				(name "A0")
				(number "5")
			)
			(pin input line
				(at -12.7 13.97 0)
				(length 7.62)
				(name "A1")
				(number "6")
			)
			(pin input line
				(at -12.7 11.43 0)
				(length 7.62)
				(name "A2")
				(number "7")
			)
			(pin input line
				(at -12.7 8.89 0)
				(length 7.62)
				(name "WR")
				(number "4")
			)
			(pin input line
				(at -12.7 6.35 0)
				(length 7.62)
				(name "D")
				(number "3")
			)
			(pin input line
				(at -12.7 3.81 0)
				(length 7.62)
				(name "R")
				(number "2")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "Vdd")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "Vss")
				(number "8")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "Q0")
				(number "9")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 7.62)
				(name "Q1")
				(number "10")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 7.62)
				(name "Q2")
				(number "11")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 7.62)
				(name "Q3")
				(number "12")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 7.62)
				(name "Q4")
				(number "13")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 7.62)
				(name "Q5")
				(number "14")
			)
			(pin output line
				(at 12.7 -15.24 180)
				(length 7.62)
				(name "Q7")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4104"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 8.89 0)
		)
		(property "Value" "4104"
			(at 5.08 -20.32 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4104_0_0")
		(symbol "4104_1_1"
			(pin power_in line
				(at -12.7 13.97 0)
				(length 7.62)
				(name "Vddo")
				(number "1")
			)
			(pin power_in line
				(at -12.7 11.43 0)
				(length 7.62)
				(name "Vss")
				(number "8")
			)
			(pin power_in line
				(at -12.7 8.89 0)
				(length 7.62)
				(name "Vddi")
				(number "16")
			)
			(pin input line
				(at -12.7 6.35 0)
				(length 7.62)
				(name "EN")
				(number "15")
			)
			(pin input line
				(at -12.7 1.27 0)
				(length 7.62)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -12.7 -3.81 0)
				(length 7.62)
				(name "~")
				(number "5")
			)
			(pin input line
				(at -12.7 -8.89 0)
				(length 7.62)
				(name "~")
				(number "11")
			)
			(pin input line
				(at -12.7 -13.97 0)
				(length 7.62)
				(name "~")
				(number "12")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 7.62)
				(name "~")
				(number "3")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 7.62)
				(name "~")
				(number "6")
			)
			(pin output inverted
				(at 12.7 -5.08 180)
				(length 7.62)
				(name "~")
				(number "7")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 7.62)
				(name "~")
				(number "10")
			)
			(pin output inverted
				(at 12.7 -10.16 180)
				(length 7.62)
				(name "~")
				(number "9")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 7.62)
				(name "~")
				(number "13")
			)
			(pin output inverted
				(at 12.7 -15.24 180)
				(length 7.62)
				(name "~")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4160"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.89 8.89 0)
		)
		(property "Value" "4160"
			(at 8.89 -19.05 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4160_0_0"
			(text "1"
				(at 2.54 -7.62 0)
			)
			(text "2"
				(at 2.54 -10.16 0)
			)
			(text "4"
				(at 2.54 -12.7 0)
			)
			(text "8"
				(at 2.54 -15.24 0)
			)
		)
		(symbol "4160_1_1"
			(pin input input_low
				(at -15.24 7.62 0)
				(length 7.62)
				(name "MR")
				(number "1")
			)
			(pin input input_low
				(at -15.24 5.08 0)
				(length 7.62)
				(name "PE")
				(number "9")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 7.62)
				(name "CET")
				(number "10")
			)
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "CEP")
				(number "7")
			)
			(pin input clock
				(at -15.24 -2.54 0)
				(length 7.62)
				(name "CP")
				(number "2")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 7.62)
				(name "P0")
				(number "3")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 7.62)
				(name "P1")
				(number "4")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 7.62)
				(name "P2")
				(number "5")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 7.62)
				(name "P3")
				(number "6")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 3.81)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "8")
			)
			(pin output line
				(at 15.24 3.81 180)
				(length 7.62)
				(name "TC")
				(number "15")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 7.62)
				(name "Q0")
				(number "14")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 7.62)
				(name "Q1")
				(number "13")
			)
			(pin output line
				(at 15.24 -12.7 180)
				(length 7.62)
				(name "Q2")
				(number "12")
			)
			(pin output line
				(at 15.24 -15.24 180)
				(length 7.62)
				(name "Q3")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4161"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.89 8.89 0)
		)
		(property "Value" "4161"
			(at 8.89 -19.05 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4161_0_0"
			(text "1"
				(at 2.54 -7.62 0)
			)
			(text "2"
				(at 2.54 -10.16 0)
			)
			(text "4"
				(at 2.54 -12.7 0)
			)
			(text "8"
				(at 2.54 -15.24 0)
			)
		)
		(symbol "4161_1_1"
			(pin input input_low
				(at -15.24 7.62 0)
				(length 7.62)
				(name "MR")
				(number "1")
			)
			(pin input input_low
				(at -15.24 5.08 0)
				(length 7.62)
				(name "PE")
				(number "9")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 7.62)
				(name "CET")
				(number "10")
			)
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "CEP")
				(number "7")
			)
			(pin input clock
				(at -15.24 -2.54 0)
				(length 7.62)
				(name "CP")
				(number "2")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 7.62)
				(name "P0")
				(number "3")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 7.62)
				(name "P1")
				(number "4")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 7.62)
				(name "P2")
				(number "5")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 7.62)
				(name "P3")
				(number "6")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 3.81)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "8")
			)
			(pin output line
				(at 15.24 3.81 180)
				(length 7.62)
				(name "TC")
				(number "15")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 7.62)
				(name "Q0")
				(number "14")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 7.62)
				(name "Q1")
				(number "13")
			)
			(pin output line
				(at 15.24 -12.7 180)
				(length 7.62)
				(name "Q2")
				(number "12")
			)
			(pin output line
				(at 15.24 -15.24 180)
				(length 7.62)
				(name "Q3")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4162"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.89 8.89 0)
		)
		(property "Value" "4162"
			(at 8.89 -19.05 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4162_0_0"
			(text "1"
				(at 2.54 -7.62 0)
			)
			(text "2"
				(at 2.54 -10.16 0)
			)
			(text "4"
				(at 2.54 -12.7 0)
			)
			(text "8"
				(at 2.54 -15.24 0)
			)
		)
		(symbol "4162_1_1"
			(pin input input_low
				(at -15.24 7.62 0)
				(length 7.62)
				(name "MR")
				(number "1")
			)
			(pin input input_low
				(at -15.24 5.08 0)
				(length 7.62)
				(name "PE")
				(number "9")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 7.62)
				(name "CET")
				(number "10")
			)
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "CEP")
				(number "7")
			)
			(pin input clock
				(at -15.24 -2.54 0)
				(length 7.62)
				(name "CP")
				(number "2")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 7.62)
				(name "P0")
				(number "3")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 7.62)
				(name "P1")
				(number "4")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 7.62)
				(name "P2")
				(number "5")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 7.62)
				(name "P3")
				(number "6")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 3.81)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "8")
			)
			(pin output line
				(at 15.24 3.81 180)
				(length 7.62)
				(name "TC")
				(number "15")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 7.62)
				(name "Q0")
				(number "14")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 7.62)
				(name "Q1")
				(number "13")
			)
			(pin output line
				(at 15.24 -12.7 180)
				(length 7.62)
				(name "Q2")
				(number "12")
			)
			(pin output line
				(at 15.24 -15.24 180)
				(length 7.62)
				(name "Q3")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4163"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.89 10.16 0)
		)
		(property "Value" "4163"
			(at 8.89 -17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4163_0_0"
			(text "1"
				(at 2.54 -6.35 0)
			)
			(text "2"
				(at 2.54 -8.89 0)
			)
			(text "4"
				(at 2.54 -11.43 0)
			)
			(text "8"
				(at 2.54 -13.97 0)
			)
		)
		(symbol "4163_1_1"
			(pin input input_low
				(at -15.24 8.89 0)
				(length 7.62)
				(name "MR")
				(number "1")
			)
			(pin input input_low
				(at -15.24 6.35 0)
				(length 7.62)
				(name "PE")
				(number "9")
			)
			(pin input line
				(at -15.24 3.81 0)
				(length 7.62)
				(name "CET")
				(number "10")
			)
			(pin input line
				(at -15.24 1.27 0)
				(length 7.62)
				(name "CEP")
				(number "7")
			)
			(pin input clock
				(at -15.24 -1.27 0)
				(length 7.62)
				(name "CP")
				(number "2")
			)
			(pin input line
				(at -15.24 -6.35 0)
				(length 7.62)
				(name "P0")
				(number "3")
			)
			(pin input line
				(at -15.24 -8.89 0)
				(length 7.62)
				(name "P1")
				(number "4")
			)
			(pin input line
				(at -15.24 -11.43 0)
				(length 7.62)
				(name "P2")
				(number "5")
			)
			(pin input line
				(at -15.24 -13.97 0)
				(length 7.62)
				(name "P3")
				(number "6")
			)
			(pin power_in line
				(at 0 16.51 270)
				(length 3.81)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -19.05 90)
				(length 3.81)
				(name "VSS")
				(number "8")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 7.62)
				(name "TC")
				(number "15")
			)
			(pin output line
				(at 15.24 -6.35 180)
				(length 7.62)
				(name "Q0")
				(number "14")
			)
			(pin output line
				(at 15.24 -8.89 180)
				(length 7.62)
				(name "Q1")
				(number "13")
			)
			(pin output line
				(at 15.24 -11.43 180)
				(length 7.62)
				(name "Q2")
				(number "12")
			)
			(pin output line
				(at 15.24 -13.97 180)
				(length 7.62)
				(name "Q3")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4174"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 8.89 0)
		)
		(property "Value" "4174"
			(at 7.62 -11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4174_0_0"
			(pin input line
				(at -12.7 10.16 0)
				(length 7.62)
				(name "~{R}")
				(number "1")
			)
			(pin input clock
				(at -12.7 7.62 0)
				(length 7.62)
				(name "Ck")
				(number "9")
			)
			(pin power_in line
				(at 0 16.51 270)
				(length 3.81)
				(name "Vdd")
				(number "16")
			)
			(pin power_in line
				(at 0 -13.97 90)
				(length 3.81)
				(name "Vss")
				(number "8")
			)
		)
		(symbol "4174_0_1")
		(symbol "4174_1_0"
			(pin input line
				(at -12.7 3.81 0)
				(length 7.62)
				(name "~")
				(number "3")
			)
			(pin input line
				(at -12.7 1.27 0)
				(length 7.62)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -12.7 -1.27 0)
				(length 7.62)
				(name "~")
				(number "6")
			)
			(pin input line
				(at -12.7 -3.81 0)
				(length 7.62)
				(name "~")
				(number "11")
			)
			(pin input line
				(at -12.7 -6.35 0)
				(length 7.62)
				(name "~")
				(number "13")
			)
			(pin input line
				(at -12.7 -8.89 0)
				(length 7.62)
				(name "~")
				(number "14")
			)
			(pin output line
				(at 12.7 3.81 180)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin output line
				(at 12.7 1.27 180)
				(length 7.62)
				(name "~")
				(number "5")
			)
			(pin output line
				(at 12.7 -1.27 180)
				(length 7.62)
				(name "~")
				(number "7")
			)
			(pin output line
				(at 12.7 -3.81 180)
				(length 7.62)
				(name "~")
				(number "10")
			)
			(pin output line
				(at 12.7 -6.35 180)
				(length 7.62)
				(name "~")
				(number "12")
			)
			(pin output line
				(at 12.7 -8.89 180)
				(length 7.62)
				(name "~")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4175"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 11.43 0)
		)
		(property "Value" "4175"
			(at 7.62 -15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4175_0_1")
		(symbol "4175_1_0"
			(pin input line
				(at -12.7 11.43 0)
				(length 7.62)
				(name "~{R}")
				(number "1")
			)
			(pin input clock
				(at -12.7 8.89 0)
				(length 7.62)
				(name "Ck")
				(number "9")
			)
			(pin input line
				(at -12.7 3.81 0)
				(length 7.62)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -12.7 -1.27 0)
				(length 7.62)
				(name "~")
				(number "5")
			)
			(pin input line
				(at -12.7 -6.35 0)
				(length 7.62)
				(name "~")
				(number "12")
			)
			(pin input line
				(at -12.7 -11.43 0)
				(length 7.62)
				(name "~")
				(number "13")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "Vdd")
				(number "16")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 3.81)
				(name "Vss")
				(number "8")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin output inverted
				(at 12.7 2.54 180)
				(length 7.62)
				(name "~")
				(number "3")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "7")
			)
			(pin output inverted
				(at 12.7 -2.54 180)
				(length 7.62)
				(name "~")
				(number "6")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 7.62)
				(name "~")
				(number "10")
			)
			(pin output inverted
				(at 12.7 -7.62 180)
				(length 7.62)
				(name "~")
				(number "11")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 7.62)
				(name "~")
				(number "15")
			)
			(pin output inverted
				(at 12.7 -12.7 180)
				(length 7.62)
				(name "~")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4502"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 13.97 0)
		)
		(property "Value" "4502"
			(at 6.35 -10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4502_0_0"
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "Vdd")
				(number "16")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "Vss")
				(number "8")
			)
		)
		(symbol "4502_1_1"
			(pin input line
				(at -15.24 12.7 0)
				(length 7.62)
				(name "~{EN}")
				(number "4")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 7.62)
				(name "~{V1}")
				(number "12")
			)
			(pin input line
				(at -15.24 6.35 0)
				(length 7.62)
				(name "A1")
				(number "3")
			)
			(pin input line
				(at -15.24 3.81 0)
				(length 7.62)
				(name "A2")
				(number "6")
			)
			(pin input line
				(at -15.24 1.27 0)
				(length 7.62)
				(name "A3")
				(number "1")
			)
			(pin input line
				(at -15.24 -1.27 0)
				(length 7.62)
				(name "A4")
				(number "10")
			)
			(pin input line
				(at -15.24 -3.81 0)
				(length 7.62)
				(name "A5")
				(number "13")
			)
			(pin input line
				(at -15.24 -6.35 0)
				(length 7.62)
				(name "A6")
				(number "15")
			)
			(pin output line
				(at 10.16 6.35 180)
				(length 3.81)
				(name "~{Y1}")
				(number "5")
			)
			(pin output line
				(at 10.16 3.81 180)
				(length 3.81)
				(name "~{Y2}")
				(number "7")
			)
			(pin output line
				(at 10.16 1.27 180)
				(length 3.81)
				(name "~{Y3}")
				(number "2")
			)
			(pin output line
				(at 10.16 -1.27 180)
				(length 3.81)
				(name "~{Y4}")
				(number "9")
			)
			(pin output line
				(at 10.16 -3.81 180)
				(length 3.81)
				(name "~{Y5}")
				(number "11")
			)
			(pin output line
				(at 10.16 -6.35 180)
				(length 3.81)
				(name "~{Y6}")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4504"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 12.7 0)
		)
		(property "Value" "4504"
			(at 2.54 -15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/cd4504b.pdf"
			(at 0 0 0)
		)
		(property "Description" "4504 Hex Voltage-level Shifter"
			(at 0 0 0)
		)
		(property "ki_keywords" "cmos, level converter"
			(at 0 0 0)
		)
		(symbol "4504_0_0"
			(text "1"
				(at 0 0 0)
			)
		)
		(symbol "4504_1_1"
			(pin power_in line
				(at -12.7 11.43 0)
				(length 7.62)
				(name "Vdd")
				(number "16")
			)
			(pin power_in line
				(at -12.7 8.89 0)
				(length 7.62)
				(name "Vcc")
				(number "1")
			)
			(pin power_in line
				(at -12.7 6.35 0)
				(length 7.62)
				(name "Vss")
				(number "8")
			)
			(pin input line
				(at -12.7 3.81 0)
				(length 7.62)
				(name "EN")
				(number "13")
			)
			(pin input line
				(at -12.7 0 0)
				(length 7.62)
				(name "~")
				(number "3")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "5")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 7.62)
				(name "~")
				(number "7")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 7.62)
				(name "~")
				(number "9")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 7.62)
				(name "~")
				(number "11")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 7.62)
				(name "~")
				(number "14")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 7.62)
				(name "~")
				(number "4")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 7.62)
				(name "~")
				(number "6")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 7.62)
				(name "~")
				(number "10")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 7.62)
				(name "~")
				(number "12")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 7.62)
				(name "~")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4507"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "4507"
			(at 6.35 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4507_0_0"
			(text "=1"
				(at 0.254 0 0)
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "Vdd")
				(number "14")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "Vss")
				(number "7")
			)
		)
		(symbol "4507_1_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "3")
			)
		)
		(symbol "4507_2_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "5")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "6")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "4")
			)
		)
		(symbol "4507_3_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "8")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "9")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "10")
			)
		)
		(symbol "4507_4_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "12")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "13")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4508"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 8.89 0)
		)
		(property "Value" "4508"
			(at 6.35 -11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4508_0_1"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "Vdd")
				(number "24")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "Vss")
				(number "12")
			)
		)
		(symbol "4508_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 3.81)
				(name "~{EN}")
				(number "3")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 3.81)
				(name "MR")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 3.81)
				(name "ST")
				(number "2")
			)
			(pin input line
				(at -10.16 -1.27 0)
				(length 3.81)
				(name "D0")
				(number "4")
			)
			(pin input line
				(at -10.16 -3.81 0)
				(length 3.81)
				(name "D1")
				(number "6")
			)
			(pin input line
				(at -10.16 -6.35 0)
				(length 3.81)
				(name "D2")
				(number "8")
			)
			(pin input line
				(at -10.16 -8.89 0)
				(length 3.81)
				(name "D3")
				(number "10")
			)
			(pin output line
				(at 10.16 -1.27 180)
				(length 3.81)
				(name "Q0")
				(number "5")
			)
			(pin output line
				(at 10.16 -3.81 180)
				(length 3.81)
				(name "Q1")
				(number "7")
			)
			(pin output line
				(at 10.16 -6.35 180)
				(length 3.81)
				(name "Q2")
				(number "9")
			)
			(pin output line
				(at 10.16 -8.89 180)
				(length 3.81)
				(name "Q3")
				(number "11")
			)
		)
		(symbol "4508_2_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 3.81)
				(name "~{EN}")
				(number "15")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 3.81)
				(name "MR")
				(number "13")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 3.81)
				(name "ST")
				(number "14")
			)
			(pin input line
				(at -10.16 -1.27 0)
				(length 3.81)
				(name "D0")
				(number "16")
			)
			(pin input line
				(at -10.16 -3.81 0)
				(length 3.81)
				(name "D1")
				(number "18")
			)
			(pin input line
				(at -10.16 -6.35 0)
				(length 3.81)
				(name "D2")
				(number "20")
			)
			(pin input line
				(at -10.16 -8.89 0)
				(length 3.81)
				(name "D3")
				(number "22")
			)
			(pin output line
				(at 10.16 -1.27 180)
				(length 3.81)
				(name "Q0")
				(number "17")
			)
			(pin output line
				(at 10.16 -3.81 180)
				(length 3.81)
				(name "Q1")
				(number "19")
			)
			(pin output line
				(at 10.16 -6.35 180)
				(length 3.81)
				(name "Q2")
				(number "21")
			)
			(pin output line
				(at 10.16 -8.89 180)
				(length 3.81)
				(name "Q3")
				(number "23")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4510"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0.508 15.24 0)
		)
		(property "Value" "4510"
			(at 1.27 -15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4510_0_1")
		(symbol "4510_1_1"
			(pin input line
				(at -15.24 11.43 0)
				(length 7.62)
				(name "A1")
				(number "4")
			)
			(pin input line
				(at -15.24 8.89 0)
				(length 7.62)
				(name "A2")
				(number "12")
			)
			(pin input line
				(at -15.24 6.35 0)
				(length 7.62)
				(name "A3")
				(number "13")
			)
			(pin input line
				(at -15.24 3.81 0)
				(length 7.62)
				(name "A4")
				(number "3")
			)
			(pin input line
				(at -15.24 -1.27 0)
				(length 7.62)
				(name "~{Cin}")
				(number "5")
			)
			(pin input line
				(at -15.24 -3.81 0)
				(length 7.62)
				(name "U/D")
				(number "10")
			)
			(pin input clock
				(at -15.24 -6.35 0)
				(length 7.62)
				(name "CLK")
				(number "15")
			)
			(pin input line
				(at -15.24 -8.89 0)
				(length 7.62)
				(name "PE")
				(number "1")
			)
			(pin input line
				(at -15.24 -11.43 0)
				(length 7.62)
				(name "RST")
				(number "9")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "Vdd")
				(number "16")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "Vss")
				(number "8")
			)
			(pin output line
				(at 15.24 11.43 180)
				(length 7.62)
				(name "Q1")
				(number "6")
			)
			(pin output line
				(at 15.24 8.89 180)
				(length 7.62)
				(name "Q2")
				(number "11")
			)
			(pin output line
				(at 15.24 6.35 180)
				(length 7.62)
				(name "Q3")
				(number "14")
			)
			(pin output line
				(at 15.24 3.81 180)
				(length 7.62)
				(name "Q4")
				(number "2")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 7.62)
				(name "~{Cout}")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4511"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.89 11.43 0)
		)
		(property "Value" "4511"
			(at 8.89 -11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4511_0_1")
		(symbol "4511_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 3.81)
				(name "~{EL}")
				(number "5")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 3.81)
				(name "DA")
				(number "7")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 3.81)
				(name "DB")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 3.81)
				(name "DC")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 3.81)
				(name "DD")
				(number "6")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 3.81)
				(name "~{LT}")
				(number "3")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 3.81)
				(name "~{BI}")
				(number "4")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "Vdd")
				(number "16")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "Vss")
				(number "8")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 3.81)
				(name "Qa")
				(number "13")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 3.81)
				(name "Qb")
				(number "12")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 3.81)
				(name "Qc")
				(number "11")
			)
			(pin output line
				(at 10.16 0 180)
				(length 3.81)
				(name "Qd")
				(number "10")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 3.81)
				(name "Qe")
				(number "9")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 3.81)
				(name "Qf")
				(number "15")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 3.81)
				(name "Qg")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4512"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 10.16 12.7 0)
		)
		(property "Value" "4512"
			(at 11.43 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4512_0_1")
		(symbol "4512_1_1"
			(pin input line
				(at -10.16 15.24 0)
				(length 3.81)
				(name "~{EN}")
				(number "15")
			)
			(pin input line
				(at -10.16 12.7 0)
				(length 3.81)
				(name "~{E}")
				(number "10")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 3.81)
				(name "S0")
				(number "11")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 3.81)
				(name "S1")
				(number "12")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 3.81)
				(name "S2")
				(number "13")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 3.81)
				(name "I0")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 3.81)
				(name "I1")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 3.81)
				(name "I2")
				(number "3")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 3.81)
				(name "I3")
				(number "4")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 3.81)
				(name "I4")
				(number "5")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 3.81)
				(name "I5")
				(number "6")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 3.81)
				(name "I6")
				(number "7")
			)
			(pin input line
				(at -10.16 -15.24 0)
				(length 3.81)
				(name "I7")
				(number "9")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "Vdd")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "Vss")
				(number "8")
			)
			(pin output line
				(at 10.16 0 180)
				(length 3.81)
				(name "Q")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4514"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 21.59 0)
		)
		(property "Value" "4514"
			(at 7.62 -22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4514_0_1")
		(symbol "4514_1_1"
			(pin input line
				(at -15.24 13.97 0)
				(length 7.62)
				(name "EL")
				(number "1")
			)
			(pin input line
				(at -15.24 3.81 0)
				(length 7.62)
				(name "A0")
				(number "2")
			)
			(pin input line
				(at -15.24 1.27 0)
				(length 7.62)
				(name "A1")
				(number "3")
			)
			(pin input line
				(at -15.24 -1.27 0)
				(length 7.62)
				(name "A2")
				(number "21")
			)
			(pin input line
				(at -15.24 -3.81 0)
				(length 7.62)
				(name "A3")
				(number "22")
			)
			(pin input line
				(at -15.24 -13.97 0)
				(length 7.62)
				(name "~{EN}")
				(number "23")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "Vdd")
				(number "24")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "Vss")
				(number "12")
			)
			(pin output line
				(at 15.24 19.05 180)
				(length 7.62)
				(name "Q0")
				(number "11")
			)
			(pin output line
				(at 15.24 16.51 180)
				(length 7.62)
				(name "Q1")
				(number "9")
			)
			(pin output line
				(at 15.24 13.97 180)
				(length 7.62)
				(name "Q2")
				(number "10")
			)
			(pin output line
				(at 15.24 11.43 180)
				(length 7.62)
				(name "Q3")
				(number "8")
			)
			(pin output line
				(at 15.24 8.89 180)
				(length 7.62)
				(name "Q4")
				(number "7")
			)
			(pin output line
				(at 15.24 6.35 180)
				(length 7.62)
				(name "Q5")
				(number "6")
			)
			(pin output line
				(at 15.24 3.81 180)
				(length 7.62)
				(name "Q6")
				(number "5")
			)
			(pin output line
				(at 15.24 1.27 180)
				(length 7.62)
				(name "Q7")
				(number "4")
			)
			(pin output line
				(at 15.24 -1.27 180)
				(length 7.62)
				(name "Q8")
				(number "18")
			)
			(pin output line
				(at 15.24 -3.81 180)
				(length 7.62)
				(name "Q9")
				(number "17")
			)
			(pin output line
				(at 15.24 -6.35 180)
				(length 7.62)
				(name "Q10")
				(number "20")
			)
			(pin output line
				(at 15.24 -8.89 180)
				(length 7.62)
				(name "Q11")
				(number "19")
			)
			(pin output line
				(at 15.24 -11.43 180)
				(length 7.62)
				(name "Q12")
				(number "14")
			)
			(pin output line
				(at 15.24 -13.97 180)
				(length 7.62)
				(name "Q13")
				(number "13")
			)
			(pin output line
				(at 15.24 -16.51 180)
				(length 7.62)
				(name "Q14")
				(number "16")
			)
			(pin output line
				(at 15.24 -19.05 180)
				(length 7.62)
				(name "Q15")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4515"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 24.13 0)
		)
		(property "Value" "4515"
			(at 3.81 -24.13 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4515_0_1")
		(symbol "4515_1_1"
			(pin input line
				(at -15.24 15.24 0)
				(length 7.62)
				(name "EL")
				(number "1")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 7.62)
				(name "A0")
				(number "2")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 7.62)
				(name "A1")
				(number "3")
			)
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "A2")
				(number "21")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 7.62)
				(name "A3")
				(number "22")
			)
			(pin input inverted
				(at -15.24 -15.24 0)
				(length 7.62)
				(name "EN")
				(number "23")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "Vdd")
				(number "24")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "Vss")
				(number "12")
			)
			(pin output inverted
				(at 15.24 20.32 180)
				(length 7.62)
				(name "Q0")
				(number "11")
			)
			(pin output inverted
				(at 15.24 17.78 180)
				(length 7.62)
				(name "Q1")
				(number "9")
			)
			(pin output inverted
				(at 15.24 15.24 180)
				(length 7.62)
				(name "Q2")
				(number "10")
			)
			(pin output inverted
				(at 15.24 12.7 180)
				(length 7.62)
				(name "Q3")
				(number "8")
			)
			(pin output inverted
				(at 15.24 10.16 180)
				(length 7.62)
				(name "Q4")
				(number "7")
			)
			(pin output inverted
				(at 15.24 7.62 180)
				(length 7.62)
				(name "Q5")
				(number "6")
			)
			(pin output inverted
				(at 15.24 5.08 180)
				(length 7.62)
				(name "Q6")
				(number "5")
			)
			(pin output inverted
				(at 15.24 2.54 180)
				(length 7.62)
				(name "Q7")
				(number "4")
			)
			(pin output inverted
				(at 15.24 0 180)
				(length 7.62)
				(name "Q8")
				(number "18")
			)
			(pin output inverted
				(at 15.24 -2.54 180)
				(length 7.62)
				(name "Q9")
				(number "17")
			)
			(pin output inverted
				(at 15.24 -5.08 180)
				(length 7.62)
				(name "Q10")
				(number "20")
			)
			(pin output inverted
				(at 15.24 -7.62 180)
				(length 7.62)
				(name "Q11")
				(number "19")
			)
			(pin output inverted
				(at 15.24 -10.16 180)
				(length 7.62)
				(name "Q12")
				(number "14")
			)
			(pin output inverted
				(at 15.24 -12.7 180)
				(length 7.62)
				(name "Q13")
				(number "13")
			)
			(pin output inverted
				(at 15.24 -15.24 180)
				(length 7.62)
				(name "Q14")
				(number "16")
			)
			(pin output inverted
				(at 15.24 -17.78 180)
				(length 7.62)
				(name "Q15")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4518"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 8.89 0)
		)
		(property "Value" "4518"
			(at 5.08 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4518_0_0"
			(text "1"
				(at -2.54 3.556 0)
			)
		)
		(symbol "4518_0_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "Vdd")
				(number "16")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "Vss")
				(number "8")
			)
		)
		(symbol "4518_1_1"
			(pin input line
				(at -15.24 5.08 0)
				(length 7.62)
				(name "CP0")
				(number "1")
			)
			(pin input inverted
				(at -15.24 2.54 0)
				(length 7.62)
				(name "CP1")
				(number "2")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 7.62)
				(name "MR")
				(number "7")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 7.62)
				(name "Q0")
				(number "3")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 7.62)
				(name "Q1")
				(number "4")
			)
			(pin output line
				(at 15.24 0 180)
				(length 7.62)
				(name "Q2")
				(number "5")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 7.62)
				(name "Q3")
				(number "6")
			)
		)
		(symbol "4518_2_1"
			(pin input line
				(at -15.24 5.08 0)
				(length 7.62)
				(name "CP0")
				(number "9")
			)
			(pin input inverted
				(at -15.24 2.54 0)
				(length 7.62)
				(name "CP1")
				(number "10")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 7.62)
				(name "MR")
				(number "15")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 7.62)
				(name "Q0")
				(number "11")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 7.62)
				(name "Q1")
				(number "12")
			)
			(pin output line
				(at 15.24 0 180)
				(length 7.62)
				(name "Q2")
				(number "13")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 7.62)
				(name "Q3")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4520"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 8.89 0)
		)
		(property "Value" "4520"
			(at 6.35 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4520_0_0"
			(text "1"
				(at -2.54 3.556 0)
			)
		)
		(symbol "4520_0_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "Vdd")
				(number "16")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "Vss")
				(number "8")
			)
		)
		(symbol "4520_1_1"
			(pin input line
				(at -15.24 5.08 0)
				(length 7.62)
				(name "CP0")
				(number "1")
			)
			(pin input inverted
				(at -15.24 2.54 0)
				(length 7.62)
				(name "CP1")
				(number "2")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 7.62)
				(name "MR")
				(number "7")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 7.62)
				(name "Q0")
				(number "3")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 7.62)
				(name "Q1")
				(number "4")
			)
			(pin output line
				(at 15.24 0 180)
				(length 7.62)
				(name "Q2")
				(number "5")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 7.62)
				(name "Q3")
				(number "6")
			)
		)
		(symbol "4520_2_1"
			(pin input line
				(at -15.24 5.08 0)
				(length 7.62)
				(name "CP0")
				(number "9")
			)
			(pin input inverted
				(at -15.24 2.54 0)
				(length 7.62)
				(name "CP1")
				(number "10")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 7.62)
				(name "MR")
				(number "15")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 7.62)
				(name "Q0")
				(number "11")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 7.62)
				(name "Q1")
				(number "12")
			)
			(pin output line
				(at 15.24 0 180)
				(length 7.62)
				(name "Q2")
				(number "13")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 7.62)
				(name "Q3")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4529"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 21.59 0)
		)
		(property "Value" "4529"
			(at 5.08 -19.05 0)
		)
		(property "Footprint" ""
			(at 0 2.54 0)
		)
		(property "Datasheet" ""
			(at 0 2.54 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4529_0_1")
		(symbol "4529_1_1"
			(pin input line
				(at -15.24 17.78 0)
				(length 7.62)
				(name "X0")
				(number "2")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 7.62)
				(name "X1")
				(number "3")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 7.62)
				(name "X2")
				(number "4")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 7.62)
				(name "X3")
				(number "5")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 7.62)
				(name "Y0")
				(number "14")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 7.62)
				(name "Y1")
				(number "13")
			)
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "Y2")
				(number "12")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 7.62)
				(name "Y3")
				(number "11")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 7.62)
				(name "A")
				(number "6")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 7.62)
				(name "B")
				(number "7")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 7.62)
				(name "STX")
				(number "1")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 7.62)
				(name "STY")
				(number "15")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "VSS")
				(number "8")
			)
			(pin tri_state line
				(at 15.24 15.24 180)
				(length 7.62)
				(name "Z")
				(number "9")
			)
			(pin tri_state line
				(at 15.24 0 180)
				(length 7.62)
				(name "W")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4530"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 7.62 0)
		)
		(property "Value" "4530"
			(at 5.08 -10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4530_0_0"
			(text "M5"
				(at -3.048 0 0)
			)
			(text "=1"
				(at 2.54 -2.54 0)
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 3.81)
				(name "Vdd")
				(number "16")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 3.81)
				(name "Vss")
				(number "8")
			)
		)
		(symbol "4530_0_1")
		(symbol "4530_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin input line
				(at -12.7 0 0)
				(length 7.62)
				(name "~")
				(number "3")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 7.62)
				(name "~")
				(number "5")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 7.62)
				(name "~")
				(number "6")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "Y")
				(number "7")
			)
		)
		(symbol "4530_2_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 7.62)
				(name "~")
				(number "9")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "~")
				(number "10")
			)
			(pin input line
				(at -12.7 0 0)
				(length 7.62)
				(name "~")
				(number "11")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "~")
				(number "12")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 7.62)
				(name "~")
				(number "13")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 7.62)
				(name "~")
				(number "14")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "Y")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4538"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 10.16 0)
		)
		(property "Value" "4538"
			(at 5.08 -10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4538_0_0"
			(text "1"
				(at -2.54 -3.81 0)
			)
		)
		(symbol "4538_0_1")
		(symbol "4538_1_1"
			(pin input line
				(at -15.24 7.62 0)
				(length 7.62)
				(name "Rx")
				(number "2")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 7.62)
				(name "CX")
				(number "1")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 7.62)
				(name "B")
				(number "4")
			)
			(pin input inverted
				(at -15.24 -5.08 0)
				(length 7.62)
				(name "A")
				(number "5")
			)
			(pin input inverted
				(at -5.08 -15.24 90)
				(length 6.35)
				(name "R")
				(number "3")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 3.81)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 6.35)
				(name "VSS")
				(number "8")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 7.62)
				(name "Q")
				(number "6")
			)
			(pin output inverted
				(at 15.24 -5.08 180)
				(length 7.62)
				(name "Q")
				(number "7")
			)
		)
		(symbol "4538_2_1"
			(pin input line
				(at -15.24 7.62 0)
				(length 7.62)
				(name "Rx")
				(number "14")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 7.62)
				(name "CX")
				(number "15")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 7.62)
				(name "B")
				(number "12")
			)
			(pin input inverted
				(at -15.24 -5.08 0)
				(length 7.62)
				(name "A")
				(number "11")
			)
			(pin input inverted
				(at -5.08 -15.24 90)
				(length 6.35)
				(name "R")
				(number "13")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 3.81)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 6.35)
				(name "VSS")
				(number "8")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 7.62)
				(name "Q")
				(number "10")
			)
			(pin output inverted
				(at 15.24 -5.08 180)
				(length 7.62)
				(name "Q")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4539"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.89 10.16 0)
		)
		(property "Value" "4539"
			(at 5.08 -11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4539_0_1"
			(pin input line
				(at -10.16 10.16 0)
				(length 3.81)
				(name "S0")
				(number "14")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 3.81)
				(name "S1")
				(number "2")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 3.81)
				(name "Vdd")
				(number "16")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "Vss")
				(number "8")
			)
		)
		(symbol "4539_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 3.81)
				(name "~{EN}")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 3.81)
				(name "I0")
				(number "6")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 3.81)
				(name "I1")
				(number "5")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 3.81)
				(name "I2")
				(number "4")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 3.81)
				(name "I3")
				(number "3")
			)
			(pin output line
				(at 10.16 -1.27 180)
				(length 3.81)
				(name "Q")
				(number "7")
			)
		)
		(symbol "4539_2_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 3.81)
				(name "~{EN}")
				(number "15")
			)
			(pin input line
				(at -10.16 0 0)
				(length 3.81)
				(name "I0")
				(number "10")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 3.81)
				(name "I1")
				(number "11")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 3.81)
				(name "I2")
				(number "12")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 3.81)
				(name "I3")
				(number "13")
			)
			(pin output line
				(at 10.16 -1.27 180)
				(length 3.81)
				(name "Q")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4543"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.89 11.43 0)
		)
		(property "Value" "4543"
			(at 8.89 -11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4543_0_1")
		(symbol "4543_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 7.62)
				(name "LD")
				(number "1")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 7.62)
				(name "DA")
				(number "5")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "DB")
				(number "3")
			)
			(pin input line
				(at -12.7 0 0)
				(length 7.62)
				(name "DC")
				(number "2")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "DD")
				(number "4")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 7.62)
				(name "PH")
				(number "6")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 7.62)
				(name "BI")
				(number "7")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 3.81)
				(name "Vdd")
				(number "16")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 3.81)
				(name "Vss")
				(number "8")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 7.62)
				(name "Qa")
				(number "9")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 7.62)
				(name "Qb")
				(number "10")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 7.62)
				(name "Qc")
				(number "11")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "Qd")
				(number "12")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 7.62)
				(name "Qe")
				(number "13")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 7.62)
				(name "Qf")
				(number "15")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 7.62)
				(name "Qg")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4555"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 8.89 0)
		)
		(property "Value" "4555"
			(at 6.35 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4555_0_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 3.81)
				(name "Vdd")
				(number "16")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 3.81)
				(name "Vss")
				(number "8")
			)
		)
		(symbol "4555_1_1"
			(pin input line
				(at -10.16 3.81 0)
				(length 3.81)
				(name "A0")
				(number "2")
			)
			(pin input line
				(at -10.16 1.27 0)
				(length 3.81)
				(name "A1")
				(number "3")
			)
			(pin input line
				(at -10.16 -3.81 0)
				(length 3.81)
				(name "~{EN}")
				(number "1")
			)
			(pin output line
				(at 10.16 3.81 180)
				(length 3.81)
				(name "Q0")
				(number "4")
			)
			(pin output line
				(at 10.16 1.27 180)
				(length 3.81)
				(name "Q1")
				(number "5")
			)
			(pin output line
				(at 10.16 -1.27 180)
				(length 3.81)
				(name "Q2")
				(number "6")
			)
			(pin output line
				(at 10.16 -3.81 180)
				(length 3.81)
				(name "Q3")
				(number "7")
			)
		)
		(symbol "4555_2_1"
			(pin input line
				(at -10.16 3.81 0)
				(length 3.81)
				(name "A0")
				(number "14")
			)
			(pin input line
				(at -10.16 1.27 0)
				(length 3.81)
				(name "A1")
				(number "13")
			)
			(pin input line
				(at -10.16 -3.81 0)
				(length 3.81)
				(name "~{EN}")
				(number "15")
			)
			(pin output line
				(at 10.16 3.81 180)
				(length 3.81)
				(name "Q0")
				(number "12")
			)
			(pin output line
				(at 10.16 1.27 180)
				(length 3.81)
				(name "Q1")
				(number "11")
			)
			(pin output line
				(at 10.16 -1.27 180)
				(length 3.81)
				(name "Q2")
				(number "10")
			)
			(pin output line
				(at 10.16 -3.81 180)
				(length 3.81)
				(name "Q3")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4556"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "4556"
			(at 6.35 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4556_0_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 3.81)
				(name "Vdd")
				(number "16")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 3.81)
				(name "Vss")
				(number "8")
			)
		)
		(symbol "4556_1_1"
			(pin input line
				(at -10.16 3.81 0)
				(length 3.81)
				(name "A0")
				(number "2")
			)
			(pin input line
				(at -10.16 1.27 0)
				(length 3.81)
				(name "A1")
				(number "3")
			)
			(pin input line
				(at -10.16 -3.81 0)
				(length 3.81)
				(name "~{EN}")
				(number "1")
			)
			(pin output line
				(at 10.16 3.81 180)
				(length 3.81)
				(name "~{Q0}")
				(number "4")
			)
			(pin output line
				(at 10.16 1.27 180)
				(length 3.81)
				(name "~{Q1}")
				(number "5")
			)
			(pin output line
				(at 10.16 -1.27 180)
				(length 3.81)
				(name "~{Q2}")
				(number "6")
			)
			(pin output line
				(at 10.16 -3.81 180)
				(length 3.81)
				(name "~{Q3}")
				(number "7")
			)
		)
		(symbol "4556_2_1"
			(pin input line
				(at -10.16 3.81 0)
				(length 3.81)
				(name "A0")
				(number "14")
			)
			(pin input line
				(at -10.16 1.27 0)
				(length 3.81)
				(name "A1")
				(number "13")
			)
			(pin input line
				(at -10.16 -3.81 0)
				(length 3.81)
				(name "~{EN}")
				(number "15")
			)
			(pin output line
				(at 10.16 3.81 180)
				(length 3.81)
				(name "~{Q0}")
				(number "12")
			)
			(pin output line
				(at 10.16 1.27 180)
				(length 3.81)
				(name "~{Q1}")
				(number "11")
			)
			(pin output line
				(at 10.16 -1.27 180)
				(length 3.81)
				(name "~{Q2}")
				(number "10")
			)
			(pin output line
				(at 10.16 -3.81 180)
				(length 3.81)
				(name "~{Q3}")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4585"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 15.24 0)
		)
		(property "Value" "4585"
			(at 6.35 -15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4585_0_0"
			(text "A"
				(at -1.27 8.89 0)
			)
			(text "B"
				(at -1.27 -8.89 0)
			)
		)
		(symbol "4585_0_1"
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "Vdd")
				(number "16")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 3.81)
				(name "Vss")
				(number "8")
			)
		)
		(symbol "4585_1_1"
			(pin input line
				(at -10.16 12.7 0)
				(length 3.81)
				(name "A0")
				(number "10")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 3.81)
				(name "A1")
				(number "7")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 3.81)
				(name "A2")
				(number "2")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 3.81)
				(name "A3")
				(number "15")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 3.81)
				(name "Ia<b")
				(number "5")
			)
			(pin input line
				(at -10.16 0 0)
				(length 3.81)
				(name "Ia=b")
				(number "6")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 3.81)
				(name "Ia>b")
				(number "4")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 3.81)
				(name "B0")
				(number "11")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 3.81)
				(name "B1")
				(number "9")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 3.81)
				(name "B2")
				(number "1")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 3.81)
				(name "B3")
				(number "14")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 3.81)
				(name "Qa>b")
				(number "13")
			)
			(pin output line
				(at 10.16 0 180)
				(length 3.81)
				(name "Qa=b")
				(number "3")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 3.81)
				(name "Qa<b")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "40160"
		(extends "4160")
		(property "Reference" "U"
			(at 8.89 8.89 0)
		)
		(property "Value" "40160"
			(at 8.89 -19.05 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
	)
	(symbol "40161"
		(extends "4161")
		(property "Reference" "U"
			(at 8.89 8.89 0)
		)
		(property "Value" "40161"
			(at 8.89 -19.05 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
	)
	(symbol "40162"
		(extends "4162")
		(property "Reference" "U"
			(at 8.89 8.89 0)
		)
		(property "Value" "40162"
			(at 8.89 -19.05 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
	)
	(symbol "40163"
		(extends "4163")
		(property "Reference" "U"
			(at 8.89 10.16 0)
		)
		(property "Value" "40163"
			(at 8.89 -17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
	)
	(symbol "40244"
		(extends "40240")
		(property "Reference" "U"
			(at 7.62 8.89 0)
		)
		(property "Value" "40244"
			(at 8.89 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
	)
	(symbol "4066"
		(extends "4016")
		(property "Reference" "U"
			(at 2.54 5.08 0)
		)
		(property "Value" "4066"
			(at 5.08 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
	)
	(symbol "4528"
		(extends "4538")
		(property "Reference" "U"
			(at 1.27 10.16 0)
		)
		(property "Value" "4528"
			(at 5.08 -10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
	)
	(symbol "4584"
		(extends "40106")
		(property "Reference" "U"
			(at 5.08 5.08 0)
		)
		(property "Value" "4584"
			(at 1.27 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
	)
)
