(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "74AHC1G4210"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "74AHC1G4210"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74AHC1G4210.pdf"
			(at 0 0 0)
		)
		(property "Description" "10-stage divider and oscillator, SOT353-1"
			(at 0 0 0)
		)
		(property "ki_keywords" "divider oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*353*"
			(at 0 0 0)
		)
		(symbol "74AHC1G4210_0_1")
		(symbol "74AHC1G4210_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 5.08)
				(name "X1")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 5.08)
				(name "X2")
				(number "2")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 10.16 0 180)
				(length 5.08)
				(name "Q")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74AUC1G74"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 10.16 0)
		)
		(property "Value" "74AUC1G74"
			(at 10.16 -10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single D Flip-Flop, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single D Flip-Flop D CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP* VSSOP*"
			(at 0 0 0)
		)
		(symbol "74AUC1G74_0_1")
		(symbol "74AUC1G74_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "D")
				(number "2")
			)
			(pin input clock
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "C")
				(number "1")
			)
			(pin input line
				(at -2.54 12.7 270)
				(length 5.08)
				(name "~{PRE}")
				(number "7")
			)
			(pin input line
				(at -2.54 -12.7 90)
				(length 5.08)
				(name "~{CLR}")
				(number "6")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q")
				(number "5")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "~{Q}")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74CBT1G125"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 10.16 0)
		)
		(property "Value" "74CBT1G125"
			(at 0 -10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single FET Bus Switch"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single FET Bus Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SC*"
			(at 0 0 0)
		)
		(symbol "74CBT1G125_0_1")
		(symbol "74CBT1G125_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "A")
				(number "2")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "~{OE}")
				(number "1")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "3")
			)
			(pin tri_state line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "B")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74CBT1G384"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 10.16 0)
		)
		(property "Value" "74CBT1G384"
			(at 0 -10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single FET Bus Switch"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single FET Bus Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SC*"
			(at 0 0 0)
		)
		(symbol "74CBT1G384_0_1")
		(symbol "74CBT1G384_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "A")
				(number "1")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "~{OE}")
				(number "4")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "3")
			)
			(pin tri_state line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "B")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC1G00"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 7.62 0)
		)
		(property "Value" "74LVC1G00"
			(at 7.62 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lvc1g00.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single NAND Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate NAND LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* Texas?R-PDSO-G5?DCK* Texas?R-PDSO-N5?DRL* Texas?X2SON*0.8x0.8mm*P0.48mm*"
			(at 0 0 0)
		)
		(symbol "74LVC1G00_0_1")
		(symbol "74LVC1G00_1_1"
			(pin input line
				(at -15.24 2.54 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "3")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC1G02"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 7.62 0)
		)
		(property "Value" "74LVC1G02"
			(at 7.62 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lvc1g02.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single NOR Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate NOR LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* Texas?R-PDSO-G5?DCK* Texas?R-PDSO-N5?DRL* Texas?X2SON*0.8x0.8mm*P0.48mm*"
			(at 0 0 0)
		)
		(symbol "74LVC1G02_0_1")
		(symbol "74LVC1G02_1_1"
			(pin input line
				(at -15.24 2.54 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "3")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC1G04"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "74LVC1G04"
			(at 5.08 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lvc1g04.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single NOT Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate NOT LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* Texas?R-PDSO-G5?DCK* Texas?R-PDSO-N5?DRL* Texas?X2SON*0.8x0.8mm*P0.48mm*"
			(at 0 0 0)
		)
		(symbol "74LVC1G04_0_1")
		(symbol "74LVC1G04_1_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin power_in line
				(at -5.08 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at -5.08 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "3")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC1G06"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "74LVC1G06"
			(at 2.54 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single NOT Gate, Open Drain, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate NOT LVC CMOS Open Drain"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
		(symbol "74LVC1G06_0_1")
		(symbol "74LVC1G06_1_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin power_in line
				(at -5.08 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at -5.08 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "3")
			)
			(pin open_collector inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC1G07"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "74LVC1G07"
			(at 3.81 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lvc1g07.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Buffer Gate, Open Drain, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate Buff LVC CMOS Open Drain"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* Texas?R-PDSO-G5?DCK* Texas?R-PDSO-N5?DRL* Texas?X2SON*0.8x0.8mm*P0.48mm*"
			(at 0 0 0)
		)
		(symbol "74LVC1G07_0_1")
		(symbol "74LVC1G07_1_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin power_in line
				(at -5.08 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at -5.08 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "3")
			)
			(pin free line
				(at -2.54 -10.16 90)
				(length 6.35)
				(name "NC")
				(number "1")
			)
			(pin open_collector line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC1G08"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 7.62 0)
		)
		(property "Value" "74LVC1G08"
			(at 7.62 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lvc1g08.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single AND Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate AND LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* Texas?R-PDSO-G5?DCK* Texas?R-PDSO-N5?DRL* Texas?X2SON*0.8x0.8mm*P0.48mm*"
			(at 0 0 0)
		)
		(symbol "74LVC1G08_0_1")
		(symbol "74LVC1G08_1_1"
			(pin input line
				(at -15.24 2.54 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC1G0832"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 10.16 0)
		)
		(property "Value" "74LVC1G0832"
			(at 0 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single AND-OR Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate AND-OR LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
		(symbol "74LVC1G0832_0_1")
		(symbol "74LVC1G0832_1_1"
			(pin input line
				(at -17.78 5.08 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -17.78 0 0)
				(length 7.62)
				(name "~")
				(number "3")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 7.62)
				(name "~")
				(number "6")
			)
			(pin power_in line
				(at 5.08 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 5.08 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 20.32 0 180)
				(length 7.62)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC1G10"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 10.16 0)
		)
		(property "Value" "74LVC1G10"
			(at 7.62 -10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single NAND 3-Input Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate NAND triple LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
		(symbol "74LVC1G10_0_1")
		(symbol "74LVC1G10_1_1"
			(pin input line
				(at -15.24 5.08 0)
				(length 7.62)
				(name "~")
				(number "6")
			)
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 7.62)
				(name "~")
				(number "3")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 3.81)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 3.81)
				(name "GND")
				(number "2")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 6.35)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC1G11"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 10.16 0)
		)
		(property "Value" "74LVC1G11"
			(at 7.62 -10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single AND 3-Input Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate AND triple LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
		(symbol "74LVC1G11_0_1")
		(symbol "74LVC1G11_1_1"
			(pin input line
				(at -15.24 5.08 0)
				(length 7.62)
				(name "~")
				(number "6")
			)
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 7.62)
				(name "~")
				(number "3")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 3.81)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 3.81)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 12.7 0 180)
				(length 6.35)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC1G123"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "74LVC1G123"
			(at 3.81 8.89 0)
		)
		(property "Footprint" ""
			(at 0 -2.54 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74lvc1g123.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Retriggerable Monostable Multivibrator, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Mono Multivibrator CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*2.95x2.8mm*P0.65* VSSOP*2.3x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "74LVC1G123_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "RCext")
				(number "7")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "Cext")
				(number "6")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "~{A}")
				(number "1")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "B")
				(number "2")
			)
			(pin input line
				(at 0 -12.7 90)
				(length 5.08)
				(name "~{CLR}")
				(number "3")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q")
				(number "5")
			)
		)
		(symbol "74LVC1G123_2_1"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC1G125"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "74LVC1G125"
			(at 2.54 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lvc1g125.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Buffer Gate Tri-State, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate Buff Tri-State LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* Texas?R-PDSO-G5?DCK* Texas?R-PDSO-N5?DRL* Texas?X2SON*0.8x0.8mm*P0.48mm*"
			(at 0 0 0)
		)
		(symbol "74LVC1G125_0_1")
		(symbol "74LVC1G125_1_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin power_in line
				(at -5.08 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at -5.08 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "3")
			)
			(pin input inverted
				(at 0 10.16 270)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin tri_state line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC1G126"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 7.62 0)
		)
		(property "Value" "74LVC1G126"
			(at 2.54 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Buffer Gate Tri-State, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate Buff Tri-State LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
		(symbol "74LVC1G126_0_1")
		(symbol "74LVC1G126_1_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin power_in line
				(at -5.08 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at -5.08 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "3")
			)
			(pin input line
				(at 0 10.16 270)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin tri_state line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC1G139"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 10.16 0)
		)
		(property "Value" "74LVC1G139"
			(at 7.62 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "2 to 4 Decoder, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Decoder LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP* VSSOP*"
			(at 0 0 0)
		)
		(symbol "74LVC1G139_0_1")
		(symbol "74LVC1G139_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 6.35)
				(name "A")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 6.35)
				(name "B")
				(number "2")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 6.35)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 6.35)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 6.35)
				(name "Y0")
				(number "7")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 6.35)
				(name "Y1")
				(number "6")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 6.35)
				(name "Y2")
				(number "5")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 6.35)
				(name "Y3")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC1G14"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 3.81 0)
		)
		(property "Value" "74LVC1G14"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "Single Schmitt NOT Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate NOT Schmitt LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SOT?553*"
			(at 0 0 0)
		)
		(symbol "74LVC1G14_0_1")
		(symbol "74LVC1G14_1_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin no_connect line
				(at -7.62 5.08 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at -5.08 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at -5.08 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "3")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC1G17"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 3.81 0)
		)
		(property "Value" "74LVC1G17"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at -2.54 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lvc1g17.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "Single Schmitt Buffer Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate Buff Schmitt LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SOT?553* Texas?R-PDSO-G5?DCK* Texas?R-PDSO-N5?DRL* Texas?X2SON*0.8x0.8mm*P0.48mm*"
			(at 0 0 0)
		)
		(symbol "74LVC1G17_0_1")
		(symbol "74LVC1G17_1_1"
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "~")
				(number "2")
			)
			(pin no_connect line
				(at -7.62 5.08 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at -5.08 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at -5.08 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 10.16 0 180)
				(length 5.08)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC1G175"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 10.16 0)
		)
		(property "Value" "74LVC1G175"
			(at 10.16 -10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single D Flip-Flop, Asynchronous Clear, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single D Flip-Flop Clear CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SC*"
			(at 0 0 0)
		)
		(symbol "74LVC1G175_0_1")
		(symbol "74LVC1G175_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "D")
				(number "3")
			)
			(pin input clock
				(at -12.7 0 0)
				(length 5.08)
				(name "C")
				(number "1")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "~{CLR}")
				(number "6")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC1G18"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 7.62 0)
		)
		(property "Value" "74LVC1G18"
			(at 7.62 -7.62 0)
		)
		(property "Footprint" ""
			(at -2.54 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Demultiplexer, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Demux LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
		(symbol "74LVC1G18_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 7.62)
				(name "~")
				(number "3")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin tri_state line
				(at 10.16 2.54 180)
				(length 7.62)
				(name "~")
				(number "6")
			)
			(pin tri_state line
				(at 10.16 -2.54 180)
				(length 7.62)
				(name "~")
				(number "4")
			)
		)
		(symbol "74LVC1G18_2_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 7.62)
				(name "GND")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC1G19"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 10.16 0)
		)
		(property "Value" "74LVC1G19"
			(at 7.62 -10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "1 of 2 Decoder, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Decoder LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
		(symbol "74LVC1G19_0_1")
		(symbol "74LVC1G19_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "A")
				(number "1")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "~{E}")
				(number "3")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Y0")
				(number "6")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "Y1")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC1G240"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 7.62 0)
		)
		(property "Value" "74LVC1G240"
			(at 2.54 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Buffer/Driver Gate Tri-State, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate Buff/Drv Tri-State LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
		(symbol "74LVC1G240_0_1")
		(symbol "74LVC1G240_1_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin power_in line
				(at -5.08 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at -5.08 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "3")
			)
			(pin input inverted
				(at 0 10.16 270)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin tri_state inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC1G27"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 10.16 0)
		)
		(property "Value" "74LVC1G27"
			(at 7.62 -10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single NOR 3-Input Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate NOR triple LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG*"
			(at 0 0 0)
		)
		(symbol "74LVC1G27_0_1")
		(symbol "74LVC1G27_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "~")
				(number "6")
			)
			(pin input line
				(at -12.7 0 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "~")
				(number "3")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 3.81)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 3.81)
				(name "GND")
				(number "2")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 6.35)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC1G29"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 10.16 0)
		)
		(property "Value" "74LVC1G29"
			(at 7.62 -10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "2 of 3 Decoder, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Decoder LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP* VSSOP*"
			(at 0 0 0)
		)
		(symbol "74LVC1G29_0_1")
		(symbol "74LVC1G29_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "A1")
				(number "6")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "A2")
				(number "3")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "~{G}")
				(number "1")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Y0")
				(number "7")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "Y1")
				(number "2")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "Y2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC1G3157"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 7.62 0)
		)
		(property "Value" "74LVC1G3157"
			(at 10.16 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "SPDT Analog Switch, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "SPDT Analog Switch CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SC*"
			(at 0 0 0)
		)
		(symbol "74LVC1G3157_1_1"
			(pin bidirectional line
				(at -10.16 0 0)
				(length 5.08)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 5.08)
				(name "~")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 5.08)
				(name "~")
				(number "1")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 5.08)
				(name "~")
				(number "3")
			)
		)
		(symbol "74LVC1G3157_2_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC1G32"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 7.62 0)
		)
		(property "Value" "74LVC1G32"
			(at 7.62 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single OR Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate OR LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
		(symbol "74LVC1G32_0_1")
		(symbol "74LVC1G32_1_1"
			(pin input line
				(at -15.24 2.54 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC1G3208"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 10.16 0)
		)
		(property "Value" "74LVC1G3208"
			(at 0 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single OR-AND Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate OR-AND LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
		(symbol "74LVC1G3208_0_1")
		(symbol "74LVC1G3208_1_1"
			(pin input line
				(at -17.78 5.08 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -17.78 0 0)
				(length 7.62)
				(name "~")
				(number "3")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 7.62)
				(name "~")
				(number "6")
			)
			(pin power_in line
				(at 5.08 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 5.08 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 20.32 0 180)
				(length 7.62)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC1G332"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.112 7.366 0)
		)
		(property "Value" "74LVC1G332"
			(at 6.096 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single OR 3-Input Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate OR triple LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG*"
			(at 0 0 0)
		)
		(symbol "74LVC1G332_0_1")
		(symbol "74LVC1G332_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "~")
				(number "6")
			)
			(pin input line
				(at -12.7 0 0)
				(length 6.35)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "~")
				(number "3")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 3.81)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 3.81)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 12.7 0 180)
				(length 6.35)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC1G34"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "74LVC1G34"
			(at 5.08 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lvc1g34.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Buffer Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate Buff LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* Texas?R-PDSO-G5?DCK* Texas?R-PDSO-N5?DRL* Texas?X2SON*0.8x0.8mm*P0.48mm*"
			(at 0 0 0)
		)
		(symbol "74LVC1G34_0_1")
		(symbol "74LVC1G34_1_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin power_in line
				(at -5.08 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at -5.08 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "3")
			)
			(pin free line
				(at -2.54 -10.16 90)
				(length 6.35)
				(name "NC")
				(number "1")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC1G373"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 10.16 0)
		)
		(property "Value" "74LVC1G373"
			(at 7.62 -10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single D Latch, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single D Latch CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SC*"
			(at 0 0 0)
		)
		(symbol "74LVC1G373_0_1")
		(symbol "74LVC1G373_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "D")
				(number "3")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "LE")
				(number "1")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "2")
			)
			(pin tri_state line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q")
				(number "4")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "~{OE}")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC1G374"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 10.16 0)
		)
		(property "Value" "74LVC1G374"
			(at 7.62 -10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single D Flip-Flop Tri-State Output, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single D Flip-Flop Tri-State CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SC*"
			(at 0 0 0)
		)
		(symbol "74LVC1G374_0_1")
		(symbol "74LVC1G374_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "D")
				(number "3")
			)
			(pin input clock
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "CLK")
				(number "1")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "2")
			)
			(pin tri_state line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q")
				(number "4")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "~{OE}")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC1G38"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 7.62 0)
		)
		(property "Value" "74LVC1G38"
			(at 7.62 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single NAND Gate Open Drain, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate NAND Open Drain LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
		(symbol "74LVC1G38_0_1")
		(symbol "74LVC1G38_1_1"
			(pin input line
				(at -15.24 2.54 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "3")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC1G386"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.382 7.366 0)
		)
		(property "Value" "74LVC1G386"
			(at 6.096 -7.366 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single XOR 3-Input Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate XOR triple LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG*"
			(at 0 0 0)
		)
		(symbol "74LVC1G386_0_1")
		(symbol "74LVC1G386_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 3.81)
				(name "~")
				(number "6")
			)
			(pin input line
				(at -12.7 0 0)
				(length 6.35)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 3.81)
				(name "~")
				(number "3")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 3.81)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 3.81)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 12.7 0 180)
				(length 6.35)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC1G57"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 10.16 0)
		)
		(property "Value" "74LVC1G57"
			(at 7.62 -10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Configurable Multi-Function Single Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Configurable Single Gate LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SC*"
			(at 0 0 0)
		)
		(symbol "74LVC1G57_0_1")
		(symbol "74LVC1G57_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "IN0")
				(number "3")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "IN1")
				(number "1")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "IN2")
				(number "6")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "Y")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC1G58"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 10.16 0)
		)
		(property "Value" "74LVC1G58"
			(at 7.62 -10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Configurable Multi-Function Single Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Configurable Single Gate LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SC*"
			(at 0 0 0)
		)
		(symbol "74LVC1G58_0_1")
		(symbol "74LVC1G58_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "IN0")
				(number "3")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "IN1")
				(number "1")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "IN2")
				(number "6")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "~{Y}")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC1G66"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 7.62 0)
		)
		(property "Value" "74LVC1G66"
			(at 7.62 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74lvc1g66.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Bilateral Analog Switch, SOT-23-5/SC-70-5"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Bilateral Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SC*"
			(at 0 0 0)
		)
		(symbol "74LVC1G66_1_1"
			(pin bidirectional line
				(at -12.7 0 0)
				(length 5.08)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "~")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 6.35)
				(name "~")
				(number "2")
			)
		)
		(symbol "74LVC1G66_2_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC1G79"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 10.16 0)
		)
		(property "Value" "74LVC1G79"
			(at 7.62 -10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single D Flip-Flop, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single D Flip-Flop D CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG*"
			(at 0 0 0)
		)
		(symbol "74LVC1G79_0_1")
		(symbol "74LVC1G79_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "D")
				(number "1")
			)
			(pin input clock
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "C")
				(number "2")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC1G80"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 10.16 0)
		)
		(property "Value" "74LVC1G80"
			(at 7.62 -10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single D Flip-Flop, Inverted Output, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single D Flip-Flop CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG*"
			(at 0 0 0)
		)
		(symbol "74LVC1G80_0_1")
		(symbol "74LVC1G80_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "D")
				(number "1")
			)
			(pin input clock
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "C")
				(number "2")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "~{Q}")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC1G86"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 7.62 0)
		)
		(property "Value" "74LVC1G86"
			(at 7.62 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single XOR Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate XOR LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
		(symbol "74LVC1G86_0_1")
		(symbol "74LVC1G86_1_1"
			(pin input line
				(at -15.24 2.54 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC1G99"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 7.62 0)
		)
		(property "Value" "74LVC1G99"
			(at 1.27 7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/sn74lvc1g99"
			(at 0 11.43 0)
		)
		(property "Description" "Configurable Multi-Function Single Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Configurable Single Gate LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP* VSSOP*"
			(at 0 0 0)
		)
		(symbol "74LVC1G99_0_1")
		(symbol "74LVC1G99_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 5.08)
				(name "~{OE}")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 5.08)
				(name "A")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 5.08)
				(name "B")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 5.08)
				(name "C")
				(number "5")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 5.08)
				(name "D")
				(number "6")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 10.16 0 180)
				(length 5.08)
				(name "Y")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC1GU04DRL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 10.16 0)
		)
		(property "Value" "74LVC1GU04DRL"
			(at 17.78 10.16 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-553"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74lvc1gu04.pdf"
			(at -3.81 0 0)
		)
		(property "Description" "Single Inverter Gate, SOT-553"
			(at 0 0 0)
		)
		(property "ki_keywords" "inverter cmos"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*553*"
			(at 0 0 0)
		)
		(symbol "74LVC1GU04DRL_0_1")
		(symbol "74LVC1GU04DRL_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 5.08)
				(name "~")
				(number "2")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "3")
			)
			(pin no_connect line
				(at 10.16 0 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin output line
				(at 17.78 0 180)
				(length 5.08)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC2G00"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 7.62 0)
		)
		(property "Value" "74LVC2G00"
			(at 7.62 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual NAND Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Gate NAND LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP* VSSOP*"
			(at 0 0 0)
		)
		(symbol "74LVC2G00_1_1"
			(pin input line
				(at -15.24 2.54 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "7")
			)
		)
		(symbol "74LVC2G00_2_1"
			(pin input line
				(at -15.24 2.54 0)
				(length 7.62)
				(name "~")
				(number "5")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 7.62)
				(name "~")
				(number "6")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "3")
			)
		)
		(symbol "74LVC2G00_3_0")
		(symbol "74LVC2G00_3_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC2G02"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 7.62 0)
		)
		(property "Value" "74LVC2G02"
			(at 7.62 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual NOR Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Gate NOR LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP* VSSOP*"
			(at 0 0 0)
		)
		(symbol "74LVC2G02_1_1"
			(pin input line
				(at -15.24 2.54 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "7")
			)
		)
		(symbol "74LVC2G02_2_1"
			(pin input line
				(at -15.24 2.54 0)
				(length 7.62)
				(name "~")
				(number "5")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 7.62)
				(name "~")
				(number "6")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "3")
			)
		)
		(symbol "74LVC2G02_3_0")
		(symbol "74LVC2G02_3_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC2G04"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "74LVC2G04"
			(at 2.54 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual NOT Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Gate NOT LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SG-* SOT*"
			(at 0 0 0)
		)
		(symbol "74LVC2G04_1_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LVC2G04_2_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "~")
				(number "3")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "4")
			)
		)
		(symbol "74LVC2G04_3_0")
		(symbol "74LVC2G04_3_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC2G06"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 7.62 0)
		)
		(property "Value" "74LVC2G06"
			(at 2.54 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual NOT Gate, Open Drain, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Gate NOT Open Drain LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SG-* SOT*"
			(at 0 0 0)
		)
		(symbol "74LVC2G06_1_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin open_collector inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LVC2G06_2_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "~")
				(number "3")
			)
			(pin open_collector inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "4")
			)
		)
		(symbol "74LVC2G06_3_0")
		(symbol "74LVC2G06_3_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC2G07"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "74LVC2G07"
			(at 2.54 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Buffer, Open Drain, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Gate Buffer Open Drain LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SG-* SOT*"
			(at 0 0 0)
		)
		(symbol "74LVC2G07_1_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin open_collector line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LVC2G07_2_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "~")
				(number "3")
			)
			(pin open_collector line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "4")
			)
		)
		(symbol "74LVC2G07_3_0")
		(symbol "74LVC2G07_3_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC2G08"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "74LVC2G08"
			(at -10.16 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual AND Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Gate AND LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP* VSSOP*"
			(at 0 0 0)
		)
		(symbol "74LVC2G08_1_1"
			(pin input line
				(at -15.24 2.54 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "7")
			)
		)
		(symbol "74LVC2G08_2_1"
			(pin input line
				(at -15.24 2.54 0)
				(length 7.62)
				(name "~")
				(number "5")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 7.62)
				(name "~")
				(number "6")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "3")
			)
		)
		(symbol "74LVC2G08_3_0")
		(symbol "74LVC2G08_3_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC2G125"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 7.62 0)
		)
		(property "Value" "74LVC2G125"
			(at 2.54 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Buffer Tri-State, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Buff Tri-State LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*"
			(at 0 0 0)
		)
		(symbol "74LVC2G125_1_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin input inverted
				(at 0 10.16 270)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin tri_state line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LVC2G125_2_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "~")
				(number "5")
			)
			(pin input inverted
				(at 0 10.16 270)
				(length 7.62)
				(name "~")
				(number "7")
			)
			(pin tri_state line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "3")
			)
		)
		(symbol "74LVC2G125_3_0")
		(symbol "74LVC2G125_3_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC2G126"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 7.62 0)
		)
		(property "Value" "74LVC2G126"
			(at 2.54 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Buffer Tri-State, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Buff Tri-State LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*"
			(at 0 0 0)
		)
		(symbol "74LVC2G126_1_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "~")
				(number "1")
			)
			(pin tri_state line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LVC2G126_2_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "~")
				(number "5")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "~")
				(number "7")
			)
			(pin tri_state line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "3")
			)
		)
		(symbol "74LVC2G126_3_0")
		(symbol "74LVC2G126_3_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC2G14"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "74LVC2G14"
			(at 2.54 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lvc2g14.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual NOT Gate, Schmitt Triggered, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Gate NOT Schmitt LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SG-* SOT*"
			(at 0 0 0)
		)
		(symbol "74LVC2G14_1_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LVC2G14_2_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "~")
				(number "3")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "4")
			)
		)
		(symbol "74LVC2G14_3_0")
		(symbol "74LVC2G14_3_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC2G157"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 10.16 0)
		)
		(property "Value" "74LVC2G157"
			(at 7.62 -10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single 2 to 1 Multiplexer, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Mux CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP* VSSOP*"
			(at 0 0 0)
		)
		(symbol "74LVC2G157_0_1")
		(symbol "74LVC2G157_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 6.35)
				(name "A")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 6.35)
				(name "B")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 6.35)
				(name "~{A}/B")
				(number "6")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 6.35)
				(name "~{G}")
				(number "7")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 6.35)
				(name "Y")
				(number "5")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 6.35)
				(name "~{Y}")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC2G17"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "74LVC2G17"
			(at 2.54 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Buffer, Schmitt Triggered, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Buffer Schmitt LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SG-* SOT*"
			(at 0 0 0)
		)
		(symbol "74LVC2G17_1_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LVC2G17_2_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "~")
				(number "3")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "4")
			)
		)
		(symbol "74LVC2G17_3_0")
		(symbol "74LVC2G17_3_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC2G240"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 5.08 0)
		)
		(property "Value" "74LVC2G240"
			(at 5.08 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Inverter Buffer Tri-State, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Inv Buff Tri-State LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*"
			(at 0 0 0)
		)
		(symbol "74LVC2G240_1_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin input inverted
				(at 0 10.16 270)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin tri_state inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LVC2G240_2_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "~")
				(number "5")
			)
			(pin input inverted
				(at 0 10.16 270)
				(length 7.62)
				(name "~")
				(number "7")
			)
			(pin tri_state inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "3")
			)
		)
		(symbol "74LVC2G240_3_0")
		(symbol "74LVC2G240_3_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC2G241"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 5.08 0)
		)
		(property "Value" "74LVC2G241"
			(at 2.54 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "Dual Buffer Tri-State, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Buff Tri-State LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*"
			(at 0 0 0)
		)
		(symbol "74LVC2G241_1_1"
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "~")
				(number "2")
			)
			(pin input inverted
				(at 0 7.62 270)
				(length 5.08)
				(name "~")
				(number "1")
			)
			(pin tri_state line
				(at 10.16 0 180)
				(length 5.08)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LVC2G241_2_1"
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "~")
				(number "5")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "~")
				(number "7")
			)
			(pin tri_state line
				(at 10.16 0 180)
				(length 5.08)
				(name "~")
				(number "3")
			)
		)
		(symbol "74LVC2G241_3_0")
		(symbol "74LVC2G241_3_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC2G32"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 7.62 0)
		)
		(property "Value" "74LVC2G32"
			(at -7.62 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual OR Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Gate OR LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP* VSSOP*"
			(at 0 0 0)
		)
		(symbol "74LVC2G32_1_1"
			(pin input line
				(at -15.24 2.54 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "7")
			)
		)
		(symbol "74LVC2G32_2_1"
			(pin input line
				(at -15.24 2.54 0)
				(length 7.62)
				(name "~")
				(number "5")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 7.62)
				(name "~")
				(number "6")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "3")
			)
		)
		(symbol "74LVC2G32_3_0")
		(symbol "74LVC2G32_3_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC2G34"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "74LVC2G34"
			(at 2.54 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Buffer, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Buffer LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SG-* SOT*"
			(at 0 0 0)
		)
		(symbol "74LVC2G34_1_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LVC2G34_2_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "~")
				(number "3")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "4")
			)
		)
		(symbol "74LVC2G34_3_0")
		(symbol "74LVC2G34_3_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC2G38"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 7.62 0)
		)
		(property "Value" "74LVC2G38"
			(at 0 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual NAND Gate, Open Drain, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Gate NAND Open Drain LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP* VSSOP*"
			(at 0 0 0)
		)
		(symbol "74LVC2G38_1_1"
			(pin input line
				(at -15.24 2.54 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin open_collector inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "7")
			)
		)
		(symbol "74LVC2G38_2_1"
			(pin input line
				(at -15.24 2.54 0)
				(length 7.62)
				(name "~")
				(number "5")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 7.62)
				(name "~")
				(number "6")
			)
			(pin open_collector inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "3")
			)
		)
		(symbol "74LVC2G38_3_0")
		(symbol "74LVC2G38_3_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC2G53"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "74LVC2G53"
			(at 6.35 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "1 to 2 Analog Switch Mux/Demux, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "Analog Switch 1 to 2 CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP* VSSOP*"
			(at 0 0 0)
		)
		(symbol "74LVC2G53_1_1"
			(pin bidirectional line
				(at -10.16 0 0)
				(length 6.35)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 6.35)
				(name "~")
				(number "5")
			)
			(pin bidirectional line
				(at 7.62 2.54 180)
				(length 5.08)
				(name "~")
				(number "7")
			)
			(pin bidirectional line
				(at 7.62 -2.54 180)
				(length 5.08)
				(name "~")
				(number "6")
			)
			(pin input line
				(at 7.62 -5.08 180)
				(length 5.08)
				(name "~")
				(number "2")
			)
		)
		(symbol "74LVC2G53_2_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC2G66"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 10.16 0)
		)
		(property "Value" "74LVC2G66"
			(at 7.62 -10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Analog Switch"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP* VSSOP*"
			(at 0 0 0)
		)
		(symbol "74LVC2G66_1_1"
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "~")
				(number "7")
			)
			(pin tri_state line
				(at 12.7 0 180)
				(length 5.08)
				(name "~")
				(number "2")
			)
		)
		(symbol "74LVC2G66_2_1"
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "~")
				(number "5")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "~")
				(number "3")
			)
			(pin tri_state line
				(at 12.7 0 180)
				(length 5.08)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LVC2G66_3_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC2G74"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 10.16 0)
		)
		(property "Value" "74LVC2G74"
			(at 10.16 -10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "74AUC1G74, Single D Flip-Flop, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single D Flip-Flop D CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP* VSSOP*"
			(at 0 0 0)
		)
		(symbol "74LVC2G74_0_1")
		(symbol "74LVC2G74_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "~{PRE}")
				(number "7")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "D")
				(number "2")
			)
			(pin input clock
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "C")
				(number "1")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "~{CLR}")
				(number "6")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q")
				(number "5")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "~{Q}")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC2G79"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 10.16 0)
		)
		(property "Value" "74LVC2G79"
			(at 7.62 -10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual D Flip-Flop, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual D Flip-Flop D CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP* VSSOP*"
			(at 0 0 0)
		)
		(symbol "74LVC2G79_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "D")
				(number "2")
			)
			(pin input clock
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "C")
				(number "1")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q")
				(number "7")
			)
		)
		(symbol "74LVC2G79_2_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "D")
				(number "6")
			)
			(pin input clock
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "C")
				(number "5")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q")
				(number "3")
			)
		)
		(symbol "74LVC2G79_3_0")
		(symbol "74LVC2G79_3_1"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC2G80"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 10.16 0)
		)
		(property "Value" "74LVC2G80"
			(at 7.62 -10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual D Flip-Flop, Negative Output, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual D Flip-Flop Negative CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP* VSSOP*"
			(at 0 0 0)
		)
		(symbol "74LVC2G80_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "D")
				(number "2")
			)
			(pin input clock
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "C")
				(number "1")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "~{Q}")
				(number "7")
			)
		)
		(symbol "74LVC2G80_2_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "D")
				(number "6")
			)
			(pin input clock
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "C")
				(number "5")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "~{Q}")
				(number "3")
			)
		)
		(symbol "74LVC2G80_3_0")
		(symbol "74LVC2G80_3_1"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC2G86"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 7.62 0)
		)
		(property "Value" "74LVC2G86"
			(at 0 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual XOR Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Gate XOR LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP* VSSOP*"
			(at 0 0 0)
		)
		(symbol "74LVC2G86_1_1"
			(pin input line
				(at -15.24 2.54 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "7")
			)
		)
		(symbol "74LVC2G86_2_1"
			(pin input line
				(at -15.24 2.54 0)
				(length 7.62)
				(name "~")
				(number "5")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 7.62)
				(name "~")
				(number "6")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "3")
			)
		)
		(symbol "74LVC2G86_3_0")
		(symbol "74LVC2G86_3_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC3G04"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "74LVC3G04"
			(at 2.54 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Triple NOT Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Triple Gate NOT LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP* VSSOP*"
			(at 0 0 0)
		)
		(symbol "74LVC3G04_1_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "7")
			)
		)
		(symbol "74LVC3G04_2_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "~")
				(number "6")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "2")
			)
		)
		(symbol "74LVC3G04_3_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "~")
				(number "3")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "5")
			)
		)
		(symbol "74LVC3G04_4_0")
		(symbol "74LVC3G04_4_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC3G06"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 7.62 0)
		)
		(property "Value" "74LVC3G06"
			(at 2.54 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Triple NOT Gate, Open Drain, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Triple Gate NOT Open Drain LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP* VSSOP*"
			(at 0 0 0)
		)
		(symbol "74LVC3G06_1_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin open_collector inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "7")
			)
		)
		(symbol "74LVC3G06_2_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "~")
				(number "6")
			)
			(pin open_collector inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "2")
			)
		)
		(symbol "74LVC3G06_3_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "~")
				(number "3")
			)
			(pin open_collector inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "5")
			)
		)
		(symbol "74LVC3G06_4_0")
		(symbol "74LVC3G06_4_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC3G07"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 7.62 0)
		)
		(property "Value" "74LVC3G07"
			(at 1.27 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Triple Buffer, Open Drain, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Triple Buff Open Drain LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP* VSSOP*"
			(at 0 0 0)
		)
		(symbol "74LVC3G07_1_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin open_collector line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "7")
			)
		)
		(symbol "74LVC3G07_2_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "~")
				(number "6")
			)
			(pin open_collector line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "2")
			)
		)
		(symbol "74LVC3G07_3_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "~")
				(number "3")
			)
			(pin open_collector line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "5")
			)
		)
		(symbol "74LVC3G07_4_0")
		(symbol "74LVC3G07_4_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC3G14"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 7.62 0)
		)
		(property "Value" "74LVC3G14"
			(at 2.54 -7.62 0)
		)
		(property "Footprint" ""
			(at -1.27 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lvc3g14.pdf"
			(at 0 0 0)
		)
		(property "Description" "Triple NOT Gate Schmitt, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Triple NOT Schmitt LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP* VSSOP*"
			(at 0 0 0)
		)
		(symbol "74LVC3G14_1_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "7")
			)
		)
		(symbol "74LVC3G14_2_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "~")
				(number "6")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "2")
			)
		)
		(symbol "74LVC3G14_3_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "~")
				(number "3")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "5")
			)
		)
		(symbol "74LVC3G14_4_0")
		(symbol "74LVC3G14_4_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC3G17"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 7.62 0)
		)
		(property "Value" "74LVC3G17"
			(at 2.54 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Triple Buffer Schmitt, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Triple Buf Schmitt LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP* VSSOP*"
			(at 0 0 0)
		)
		(symbol "74LVC3G17_1_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "7")
			)
		)
		(symbol "74LVC3G17_2_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "~")
				(number "6")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "2")
			)
		)
		(symbol "74LVC3G17_3_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "~")
				(number "3")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "5")
			)
		)
		(symbol "74LVC3G17_4_0")
		(symbol "74LVC3G17_4_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC3G34"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 7.62 0)
		)
		(property "Value" "74LVC3G34"
			(at 1.27 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Triple Buffer, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Triple Buf LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP* VSSOP*"
			(at 0 0 0)
		)
		(symbol "74LVC3G34_1_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "7")
			)
		)
		(symbol "74LVC3G34_2_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "~")
				(number "6")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "2")
			)
		)
		(symbol "74LVC3G34_3_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "~")
				(number "3")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "5")
			)
		)
		(symbol "74LVC3G34_4_0")
		(symbol "74LVC3G34_4_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Inverter_Schmitt_Dual"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 12.7 0)
		)
		(property "Value" "Inverter_Schmitt_Dual"
			(at 2.54 10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Dual schmitt inverter"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual schmitt inverter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SOT?363* SC?70*"
			(at 0 0 0)
		)
		(symbol "Inverter_Schmitt_Dual_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "1A")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "2A")
				(number "3")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V_{CC}")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "1Y")
				(number "6")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "2Y")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NC7SVU04P5X"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 10.16 0)
		)
		(property "Value" "NC7SVU04P5X"
			(at 15.24 10.16 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NC7SVU04-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed Logic Inverter, SOT-353"
			(at 0 0 0)
		)
		(property "ki_keywords" "inverter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*353*SC*70*"
			(at 0 0 0)
		)
		(symbol "NC7SVU04P5X_0_1")
		(symbol "NC7SVU04P5X_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 5.08)
				(name "~")
				(number "2")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "3")
			)
			(pin no_connect line
				(at 10.16 0 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin output line
				(at 17.78 0 180)
				(length 5.08)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NC7SZ125M5X"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "NC7SZ125M5X"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 16.51 -6.35 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/nc7sz125-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "TinyLogic UHS Buffer, Tri-State Output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "buffer three-state"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "NC7SZ125M5X_0_1")
		(symbol "NC7SZ125M5X_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 5.08)
				(name "A")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 5.08)
				(name "~{OE}")
				(number "1")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 5.08)
				(name "Y")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74AHC1G00"
		(extends "74LVC1G00")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AHC1G00"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single NAND Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate NAND LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
	)
	(symbol "74AHC1G02"
		(extends "74LVC1G02")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AHC1G02"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single NOR Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate NOR LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
	)
	(symbol "74AHC1G04"
		(extends "74LVC1G04")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AHC1G04"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single NOT Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate NOT LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
	)
	(symbol "74AHC1G08"
		(extends "74LVC1G08")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AHC1G08"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single AND Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate AND LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
	)
	(symbol "74AHC1G125"
		(extends "74LVC1G125")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AHC1G125"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Buffer Gate Tri-State, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate Buff Tri-State LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
	)
	(symbol "74AHC1G126"
		(extends "74LVC1G126")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AHC1G126"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Buffer Gate Tri-State, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate Buff Tri-State LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
	)
	(symbol "74AHC1G14"
		(extends "74LVC1G14")
		(property "Reference" "U"
			(at 0 3.81 0)
		)
		(property "Value" "74AHC1G14"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lvc1g14.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "Single Schmitt NOT Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate NOT Schmitt LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SOT?553*"
			(at 0 0 0)
		)
	)
	(symbol "74AHC1G32"
		(extends "74LVC1G32")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AHC1G32"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single OR Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate OR LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
	)
	(symbol "74AHC1G86"
		(extends "74LVC1G86")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AHC1G86"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single XOR Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate XOR LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
	)
	(symbol "74AHC1GU04"
		(extends "74LVC1G04")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AHC1GU04"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "74AHC1G04, Single NOT Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate NOT LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
	)
	(symbol "74AHC2G00"
		(extends "74LVC2G00")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AHC2G00"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74AHC_AHCT2G00.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual NAND Gate, High-speed Si-gate CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Gate NAND LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP* VSSOP*"
			(at 0 0 0)
		)
	)
	(symbol "74AHCT1G00"
		(extends "74LVC1G00")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AHCT1G00"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single NAND Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate NAND LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
	)
	(symbol "74AHCT1G02"
		(extends "74LVC1G02")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AHCT1G02"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single NOR Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate NOR LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
	)
	(symbol "74AHCT1G04"
		(extends "74LVC1G04")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AHCT1G04"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single NOT Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate NOT LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
	)
	(symbol "74AHCT1G08"
		(extends "74LVC1G08")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AHCT1G08"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single AND Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate AND LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
	)
	(symbol "74AHCT1G125"
		(extends "74LVC1G125")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AHCT1G125"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Buffer Gate Tri-State, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate Buff Tri-State LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
	)
	(symbol "74AHCT1G126"
		(extends "74LVC1G126")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AHCT1G126"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Buffer Gate Tri-State, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate Buff Tri-State LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
	)
	(symbol "74AHCT1G14"
		(extends "74LVC1G14")
		(property "Reference" "U"
			(at 0 3.81 0)
		)
		(property "Value" "74AHCT1G14"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "Single Schmitt NOT Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate NOT Schmitt LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SOT?553*"
			(at 0 0 0)
		)
	)
	(symbol "74AHCT1G32"
		(extends "74LVC1G32")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AHCT1G32"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single OR Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate OR LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
	)
	(symbol "74AHCT1G86"
		(extends "74LVC1G86")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AHCT1G86"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single XOR Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate XOR LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
	)
	(symbol "74AHCT1GU04"
		(extends "74LVC1G04")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AHCT1GU04"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "74AHCT1G04, Single NOT Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate NOT LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
	)
	(symbol "74AHCT2G00"
		(extends "74LVC2G00")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AHCT2G00"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74AHC_AHCT2G00.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual NAND Gate, TTL input High-speed Si-gate CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Gate NAND LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP* VSSOP*"
			(at 0 0 0)
		)
	)
	(symbol "74AUC1G00"
		(extends "74LVC1G00")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AUC1G00"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single NAND Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate NAND LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
	)
	(symbol "74AUC1G02"
		(extends "74LVC1G02")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AUC1G02"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single NOR Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate NOR LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
	)
	(symbol "74AUC1G04"
		(extends "74LVC1G04")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AUC1G04"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single NOT Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate NOT LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
	)
	(symbol "74AUC1G06"
		(extends "74LVC1G06")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AUC1G06"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single NOT Gate, Open Drain, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate NOT LVC CMOS Open Drain"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
	)
	(symbol "74AUC1G07"
		(extends "74LVC1G07")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AUC1G07"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Buffer Gate, Open Drain, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate Buff LVC CMOS Open Drain"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
	)
	(symbol "74AUC1G08"
		(extends "74LVC1G08")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AUC1G08"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single AND Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate AND LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
	)
	(symbol "74AUC1G125"
		(extends "74LVC1G125")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AUC1G125"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Buffer Gate Tri-State, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate Buff Tri-State LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
	)
	(symbol "74AUC1G126"
		(extends "74LVC1G126")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AUC1G126"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Buffer Gate Tri-State, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate Buff Tri-State LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
	)
	(symbol "74AUC1G14"
		(extends "74LVC1G14")
		(property "Reference" "U"
			(at 0 3.81 0)
		)
		(property "Value" "74AUC1G14"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "Single Schmitt NOT Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate NOT Schmitt LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SOT?553*"
			(at 0 0 0)
		)
	)
	(symbol "74AUC1G17"
		(extends "74LVC1G17")
		(property "Reference" "U"
			(at 0 3.81 0)
		)
		(property "Value" "74AUC1G17"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "Single Schmitt Buffer Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate Buff Schmitt LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SOT?553* Texas?R-PDSO-G5?DCK* Texas?R-PDSO-N5?DRL* Texas?X2SON*0.8x0.8mm*P0.48mm*"
			(at 0 0 0)
		)
	)
	(symbol "74AUC1G18"
		(extends "74LVC1G18")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AUC1G18"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Demultiplexer, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Demux LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
	)
	(symbol "74AUC1G19"
		(extends "74LVC1G19")
		(property "Reference" "U"
			(at -2.54 5.08 0)
		)
		(property "Value" "74AUC1G19"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single 1 of 2 Decoder, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Decoder LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
	)
	(symbol "74AUC1G240"
		(extends "74LVC1G240")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AUC1G240"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Buffer/Driver Gate Tri-State, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate Buff/Drv Tri-State LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
	)
	(symbol "74AUC1G32"
		(extends "74LVC1G32")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AUC1G32"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single OR Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate OR LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
	)
	(symbol "74AUC1G66"
		(extends "74LVC1G66")
		(property "Reference" "U"
			(at -2.54 5.08 0)
		)
		(property "Value" "74AUC1G66"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74auc1g66.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Bilateral Analog Switch, SOT-23-5/SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Bilateral Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SC*"
			(at 0 0 0)
		)
	)
	(symbol "74AUC1G79"
		(extends "74LVC1G79")
		(property "Reference" "U"
			(at -2.54 5.08 0)
		)
		(property "Value" "74AUC1G79"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single D Flip-Flop, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single D Flip-Flop D CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG*"
			(at 0 0 0)
		)
	)
	(symbol "74AUC1G80"
		(extends "74LVC1G80")
		(property "Reference" "U"
			(at -2.54 5.08 0)
		)
		(property "Value" "74AUC1G80"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single D Flip-Flop, Inverted Output, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single D Flip-Flop CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG*"
			(at 0 0 0)
		)
	)
	(symbol "74AUC1G86"
		(extends "74LVC1G86")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AUC1G86"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single XOR Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate XOR LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
	)
	(symbol "74AUC1GU04"
		(extends "74LVC1G04")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AUC1GU04"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "74AUC1G04, Single NOT Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate NOT LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
	)
	(symbol "74AUC2G00"
		(extends "74LVC2G00")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AUC2G00"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual NAND Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Gate NAND LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP* VSSOP*"
			(at 0 0 0)
		)
	)
	(symbol "74AUC2G02"
		(extends "74LVC2G02")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AUC2G02"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual NOR Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Gate NOR LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP* VSSOP*"
			(at 0 0 0)
		)
	)
	(symbol "74AUC2G04"
		(extends "74LVC2G04")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AUC2G04"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual NOT Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Gate NOT LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SG-* SOT*"
			(at 0 0 0)
		)
	)
	(symbol "74AUC2G06"
		(extends "74LVC2G06")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AUC2G06"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual NOT Gate, Open Drain, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Gate NOT Open Drain LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SG-* SOT*"
			(at 0 0 0)
		)
	)
	(symbol "74AUC2G07"
		(extends "74LVC2G07")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AUC2G07"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Buffer, Open Drain, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Gate Buffer Open Drain LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SG-* SOT*"
			(at 0 0 0)
		)
	)
	(symbol "74AUC2G08"
		(extends "74LVC2G08")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AUC2G08"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual AND Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Gate AND LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP* VSSOP*"
			(at 0 0 0)
		)
	)
	(symbol "74AUC2G125"
		(extends "74LVC2G125")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AUC2G125"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Buffer Tri-State, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Buff Tri-State LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*"
			(at 0 0 0)
		)
	)
	(symbol "74AUC2G126"
		(extends "74LVC2G126")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AUC2G126"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Buffer Tri-State, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Buff Tri-State LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*"
			(at 0 0 0)
		)
	)
	(symbol "74AUC2G240"
		(extends "74LVC2G240")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AUC2G240"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Inverter Buffer Tri-State, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Inv Buff Tri-State LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*"
			(at 0 0 0)
		)
	)
	(symbol "74AUC2G241"
		(extends "74LVC2G241")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AUC2G241"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Buffer Tri-State, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Buff Tri-State LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*"
			(at 0 0 0)
		)
	)
	(symbol "74AUC2G32"
		(extends "74LVC2G32")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AUC2G32"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual OR Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Gate OR LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP* VSSOP*"
			(at 0 0 0)
		)
	)
	(symbol "74AUC2G34"
		(extends "74LVC2G34")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AUC2G34"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Buffer, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Buffer LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SG-* SOT*"
			(at 0 0 0)
		)
	)
	(symbol "74AUC2G53"
		(extends "74LVC2G53")
		(property "Reference" "U"
			(at -2.54 5.08 0)
		)
		(property "Value" "74AUC2G53"
			(at 0 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "1 to 2 Analog Switch Mux/Demux, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Analog Switch 1 to 2 CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP* VSSOP*"
			(at 0 0 0)
		)
	)
	(symbol "74AUC2G66"
		(extends "74LVC2G66")
		(property "Reference" "U"
			(at -2.54 5.08 0)
		)
		(property "Value" "74AUC2G66"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Analog Switch"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP* VSSOP*"
			(at 0 0 0)
		)
	)
	(symbol "74AUC2G79"
		(extends "74LVC2G79")
		(property "Reference" "U"
			(at -2.54 5.08 0)
		)
		(property "Value" "74AUC2G79"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual D Flip-Flop, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual D Flip-Flop D CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP* VSSOP*"
			(at 0 0 0)
		)
	)
	(symbol "74AUC2G80"
		(extends "74LVC2G80")
		(property "Reference" "U"
			(at -2.54 5.08 0)
		)
		(property "Value" "74AUC2G80"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual D Flip-Flop, Negative Output, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual D Flip-Flop Negative CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP* VSSOP*"
			(at 0 0 0)
		)
	)
	(symbol "74AUC2G86"
		(extends "74LVC2G86")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AUC2G86"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual XOR Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Gate XOR LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP* VSSOP*"
			(at 0 0 0)
		)
	)
	(symbol "74AUC2GU04"
		(extends "74LVC2G04")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AUC2GU04"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "74AUC2G04, Dual NOT Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Gate NOT LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SG-* SOT*"
			(at 0 0 0)
		)
	)
	(symbol "74AUP1G00"
		(extends "74LVC1G00")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AUP1G00"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74aup1g00.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single NAND Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate NAND LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* Texas?R-PDSO-G5?DCK* Texas?R-PDSO-N5?DRL* Texas?X2SON*0.8x0.8mm*P0.48mm*"
			(at 0 0 0)
		)
	)
	(symbol "74AUP1G02"
		(extends "74LVC1G02")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AUP1G02"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74aup1g02.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single NOR Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate NOR LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* Texas?R-PDSO-G5?DCK* Texas?R-PDSO-N5?DRL* Texas?X2SON*0.8x0.8mm*P0.48mm*"
			(at 0 0 0)
		)
	)
	(symbol "74AUP1G04"
		(extends "74LVC1G04")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AUP1G04"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74aup1g04.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single NOT Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate NOT LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* Texas?R-PDSO-G5?DCK* Texas?R-PDSO-N5?DRL* Texas?X2SON*0.8x0.8mm*P0.48mm*"
			(at 0 0 0)
		)
	)
	(symbol "74AUP1G06"
		(extends "74LVC1G06")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AUP1G06"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single NOT Gate, Open Drain, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate NOT LVC CMOS Open Drain"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
	)
	(symbol "74AUP1G07"
		(extends "74LVC1G07")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AUP1G07"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74aup1g07"
			(at 0 0 0)
		)
		(property "Description" "Single Buffer Gate, Open Drain, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate Buff LVC CMOS Open Drain"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* Texas?R-PDSO-G5?DCK* Texas?R-PDSO-N5?DRL* Texas?X2SON*0.8x0.8mm*P0.48mm*"
			(at 0 0 0)
		)
	)
	(symbol "74AUP1G08"
		(extends "74LVC1G08")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AUP1G08"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74aup1g08.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single AND Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate AND LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* Texas?R-PDSO-G5?DCK* Texas?R-PDSO-N5?DRL* Texas?X2SON*0.8x0.8mm*P0.48mm*"
			(at 0 0 0)
		)
	)
	(symbol "74AUP1G125"
		(extends "74LVC1G125")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AUP1G125"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Buffer Gate Tri-State, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate Buff Tri-State LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
	)
	(symbol "74AUP1G126"
		(extends "74LVC1G126")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AUP1G126"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Buffer Gate Tri-State, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate Buff Tri-State LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
	)
	(symbol "74AUP1G14"
		(extends "74LVC1G14")
		(property "Reference" "U"
			(at 0 3.81 0)
		)
		(property "Value" "74AUP1G14"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "Single Schmitt NOT Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate NOT Schmitt LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SOT?553*"
			(at 0 0 0)
		)
	)
	(symbol "74AUP1G17"
		(extends "74LVC1G17")
		(property "Reference" "U"
			(at 0 3.81 0)
		)
		(property "Value" "74AUP1G17"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "Single Schmitt Buffer Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate Buff Schmitt LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SOT?553* Texas?R-PDSO-G5?DCK* Texas?R-PDSO-N5?DRL* Texas?X2SON*0.8x0.8mm*P0.48mm*"
			(at 0 0 0)
		)
	)
	(symbol "74AUP1G240"
		(extends "74LVC1G240")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AUP1G240"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Buffer/Driver Gate Tri-State, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate Buff/Drv Tri-State LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
	)
	(symbol "74AUP1G32"
		(extends "74LVC1G32")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AUP1G32"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74aup1g32.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single OR Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate OR LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* Texas?R-PDSO-G5?DCK* Texas?R-PDSO-N5?DRL* Texas?X2SON*0.8x0.8mm*P0.48mm*"
			(at 0 0 0)
		)
	)
	(symbol "74AUP1G34"
		(extends "74LVC1G34")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AUP1G34"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74aup1g34.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Buffer Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate Buff LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* Texas?R-PDSO-G5?DCK* Texas?R-PDSO-N5?DRL* Texas?X2SON*0.8x0.8mm*P0.48mm*"
			(at 0 0 0)
		)
	)
	(symbol "74AUP1G57"
		(extends "74LVC1G57")
		(property "Reference" "U"
			(at -2.54 5.08 0)
		)
		(property "Value" "74AUP1G57"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Configurable Multi-Function Single Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Configurable Single Gate LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SC*"
			(at 0 0 0)
		)
	)
	(symbol "74AUP1G58"
		(extends "74LVC1G58")
		(property "Reference" "U"
			(at -2.54 5.08 0)
		)
		(property "Value" "74AUP1G58"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "74LAUP1G58, Configurable Multi-Function Single Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Configurable Single Gate LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SC*"
			(at 0 0 0)
		)
	)
	(symbol "74AUP1G74"
		(extends "74AUC1G74")
		(property "Reference" "U"
			(at -2.54 5.08 0)
		)
		(property "Value" "74AUP1G74"
			(at 5.08 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single D Flip-Flop, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single D Flip-Flop D CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP* VSSOP*"
			(at 0 0 0)
		)
	)
	(symbol "74AUP1G79"
		(extends "74LVC1G79")
		(property "Reference" "U"
			(at -2.54 5.08 0)
		)
		(property "Value" "74AUP1G79"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single D Flip-Flop, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single D Flip-Flop D CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG*"
			(at 0 0 0)
		)
	)
	(symbol "74AUP1G80"
		(extends "74LVC1G80")
		(property "Reference" "U"
			(at -2.54 5.08 0)
		)
		(property "Value" "74AUP1G80"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single D Flip-Flop, Inverted Output, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single D Flip-Flop CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG*"
			(at 0 0 0)
		)
	)
	(symbol "74AUP1G97"
		(extends "74LVC1G57")
		(property "Reference" "U"
			(at -2.54 5.08 0)
		)
		(property "Value" "74AUP1G97"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Configurable Multi-Function Single Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Configurable Single Gate LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SC*"
			(at 0 0 0)
		)
	)
	(symbol "74AUP1G98"
		(extends "74LVC1G58")
		(property "Reference" "U"
			(at -2.54 5.08 0)
		)
		(property "Value" "74AUP1G98"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Configurable Multi-Function Single Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Configurable Single Gate LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SC*"
			(at 0 0 0)
		)
	)
	(symbol "74AUP1G99"
		(extends "74LVC1G99")
		(property "Reference" "U"
			(at -3.81 6.985 0)
		)
		(property "Value" "74AUP1G99"
			(at -3.81 5.715 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Configurable Multi-Function Single Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Configurable Single Gate LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP* VSSOP*"
			(at 0 0 0)
		)
	)
	(symbol "74AUP1GU04"
		(extends "74LVC1G04")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74AUP1GU04"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "74AUP1G04, Single NOT Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate NOT LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
	)
	(symbol "74CB3T1G125"
		(extends "74CBT1G125")
		(property "Reference" "U"
			(at -2.54 5.08 0)
		)
		(property "Value" "74CB3T1G125"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single FET Bus Switch"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single FET Bus Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SC*"
			(at 0 0 0)
		)
	)
	(symbol "74CBTD1G125"
		(extends "74CBT1G125")
		(property "Reference" "U"
			(at -2.54 5.08 0)
		)
		(property "Value" "74CBTD1G125"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single FET Bus Switch"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single FET Bus Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SC*"
			(at 0 0 0)
		)
	)
	(symbol "74CBTD1G384"
		(extends "74CBT1G384")
		(property "Reference" "U"
			(at -2.54 5.08 0)
		)
		(property "Value" "74CBTD1G384"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single FET Bus Switch"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single FET Bus Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SC*"
			(at 0 0 0)
		)
	)
	(symbol "74CBTLV1G125"
		(extends "74CBT1G125")
		(property "Reference" "U"
			(at -2.54 5.08 0)
		)
		(property "Value" "74CBTLV1G125"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single FET Bus Switch"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single FET Bus Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SC*"
			(at 0 0 0)
		)
	)
	(symbol "74LVC1G97"
		(extends "74LVC1G57")
		(property "Reference" "U"
			(at -2.54 5.08 0)
		)
		(property "Value" "74LVC1G97"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Configurable Multi-Function Single Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Configurable Single Gate LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SC*"
			(at 0 0 0)
		)
	)
	(symbol "74LVC1G98"
		(extends "74LVC1G58")
		(property "Reference" "U"
			(at -2.54 5.08 0)
		)
		(property "Value" "74LVC1G98"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Configurable Multi-Function Single Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Configurable Single Gate LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SC*"
			(at 0 0 0)
		)
	)
	(symbol "74LVC1GU04"
		(extends "74LVC1G04")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74LVC1GU04"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "74LVC1G04, Single NOT Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate NOT LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
		)
	)
	(symbol "74LVC2GU04"
		(extends "74LVC2G04")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74LVC2GU04"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "74LVC2G04, Dual NOT Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Gate NOT LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SG-* SOT*"
			(at 0 0 0)
		)
	)
	(symbol "74LVC3GU04"
		(extends "74LVC3G04")
		(property "Reference" "U"
			(at -2.54 3.81 0)
		)
		(property "Value" "74LVC3GU04"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
		)
		(property "Description" "74LVC3G04, Triple NOT Gate, Low-Voltage CMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Triple Gate NOT LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP* VSSOP*"
			(at 0 0 0)
		)
	)
	(symbol "NC7SZ125P5X"
		(extends "NC7SZ125M5X")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "NC7SZ125P5X"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 20.32 -6.35 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/nc7sz125-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "TinyLogic UHS Buffer, Tri-State Output, SOT-353"
			(at 0 0 0)
		)
		(property "ki_keywords" "buffer three-state"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*353*"
			(at 0 0 0)
		)
	)
	(symbol "SN74LVC1G00DBV"
		(extends "74LVC1G00")
		(property "Reference" "U"
			(at -5.08 7.62 0)
		)
		(property "Value" "SN74LVC1G00DBV"
			(at 7.62 -7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74lvc1g00.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single NAND Gate, Low-Voltage CMOS, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate NAND LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "SN74LVC1G00DCK"
		(extends "74LVC1G00")
		(property "Reference" "U"
			(at -5.08 7.62 0)
		)
		(property "Value" "SN74LVC1G00DCK"
			(at 7.62 -7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Texas_R-PDSO-G5_DCK-5"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74lvc1g00.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single NAND Gate, Low-Voltage CMOS, SOT-353"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate NAND LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas?R?PDSO?G5?DCK*"
			(at 0 0 0)
		)
	)
	(symbol "SN74LVC1G00DRL"
		(extends "74LVC1G00")
		(property "Reference" "U"
			(at -5.08 7.62 0)
		)
		(property "Value" "SN74LVC1G00DRL"
			(at 7.62 -7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Texas_R-PDSO-N5_DRL-5"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74lvc1g00.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single NAND Gate, Low-Voltage CMOS, SOT-553"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate NAND LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas?R?PDSO?N5?DRL*"
			(at 0 0 0)
		)
	)
	(symbol "SN74LVC1G125DBV"
		(extends "74LVC1G125")
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "SN74LVC1G125DBV"
			(at 2.54 -7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74lvc1g125.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Buffer Gate Tri-State, Low-Voltage CMOS, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate Buff Tri-State LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "SN74LVC1G125DCK"
		(extends "74LVC1G125")
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "SN74LVC1G125DCK"
			(at 2.54 -7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Texas_R-PDSO-G5_DCK-5"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74lvc1g125.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Buffer Gate Tri-State, Low-Voltage CMOS, SOT-353"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate Buff Tri-State LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas?R?PDSO?G5?DCK*"
			(at 0 0 0)
		)
	)
	(symbol "SN74LVC1G125DRL"
		(extends "74LVC1G125")
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "SN74LVC1G125DRL"
			(at 2.54 -7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Texas_R-PDSO-N5_DRL-5"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74lvc1g125.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Buffer Gate Tri-State, Low-Voltage CMOS, SOT-553"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate Buff Tri-State LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas?R?PDSO?N5?DRL*"
			(at 0 0 0)
		)
	)
	(symbol "SN74LVC1G14DBV"
		(extends "74LVC1G14")
		(property "Reference" "U"
			(at 0 3.81 0)
		)
		(property "Value" "SN74LVC1G14DBV"
			(at 0 -3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lvc1g14.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "Single Schmitt NOT Gate, Low-Voltage CMOS, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate NOT Schmitt LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*23*"
			(at 0 0 0)
		)
	)
	(symbol "SN74LVC1G14DRL"
		(extends "74LVC1G14")
		(property "Reference" "U"
			(at 0 3.81 0)
		)
		(property "Value" "SN74LVC1G14DRL"
			(at 0 -3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-553"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lvc1g14.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "Single Schmitt NOT Gate, Low-Voltage CMOS, SOT-553"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Gate NOT Schmitt LVC CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*553*"
			(at 0 0 0)
		)
	)
	(symbol "SN74LVC2G14DBV"
		(extends "Inverter_Schmitt_Dual")
		(property "Reference" "U"
			(at 2.54 12.7 0)
		)
		(property "Value" "SN74LVC2G14DBV"
			(at 2.54 10.16 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lvc2g14.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual schmitt inverter, VCC from 1.65 to 5.5 V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual schmitt inverter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TC7PZ14FU"
		(extends "Inverter_Schmitt_Dual")
		(property "Reference" "U"
			(at 2.54 12.7 0)
		)
		(property "Value" "TC7PZ14FU"
			(at 2.54 10.16 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 0 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=14431&prodName=TC7PZ14FU"
			(at 0 0 0)
		)
		(property "Description" "Dual schmitt inverter, VCC from 1.65 to 5.5 V, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual schmitt inverter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
	)
)
