(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "74469"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 19.05 0)
		)
		(property "Value" "74469"
			(at -7.62 -19.05 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74469"
			(at 0 0 0)
		)
		(property "Description" "8-bit synchronous up/down counter, parallel load and hold capability (obsolete)"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "counter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?24*"
			(at 0 0 0)
		)
		(symbol "74469_1_0"
			(pin input line
				(at -12.7 15.24 0)
				(length 5.08)
				(name "D0")
				(number "3")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "D1")
				(number "4")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "D2")
				(number "5")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "D3")
				(number "6")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "D4")
				(number "7")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "D5")
				(number "8")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "D6")
				(number "9")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "D7")
				(number "10")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "CLK")
				(number "1")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "LD")
				(number "2")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "UD")
				(number "11")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 5.08)
				(name "CBI")
				(number "23")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 5.08)
				(name "VCC")
				(number "24")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 5.08)
				(name "GND")
				(number "12")
			)
			(pin tri_state line
				(at 12.7 15.24 180)
				(length 5.08)
				(name "Q0")
				(number "22")
			)
			(pin tri_state line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "Q1")
				(number "21")
			)
			(pin tri_state line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "Q2")
				(number "20")
			)
			(pin tri_state line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Q3")
				(number "19")
			)
			(pin tri_state line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q4")
				(number "18")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "Q5")
				(number "17")
			)
			(pin tri_state line
				(at 12.7 0 180)
				(length 5.08)
				(name "Q6")
				(number "16")
			)
			(pin tri_state line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "Q7")
				(number "15")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "OE")
				(number "13")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 5.08)
				(name "CBO")
				(number "14")
			)
		)
		(symbol "74469_1_1")
		(embedded_fonts no)
	)
	(symbol "7454"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 12.446 0)
		)
		(property "Value" "7454"
			(at 0 -12.192 0)
		)
		(property "Footprint" ""
			(at 0.7697 3.81 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn54ls54.pdf"
			(at 0 0 0)
		)
		(property "Description" "And-Nor (Y = /(AB + CD + EF + GH) ), DIP-14"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL ANDNOR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "7454_1_0"
			(pin input line
				(at -7.62 10.16 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -7.62 7.62 0)
				(length 3.81)
				(name "~")
				(number "13")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin input line
				(at -7.62 -7.62 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin input line
				(at -7.62 -10.16 0)
				(length 3.81)
				(name "~")
				(number "10")
			)
			(pin output inverted
				(at 10.16 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "7454_1_1")
		(symbol "7454_2_0"
			(pin power_in line
				(at 0 10.16 270)
				(length 3.81)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 3.81)
				(name "GND")
				(number "7")
			)
		)
		(symbol "7454_2_1")
		(embedded_fonts no)
	)
	(symbol "74ALVC164245"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 29.21 0)
		)
		(property "Value" "74ALVC164245"
			(at 1.27 -29.21 0)
		)
		(property "Footprint" "Package_SO:TSSOP-48_6.1x12.5mm_P0.5mm"
			(at 0 -1.27 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74ALVC164245.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "16-Bit 2.5V to 3.3V or 3.3V to 5V Level-Shifting Transceiver With 3-State Outputs, TSSOP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*6.1x12.5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "74ALVC164245_0_1")
		(symbol "74ALVC164245_1_1"
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "1DIR")
				(number "1")
			)
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "2DIR")
				(number "24")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "1B0")
				(number "2")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "1B1")
				(number "3")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "1B2")
				(number "5")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "1B3")
				(number "6")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "1B4")
				(number "8")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "1B5")
				(number "9")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "1B6")
				(number "11")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "1B7")
				(number "12")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "2B0")
				(number "13")
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "2B1")
				(number "14")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "2B2")
				(number "16")
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "2B3")
				(number "17")
			)
			(pin bidirectional line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "2B4")
				(number "19")
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "2B5")
				(number "20")
			)
			(pin bidirectional line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "2B6")
				(number "22")
			)
			(pin bidirectional line
				(at -12.7 -25.4 0)
				(length 2.54)
				(name "2B7")
				(number "23")
			)
			(pin passive line
				(at 0 30.48 270)
				(length 2.54)
				(hide yes)
				(name "V_{CC(B)}")
				(number "18")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 2.54)
				(name "V_{CC(B)}")
				(number "7")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "28")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "34")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "39")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "45")
			)
			(pin power_in line
				(at 2.54 30.48 270)
				(length 2.54)
				(name "V_{CC(A)}")
				(number "31")
			)
			(pin passive line
				(at 2.54 30.48 270)
				(length 2.54)
				(hide yes)
				(name "V_{CC(A)}")
				(number "42")
			)
			(pin input line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "1~{OE}")
				(number "48")
			)
			(pin input line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "2~{OE}")
				(number "25")
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "1A0")
				(number "47")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "1A1")
				(number "46")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "1A2")
				(number "44")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "1A3")
				(number "43")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "1A4")
				(number "41")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "1A5")
				(number "40")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "1A6")
				(number "38")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "1A7")
				(number "37")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "2A0")
				(number "36")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "2A1")
				(number "35")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "2A2")
				(number "33")
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "2A3")
				(number "32")
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "2A4")
				(number "30")
			)
			(pin bidirectional line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "2A5")
				(number "29")
			)
			(pin bidirectional line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "2A6")
				(number "27")
			)
			(pin bidirectional line
				(at 12.7 -25.4 180)
				(length 2.54)
				(name "2A7")
				(number "26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74CB3Q16210DGG"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 31.75 0)
		)
		(property "Value" "74CB3Q16210DGG"
			(at 8.89 31.75 0)
		)
		(property "Footprint" "Package_SO:TSSOP-48_6.1x12.5mm_P0.5mm"
			(at 21.59 -34.29 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74cb3q16210.pdf"
			(at 0 0 0)
		)
		(property "Description" "20-bit FET bus switch with 10-bit output enables, TSSOP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "bus transmission gates fet switch bidirectional"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*6.1x12.5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "74CB3Q16210DGG_0_1")
		(symbol "74CB3Q16210DGG_1_0"
			(pin passive line
				(at -10.16 27.94 0)
				(length 2.54)
				(name "1A1")
				(number "2")
			)
			(pin passive line
				(at -10.16 25.4 0)
				(length 2.54)
				(name "1A2")
				(number "3")
			)
			(pin passive line
				(at -10.16 22.86 0)
				(length 2.54)
				(name "1A3")
				(number "4")
			)
			(pin passive line
				(at -10.16 20.32 0)
				(length 2.54)
				(name "1A4")
				(number "5")
			)
			(pin passive line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "1A5")
				(number "6")
			)
			(pin passive line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "1A6")
				(number "7")
			)
			(pin passive line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "1A7")
				(number "9")
			)
			(pin passive line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "1A8")
				(number "10")
			)
			(pin passive line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "1A9")
				(number "11")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "1A10")
				(number "12")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "2A1")
				(number "13")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "2A2")
				(number "14")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "2A3")
				(number "16")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "2A4")
				(number "18")
			)
			(pin passive line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "2A5")
				(number "19")
			)
			(pin passive line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "2A6")
				(number "20")
			)
			(pin passive line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "2A7")
				(number "21")
			)
			(pin passive line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "2A8")
				(number "22")
			)
			(pin passive line
				(at -10.16 -20.32 0)
				(length 2.54)
				(name "2A9")
				(number "23")
			)
			(pin passive line
				(at -10.16 -22.86 0)
				(length 2.54)
				(name "2A10")
				(number "24")
			)
			(pin input line
				(at -10.16 -27.94 0)
				(length 2.54)
				(name "1~{OE}")
				(number "48")
			)
			(pin input line
				(at -10.16 -30.48 0)
				(length 2.54)
				(name "2~{OE}")
				(number "47")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "VCC")
				(number "15")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "32")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "41")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 10.16 27.94 180)
				(length 2.54)
				(name "1B1")
				(number "46")
			)
			(pin passive line
				(at 10.16 25.4 180)
				(length 2.54)
				(name "1B2")
				(number "45")
			)
			(pin passive line
				(at 10.16 22.86 180)
				(length 2.54)
				(name "1B3")
				(number "44")
			)
			(pin passive line
				(at 10.16 20.32 180)
				(length 2.54)
				(name "1B4")
				(number "43")
			)
			(pin passive line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "1B5")
				(number "42")
			)
			(pin passive line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "1B6")
				(number "40")
			)
			(pin passive line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "1B7")
				(number "39")
			)
			(pin passive line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "1B8")
				(number "38")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "1B9")
				(number "37")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "1B10")
				(number "36")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "2B1")
				(number "35")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "2B2")
				(number "34")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "2B3")
				(number "33")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "2B4")
				(number "31")
			)
			(pin passive line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "2B5")
				(number "30")
			)
			(pin passive line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "2B6")
				(number "29")
			)
			(pin passive line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "2B7")
				(number "28")
			)
			(pin passive line
				(at 10.16 -17.78 180)
				(length 2.54)
				(name "2B8")
				(number "27")
			)
			(pin passive line
				(at 10.16 -20.32 180)
				(length 2.54)
				(name "2B9")
				(number "26")
			)
			(pin passive line
				(at 10.16 -22.86 180)
				(length 2.54)
				(name "2B10")
				(number "25")
			)
		)
		(symbol "74CB3Q16210DGG_1_1"
			(pin no_connect line
				(at 7.62 -30.48 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74CBTLV16212"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 40.64 0)
		)
		(property "Value" "74CBTLV16212"
			(at 10.16 40.64 0)
		)
		(property "Footprint" ""
			(at 0 20.32 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74cbtlv16212.pdf"
			(at 0 20.32 0)
		)
		(property "Description" "Low-voltage 24-bit FET Bus-exchange switch"
			(at 0 0 0)
		)
		(property "ki_keywords" "bus"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP* TSSOP*"
			(at 0 0 0)
		)
		(symbol "74CBTLV16212_0_1")
		(symbol "74CBTLV16212_1_0"
			(pin input line
				(at -12.7 33.02 0)
				(length 5.08)
				(name "S1")
				(number "56")
			)
			(pin input line
				(at -12.7 30.48 0)
				(length 5.08)
				(name "S2")
				(number "55")
			)
			(pin bidirectional line
				(at -12.7 25.4 0)
				(length 5.08)
				(name "1A1")
				(number "2")
			)
			(pin bidirectional line
				(at -12.7 22.86 0)
				(length 5.08)
				(name "2A1")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 5.08)
				(name "3A1")
				(number "6")
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 5.08)
				(name "4A1")
				(number "9")
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 5.08)
				(name "5A1")
				(number "11")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "6A1")
				(number "13")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "7A1")
				(number "15")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "8A1")
				(number "18")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "9A1")
				(number "21")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "10A1")
				(number "23")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 5.08)
				(name "11A1")
				(number "25")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "12A1")
				(number "27")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "1A2")
				(number "3")
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "2A2")
				(number "5")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "3A2")
				(number "7")
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 5.08)
				(name "4A2")
				(number "10")
			)
			(pin bidirectional line
				(at -12.7 -17.78 0)
				(length 5.08)
				(name "5A2")
				(number "12")
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 5.08)
				(name "6A2")
				(number "14")
			)
			(pin bidirectional line
				(at -12.7 -22.86 0)
				(length 5.08)
				(name "7A2")
				(number "16")
			)
			(pin bidirectional line
				(at -12.7 -25.4 0)
				(length 5.08)
				(name "8A2")
				(number "20")
			)
			(pin bidirectional line
				(at -12.7 -27.94 0)
				(length 5.08)
				(name "9A2")
				(number "22")
			)
			(pin bidirectional line
				(at -12.7 -30.48 0)
				(length 5.08)
				(name "10A2")
				(number "24")
			)
			(pin bidirectional line
				(at -12.7 -33.02 0)
				(length 5.08)
				(name "11A2")
				(number "26")
			)
			(pin bidirectional line
				(at -12.7 -35.56 0)
				(length 5.08)
				(name "12A2")
				(number "28")
			)
			(pin power_in line
				(at 0 43.18 270)
				(length 5.08)
				(name "VCC")
				(number "17")
			)
			(pin passive line
				(at 0 -43.18 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "19")
			)
			(pin passive line
				(at 0 -43.18 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "38")
			)
			(pin passive line
				(at 0 -43.18 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "49")
			)
			(pin power_in line
				(at 0 -43.18 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 25.4 180)
				(length 5.08)
				(name "1B1")
				(number "54")
			)
			(pin bidirectional line
				(at 12.7 22.86 180)
				(length 5.08)
				(name "2B1")
				(number "52")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 5.08)
				(name "3B1")
				(number "50")
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 5.08)
				(name "4B1")
				(number "47")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 5.08)
				(name "5B1")
				(number "45")
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "6B1")
				(number "43")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "7B1")
				(number "41")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "8B1")
				(number "39")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "9B1")
				(number "36")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "10B1")
				(number "34")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 5.08)
				(name "11B1")
				(number "32")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "12B1")
				(number "30")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "1B2")
				(number "53")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 5.08)
				(name "2B2")
				(number "51")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 5.08)
				(name "3B2")
				(number "48")
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 5.08)
				(name "4B2")
				(number "46")
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 5.08)
				(name "5B2")
				(number "44")
			)
			(pin bidirectional line
				(at 12.7 -20.32 180)
				(length 5.08)
				(name "6B2")
				(number "42")
			)
			(pin bidirectional line
				(at 12.7 -22.86 180)
				(length 5.08)
				(name "7B2")
				(number "40")
			)
			(pin bidirectional line
				(at 12.7 -25.4 180)
				(length 5.08)
				(name "8B2")
				(number "37")
			)
			(pin bidirectional line
				(at 12.7 -27.94 180)
				(length 5.08)
				(name "9B2")
				(number "35")
			)
			(pin bidirectional line
				(at 12.7 -30.48 180)
				(length 5.08)
				(name "10B2")
				(number "33")
			)
			(pin bidirectional line
				(at 12.7 -33.02 180)
				(length 5.08)
				(name "11B2")
				(number "31")
			)
			(pin bidirectional line
				(at 12.7 -35.56 180)
				(length 5.08)
				(name "12B2")
				(number "29")
			)
		)
		(symbol "74CBTLV16212_1_1"
			(pin input line
				(at -12.7 35.56 0)
				(length 5.08)
				(name "S0")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74CBTLV3257"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 17.78 1.27 0)
		)
		(property "Value" "74CBTLV3257"
			(at 15.24 -1.27 0)
		)
		(property "Footprint" ""
			(at -1.27 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74cbtlv3257.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Quad 1:2 FET Multiplexer/Demultiplexer, Low-Voltage"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "mux demux low-voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*3.9x4.9mm*P0.635mm* TSSOP*4.4x5mm*P0.65mm* TVSOP*4.4x3.6mm*P0.4mm* SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "74CBTLV3257_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(symbol "74CBTLV3257_2_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(symbol "74CBTLV3257_3_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "10")
			)
		)
		(symbol "74CBTLV3257_4_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "13")
			)
		)
		(symbol "74CBTLV3257_5_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 3.81)
				(name "S")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 3.81)
				(name "~{OE}")
				(number "15")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 3.81)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 3.81)
				(name "GND")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74CBTLV3861"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 19.05 0)
		)
		(property "Value" "74CBTLV3861"
			(at -8.255 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74cbtlv3861"
			(at 0 0 0)
		)
		(property "Description" "Low-voltage 10-bit FET bus switch"
			(at 0 0 0)
		)
		(property "ki_keywords" "bus"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?24*"
			(at 0 0 0)
		)
		(symbol "74CBTLV3861_1_0"
			(pin passive line
				(at -12.7 15.24 0)
				(length 5.08)
				(name "A1")
				(number "2")
			)
			(pin passive line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "A2")
				(number "3")
			)
			(pin passive line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "A3")
				(number "4")
			)
			(pin passive line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "A4")
				(number "5")
			)
			(pin passive line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "A5")
				(number "6")
			)
			(pin passive line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "A6")
				(number "7")
			)
			(pin passive line
				(at -12.7 0 0)
				(length 5.08)
				(name "A7")
				(number "8")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "A8")
				(number "9")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "A9")
				(number "10")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "A10")
				(number "11")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "~{OE}")
				(number "23")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 5.08)
				(name "VCC")
				(number "24")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 5.08)
				(name "GND")
				(number "12")
			)
			(pin no_connect line
				(at 7.62 -12.7 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin passive line
				(at 12.7 15.24 180)
				(length 5.08)
				(name "B1")
				(number "22")
			)
			(pin passive line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "B2")
				(number "21")
			)
			(pin passive line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "B3")
				(number "20")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "B4")
				(number "19")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "B5")
				(number "18")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "B6")
				(number "17")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 5.08)
				(name "B7")
				(number "16")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "B8")
				(number "15")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "B9")
				(number "14")
			)
			(pin passive line
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "B10")
				(number "13")
			)
		)
		(symbol "74CBTLV3861_1_1")
		(embedded_fonts no)
	)
	(symbol "74HC137"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74HC137"
			(at 2.54 -11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/cd74hc237.pdf"
			(at 0 0 0)
		)
		(property "Description" "3-to-8 line decoder/multiplexer with address latches, DIP-16/SOIC-16/SSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "demux"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* SSOP*5.3x6.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "74HC137_0_1")
		(symbol "74HC137_1_1"
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "A0")
				(number "1")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{LE}")
				(number "4")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{E1}")
				(number "5")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "E2")
				(number "6")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "~{Y0}")
				(number "15")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "~{Y1}")
				(number "14")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "~{Y2}")
				(number "13")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~{Y3}")
				(number "12")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "~{Y4}")
				(number "11")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{Y5}")
				(number "10")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "~{Y6}")
				(number "9")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "~{Y7}")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74HC138"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74HC138"
			(at 2.54 -11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/cd74hc238.pdf"
			(at 0 0 0)
		)
		(property "Description" "3-to-8 line decoder/multiplexer inverting, DIP-16/SOIC-16/SSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "demux"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* SSOP*5.3x6.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "74HC138_0_1")
		(symbol "74HC138_1_1"
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "A0")
				(number "1")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{E0}")
				(number "4")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{E1}")
				(number "5")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "E2")
				(number "6")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "~{Y0}")
				(number "15")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "~{Y1}")
				(number "14")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "~{Y2}")
				(number "13")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~{Y3}")
				(number "12")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "~{Y4}")
				(number "11")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{Y5}")
				(number "10")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "~{Y6}")
				(number "9")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "~{Y7}")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74HC14"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74HC14"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74HC14"
			(at 0 0 0)
		)
		(property "Description" "Hex inverter schmitt trigger"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "HCMOS not inverter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "74HC14_1_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "2")
			)
		)
		(symbol "74HC14_1_1")
		(symbol "74HC14_2_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "3")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "4")
			)
		)
		(symbol "74HC14_2_1")
		(symbol "74HC14_3_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "74HC14_3_1")
		(symbol "74HC14_4_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "74HC14_4_1")
		(symbol "74HC14_5_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "11")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "10")
			)
		)
		(symbol "74HC14_5_1")
		(symbol "74HC14_6_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "13")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "12")
			)
		)
		(symbol "74HC14_6_1")
		(symbol "74HC14_7_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74HC14_7_1")
		(embedded_fonts no)
	)
	(symbol "74HC164"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.905 -13.97 0)
		)
		(property "Value" "74HC164"
			(at 1.905 -16.51 0)
		)
		(property "Footprint" ""
			(at 22.86 -7.62 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74HC_HCT164.pdf"
			(at 22.86 -7.62 0)
		)
		(property "Description" "8-bit serial-in parallel-out shift register"
			(at 0 0 0)
		)
		(property "ki_keywords" "8-bit shift register"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7*P1.27mm* ?SSOP*P0.65mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "74HC164_0_1")
		(symbol "74HC164_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "~{MR}")
				(number "9")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "DSA")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "DSB")
				(number "2")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "CP")
				(number "8")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "Q0")
				(number "3")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "Q1")
				(number "4")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "Q2")
				(number "5")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "Q3")
				(number "6")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "Q4")
				(number "10")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "Q5")
				(number "11")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "Q6")
				(number "12")
			)
			(pin output line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "Q7")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74HC237"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74HC237"
			(at 2.54 -11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/cd74hc237.pdf"
			(at 0 0 0)
		)
		(property "Description" "3-to-8 line decoder/multiplexer with address latches, DIP-16/SOIC-16/SSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "demux"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* SSOP*5.3x6.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "74HC237_0_1")
		(symbol "74HC237_1_1"
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "A0")
				(number "1")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{LE}")
				(number "4")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{E1}")
				(number "5")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "E2")
				(number "6")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "Y0")
				(number "15")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "Y1")
				(number "14")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "Y2")
				(number "13")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "Y3")
				(number "12")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "Y4")
				(number "11")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "Y5")
				(number "10")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "Y6")
				(number "9")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "Y7")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74HC238"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74HC238"
			(at 2.54 -11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/cd74hc238.pdf"
			(at 0 0 0)
		)
		(property "Description" "3-to-8 line decoder/multiplexer, DIP-16/SOIC-16/SSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "demux"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "74HC238_0_1")
		(symbol "74HC238_1_1"
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "A0")
				(number "1")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{E1}")
				(number "4")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{E2}")
				(number "5")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "E3")
				(number "6")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "Y0")
				(number "15")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "Y1")
				(number "14")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "Y2")
				(number "13")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "Y3")
				(number "12")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "Y4")
				(number "11")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "Y5")
				(number "10")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "Y6")
				(number "9")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "Y7")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74HC240"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74HC240"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74HC_HCT240.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit Buffer/Line Driver 3-state Inverting"
			(at 0 0 0)
		)
		(property "ki_keywords" "HCMOS BUFFER 3State inv"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*7.5x12.8mm*P1.27mm* TSSOP*4.4x6.5mm*P0.65mm* SSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "74HC240_1_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "1A0")
				(number "2")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "1A1")
				(number "4")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "1A2")
				(number "6")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "1A3")
				(number "8")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "2A0")
				(number "17")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "2A1")
				(number "15")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "2A2")
				(number "13")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "2A3")
				(number "11")
			)
			(pin input inverted
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "1OE")
				(number "1")
			)
			(pin input inverted
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "2OE")
				(number "19")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 5.08)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 5.08)
				(name "GND")
				(number "10")
			)
			(pin tri_state line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "1Y0")
				(number "18")
			)
			(pin tri_state line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "1Y1")
				(number "16")
			)
			(pin tri_state line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "1Y2")
				(number "14")
			)
			(pin tri_state line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "1Y3")
				(number "12")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "2Y0")
				(number "3")
			)
			(pin tri_state line
				(at 12.7 0 180)
				(length 5.08)
				(name "2Y1")
				(number "5")
			)
			(pin tri_state line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "2Y2")
				(number "7")
			)
			(pin tri_state line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "2Y3")
				(number "9")
			)
		)
		(symbol "74HC240_1_1")
		(embedded_fonts no)
	)
	(symbol "74HC244"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74HC244"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74HC_HCT244.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit Buffer/Line Driver 3-state"
			(at 0 0 0)
		)
		(property "ki_keywords" "HCMOS BUFFER 3State"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm* SSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "74HC244_1_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "1A0")
				(number "2")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "1A1")
				(number "4")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "1A2")
				(number "6")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "1A3")
				(number "8")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "2A0")
				(number "17")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "2A1")
				(number "15")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "2A2")
				(number "13")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "2A3")
				(number "11")
			)
			(pin input inverted
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "1OE")
				(number "1")
			)
			(pin input inverted
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "2OE")
				(number "19")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 5.08)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 5.08)
				(name "GND")
				(number "10")
			)
			(pin tri_state line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "1Y0")
				(number "18")
			)
			(pin tri_state line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "1Y1")
				(number "16")
			)
			(pin tri_state line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "1Y2")
				(number "14")
			)
			(pin tri_state line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "1Y3")
				(number "12")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "2Y0")
				(number "3")
			)
			(pin tri_state line
				(at 12.7 0 180)
				(length 5.08)
				(name "2Y1")
				(number "5")
			)
			(pin tri_state line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "2Y2")
				(number "7")
			)
			(pin tri_state line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "2Y3")
				(number "9")
			)
		)
		(symbol "74HC244_1_1")
		(embedded_fonts no)
	)
	(symbol "74HC4024"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "74HC4024"
			(at 6.35 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 1.27 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74HC4024.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "7-stage binary ripple counter, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "binary counter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "74HC4024_0_1")
		(symbol "74HC4024_1_0"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{CP}")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "MR")
				(number "2")
			)
			(pin no_connect line
				(at -7.62 7.62 0)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "8")
			)
			(pin no_connect line
				(at -7.62 5.08 0)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "10")
			)
			(pin no_connect line
				(at -7.62 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "13")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "Q0")
				(number "12")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "Q1")
				(number "11")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "Q2")
				(number "9")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "Q3")
				(number "6")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "Q4")
				(number "5")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "Q5")
				(number "4")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "Q6")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74HC4051"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 11.43 0)
		)
		(property "Value" "74HC4051"
			(at -7.62 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/cd74hc4051.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "8-channel analog multiplexer/demultiplexer, DIP-16/SOIC-16/TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "HCMOS Multiplexer Demultiplexer Analog"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* SOIC*5.3x10.2mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "74HC4051_0_1")
		(symbol "74HC4051_1_1"
			(pin passive line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "A")
				(number "3")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "S0")
				(number "11")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "S1")
				(number "10")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "S2")
				(number "9")
			)
			(pin input line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "~{E}")
				(number "6")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "VEE")
				(number "7")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "A0")
				(number "13")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "A1")
				(number "14")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "A2")
				(number "15")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "A3")
				(number "12")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "A4")
				(number "1")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "A5")
				(number "5")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "A6")
				(number "2")
			)
			(pin passive line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "A7")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74HC4060"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 16.51 0)
		)
		(property "Value" "74HC4060"
			(at 7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/m74hc4060.pdf"
			(at 0 0 0)
		)
		(property "Description" "Binary counter (14-stages) and oscillator"
			(at 0 0 0)
		)
		(property "ki_keywords" "binary counter oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*7.62* TSSOP*16*4.4x5* SOIC*16*3.9x9.9*"
			(at 0 0 0)
		)
		(symbol "74HC4060_1_0"
			(pin input inverted_clock
				(at -12.7 12.7 0)
				(length 5.08)
				(name "~{Φ0}")
				(number "9")
			)
			(pin input clock
				(at -12.7 10.16 0)
				(length 5.08)
				(name "Φ0")
				(number "10")
			)
			(pin input inverted_clock
				(at -12.7 7.62 0)
				(length 5.08)
				(name "~{Φ1}")
				(number "11")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "CLR")
				(number "12")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 5.08)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "Q4")
				(number "7")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "Q5")
				(number "5")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Q6")
				(number "4")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q7")
				(number "6")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "Q8")
				(number "14")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "Q9")
				(number "13")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "Q10")
				(number "15")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "Q12")
				(number "1")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 5.08)
				(name "Q13")
				(number "2")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 5.08)
				(name "Q14")
				(number "3")
			)
		)
		(symbol "74HC4060_1_1")
		(embedded_fonts no)
	)
	(symbol "74HC590"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74HC590"
			(at -7.62 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 1.27 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74HC590.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "8-bit Binary Counter with Output Register 3-State Outputs, SOIC-16/TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "HCMOS Counter 3State"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm* SOIC*5.3x10.2mm*P1.27mm* SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "74HC590_1_0"
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "~{CE}")
				(number "12")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "CPC")
				(number "11")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "CPR")
				(number "13")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{MRC}")
				(number "10")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{OE}")
				(number "14")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin tri_state line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "Q0")
				(number "15")
			)
			(pin tri_state line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "Q1")
				(number "1")
			)
			(pin tri_state line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "Q2")
				(number "2")
			)
			(pin tri_state line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "Q3")
				(number "3")
			)
			(pin tri_state line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "Q4")
				(number "4")
			)
			(pin tri_state line
				(at 10.16 0 180)
				(length 2.54)
				(name "Q5")
				(number "5")
			)
			(pin tri_state line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "Q6")
				(number "6")
			)
			(pin tri_state line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "Q7")
				(number "7")
			)
			(pin output line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "~{RCO}")
				(number "9")
			)
		)
		(symbol "74HC590_1_1")
		(embedded_fonts no)
	)
	(symbol "74HC594"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74HC594"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74hc594.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-Bit Shift Registers With Output Registers"
			(at 0 0 0)
		)
		(property "ki_keywords" "HCMOS SR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm* SOIC*5.3x10.2mm*P1.27mm* SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "74HC594_1_0"
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "SER")
				(number "14")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SRCLK")
				(number "11")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{SRCLR}")
				(number "10")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "RCLK")
				(number "12")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{RCLR}")
				(number "13")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "QA")
				(number "15")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "QB")
				(number "1")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "QC")
				(number "2")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "QD")
				(number "3")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "QE")
				(number "4")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "QF")
				(number "5")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "QG")
				(number "6")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "QH")
				(number "7")
			)
			(pin output line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "QH'")
				(number "9")
			)
		)
		(symbol "74HC594_1_1")
		(embedded_fonts no)
	)
	(symbol "74HC595"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74HC595"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74hc595.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit serial in/out Shift Register 3-State Outputs"
			(at 0 0 0)
		)
		(property "ki_keywords" "HCMOS SR 3State"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm* SOIC*5.3x10.2mm*P1.27mm* SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "74HC595_1_0"
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "SER")
				(number "14")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SRCLK")
				(number "11")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{SRCLR}")
				(number "10")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "RCLK")
				(number "12")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{OE}")
				(number "13")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin tri_state line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "QA")
				(number "15")
			)
			(pin tri_state line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "QB")
				(number "1")
			)
			(pin tri_state line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "QC")
				(number "2")
			)
			(pin tri_state line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "QD")
				(number "3")
			)
			(pin tri_state line
				(at 10.16 0 180)
				(length 2.54)
				(name "QE")
				(number "4")
			)
			(pin tri_state line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "QF")
				(number "5")
			)
			(pin tri_state line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "QG")
				(number "6")
			)
			(pin tri_state line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "QH")
				(number "7")
			)
			(pin output line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "QH'")
				(number "9")
			)
		)
		(symbol "74HC595_1_1")
		(embedded_fonts no)
	)
	(symbol "74HC596"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74HC596"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74HC_HCT595.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit serial in/out Shift Register Open Collector Outputs"
			(at 0 0 0)
		)
		(property "ki_keywords" "HCMOS SR OpenCollector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm* SOIC*5.3x10.2mm*P1.27mm* SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "74HC596_1_0"
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "SER")
				(number "14")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SRCLK")
				(number "11")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{SRCLR}")
				(number "10")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "RCLK")
				(number "12")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{OE}")
				(number "13")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin open_collector line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "QA")
				(number "15")
			)
			(pin open_collector line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "QB")
				(number "1")
			)
			(pin open_collector line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "QC")
				(number "2")
			)
			(pin open_collector line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "QD")
				(number "3")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "QE")
				(number "4")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "QF")
				(number "5")
			)
			(pin open_collector line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "QG")
				(number "6")
			)
			(pin open_collector line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "QH")
				(number "7")
			)
			(pin output line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "QH'")
				(number "9")
			)
		)
		(symbol "74HC596_1_1")
		(embedded_fonts no)
	)
	(symbol "74HC7014"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74HC7014"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74HC7014.pdf"
			(at 0 0 0)
		)
		(property "Description" "Hex non-inverting buffer with precision Schmitt Trigger inputs, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "Hex non-inverting Schmitt buffer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "74HC7014_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "2")
			)
		)
		(symbol "74HC7014_2_1"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "3")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "4")
			)
		)
		(symbol "74HC7014_3_1"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "74HC7014_4_1"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "74HC7014_5_1"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "11")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "10")
			)
		)
		(symbol "74HC7014_6_1"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "13")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "12")
			)
		)
		(symbol "74HC7014_7_1"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LCX07"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74LCX07"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "www.st.com/resource/en/datasheet/74lcx07.pdf"
			(at 0 0 0)
		)
		(property "Description" "CMOS hex buffer (open drain) with 5V tolerant inputs"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS hex buffer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "74LCX07_1_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "2")
			)
		)
		(symbol "74LCX07_2_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "3")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "4")
			)
		)
		(symbol "74LCX07_3_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LCX07_4_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "74LCX07_5_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "11")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "10")
			)
		)
		(symbol "74LCX07_6_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "13")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "12")
			)
		)
		(symbol "74LCX07_7_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74LCX07_7_1")
		(embedded_fonts no)
	)
	(symbol "74LS00"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74LS00"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74ls00"
			(at 0 0 0)
		)
		(property "Description" "quad 2-input NAND gate"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL nand 2-input"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SO14*"
			(at 0 0 0)
		)
		(symbol "74LS00_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "3")
			)
		)
		(symbol "74LS00_1_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "1")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "3")
			)
		)
		(symbol "74LS00_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LS00_2_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "4")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LS00_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "10")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "74LS00_3_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "9")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "10")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "74LS00_4_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "12")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "13")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "11")
			)
		)
		(symbol "74LS00_4_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "12")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "13")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "11")
			)
		)
		(symbol "74LS00_5_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74LS00_5_1")
		(embedded_fonts no)
	)
	(symbol "74LS01"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74LS01"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.nteinc.com/specs/7400to7499/pdf/nte74LS01.pdf"
			(at 0 0 0)
		)
		(property "Description" "quad 2-input NAND gate, open collector outputs NRND"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL nand 2-input open collector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "74LS01_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "3")
			)
			(pin open_collector inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "1")
			)
		)
		(symbol "74LS01_1_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "2")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "3")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "1")
			)
		)
		(symbol "74LS01_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "6")
			)
			(pin open_collector inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "4")
			)
		)
		(symbol "74LS01_2_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "5")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "6")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "4")
			)
		)
		(symbol "74LS01_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "8")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin open_collector inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "10")
			)
		)
		(symbol "74LS01_3_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "8")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "9")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "10")
			)
		)
		(symbol "74LS01_4_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "11")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "12")
			)
			(pin open_collector inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "13")
			)
		)
		(symbol "74LS01_4_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "11")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "12")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "13")
			)
		)
		(symbol "74LS01_5_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74LS01_5_1")
		(embedded_fonts no)
	)
	(symbol "74LS02"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74LS02"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74ls02"
			(at 0 0 0)
		)
		(property "Description" "quad 2-input NOR gate"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL Nor2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO14* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "74LS02_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "3")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "1")
			)
		)
		(symbol "74LS02_1_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "3")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "1")
			)
		)
		(symbol "74LS02_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "6")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "4")
			)
		)
		(symbol "74LS02_2_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "4")
			)
		)
		(symbol "74LS02_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "8")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "9")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "10")
			)
		)
		(symbol "74LS02_3_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "8")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "10")
			)
		)
		(symbol "74LS02_4_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "11")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "12")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "13")
			)
		)
		(symbol "74LS02_4_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "11")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "12")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "13")
			)
		)
		(symbol "74LS02_5_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74LS02_5_1")
		(embedded_fonts no)
	)
	(symbol "74LS03"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74LS03"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS03"
			(at 0 0 0)
		)
		(property "Description" "Quad 2-input NAND open collector"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL Nand2 OpenColl"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm**"
			(at 0 0 0)
		)
		(symbol "74LS03_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin open_collector inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "3")
			)
		)
		(symbol "74LS03_1_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "1")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "2")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "3")
			)
		)
		(symbol "74LS03_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin open_collector inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LS03_2_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "4")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "5")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LS03_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "10")
			)
			(pin open_collector inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "74LS03_3_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "9")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "10")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "74LS03_4_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "12")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "13")
			)
			(pin open_collector inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "11")
			)
		)
		(symbol "74LS03_4_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "12")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "13")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "11")
			)
		)
		(symbol "74LS03_5_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74LS03_5_1")
		(embedded_fonts no)
	)
	(symbol "74LS04"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74LS04"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS04"
			(at 0 0 0)
		)
		(property "Description" "Hex Inverter"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL not inv"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SSOP?14* TSSOP?14*"
			(at 0 0 0)
		)
		(symbol "74LS04_1_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "2")
			)
		)
		(symbol "74LS04_2_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "3")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "4")
			)
		)
		(symbol "74LS04_3_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LS04_4_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "74LS04_5_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "11")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "10")
			)
		)
		(symbol "74LS04_6_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "13")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "12")
			)
		)
		(symbol "74LS04_7_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74LS04_7_1")
		(embedded_fonts no)
	)
	(symbol "74LS05"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74LS05"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS05"
			(at 0 0 0)
		)
		(property "Description" "Inverter Open Collect"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL not inv OpenCol"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "74LS05_1_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin open_collector inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "2")
			)
		)
		(symbol "74LS05_2_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "3")
			)
			(pin open_collector inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "4")
			)
		)
		(symbol "74LS05_3_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin open_collector inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LS05_4_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin open_collector inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "74LS05_5_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "11")
			)
			(pin open_collector inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "10")
			)
		)
		(symbol "74LS05_6_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "13")
			)
			(pin open_collector inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "12")
			)
		)
		(symbol "74LS05_7_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74LS05_7_1")
		(embedded_fonts no)
	)
	(symbol "74LS08"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74LS08"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS08"
			(at 0 0 0)
		)
		(property "Description" "Quad And2"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL and2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "74LS08_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "3")
			)
		)
		(symbol "74LS08_1_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "1")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "2")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "3")
			)
		)
		(symbol "74LS08_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LS08_2_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "4")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "5")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LS08_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "10")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "74LS08_3_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "9")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "10")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "74LS08_4_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "12")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "13")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "11")
			)
		)
		(symbol "74LS08_4_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "12")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "13")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "11")
			)
		)
		(symbol "74LS08_5_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74LS08_5_1")
		(embedded_fonts no)
	)
	(symbol "74LS09"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74LS09"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS09"
			(at 0 0 0)
		)
		(property "Description" "Quad 2-input AND Open Collect"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL and2 OpenCol"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "74LS09_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "3")
			)
		)
		(symbol "74LS09_1_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "1")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "2")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "3")
			)
		)
		(symbol "74LS09_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LS09_2_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "4")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "5")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LS09_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "10")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "74LS09_3_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "9")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "10")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "74LS09_4_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "12")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "13")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "11")
			)
		)
		(symbol "74LS09_4_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "12")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "13")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "11")
			)
		)
		(symbol "74LS09_5_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74LS09_5_1")
		(embedded_fonts no)
	)
	(symbol "74LS10"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74LS10"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS10"
			(at 0 0 0)
		)
		(property "Description" "Triple 3-input NAND"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL Nand3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "74LS10_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "13")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "12")
			)
		)
		(symbol "74LS10_1_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "1")
			)
			(pin input inverted
				(at -7.62 0 0)
				(length 4.953)
				(name "~")
				(number "2")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "13")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "12")
			)
		)
		(symbol "74LS10_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "3")
			)
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LS10_2_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "3")
			)
			(pin input inverted
				(at -7.62 0 0)
				(length 4.953)
				(name "~")
				(number "4")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LS10_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "10")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "11")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "74LS10_3_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "9")
			)
			(pin input inverted
				(at -7.62 0 0)
				(length 4.953)
				(name "~")
				(number "10")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "11")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "74LS10_4_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74LS10_4_1")
		(embedded_fonts no)
	)
	(symbol "74LS107"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "74LS107"
			(at -7.62 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS107"
			(at 0 0 0)
		)
		(property "Description" "Dual JK Flip-Flop, reset"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL JK"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "74LS107_1_0"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "J")
				(number "1")
			)
			(pin input clock
				(at -7.62 0 0)
				(length 2.54)
				(name "C")
				(number "12")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "K")
				(number "4")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~{R}")
				(number "13")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "Q")
				(number "3")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~{Q}")
				(number "2")
			)
		)
		(symbol "74LS107_1_1")
		(symbol "74LS107_2_0"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "J")
				(number "8")
			)
			(pin input clock
				(at -7.62 0 0)
				(length 2.54)
				(name "C")
				(number "9")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "K")
				(number "11")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~{R}")
				(number "10")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "Q")
				(number "5")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~{Q}")
				(number "6")
			)
		)
		(symbol "74LS107_2_1")
		(symbol "74LS107_3_0"
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74LS107_3_1")
		(embedded_fonts no)
	)
	(symbol "74LS109"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "74LS109"
			(at -7.62 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS109"
			(at 0 0 0)
		)
		(property "Description" "Dual JK Flip-Flop, Set & Reset"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL JK"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "74LS109_1_0"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "J")
				(number "2")
			)
			(pin input clock
				(at -7.62 0 0)
				(length 2.54)
				(name "C")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~{K}")
				(number "3")
			)
			(pin input line
				(at 0 7.62 270)
				(length 2.54)
				(name "~{S}")
				(number "5")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~{R}")
				(number "1")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "Q")
				(number "6")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~{Q}")
				(number "7")
			)
		)
		(symbol "74LS109_1_1")
		(symbol "74LS109_2_0"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "J")
				(number "14")
			)
			(pin input clock
				(at -7.62 0 0)
				(length 2.54)
				(name "C")
				(number "12")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~{K}")
				(number "13")
			)
			(pin input line
				(at 0 7.62 270)
				(length 2.54)
				(name "~{S}")
				(number "11")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~{R}")
				(number "15")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "Q")
				(number "10")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~{Q}")
				(number "9")
			)
		)
		(symbol "74LS109_2_1")
		(symbol "74LS109_3_0"
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
		)
		(symbol "74LS109_3_1")
		(embedded_fonts no)
	)
	(symbol "74LS11"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74LS11"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS11"
			(at 0 0 0)
		)
		(property "Description" "Triple 3-input AND"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL And3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "74LS11_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "13")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "12")
			)
		)
		(symbol "74LS11_1_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "1")
			)
			(pin input inverted
				(at -7.62 0 0)
				(length 4.953)
				(name "~")
				(number "2")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "13")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "12")
			)
		)
		(symbol "74LS11_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "3")
			)
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LS11_2_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "3")
			)
			(pin input inverted
				(at -7.62 0 0)
				(length 4.953)
				(name "~")
				(number "4")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "5")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LS11_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "10")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "11")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "74LS11_3_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "9")
			)
			(pin input inverted
				(at -7.62 0 0)
				(length 4.953)
				(name "~")
				(number "10")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "11")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "74LS11_4_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74LS11_4_1")
		(embedded_fonts no)
	)
	(symbol "74LS112"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "74LS112"
			(at -7.62 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS112"
			(at 0 0 0)
		)
		(property "Description" "dual JK Flip-Flop, Set & Reset"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL JK"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS112_1_0"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "J")
				(number "3")
			)
			(pin input clock
				(at -7.62 0 0)
				(length 2.54)
				(name "C")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "K")
				(number "2")
			)
			(pin input line
				(at 0 7.62 270)
				(length 2.54)
				(name "~{S}")
				(number "4")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~{R}")
				(number "15")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "Q")
				(number "5")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~{Q}")
				(number "6")
			)
		)
		(symbol "74LS112_1_1")
		(symbol "74LS112_2_0"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "J")
				(number "11")
			)
			(pin input clock
				(at -7.62 0 0)
				(length 2.54)
				(name "C")
				(number "13")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "K")
				(number "12")
			)
			(pin input line
				(at 0 7.62 270)
				(length 2.54)
				(name "~{S}")
				(number "10")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~{R}")
				(number "14")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "Q")
				(number "9")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~{Q}")
				(number "7")
			)
		)
		(symbol "74LS112_2_1")
		(symbol "74LS112_3_0"
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
		)
		(symbol "74LS112_3_1")
		(embedded_fonts no)
	)
	(symbol "74LS113"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "74LS113"
			(at -7.62 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS113"
			(at 0 0 0)
		)
		(property "Description" "dual JK flip-flop, Set"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL JK"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "74LS113_1_0"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "J")
				(number "3")
			)
			(pin input clock
				(at -7.62 0 0)
				(length 2.54)
				(name "C")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "K")
				(number "2")
			)
			(pin input line
				(at 0 7.62 270)
				(length 2.54)
				(name "~{S}")
				(number "4")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "Q")
				(number "5")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~{Q}")
				(number "6")
			)
		)
		(symbol "74LS113_1_1")
		(symbol "74LS113_2_0"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "J")
				(number "11")
			)
			(pin input clock
				(at -7.62 0 0)
				(length 2.54)
				(name "C")
				(number "13")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "K")
				(number "12")
			)
			(pin input line
				(at 0 7.62 270)
				(length 2.54)
				(name "~{S}")
				(number "10")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "Q")
				(number "9")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~{Q}")
				(number "8")
			)
		)
		(symbol "74LS113_2_1")
		(symbol "74LS113_3_0"
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74LS113_3_1")
		(embedded_fonts no)
	)
	(symbol "74LS114"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "74LS114"
			(at -7.62 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS114"
			(at 0 0 0)
		)
		(property "Description" "Dual JK flip-flop, common Clock & Reset, Set"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL JK"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "74LS114_1_0"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "J")
				(number "3")
			)
			(pin input clock
				(at -7.62 0 0)
				(length 2.54)
				(name "C")
				(number "13")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "K")
				(number "2")
			)
			(pin input line
				(at 0 7.62 270)
				(length 2.54)
				(name "~{S}")
				(number "4")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~{R}")
				(number "1")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "Q")
				(number "5")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~{Q}")
				(number "6")
			)
		)
		(symbol "74LS114_1_1")
		(symbol "74LS114_2_0"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "J")
				(number "11")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "K")
				(number "12")
			)
			(pin input line
				(at 0 7.62 270)
				(length 2.54)
				(name "~{S}")
				(number "10")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "Q")
				(number "9")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~{Q}")
				(number "8")
			)
		)
		(symbol "74LS114_2_1")
		(symbol "74LS114_3_0"
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74LS114_3_1")
		(embedded_fonts no)
	)
	(symbol "74LS12"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74LS12"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS12"
			(at 0 0 0)
		)
		(property "Description" "Triple 3-input NAND Open Collector"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL Nand3 OpenCol"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "74LS12_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "13")
			)
			(pin open_collector inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "12")
			)
		)
		(symbol "74LS12_1_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "1")
			)
			(pin input inverted
				(at -7.62 0 0)
				(length 4.953)
				(name "~")
				(number "2")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "13")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "12")
			)
		)
		(symbol "74LS12_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "3")
			)
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin open_collector inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LS12_2_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "3")
			)
			(pin input inverted
				(at -7.62 0 0)
				(length 4.953)
				(name "~")
				(number "4")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "5")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LS12_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "10")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "11")
			)
			(pin open_collector inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "74LS12_3_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "9")
			)
			(pin input inverted
				(at -7.62 0 0)
				(length 4.953)
				(name "~")
				(number "10")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "11")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "74LS12_4_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74LS12_4_1")
		(embedded_fonts no)
	)
	(symbol "74LS121"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "74LS121"
			(at -7.62 -11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74121"
			(at 0 0 0)
		)
		(property "Description" "monostable multivibrator with Schmitt-trigger inputs"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "monostable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "74LS121_1_0"
			(pin input line
				(at -15.24 7.62 0)
				(length 5.08)
				(name "R/Cext")
				(number "11")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 5.08)
				(name "Rint")
				(number "9")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "Cext")
				(number "10")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "A1")
				(number "3")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 5.08)
				(name "A2")
				(number "4")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 5.08)
				(name "B")
				(number "5")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 5.08)
				(name "Q")
				(number "6")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 5.08)
				(name "~{Q}")
				(number "1")
			)
		)
		(symbol "74LS121_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS122"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74LS122"
			(at -7.62 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS122"
			(at 0 0 0)
		)
		(property "Description" "Retriggerable Monostable"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL monostable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "74LS122_1_0"
			(pin input line
				(at -15.24 10.16 0)
				(length 5.08)
				(name "R/Cext")
				(number "13")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 5.08)
				(name "Rint")
				(number "9")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 5.08)
				(name "Cext")
				(number "11")
			)
			(pin input inverted
				(at -15.24 0 0)
				(length 5.08)
				(name "A1")
				(number "1")
			)
			(pin input inverted
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "A2")
				(number "2")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 5.08)
				(name "B1")
				(number "3")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 5.08)
				(name "B2")
				(number "4")
			)
			(pin input inverted
				(at -15.24 -10.16 0)
				(length 5.08)
				(name "Clr")
				(number "5")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 5.08)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 5.08)
				(name "Q")
				(number "8")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 5.08)
				(name "~{Q}")
				(number "6")
			)
		)
		(symbol "74LS122_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS123"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "74LS123"
			(at -7.62 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS123"
			(at 0 0 0)
		)
		(property "Description" "Dual retriggerable Monostable"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL monostable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS123_1_0"
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "RCext")
				(number "15")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "Cext")
				(number "14")
			)
			(pin input inverted
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "A")
				(number "1")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "B")
				(number "2")
			)
			(pin input inverted
				(at 0 -12.7 90)
				(length 5.08)
				(name "Clr")
				(number "3")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q")
				(number "13")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "~{Q}")
				(number "4")
			)
		)
		(symbol "74LS123_1_1")
		(symbol "74LS123_2_0"
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "RCext")
				(number "7")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "Cext")
				(number "6")
			)
			(pin input inverted
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "A")
				(number "9")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "B")
				(number "10")
			)
			(pin input inverted
				(at 0 -12.7 90)
				(length 5.08)
				(name "Clr")
				(number "11")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q")
				(number "5")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "~{Q}")
				(number "12")
			)
		)
		(symbol "74LS123_2_1")
		(symbol "74LS123_3_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
		)
		(symbol "74LS123_3_1")
		(embedded_fonts no)
	)
	(symbol "74LS125"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74LS125"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS125"
			(at 0 0 0)
		)
		(property "Description" "Quad buffer 3-State outputs"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL buffer 3State"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "74LS125_1_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin input inverted
				(at 0 -6.35 90)
				(length 4.445)
				(name "~")
				(number "1")
			)
			(pin tri_state line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "3")
			)
		)
		(symbol "74LS125_2_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin input inverted
				(at 0 -6.35 90)
				(length 4.445)
				(name "~")
				(number "4")
			)
			(pin tri_state line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LS125_3_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin input inverted
				(at 0 -6.35 90)
				(length 4.445)
				(name "~")
				(number "10")
			)
			(pin tri_state line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "74LS125_4_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "12")
			)
			(pin input inverted
				(at 0 -6.35 90)
				(length 4.445)
				(name "~")
				(number "13")
			)
			(pin tri_state line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "11")
			)
		)
		(symbol "74LS125_5_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74LS125_5_1")
		(embedded_fonts no)
	)
	(symbol "74LS126"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74LS126"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS126"
			(at 0 0 0)
		)
		(property "Description" "Quad buffer 3-State outputs"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL Buffer 3State"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "74LS126_1_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin input line
				(at 0 -6.35 90)
				(length 4.445)
				(name "~")
				(number "1")
			)
			(pin tri_state line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "3")
			)
		)
		(symbol "74LS126_2_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin input line
				(at 0 -6.35 90)
				(length 4.445)
				(name "~")
				(number "4")
			)
			(pin tri_state line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LS126_3_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin input line
				(at 0 -6.35 90)
				(length 4.445)
				(name "~")
				(number "10")
			)
			(pin tri_state line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "74LS126_4_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "12")
			)
			(pin input line
				(at 0 -6.35 90)
				(length 4.445)
				(name "~")
				(number "13")
			)
			(pin tri_state line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "11")
			)
		)
		(symbol "74LS126_5_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74LS126_5_1")
		(embedded_fonts no)
	)
	(symbol "74LS13"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74LS13"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS13"
			(at 0 0 0)
		)
		(property "Description" "Dual 4-input NAND Schmitt trigger"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL Nand4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "74LS13_1_1"
			(pin input line
				(at -7.62 3.81 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -7.62 1.27 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin input line
				(at -7.62 -1.27 0)
				(length 3.81)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -7.62 -3.81 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LS13_1_2"
			(pin input inverted
				(at -7.62 3.81 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin input inverted
				(at -7.62 1.27 0)
				(length 4.826)
				(name "~")
				(number "2")
			)
			(pin input inverted
				(at -7.62 -1.27 0)
				(length 4.826)
				(name "~")
				(number "4")
			)
			(pin input inverted
				(at -7.62 -3.81 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LS13_2_1"
			(pin input line
				(at -7.62 3.81 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin input line
				(at -7.62 1.27 0)
				(length 3.81)
				(name "~")
				(number "10")
			)
			(pin input line
				(at -7.62 -1.27 0)
				(length 3.81)
				(name "~")
				(number "12")
			)
			(pin input line
				(at -7.62 -3.81 0)
				(length 3.81)
				(name "~")
				(number "13")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "74LS13_2_2"
			(pin input inverted
				(at -7.62 3.81 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin input inverted
				(at -7.62 1.27 0)
				(length 4.826)
				(name "~")
				(number "10")
			)
			(pin input inverted
				(at -7.62 -1.27 0)
				(length 4.826)
				(name "~")
				(number "12")
			)
			(pin input inverted
				(at -7.62 -3.81 0)
				(length 3.81)
				(name "~")
				(number "13")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "74LS13_3_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74LS13_3_1")
		(embedded_fonts no)
	)
	(symbol "74LS132"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74LS132"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS132"
			(at 0 0 0)
		)
		(property "Description" "Quad 2-input NAND Schmitt trigger"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL Nand2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "74LS132_1_0")
		(symbol "74LS132_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "3")
			)
		)
		(symbol "74LS132_1_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "1")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "3")
			)
		)
		(symbol "74LS132_2_0")
		(symbol "74LS132_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LS132_2_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "4")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LS132_3_0")
		(symbol "74LS132_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "10")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "74LS132_3_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "9")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "10")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "74LS132_4_0")
		(symbol "74LS132_4_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "12")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "13")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "11")
			)
		)
		(symbol "74LS132_4_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "12")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "13")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "11")
			)
		)
		(symbol "74LS132_5_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74LS132_5_1")
		(embedded_fonts no)
	)
	(symbol "74LS133"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74LS133"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS133"
			(at 0 0 0)
		)
		(property "Description" "NAND 13-input"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL Nand13"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS133_1_1"
			(pin input line
				(at -7.62 15.24 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -7.62 12.7 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin input line
				(at -7.62 10.16 0)
				(length 3.81)
				(name "~")
				(number "3")
			)
			(pin input line
				(at -7.62 7.62 0)
				(length 3.81)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "6")
			)
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "7")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "10")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 3.81)
				(name "~")
				(number "11")
			)
			(pin input line
				(at -7.62 -7.62 0)
				(length 3.81)
				(name "~")
				(number "12")
			)
			(pin input line
				(at -7.62 -10.16 0)
				(length 3.81)
				(name "~")
				(number "13")
			)
			(pin input line
				(at -7.62 -12.7 0)
				(length 3.81)
				(name "~")
				(number "14")
			)
			(pin input line
				(at -7.62 -15.24 0)
				(length 3.81)
				(name "~")
				(number "15")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "9")
			)
		)
		(symbol "74LS133_1_2"
			(pin input inverted
				(at -7.62 15.24 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin input inverted
				(at -7.62 12.7 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin input inverted
				(at -7.62 10.16 0)
				(length 3.81)
				(name "~")
				(number "3")
			)
			(pin input inverted
				(at -7.62 7.62 0)
				(length 3.81)
				(name "~")
				(number "4")
			)
			(pin input inverted
				(at -7.62 5.08 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.5466)
				(name "~")
				(number "6")
			)
			(pin input inverted
				(at -7.62 0 0)
				(length 5.08)
				(name "~")
				(number "7")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.5466)
				(name "~")
				(number "10")
			)
			(pin input inverted
				(at -7.62 -5.08 0)
				(length 3.81)
				(name "~")
				(number "11")
			)
			(pin input inverted
				(at -7.62 -7.62 0)
				(length 3.81)
				(name "~")
				(number "12")
			)
			(pin input inverted
				(at -7.62 -10.16 0)
				(length 3.81)
				(name "~")
				(number "13")
			)
			(pin input inverted
				(at -7.62 -12.7 0)
				(length 3.81)
				(name "~")
				(number "14")
			)
			(pin input inverted
				(at -7.62 -15.24 0)
				(length 3.81)
				(name "~")
				(number "15")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "9")
			)
		)
		(symbol "74LS133_2_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
		)
		(symbol "74LS133_2_1")
		(embedded_fonts no)
	)
	(symbol "74LS136"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74LS136"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn54ls136.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad 2-input XOR Open Collector"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL XOR2 OpenCol"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "74LS136_1_0"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.445)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.445)
				(name "~")
				(number "2")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "3")
			)
		)
		(symbol "74LS136_1_1")
		(symbol "74LS136_2_0"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.445)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.445)
				(name "~")
				(number "5")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LS136_2_1")
		(symbol "74LS136_3_0"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.445)
				(name "~")
				(number "9")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.445)
				(name "~")
				(number "10")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "74LS136_3_1")
		(symbol "74LS136_4_0"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.445)
				(name "~")
				(number "12")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.445)
				(name "~")
				(number "13")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "11")
			)
		)
		(symbol "74LS136_4_1")
		(symbol "74LS136_5_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74LS136_5_1")
		(embedded_fonts no)
	)
	(symbol "74LS137"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "74LS137"
			(at -7.62 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS137"
			(at 0 0 0)
		)
		(property "Description" "Decoder 3 to 8, address latches"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL DECOD8 DECOD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS137_1_0"
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "A0")
				(number "1")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "A2")
				(number "3")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "~{GL}")
				(number "4")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "~{G2}")
				(number "5")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "G1")
				(number "6")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin output inverted
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Y7")
				(number "7")
			)
			(pin output inverted
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Y6")
				(number "9")
			)
			(pin output inverted
				(at 12.7 2.54 180)
				(length 5.08)
				(name "Y5")
				(number "10")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 5.08)
				(name "Y4")
				(number "11")
			)
			(pin output inverted
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "Y3")
				(number "12")
			)
			(pin output inverted
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "Y2")
				(number "13")
			)
			(pin output inverted
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "Y1")
				(number "14")
			)
			(pin output inverted
				(at 12.7 -10.16 180)
				(length 5.08)
				(name "Y0")
				(number "15")
			)
		)
		(symbol "74LS137_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS138"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "74LS138"
			(at -7.62 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS138"
			(at 0 0 0)
		)
		(property "Description" "Decoder 3 to 8 active low outputs"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL DECOD DECOD8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS138_1_0"
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "A0")
				(number "1")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "A2")
				(number "3")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "E3")
				(number "6")
			)
			(pin input input_low
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "E2")
				(number "5")
			)
			(pin input input_low
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "E1")
				(number "4")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin output output_low
				(at 12.7 7.62 180)
				(length 5.08)
				(name "O0")
				(number "15")
			)
			(pin output output_low
				(at 12.7 5.08 180)
				(length 5.08)
				(name "O1")
				(number "14")
			)
			(pin output output_low
				(at 12.7 2.54 180)
				(length 5.08)
				(name "O2")
				(number "13")
			)
			(pin output output_low
				(at 12.7 0 180)
				(length 5.08)
				(name "O3")
				(number "12")
			)
			(pin output output_low
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "O4")
				(number "11")
			)
			(pin output output_low
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "O5")
				(number "10")
			)
			(pin output output_low
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "O6")
				(number "9")
			)
			(pin output output_low
				(at 12.7 -10.16 180)
				(length 5.08)
				(name "O7")
				(number "7")
			)
		)
		(symbol "74LS138_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS139"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "74LS139"
			(at -7.62 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74ls139a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Decoder 1 of 4, Active low outputs"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL DECOD4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS139_1_0"
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "A1")
				(number "3")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "A0")
				(number "2")
			)
			(pin input inverted
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "E")
				(number "1")
			)
			(pin output inverted
				(at 12.7 2.54 180)
				(length 5.08)
				(name "O0")
				(number "4")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 5.08)
				(name "O1")
				(number "5")
			)
			(pin output inverted
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "O2")
				(number "6")
			)
			(pin output inverted
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "O3")
				(number "7")
			)
		)
		(symbol "74LS139_1_1")
		(symbol "74LS139_2_0"
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "A1")
				(number "13")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "A0")
				(number "14")
			)
			(pin input inverted
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "E")
				(number "15")
			)
			(pin output inverted
				(at 12.7 2.54 180)
				(length 5.08)
				(name "O0")
				(number "12")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 5.08)
				(name "O1")
				(number "11")
			)
			(pin output inverted
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "O2")
				(number "10")
			)
			(pin output inverted
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "O3")
				(number "9")
			)
		)
		(symbol "74LS139_2_1")
		(symbol "74LS139_3_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
		)
		(symbol "74LS139_3_1")
		(embedded_fonts no)
	)
	(symbol "74LS145"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74LS145"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS145"
			(at 0 0 0)
		)
		(property "Description" "Decoder 1 to 10, Open Collector"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL DECOD10 OpenColl"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS145_1_0"
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "P0")
				(number "15")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "P1")
				(number "14")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "P2")
				(number "13")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "P3")
				(number "12")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin open_collector inverted
				(at 12.7 10.16 180)
				(length 5.08)
				(name "Q0")
				(number "1")
			)
			(pin open_collector inverted
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Q1")
				(number "2")
			)
			(pin open_collector inverted
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q2")
				(number "3")
			)
			(pin open_collector inverted
				(at 12.7 2.54 180)
				(length 5.08)
				(name "Q3")
				(number "4")
			)
			(pin open_collector inverted
				(at 12.7 0 180)
				(length 5.08)
				(name "Q4")
				(number "5")
			)
			(pin open_collector inverted
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "Q5")
				(number "6")
			)
			(pin open_collector inverted
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "Q6")
				(number "7")
			)
			(pin open_collector inverted
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "Q7")
				(number "9")
			)
			(pin open_collector inverted
				(at 12.7 -10.16 180)
				(length 5.08)
				(name "Q8")
				(number "10")
			)
			(pin open_collector inverted
				(at 12.7 -12.7 180)
				(length 5.08)
				(name "Q9")
				(number "11")
			)
		)
		(symbol "74LS145_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS147"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74LS147"
			(at -7.62 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS147"
			(at 0 0 0)
		)
		(property "Description" "Priority Encoder, 10 to 4"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL ENCOD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS147_1_0"
			(pin input inverted
				(at -12.7 10.16 0)
				(length 5.08)
				(name "E1")
				(number "11")
			)
			(pin input inverted
				(at -12.7 7.62 0)
				(length 5.08)
				(name "E2")
				(number "12")
			)
			(pin input inverted
				(at -12.7 5.08 0)
				(length 5.08)
				(name "E3")
				(number "13")
			)
			(pin input inverted
				(at -12.7 2.54 0)
				(length 5.08)
				(name "E4")
				(number "1")
			)
			(pin input inverted
				(at -12.7 0 0)
				(length 5.08)
				(name "E5")
				(number "2")
			)
			(pin input inverted
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "E6")
				(number "3")
			)
			(pin input inverted
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "E7")
				(number "4")
			)
			(pin input inverted
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "E8")
				(number "5")
			)
			(pin input inverted
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "E9")
				(number "10")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin output inverted
				(at 12.7 10.16 180)
				(length 5.08)
				(name "S0")
				(number "9")
			)
			(pin output inverted
				(at 12.7 7.62 180)
				(length 5.08)
				(name "S1")
				(number "7")
			)
			(pin output inverted
				(at 12.7 5.08 180)
				(length 5.08)
				(name "S2")
				(number "6")
			)
			(pin output inverted
				(at 12.7 2.54 180)
				(length 5.08)
				(name "S3")
				(number "14")
			)
		)
		(symbol "74LS147_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS148"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74LS148"
			(at -7.62 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS148"
			(at 0 0 0)
		)
		(property "Description" "Priority Encoder 3 to 8 cascadable"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL ENCOD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS148_1_0"
			(pin input inverted
				(at -12.7 10.16 0)
				(length 5.08)
				(name "IO")
				(number "10")
			)
			(pin input inverted
				(at -12.7 7.62 0)
				(length 5.08)
				(name "I1")
				(number "11")
			)
			(pin input inverted
				(at -12.7 5.08 0)
				(length 5.08)
				(name "I2")
				(number "12")
			)
			(pin input inverted
				(at -12.7 2.54 0)
				(length 5.08)
				(name "I3")
				(number "13")
			)
			(pin input inverted
				(at -12.7 0 0)
				(length 5.08)
				(name "I4")
				(number "1")
			)
			(pin input inverted
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "I5")
				(number "2")
			)
			(pin input inverted
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "I6")
				(number "3")
			)
			(pin input inverted
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "I7")
				(number "4")
			)
			(pin input inverted
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "EI")
				(number "5")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin output inverted
				(at 12.7 10.16 180)
				(length 5.08)
				(name "S0")
				(number "9")
			)
			(pin output inverted
				(at 12.7 7.62 180)
				(length 5.08)
				(name "S1")
				(number "7")
			)
			(pin output inverted
				(at 12.7 5.08 180)
				(length 5.08)
				(name "S2")
				(number "6")
			)
			(pin output inverted
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "GS")
				(number "14")
			)
			(pin output inverted
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "EO")
				(number "15")
			)
		)
		(symbol "74LS148_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS15"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74LS15"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS15"
			(at 0 0 0)
		)
		(property "Description" "Triple 3-input AND"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL And3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "74LS15_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "13")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "12")
			)
		)
		(symbol "74LS15_1_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "1")
			)
			(pin input inverted
				(at -7.62 0 0)
				(length 4.953)
				(name "~")
				(number "2")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "13")
			)
			(pin open_collector inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "12")
			)
		)
		(symbol "74LS15_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "3")
			)
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LS15_2_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "3")
			)
			(pin input inverted
				(at -7.62 0 0)
				(length 4.953)
				(name "~")
				(number "4")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "5")
			)
			(pin open_collector inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LS15_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "10")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "11")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "74LS15_3_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "9")
			)
			(pin input inverted
				(at -7.62 0 0)
				(length 4.953)
				(name "~")
				(number "10")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "11")
			)
			(pin open_collector inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "74LS15_4_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74LS15_4_1")
		(embedded_fonts no)
	)
	(symbol "74LS151"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 19.05 0)
		)
		(property "Value" "74LS151"
			(at -7.62 -21.59 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS151"
			(at 0 0 0)
		)
		(property "Description" "Multiplexer 8 to 1"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL MUX8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS151_1_0"
			(pin input line
				(at -12.7 15.24 0)
				(length 5.08)
				(name "I0")
				(number "4")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "I1")
				(number "3")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "I2")
				(number "2")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "I3")
				(number "1")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "I4")
				(number "15")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "I5")
				(number "14")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "I6")
				(number "13")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "I7")
				(number "12")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "S0")
				(number "11")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "S1")
				(number "10")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "S2")
				(number "9")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 5.08)
				(name "~{E}")
				(number "7")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 12.7 15.24 180)
				(length 5.08)
				(name "Z")
				(number "5")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "~{Z}")
				(number "6")
			)
		)
		(symbol "74LS151_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS153"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 21.59 0)
		)
		(property "Value" "74LS153"
			(at -7.62 -24.13 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS153"
			(at 0 0 0)
		)
		(property "Description" "Dual Multiplexer 4 to 1"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL Mux4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS153_1_0"
			(pin input line
				(at -12.7 17.78 0)
				(length 5.08)
				(name "I0a")
				(number "6")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 5.08)
				(name "I1a")
				(number "5")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "I2a")
				(number "4")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "I3a")
				(number "3")
			)
			(pin input inverted
				(at -12.7 5.08 0)
				(length 5.08)
				(name "Ea")
				(number "1")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "I0b")
				(number "10")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "I1b")
				(number "11")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "I2b")
				(number "12")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "I3b")
				(number "13")
			)
			(pin input inverted
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "Eb")
				(number "15")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 5.08)
				(name "S0")
				(number "14")
			)
			(pin input line
				(at -12.7 -20.32 0)
				(length 5.08)
				(name "S1")
				(number "2")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 12.7 17.78 180)
				(length 5.08)
				(name "Za")
				(number "7")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "Zb")
				(number "9")
			)
		)
		(symbol "74LS153_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS154"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 21.59 0)
		)
		(property "Value" "74LS154"
			(at -7.62 -24.13 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS154"
			(at 0 0 0)
		)
		(property "Description" "Decoder 4 to 16"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL DECOD16 DECOD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?24*"
			(at 0 0 0)
		)
		(symbol "74LS154_1_0"
			(pin input line
				(at -12.7 17.78 0)
				(length 5.08)
				(name "A0")
				(number "23")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 5.08)
				(name "A1")
				(number "22")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "A2")
				(number "21")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "A3")
				(number "20")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "E0")
				(number "18")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "E1")
				(number "19")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 5.08)
				(name "VCC")
				(number "24")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 5.08)
				(name "GND")
				(number "12")
			)
			(pin output line
				(at 12.7 17.78 180)
				(length 5.08)
				(name "S0")
				(number "1")
			)
			(pin output line
				(at 12.7 15.24 180)
				(length 5.08)
				(name "S1")
				(number "2")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "S2")
				(number "3")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "S3")
				(number "4")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "S4")
				(number "5")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "S5")
				(number "6")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "S6")
				(number "7")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "S7")
				(number "8")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "S8")
				(number "9")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "S9")
				(number "10")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "S10")
				(number "11")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 5.08)
				(name "S11")
				(number "13")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 5.08)
				(name "S12")
				(number "14")
			)
			(pin output line
				(at 12.7 -15.24 180)
				(length 5.08)
				(name "S13")
				(number "15")
			)
			(pin output line
				(at 12.7 -17.78 180)
				(length 5.08)
				(name "S14")
				(number "16")
			)
			(pin output line
				(at 12.7 -20.32 180)
				(length 5.08)
				(name "S15")
				(number "17")
			)
		)
		(symbol "74LS154_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS155"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74LS155"
			(at -7.62 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS155"
			(at 0 0 0)
		)
		(property "Description" "Dual 2 to 4 lines Decoder/Demultiplexer"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL DECOD8 DECOD4 DEMUX4 DEMUX8 DEMUX DECOD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS155_1_0"
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "Ea1")
				(number "1")
			)
			(pin input inverted
				(at -12.7 7.62 0)
				(length 5.08)
				(name "Ea2")
				(number "2")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "A0")
				(number "13")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "A1")
				(number "3")
			)
			(pin input inverted
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "Eb1")
				(number "14")
			)
			(pin input inverted
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "Eb2")
				(number "15")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin output inverted
				(at 12.7 10.16 180)
				(length 5.08)
				(name "Q0a")
				(number "7")
			)
			(pin output inverted
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Q1a")
				(number "6")
			)
			(pin output inverted
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q2a")
				(number "5")
			)
			(pin output inverted
				(at 12.7 2.54 180)
				(length 5.08)
				(name "Q3a")
				(number "4")
			)
			(pin output inverted
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "Q0b")
				(number "9")
			)
			(pin output inverted
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "Q1b")
				(number "10")
			)
			(pin output inverted
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "Q2b")
				(number "11")
			)
			(pin output inverted
				(at 12.7 -10.16 180)
				(length 5.08)
				(name "Q3b")
				(number "12")
			)
		)
		(symbol "74LS155_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS157"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 19.05 0)
		)
		(property "Value" "74LS157"
			(at -7.62 -21.59 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS157"
			(at 0 0 0)
		)
		(property "Description" "Quad 2 to 1 line Multiplexer"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL MUX MUX2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS157_1_0"
			(pin input line
				(at -12.7 15.24 0)
				(length 5.08)
				(name "I0a")
				(number "2")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "I1a")
				(number "3")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "I0b")
				(number "5")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "I1b")
				(number "6")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "I0c")
				(number "11")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "I1c")
				(number "10")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "I0d")
				(number "14")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "I1d")
				(number "13")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 5.08)
				(name "S")
				(number "1")
			)
			(pin input inverted
				(at -12.7 -17.78 0)
				(length 5.08)
				(name "E")
				(number "15")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 12.7 15.24 180)
				(length 5.08)
				(name "Za")
				(number "4")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Zb")
				(number "7")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "Zc")
				(number "9")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "Zd")
				(number "12")
			)
		)
		(symbol "74LS157_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS158"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 19.05 0)
		)
		(property "Value" "74LS158"
			(at -7.62 -21.59 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS158"
			(at 0 0 0)
		)
		(property "Description" "Quad 2 to 1 multiplexer"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL Mux MUX2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS158_1_0"
			(pin input line
				(at -12.7 15.24 0)
				(length 5.08)
				(name "I0a")
				(number "2")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "I1a")
				(number "3")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "I0b")
				(number "5")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "I1b")
				(number "6")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "I0c")
				(number "14")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "I1c")
				(number "13")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "I0d")
				(number "11")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "I1d")
				(number "10")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 5.08)
				(name "S")
				(number "1")
			)
			(pin input inverted
				(at -12.7 -17.78 0)
				(length 5.08)
				(name "E")
				(number "15")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin output inverted
				(at 12.7 15.24 180)
				(length 5.08)
				(name "Za")
				(number "4")
			)
			(pin output inverted
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Zb")
				(number "7")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 5.08)
				(name "Zc")
				(number "12")
			)
			(pin output inverted
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "Zd")
				(number "9")
			)
		)
		(symbol "74LS158_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS161"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74LS161"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS161"
			(at 0 0 0)
		)
		(property "Description" "Synchronous 4-bit programmable binary Counter"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL CNT CNT4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS161_1_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "D0")
				(number "3")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "D1")
				(number "4")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "D2")
				(number "5")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "D3")
				(number "6")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "~{PE}")
				(number "9")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "CEP")
				(number "7")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "CET")
				(number "10")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "CP")
				(number "2")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "~{MR}")
				(number "1")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "Q0")
				(number "14")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "Q1")
				(number "13")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Q2")
				(number "12")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q3")
				(number "11")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "TC")
				(number "15")
			)
		)
		(symbol "74LS161_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS165"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 19.05 0)
		)
		(property "Value" "74LS165"
			(at -7.62 -21.59 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74ls165a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Shift Register 8-bit, parallel load"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL SR SR8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16* SO*16*3.9x9.9mm*P1.27mm* SSOP*16*5.3x6.2mm*P0.65mm* TSSOP*16*4.4x5mm*P0.65*"
			(at 0 0 0)
		)
		(symbol "74LS165_1_0"
			(pin input line
				(at -12.7 15.24 0)
				(length 5.08)
				(name "DS")
				(number "10")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "D0")
				(number "11")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "D1")
				(number "12")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "D2")
				(number "13")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "D3")
				(number "14")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "D4")
				(number "3")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "D5")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "D6")
				(number "5")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "D7")
				(number "6")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "~{PL}")
				(number "1")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 5.08)
				(name "CP")
				(number "2")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 5.08)
				(name "~{CE}")
				(number "15")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 12.7 15.24 180)
				(length 5.08)
				(name "Q7")
				(number "9")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "~{Q7}")
				(number "7")
			)
		)
		(symbol "74LS165_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS166"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 21.59 0)
		)
		(property "Value" "74LS166"
			(at -7.62 -21.59 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS166"
			(at 0 0 0)
		)
		(property "Description" "Shift Register 8-bit, parallel load"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL SR SR8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS166_1_0"
			(pin input line
				(at -12.7 17.78 0)
				(length 5.08)
				(name "Ds")
				(number "1")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 5.08)
				(name "A")
				(number "2")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "B")
				(number "3")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "C")
				(number "4")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "D")
				(number "5")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "E")
				(number "10")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "F")
				(number "11")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "G")
				(number "12")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "H")
				(number "14")
			)
			(pin input inverted
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "PE")
				(number "15")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "Clk")
				(number "7")
			)
			(pin input inverted
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "CE")
				(number "6")
			)
			(pin input inverted
				(at -12.7 -17.78 0)
				(length 5.08)
				(name "Clr")
				(number "9")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 12.7 17.78 180)
				(length 5.08)
				(name "Qh")
				(number "13")
			)
		)
		(symbol "74LS166_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS168"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 19.05 0)
		)
		(property "Value" "74LS168"
			(at -7.62 -19.05 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS168"
			(at 0 0 0)
		)
		(property "Description" "Synchronous 4-bit Up/Down Decimal counter"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL CNT CNT4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS168_1_0"
			(pin input line
				(at -12.7 15.24 0)
				(length 5.08)
				(name "P0")
				(number "3")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "P1")
				(number "4")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "P2")
				(number "5")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "P3")
				(number "6")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "~{PE}")
				(number "9")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "U/~{D}")
				(number "1")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "~{CEP}")
				(number "7")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "~{CET}")
				(number "10")
			)
			(pin input clock
				(at -12.7 -15.24 0)
				(length 5.08)
				(name "CP")
				(number "2")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 12.7 15.24 180)
				(length 5.08)
				(name "Q0")
				(number "14")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "Q1")
				(number "13")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "Q2")
				(number "12")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Q3")
				(number "11")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "~{TC}")
				(number "15")
			)
		)
		(symbol "74LS168_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS170"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74LS170"
			(at -7.62 -19.05 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS170"
			(at 0 0 0)
		)
		(property "Description" "4 x 4 Register Files Open Collector"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL Register OpenCol"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS170_1_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "D1")
				(number "15")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "D2")
				(number "1")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "D3")
				(number "2")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "D4")
				(number "3")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "Wa")
				(number "14")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "Wb")
				(number "13")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "~{Ew}")
				(number "12")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "Ra")
				(number "5")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "Rb")
				(number "4")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 5.08)
				(name "~{Er}")
				(number "11")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin tri_state line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "Q1")
				(number "10")
			)
			(pin tri_state line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "Q2")
				(number "9")
			)
			(pin tri_state line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Q3")
				(number "7")
			)
			(pin tri_state line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q4")
				(number "6")
			)
		)
		(symbol "74LS170_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS173"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 19.05 0)
		)
		(property "Value" "74LS173"
			(at -7.62 -19.05 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS173"
			(at 0 0 0)
		)
		(property "Description" "4-bit D-type Register, 3 state out"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL REG REG4 3State DFF"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS173_1_0"
			(pin input line
				(at -12.7 15.24 0)
				(length 5.08)
				(name "D0")
				(number "14")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "D1")
				(number "13")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "D2")
				(number "12")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "D3")
				(number "11")
			)
			(pin input inverted
				(at -12.7 2.54 0)
				(length 5.08)
				(name "Oe1")
				(number "1")
			)
			(pin input inverted
				(at -12.7 0 0)
				(length 5.08)
				(name "Oe2")
				(number "2")
			)
			(pin input inverted
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "E1")
				(number "9")
			)
			(pin input inverted
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "E2")
				(number "10")
			)
			(pin input clock
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "Cp")
				(number "7")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 5.08)
				(name "Mr")
				(number "15")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin tri_state line
				(at 12.7 15.24 180)
				(length 5.08)
				(name "Q0")
				(number "3")
			)
			(pin tri_state line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "Q1")
				(number "4")
			)
			(pin tri_state line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "Q2")
				(number "5")
			)
			(pin tri_state line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Q3")
				(number "6")
			)
		)
		(symbol "74LS173_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS174"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74LS174"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS174"
			(at 0 0 0)
		)
		(property "Description" "Hex D-type Flip-Flop, reset"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL REG REG6 DFF"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS174_1_0"
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "D0")
				(number "3")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "D1")
				(number "4")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "D2")
				(number "6")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "D3")
				(number "11")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "D4")
				(number "13")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "D5")
				(number "14")
			)
			(pin input clock
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "Cp")
				(number "9")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "~{Mr}")
				(number "1")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "Q0")
				(number "2")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Q1")
				(number "5")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q2")
				(number "7")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "Q3")
				(number "10")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "Q4")
				(number "12")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "Q5")
				(number "15")
			)
		)
		(symbol "74LS174_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS175"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74LS175"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS175"
			(at 0 0 0)
		)
		(property "Description" "4-bit D Flip-Flop, reset"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL REG REG4 DFF"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS175_1_0"
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "D0")
				(number "4")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "D1")
				(number "5")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "D2")
				(number "12")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "D3")
				(number "13")
			)
			(pin input clock
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "Cp")
				(number "9")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "~{Mr}")
				(number "1")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "Q0")
				(number "2")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "~{Q0}")
				(number "3")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q1")
				(number "7")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "~{Q1}")
				(number "6")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "Q2")
				(number "10")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "~{Q2}")
				(number "11")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "Q3")
				(number "15")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "~{Q3}")
				(number "14")
			)
		)
		(symbol "74LS175_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS181"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 21.59 0)
		)
		(property "Value" "74LS181"
			(at -7.62 -21.59 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "74xx/74F181.pdf"
			(at 0 0 0)
		)
		(property "Description" "Arithmetic logic unit"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL ALU ARITH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?24*"
			(at 0 0 0)
		)
		(symbol "74LS181_1_0"
			(text "Decod"
				(at -5.08 -6.35 900)
			)
			(text "A"
				(at -3.302 13.97 0)
			)
			(text "B"
				(at -3.302 3.81 0)
			)
			(text "S"
				(at 3.302 9.144 0)
			)
			(pin input line
				(at -15.24 17.78 0)
				(length 5.08)
				(name "A0")
				(number "2")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 5.08)
				(name "A1")
				(number "23")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 5.08)
				(name "A2")
				(number "21")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 5.08)
				(name "A3")
				(number "19")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 5.08)
				(name "B0")
				(number "1")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 5.08)
				(name "B1")
				(number "22")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "B2")
				(number "20")
			)
			(pin input line
				(at -15.24 0 0)
				(length 5.08)
				(name "B3")
				(number "18")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "S0")
				(number "6")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 5.08)
				(name "S1")
				(number "5")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 5.08)
				(name "S2")
				(number "4")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 5.08)
				(name "S3")
				(number "3")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 5.08)
				(name "M")
				(number "8")
			)
			(pin input inverted
				(at -15.24 -17.78 0)
				(length 5.08)
				(name "Cn")
				(number "7")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 5.08)
				(name "VCC")
				(number "24")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 5.08)
				(name "GND")
				(number "12")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 5.08)
				(name "F0")
				(number "9")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 5.08)
				(name "F1")
				(number "10")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 5.08)
				(name "F2")
				(number "11")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 5.08)
				(name "F3")
				(number "13")
			)
			(pin output inverted
				(at 15.24 -5.08 180)
				(length 5.08)
				(name "Cn+4")
				(number "16")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 5.08)
				(name "A=B")
				(number "14")
			)
			(pin output line
				(at 15.24 -12.7 180)
				(length 5.08)
				(name "Y")
				(number "17")
			)
			(pin output line
				(at 15.24 -15.24 180)
				(length 5.08)
				(name "X")
				(number "15")
			)
		)
		(symbol "74LS181_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS182"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74LS182"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS182"
			(at 0 0 0)
		)
		(property "Description" "Carry generator"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL ALU ARITH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS182_1_0"
			(pin input inverted
				(at -12.7 10.16 0)
				(length 5.08)
				(name "P0")
				(number "4")
			)
			(pin input inverted
				(at -12.7 7.62 0)
				(length 5.08)
				(name "P1")
				(number "2")
			)
			(pin input inverted
				(at -12.7 5.08 0)
				(length 5.08)
				(name "P2")
				(number "15")
			)
			(pin input inverted
				(at -12.7 2.54 0)
				(length 5.08)
				(name "P3")
				(number "6")
			)
			(pin input inverted
				(at -12.7 0 0)
				(length 5.08)
				(name "G0")
				(number "3")
			)
			(pin input inverted
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "G1")
				(number "1")
			)
			(pin input inverted
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "G2")
				(number "14")
			)
			(pin input inverted
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "G3")
				(number "5")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "Cn")
				(number "13")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "Cn+x")
				(number "12")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Cn+y")
				(number "11")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Cn+z")
				(number "9")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 5.08)
				(name "P")
				(number "7")
			)
			(pin output inverted
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "G")
				(number "10")
			)
		)
		(symbol "74LS182_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS190"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74LS190"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS190"
			(at 0 0 0)
		)
		(property "Description" "4-bit Synchronous Up/Down BCD Counter"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL CNT CNT4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS190_1_0"
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "P0")
				(number "15")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "P1")
				(number "1")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "P2")
				(number "10")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "P3")
				(number "9")
			)
			(pin input inverted
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "Pl")
				(number "11")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "D/U")
				(number "5")
			)
			(pin input inverted
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "Ce")
				(number "4")
			)
			(pin input clock
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "Cp")
				(number "14")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "Q0")
				(number "3")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Q1")
				(number "2")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q2")
				(number "6")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "Q3")
				(number "7")
			)
			(pin output inverted
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "Rc")
				(number "13")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "Tc")
				(number "12")
			)
		)
		(symbol "74LS190_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS192"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74LS192"
			(at 5.08 13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74ls193.pdf"
			(at 0 0 0)
		)
		(property "Description" "Synchronous 4-bit Up/Down (2 clk) counter"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL CNT CNT4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "74LS192_1_0"
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "A")
				(number "15")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "B")
				(number "1")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "C")
				(number "10")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "D")
				(number "9")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "~{LOAD}")
				(number "11")
			)
			(pin input clock
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "UP")
				(number "5")
			)
			(pin input clock
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "DOWN")
				(number "4")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "CLR")
				(number "14")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "QA")
				(number "3")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "QB")
				(number "2")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "QC")
				(number "6")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "QD")
				(number "7")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "~{CO}")
				(number "12")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "~{BO}")
				(number "13")
			)
		)
		(symbol "74LS192_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS194"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 19.05 0)
		)
		(property "Value" "74LS194"
			(at -7.62 -21.59 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS194"
			(at 0 0 0)
		)
		(property "Description" "Shift Register 4-bit Bidirectional"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL RS SR4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS194_1_0"
			(pin input line
				(at -12.7 15.24 0)
				(length 5.08)
				(name "P0")
				(number "3")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "P1")
				(number "4")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "P2")
				(number "5")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "P3")
				(number "6")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "Dsr")
				(number "2")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "Dsl")
				(number "7")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "S0")
				(number "9")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "S1")
				(number "10")
			)
			(pin input clock
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "Cp")
				(number "11")
			)
			(pin input inverted
				(at -12.7 -17.78 0)
				(length 5.08)
				(name "Mr")
				(number "1")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 12.7 15.24 180)
				(length 5.08)
				(name "Q0")
				(number "15")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "Q1")
				(number "14")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "Q2")
				(number "13")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Q3")
				(number "12")
			)
		)
		(symbol "74LS194_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS195"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74LS195"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS195"
			(at 0 0 0)
		)
		(property "Description" "Shift Register 4-bit, parallel"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL SR SR4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS195_1_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "P0")
				(number "4")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "P1")
				(number "5")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "P2")
				(number "6")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "P3")
				(number "7")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "J")
				(number "2")
			)
			(pin input clock
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "CP")
				(number "10")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "~{K}")
				(number "3")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "~{PE}")
				(number "9")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "~{MR}")
				(number "1")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "Q0")
				(number "15")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "Q1")
				(number "14")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Q2")
				(number "13")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q3")
				(number "12")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "~{Q3}")
				(number "11")
			)
		)
		(symbol "74LS195_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS196"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74LS196"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS196"
			(at 0 0 0)
		)
		(property "Description" "4 (3+1)-bit presettable BCD counter"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL CNT CNT4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "74LS196_1_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "P0")
				(number "4")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "P1")
				(number "10")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "P2")
				(number "3")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "P3")
				(number "11")
			)
			(pin input inverted
				(at -12.7 0 0)
				(length 5.08)
				(name "Pl")
				(number "1")
			)
			(pin input inverted_clock
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "Cp0")
				(number "8")
			)
			(pin input inverted_clock
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "Cp1")
				(number "6")
			)
			(pin input inverted
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "Mr")
				(number "13")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 5.08)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "Q0")
				(number "5")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "Q1")
				(number "9")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Q2")
				(number "2")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q3")
				(number "12")
			)
		)
		(symbol "74LS196_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS20"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74LS20"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS20"
			(at 0 0 0)
		)
		(property "Description" "Dual 4-input NAND"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL Nand4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?12*"
			(at 0 0 0)
		)
		(symbol "74LS20_1_1"
			(pin input line
				(at -7.62 3.81 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -7.62 1.27 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin input line
				(at -7.62 -1.27 0)
				(length 3.81)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -7.62 -3.81 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LS20_1_2"
			(pin input inverted
				(at -7.62 3.81 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin input inverted
				(at -7.62 1.27 0)
				(length 4.826)
				(name "~")
				(number "2")
			)
			(pin input inverted
				(at -7.62 -1.27 0)
				(length 4.826)
				(name "~")
				(number "4")
			)
			(pin input inverted
				(at -7.62 -3.81 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LS20_2_1"
			(pin input line
				(at -7.62 3.81 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin input line
				(at -7.62 1.27 0)
				(length 3.81)
				(name "~")
				(number "10")
			)
			(pin input line
				(at -7.62 -1.27 0)
				(length 3.81)
				(name "~")
				(number "12")
			)
			(pin input line
				(at -7.62 -3.81 0)
				(length 3.81)
				(name "~")
				(number "13")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "74LS20_2_2"
			(pin input inverted
				(at -7.62 3.81 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin input inverted
				(at -7.62 1.27 0)
				(length 4.826)
				(name "~")
				(number "10")
			)
			(pin input inverted
				(at -7.62 -1.27 0)
				(length 4.826)
				(name "~")
				(number "12")
			)
			(pin input inverted
				(at -7.62 -3.81 0)
				(length 3.81)
				(name "~")
				(number "13")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "74LS20_3_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74LS20_3_1")
		(embedded_fonts no)
	)
	(symbol "74LS21"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74LS21"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS21"
			(at 0 0 0)
		)
		(property "Description" "Dual 4-input AND"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL And4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?12*"
			(at 0 0 0)
		)
		(symbol "74LS21_1_1"
			(pin input line
				(at -7.62 3.81 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -7.62 1.27 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin input line
				(at -7.62 -1.27 0)
				(length 3.81)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -7.62 -3.81 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LS21_1_2"
			(pin input inverted
				(at -7.62 3.81 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin input inverted
				(at -7.62 1.27 0)
				(length 4.826)
				(name "~")
				(number "2")
			)
			(pin input inverted
				(at -7.62 -1.27 0)
				(length 4.826)
				(name "~")
				(number "4")
			)
			(pin input inverted
				(at -7.62 -3.81 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LS21_2_1"
			(pin input line
				(at -7.62 3.81 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin input line
				(at -7.62 1.27 0)
				(length 3.81)
				(name "~")
				(number "10")
			)
			(pin input line
				(at -7.62 -1.27 0)
				(length 3.81)
				(name "~")
				(number "12")
			)
			(pin input line
				(at -7.62 -3.81 0)
				(length 3.81)
				(name "~")
				(number "13")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "74LS21_2_2"
			(pin input inverted
				(at -7.62 3.81 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin input inverted
				(at -7.62 1.27 0)
				(length 4.826)
				(name "~")
				(number "10")
			)
			(pin input inverted
				(at -7.62 -1.27 0)
				(length 4.826)
				(name "~")
				(number "12")
			)
			(pin input inverted
				(at -7.62 -3.81 0)
				(length 3.81)
				(name "~")
				(number "13")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "74LS21_3_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74LS21_3_1")
		(embedded_fonts no)
	)
	(symbol "74LS221"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "74LS221"
			(at -7.62 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS221"
			(at 0 0 0)
		)
		(property "Description" "Dual Monostable"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL Monostable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS221_1_0"
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "~{A}")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "B")
				(number "2")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "~{CLR}")
				(number "3")
			)
			(pin input line
				(at 0 12.7 270)
				(length 5.08)
				(name "Cext")
				(number "14")
			)
			(pin input line
				(at 2.54 12.7 270)
				(length 5.08)
				(name "RCext")
				(number "15")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q")
				(number "13")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "~{Q}")
				(number "4")
			)
		)
		(symbol "74LS221_1_1")
		(symbol "74LS221_2_0"
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "~{A}")
				(number "9")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "B")
				(number "10")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "~{CLR}")
				(number "11")
			)
			(pin input line
				(at 0 12.7 270)
				(length 5.08)
				(name "Cext")
				(number "6")
			)
			(pin input line
				(at 2.54 12.7 270)
				(length 5.08)
				(name "RCext")
				(number "7")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q")
				(number "5")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "~{Q}")
				(number "12")
			)
		)
		(symbol "74LS221_2_1")
		(symbol "74LS221_3_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
		)
		(symbol "74LS221_3_1")
		(embedded_fonts no)
	)
	(symbol "74LS240"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74LS240"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74ls240.pdf"
			(at 0 0 0)
		)
		(property "Description" "Octal Buffer and Line Driver With 3-State Output, active-low enables, inverting outputs"
			(at 0 0 0)
		)
		(property "ki_keywords" "7400 logic ttl low power schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?20*"
			(at 0 0 0)
		)
		(symbol "74LS240_1_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "I0a")
				(number "2")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "I1a")
				(number "4")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "I2a")
				(number "6")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "I3a")
				(number "8")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "I0b")
				(number "11")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "I1b")
				(number "13")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "I2b")
				(number "15")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "I3b")
				(number "17")
			)
			(pin input inverted
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "OEa")
				(number "1")
			)
			(pin input inverted
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "OEb")
				(number "19")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 5.08)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 5.08)
				(name "GND")
				(number "10")
			)
			(pin tri_state inverted
				(at 12.7 12.7 180)
				(length 5.08)
				(name "O0a")
				(number "18")
			)
			(pin tri_state inverted
				(at 12.7 10.16 180)
				(length 5.08)
				(name "O1a")
				(number "16")
			)
			(pin tri_state inverted
				(at 12.7 7.62 180)
				(length 5.08)
				(name "O2a")
				(number "14")
			)
			(pin tri_state inverted
				(at 12.7 5.08 180)
				(length 5.08)
				(name "O3a")
				(number "12")
			)
			(pin tri_state inverted
				(at 12.7 2.54 180)
				(length 5.08)
				(name "O0b")
				(number "9")
			)
			(pin tri_state inverted
				(at 12.7 0 180)
				(length 5.08)
				(name "O1b")
				(number "7")
			)
			(pin tri_state inverted
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "O2b")
				(number "5")
			)
			(pin tri_state inverted
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "O3b")
				(number "3")
			)
		)
		(symbol "74LS240_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS240_Split"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74LS240_Split"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74ls240.pdf"
			(at 0 0 0)
		)
		(property "Description" "Octal Buffer and Line Driver With 3-State Output, active-low enables, inverting outputs, split symbol"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "7400 logic ttl low power schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*7.5x12.8mm*P1.27mm* *SSOP*5.3x7.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "74LS240_Split_1_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin input inverted
				(at 0 -6.35 90)
				(length 4.445)
				(name "~")
				(number "1")
			)
			(pin tri_state inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "18")
			)
		)
		(symbol "74LS240_Split_1_1")
		(symbol "74LS240_Split_2_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "4")
			)
			(pin tri_state inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "16")
			)
		)
		(symbol "74LS240_Split_2_1")
		(symbol "74LS240_Split_3_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "6")
			)
			(pin tri_state inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "14")
			)
		)
		(symbol "74LS240_Split_3_1")
		(symbol "74LS240_Split_4_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "8")
			)
			(pin tri_state inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "12")
			)
		)
		(symbol "74LS240_Split_4_1")
		(symbol "74LS240_Split_5_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "11")
			)
			(pin input inverted
				(at 0 -6.35 90)
				(length 4.445)
				(name "~")
				(number "19")
			)
			(pin tri_state inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "9")
			)
		)
		(symbol "74LS240_Split_5_1")
		(symbol "74LS240_Split_6_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "13")
			)
			(pin tri_state inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "7")
			)
		)
		(symbol "74LS240_Split_6_1")
		(symbol "74LS240_Split_7_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "15")
			)
			(pin tri_state inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "5")
			)
		)
		(symbol "74LS240_Split_7_1")
		(symbol "74LS240_Split_8_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "17")
			)
			(pin tri_state inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "3")
			)
		)
		(symbol "74LS240_Split_8_1")
		(symbol "74LS240_Split_9_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "10")
			)
		)
		(symbol "74LS240_Split_9_1")
		(embedded_fonts no)
	)
	(symbol "74LS241"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74LS241"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74ls241.pdf"
			(at 0 0 0)
		)
		(property "Description" "Octal Buffer and Line Driver With 3-State Output, complementary enables, non-inverting outputs"
			(at 0 0 0)
		)
		(property "ki_keywords" "7400 logic ttl low power schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?20*"
			(at 0 0 0)
		)
		(symbol "74LS241_1_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "I0a")
				(number "2")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "I1a")
				(number "4")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "I2a")
				(number "6")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "I3a")
				(number "8")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "I0b")
				(number "11")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "I1b")
				(number "13")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "I2b")
				(number "15")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "I3b")
				(number "17")
			)
			(pin input inverted
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "OEa")
				(number "1")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "OEb")
				(number "19")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 5.08)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 5.08)
				(name "GND")
				(number "10")
			)
			(pin tri_state line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "O0a")
				(number "18")
			)
			(pin tri_state line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "O1a")
				(number "16")
			)
			(pin tri_state line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "O2a")
				(number "14")
			)
			(pin tri_state line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "O3a")
				(number "12")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "O0b")
				(number "9")
			)
			(pin tri_state line
				(at 12.7 0 180)
				(length 5.08)
				(name "O1b")
				(number "7")
			)
			(pin tri_state line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "O2b")
				(number "5")
			)
			(pin tri_state line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "O3b")
				(number "3")
			)
		)
		(symbol "74LS241_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS241_Split"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74LS241_Split"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74ls241.pdf"
			(at 0 0 0)
		)
		(property "Description" "Octal Buffer and Line Driver With 3-State Output, complementary enables, non-inverting outputs, split symbol"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "7400 logic ttl low power schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*7.5x12.8mm*P1.27mm* *SSOP*5.3x7.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "74LS241_Split_1_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin input inverted
				(at 0 -6.35 90)
				(length 4.445)
				(name "~")
				(number "1")
			)
			(pin tri_state line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "18")
			)
		)
		(symbol "74LS241_Split_1_1")
		(symbol "74LS241_Split_2_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "4")
			)
			(pin tri_state line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "16")
			)
		)
		(symbol "74LS241_Split_2_1")
		(symbol "74LS241_Split_3_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "6")
			)
			(pin tri_state line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "14")
			)
		)
		(symbol "74LS241_Split_3_1")
		(symbol "74LS241_Split_4_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "8")
			)
			(pin tri_state line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "12")
			)
		)
		(symbol "74LS241_Split_4_1")
		(symbol "74LS241_Split_5_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "11")
			)
			(pin input line
				(at 0 -6.35 90)
				(length 4.445)
				(name "~")
				(number "19")
			)
			(pin tri_state line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "9")
			)
		)
		(symbol "74LS241_Split_5_1")
		(symbol "74LS241_Split_6_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "13")
			)
			(pin tri_state line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "7")
			)
		)
		(symbol "74LS241_Split_6_1")
		(symbol "74LS241_Split_7_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "15")
			)
			(pin tri_state line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "5")
			)
		)
		(symbol "74LS241_Split_7_1")
		(symbol "74LS241_Split_8_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "17")
			)
			(pin tri_state line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "3")
			)
		)
		(symbol "74LS241_Split_8_1")
		(symbol "74LS241_Split_9_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "10")
			)
		)
		(symbol "74LS241_Split_9_1")
		(embedded_fonts no)
	)
	(symbol "74LS242"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "74LS242"
			(at -7.62 -11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS242"
			(at 0 0 0)
		)
		(property "Description" "quad bus transceiver, inverting 3-state outputs"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "bus 3state"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?12*"
			(at 0 0 0)
		)
		(symbol "74LS242_1_0"
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "A0")
				(number "3")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "A1")
				(number "4")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "A2")
				(number "5")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "A3")
				(number "6")
			)
			(pin input inverted
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "OEa")
				(number "1")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "OEb")
				(number "13")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
			(pin tri_state inverted
				(at 12.7 7.62 180)
				(length 5.08)
				(name "B0")
				(number "11")
			)
			(pin tri_state inverted
				(at 12.7 5.08 180)
				(length 5.08)
				(name "B1")
				(number "10")
			)
			(pin tri_state inverted
				(at 12.7 2.54 180)
				(length 5.08)
				(name "B2")
				(number "9")
			)
			(pin tri_state inverted
				(at 12.7 0 180)
				(length 5.08)
				(name "B3")
				(number "8")
			)
		)
		(symbol "74LS242_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS243"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "74LS243"
			(at -7.62 -11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS243"
			(at 0 0 0)
		)
		(property "Description" "4-bit Bus Transceiver"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL Buffer 3State BUS BIDI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?12*"
			(at 0 0 0)
		)
		(symbol "74LS243_1_0"
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "A0")
				(number "3")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "A1")
				(number "4")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "A2")
				(number "5")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "A3")
				(number "6")
			)
			(pin input inverted
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "OEa")
				(number "1")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "OEb")
				(number "13")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
			(pin tri_state line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "B0")
				(number "11")
			)
			(pin tri_state line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "B1")
				(number "10")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "B2")
				(number "9")
			)
			(pin tri_state line
				(at 12.7 0 180)
				(length 5.08)
				(name "B3")
				(number "8")
			)
		)
		(symbol "74LS243_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS244"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74LS244"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74ls244.pdf"
			(at 0 0 0)
		)
		(property "Description" "Octal Buffer and Line Driver With 3-State Output, active-low enables, non-inverting outputs"
			(at 0 0 0)
		)
		(property "ki_keywords" "7400 logic ttl low power schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?20*"
			(at 0 0 0)
		)
		(symbol "74LS244_1_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "I0a")
				(number "2")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "I1a")
				(number "4")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "I2a")
				(number "6")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "I3a")
				(number "8")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "I0b")
				(number "11")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "I1b")
				(number "13")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "I2b")
				(number "15")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "I3b")
				(number "17")
			)
			(pin input inverted
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "OEa")
				(number "1")
			)
			(pin input inverted
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "OEb")
				(number "19")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 5.08)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 5.08)
				(name "GND")
				(number "10")
			)
			(pin tri_state line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "O0a")
				(number "18")
			)
			(pin tri_state line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "O1a")
				(number "16")
			)
			(pin tri_state line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "O2a")
				(number "14")
			)
			(pin tri_state line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "O3a")
				(number "12")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "O0b")
				(number "9")
			)
			(pin tri_state line
				(at 12.7 0 180)
				(length 5.08)
				(name "O1b")
				(number "7")
			)
			(pin tri_state line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "O2b")
				(number "5")
			)
			(pin tri_state line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "O3b")
				(number "3")
			)
		)
		(symbol "74LS244_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS244_Split"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74LS244_Split"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74ls241.pdf"
			(at 0 0 0)
		)
		(property "Description" "Octal Buffer and Line Driver With 3-State Output, active-low enables, non-inverting outputs, split symbol"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "7400 logic ttl low power schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*7.5x12.8mm*P1.27mm* *SSOP*5.3x7.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "74LS244_Split_1_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin input inverted
				(at 0 -6.35 90)
				(length 4.445)
				(name "~")
				(number "1")
			)
			(pin tri_state line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "18")
			)
		)
		(symbol "74LS244_Split_1_1")
		(symbol "74LS244_Split_2_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "4")
			)
			(pin tri_state line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "16")
			)
		)
		(symbol "74LS244_Split_2_1")
		(symbol "74LS244_Split_3_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "6")
			)
			(pin tri_state line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "14")
			)
		)
		(symbol "74LS244_Split_3_1")
		(symbol "74LS244_Split_4_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "8")
			)
			(pin tri_state line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "12")
			)
		)
		(symbol "74LS244_Split_4_1")
		(symbol "74LS244_Split_5_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "11")
			)
			(pin input inverted
				(at 0 -6.35 90)
				(length 4.445)
				(name "~")
				(number "19")
			)
			(pin tri_state line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "9")
			)
		)
		(symbol "74LS244_Split_5_1")
		(symbol "74LS244_Split_6_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "13")
			)
			(pin tri_state line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "7")
			)
		)
		(symbol "74LS244_Split_6_1")
		(symbol "74LS244_Split_7_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "15")
			)
			(pin tri_state line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "5")
			)
		)
		(symbol "74LS244_Split_7_1")
		(symbol "74LS244_Split_8_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "17")
			)
			(pin tri_state line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "3")
			)
		)
		(symbol "74LS244_Split_8_1")
		(symbol "74LS244_Split_9_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "10")
			)
		)
		(symbol "74LS244_Split_9_1")
		(embedded_fonts no)
	)
	(symbol "74LS245"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74LS245"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS245"
			(at 0 0 0)
		)
		(property "Description" "Octal BUS Transceivers, 3-State outputs"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL BUS 3State"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?20*"
			(at 0 0 0)
		)
		(symbol "74LS245_1_0"
			(pin tri_state line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "A0")
				(number "2")
			)
			(pin tri_state line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "A1")
				(number "3")
			)
			(pin tri_state line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "A2")
				(number "4")
			)
			(pin tri_state line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "A3")
				(number "5")
			)
			(pin tri_state line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "A4")
				(number "6")
			)
			(pin tri_state line
				(at -12.7 0 0)
				(length 5.08)
				(name "A5")
				(number "7")
			)
			(pin tri_state line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "A6")
				(number "8")
			)
			(pin tri_state line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "A7")
				(number "9")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "A->B")
				(number "1")
			)
			(pin input inverted
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "CE")
				(number "19")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 5.08)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 5.08)
				(name "GND")
				(number "10")
			)
			(pin tri_state line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "B0")
				(number "18")
			)
			(pin tri_state line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "B1")
				(number "17")
			)
			(pin tri_state line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "B2")
				(number "16")
			)
			(pin tri_state line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "B3")
				(number "15")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "B4")
				(number "14")
			)
			(pin tri_state line
				(at 12.7 0 180)
				(length 5.08)
				(name "B5")
				(number "13")
			)
			(pin tri_state line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "B6")
				(number "12")
			)
			(pin tri_state line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "B7")
				(number "11")
			)
		)
		(symbol "74LS245_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS247"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74LS247"
			(at -7.62 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS247"
			(at 0 0 0)
		)
		(property "Description" "BCD to 7 segments Decoder Open Collector active Low"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL DECOD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS247_1_0"
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "A")
				(number "7")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "B")
				(number "1")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "C")
				(number "2")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "D")
				(number "6")
			)
			(pin input inverted
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "Lt")
				(number "3")
			)
			(pin input inverted
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "Rbi")
				(number "5")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin open_collector inverted
				(at 12.7 10.16 180)
				(length 5.08)
				(name "a")
				(number "13")
			)
			(pin open_collector inverted
				(at 12.7 7.62 180)
				(length 5.08)
				(name "b")
				(number "12")
			)
			(pin open_collector inverted
				(at 12.7 5.08 180)
				(length 5.08)
				(name "c")
				(number "11")
			)
			(pin open_collector inverted
				(at 12.7 2.54 180)
				(length 5.08)
				(name "d")
				(number "10")
			)
			(pin open_collector inverted
				(at 12.7 0 180)
				(length 5.08)
				(name "e")
				(number "9")
			)
			(pin open_collector inverted
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "f")
				(number "15")
			)
			(pin open_collector inverted
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "g")
				(number "14")
			)
			(pin output inverted
				(at 12.7 -10.16 180)
				(length 5.08)
				(name "Rbo")
				(number "4")
			)
		)
		(symbol "74LS247_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS248"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74LS248"
			(at -7.62 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS248"
			(at 0 0 0)
		)
		(property "Description" "BCD to 7-segment Decoder, Active High"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL DECOD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS248_1_0"
			(pin input line
				(at -15.24 10.16 0)
				(length 5.08)
				(name "A")
				(number "7")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 5.08)
				(name "B")
				(number "1")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 5.08)
				(name "C")
				(number "2")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "D")
				(number "6")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 5.08)
				(name "~{LT}")
				(number "3")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 5.08)
				(name "~{RBI}")
				(number "5")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin open_collector line
				(at 15.24 10.16 180)
				(length 5.08)
				(name "a")
				(number "13")
			)
			(pin open_collector line
				(at 15.24 7.62 180)
				(length 5.08)
				(name "b")
				(number "12")
			)
			(pin open_collector line
				(at 15.24 5.08 180)
				(length 5.08)
				(name "c")
				(number "11")
			)
			(pin open_collector line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "d")
				(number "10")
			)
			(pin open_collector line
				(at 15.24 0 180)
				(length 5.08)
				(name "e")
				(number "9")
			)
			(pin open_collector line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "f")
				(number "15")
			)
			(pin open_collector line
				(at 15.24 -5.08 180)
				(length 5.08)
				(name "g")
				(number "14")
			)
			(pin open_collector line
				(at 15.24 -10.16 180)
				(length 5.08)
				(name "~{BI}/~{RBO}")
				(number "4")
			)
		)
		(symbol "74LS248_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS251"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 19.05 0)
		)
		(property "Value" "74LS251"
			(at -7.62 -21.59 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS251"
			(at 0 0 0)
		)
		(property "Description" "Multiplexer 8 to 1, 3-state Outputs"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL MUX MUX8 3State"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS251_1_0"
			(pin input line
				(at -12.7 15.24 0)
				(length 5.08)
				(name "I0")
				(number "4")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "I1")
				(number "3")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "I2")
				(number "2")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "I3")
				(number "1")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "I4")
				(number "15")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "I5")
				(number "14")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "I6")
				(number "13")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "I7")
				(number "12")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "S0")
				(number "11")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "S1")
				(number "10")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "S2")
				(number "9")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 5.08)
				(name "~{OE}")
				(number "7")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin tri_state line
				(at 12.7 15.24 180)
				(length 5.08)
				(name "Y")
				(number "5")
			)
			(pin tri_state line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "~{Y}")
				(number "6")
			)
		)
		(symbol "74LS251_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS253"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 21.59 0)
		)
		(property "Value" "74LS253"
			(at -7.62 -24.13 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS253"
			(at 0 0 0)
		)
		(property "Description" "Dual Multiplexer 4 to 1, 3-State Outputs"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL MUX MUX4 3State"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS253_1_0"
			(pin input line
				(at -12.7 17.78 0)
				(length 5.08)
				(name "I0a")
				(number "6")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 5.08)
				(name "I1a")
				(number "5")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "I2a")
				(number "4")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "I3a")
				(number "3")
			)
			(pin input inverted
				(at -12.7 5.08 0)
				(length 5.08)
				(name "OEa")
				(number "1")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "I0b")
				(number "10")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "I1b")
				(number "11")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "I2b")
				(number "12")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "I3b")
				(number "13")
			)
			(pin input inverted
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "OEb")
				(number "15")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 5.08)
				(name "A0")
				(number "14")
			)
			(pin input line
				(at -12.7 -20.32 0)
				(length 5.08)
				(name "A1")
				(number "2")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin tri_state line
				(at 12.7 17.78 180)
				(length 5.08)
				(name "Za")
				(number "7")
			)
			(pin tri_state line
				(at 12.7 0 180)
				(length 5.08)
				(name "Zb")
				(number "9")
			)
		)
		(symbol "74LS253_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS256"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74LS256"
			(at -7.62 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://alfter.us/wp-content/uploads/2022/12/74LS256.pdf"
			(at 0 0 0)
		)
		(property "Description" "dual 4-bit addressable latch"
			(at 0 0 0)
		)
		(property "ki_keywords" "latch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS256_1_0"
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "A0")
				(number "1")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "Da")
				(number "3")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "Db")
				(number "13")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "~{E}")
				(number "14")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "~{CL}")
				(number "15")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "Q_{0a}")
				(number "4")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Q_{1a}")
				(number "5")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q_{2a}")
				(number "6")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "Q_{3a}")
				(number "7")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "Q_{0b}")
				(number "9")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "Q_{1b}")
				(number "10")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "Q_{2b}")
				(number "11")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 5.08)
				(name "Q_{3b}")
				(number "12")
			)
		)
		(symbol "74LS256_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS257"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 19.05 0)
		)
		(property "Value" "74LS257"
			(at -7.62 -21.59 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS257"
			(at 0 0 0)
		)
		(property "Description" "Quad 2 to 1 Multiplexer"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL MUX MUX2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS257_1_0"
			(pin input line
				(at -12.7 15.24 0)
				(length 5.08)
				(name "I0a")
				(number "2")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "I1a")
				(number "3")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "I0b")
				(number "5")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "I1b")
				(number "6")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "I0c")
				(number "14")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "I1c")
				(number "13")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "I0d")
				(number "11")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "I1d")
				(number "10")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 5.08)
				(name "S")
				(number "1")
			)
			(pin input inverted
				(at -12.7 -17.78 0)
				(length 5.08)
				(name "OE")
				(number "15")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin tri_state line
				(at 12.7 15.24 180)
				(length 5.08)
				(name "Za")
				(number "4")
			)
			(pin tri_state line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Zb")
				(number "7")
			)
			(pin tri_state line
				(at 12.7 0 180)
				(length 5.08)
				(name "Zc")
				(number "12")
			)
			(pin tri_state line
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "Zd")
				(number "9")
			)
		)
		(symbol "74LS257_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS258"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 19.05 0)
		)
		(property "Value" "74LS258"
			(at -7.62 -21.59 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS258"
			(at 0 0 0)
		)
		(property "Description" "Quad 2 to 1 Multiplexer, inverting"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL MUX MUX2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS258_1_0"
			(pin input line
				(at -12.7 15.24 0)
				(length 5.08)
				(name "I0a")
				(number "2")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "I1a")
				(number "3")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "I0b")
				(number "5")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "I1b")
				(number "6")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "I0c")
				(number "14")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "I1c")
				(number "13")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "I0d")
				(number "11")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "I1d")
				(number "10")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 5.08)
				(name "S")
				(number "1")
			)
			(pin input inverted
				(at -12.7 -17.78 0)
				(length 5.08)
				(name "OE")
				(number "15")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin tri_state inverted
				(at 12.7 15.24 180)
				(length 5.08)
				(name "Za")
				(number "4")
			)
			(pin tri_state inverted
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Zb")
				(number "7")
			)
			(pin tri_state inverted
				(at 12.7 0 180)
				(length 5.08)
				(name "Zc")
				(number "12")
			)
			(pin tri_state inverted
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "Zd")
				(number "9")
			)
		)
		(symbol "74LS258_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS259"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74LS259"
			(at -7.62 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS259"
			(at 0 0 0)
		)
		(property "Description" "8-bit addressable latch"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL REG DFF"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS259_1_0"
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "D")
				(number "13")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "A0")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "A2")
				(number "3")
			)
			(pin input inverted
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "E")
				(number "14")
			)
			(pin input inverted
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "Clr")
				(number "15")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "Q0")
				(number "4")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Q1")
				(number "5")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q2")
				(number "6")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "Q3")
				(number "7")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "Q4")
				(number "9")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "Q5")
				(number "10")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "Q6")
				(number "11")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "Q7")
				(number "12")
			)
		)
		(symbol "74LS259_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS26"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74LS26"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS26"
			(at 0 0 0)
		)
		(property "Description" "Quad 2-input NAND Open collector"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL Nand2 OpenCol"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "74LS26_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin open_collector inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "3")
			)
		)
		(symbol "74LS26_1_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "1")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "2")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "3")
			)
		)
		(symbol "74LS26_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin open_collector inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LS26_2_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "4")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "5")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LS26_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "10")
			)
			(pin open_collector inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "74LS26_3_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "9")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "10")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "74LS26_4_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "12")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "13")
			)
			(pin open_collector inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "11")
			)
		)
		(symbol "74LS26_4_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "12")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "13")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "11")
			)
		)
		(symbol "74LS26_5_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74LS26_5_1")
		(embedded_fonts no)
	)
	(symbol "74LS27"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74LS27"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS27"
			(at 0 0 0)
		)
		(property "Description" "Triple 3-input NOR"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL Nor3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "74LS27_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -7.62 0 0)
				(length 4.953)
				(name "~")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "13")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "12")
			)
		)
		(symbol "74LS27_1_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin input inverted
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "13")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "12")
			)
		)
		(symbol "74LS27_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "3")
			)
			(pin input line
				(at -7.62 0 0)
				(length 4.953)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "5")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LS27_2_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "3")
			)
			(pin input inverted
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "4")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LS27_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "9")
			)
			(pin input line
				(at -7.62 0 0)
				(length 4.953)
				(name "~")
				(number "10")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "11")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "74LS27_3_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin input inverted
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "10")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "11")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "74LS27_4_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74LS27_4_1")
		(embedded_fonts no)
	)
	(symbol "74LS273"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74LS273"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS273"
			(at 0 0 0)
		)
		(property "Description" "8-bit D Flip-Flop, reset"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL DFF DFF8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?20* SO?20* SOIC?20*"
			(at 0 0 0)
		)
		(symbol "74LS273_1_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "D0")
				(number "3")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "D1")
				(number "4")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "D2")
				(number "7")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "D3")
				(number "8")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "D4")
				(number "13")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "D5")
				(number "14")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "D6")
				(number "17")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "D7")
				(number "18")
			)
			(pin input clock
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "Cp")
				(number "11")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "~{Mr}")
				(number "1")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 5.08)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 5.08)
				(name "GND")
				(number "10")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "Q0")
				(number "2")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "Q1")
				(number "5")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Q2")
				(number "6")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q3")
				(number "9")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "Q4")
				(number "12")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "Q5")
				(number "15")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "Q6")
				(number "16")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "Q7")
				(number "19")
			)
		)
		(symbol "74LS273_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS279"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.874 8.636 0)
		)
		(property "Value" "74LS279"
			(at -4.318 -8.636 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/sn54ls279a"
			(at 10.922 -12.954 0)
		)
		(property "Description" "Quad SR latch, DIP-16/SOIC-16/SOIC-16W"
			(at 7.62 -10.668 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL latch set reset srs flip flop flipflop rs-flipflop"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* SOIC*5.3x10.2mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "74LS279_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~{S}")
				(number "2")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "~{S}")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~{R}")
				(number "1")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "Q")
				(number "4")
			)
		)
		(symbol "74LS279_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~{S}")
				(number "6")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~{R}")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "Q")
				(number "7")
			)
		)
		(symbol "74LS279_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~{S}")
				(number "11")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "~{S}")
				(number "12")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~{R}")
				(number "10")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "Q")
				(number "9")
			)
		)
		(symbol "74LS279_4_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~{S}")
				(number "15")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~{R}")
				(number "14")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "Q")
				(number "13")
			)
		)
		(symbol "74LS279_5_0"
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
		)
		(symbol "74LS279_5_1")
		(embedded_fonts no)
	)
	(symbol "74LS280"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74LS280"
			(at -7.62 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS280"
			(at 0 0 0)
		)
		(property "Description" "Parity Generator/Checker"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL ALU Arith"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "74LS280_1_0"
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "A")
				(number "8")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "B")
				(number "9")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "C")
				(number "10")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "D")
				(number "11")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "E")
				(number "12")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "F")
				(number "13")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "G")
				(number "1")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "H")
				(number "2")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "I")
				(number "4")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 5.08)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "Even")
				(number "5")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Odd")
				(number "6")
			)
		)
		(symbol "74LS280_1_1"
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LS283"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74LS283"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS283"
			(at 0 0 0)
		)
		(property "Description" "4-bit full Adder"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL ADD Arith ALU"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS283_1_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "C0")
				(number "7")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "A1")
				(number "5")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "A2")
				(number "3")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "A3")
				(number "14")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "A4")
				(number "12")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "B1")
				(number "6")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "B2")
				(number "2")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "B3")
				(number "15")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "B4")
				(number "11")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "S1")
				(number "4")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "S2")
				(number "1")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "S3")
				(number "13")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "S4")
				(number "10")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "C4")
				(number "9")
			)
		)
		(symbol "74LS283_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS290"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "74LS290"
			(at -7.62 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS290"
			(at 0 0 0)
		)
		(property "Description" "4-bit BCD counter"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL CNT CNT4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?12*"
			(at 0 0 0)
		)
		(symbol "74LS290_1_0"
			(pin input inverted_clock
				(at -12.7 7.62 0)
				(length 5.08)
				(name "Cp0")
				(number "10")
			)
			(pin input inverted_clock
				(at -12.7 5.08 0)
				(length 5.08)
				(name "Cp1")
				(number "11")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "Ms2")
				(number "3")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "Ms1")
				(number "1")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "Mr1")
				(number "12")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "Mr2")
				(number "13")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Q0")
				(number "9")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q1")
				(number "5")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "Q2")
				(number "4")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "Q3")
				(number "8")
			)
		)
		(symbol "74LS290_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS295"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74LS295"
			(at -7.62 -19.05 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS295"
			(at 0 0 0)
		)
		(property "Description" "4-bit bidirectional register, 3-state outputs"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "register"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "74LS295_1_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "Ds")
				(number "1")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "P0")
				(number "2")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "P1")
				(number "3")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "P2")
				(number "4")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "P3")
				(number "5")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "Pe")
				(number "6")
			)
			(pin input inverted_clock
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "Cp")
				(number "9")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 5.08)
				(name "OE")
				(number "8")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 5.08)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "Q0")
				(number "13")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "Q1")
				(number "12")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Q2")
				(number "11")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q3")
				(number "10")
			)
		)
		(symbol "74LS295_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS298"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74LS298"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS298"
			(at 0 0 0)
		)
		(property "Description" "Quad 2 to 1 multiplexer with storage"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL MUX MUX2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS298_1_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "I0a")
				(number "3")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "I1a")
				(number "2")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "I0b")
				(number "4")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "I1b")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "I0c")
				(number "9")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "I1c")
				(number "5")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "I0d")
				(number "7")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "I1d")
				(number "6")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "S")
				(number "10")
			)
			(pin input inverted_clock
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "Cp")
				(number "11")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "Qa")
				(number "15")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Qb")
				(number "14")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "Qc")
				(number "13")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "Qd")
				(number "12")
			)
		)
		(symbol "74LS298_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS299"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74LS299"
			(at -7.62 -19.05 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS299"
			(at 0 0 0)
		)
		(property "Description" "8-bit Universal shift/storage Register"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL REG SR SR8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?20*"
			(at 0 0 0)
		)
		(symbol "74LS299_1_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "Ds0")
				(number "11")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "Ds7")
				(number "18")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "S0")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "S1")
				(number "19")
			)
			(pin input inverted
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "OE1")
				(number "2")
			)
			(pin input inverted
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "OE2")
				(number "3")
			)
			(pin input clock
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "Cp")
				(number "12")
			)
			(pin input inverted
				(at -12.7 -15.24 0)
				(length 5.08)
				(name "Mr")
				(number "9")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 5.08)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 5.08)
				(name "GND")
				(number "10")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "Q0")
				(number "8")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "Q7")
				(number "17")
			)
			(pin tri_state line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "IO0")
				(number "7")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "IO1")
				(number "13")
			)
			(pin tri_state line
				(at 12.7 0 180)
				(length 5.08)
				(name "IO2")
				(number "6")
			)
			(pin tri_state line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "IO3")
				(number "14")
			)
			(pin tri_state line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "IO4")
				(number "5")
			)
			(pin tri_state line
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "IO5")
				(number "15")
			)
			(pin tri_state line
				(at 12.7 -10.16 180)
				(length 5.08)
				(name "IO6")
				(number "4")
			)
			(pin tri_state line
				(at 12.7 -12.7 180)
				(length 5.08)
				(name "IO7")
				(number "16")
			)
		)
		(symbol "74LS299_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS30"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74LS30"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS30"
			(at 0 0 0)
		)
		(property "Description" "8-input NAND"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL Nand8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "74LS30_1_1"
			(pin input line
				(at -7.62 7.62 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "3")
			)
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 3.81)
				(name "~")
				(number "6")
			)
			(pin input line
				(at -7.62 -7.62 0)
				(length 3.81)
				(name "~")
				(number "11")
			)
			(pin input line
				(at -7.62 -10.16 0)
				(length 3.81)
				(name "~")
				(number "12")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "74LS30_1_2"
			(pin input inverted
				(at -7.62 7.62 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin input inverted
				(at -7.62 5.08 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin input inverted
				(at -7.62 2.54 0)
				(length 4.5466)
				(name "~")
				(number "3")
			)
			(pin input inverted
				(at -7.62 0 0)
				(length 5.08)
				(name "~")
				(number "4")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 4.5466)
				(name "~")
				(number "5")
			)
			(pin input inverted
				(at -7.62 -5.08 0)
				(length 3.81)
				(name "~")
				(number "6")
			)
			(pin input inverted
				(at -7.62 -7.62 0)
				(length 3.81)
				(name "~")
				(number "11")
			)
			(pin input inverted
				(at -7.62 -10.16 0)
				(length 3.81)
				(name "~")
				(number "12")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "74LS30_2_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74LS30_2_1")
		(embedded_fonts no)
	)
	(symbol "74LS32"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74LS32"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS32"
			(at 0 0 0)
		)
		(property "Description" "Quad 2-input OR"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL Or2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?14*"
			(at 0 0 0)
		)
		(symbol "74LS32_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "3")
			)
		)
		(symbol "74LS32_1_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "3")
			)
		)
		(symbol "74LS32_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LS32_2_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "4")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LS32_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "9")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "10")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "74LS32_3_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "10")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "74LS32_4_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "12")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "13")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "11")
			)
		)
		(symbol "74LS32_4_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "12")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "13")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "11")
			)
		)
		(symbol "74LS32_5_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74LS32_5_1")
		(embedded_fonts no)
	)
	(symbol "74LS322"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74LS322"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS322"
			(at 0 0 0)
		)
		(property "Description" "8-bit shift register, sign extend, 3-state outputs"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "register"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?20*"
			(at 0 0 0)
		)
		(symbol "74LS322_1_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "D0")
				(number "3")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "D1")
				(number "17")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "DS")
				(number "19")
			)
			(pin input inverted
				(at -12.7 5.08 0)
				(length 5.08)
				(name "SE")
				(number "18")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "S/P")
				(number "2")
			)
			(pin input inverted
				(at -12.7 0 0)
				(length 5.08)
				(name "G")
				(number "1")
			)
			(pin input inverted
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "OE")
				(number "8")
			)
			(pin input clock
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "Clk")
				(number "11")
			)
			(pin input inverted
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "Clr")
				(number "9")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 5.08)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 5.08)
				(name "GND")
				(number "10")
			)
			(pin tri_state line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "A/Qa")
				(number "4")
			)
			(pin tri_state line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "B/Qb")
				(number "16")
			)
			(pin tri_state line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "C/Qc")
				(number "5")
			)
			(pin tri_state line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "D/Qd")
				(number "15")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "E/Qe")
				(number "6")
			)
			(pin tri_state line
				(at 12.7 0 180)
				(length 5.08)
				(name "F/Qf")
				(number "14")
			)
			(pin tri_state line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "G/Qg")
				(number "7")
			)
			(pin tri_state line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "H/Qh")
				(number "13")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 5.08)
				(name "Qh")
				(number "12")
			)
		)
		(symbol "74LS322_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS323"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74LS323"
			(at -7.62 -19.05 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS323"
			(at 0 0 0)
		)
		(property "Description" "8-bit Universal Shift/Storage Register"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL REG SR SR8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?20*"
			(at 0 0 0)
		)
		(symbol "74LS323_1_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "DS0")
				(number "11")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "DS7")
				(number "18")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "S0")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "S1")
				(number "19")
			)
			(pin input inverted
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "SR")
				(number "9")
			)
			(pin input clock
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "Cp")
				(number "12")
			)
			(pin input inverted
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "OE1")
				(number "2")
			)
			(pin input inverted
				(at -12.7 -15.24 0)
				(length 5.08)
				(name "OE2")
				(number "3")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 5.08)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 5.08)
				(name "GND")
				(number "10")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "Q7")
				(number "17")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "Q0")
				(number "8")
			)
			(pin tri_state line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "IO0")
				(number "7")
			)
			(pin tri_state line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "IO1")
				(number "13")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "IO2")
				(number "6")
			)
			(pin tri_state line
				(at 12.7 0 180)
				(length 5.08)
				(name "IO3")
				(number "14")
			)
			(pin tri_state line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "IO4")
				(number "5")
			)
			(pin tri_state line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "IO5")
				(number "15")
			)
			(pin tri_state line
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "IO6")
				(number "4")
			)
			(pin tri_state line
				(at 12.7 -10.16 180)
				(length 5.08)
				(name "IO7")
				(number "16")
			)
		)
		(symbol "74LS323_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS33"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74LS33"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS33"
			(at 0 0 0)
		)
		(property "Description" "Quad 2-input NOR, Open collector"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL Nor2 OpenColl"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "74LS33_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "3")
			)
			(pin open_collector inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "1")
			)
		)
		(symbol "74LS33_1_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "3")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "1")
			)
		)
		(symbol "74LS33_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "6")
			)
			(pin open_collector inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "4")
			)
		)
		(symbol "74LS33_2_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "6")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "4")
			)
		)
		(symbol "74LS33_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "8")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "9")
			)
			(pin open_collector inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "10")
			)
		)
		(symbol "74LS33_3_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "8")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "10")
			)
		)
		(symbol "74LS33_4_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.318)
				(name "~")
				(number "11")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.318)
				(name "~")
				(number "12")
			)
			(pin open_collector inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "13")
			)
		)
		(symbol "74LS33_4_2"
			(pin input inverted
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "11")
			)
			(pin input inverted
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "12")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "13")
			)
		)
		(symbol "74LS33_5_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74LS33_5_1")
		(embedded_fonts no)
	)
	(symbol "74LS348"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74LS348"
			(at -7.62 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS348"
			(at 0 0 0)
		)
		(property "Description" "8 to 3 lines Priority Encoder"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL ENCOD Arith"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS348_1_0"
			(pin input inverted
				(at -12.7 10.16 0)
				(length 5.08)
				(name "EI")
				(number "5")
			)
			(pin input inverted
				(at -12.7 7.62 0)
				(length 5.08)
				(name "0")
				(number "10")
			)
			(pin input inverted
				(at -12.7 5.08 0)
				(length 5.08)
				(name "1")
				(number "11")
			)
			(pin input inverted
				(at -12.7 2.54 0)
				(length 5.08)
				(name "2")
				(number "12")
			)
			(pin input inverted
				(at -12.7 0 0)
				(length 5.08)
				(name "3")
				(number "13")
			)
			(pin input inverted
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "4")
				(number "1")
			)
			(pin input inverted
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "5")
				(number "2")
			)
			(pin input inverted
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "6")
				(number "3")
			)
			(pin input inverted
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "7")
				(number "4")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin tri_state inverted
				(at 12.7 10.16 180)
				(length 5.08)
				(name "A0")
				(number "9")
			)
			(pin tri_state inverted
				(at 12.7 7.62 180)
				(length 5.08)
				(name "A1")
				(number "7")
			)
			(pin tri_state inverted
				(at 12.7 5.08 180)
				(length 5.08)
				(name "A2")
				(number "6")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 5.08)
				(name "GS")
				(number "14")
			)
			(pin output inverted
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "E0")
				(number "15")
			)
		)
		(symbol "74LS348_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS352"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 21.59 0)
		)
		(property "Value" "74LS352"
			(at -7.62 -24.13 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS352"
			(at 0 0 0)
		)
		(property "Description" "Dual 4 to 1 line Multiplexer"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL Mux MUX4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS352_1_0"
			(pin input line
				(at -12.7 17.78 0)
				(length 5.08)
				(name "I0a")
				(number "6")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 5.08)
				(name "I1a")
				(number "5")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "I2a")
				(number "4")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "I3a")
				(number "3")
			)
			(pin input inverted
				(at -12.7 5.08 0)
				(length 5.08)
				(name "Ea")
				(number "1")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "I0b")
				(number "10")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "I1b")
				(number "11")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "I2b")
				(number "12")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "I3b")
				(number "13")
			)
			(pin input inverted
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "Eb")
				(number "15")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 5.08)
				(name "S0")
				(number "14")
			)
			(pin input line
				(at -12.7 -20.32 0)
				(length 5.08)
				(name "S1")
				(number "2")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin output inverted
				(at 12.7 17.78 180)
				(length 5.08)
				(name "Za")
				(number "7")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 5.08)
				(name "Zb")
				(number "9")
			)
		)
		(symbol "74LS352_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS353"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 21.59 0)
		)
		(property "Value" "74LS353"
			(at -7.62 -24.13 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS353"
			(at 0 0 0)
		)
		(property "Description" "Dual 4 to 1 line Multiplexer, inverter"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL MUX MUX2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS353_1_0"
			(pin input line
				(at -12.7 17.78 0)
				(length 5.08)
				(name "I0a")
				(number "6")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 5.08)
				(name "I1a")
				(number "5")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "I2a")
				(number "4")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "I3a")
				(number "3")
			)
			(pin input inverted
				(at -12.7 5.08 0)
				(length 5.08)
				(name "OEa")
				(number "1")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "I0b")
				(number "10")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "I1b")
				(number "11")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "I2b")
				(number "12")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "I3b")
				(number "13")
			)
			(pin input inverted
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "OEb")
				(number "15")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 5.08)
				(name "A0")
				(number "14")
			)
			(pin input line
				(at -12.7 -20.32 0)
				(length 5.08)
				(name "A1")
				(number "2")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin tri_state inverted
				(at 12.7 17.78 180)
				(length 5.08)
				(name "Za")
				(number "7")
			)
			(pin tri_state inverted
				(at 12.7 0 180)
				(length 5.08)
				(name "Zb")
				(number "9")
			)
		)
		(symbol "74LS353_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS365"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74LS365"
			(at -7.62 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS365"
			(at 0 0 0)
		)
		(property "Description" "Hex Bus Driver, 3-State Outputs"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL Buffer BUS 3State"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS365_1_0"
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "I1")
				(number "2")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "I2")
				(number "4")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "I3")
				(number "6")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "I4")
				(number "10")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "I5")
				(number "12")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "I6")
				(number "14")
			)
			(pin input inverted
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "E1")
				(number "1")
			)
			(pin input inverted
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "E2")
				(number "15")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin tri_state line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "O1")
				(number "3")
			)
			(pin tri_state line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "O2")
				(number "5")
			)
			(pin tri_state line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "O3")
				(number "7")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "O4")
				(number "9")
			)
			(pin tri_state line
				(at 12.7 0 180)
				(length 5.08)
				(name "O5")
				(number "11")
			)
			(pin tri_state line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "O6")
				(number "13")
			)
		)
		(symbol "74LS365_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS366"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74LS366"
			(at -7.62 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS366"
			(at 0 0 0)
		)
		(property "Description" "Hex Bus Driver inverter, 3-state outputs"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL Buffer BUS 3State"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS366_1_0"
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "I1")
				(number "2")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "I2")
				(number "4")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "I3")
				(number "6")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "I4")
				(number "10")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "I5")
				(number "12")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "I6")
				(number "14")
			)
			(pin input inverted
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "E1")
				(number "1")
			)
			(pin input inverted
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "E2")
				(number "15")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin tri_state inverted
				(at 12.7 10.16 180)
				(length 5.08)
				(name "O1")
				(number "3")
			)
			(pin tri_state inverted
				(at 12.7 7.62 180)
				(length 5.08)
				(name "O2")
				(number "5")
			)
			(pin tri_state inverted
				(at 12.7 5.08 180)
				(length 5.08)
				(name "O3")
				(number "7")
			)
			(pin tri_state inverted
				(at 12.7 2.54 180)
				(length 5.08)
				(name "O4")
				(number "9")
			)
			(pin tri_state inverted
				(at 12.7 0 180)
				(length 5.08)
				(name "O5")
				(number "11")
			)
			(pin tri_state inverted
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "O6")
				(number "13")
			)
		)
		(symbol "74LS366_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS367"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74LS367"
			(at -7.62 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS367"
			(at 0 0 0)
		)
		(property "Description" "Hex Bus Driver 3-state outputs"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL Buffer BUS 3State"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS367_1_0"
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "I1")
				(number "2")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "I2")
				(number "4")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "I3")
				(number "6")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "I4")
				(number "10")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "I5")
				(number "12")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "I6")
				(number "14")
			)
			(pin input inverted
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "OEa")
				(number "1")
			)
			(pin input inverted
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "OEb")
				(number "15")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin tri_state line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "O1a")
				(number "3")
			)
			(pin tri_state line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "O2a")
				(number "5")
			)
			(pin tri_state line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "O3a")
				(number "7")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "O4a")
				(number "9")
			)
			(pin tri_state line
				(at 12.7 0 180)
				(length 5.08)
				(name "O5b")
				(number "11")
			)
			(pin tri_state line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "O6b")
				(number "13")
			)
		)
		(symbol "74LS367_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS368"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74LS368"
			(at -7.62 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS368"
			(at 0 0 0)
		)
		(property "Description" "Hex Bus Driver inverter, 3-state outputs"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL Buffer BUS 3State"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS368_1_0"
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "I1")
				(number "2")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "I2")
				(number "4")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "I3")
				(number "6")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "I4")
				(number "10")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "I5")
				(number "12")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "I6")
				(number "14")
			)
			(pin input inverted
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "OEa")
				(number "1")
			)
			(pin input inverted
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "OEb")
				(number "15")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin tri_state inverted
				(at 12.7 10.16 180)
				(length 5.08)
				(name "O1a")
				(number "3")
			)
			(pin tri_state inverted
				(at 12.7 7.62 180)
				(length 5.08)
				(name "O2a")
				(number "5")
			)
			(pin tri_state inverted
				(at 12.7 5.08 180)
				(length 5.08)
				(name "O3a")
				(number "7")
			)
			(pin tri_state inverted
				(at 12.7 2.54 180)
				(length 5.08)
				(name "O4a")
				(number "9")
			)
			(pin tri_state inverted
				(at 12.7 0 180)
				(length 5.08)
				(name "O5b")
				(number "11")
			)
			(pin tri_state inverted
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "O6b")
				(number "13")
			)
		)
		(symbol "74LS368_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS373"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74LS373"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS373"
			(at 0 0 0)
		)
		(property "Description" "8-bit Latch, 3-state outputs"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL REG DFF DFF8 LATCH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?20* SOIC?20* SO?20* SSOP?20* TSSOP?20*"
			(at 0 0 0)
		)
		(symbol "74LS373_1_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "D0")
				(number "3")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "D1")
				(number "4")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "D2")
				(number "7")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "D3")
				(number "8")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "D4")
				(number "13")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "D5")
				(number "14")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "D6")
				(number "17")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "D7")
				(number "18")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "LE")
				(number "11")
			)
			(pin input inverted
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "OE")
				(number "1")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 5.08)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 5.08)
				(name "GND")
				(number "10")
			)
			(pin tri_state line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "O0")
				(number "2")
			)
			(pin tri_state line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "O1")
				(number "5")
			)
			(pin tri_state line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "O2")
				(number "6")
			)
			(pin tri_state line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "O3")
				(number "9")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "O4")
				(number "12")
			)
			(pin tri_state line
				(at 12.7 0 180)
				(length 5.08)
				(name "O5")
				(number "15")
			)
			(pin tri_state line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "O6")
				(number "16")
			)
			(pin tri_state line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "O7")
				(number "19")
			)
		)
		(symbol "74LS373_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS374"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74LS374"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS374"
			(at 0 0 0)
		)
		(property "Description" "8-bit Register, 3-state outputs"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL DFF DFF8 REG 3State"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?20* SOIC?20* SO?20*"
			(at 0 0 0)
		)
		(symbol "74LS374_1_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "D0")
				(number "3")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "D1")
				(number "4")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "D2")
				(number "7")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "D3")
				(number "8")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "D4")
				(number "13")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "D5")
				(number "14")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "D6")
				(number "17")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "D7")
				(number "18")
			)
			(pin input clock
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "Cp")
				(number "11")
			)
			(pin input inverted
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "OE")
				(number "1")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 5.08)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 5.08)
				(name "GND")
				(number "10")
			)
			(pin tri_state line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "O0")
				(number "2")
			)
			(pin tri_state line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "O1")
				(number "5")
			)
			(pin tri_state line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "O2")
				(number "6")
			)
			(pin tri_state line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "O3")
				(number "9")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "O4")
				(number "12")
			)
			(pin tri_state line
				(at 12.7 0 180)
				(length 5.08)
				(name "O5")
				(number "15")
			)
			(pin tri_state line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "O6")
				(number "16")
			)
			(pin tri_state line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "O7")
				(number "19")
			)
		)
		(symbol "74LS374_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS375"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74LS375"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS375"
			(at 0 0 0)
		)
		(property "Description" "4-bit Latch"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL DFF DFF4 Latch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS375_1_0"
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "D0")
				(number "1")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "D1")
				(number "7")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "D2")
				(number "9")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "D3")
				(number "15")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "E01")
				(number "4")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "E23")
				(number "12")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "Q0")
				(number "3")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "~{Q0}")
				(number "2")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q1")
				(number "5")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "~{Q1}")
				(number "6")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "Q2")
				(number "11")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "~{Q2}")
				(number "10")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "Q3")
				(number "13")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "~{Q3}")
				(number "14")
			)
		)
		(symbol "74LS375_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS377"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74LS377"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS377"
			(at 0 0 0)
		)
		(property "Description" "8-bit Register"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL REG DFF DFF8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?20*"
			(at 0 0 0)
		)
		(symbol "74LS377_1_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "D0")
				(number "3")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "D1")
				(number "4")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "D2")
				(number "7")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "D3")
				(number "8")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "D4")
				(number "13")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "D5")
				(number "14")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "D6")
				(number "17")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "D7")
				(number "18")
			)
			(pin input clock
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "CP")
				(number "11")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "~{E}")
				(number "1")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 5.08)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 5.08)
				(name "GND")
				(number "10")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "Q0")
				(number "2")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "Q1")
				(number "5")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Q2")
				(number "6")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q3")
				(number "9")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "Q4")
				(number "12")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "Q5")
				(number "15")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "Q6")
				(number "16")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "Q7")
				(number "19")
			)
		)
		(symbol "74LS377_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS378"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74LS378"
			(at -7.62 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS378"
			(at 0 0 0)
		)
		(property "Description" "6-bit Register"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL REG DFF DFF6"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS378_1_0"
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "D0")
				(number "3")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "D1")
				(number "4")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "D2")
				(number "6")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "D3")
				(number "11")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "D4")
				(number "13")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "D5")
				(number "14")
			)
			(pin input clock
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "C")
				(number "9")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "~{E}")
				(number "1")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "Q0")
				(number "2")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Q1")
				(number "5")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q2")
				(number "7")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "Q3")
				(number "10")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "Q4")
				(number "12")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "Q5")
				(number "15")
			)
		)
		(symbol "74LS378_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS379"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74LS379"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS379"
			(at 0 0 0)
		)
		(property "Description" "4-bit Register"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL REG DFF DFF4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS379_1_0"
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "D0")
				(number "4")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "D1")
				(number "5")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "D2")
				(number "12")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "D3")
				(number "13")
			)
			(pin input clock
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "CP")
				(number "9")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "~{E}")
				(number "1")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "Q0")
				(number "2")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "~{Q0}")
				(number "3")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q1")
				(number "7")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "~{Q1}")
				(number "6")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "Q2")
				(number "10")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "~{Q2}")
				(number "11")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "Q3")
				(number "15")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "~{Q3}")
				(number "14")
			)
		)
		(symbol "74LS379_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS385"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74LS385"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS385"
			(at 0 0 0)
		)
		(property "Description" "Quad serial Adder"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL ADD Arith ALU"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?20*"
			(at 0 0 0)
		)
		(symbol "74LS385_1_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "1S")
				(number "2")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "1S/A")
				(number "3")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "1B")
				(number "4")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "1A")
				(number "5")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "2A")
				(number "6")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "2B")
				(number "7")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "2S/A")
				(number "8")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "2S")
				(number "9")
			)
			(pin input clock
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "Clk")
				(number "1")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "Clr")
				(number "11")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 5.08)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 5.08)
				(name "GND")
				(number "10")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "4S")
				(number "19")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "4S/A")
				(number "18")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "4B")
				(number "17")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "4A")
				(number "16")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "3A")
				(number "15")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "3B")
				(number "14")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "3S/A")
				(number "13")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "3S")
				(number "12")
			)
		)
		(symbol "74LS385_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS386"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74LS386"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS386"
			(at 0 0 0)
		)
		(property "Description" "Quad 2-input XOR"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL XOR2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "74LS386_1_0"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.445)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.445)
				(name "~")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "3")
			)
		)
		(symbol "74LS386_1_1")
		(symbol "74LS386_2_0"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.445)
				(name "~")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.445)
				(name "~")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "4")
			)
		)
		(symbol "74LS386_2_1")
		(symbol "74LS386_3_0"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.445)
				(name "~")
				(number "8")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.445)
				(name "~")
				(number "9")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "10")
			)
		)
		(symbol "74LS386_3_1")
		(symbol "74LS386_4_0"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.445)
				(name "~")
				(number "12")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.445)
				(name "~")
				(number "13")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "11")
			)
		)
		(symbol "74LS386_4_1")
		(symbol "74LS386_5_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74LS386_5_1")
		(embedded_fonts no)
	)
	(symbol "74LS390"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "74LS390"
			(at -7.62 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS390"
			(at 0 0 0)
		)
		(property "Description" "Dual BCD 4-bit counter"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL CNT CNT4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16* SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "74LS390_1_0"
			(pin input clock
				(at -12.7 2.54 0)
				(length 5.08)
				(name "~{CP0}")
				(number "1")
			)
			(pin input clock
				(at -12.7 0 0)
				(length 5.08)
				(name "~{CP1}")
				(number "4")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "MR")
				(number "2")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "Q0")
				(number "3")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "Q1")
				(number "5")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "Q2")
				(number "6")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "Q3")
				(number "7")
			)
		)
		(symbol "74LS390_1_1")
		(symbol "74LS390_2_0"
			(pin input clock
				(at -12.7 2.54 0)
				(length 5.08)
				(name "~{CP0}")
				(number "15")
			)
			(pin input clock
				(at -12.7 0 0)
				(length 5.08)
				(name "~{CP1}")
				(number "12")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "MR")
				(number "14")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "Q0")
				(number "13")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "Q1")
				(number "11")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "Q2")
				(number "10")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "Q3")
				(number "9")
			)
		)
		(symbol "74LS390_2_1")
		(symbol "74LS390_3_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
		)
		(symbol "74LS390_3_1")
		(embedded_fonts no)
	)
	(symbol "74LS393"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "74LS393"
			(at -7.62 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "74xx\\74LS393.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual BCD 4-bit counter"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL CNT CNT4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "74LS393_1_0"
			(pin input clock
				(at -12.7 2.54 0)
				(length 5.08)
				(name "CP")
				(number "1")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "MR")
				(number "2")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "Q0")
				(number "3")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "Q1")
				(number "4")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "Q2")
				(number "5")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "Q3")
				(number "6")
			)
		)
		(symbol "74LS393_1_1")
		(symbol "74LS393_2_0"
			(pin input clock
				(at -12.7 2.54 0)
				(length 5.08)
				(name "CP")
				(number "13")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "MR")
				(number "12")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "Q0")
				(number "11")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "Q1")
				(number "10")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "Q2")
				(number "9")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "Q3")
				(number "8")
			)
		)
		(symbol "74LS393_2_1")
		(symbol "74LS393_3_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74LS393_3_1")
		(embedded_fonts no)
	)
	(symbol "74LS395"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74LS395"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS395"
			(at 0 0 0)
		)
		(property "Description" "4-bit universal shift register, 3-state outputs"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL SR SR4 REG 3State"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS395_1_0"
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "Ds")
				(number "2")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "P0")
				(number "3")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "P1")
				(number "4")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "P2")
				(number "5")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "P3")
				(number "6")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "LD/~{SH}")
				(number "7")
			)
			(pin input clock
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "~{CP}")
				(number "10")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "~{OE}")
				(number "9")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "~{MR}")
				(number "1")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin tri_state line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "Q0")
				(number "15")
			)
			(pin tri_state line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Q1")
				(number "14")
			)
			(pin tri_state line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q2")
				(number "13")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "Q3")
				(number "12")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "Q'3")
				(number "11")
			)
		)
		(symbol "74LS395_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS398"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74LS398"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS398"
			(at 0 0 0)
		)
		(property "Description" "Quad 2 to 1 line Multiplexer, 3-state outputs"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL MUX MUX2 3State"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?20*"
			(at 0 0 0)
		)
		(symbol "74LS398_1_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "I0a")
				(number "4")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "I1a")
				(number "5")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "I0b")
				(number "7")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "I1b")
				(number "6")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "I0c")
				(number "14")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "I1c")
				(number "15")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "I0d")
				(number "17")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "I1d")
				(number "16")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "S")
				(number "1")
			)
			(pin input clock
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "CP")
				(number "11")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 5.08)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 5.08)
				(name "GND")
				(number "10")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "Qa")
				(number "2")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "~{Qa}")
				(number "3")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Qb")
				(number "9")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "~{Qb}")
				(number "8")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "Qc")
				(number "12")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "~{Qc}")
				(number "13")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "Qd")
				(number "19")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "~{Qd}")
				(number "18")
			)
		)
		(symbol "74LS398_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS399"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74LS399"
			(at -7.62 -19.05 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS399"
			(at 0 0 0)
		)
		(property "Description" "Quad 2 to 1 line multiplexer with storage"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL MUX MUX2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS399_1_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "I0a")
				(number "3")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "I1a")
				(number "4")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "I0b")
				(number "6")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "I1b")
				(number "5")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "I0c")
				(number "11")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "I1c")
				(number "12")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "I0d")
				(number "14")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "I1d")
				(number "13")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "S")
				(number "1")
			)
			(pin input clock
				(at -12.7 -15.24 0)
				(length 5.08)
				(name "CP")
				(number "9")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "Qa")
				(number "2")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Qb")
				(number "7")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "Qc")
				(number "10")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "Qd")
				(number "15")
			)
		)
		(symbol "74LS399_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS42"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74LS42"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS42"
			(at 0 0 0)
		)
		(property "Description" "4 to 10 line Decoder"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL DECOD DECOD10"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS42_1_0"
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "A0")
				(number "15")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "A1")
				(number "14")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "A2")
				(number "13")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "A3")
				(number "12")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin output inverted
				(at 12.7 10.16 180)
				(length 5.08)
				(name "0")
				(number "1")
			)
			(pin output inverted
				(at 12.7 7.62 180)
				(length 5.08)
				(name "1")
				(number "2")
			)
			(pin output inverted
				(at 12.7 5.08 180)
				(length 5.08)
				(name "2")
				(number "3")
			)
			(pin output inverted
				(at 12.7 2.54 180)
				(length 5.08)
				(name "3")
				(number "4")
			)
			(pin output inverted
				(at 12.7 0 180)
				(length 5.08)
				(name "4")
				(number "5")
			)
			(pin output inverted
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "5")
				(number "6")
			)
			(pin output inverted
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "6")
				(number "7")
			)
			(pin output inverted
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "7")
				(number "9")
			)
			(pin output inverted
				(at 12.7 -10.16 180)
				(length 5.08)
				(name "8")
				(number "10")
			)
			(pin output inverted
				(at 12.7 -12.7 180)
				(length 5.08)
				(name "9")
				(number "11")
			)
		)
		(symbol "74LS42_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS47"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "74LS47"
			(at -7.62 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS47"
			(at 0 0 0)
		)
		(property "Description" "BCD to 7-segment Driver, Open Collector, 30V outputs"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL DECOD DECOD7 OpenCol"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS47_1_0"
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "A")
				(number "7")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "B")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "C")
				(number "2")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "D")
				(number "6")
			)
			(pin input inverted
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "LT")
				(number "3")
			)
			(pin input inverted
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "BI")
				(number "4")
			)
			(pin input inverted
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "RBI")
				(number "5")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin open_collector inverted
				(at 12.7 7.62 180)
				(length 5.08)
				(name "a")
				(number "13")
			)
			(pin open_collector inverted
				(at 12.7 5.08 180)
				(length 5.08)
				(name "b")
				(number "12")
			)
			(pin open_collector inverted
				(at 12.7 2.54 180)
				(length 5.08)
				(name "c")
				(number "11")
			)
			(pin open_collector inverted
				(at 12.7 0 180)
				(length 5.08)
				(name "d")
				(number "10")
			)
			(pin open_collector inverted
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "e")
				(number "9")
			)
			(pin open_collector inverted
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "f")
				(number "15")
			)
			(pin open_collector inverted
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "g")
				(number "14")
			)
		)
		(symbol "74LS47_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS48"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "74LS48"
			(at -7.62 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS48"
			(at 0 0 0)
		)
		(property "Description" "BCD to 7-segment Decoder/driver, Active High outputs"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL DECOD DECOD7"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS48_1_0"
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "A")
				(number "7")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "B")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "C")
				(number "2")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "D")
				(number "6")
			)
			(pin input inverted
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "LT")
				(number "3")
			)
			(pin input inverted
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "BI")
				(number "4")
			)
			(pin input inverted
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "RBI")
				(number "5")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin open_collector line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "a")
				(number "13")
			)
			(pin open_collector line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "b")
				(number "12")
			)
			(pin open_collector line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "c")
				(number "11")
			)
			(pin open_collector line
				(at 12.7 0 180)
				(length 5.08)
				(name "d")
				(number "10")
			)
			(pin open_collector line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "e")
				(number "9")
			)
			(pin open_collector line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "f")
				(number "15")
			)
			(pin open_collector line
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "g")
				(number "14")
			)
		)
		(symbol "74LS48_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS49"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "74LS49"
			(at -7.62 -11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74ls47"
			(at 0 0 0)
		)
		(property "Description" "BCD to 7-segment decoder/driver, Open collector"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL DECOD DECOD7 OpenCol"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "74LS49_1_0"
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "A")
				(number "5")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "B")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "C")
				(number "2")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "D")
				(number "4")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "~{BI}")
				(number "3")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
			(pin open_collector line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "a")
				(number "11")
			)
			(pin open_collector line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "b")
				(number "10")
			)
			(pin open_collector line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "c")
				(number "9")
			)
			(pin open_collector line
				(at 12.7 0 180)
				(length 5.08)
				(name "d")
				(number "8")
			)
			(pin open_collector line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "e")
				(number "6")
			)
			(pin open_collector line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "f")
				(number "13")
			)
			(pin open_collector line
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "g")
				(number "12")
			)
		)
		(symbol "74LS49_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS51"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 10.16 0)
		)
		(property "Value" "74LS51"
			(at -7.62 -10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74ls51.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual 3- and 2-input AND-NOR ( S = /(AB[C] + DE[F]) )"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL ANDNOR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "74LS51_1_0"
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "~")
				(number "12")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "~")
				(number "13")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "~")
				(number "9")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "~")
				(number "10")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "~")
				(number "11")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "~")
				(number "8")
			)
		)
		(symbol "74LS51_2_0"
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "~")
				(number "2")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "~")
				(number "3")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "~")
				(number "5")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LS51_3_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74LS51_3_1")
		(embedded_fonts no)
	)
	(symbol "74LS540"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74LS540"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS540"
			(at 0 0 0)
		)
		(property "Description" "8-bit Buffer/Line driver Inverter, 3-state outputs"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "BUFFER BUS TTL 3State"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?20*"
			(at 0 0 0)
		)
		(symbol "74LS540_1_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "A0")
				(number "2")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "A1")
				(number "3")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "A2")
				(number "4")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "A3")
				(number "5")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "A4")
				(number "6")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "A5")
				(number "7")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "A6")
				(number "8")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "A7")
				(number "9")
			)
			(pin input inverted
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "G1")
				(number "1")
			)
			(pin input inverted
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "G2")
				(number "19")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 5.08)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 5.08)
				(name "GND")
				(number "10")
			)
			(pin tri_state inverted
				(at 12.7 12.7 180)
				(length 5.08)
				(name "Y0")
				(number "18")
			)
			(pin tri_state inverted
				(at 12.7 10.16 180)
				(length 5.08)
				(name "Y1")
				(number "17")
			)
			(pin tri_state inverted
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Y2")
				(number "16")
			)
			(pin tri_state inverted
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Y3")
				(number "15")
			)
			(pin tri_state inverted
				(at 12.7 2.54 180)
				(length 5.08)
				(name "Y4")
				(number "14")
			)
			(pin tri_state inverted
				(at 12.7 0 180)
				(length 5.08)
				(name "Y5")
				(number "13")
			)
			(pin tri_state inverted
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "Y6")
				(number "12")
			)
			(pin tri_state inverted
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "Y7")
				(number "11")
			)
		)
		(symbol "74LS540_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS541"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74LS541"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS541"
			(at 0 0 0)
		)
		(property "Description" "8-bit Buffer/Line Driver 3-state outputs"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL BUFFER 3State BUS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?20*"
			(at 0 0 0)
		)
		(symbol "74LS541_1_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "A0")
				(number "2")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "A1")
				(number "3")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "A2")
				(number "4")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "A3")
				(number "5")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "A4")
				(number "6")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "A5")
				(number "7")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "A6")
				(number "8")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "A7")
				(number "9")
			)
			(pin input inverted
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "G1")
				(number "1")
			)
			(pin input inverted
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "G2")
				(number "19")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 5.08)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 5.08)
				(name "GND")
				(number "10")
			)
			(pin tri_state line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "Y0")
				(number "18")
			)
			(pin tri_state line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "Y1")
				(number "17")
			)
			(pin tri_state line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Y2")
				(number "16")
			)
			(pin tri_state line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Y3")
				(number "15")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "Y4")
				(number "14")
			)
			(pin tri_state line
				(at 12.7 0 180)
				(length 5.08)
				(name "Y5")
				(number "13")
			)
			(pin tri_state line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "Y6")
				(number "12")
			)
			(pin tri_state line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "Y7")
				(number "11")
			)
		)
		(symbol "74LS541_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS54N"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 15.24 0)
		)
		(property "Value" "74LS54N"
			(at -0.254 -15.24 0)
		)
		(property "Footprint" ""
			(at 0.7697 3.81 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn54ls54.pdf"
			(at 0 0 0)
		)
		(property "Description" "And-Nor (Y = /(AB + CDE + FGH + IJ) ), DIP-14"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL ANDNOR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "74LS54N_1_0"
			(pin input line
				(at -7.62 12.7 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -7.62 10.16 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin input line
				(at -7.62 7.62 0)
				(length 3.81)
				(name "~")
				(number "3")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 3.81)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 3.81)
				(name "~")
				(number "10")
			)
			(pin input line
				(at -7.62 -7.62 0)
				(length 3.81)
				(name "~")
				(number "11")
			)
			(pin input line
				(at -7.62 -10.16 0)
				(length 3.81)
				(name "~")
				(number "12")
			)
			(pin input line
				(at -7.62 -12.7 0)
				(length 3.81)
				(name "~")
				(number "13")
			)
			(pin output inverted
				(at 10.16 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LS54N_1_1")
		(symbol "74LS54N_2_0"
			(pin power_in line
				(at 0 10.16 270)
				(length 3.81)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 3.81)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74LS54N_2_1")
		(embedded_fonts no)
	)
	(symbol "74LS55"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 10.16 0)
		)
		(property "Value" "74LS55"
			(at -7.62 -12.7 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS55"
			(at 0 0 0)
		)
		(property "Description" "AND-NOR ( S = / (ABCD + EFGH) )"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL ANDNOR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "74LS55_1_0"
			(pin input line
				(at -7.62 7.62 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "3")
			)
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "10")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 3.81)
				(name "~")
				(number "11")
			)
			(pin input line
				(at -7.62 -7.62 0)
				(length 3.81)
				(name "~")
				(number "12")
			)
			(pin input line
				(at -7.62 -10.16 0)
				(length 3.81)
				(name "~")
				(number "13")
			)
			(pin output inverted
				(at 7.62 -1.27 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "74LS55_2_0"
			(pin power_in line
				(at 0 11.43 270)
				(length 3.81)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -11.43 90)
				(length 3.81)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74LS55_2_1")
		(embedded_fonts no)
	)
	(symbol "74LS573"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74LS573"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "74xx/74hc573.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit Latch 3-state outputs"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL DFF DFF8 LATCH 3State"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?20*"
			(at 0 0 0)
		)
		(symbol "74LS573_1_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "D0")
				(number "2")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "D1")
				(number "3")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "D2")
				(number "4")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "D3")
				(number "5")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "D4")
				(number "6")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "D5")
				(number "7")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "D6")
				(number "8")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "D7")
				(number "9")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "Load")
				(number "11")
			)
			(pin input inverted
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "OE")
				(number "1")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 5.08)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 5.08)
				(name "GND")
				(number "10")
			)
			(pin tri_state line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "Q0")
				(number "19")
			)
			(pin tri_state line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "Q1")
				(number "18")
			)
			(pin tri_state line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Q2")
				(number "17")
			)
			(pin tri_state line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q3")
				(number "16")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "Q4")
				(number "15")
			)
			(pin tri_state line
				(at 12.7 0 180)
				(length 5.08)
				(name "Q5")
				(number "14")
			)
			(pin tri_state line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "Q6")
				(number "13")
			)
			(pin tri_state line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "Q7")
				(number "12")
			)
		)
		(symbol "74LS573_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS574"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74LS574"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS574"
			(at 0 0 0)
		)
		(property "Description" "8-bit Register, 3-state outputs"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL REG DFF DFF8 3State"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?20*"
			(at 0 0 0)
		)
		(symbol "74LS574_1_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "D0")
				(number "2")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "D1")
				(number "3")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "D2")
				(number "4")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "D3")
				(number "5")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "D4")
				(number "6")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "D5")
				(number "7")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "D6")
				(number "8")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "D7")
				(number "9")
			)
			(pin input clock
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "Cp")
				(number "11")
			)
			(pin input inverted
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "OE")
				(number "1")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 5.08)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 5.08)
				(name "GND")
				(number "10")
			)
			(pin tri_state line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "Q0")
				(number "19")
			)
			(pin tri_state line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "Q1")
				(number "18")
			)
			(pin tri_state line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Q2")
				(number "17")
			)
			(pin tri_state line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q3")
				(number "16")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "Q4")
				(number "15")
			)
			(pin tri_state line
				(at 12.7 0 180)
				(length 5.08)
				(name "Q5")
				(number "14")
			)
			(pin tri_state line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "Q6")
				(number "13")
			)
			(pin tri_state line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "Q7")
				(number "12")
			)
		)
		(symbol "74LS574_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS629"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "74LS629"
			(at -7.62 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS629"
			(at 0 0 0)
		)
		(property "Description" "dual voltage-controlled oscillator, enable control, range control"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "VCO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS629_1_0"
			(pin input inverted
				(at -12.7 5.08 0)
				(length 5.08)
				(name "EN")
				(number "6")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "RNG")
				(number "3")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "FC")
				(number "2")
			)
			(pin passive line
				(at 0 12.7 270)
				(length 5.08)
				(name "OSC")
				(number "15")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Y")
				(number "7")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 5.08)
				(name "CX1")
				(number "4")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "CX2")
				(number "5")
			)
		)
		(symbol "74LS629_1_1")
		(symbol "74LS629_2_0"
			(pin input inverted
				(at -12.7 5.08 0)
				(length 5.08)
				(name "EN")
				(number "11")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "RNG")
				(number "14")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "FC")
				(number "1")
			)
			(pin passive line
				(at 0 12.7 270)
				(length 5.08)
				(name "OSC")
				(number "8")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Y")
				(number "10")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 5.08)
				(name "CX1")
				(number "13")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "CX2")
				(number "12")
			)
		)
		(symbol "74LS629_2_1")
		(symbol "74LS629_3_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "9")
			)
		)
		(symbol "74LS629_3_1")
		(embedded_fonts no)
	)
	(symbol "74LS688"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 26.67 0)
		)
		(property "Value" "74LS688"
			(at -7.62 -26.67 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS688"
			(at 0 0 0)
		)
		(property "Description" "8-bit magnitude comparator"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL DECOD Arith"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?20* SOIC?20* SO?20* TSSOP?20*"
			(at 0 0 0)
		)
		(symbol "74LS688_1_0"
			(pin input line
				(at -12.7 22.86 0)
				(length 5.08)
				(name "P0")
				(number "2")
			)
			(pin input line
				(at -12.7 20.32 0)
				(length 5.08)
				(name "P1")
				(number "4")
			)
			(pin input line
				(at -12.7 17.78 0)
				(length 5.08)
				(name "P2")
				(number "6")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 5.08)
				(name "P3")
				(number "8")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "P4")
				(number "11")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "P5")
				(number "13")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "P6")
				(number "15")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "P7")
				(number "17")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "R0")
				(number "3")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "R1")
				(number "5")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "R2")
				(number "7")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "R3")
				(number "9")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "R4")
				(number "12")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "R5")
				(number "14")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 5.08)
				(name "R6")
				(number "16")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 5.08)
				(name "R7")
				(number "18")
			)
			(pin input inverted
				(at -12.7 -22.86 0)
				(length 5.08)
				(name "G")
				(number "1")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 5.08)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 5.08)
				(name "GND")
				(number "10")
			)
			(pin output inverted
				(at 12.7 22.86 180)
				(length 5.08)
				(name "P=R")
				(number "19")
			)
		)
		(symbol "74LS688_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS73"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "74LS73"
			(at -7.62 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS73"
			(at 0 0 0)
		)
		(property "Description" "Dual JK Flip-Flop, reset"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL JK JKFF"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "74LS73_1_0"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "J")
				(number "7")
			)
			(pin input clock
				(at -7.62 0 0)
				(length 2.54)
				(name "C")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "K")
				(number "10")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~{R}")
				(number "6")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "Q")
				(number "9")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~{Q}")
				(number "8")
			)
		)
		(symbol "74LS73_1_1")
		(symbol "74LS73_2_0"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "J")
				(number "14")
			)
			(pin input clock
				(at -7.62 0 0)
				(length 2.54)
				(name "C")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "K")
				(number "3")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~{R}")
				(number "2")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "Q")
				(number "12")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~{Q}")
				(number "13")
			)
		)
		(symbol "74LS73_2_1")
		(symbol "74LS73_3_0"
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
		)
		(symbol "74LS73_3_1")
		(embedded_fonts no)
	)
	(symbol "74LS74"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "74LS74"
			(at -7.62 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "74xx/74hc_hct74.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual D Flip-flop, Set & Reset"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL DFF"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "74LS74_1_0"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "D")
				(number "2")
			)
			(pin input clock
				(at -7.62 0 0)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin input line
				(at 0 7.62 270)
				(length 2.54)
				(name "~{S}")
				(number "4")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~{R}")
				(number "1")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "Q")
				(number "5")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~{Q}")
				(number "6")
			)
		)
		(symbol "74LS74_1_1")
		(symbol "74LS74_2_0"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "D")
				(number "12")
			)
			(pin input clock
				(at -7.62 0 0)
				(length 2.54)
				(name "C")
				(number "11")
			)
			(pin input line
				(at 0 7.62 270)
				(length 2.54)
				(name "~{S}")
				(number "10")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~{R}")
				(number "13")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "Q")
				(number "9")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~{Q}")
				(number "8")
			)
		)
		(symbol "74LS74_2_1")
		(symbol "74LS74_3_0"
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74LS74_3_1")
		(embedded_fonts no)
	)
	(symbol "74LS75"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "74LS75"
			(at -7.62 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS75"
			(at 0 0 0)
		)
		(property "Description" "4-bit Latch"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL DFF Latch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS75_1_0"
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "D0")
				(number "2")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "D1")
				(number "3")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "D2")
				(number "6")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "D3")
				(number "7")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "E01")
				(number "13")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "E23")
				(number "4")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 5.08)
				(name "GND")
				(number "12")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Q0")
				(number "16")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q1")
				(number "15")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "Q2")
				(number "10")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "Q3")
				(number "9")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "~{Q0}")
				(number "1")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "~{Q1}")
				(number "14")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "~{Q2}")
				(number "11")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 5.08)
				(name "~{Q3}")
				(number "8")
			)
		)
		(symbol "74LS75_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS76"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "74LS76"
			(at -7.62 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS76"
			(at 0 0 0)
		)
		(property "Description" "Dual JK Flip-flop, Set & Reset"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL JK JKFF"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS76_1_0"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "J")
				(number "4")
			)
			(pin input clock
				(at -7.62 0 0)
				(length 2.54)
				(name "C")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "K")
				(number "16")
			)
			(pin input line
				(at 0 7.62 270)
				(length 2.54)
				(name "~{S}")
				(number "2")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~{R}")
				(number "3")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "Q")
				(number "15")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~{Q}")
				(number "14")
			)
		)
		(symbol "74LS76_1_1")
		(symbol "74LS76_2_0"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "J")
				(number "9")
			)
			(pin input clock
				(at -7.62 0 0)
				(length 2.54)
				(name "C")
				(number "6")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "K")
				(number "12")
			)
			(pin input line
				(at 0 7.62 270)
				(length 2.54)
				(name "~{S}")
				(number "7")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~{R}")
				(number "8")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "Q")
				(number "11")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~{Q}")
				(number "10")
			)
		)
		(symbol "74LS76_2_1")
		(symbol "74LS76_3_0"
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "13")
			)
		)
		(symbol "74LS76_3_1")
		(embedded_fonts no)
	)
	(symbol "74LS77"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "74LS77"
			(at -7.62 -11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS77"
			(at 0 0 0)
		)
		(property "Description" "4-bit Latch"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL DFF Latch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?12*"
			(at 0 0 0)
		)
		(symbol "74LS77_1_0"
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "D0")
				(number "1")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "D1")
				(number "2")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "D2")
				(number "5")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "D3")
				(number "6")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "E01")
				(number "12")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "E23")
				(number "3")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VCC")
				(number "4")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "GND")
				(number "11")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Q0")
				(number "14")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q1")
				(number "13")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "Q2")
				(number "9")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "Q3")
				(number "8")
			)
		)
		(symbol "74LS77_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS78"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "74LS78"
			(at -7.62 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS78"
			(at 0 0 0)
		)
		(property "Description" "Dual JK Flip-flop, Set, Common clock & reset"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL JK JKFF"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "74LS78_1_0"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "J")
				(number "3")
			)
			(pin input clock
				(at -7.62 0 0)
				(length 2.54)
				(name "C")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "K")
				(number "14")
			)
			(pin input line
				(at 0 7.62 270)
				(length 2.54)
				(name "~{S}")
				(number "2")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~{R}")
				(number "5")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "Q")
				(number "13")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~{Q}")
				(number "12")
			)
		)
		(symbol "74LS78_1_1")
		(symbol "74LS78_2_0"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "J")
				(number "10")
			)
			(pin input clock
				(at -7.62 0 0)
				(length 2.54)
				(name "C")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "K")
				(number "7")
			)
			(pin input line
				(at 0 7.62 270)
				(length 2.54)
				(name "~{S}")
				(number "6")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~{R}")
				(number "5")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "Q")
				(number "8")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~{Q}")
				(number "9")
			)
		)
		(symbol "74LS78_2_1")
		(symbol "74LS78_3_0"
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
		)
		(symbol "74LS78_3_1")
		(embedded_fonts no)
	)
	(symbol "74LS83"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74LS83"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS83"
			(at 0 0 0)
		)
		(property "Description" "4-bit Full Adder"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL ADD ARITH ALU"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS83_1_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "C0")
				(number "13")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "B4")
				(number "16")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "B3")
				(number "4")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "B2")
				(number "7")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "B1")
				(number "11")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "A4")
				(number "1")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "A3")
				(number "3")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "A2")
				(number "8")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "A1")
				(number "10")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 5.08)
				(name "GND")
				(number "12")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "S1")
				(number "9")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "S2")
				(number "6")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "S3")
				(number "2")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "S4")
				(number "15")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "C4")
				(number "14")
			)
		)
		(symbol "74LS83_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS85"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74LS85"
			(at -7.62 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS85"
			(at 0 0 0)
		)
		(property "Description" "4-bit Comparator"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL COMP ARITH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LS85_1_0"
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "B3")
				(number "1")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "B2")
				(number "14")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "B1")
				(number "11")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "B0")
				(number "9")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "A3")
				(number "15")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "A2")
				(number "13")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "A1")
				(number "12")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "A0")
				(number "10")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "Ia>b")
				(number "4")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Ia<b")
				(number "2")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Ia=b")
				(number "3")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "Oa>b")
				(number "5")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "Oa<b")
				(number "7")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 5.08)
				(name "Oa=b")
				(number "6")
			)
		)
		(symbol "74LS85_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS86"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74LS86"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "74xx/74ls86.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad 2-input XOR"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL XOR2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "74LS86_1_0"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.445)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.445)
				(name "~")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "3")
			)
		)
		(symbol "74LS86_1_1")
		(symbol "74LS86_2_0"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.445)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.445)
				(name "~")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LS86_2_1")
		(symbol "74LS86_3_0"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.445)
				(name "~")
				(number "9")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.445)
				(name "~")
				(number "10")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "74LS86_3_1")
		(symbol "74LS86_4_0"
			(pin input line
				(at -7.62 2.54 0)
				(length 4.445)
				(name "~")
				(number "12")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 4.445)
				(name "~")
				(number "13")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "11")
			)
		)
		(symbol "74LS86_4_1")
		(symbol "74LS86_5_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74LS86_5_1")
		(embedded_fonts no)
	)
	(symbol "74LS90"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "74LS90"
			(at -7.62 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS90"
			(at 0 0 0)
		)
		(property "Description" "BCD Counter ( div 2 & div 5 )"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL CNT CNT4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?12*"
			(at 0 0 0)
		)
		(symbol "74LS90_1_0"
			(pin input inverted_clock
				(at -12.7 7.62 0)
				(length 5.08)
				(name "CP0")
				(number "14")
			)
			(pin input inverted_clock
				(at -12.7 5.08 0)
				(length 5.08)
				(name "CP1..3")
				(number "1")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "R0(1)")
				(number "2")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "R0(2)")
				(number "3")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "R9(1)")
				(number "6")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "R9(2)")
				(number "7")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 5.08)
				(name "GND")
				(number "10")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Q0")
				(number "12")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q1")
				(number "9")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "Q2")
				(number "8")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "Q3")
				(number "11")
			)
		)
		(symbol "74LS90_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS91"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "74LS91"
			(at -7.62 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS91"
			(at 0 0 0)
		)
		(property "Description" "8-bit Serial Register"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL SR SR8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "74LS91_1_0"
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "A")
				(number "12")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "B")
				(number "11")
			)
			(pin input clock
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "CLK")
				(number "9")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "10")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "Qh")
				(number "13")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "~{Qh}")
				(number "14")
			)
		)
		(symbol "74LS91_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS92"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "74LS92"
			(at -7.62 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS92"
			(at 0 0 0)
		)
		(property "Description" "Divide by 12 counter"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL CNT CNT4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "74LS92_1_0"
			(pin input inverted_clock
				(at -12.7 5.08 0)
				(length 5.08)
				(name "CP0")
				(number "14")
			)
			(pin input inverted_clock
				(at -12.7 2.54 0)
				(length 5.08)
				(name "CP1..3")
				(number "1")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "R0(1)")
				(number "6")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "R0(2)")
				(number "7")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "10")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q0")
				(number "12")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "Q1")
				(number "11")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "Q2")
				(number "9")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "Q3")
				(number "8")
			)
		)
		(symbol "74LS92_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS93"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "74LS93"
			(at -7.62 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS93"
			(at 0 0 0)
		)
		(property "Description" "Divide by 2 & 8 counter"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL CNT CNT4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "74LS93_1_0"
			(pin input inverted_clock
				(at -12.7 5.08 0)
				(length 5.08)
				(name "CP0")
				(number "14")
			)
			(pin input inverted_clock
				(at -12.7 2.54 0)
				(length 5.08)
				(name "CP1..3")
				(number "1")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "R0(1)")
				(number "2")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "R0(2)")
				(number "3")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "10")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Q0")
				(number "12")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "Q1")
				(number "9")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "Q2")
				(number "8")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "Q3")
				(number "11")
			)
		)
		(symbol "74LS93_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS95"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74LS95"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS95"
			(at 0 0 0)
		)
		(property "Description" "Shift Register 5-bit (in/out)"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL SR SR4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "74LS95_1_0"
			(pin input line
				(at -17.78 12.7 0)
				(length 5.08)
				(name "Ds")
				(number "1")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 5.08)
				(name "P0")
				(number "2")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 5.08)
				(name "P1")
				(number "3")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 5.08)
				(name "P2")
				(number "4")
			)
			(pin input line
				(at -17.78 0 0)
				(length 5.08)
				(name "P3")
				(number "5")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 5.08)
				(name "Mode")
				(number "6")
			)
			(pin input inverted_clock
				(at -17.78 -10.16 0)
				(length 5.08)
				(name "Cp1.Rshift")
				(number "9")
			)
			(pin input inverted_clock
				(at -17.78 -12.7 0)
				(length 5.08)
				(name "Cp2.Lshift")
				(number "8")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 5.08)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 5.08)
				(name "Q0")
				(number "13")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 5.08)
				(name "Q1")
				(number "12")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "Q2")
				(number "11")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 5.08)
				(name "Q3")
				(number "10")
			)
		)
		(symbol "74LS95_1_1")
		(embedded_fonts no)
	)
	(symbol "74LV14"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74LV14"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LV14"
			(at 0 0 0)
		)
		(property "Description" "Hex Inverter"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL not inv"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "74LV14_1_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "2")
			)
		)
		(symbol "74LV14_2_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "3")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "4")
			)
		)
		(symbol "74LV14_3_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LV14_4_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "74LV14_5_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "11")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "10")
			)
		)
		(symbol "74LV14_6_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "13")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "12")
			)
		)
		(symbol "74LV14_7_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "3.3V")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74LV14_7_1")
		(embedded_fonts no)
	)
	(symbol "74LV8154"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 16.51 0)
		)
		(property "Value" "74LV8154"
			(at 6.35 16.51 0)
		)
		(property "Footprint" ""
			(at -6.35 16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74lv8154.pdf"
			(at -6.35 16.51 0)
		)
		(property "Description" "Dual 16-bit binary counter"
			(at 0 0 0)
		)
		(property "ki_keywords" "counter binary"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "74LV8154_0_1")
		(symbol "74LV8154_1_1"
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "CKLA")
				(number "1")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "CLKB")
				(number "2")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "~{GAL}")
				(number "3")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "~{GAU}")
				(number "4")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{GBL}")
				(number "5")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{GBU}")
				(number "6")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "RCLK")
				(number "7")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "~{CCLR}")
				(number "11")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "~{CLKBEN}")
				(number "9")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin output line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "Y0")
				(number "19")
			)
			(pin output line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "Y1")
				(number "18")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "Y2")
				(number "17")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "Y3")
				(number "16")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "Y4")
				(number "15")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "Y5")
				(number "14")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "Y6")
				(number "13")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "Y7")
				(number "12")
			)
			(pin output line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "~{RCOA}")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74VHC9164FT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 16.51 0)
		)
		(property "Value" "74VHC9164FT"
			(at -8.89 16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=15655&prodName=74VHC9164FT"
			(at 0 0 0)
		)
		(property "Description" "8-bit Universal Shift Register, 2V to 5.5V, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "shift register universal serial parallel"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "74VHC9164FT_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "P/S_CONT")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "~{CLR_LOAD}")
				(number "2")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SI")
				(number "3")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "CK")
				(number "4")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "Q/D1")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "Q/D2")
				(number "6")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "Q/D3")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "Q/D4")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "Q/D5")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "Q/D6")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "Q/D7")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "Q/D8")
				(number "13")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "Q8'")
				(number "14")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "Q8C")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CD74HC4067M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 22.86 0)
		)
		(property "Value" "CD74HC4067M"
			(at 1.27 22.86 0)
		)
		(property "Footprint" "Package_SO:SOIC-24W_7.5x15.4mm_P1.27mm"
			(at 22.86 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/cd74hc4067.pdf"
			(at -8.89 21.59 0)
		)
		(property "Description" "High-Speed CMOS Logic 16-Channel Analog Multiplexer/Demultiplexer, SOIC-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "multiplexer demultiplexer mux demux"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*W*7.5x15.4mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "CD74HC4067M_0_1")
		(symbol "CD74HC4067M_1_1"
			(pin passive line
				(at -12.7 12.7 0)
				(length 3.81)
				(name "COM")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 3.81)
				(name "S0")
				(number "10")
			)
			(pin input line
				(at -12.7 0 0)
				(length 3.81)
				(name "S1")
				(number "11")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 3.81)
				(name "S2")
				(number "14")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 3.81)
				(name "S3")
				(number "13")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 3.81)
				(name "~{E}")
				(number "15")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 3.81)
				(name "VCC")
				(number "24")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 3.81)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 12.7 17.78 180)
				(length 3.81)
				(name "I0")
				(number "9")
			)
			(pin passive line
				(at 12.7 15.24 180)
				(length 3.81)
				(name "I1")
				(number "8")
			)
			(pin passive line
				(at 12.7 12.7 180)
				(length 3.81)
				(name "I2")
				(number "7")
			)
			(pin passive line
				(at 12.7 10.16 180)
				(length 3.81)
				(name "I3")
				(number "6")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 3.81)
				(name "I4")
				(number "5")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 3.81)
				(name "I5")
				(number "4")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 3.81)
				(name "I6")
				(number "3")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 3.81)
				(name "I7")
				(number "2")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 3.81)
				(name "I8")
				(number "23")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 3.81)
				(name "I9")
				(number "22")
			)
			(pin passive line
				(at 12.7 -7.62 180)
				(length 3.81)
				(name "I10")
				(number "21")
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 3.81)
				(name "I11")
				(number "20")
			)
			(pin passive line
				(at 12.7 -12.7 180)
				(length 3.81)
				(name "I12")
				(number "19")
			)
			(pin passive line
				(at 12.7 -15.24 180)
				(length 3.81)
				(name "I13")
				(number "18")
			)
			(pin passive line
				(at 12.7 -17.78 180)
				(length 3.81)
				(name "I14")
				(number "17")
			)
			(pin passive line
				(at 12.7 -20.32 180)
				(length 3.81)
				(name "I15")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CD74HC4067SM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 22.86 0)
		)
		(property "Value" "CD74HC4067SM"
			(at 1.27 22.86 0)
		)
		(property "Footprint" "Package_SO:SSOP-24_5.3x8.2mm_P0.65mm"
			(at 26.67 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/cd74hc4067.pdf"
			(at -8.89 21.59 0)
		)
		(property "Description" "High-Speed CMOS Logic 16-Channel Analog Multiplexer/Demultiplexer, SSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "multiplexer demultiplexer mux demux"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x8.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "CD74HC4067SM_0_1")
		(symbol "CD74HC4067SM_1_1"
			(pin passive line
				(at -12.7 12.7 0)
				(length 3.81)
				(name "COM")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 3.81)
				(name "S0")
				(number "10")
			)
			(pin input line
				(at -12.7 0 0)
				(length 3.81)
				(name "S1")
				(number "11")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 3.81)
				(name "S2")
				(number "14")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 3.81)
				(name "S3")
				(number "13")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 3.81)
				(name "~{E}")
				(number "15")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 3.81)
				(name "VCC")
				(number "24")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 3.81)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 12.7 17.78 180)
				(length 3.81)
				(name "I0")
				(number "9")
			)
			(pin passive line
				(at 12.7 15.24 180)
				(length 3.81)
				(name "I1")
				(number "8")
			)
			(pin passive line
				(at 12.7 12.7 180)
				(length 3.81)
				(name "I2")
				(number "7")
			)
			(pin passive line
				(at 12.7 10.16 180)
				(length 3.81)
				(name "I3")
				(number "6")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 3.81)
				(name "I4")
				(number "5")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 3.81)
				(name "I5")
				(number "4")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 3.81)
				(name "I6")
				(number "3")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 3.81)
				(name "I7")
				(number "2")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 3.81)
				(name "I8")
				(number "23")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 3.81)
				(name "I9")
				(number "22")
			)
			(pin passive line
				(at 12.7 -7.62 180)
				(length 3.81)
				(name "I10")
				(number "21")
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 3.81)
				(name "I11")
				(number "20")
			)
			(pin passive line
				(at 12.7 -12.7 180)
				(length 3.81)
				(name "I12")
				(number "19")
			)
			(pin passive line
				(at 12.7 -15.24 180)
				(length 3.81)
				(name "I13")
				(number "18")
			)
			(pin passive line
				(at 12.7 -17.78 180)
				(length 3.81)
				(name "I14")
				(number "17")
			)
			(pin passive line
				(at 12.7 -20.32 180)
				(length 3.81)
				(name "I15")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC74LCX16245DT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 29.21 0)
		)
		(property "Value" "MC74LCX16245DT"
			(at 2.54 -29.21 0)
		)
		(property "Footprint" "Package_SO:TSSOP-48_6.1x12.5mm_P0.5mm"
			(at 0 -1.27 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/mc74lcx16245-d.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "Low Voltage 16-Bit Bidirectional Transceiver with 5V Tolerant Inputs and Outputs, TSSOP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*6.1x12.5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MC74LCX16245DT_0_1")
		(symbol "MC74LCX16245DT_1_1"
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "T/~{R}1")
				(number "1")
			)
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "T/~{R}2")
				(number "24")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "B0")
				(number "2")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "B1")
				(number "3")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "B2")
				(number "5")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "B3")
				(number "6")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "B4")
				(number "8")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "B5")
				(number "9")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "B6")
				(number "11")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "B7")
				(number "12")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "B8")
				(number "13")
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "B9")
				(number "14")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "B10")
				(number "16")
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "B11")
				(number "17")
			)
			(pin bidirectional line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "B12")
				(number "19")
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "B13")
				(number "20")
			)
			(pin bidirectional line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "B14")
				(number "22")
			)
			(pin bidirectional line
				(at -12.7 -25.4 0)
				(length 2.54)
				(name "B15")
				(number "23")
			)
			(pin passive line
				(at 0 30.48 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "18")
			)
			(pin passive line
				(at 0 30.48 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "31")
			)
			(pin passive line
				(at 0 30.48 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "42")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 2.54)
				(name "VCC")
				(number "7")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "28")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "34")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "39")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "45")
			)
			(pin input line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "~{OE1}")
				(number "48")
			)
			(pin input line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "~{OE2}")
				(number "25")
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "A0")
				(number "47")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "A1")
				(number "46")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "A2")
				(number "44")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "A3")
				(number "43")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "A4")
				(number "41")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "A5")
				(number "40")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "A6")
				(number "38")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "A7")
				(number "37")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "A8")
				(number "36")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "A9")
				(number "35")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "A10")
				(number "33")
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "A11")
				(number "32")
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "A12")
				(number "30")
			)
			(pin bidirectional line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "A13")
				(number "29")
			)
			(pin bidirectional line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "A14")
				(number "27")
			)
			(pin bidirectional line
				(at 12.7 -25.4 180)
				(length 2.54)
				(name "A15")
				(number "26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MM74C923"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "MM74C923"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/snMM74C923"
			(at 0 0 0)
		)
		(property "Description" "20-key encoder"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "encoder"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?20*"
			(at 0 0 0)
		)
		(symbol "MM74C923_1_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "Y1")
				(number "1")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "Y2")
				(number "2")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "Y3")
				(number "3")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "Y4")
				(number "4")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "Y5")
				(number "5")
			)
			(pin output line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "X1")
				(number "12")
			)
			(pin output line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "X2")
				(number "11")
			)
			(pin output line
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "X3")
				(number "9")
			)
			(pin output line
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "X4")
				(number "8")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 5.08)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 5.08)
				(name "GND")
				(number "10")
			)
			(pin tri_state line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "A")
				(number "19")
			)
			(pin tri_state line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "B")
				(number "18")
			)
			(pin tri_state line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "C")
				(number "17")
			)
			(pin tri_state line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "D")
				(number "16")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "E")
				(number "15")
			)
			(pin input inverted
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "XOE")
				(number "14")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "DA")
				(number "13")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 5.08)
				(name "OSC")
				(number "6")
			)
			(pin input line
				(at 12.7 -12.7 180)
				(length 5.08)
				(name "KBM")
				(number "7")
			)
		)
		(symbol "MM74C923_1_1")
		(embedded_fonts no)
	)
	(symbol "SN74AVC16827DGGR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 34.29 0)
		)
		(property "Value" "SN74AVC16827DGGR"
			(at 10.16 34.29 0)
		)
		(property "Footprint" "Package_SO:TSSOP-56_6.1x14mm_P0.5mm"
			(at -22.86 -34.29 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74avc16827.pdf"
			(at -27.94 -38.1 0)
		)
		(property "Description" "20-Bit Buffer/Driver With 3-State Outputs"
			(at 0 0 0)
		)
		(property "ki_keywords" "Buffer Driver 3-State"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*6.1x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "SN74AVC16827DGGR_0_1")
		(symbol "SN74AVC16827DGGR_1_1"
			(pin input line
				(at -12.7 30.48 0)
				(length 5.08)
				(name "1A1")
				(number "55")
			)
			(pin input line
				(at -12.7 27.94 0)
				(length 5.08)
				(name "1A2")
				(number "54")
			)
			(pin input line
				(at -12.7 25.4 0)
				(length 5.08)
				(name "1A3")
				(number "52")
			)
			(pin input line
				(at -12.7 22.86 0)
				(length 5.08)
				(name "1A4")
				(number "51")
			)
			(pin input line
				(at -12.7 20.32 0)
				(length 5.08)
				(name "1A5")
				(number "49")
			)
			(pin input line
				(at -12.7 17.78 0)
				(length 5.08)
				(name "1A6")
				(number "48")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 5.08)
				(name "1A7")
				(number "47")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "1A8")
				(number "45")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "1A9")
				(number "44")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "1A10")
				(number "43")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "2A1")
				(number "42")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "2A2")
				(number "41")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "2A3")
				(number "40")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "2A4")
				(number "38")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "2A5")
				(number "37")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "2A6")
				(number "36")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "2A7")
				(number "34")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "2A8")
				(number "33")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 5.08)
				(name "2A9")
				(number "31")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 5.08)
				(name "2A10")
				(number "30")
			)
			(pin input inverted
				(at -12.7 -22.86 0)
				(length 5.08)
				(name "1OE1")
				(number "1")
			)
			(pin input inverted
				(at -12.7 -25.4 0)
				(length 5.08)
				(name "1OE2")
				(number "56")
			)
			(pin input inverted
				(at -12.7 -27.94 0)
				(length 5.08)
				(name "2OE1")
				(number "28")
			)
			(pin input inverted
				(at -12.7 -30.48 0)
				(length 5.08)
				(name "2OE2")
				(number "29")
			)
			(pin passive line
				(at 0 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "22")
			)
			(pin passive line
				(at 0 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "35")
			)
			(pin passive line
				(at 0 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "50")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 5.08)
				(name "VCC")
				(number "7")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "32")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "39")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 5.08)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "46")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "53")
			)
			(pin output line
				(at 12.7 30.48 180)
				(length 5.08)
				(name "1Y1")
				(number "2")
			)
			(pin output line
				(at 12.7 27.94 180)
				(length 5.08)
				(name "1Y2")
				(number "3")
			)
			(pin output line
				(at 12.7 25.4 180)
				(length 5.08)
				(name "1Y3")
				(number "5")
			)
			(pin output line
				(at 12.7 22.86 180)
				(length 5.08)
				(name "1Y4")
				(number "6")
			)
			(pin output line
				(at 12.7 20.32 180)
				(length 5.08)
				(name "1Y5")
				(number "8")
			)
			(pin output line
				(at 12.7 17.78 180)
				(length 5.08)
				(name "1Y6")
				(number "9")
			)
			(pin output line
				(at 12.7 15.24 180)
				(length 5.08)
				(name "1Y7")
				(number "10")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "1Y8")
				(number "12")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "1Y9")
				(number "13")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "1Y10")
				(number "14")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "2Y1")
				(number "15")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "2Y2")
				(number "16")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "2Y3")
				(number "17")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "2Y4")
				(number "19")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "2Y5")
				(number "20")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "2Y6")
				(number "21")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 5.08)
				(name "2Y7")
				(number "23")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 5.08)
				(name "2Y8")
				(number "24")
			)
			(pin output line
				(at 12.7 -15.24 180)
				(length 5.08)
				(name "2Y9")
				(number "26")
			)
			(pin output line
				(at 12.7 -17.78 180)
				(length 5.08)
				(name "2Y10")
				(number "27")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SN74CB3Q3384ADBQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 22.86 0)
		)
		(property "Value" "SN74CB3Q3384ADBQ"
			(at 10.16 22.86 0)
		)
		(property "Footprint" "Package_SO:SSOP-24_3.9x8.7mm_P0.635mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74cb3q3384a.pdf?ts=1634790233466"
			(at 0 0 0)
		)
		(property "Description" "FET Bus Switch, 10bit, 500MHz, 3.3V, SSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "low voltage high bandwidth"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*3.9x8.7mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "SN74CB3Q3384ADBQ_0_1"
			(pin tri_state line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "1A1")
				(number "3")
			)
			(pin tri_state line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "1A2")
				(number "4")
			)
			(pin tri_state line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "1A3")
				(number "7")
			)
			(pin tri_state line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "1A4")
				(number "8")
			)
			(pin tri_state line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "1A5")
				(number "11")
			)
			(pin tri_state line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "2A1")
				(number "14")
			)
			(pin tri_state line
				(at -10.16 0 0)
				(length 2.54)
				(name "2A2")
				(number "17")
			)
			(pin tri_state line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "2A3")
				(number "18")
			)
			(pin tri_state line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "2A4")
				(number "21")
			)
			(pin tri_state line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "2A5")
				(number "22")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "~{1OE}")
				(number "1")
			)
			(pin input line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "~{2OE}")
				(number "13")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "24")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "12")
			)
			(pin tri_state line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "1B1")
				(number "2")
			)
			(pin tri_state line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "1B2")
				(number "5")
			)
			(pin tri_state line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "1B3")
				(number "6")
			)
			(pin tri_state line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "1B4")
				(number "9")
			)
			(pin tri_state line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "1B5")
				(number "10")
			)
			(pin tri_state line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "2B1")
				(number "15")
			)
			(pin tri_state line
				(at 10.16 0 180)
				(length 2.54)
				(name "2B2")
				(number "16")
			)
			(pin tri_state line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "2B3")
				(number "19")
			)
			(pin tri_state line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "2B4")
				(number "20")
			)
			(pin tri_state line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "2B5")
				(number "23")
			)
		)
		(symbol "SN74CB3Q3384ADBQ_1_1")
		(embedded_fonts no)
	)
	(symbol "7400"
		(extends "74LS00")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "7400"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn7400"
			(at 0 0 0)
		)
		(property "Description" "quad 2-input NAND gate"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL nand 2-input"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SO14*"
			(at 0 0 0)
		)
	)
	(symbol "7402"
		(extends "74LS02")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "7402"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn7402"
			(at 0 0 0)
		)
		(property "Description" "quad 2-input NOR gate"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL Nor2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO14* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "74AHC04"
		(extends "74LS04")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74AHC04"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74AHC_AHCT04.pdf"
			(at 0 0 0)
		)
		(property "Description" "Hex Inverter"
			(at 0 0 0)
		)
		(property "ki_keywords" "AHCMOS not inv"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SSOP?14* TSSOP?14*"
			(at 0 0 0)
		)
	)
	(symbol "74AHC240"
		(extends "74HC240")
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74AHC240"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn54ahc240.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit Buffer/Line Driver 3-state Inverting"
			(at 0 0 0)
		)
		(property "ki_keywords" "AHCMOS BUFFER 3State inv"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*7.5x12.8mm*P1.27mm* TSSOP*4.4x6.5mm*P0.65mm* SSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "74AHC244"
		(extends "74HC244")
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74AHC244"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74AHC_AHCT244.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit Buffer/Line Driver 3-state"
			(at 0 0 0)
		)
		(property "ki_keywords" "AHCMOS BUFFER 3State"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm* SSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "74AHC273"
		(extends "74LS273")
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74AHC273"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74AHC_AHCT273.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit D Flip-Flop, reset"
			(at 0 0 0)
		)
		(property "ki_keywords" "AHCMOS DFF DFF8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?20* SO?20* SOIC?20*"
			(at 0 0 0)
		)
	)
	(symbol "74AHC373"
		(extends "74LS373")
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74AHC373"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74AHC373.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit Latch, 3-state outputs"
			(at 0 0 0)
		)
		(property "ki_keywords" "AHCMOS REG DFF DFF8 LATCH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?20* SOIC?20* SO?20* SSOP?20* TSSOP?20*"
			(at 0 0 0)
		)
	)
	(symbol "74AHC374"
		(extends "74LS374")
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74AHC374"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74AHC_AHCT374.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit Register, 3-state outputs"
			(at 0 0 0)
		)
		(property "ki_keywords" "AHCMOS DFF DFF8 REG 3State"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?20* SOIC?20* SO?20*"
			(at 0 0 0)
		)
	)
	(symbol "74AHC541"
		(extends "74LS541")
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74AHC541"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74ahc541.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit Buffer/Line Driver 3-state outputs"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL BUFFER 3State BUS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?20* SOIC*7.5x12.8mm*P1.27mm* TSSOP*4.4x6.5mm*P0.65mm* SSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "74AHC595"
		(extends "74HC595")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74AHC595"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74AHC_AHCT595.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit serial in/out Shift Register 3-State Outputs"
			(at 0 0 0)
		)
		(property "ki_keywords" "AHCMOS SR 3State"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm* SOIC*5.3x10.2mm*P1.27mm* SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "74AHCT04"
		(extends "74LS04")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74AHCT04"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74AHC_AHCT04.pdf"
			(at 0 0 0)
		)
		(property "Description" "Hex Inverter"
			(at 0 0 0)
		)
		(property "ki_keywords" "AHCTMOS not inv"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SSOP?14* TSSOP?14*"
			(at 0 0 0)
		)
	)
	(symbol "74AHCT123"
		(extends "74LS123")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "74AHCT123"
			(at -7.62 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74ahct123a"
			(at 0 0 0)
		)
		(property "Description" "Dual retriggerable monostable multivibrator"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL monostable, multivibrator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
	)
	(symbol "74AHCT125"
		(extends "74LS125")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74AHCT125"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74ahct125.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quadruple Bus Buffer Gates With 3-State Outputs"
			(at 0 0 0)
		)
		(property "ki_keywords" "buffer 3State"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SO14* SSOP?14* TSSOP?14* SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "74AHCT240"
		(extends "74HC240")
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74AHCT240"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74AHCT240.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit Buffer/Line Driver 3-state Inverting"
			(at 0 0 0)
		)
		(property "ki_keywords" "AHCTMOS BUFFER 3State inv"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*7.5x12.8mm*P1.27mm* TSSOP*4.4x6.5mm*P0.65mm* SSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "74AHCT244"
		(extends "74HC244")
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74AHCT244"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74AHC_AHCT244.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit Buffer/Line Driver 3-state"
			(at 0 0 0)
		)
		(property "ki_keywords" "AHCTMOS BUFFER 3State"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm* SSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "74AHCT273"
		(extends "74LS273")
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74AHCT273"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74AHC_AHCT273.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit D Flip-Flop, reset"
			(at 0 0 0)
		)
		(property "ki_keywords" "AHCTMOS DFF DFF8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?20* SO?20* SOIC?20*"
			(at 0 0 0)
		)
	)
	(symbol "74AHCT373"
		(extends "74LS373")
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74AHCT373"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74ahct373.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit Latch, 3-state outputs"
			(at 0 0 0)
		)
		(property "ki_keywords" "AHCTMOS REG DFF DFF8 LATCH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?20* SOIC?20* SO?20* SSOP?20* TSSOP?20*"
			(at 0 0 0)
		)
	)
	(symbol "74AHCT374"
		(extends "74LS374")
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74AHCT374"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74AHC_AHCT374.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit Register, 3-state outputs"
			(at 0 0 0)
		)
		(property "ki_keywords" "AHCTMOS DFF DFF8 REG 3State"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?20* SOIC?20* SO?20*"
			(at 0 0 0)
		)
	)
	(symbol "74AHCT541"
		(extends "74LS541")
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74AHCT541"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74ahct541.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit Buffer/Line Driver 3-state outputs"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL BUFFER 3State BUS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?20* SOIC*7.5x12.8mm*P1.27mm* TSSOP*4.4x6.5mm*P0.65mm* SSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "74AHCT595"
		(extends "74HC595")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74AHCT595"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74AHC_AHCT595.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit serial in/out Shift Register 3-State Outputs"
			(at 0 0 0)
		)
		(property "ki_keywords" "AHCTMOS SR 3State"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm* SOIC*5.3x10.2mm*P1.27mm* SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "74CB3Q16210DGV"
		(extends "74CB3Q16210DGG")
		(property "Reference" "U"
			(at -7.62 31.75 0)
		)
		(property "Value" "74CB3Q16210DGV"
			(at -8.89 -34.29 0)
		)
		(property "Footprint" "Package_SO:TSSOP-48_4.4x9.7mm_P0.4mm"
			(at 21.59 -34.29 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74cb3q16210.pdf"
			(at 0 0 0)
		)
		(property "Description" "20-bit FET bus switch with 10-bit output enables, TVSOP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "bus transmission gates fet switch bidirectional"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "74CB3Q16210DL"
		(extends "74CB3Q16210DGG")
		(property "Reference" "U"
			(at -7.62 31.75 0)
		)
		(property "Value" "74CB3Q16210DL"
			(at -8.255 -34.29 0)
		)
		(property "Footprint" "Package_SO:SSOP-48_7.5x15.9mm_P0.635mm"
			(at 22.86 -34.29 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74cb3q16210.pdf"
			(at 0 0 0)
		)
		(property "Description" "20-bit FET bus switch with 10-bit output enables, SSOP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "bus transmission gates fet switch bidirectional"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*7.5x15.9mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "74CB3T16210DGG"
		(extends "74CB3Q16210DGG")
		(property "Reference" "U"
			(at -7.62 31.75 0)
		)
		(property "Value" "74CB3T16210DGG"
			(at -8.89 -34.29 0)
		)
		(property "Footprint" "Package_SO:TSSOP-48_6.1x12.5mm_P0.5mm"
			(at 21.59 -34.29 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74cb3t16210.pdf"
			(at 0 0 0)
		)
		(property "Description" "20-bit FET bus switch with 10-bit output enables, TSSOP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "bus transmission gates fet switch bidirectional"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*6.1x12.5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "74CB3T16210DGV"
		(extends "74CB3Q16210DGG")
		(property "Reference" "U"
			(at -7.62 31.75 0)
		)
		(property "Value" "74CB3T16210DGV"
			(at -8.89 -34.29 0)
		)
		(property "Footprint" "Package_SO:TSSOP-48_4.4x9.7mm_P0.4mm"
			(at 21.59 -34.29 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74cb3t16210.pdf"
			(at 0 0 0)
		)
		(property "Description" "20-bit FET bus switch with 10-bit output enables, TVSOP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "bus transmission gates fet switch bidirectional"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "74CBT16210CDGG"
		(extends "74CB3Q16210DGG")
		(property "Reference" "U"
			(at -7.62 31.75 0)
		)
		(property "Value" "74CBT16210CDGG"
			(at -8.255 -34.29 0)
		)
		(property "Footprint" "Package_SO:TSSOP-48_6.1x12.5mm_P0.5mm"
			(at 22.225 -34.29 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74cbt16210c.pdf"
			(at 0 0 0)
		)
		(property "Description" "20-bit FET bus switch with 10-bit output enables, TSSOP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "bus transmission gates fet switch bidirectional"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*6.1x12.5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "74CBT16210CDGV"
		(extends "74CB3Q16210DGG")
		(property "Reference" "U"
			(at -7.62 31.75 0)
		)
		(property "Value" "74CBT16210CDGV"
			(at -8.255 -34.29 0)
		)
		(property "Footprint" "Package_SO:TSSOP-48_4.4x9.7mm_P0.4mm"
			(at 21.59 -34.29 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74cbt16210c.pdf"
			(at 0 0 0)
		)
		(property "Description" "20-bit FET bus switch with 10-bit output enables, TVSOP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "bus transmission gates fet switch bidirectional"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "74CBT16210CDL"
		(extends "74CB3Q16210DGG")
		(property "Reference" "U"
			(at -7.62 31.75 0)
		)
		(property "Value" "74CBT16210CDL"
			(at -7.62 -34.29 0)
		)
		(property "Footprint" "Package_SO:SSOP-48_7.5x15.9mm_P0.635mm"
			(at 22.86 -34.29 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74cbt16210c.pdf"
			(at 0 0 0)
		)
		(property "Description" "20-bit FET bus switch with 10-bit output enables, SSOP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "bus transmission gates fet switch bidirectional"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*7.5x15.9mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "74CBT3861"
		(extends "74CBTLV3861")
		(property "Reference" "U"
			(at -7.62 19.05 0)
		)
		(property "Value" "74CBT3861"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74cbt3861.pdf"
			(at 0 0 0)
		)
		(property "Description" "10-bit FET bus switch"
			(at 0 0 0)
		)
		(property "ki_keywords" "bus"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?24*"
			(at 0 0 0)
		)
	)
	(symbol "74CBTD16210DGG"
		(extends "74CB3Q16210DGG")
		(property "Reference" "U"
			(at -7.62 31.75 0)
		)
		(property "Value" "74CBTD16210DGG"
			(at -8.89 -34.29 0)
		)
		(property "Footprint" "Package_SO:TSSOP-48_6.1x12.5mm_P0.5mm"
			(at 22.225 -34.29 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74cbtd16210.pdf"
			(at 0 0 0)
		)
		(property "Description" "20-bit FET bus switch with 10-bit output enables, TSSOP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "bus transmission gates fet switch bidirectional"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*6.1x12.5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "74CBTD16210DGV"
		(extends "74CB3Q16210DGG")
		(property "Reference" "U"
			(at -7.62 31.75 0)
		)
		(property "Value" "74CBTD16210DGV"
			(at -8.89 -34.29 0)
		)
		(property "Footprint" "Package_SO:TSSOP-48_4.4x9.7mm_P0.4mm"
			(at 21.59 -34.29 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74cbtd16210.pdf"
			(at 0 0 0)
		)
		(property "Description" "20-bit FET bus switch with 10-bit output enables, TVSOP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "bus transmission gates fet switch bidirectional"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "74CBTD16210DL"
		(extends "74CB3Q16210DGG")
		(property "Reference" "U"
			(at -7.62 31.75 0)
		)
		(property "Value" "74CBTD16210DL"
			(at -8.255 -34.29 0)
		)
		(property "Footprint" "Package_SO:SSOP-48_7.5x15.9mm_P0.635mm"
			(at 22.86 -34.29 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74cbtd16210.pdf"
			(at 0 0 0)
		)
		(property "Description" "20-bit FET bus switch with 10-bit output enables, SSOP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "bus transmission gates fet switch bidirectional"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*7.5x15.9mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "74CBTD3861"
		(extends "74CBTLV3861")
		(property "Reference" "U"
			(at -7.62 19.05 0)
		)
		(property "Value" "74CBTD3861"
			(at -8.255 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74cbtd3861.pdf"
			(at 0 0 0)
		)
		(property "Description" "10-bit FET Bus switch"
			(at 0 0 0)
		)
		(property "ki_keywords" "bus"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?24*"
			(at 0 0 0)
		)
	)
	(symbol "74HC00"
		(extends "74LS00")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74HC00"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74hc00"
			(at 0 0 0)
		)
		(property "Description" "quad 2-input NAND gate"
			(at 0 0 0)
		)
		(property "ki_keywords" "HCMOS nand 2-input"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SO14*"
			(at 0 0 0)
		)
	)
	(symbol "74HC02"
		(extends "74LS02")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74HC02"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74hc02"
			(at 0 0 0)
		)
		(property "Description" "quad 2-input NOR gate"
			(at 0 0 0)
		)
		(property "ki_keywords" "HCMOS Nor2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO14* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "74HC04"
		(extends "74LS04")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74HC04"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74HC_HCT04.pdf"
			(at 0 0 0)
		)
		(property "Description" "Hex Inverter"
			(at 0 0 0)
		)
		(property "ki_keywords" "HCMOS not inv"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SSOP?14* TSSOP?14*"
			(at 0 0 0)
		)
	)
	(symbol "74HC123"
		(extends "74LS123")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "74HC123"
			(at -7.62 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74HC_HCT123.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual retriggerable monostable multivibrator"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL monostable, multivibrator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
	)
	(symbol "74HC165"
		(extends "74LS165")
		(property "Reference" "U"
			(at -7.62 19.05 0)
		)
		(property "Value" "74HC165"
			(at -7.62 -21.59 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74HC_HCT165.pdf"
			(at 0 0 0)
		)
		(property "Description" "Shift Register, 8-bit, Parallel Load"
			(at 0 0 0)
		)
		(property "ki_keywords" "8 bit shift register parallel load cmos"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16* SO*16*3.9x9.9mm*P1.27mm* SSOP*16*5.3x6.2mm*P0.65mm* TSSOP*16*4.4x5mm*P0.65*"
			(at 0 0 0)
		)
	)
	(symbol "74HC173"
		(extends "74LS173")
		(property "Reference" "U"
			(at -7.62 19.05 0)
		)
		(property "Value" "74HC173"
			(at -7.62 -19.05 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/cd74hc173.pdf"
			(at 0 0 0)
		)
		(property "Description" "4-bit D-type Register, 3 state out"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL REG REG4 3State DFF"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62* SOIC*3.9*9.9mm*P1.27mm* TSSOP*4.4*5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "74HC192"
		(extends "74LS192")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74HC192"
			(at 5.08 13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/cd74hc192.pdf"
			(at 0 0 0)
		)
		(property "Description" "Synchronous 4-bit Up/Down (2 clk) counter"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL CNT CNT4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm* DIP*W7.62mm* SO*3.9*9.9*P1.27mm* TSSOP*4.4*5mm*P0.65*"
			(at 0 0 0)
		)
	)
	(symbol "74HC193"
		(extends "74LS192")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74HC193"
			(at 5.08 13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74HC_HCT193.pdf"
			(at 0 0 0)
		)
		(property "Description" "Synchronous 4-bit Up/Down (2 clk) counter"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL CNT CNT4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm* DIP*W7.62mm* SO*3.9*9.9mm*P1.27mm* TSSOP*4.4*5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "74HC245"
		(extends "74LS245")
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74HC245"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74HC245"
			(at 0 0 0)
		)
		(property "Description" "Octal BUS Transceivers, 3-State outputs"
			(at 0 0 0)
		)
		(property "ki_keywords" "HCMOS BUS 3State"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?20*"
			(at 0 0 0)
		)
	)
	(symbol "74HC273"
		(extends "74LS273")
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74HC273"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74HC_HCT273.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit D Flip-Flop, reset"
			(at 0 0 0)
		)
		(property "ki_keywords" "HCMOS DFF DFF8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?20* SO?20* SOIC?20*"
			(at 0 0 0)
		)
	)
	(symbol "74HC373"
		(extends "74LS373")
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74HC373"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/cd54hc373.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit Latch, 3-state outputs"
			(at 0 0 0)
		)
		(property "ki_keywords" "HCMOS REG DFF DFF8 LATCH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?20* SOIC?20* SO?20* SSOP?20* TSSOP?20*"
			(at 0 0 0)
		)
	)
	(symbol "74HC374"
		(extends "74LS374")
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74HC374"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/cd74hct374.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit Register, 3-state outputs"
			(at 0 0 0)
		)
		(property "ki_keywords" "HCMOS DFF DFF8 REG 3State"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?20* SOIC?20* SO?20*"
			(at 0 0 0)
		)
	)
	(symbol "74HC590A"
		(extends "74HC590")
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74HC590A"
			(at -7.62 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 1.27 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74hc590a.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "8-bit Binary Counter with Output Register 3-State Outputs, DIP-16/SOIC-16/SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "HCMOS Counter 3State"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm* SOIC*5.3x10.2mm*P1.27mm* SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "74HC688"
		(extends "74LS688")
		(property "Reference" "U"
			(at -7.62 26.67 0)
		)
		(property "Value" "74HC688"
			(at -7.62 -26.67 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/cd54hc688.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit magnitude comparator"
			(at 0 0 0)
		)
		(property "ki_keywords" "HCMOS DECOD Arith"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?20* SOIC?20* SO?20* TSSOP?20*"
			(at 0 0 0)
		)
	)
	(symbol "74HC74"
		(extends "74LS74")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "74HC74"
			(at -7.62 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "74xx/74hc_hct74.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual D Flip-flop, Set & Reset"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL DFF"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "74HC85"
		(extends "74LS85")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74HC85"
			(at -7.62 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74HC_HCT85.pdf"
			(at 0 0 0)
		)
		(property "Description" "4-bit Comparator"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL COMP ARITH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16* TSSOP*4.4*5mm*P0.65mm* SO*3.9*9.9mm*P1.27mm* SO*5.3*10.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "74HC86"
		(extends "74LS86")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74HC86"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74HC86"
			(at 0 0 0)
		)
		(property "Description" "Quad 2-input XOR"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL XOR2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "74HCT00"
		(extends "74LS00")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74HCT00"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74hct00"
			(at 0 0 0)
		)
		(property "Description" "quad 2-input NAND gate"
			(at 0 0 0)
		)
		(property "ki_keywords" "HCTMOS nand 2-input"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SO14*"
			(at 0 0 0)
		)
	)
	(symbol "74HCT02"
		(extends "74LS02")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74HCT02"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74hct02"
			(at 0 0 0)
		)
		(property "Description" "quad 2-input NOR gate"
			(at 0 0 0)
		)
		(property "ki_keywords" "HCTMOS Nor2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO14* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "74HCT04"
		(extends "74LS04")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74HCT04"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74HC_HCT04.pdf"
			(at 0 0 0)
		)
		(property "Description" "Hex Inverter"
			(at 0 0 0)
		)
		(property "ki_keywords" "HCTMOS not inv"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SSOP?14* TSSOP?14*"
			(at 0 0 0)
		)
	)
	(symbol "74HCT123"
		(extends "74LS123")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "74HCT123"
			(at -7.62 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74HC_HCT123.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual retriggerable monostable multivibrator"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL monostable, multivibrator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
	)
	(symbol "74HCT137"
		(extends "74HC137")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74HCT137"
			(at 2.54 -11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/cd74hc237.pdf"
			(at 0 0 0)
		)
		(property "Description" "3-to-8 line decoder/multiplexer with address latches, DIP-16/SOIC-16/SSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "demux"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* SSOP*5.3x6.2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "74HCT138"
		(extends "74HC138")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74HCT138"
			(at 2.54 -11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/cd74hc238.pdf"
			(at 0 0 0)
		)
		(property "Description" "3-to-8 line decoder/multiplexer inverting, DIP-16/SOIC-16/SSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "demux"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* SSOP*5.3x6.2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "74HCT164"
		(extends "74HC164")
		(property "Reference" "U"
			(at 1.905 -13.97 0)
		)
		(property "Value" "74HCT164"
			(at 1.905 -16.51 0)
		)
		(property "Footprint" ""
			(at 22.86 -7.62 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74HC_HCT164.pdf"
			(at 22.86 -7.62 0)
		)
		(property "Description" "8-bit serial-in parallel-out shift register"
			(at 0 0 0)
		)
		(property "ki_keywords" "8-bit shift register"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7*P1.27mm* ?SSOP*P0.65mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "74HCT173"
		(extends "74LS173")
		(property "Reference" "U"
			(at -7.62 19.05 0)
		)
		(property "Value" "74HCT173"
			(at -7.62 -19.05 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/cd74hc173.pdf"
			(at 0 0 0)
		)
		(property "Description" "4-bit D-type Register, 3 state out"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL REG REG4 3State DFF"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62* SOIC*3.9*9.9mm*P1.27mm* TSSOP*4.4*5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "74HCT193"
		(extends "74LS192")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74HCT193"
			(at 5.08 13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74HC_HCT193.pdf"
			(at 0 0 0)
		)
		(property "Description" "Synchronous 4-bit Up/Down (2 clk) counter"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL CNT CNT4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm* DIP*W7.62mm* SO*3.9*9.9mm*P1.27mm* TSSOP*4.4*5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "74HCT237"
		(extends "74HC237")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74HCT237"
			(at 2.54 -11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/cd74hc237.pdf"
			(at 0 0 0)
		)
		(property "Description" "3-to-8 line decoder/multiplexer with address latches, DIP-16/SOIC-16/SSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "demux"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* SSOP*5.3x6.2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "74HCT238"
		(extends "74HC238")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74HCT238"
			(at 2.54 -11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/cd74hc238.pdf"
			(at 0 0 0)
		)
		(property "Description" "3-to-8 line decoder/multiplexer, DIP-16/SOIC-16/SSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "demux"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "74HCT240"
		(extends "74HC240")
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74HCT240"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74HC_HCT240.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit buffer; 3-state; inverting"
			(at 0 0 0)
		)
		(property "ki_keywords" "HCTMOS BUFFER 3State inv"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*7.5x12.8mm*P1.27mm* TSSOP*4.4x6.5mm*P0.65mm* SSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "74HCT244"
		(extends "74HC244")
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74HCT244"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74HC_HCT244.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit Buffer/Line Driver 3-state"
			(at 0 0 0)
		)
		(property "ki_keywords" "HCTMOS BUFFER 3State"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm* SSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "74HCT273"
		(extends "74LS273")
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74HCT273"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74HC_HCT273.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit D Flip-Flop, reset"
			(at 0 0 0)
		)
		(property "ki_keywords" "HCTMOS DFF DFF8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?20* SO?20* SOIC?20*"
			(at 0 0 0)
		)
	)
	(symbol "74HCT373"
		(extends "74LS373")
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74HCT373"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74hct373.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit Latch, 3-state outputs"
			(at 0 0 0)
		)
		(property "ki_keywords" "HCTMOS REG DFF DFF8 LATCH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?20* SOIC?20* SO?20* SSOP?20* TSSOP?20*"
			(at 0 0 0)
		)
	)
	(symbol "74HCT374"
		(extends "74LS374")
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74HCT374"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/cd74hct374.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit Register, 3-state outputs"
			(at 0 0 0)
		)
		(property "ki_keywords" "HCTMOS DFF DFF8 REG 3State"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?20* SOIC?20* SO?20*"
			(at 0 0 0)
		)
	)
	(symbol "74HCT4051"
		(extends "74HC4051")
		(property "Reference" "U"
			(at -5.08 11.43 0)
		)
		(property "Value" "74HCT4051"
			(at -7.62 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/cd74hct4051.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "8-channel analog multiplexer/demultiplexer, DIP-16/SOIC-16/TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL Multiplexer Demultiplexer Analog"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* SOIC*5.3x10.2mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "74HCT541"
		(extends "74LS541")
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74HCT541"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74HCT541"
			(at 0 0 0)
		)
		(property "Description" "8-bit Buffer/Line Driver 3-state outputs"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL BUFFER 3State BUS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?20*"
			(at 0 0 0)
		)
	)
	(symbol "74HCT574"
		(extends "74LS574")
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74HCT574"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74HCT574"
			(at 0 0 0)
		)
		(property "Description" "8-bit Register, 3-state outputs"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL REG DFF DFF8 3State"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?20*"
			(at 0 0 0)
		)
	)
	(symbol "74HCT595"
		(extends "74HC595")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74HCT595"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74HC_HCT595.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit serial in/out Shift Register 3-State Outputs"
			(at 0 0 0)
		)
		(property "ki_keywords" "HCTMOS SR 3State"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm* SOIC*5.3x10.2mm*P1.27mm* SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "74HCT596"
		(extends "74HC596")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74HCT596"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74HC_HCT595.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit serial in/out Shift Register Open Collector Outputs"
			(at 0 0 0)
		)
		(property "ki_keywords" "HCTMOS SR OpenCollector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm* SOIC*5.3x10.2mm*P1.27mm* SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "74HCT688"
		(extends "74LS688")
		(property "Reference" "U"
			(at -7.62 26.67 0)
		)
		(property "Value" "74HCT688"
			(at -7.62 -26.67 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/cd54hc688.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit magnitude comparator"
			(at 0 0 0)
		)
		(property "ki_keywords" "HCTMOS DECOD Arith"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?20* SOIC?20* SO?20* TSSOP?20*"
			(at 0 0 0)
		)
	)
	(symbol "74HCT74"
		(extends "74LS74")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "74HCT74"
			(at -7.62 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74HC_HCT74.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual D Flip-flop, Set & Reset"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL DFF"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*3.9x8.65mm_P1.27mm* TSSOP*4.4x5mm_P0.65mm* DHVQFN*2.5x3mm_P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "74HCT85"
		(extends "74LS85")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74HCT85"
			(at -7.62 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74HC_HCT85.pdf"
			(at 0 0 0)
		)
		(property "Description" "4-bit Comparator"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL COMP ARITH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16* SO*3.9*9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "74LS06"
		(extends "74LS05")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74LS06"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS06"
			(at 0 0 0)
		)
		(property "Description" "Inverter Open Collect"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL not inv OpenCol"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "74LS06N"
		(extends "74LS05")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74LS06N"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS06N"
			(at 0 0 0)
		)
		(property "Description" "Inverter Open Collect"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL not inv OpenCol"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "74LS07"
		(extends "74LCX07")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74LS07"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "www.ti.com/lit/ds/symlink/sn74ls07.pdf"
			(at 0 0 0)
		)
		(property "Description" "Hex Buffers and Drivers With Open Collector High Voltage Outputs"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL hex buffer OpenCol"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "74LS14"
		(extends "74HC14")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74LS14"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS14"
			(at 0 0 0)
		)
		(property "Description" "Hex inverter schmitt trigger"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL not inverter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "74LS156"
		(extends "74LS155")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74LS156"
			(at -7.62 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS156"
			(at 0 0 0)
		)
		(property "Description" "Dual 2 to 4 lines Decoder/Demultiplexer, Open Collector"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL DECOD8 DECOD4 DEMUX4 DEMUX8 OpenCol"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
	)
	(symbol "74LS160"
		(extends "74LS161")
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74LS160"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS160"
			(at 0 0 0)
		)
		(property "Description" "Synchronous 4-bit programmable decimal Counter"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL CNT CNT4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
	)
	(symbol "74LS162"
		(extends "74LS161")
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74LS162"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS162"
			(at 0 0 0)
		)
		(property "Description" "Synchronous 4-bit programmable decimal Counter"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL CNT CNT4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
	)
	(symbol "74LS163"
		(extends "74LS161")
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74LS163"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS163"
			(at 0 0 0)
		)
		(property "Description" "Synchronous 4-bit programmable binary Counter"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL CNT CNT4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
	)
	(symbol "74LS169"
		(extends "74LS168")
		(property "Reference" "U"
			(at -7.62 19.05 0)
		)
		(property "Value" "74LS169"
			(at -7.62 -19.05 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS169"
			(at 0 0 0)
		)
		(property "Description" "Synchronous 4-bit Up/Down binary counter"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL CNT CNT4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
	)
	(symbol "74LS191"
		(extends "74LS190")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74LS191"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS191"
			(at 0 0 0)
		)
		(property "Description" "4-bit Synchronous Up/Down binary Counter"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL CNT CNT4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
	)
	(symbol "74LS193"
		(extends "74LS192")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74LS193"
			(at 5.08 13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74ls193.pdf"
			(at 0 0 0)
		)
		(property "Description" "Synchronous 4-bit Up/Down (2 clk) counter"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL CNT CNT4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "74LS197"
		(extends "74LS196")
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74LS197"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS197"
			(at 0 0 0)
		)
		(property "Description" "4 (3+1)-bit presettable binary counter"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL CNT CNT4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "74LS22"
		(extends "74LS20")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74LS22"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS22"
			(at 0 0 0)
		)
		(property "Description" "Dual 4-input NAND Open Collector"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL Nand4 OpenColl"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?12*"
			(at 0 0 0)
		)
	)
	(symbol "74LS246"
		(extends "74LS247")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74LS246"
			(at -7.62 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS246"
			(at 0 0 0)
		)
		(property "Description" "BCD to 7-segment Decoder Open Collector active Low"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL DECOD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
	)
	(symbol "74LS249"
		(extends "74LS248")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74LS249"
			(at -7.62 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS249"
			(at 0 0 0)
		)
		(property "Description" "BCD to 7-segment Decoder, Open collector, Active High"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL DECOD OpenCol"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
	)
	(symbol "74LS28"
		(extends "74LS02")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74LS28"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://eeshop.unl.edu/pdf/74ls28.pdf"
			(at 0 0 0)
		)
		(property "Description" "quad 2-input NOR buffer NRND"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL Nor2 Buffer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO14* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "74LS293"
		(extends "74LS290")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "74LS293"
			(at -7.62 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS293"
			(at 0 0 0)
		)
		(property "Description" "4-bit binary counter"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL CNT CNT4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?12*"
			(at 0 0 0)
		)
	)
	(symbol "74LS37"
		(extends "74LS00")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74LS37"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74ls37"
			(at 0 0 0)
		)
		(property "Description" "quad 2-input NAND buffer"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL nand 2-input buffer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SO14*"
			(at 0 0 0)
		)
	)
	(symbol "74LS38"
		(extends "74LS26")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74LS38"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS38"
			(at 0 0 0)
		)
		(property "Description" "Quad Buffer 2-input NAND Open collector"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL Nand2 OpenCol Buffer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "74LS40"
		(extends "74LS20")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74LS40"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS40"
			(at 0 0 0)
		)
		(property "Description" "Dual 4-input NAND"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL Nand4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?12*"
			(at 0 0 0)
		)
	)
	(symbol "74LS46"
		(extends "74LS47")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "74LS46"
			(at -7.62 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS46"
			(at 0 0 0)
		)
		(property "Description" "BCD to 7-segment Driver, Open Collector, 15V outputs"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL DECOD DECOD7 OpenCol"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
	)
	(symbol "74LS590"
		(extends "74HC590")
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74LS590"
			(at -7.62 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 1.27 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74ls590"
			(at 0 1.27 0)
		)
		(property "Description" "8-bit Binary Counter with Output Register 3-State Outputs, DIP-16/SOIC-16/SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL Counter 3State"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm* SOIC*5.3x10.2mm*P1.27mm* SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "74LS595"
		(extends "74HC595")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74LS595"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74ls595"
			(at 0 0 0)
		)
		(property "Description" "8-bit serial in/out Shift Register 3-State Outputs"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL SR 3State"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm* SOIC*5.3x10.2mm*P1.27mm* SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "74LS596"
		(extends "74HC596")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "74LS596"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74ls596"
			(at 0 0 0)
		)
		(property "Description" "8-bit serial in/out Shift Register Open Collector outputs"
			(at 0 0 0)
		)
		(property "ki_keywords" "HCMOS SR OpenCollector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm* SOIC*5.3x10.2mm*P1.27mm* SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "74LS670"
		(extends "74LS170")
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74LS670"
			(at -7.62 -19.05 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS670"
			(at 0 0 0)
		)
		(property "Description" "4 x 4 Register Files 3-State Outputs"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL Register 3State"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
	)
	(symbol "74LVC125"
		(extends "74LS125")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "74LVC125"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LVC125"
			(at 0 0 0)
		)
		(property "Description" "Quad buffer 3-State outputs"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL buffer 3State"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "CD74AC238"
		(extends "74HC238")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "CD74AC238"
			(at 2.54 -11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/cd74ac238.pdf"
			(at 0 0 0)
		)
		(property "Description" "3-to-8 line decoder/multiplexer, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "demux"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "SN74ALVC164245DGG"
		(extends "74ALVC164245")
		(property "Reference" "U"
			(at -10.16 29.21 0)
		)
		(property "Value" "SN74ALVC164245DGG"
			(at 1.27 -29.21 0)
		)
		(property "Footprint" "Package_SO:TSSOP-48_6.1x12.5mm_P0.5mm"
			(at 0 -1.27 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74alvc164245.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "16-Bit 2.5V to 3.3V or 3.3V to 5V Level-Shifting Transceiver With 3-State Outputs, TSSOP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*6.1x12.5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "SN74ALVC164245DL"
		(extends "74ALVC164245")
		(property "Reference" "U"
			(at -10.16 29.21 0)
		)
		(property "Value" "SN74ALVC164245DL"
			(at 1.27 -29.21 0)
		)
		(property "Footprint" "Package_SO:SSOP-48_7.5x15.9mm_P0.635mm"
			(at 0 -1.27 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74alvc164245.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "16-Bit 2.5V to 3.3V or 3.3V to 5V Level-Shifting Transceiver With 3-State Outputs, SSOP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*7.5x15.9mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "SN74CB3Q3384APW"
		(extends "SN74CB3Q3384ADBQ")
		(property "Reference" "U"
			(at -7.62 22.86 0)
		)
		(property "Value" "SN74CB3Q3384APW"
			(at 10.16 22.86 0)
		)
		(property "Footprint" "Package_SO:TSSOP-24_4.4x7.8mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74cb3q3384a.pdf?ts=1634790233466"
			(at 0 0 0)
		)
		(property "Description" "FET Bus Switch, 10bit, 500MHz, 3.3V, TSSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "low voltage high bandwidth"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x7.8mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "SN74LS07"
		(extends "74LCX07")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "SN74LS07"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "www.ti.com/lit/ds/symlink/sn74ls07.pdf"
			(at 0 0 0)
		)
		(property "Description" "Hex Buffers and Drivers With Open Collector High Voltage Outputs"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL hex buffer OpenCol"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "SN74LS07N"
		(extends "74LCX07")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "SN74LS07N"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "www.ti.com/lit/ds/symlink/sn74ls07.pdf"
			(at 0 0 0)
		)
		(property "Description" "Hex Buffers and Drivers With Open Collector High Voltage Outputs"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL hex buffer OpenCol"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "SN74LV4T125"
		(extends "74LS125")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "SN74LV4T125"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lv4t125.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Supply Logic Level Translator Quad Buffer with 3-State Outputs"
			(at 0 0 0)
		)
		(property "ki_keywords" "3State CMOS shifter translator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
)
