(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "IR4301"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 20.955 0)
		)
		(property "Value" "IR4301"
			(at -7.62 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:Infineon_PQFN-22-15-4EP_6x5mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir4301.pdf?fileId=5546d462533600a4015355d5fc691819"
			(at 0 0 0)
		)
		(property "Description" "PowIRaudio Integrated Analog Input Class D Audio Amplifier, 160W/4ohm, 80V, PQFN-22"
			(at 0 0 0)
		)
		(property "ki_keywords" "integrated class d amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*PQFN*4EP*6x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "IR4301_0_1")
		(symbol "IR4301_1_1"
			(pin power_in line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "VAA")
				(number "1")
			)
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "IN+")
				(number "3")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "IN-")
				(number "4")
			)
			(pin output line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "COMP")
				(number "5")
			)
			(pin power_in line
				(at -10.16 0 0)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "CSD")
				(number "6")
			)
			(pin power_in line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "COM")
				(number "15")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "COM")
				(number "9")
			)
			(pin power_in line
				(at 5.08 20.32 270)
				(length 2.54)
				(name "VP")
				(number "12")
			)
			(pin power_in line
				(at 5.08 -17.78 90)
				(length 2.54)
				(name "VN")
				(number "10")
			)
			(pin passive line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "CSH")
				(number "14")
			)
			(pin power_in line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "VB")
				(number "13")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "VS")
				(number "11")
			)
			(pin power_in line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IR4302"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 20.955 0)
		)
		(property "Value" "IR4302"
			(at -7.62 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:Infineon_PQFN-44-31-5EP_7x7mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir4302.pdf?fileId=5546d462533600a4015355d602a9181d"
			(at 0 0 0)
		)
		(property "Description" "PowIRaudio 2 Channel Integrated Analog Input Class D Audio Amplifier, 130W/4ohm, 80V, PQFN-44"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "integrated class d amplifier 2ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*PQFN*5EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "IR4302_0_1")
		(symbol "IR4302_1_1"
			(pin power_in line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "VAA")
				(number "7")
			)
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "IN+1")
				(number "8")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "IN-1")
				(number "9")
			)
			(pin output line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "COMP1")
				(number "10")
			)
			(pin open_collector line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "FAULT")
				(number "12")
			)
			(pin open_collector line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "CLIP")
				(number "1")
			)
			(pin power_in line
				(at -10.16 0 0)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "CSD")
				(number "11")
			)
			(pin power_in line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "VSS")
				(number "6")
			)
			(pin no_connect line
				(at -7.62 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at -7.62 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "29")
			)
			(pin no_connect line
				(at -7.62 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "30")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "COM")
				(number "15")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "COM")
				(number "28")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "COM")
				(number "31")
			)
			(pin power_in line
				(at 5.08 20.32 270)
				(length 2.54)
				(name "VP1")
				(number "19")
			)
			(pin power_in line
				(at 5.08 -17.78 90)
				(length 2.54)
				(name "VN1")
				(number "21")
			)
			(pin passive line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "CSH1")
				(number "16")
			)
			(pin power_in line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "VB1")
				(number "17")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "VS1")
				(number "18")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "VS1")
				(number "20")
			)
			(pin power_in line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "VCC")
				(number "14")
			)
		)
		(symbol "IR4302_2_1"
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "IN+2")
				(number "4")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "IN-2")
				(number "3")
			)
			(pin output line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "COMP2")
				(number "2")
			)
			(pin power_in line
				(at 5.08 20.32 270)
				(length 2.54)
				(name "VP2")
				(number "24")
			)
			(pin power_in line
				(at 5.08 -17.78 90)
				(length 2.54)
				(name "VN2")
				(number "22")
			)
			(pin passive line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "CSH2")
				(number "27")
			)
			(pin power_in line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "VB2")
				(number "26")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "VS2")
				(number "23")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "VS2")
				(number "25")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IRS2052M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 26.035 0)
		)
		(property "Value" "IRS2052M"
			(at 0 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:Infineon_MLPQ-48-1EP_7x7mm_P0.5mm_EP5.55x5.55mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irs2052mpbf.pdf?fileId=5546d462533600a401535675d3b32788"
			(at 0 0 0)
		)
		(property "Description" "2 CH Digital Audio Amplifier, PWM Modulator, ±100V, 0.5/0.6A, MLPQ-48"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver Class D 2ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*MLPQ*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "IRS2052M_0_1")
		(symbol "IRS2052M_1_1"
			(pin power_in line
				(at -10.16 20.32 0)
				(length 2.54)
				(name "VAA")
				(number "43")
			)
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "IN1")
				(number "44")
			)
			(pin output line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "COMP1")
				(number "45")
			)
			(pin open_collector line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "CLIP1")
				(number "46")
			)
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "GND")
				(number "41")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "CSD")
				(number "47")
			)
			(pin power_in line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "VSS")
				(number "42")
			)
			(pin passive line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "OTP")
				(number "29")
			)
			(pin power_out line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "VREF")
				(number "34")
			)
			(pin passive line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "OCSET")
				(number "33")
			)
			(pin passive line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "DT")
				(number "32")
			)
			(pin no_connect line
				(at -7.62 17.78 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -7.62 10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at -7.62 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "24")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "COM")
				(number "19")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "COM")
				(number "30")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "COM")
				(number "49")
			)
			(pin no_connect line
				(at 7.62 15.24 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "25")
			)
			(pin no_connect line
				(at 7.62 12.7 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "27")
			)
			(pin no_connect line
				(at 7.62 10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "28")
			)
			(pin no_connect line
				(at 7.62 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "35")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "36")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "37")
			)
			(pin no_connect line
				(at 7.62 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "48")
			)
			(pin passive line
				(at 10.16 20.32 180)
				(length 2.54)
				(name "CSH1")
				(number "16")
			)
			(pin power_in line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "VB1")
				(number "15")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "HO1")
				(number "14")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VS1")
				(number "11")
			)
			(pin power_in line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "VCC")
				(number "31")
			)
			(pin output line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "LO1")
				(number "17")
			)
		)
		(symbol "IRS2052M_2_1"
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "IN2")
				(number "40")
			)
			(pin output line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "COMP2")
				(number "39")
			)
			(pin open_collector line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "CLIP2")
				(number "38")
			)
			(pin open_collector line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "OTW")
				(number "2")
			)
			(pin open_collector line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "FAULT")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "X1A")
				(number "6")
			)
			(pin output line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "X1B")
				(number "5")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "X2A")
				(number "8")
			)
			(pin output line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "X2B")
				(number "7")
			)
			(pin input line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "XSL")
				(number "9")
			)
			(pin output line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "CKO")
				(number "4")
			)
			(pin passive line
				(at 10.16 20.32 180)
				(length 2.54)
				(name "CSH2")
				(number "21")
			)
			(pin power_in line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "VB2")
				(number "22")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "HO2")
				(number "23")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VS2")
				(number "26")
			)
			(pin power_in line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "VCC2")
				(number "18")
			)
			(pin output line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "LO2")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IRS2092"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 26.035 0)
		)
		(property "Value" "IRS2092"
			(at 0 24.13 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/irs2092.pdf?fileId=5546d462533600a401535675f1be2790"
			(at 0 0 0)
		)
		(property "Description" "Protected Digital Audio Amplifier, PWM Modulator, ±100V, 1.0/1.2A, PDIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver Class D"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "IRS2092_0_1")
		(symbol "IRS2092_1_1"
			(pin power_in line
				(at -10.16 20.32 0)
				(length 2.54)
				(name "VAA")
				(number "1")
			)
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "IN-")
				(number "3")
			)
			(pin output line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "COMP")
				(number "4")
			)
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "CSD")
				(number "5")
			)
			(pin power_in line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "VSS")
				(number "6")
			)
			(pin power_out line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "VREF")
				(number "7")
			)
			(pin passive line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "OCSET")
				(number "8")
			)
			(pin passive line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "DT")
				(number "9")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "COM")
				(number "10")
			)
			(pin passive line
				(at 10.16 20.32 180)
				(length 2.54)
				(name "CSH")
				(number "16")
			)
			(pin power_in line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "VB")
				(number "15")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "HO")
				(number "14")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VS")
				(number "13")
			)
			(pin power_in line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "VCC")
				(number "12")
			)
			(pin output line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "LO")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IRS2092S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 26.035 0)
		)
		(property "Value" "IRS2092S"
			(at 0 24.13 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/irs2092.pdf?fileId=5546d462533600a401535675f1be2790"
			(at 0 0 0)
		)
		(property "Description" "Protected Digital Audio Amplifier, PWM Modulator, ±100V, 1.0/1.2A, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver Class D"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "IRS2092S_0_1")
		(symbol "IRS2092S_1_1"
			(pin power_in line
				(at -10.16 20.32 0)
				(length 2.54)
				(name "VAA")
				(number "1")
			)
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "IN-")
				(number "3")
			)
			(pin output line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "COMP")
				(number "4")
			)
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "CSD")
				(number "5")
			)
			(pin power_in line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "VSS")
				(number "6")
			)
			(pin power_out line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "VREF")
				(number "7")
			)
			(pin passive line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "OCSET")
				(number "8")
			)
			(pin passive line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "DT")
				(number "9")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "COM")
				(number "10")
			)
			(pin passive line
				(at 10.16 20.32 180)
				(length 2.54)
				(name "CSH")
				(number "16")
			)
			(pin power_in line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "VB")
				(number "15")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "HO")
				(number "14")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VS")
				(number "13")
			)
			(pin power_in line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "VCC")
				(number "12")
			)
			(pin output line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "LO")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IRS2093M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 26.035 0)
		)
		(property "Value" "IRS2093M"
			(at 0 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:Infineon_MLPQ-48-1EP_7x7mm_P0.5mm_EP5.55x5.55mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irs2093mpbf.pdf?fileId=5546d462533600a401535675fb892793"
			(at 0 0 0)
		)
		(property "Description" "4 CH Digital Audio Amplifier, PWM Modulator, ±100V, 0.5/0.6A, MLPQ-48"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver Class D 4ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*MLPQ*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "IRS2093M_0_1")
		(symbol "IRS2093M_1_1"
			(pin power_in line
				(at -10.16 20.32 0)
				(length 2.54)
				(name "VAA")
				(number "43")
			)
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "IN1")
				(number "46")
			)
			(pin output line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "COMP1")
				(number "47")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "DS")
				(number "1")
			)
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "GND")
				(number "41")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "CSD")
				(number "48")
			)
			(pin power_in line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "VSS")
				(number "42")
			)
			(pin power_out line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "VREF")
				(number "36")
			)
			(pin passive line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "OCSET")
				(number "35")
			)
			(pin passive line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "DT")
				(number "34")
			)
			(pin no_connect line
				(at -7.62 17.78 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -7.62 10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at -7.62 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "COM")
				(number "20")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "COM")
				(number "32")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "COM")
				(number "49")
			)
			(pin no_connect line
				(at 7.62 15.24 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "18")
			)
			(pin no_connect line
				(at 7.62 12.7 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "19")
			)
			(pin no_connect line
				(at 7.62 10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "31")
			)
			(pin passive line
				(at 10.16 20.32 180)
				(length 2.54)
				(name "CSH1")
				(number "14")
			)
			(pin power_in line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "VB1")
				(number "13")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "HO1")
				(number "12")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VS1")
				(number "11")
			)
			(pin power_in line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "VCC")
				(number "33")
			)
			(pin output line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "LO1")
				(number "15")
			)
		)
		(symbol "IRS2093M_2_1"
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "IN2")
				(number "44")
			)
			(pin output line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "COMP2")
				(number "45")
			)
			(pin passive line
				(at 10.16 20.32 180)
				(length 2.54)
				(name "CSH2")
				(number "7")
			)
			(pin power_in line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "VB2")
				(number "8")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "HO2")
				(number "9")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VS2")
				(number "10")
			)
			(pin power_in line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "VCC2")
				(number "17")
			)
			(pin output line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "LO2")
				(number "16")
			)
		)
		(symbol "IRS2093M_3_1"
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "IN3")
				(number "38")
			)
			(pin output line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "COMP3")
				(number "37")
			)
			(pin passive line
				(at 10.16 20.32 180)
				(length 2.54)
				(name "CSH3")
				(number "23")
			)
			(pin power_in line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "VB3")
				(number "24")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "HO3")
				(number "25")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VS3")
				(number "26")
			)
			(pin output line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "LO3")
				(number "22")
			)
		)
		(symbol "IRS2093M_4_1"
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "IN4")
				(number "40")
			)
			(pin output line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "COMP4")
				(number "39")
			)
			(pin passive line
				(at 10.16 20.32 180)
				(length 2.54)
				(name "CSH4")
				(number "30")
			)
			(pin power_in line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "VB4")
				(number "29")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "HO4")
				(number "28")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VS4")
				(number "27")
			)
			(pin output line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "LO4")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IRS20957S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 24.13 0)
		)
		(property "Value" "IRS20957S"
			(at 0 21.59 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/irs20957spbf.pdf?fileId=5546d462533600a401535676143e2799"
			(at 0 0 0)
		)
		(property "Description" "Protected Digital Audio Driver, ±100V, 1.0/1.2A, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver Class D"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "IRS20957S_0_1")
		(symbol "IRS20957S_1_1"
			(pin power_in line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "IN")
				(number "3")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "CSD")
				(number "2")
			)
			(pin power_in line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin power_out line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "VREF")
				(number "6")
			)
			(pin passive line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "OCSET")
				(number "7")
			)
			(pin passive line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "DT")
				(number "8")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "COM")
				(number "9")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin passive line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "CSH")
				(number "16")
			)
			(pin power_in line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "VB")
				(number "15")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "HO")
				(number "14")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VS")
				(number "13")
			)
			(pin power_in line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "VCC")
				(number "11")
			)
			(pin output line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "LO")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IRS20965S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 24.13 0)
		)
		(property "Value" "IRS20965S"
			(at 0 21.59 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irs20965spbf.pdf?fileId=5546d462533600a4015356761d8b279b"
			(at 0 0 0)
		)
		(property "Description" "Class D Audio Driver, ±100V, 2.0/2.0A, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver Class D"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "IRS20965S_0_1")
		(symbol "IRS20965S_1_1"
			(pin power_in line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "HIN")
				(number "4")
			)
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "LIN")
				(number "5")
			)
			(pin open_collector line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "OC")
				(number "3")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "CSD")
				(number "2")
			)
			(pin power_in line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "VSS")
				(number "6")
			)
			(pin power_out line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "VREF")
				(number "7")
			)
			(pin passive line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "OCSET")
				(number "8")
			)
			(pin input line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "STP")
				(number "12")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "COM")
				(number "9")
			)
			(pin passive line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "CSH")
				(number "16")
			)
			(pin power_in line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "VB")
				(number "15")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "HO")
				(number "14")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VS")
				(number "13")
			)
			(pin power_in line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "VCC")
				(number "11")
			)
			(pin output line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "LO")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IRS2452AM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 26.035 0)
		)
		(property "Value" "IRS2452AM"
			(at 0 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:Infineon_MLPQ-40-32-1EP_7x7mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IRS2452AM-DS-v01_00-EN.pdf?fileId=5546d462584d1d4a01584ee4f1f00713"
			(at 0 0 0)
		)
		(property "Description" "Class D Audio IC, PWM Modulator, ±200V, 0.5/0.6A, MLPQ-32"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver Class D 2ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*MLPQ*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "IRS2452AM_0_1")
		(symbol "IRS2452AM_1_1"
			(pin power_in line
				(at -10.16 20.32 0)
				(length 2.54)
				(name "VAA")
				(number "5")
			)
			(pin input line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "IN+1")
				(number "8")
			)
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "IN-1")
				(number "9")
			)
			(pin output line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "COMP1")
				(number "10")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "BTL")
				(number "12")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "A/B")
				(number "31")
			)
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "CSD")
				(number "11")
			)
			(pin power_in line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin passive line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "OTP")
				(number "23")
			)
			(pin passive line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "DT")
				(number "24")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "19")
			)
			(pin no_connect line
				(at -7.62 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "21")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "COM")
				(number "20")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "COM")
				(number "33")
			)
			(pin passive line
				(at 10.16 20.32 180)
				(length 2.54)
				(name "CSH1")
				(number "13")
			)
			(pin power_in line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "VB1")
				(number "14")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "HO1")
				(number "15")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VS1")
				(number "16")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "CSL1")
				(number "17")
			)
			(pin power_in line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "VCC")
				(number "22")
			)
			(pin output line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "LO1")
				(number "18")
			)
		)
		(symbol "IRS2452AM_2_1"
			(pin input line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "IN+2")
				(number "3")
			)
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "IN-2")
				(number "2")
			)
			(pin output line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "COMP2")
				(number "1")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "CLK")
				(number "32")
			)
			(pin passive line
				(at 10.16 20.32 180)
				(length 2.54)
				(name "CSH2")
				(number "30")
			)
			(pin power_in line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "VB2")
				(number "29")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "HO2")
				(number "28")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VS2")
				(number "27")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "CSL2")
				(number "26")
			)
			(pin output line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "LO2")
				(number "25")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IS31AP4991-GRLS2"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 7.62 0)
		)
		(property "Value" "IS31AP4991-GRLS2"
			(at 10.16 5.08 0)
		)
		(property "Footprint" "Package_SO:SOP-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.issi.com/WW/pdf/31AP4991.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.2W, 2.7-5.5V, Audio Power Amplifier, Active-Low Standby, SOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "ultra low consumption distortion"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "IS31AP4991-GRLS2_0_1")
		(symbol "IS31AP4991-GRLS2_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "3")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "4")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "~{SDB}")
				(number "7")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 5.08)
				(name "BYP")
				(number "5")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IS31AP4991-SLS2"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 7.62 0)
		)
		(property "Value" "IS31AP4991-SLS2"
			(at 10.16 5.08 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.issi.com/WW/pdf/31AP4991.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.2W, 2.7-5.5V, Audio Power Amplifier, Active-Low Standby, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "ultra low consumption distortion"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "IS31AP4991-SLS2_0_1")
		(symbol "IS31AP4991-SLS2_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "7")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "~{SDB}")
				(number "1")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 5.08)
				(name "BYP")
				(number "2")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM1875"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "LM1875"
			(at 3.81 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-5_P3.4x3.7mm_StaggerOdd_Lead3.8mm_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm1875.pdf"
			(at 0 0 0)
		)
		(property "Description" "20W Audio Power Amplifier, TO-220-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*StaggerOdd*"
			(at 0 0 0)
		)
		(symbol "LM1875_0_1")
		(symbol "LM1875_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "3")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM1876"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 6.35 0)
		)
		(property "Value" "LM1876"
			(at 7.62 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-15_P2.54x2.54mm_StaggerOdd_Lead4.58mm_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm1876.pdf"
			(at 0 0 0)
		)
		(property "Description" "Overture Audio Power Amplifier Series Dual 20W Audio Power Amplifier with Mute and Standby Modes, TO-220-15"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier 2ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*StaggerOdd*"
			(at 0 0 0)
		)
		(symbol "LM1876_0_1")
		(symbol "LM1876_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "8")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "7")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "STBY")
				(number "9")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 5.08)
				(name "GND")
				(number "5")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 6.35)
				(name "MUTE")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(symbol "LM1876_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "13")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "12")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "15")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "STBY")
				(number "14")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 5.08)
				(name "GND")
				(number "10")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 6.35)
				(name "MUTE")
				(number "11")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM1877"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 6.35 0)
		)
		(property "Value" "LM1877"
			(at 5.08 3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm1877.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Audio Power Amplifier, PDIP-14/SOIC-14"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier 2ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "LM1877_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "6")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "7")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "BIAS")
				(number "1")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(symbol "LM1877_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "9")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "8")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "13")
			)
		)
		(symbol "LM1877_3_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "14")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM2876"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 6.35 0)
		)
		(property "Value" "LM2876"
			(at 5.08 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-11_P3.4x5.08mm_StaggerOdd_Lead4.85mm_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2876.pdf"
			(at 0 0 0)
		)
		(property "Description" "Overture Audio Power Amplifier Series High-Performance 40W Audio Power Amplifier w/Mute, TO-220-11"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier 2ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*StaggerOdd*"
			(at 0 0 0)
		)
		(symbol "LM2876_0_1")
		(symbol "LM2876_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "10")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "9")
			)
			(pin no_connect line
				(at -5.08 5.08 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin no_connect line
				(at -5.08 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "1")
			)
			(pin no_connect line
				(at -2.54 3.81 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -2.54 -3.81 270)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "MUTE")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM380N"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 6.35 0)
		)
		(property "Value" "LM380N"
			(at 6.35 3.81 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm380.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.5W Audio Power Amplifier, PDIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "LM380N_0_1")
		(symbol "LM380N_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "6")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "VS")
				(number "14")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 5.08)
				(name "BYPASS")
				(number "1")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at 0 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 5.08)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM380N-8"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 6.35 0)
		)
		(property "Value" "LM380N-8"
			(at 6.35 3.81 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm380.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.5W Audio Power Amplifier, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "LM380N-8_0_1")
		(symbol "LM380N-8_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "3")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "VS")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 5.08)
				(name "BYPASS")
				(number "8")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 5.08)
				(name "GND")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM384"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 6.35 0)
		)
		(property "Value" "LM384"
			(at 5.08 3.81 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm384.pdf"
			(at 0 0 0)
		)
		(property "Description" "5W Audio Power Amplifier, PDIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "LM384_0_1")
		(symbol "LM384_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "6")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "VS")
				(number "14")
			)
			(pin no_connect line
				(at -2.54 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 5.08)
				(name "BYPASS")
				(number "1")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 5.08)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM386"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 7.62 0)
		)
		(property "Value" "LM386"
			(at 1.27 5.08 0)
		)
		(property "Footprint" ""
			(at 2.54 2.54 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm386.pdf"
			(at 5.08 5.08 0)
		)
		(property "Description" "Low Voltage Audio Power Amplifier, DIP-8/SOIC-8/SSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single Power opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* MSSOP*P0.65mm* TSSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LM386_0_1")
		(symbol "LM386_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "4")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "BYPASS")
				(number "7")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "GAIN")
				(number "1")
			)
			(pin input line
				(at 2.54 -7.62 90)
				(length 6.35)
				(name "GAIN")
				(number "8")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM3886"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 6.35 0)
		)
		(property "Value" "LM3886"
			(at 5.08 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-11_P3.4x5.08mm_StaggerOdd_Lead4.85mm_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm3886.pdf"
			(at 0 0 0)
		)
		(property "Description" "Overture Audio Power Amplifier Series High-Performance 68W Audio Power Amplifier w/Mute, TO-220-11"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*StaggerOdd*"
			(at 0 0 0)
		)
		(symbol "LM3886_0_1")
		(symbol "LM3886_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "10")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "9")
			)
			(pin no_connect line
				(at -5.08 5.08 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin no_connect line
				(at -5.08 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "1")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 3.81)
				(hide yes)
				(name "V+")
				(number "5")
			)
			(pin no_connect line
				(at -2.54 3.81 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "MUTE")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM4752TS"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 6.35 0)
		)
		(property "Value" "LM4752TS"
			(at 5.08 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-7_TabPin4"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4752.pdf"
			(at 0 0 0)
		)
		(property "Description" "Stereo 11W Audio Power Amplifier, TO-263-7"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier 2ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*TabPin4*"
			(at 0 0 0)
		)
		(symbol "LM4752TS_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "+")
				(number "6")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "BIAS")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "LM4752TS_2_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "+")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "LM4752TS_3_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM4755TS"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 6.35 0)
		)
		(property "Value" "LM4755TS"
			(at 5.08 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-9_TabPin5"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4755.pdf"
			(at 0 0 0)
		)
		(property "Description" "Stereo 11W Audio Power Amplifier with Mute, TO-263-9"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier 2ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*TabPin5*"
			(at 0 0 0)
		)
		(symbol "LM4755TS_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "+")
				(number "7")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "MUTE")
				(number "2")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "BIAS")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(symbol "LM4755TS_2_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "LM4755TS_3_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM4766"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 6.35 0)
		)
		(property "Value" "LM4766"
			(at 5.08 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-15_P2.54x2.54mm_StaggerOdd_Lead4.58mm_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4766.pdf"
			(at 0 0 0)
		)
		(property "Description" "Overture Audio Power Amplifier Series Dual 40W Audio Power Amplifier with Mute, TO-220-15"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier 2ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*StaggerOdd*"
			(at 0 0 0)
		)
		(symbol "LM4766_0_1")
		(symbol "LM4766_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "8")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "7")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "MUTE")
				(number "6")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 5.08)
				(name "GND")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(symbol "LM4766_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "13")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "12")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "15")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "MUTE")
				(number "11")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 5.08)
				(name "GND")
				(number "10")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM4810"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "LM4810"
			(at 5.08 11.43 0)
		)
		(property "Footprint" "Package_SO:TSSOP-8_3x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4810.pdf"
			(at 0 0 0)
		)
		(property "Description" "Boomer Dual 105mW Headphone Amplifier with Active-High Shutdown Mode, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier headphone"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LM4810_0_1")
		(symbol "LM4810_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VIN1")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "VIN2")
				(number "6")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SHDN")
				(number "5")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VOUT1")
				(number "1")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "VOUT2")
				(number "7")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "BYPASS")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM4811"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "LM4811"
			(at 5.08 11.43 0)
		)
		(property "Footprint" "Package_SO:TSSOP-10_3x3mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4811.pdf"
			(at 0 0 0)
		)
		(property "Description" "Boomer Dual 105mW Headphone Amplifier with Digital Volume Control and Shutdown Mode, VSSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier headphone 2ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LM4811_0_1")
		(symbol "LM4811_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VIN1")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "VIN2")
				(number "8")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SHDN")
				(number "7")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "UP/DN")
				(number "6")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "CLOCK")
				(number "4")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "10")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VOUT1")
				(number "1")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "VOUT2")
				(number "9")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "BYPASS")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM4950TA"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 6.35 0)
		)
		(property "Value" "LM4950TA"
			(at 5.08 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-5_P3.4x3.7mm_StaggerOdd_Lead3.8mm_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4950.pdf"
			(at 0 0 0)
		)
		(property "Description" "Boomer Audio Power Amplifier Series 7.5W Mono-BTL or 3.1W Stereo Audio Power Amplifier, TO-220-9"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*StaggerOdd*"
			(at 0 0 0)
		)
		(symbol "LM4950TA_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "VINA")
				(number "1")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "~{SHDN}")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 5.08)
				(name "BYP")
				(number "8")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(symbol "LM4950TA_2_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "VINB")
				(number "9")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "LM4950TA_3_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM4950TS"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 6.35 0)
		)
		(property "Value" "LM4950TS"
			(at 5.08 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-9_TabPin5"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4950.pdf"
			(at 0 0 0)
		)
		(property "Description" "Boomer Audio Power Amplifier Series 7.5W Mono-BTL or 3.1W Stereo Audio Power Amplifier, TO-263-9"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*TabPin5*"
			(at 0 0 0)
		)
		(symbol "LM4950TS_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "VINA")
				(number "1")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "~{SHDN}")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 5.08)
				(name "BYP")
				(number "8")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(symbol "LM4950TS_2_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "VINB")
				(number "9")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "LM4950TS_3_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM4990ITL"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 7.62 0)
		)
		(property "Value" "LM4990ITL"
			(at 5.08 5.08 0)
		)
		(property "Footprint" "Package_BGA:Texas_DSBGA-9_1.4715x1.4715mm_Layout3x3_P0.5mm"
			(at 2.54 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4990.pdf"
			(at 0 0 0)
		)
		(property "Description" "Boomer 2 Watt Audio Power Amplifier with Selectable Shutdown Logic Level, DSBGA-9"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier class d"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DSBGA*1.4715x1.4715mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LM4990ITL_0_1")
		(symbol "LM4990ITL_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "A3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "A1")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "B3")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "B1")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B2")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "~{SHDN}")
				(number "C3")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "BYP")
				(number "C1")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "C2")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "A2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM4990LD"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 7.62 0)
		)
		(property "Value" "LM4990LD"
			(at 7.62 5.08 0)
		)
		(property "Footprint" "Package_SON:WSON-10-1EP_4x3mm_P0.5mm_EP2.2x2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4990.pdf"
			(at 0 0 0)
		)
		(property "Description" "Boomer 2 Watt Audio Power Amplifier with Selectable Shutdown Logic Level, WSON-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier class d"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*EP*4x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LM4990LD_0_1")
		(symbol "LM4990LD_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "5")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "9")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "SHDN")
				(number "1")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "BYP")
				(number "2")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 6.35)
				(name "SD")
				(number "3")
			)
			(pin power_in line
				(at 2.54 -7.62 90)
				(length 6.35)
				(name "~")
				(number "11")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM4990MH"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 7.62 0)
		)
		(property "Value" "LM4990MH"
			(at 7.62 5.08 0)
		)
		(property "Footprint" "Package_SO:MSOP-10-1EP_3x3mm_P0.5mm_EP1.68x1.88mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4990.pdf"
			(at 0 0 0)
		)
		(property "Description" "Boomer 2 Watt Audio Power Amplifier with Selectable Shutdown Logic Level, MSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier class d"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LM4990MH_0_1")
		(symbol "LM4990MH_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "5")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "9")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "~{SHDN}")
				(number "1")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "BYP")
				(number "2")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 6.35)
				(name "SD")
				(number "3")
			)
			(pin power_in line
				(at 2.54 -7.62 90)
				(length 6.35)
				(name "~")
				(number "11")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM4990MM"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 7.62 0)
		)
		(property "Value" "LM4990MM"
			(at 5.08 5.08 0)
		)
		(property "Footprint" "Package_SO:TSSOP-8_3x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4990.pdf"
			(at 0 0 0)
		)
		(property "Description" "Boomer 2 Watt Audio Power Amplifier with Selectable Shutdown Logic Level, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier class d"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LM4990MM_0_1")
		(symbol "LM4990MM_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "7")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "~{SHDN}")
				(number "1")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "BYP")
				(number "2")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LME49600"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 6.35 0)
		)
		(property "Value" "LME49600"
			(at 6.35 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lme49600.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Performance, High-Fidelity, High-Current Headphone Buffer, 250mA, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio buffer amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
		(symbol "LME49600_0_1")
		(symbol "LME49600_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 5.08)
				(name "BW")
				(number "1")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MA12040"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 44.45 0)
		)
		(property "Value" "MA12040"
			(at 3.81 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.45x5.45mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-MA12040-DS-v01_00-EN.pdf?fileId=5546d46264a8de7e0164b7467a3d617c"
			(at 0 0 0)
		)
		(property "Description" "Filterless and High-Efficiency +4V to +18V Audio Amplifier with Analog Input, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "integrated class d amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MA12040_0_1")
		(symbol "MA12040_1_1"
			(pin passive line
				(at -12.7 40.64 0)
				(length 2.54)
				(name "NC")
				(number "49")
			)
			(pin passive line
				(at -12.7 38.1 0)
				(length 2.54)
				(name "NC")
				(number "64")
			)
			(pin input line
				(at -12.7 33.02 0)
				(length 2.54)
				(name "IN0A")
				(number "21")
			)
			(pin input line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "IN0B")
				(number "22")
			)
			(pin input line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "IN1A")
				(number "23")
			)
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "IN1B")
				(number "24")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "CLKIO")
				(number "32")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "CLKM/S")
				(number "31")
			)
			(pin output line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "~{CLIP}")
				(number "15")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "~{ERROR}")
				(number "16")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{ENABLE}")
				(number "33")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{MUTE}")
				(number "34")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "SCL")
				(number "27")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "SDA")
				(number "30")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "AD0")
				(number "28")
			)
			(pin input line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "AD1")
				(number "29")
			)
			(pin input line
				(at -12.7 -25.4 0)
				(length 2.54)
				(name "MSEL0")
				(number "51")
			)
			(pin input line
				(at -12.7 -27.94 0)
				(length 2.54)
				(name "MSEL1")
				(number "50")
			)
			(pin passive line
				(at -12.7 -33.02 0)
				(length 2.54)
				(name "VGDC")
				(number "54")
			)
			(pin passive line
				(at -12.7 -35.56 0)
				(length 2.54)
				(name "CDC")
				(number "56")
			)
			(pin passive line
				(at -12.7 -38.1 0)
				(length 2.54)
				(name "CMSE")
				(number "18")
			)
			(pin passive line
				(at -12.7 -40.64 0)
				(length 2.54)
				(name "CREF")
				(number "20")
			)
			(pin power_in line
				(at -5.08 45.72 270)
				(length 2.54)
				(name "AVDD")
				(number "17")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "DVDD")
				(number "55")
			)
			(pin power_in line
				(at -2.54 -45.72 90)
				(length 2.54)
				(name "AVSS")
				(number "19")
			)
			(pin passive line
				(at -2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "AVSS")
				(number "25")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "PVDD")
				(number "7")
			)
			(pin passive line
				(at 0 45.72 270)
				(length 2.54)
				(hide yes)
				(name "PVDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "DVSS")
				(number "26")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "DVSS")
				(number "59")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "PVDD")
				(number "41")
			)
			(pin passive line
				(at 2.54 45.72 270)
				(length 2.54)
				(hide yes)
				(name "PVDD")
				(number "42")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 2.54)
				(name "PVSS")
				(number "1")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "PVSS")
				(number "13")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "PVSS")
				(number "14")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "PVSS")
				(number "2")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "PVSS")
				(number "35")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "PVSS")
				(number "36")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "PVSS")
				(number "47")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "PVSS")
				(number "48")
			)
			(pin passive line
				(at 12.7 40.64 180)
				(length 2.54)
				(name "CF0AP")
				(number "6")
			)
			(pin passive line
				(at 12.7 35.56 180)
				(length 2.54)
				(name "CF0AN")
				(number "3")
			)
			(pin output line
				(at 12.7 33.02 180)
				(length 2.54)
				(name "OUT0A")
				(number "4")
			)
			(pin passive line
				(at 12.7 33.02 180)
				(length 2.54)
				(hide yes)
				(name "OUT0A")
				(number "5")
			)
			(pin passive line
				(at 12.7 27.94 180)
				(length 2.54)
				(name "CF0BP")
				(number "9")
			)
			(pin passive line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "CF0BN")
				(number "12")
			)
			(pin output line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "OUT0B")
				(number "10")
			)
			(pin passive line
				(at 12.7 20.32 180)
				(length 2.54)
				(hide yes)
				(name "OUT0B")
				(number "11")
			)
			(pin passive line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "CF1AP")
				(number "43")
			)
			(pin passive line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "CF1AN")
				(number "46")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "OUT1A")
				(number "44")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 2.54)
				(hide yes)
				(name "OUT1A")
				(number "45")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CF1BP")
				(number "40")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CF1BN")
				(number "37")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "OUT1B")
				(number "38")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "OUT1B")
				(number "39")
			)
			(pin passive line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "CGD1P")
				(number "53")
			)
			(pin passive line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "CGD1N")
				(number "52")
			)
			(pin passive line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "CFDCP")
				(number "57")
			)
			(pin passive line
				(at 12.7 -25.4 180)
				(length 2.54)
				(name "CFDCN")
				(number "58")
			)
			(pin passive line
				(at 12.7 -27.94 180)
				(length 2.54)
				(name "CGD0P")
				(number "60")
			)
			(pin passive line
				(at 12.7 -33.02 180)
				(length 2.54)
				(name "CGD0N")
				(number "61")
			)
			(pin passive line
				(at 12.7 -35.56 180)
				(length 2.54)
				(name "CFGDP")
				(number "62")
			)
			(pin passive line
				(at 12.7 -40.64 180)
				(length 2.54)
				(name "CFGDN")
				(number "63")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MA12040P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 44.45 0)
		)
		(property "Value" "MA12040P"
			(at 3.81 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.45x5.45mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-MA12040P-DS-v01_00-EN.pdf?fileId=5546d46264a8de7e0164b74ff0e561a2"
			(at 0 0 0)
		)
		(property "Description" "Filterless and High-Efficiency +4V to +18V Audio Amplifier with I2S Digital Input, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "integrated class d amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MA12040P_0_1")
		(symbol "MA12040P_1_1"
			(pin passive line
				(at -12.7 40.64 0)
				(length 2.54)
				(name "NC")
				(number "49")
			)
			(pin passive line
				(at -12.7 38.1 0)
				(length 2.54)
				(name "NC")
				(number "64")
			)
			(pin input line
				(at -12.7 33.02 0)
				(length 2.54)
				(name "SCLK")
				(number "21")
			)
			(pin input line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "WS")
				(number "22")
			)
			(pin input line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "SD0")
				(number "23")
			)
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "SD1")
				(number "24")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "CLK")
				(number "32")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "CLKM/S")
				(number "31")
			)
			(pin output line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "~{CLIP}")
				(number "15")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "~{ERROR}")
				(number "16")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{ENABLE}")
				(number "33")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{MUTE}")
				(number "34")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "SCL")
				(number "27")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "SDA")
				(number "30")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "AD0")
				(number "28")
			)
			(pin input line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "AD1")
				(number "29")
			)
			(pin input line
				(at -12.7 -25.4 0)
				(length 2.54)
				(name "MSEL0")
				(number "51")
			)
			(pin input line
				(at -12.7 -27.94 0)
				(length 2.54)
				(name "MSEL1")
				(number "50")
			)
			(pin passive line
				(at -12.7 -33.02 0)
				(length 2.54)
				(name "VGDC")
				(number "54")
			)
			(pin passive line
				(at -12.7 -35.56 0)
				(length 2.54)
				(name "CDC")
				(number "56")
			)
			(pin passive line
				(at -12.7 -38.1 0)
				(length 2.54)
				(name "CMSE")
				(number "18")
			)
			(pin passive line
				(at -12.7 -40.64 0)
				(length 2.54)
				(name "CREF")
				(number "20")
			)
			(pin power_in line
				(at -5.08 45.72 270)
				(length 2.54)
				(name "AVDD")
				(number "17")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "DVDD")
				(number "55")
			)
			(pin power_in line
				(at -2.54 -45.72 90)
				(length 2.54)
				(name "AVSS")
				(number "19")
			)
			(pin passive line
				(at -2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "AVSS")
				(number "25")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "PVDD")
				(number "7")
			)
			(pin passive line
				(at 0 45.72 270)
				(length 2.54)
				(hide yes)
				(name "PVDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "DVSS")
				(number "26")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "DVSS")
				(number "59")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "PVDD")
				(number "41")
			)
			(pin passive line
				(at 2.54 45.72 270)
				(length 2.54)
				(hide yes)
				(name "PVDD")
				(number "42")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 2.54)
				(name "PVSS")
				(number "1")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "PVSS")
				(number "13")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "PVSS")
				(number "14")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "PVSS")
				(number "2")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "PVSS")
				(number "35")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "PVSS")
				(number "36")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "PVSS")
				(number "47")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "PVSS")
				(number "48")
			)
			(pin passive line
				(at 12.7 40.64 180)
				(length 2.54)
				(name "CF0AP")
				(number "6")
			)
			(pin passive line
				(at 12.7 35.56 180)
				(length 2.54)
				(name "CF0AN")
				(number "3")
			)
			(pin output line
				(at 12.7 33.02 180)
				(length 2.54)
				(name "OUT0A")
				(number "4")
			)
			(pin passive line
				(at 12.7 33.02 180)
				(length 2.54)
				(hide yes)
				(name "OUT0A")
				(number "5")
			)
			(pin passive line
				(at 12.7 27.94 180)
				(length 2.54)
				(name "CF0BP")
				(number "9")
			)
			(pin passive line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "CF0BN")
				(number "12")
			)
			(pin output line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "OUT0B")
				(number "10")
			)
			(pin passive line
				(at 12.7 20.32 180)
				(length 2.54)
				(hide yes)
				(name "OUT0B")
				(number "11")
			)
			(pin passive line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "CF1AP")
				(number "43")
			)
			(pin passive line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "CF1AN")
				(number "46")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "OUT1A")
				(number "44")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 2.54)
				(hide yes)
				(name "OUT1A")
				(number "45")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CF1BP")
				(number "40")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CF1BN")
				(number "37")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "OUT1B")
				(number "38")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "OUT1B")
				(number "39")
			)
			(pin passive line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "CGD1P")
				(number "53")
			)
			(pin passive line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "CGD1N")
				(number "52")
			)
			(pin passive line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "CFDCP")
				(number "57")
			)
			(pin passive line
				(at 12.7 -25.4 180)
				(length 2.54)
				(name "CFDCN")
				(number "58")
			)
			(pin passive line
				(at 12.7 -27.94 180)
				(length 2.54)
				(name "CGD0P")
				(number "60")
			)
			(pin passive line
				(at 12.7 -33.02 180)
				(length 2.54)
				(name "CGD0N")
				(number "61")
			)
			(pin passive line
				(at 12.7 -35.56 180)
				(length 2.54)
				(name "CFGDP")
				(number "62")
			)
			(pin passive line
				(at 12.7 -40.64 180)
				(length 2.54)
				(name "CFGDN")
				(number "63")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX9701xTG"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 15.24 22.86 0)
		)
		(property "Value" "MAX9701xTG"
			(at 15.24 20.32 0)
		)
		(property "Footprint" "Package_DFN_QFN:TQFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX9701.pdf"
			(at 0 0 0)
		)
		(property "Description" "Stereo class D power amplifier, 1.3W, TQFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "stereo power amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MAX9701xTG_0_1")
		(symbol "MAX9701xTG_1_1"
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "INL+")
				(number "23")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "INL-")
				(number "24")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "INR+")
				(number "20")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "INR-")
				(number "19")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "GAIN1")
				(number "17")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "GAIN2")
				(number "18")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "1")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "SYNC")
				(number "2")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "21")
			)
			(pin passive line
				(at -2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at -2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "PVDD")
				(number "5")
			)
			(pin passive line
				(at 2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "13")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "PGND")
				(number "6")
			)
			(pin power_in line
				(at 5.08 17.78 270)
				(length 2.54)
				(name "PVDD")
				(number "14")
			)
			(pin no_connect line
				(at 12.7 10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at 12.7 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at 12.7 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin no_connect line
				(at 12.7 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin power_out line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "OUTL+")
				(number "4")
			)
			(pin power_out line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "OUTL-")
				(number "7")
			)
			(pin power_out line
				(at 15.24 0 180)
				(length 2.54)
				(name "OUTR+")
				(number "15")
			)
			(pin power_out line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "OUTR-")
				(number "12")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "SYNC_OUT")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX9715xTE+"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "MAX9715xTE+"
			(at 10.16 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:TQFN-16-1EP_5x5mm_P0.8mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX9715.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.8W, Low-EMI, Stereo, Filterless Class D Audio Amplifier, TQFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Class-D Stereo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFN*1EP*5x5mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "MAX9715xTE+_0_1")
		(symbol "MAX9715xTE+_1_1"
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "INL")
				(number "16")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "INR")
				(number "15")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "GAIN")
				(number "6")
			)
			(pin passive line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "BIAS")
				(number "13")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "8")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(name "PAD")
				(number "17")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "PVDD")
				(number "4")
			)
			(pin passive line
				(at 2.54 17.78 270)
				(length 2.54)
				(hide yes)
				(name "PVDD")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "PGND")
				(number "1")
			)
			(pin passive line
				(at 2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "12")
			)
			(pin no_connect line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "OUTL+")
				(number "2")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "OUTL-")
				(number "3")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "OUTR+")
				(number "11")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "OUTR-")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX9744"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 -22.86 0)
		)
		(property "Value" "MAX9744"
			(at -10.16 -25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:TQFN-44-1EP_7x7mm_P0.5mm_EP4.7x4.7mm_ThermalVias"
			(at 0 -36.83 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX9744.pdf"
			(at 0 34.29 0)
		)
		(property "Description" "Filterless Class-D / Class-AB Stereo Audio Amplifier with Volume Control, 20W, 4.5..14V input, -40..85°C, QFN-44"
			(at 0 -34.29 0)
		)
		(property "ki_keywords" "Maxim"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFN?44*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MAX9744_0_1")
		(symbol "MAX9744_1_1"
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "FBL")
				(number "17")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "INL")
				(number "16")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "INR")
				(number "19")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "FBR")
				(number "18")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "MUTE")
				(number "24")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "~{SHND}")
				(number "22")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "SDA/VOL")
				(number "8")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "SCLK")
				(number "9")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "ADDR1")
				(number "13")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "ADDR2")
				(number "14")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "SYNC")
				(number "25")
			)
			(pin no_connect line
				(at -12.7 -17.78 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "23")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "10")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "21")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "27")
			)
			(pin power_in line
				(at -2.54 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 2.54 22.86 270)
				(length 2.54)
				(hide yes)
				(name "PVDD")
				(number "29")
			)
			(pin passive line
				(at 2.54 22.86 270)
				(length 2.54)
				(hide yes)
				(name "PVDD")
				(number "30")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "PVDD")
				(number "4")
			)
			(pin passive line
				(at 2.54 22.86 270)
				(length 2.54)
				(hide yes)
				(name "PVDD")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -22.86 90)
				(length 2.54)
				(name "PGND")
				(number "34")
			)
			(pin passive line
				(at 2.54 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "35")
			)
			(pin passive line
				(at 2.54 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "39")
			)
			(pin passive line
				(at 2.54 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "43")
			)
			(pin passive line
				(at 2.54 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "44")
			)
			(pin output line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "BOOTL+")
				(number "1")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "OUTL+")
				(number "2")
			)
			(pin passive line
				(at 15.24 12.7 180)
				(length 2.54)
				(hide yes)
				(name "OUTL+")
				(number "3")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "OUTL-")
				(number "41")
			)
			(pin passive line
				(at 15.24 10.16 180)
				(length 2.54)
				(hide yes)
				(name "OUTL-")
				(number "42")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "BOOTL-")
				(number "40")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "BOOTR+")
				(number "33")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "OUTR+")
				(number "31")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 2.54)
				(hide yes)
				(name "OUTR+")
				(number "32")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "OUTR-")
				(number "36")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "OUTR-")
				(number "37")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "BOOTR-")
				(number "38")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "SYNCOUT")
				(number "26")
			)
			(pin output line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "BIAS")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX9814"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 13.97 0)
		)
		(property "Value" "MAX9814"
			(at 11.43 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-14-1EP_3x3mm_P0.4mm_EP1.78x2.35mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX9814.pdf"
			(at 0 0 0)
		)
		(property "Description" "Microphone Amplifier with AGC and Low-Noise Microphone Bias, TDFN-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio microphone amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DFN*EP*3x3mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "MAX9814_0_0"
			(text "LNA"
				(at -8.89 -2.54 0)
			)
			(text "LN ref"
				(at -7.62 3.81 0)
			)
			(text "VGA"
				(at 0 -2.54 0)
			)
			(text "AGC"
				(at 1.27 3.81 0)
			)
			(text "Gain"
				(at 8.89 -2.54 0)
			)
		)
		(symbol "MAX9814_0_1")
		(symbol "MAX9814_1_1"
			(pin input line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "CT")
				(number "1")
			)
			(pin input line
				(at -22.86 7.62 0)
				(length 2.54)
				(name "A/R")
				(number "9")
			)
			(pin input line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "TH")
				(number "14")
			)
			(pin output line
				(at -22.86 0 0)
				(length 2.54)
				(name "MICBIAS")
				(number "13")
			)
			(pin input line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "MICIN")
				(number "8")
			)
			(pin input line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "GAIN")
				(number "10")
			)
			(pin passive line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "BIAS")
				(number "12")
			)
			(pin passive line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "CG")
				(number "3")
			)
			(pin input line
				(at -5.08 15.24 270)
				(length 2.54)
				(name "~{SHDN}")
				(number "2")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "5")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin output line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "MICOUT")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX98306xDT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 10.16 14.605 0)
		)
		(property "Value" "MAX98306xDT"
			(at 10.16 12.065 0)
		)
		(property "Footprint" "Package_DFN_QFN:TDFN-14-1EP_3x3mm_P0.4mm_EP1.78x2.35mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX98306.pdf"
			(at 0 0 0)
		)
		(property "Description" "Stereo 3.7 W Class D Amplifier, TDFN-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Class-D stereo amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDFN*1EP*3x3mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "MAX98306xDT_0_1")
		(symbol "MAX98306xDT_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "INL+")
				(number "3")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "INL-")
				(number "4")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "INR+")
				(number "7")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "INR-")
				(number "6")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "GAIN")
				(number "5")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "2")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "PVDD")
				(number "11")
			)
			(pin passive line
				(at 0 12.7 270)
				(length 2.54)
				(hide yes)
				(name "PVDD")
				(number "12")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "PGND")
				(number "1")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "15")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "8")
			)
			(pin power_out line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "OUTL+")
				(number "13")
			)
			(pin power_out line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OUTL-")
				(number "14")
			)
			(pin power_out line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "OUTR+")
				(number "10")
			)
			(pin power_out line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "OUTR-")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX98396EWB+"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 15.24 22.86 0)
		)
		(property "Value" "MAX98396EWB+"
			(at 15.24 25.4 0)
		)
		(property "Footprint" "Package_CSP:Maxim_WLCSP-35_2.998x2.168mm_Layout7x5_P0.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX98396.pdf"
			(at -1.27 2.54 0)
		)
		(property "Description" "20V Digital Input Class-DG Amplifier with I/V Sense and Brownout Prevention, WLP-35"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital audio amp i2s tdm class-dg"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Maxim*WLCSP*2.998x2.168mm*Layout7x5*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "MAX98396EWB+_0_1")
		(symbol "MAX98396EWB+_1_1"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "~{RESET}")
				(number "A3")
			)
			(pin open_collector line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "IRQ")
				(number "A5")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "ICC")
				(number "A7")
			)
			(pin open_collector line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "LV_EN")
				(number "D6")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "DIN")
				(number "D7")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "LRCLK")
				(number "E6")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "BCLK")
				(number "E7")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "ADDR")
				(number "B6")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "I2C1")
				(number "B7")
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "I2C2")
				(number "A6")
			)
			(pin power_in line
				(at -5.08 25.4 270)
				(length 2.54)
				(name "DVDDIO")
				(number "B5")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "DVDD")
				(number "B4")
			)
			(pin power_in line
				(at -2.54 -25.4 90)
				(length 2.54)
				(name "DGND")
				(number "C5")
			)
			(pin passive line
				(at -2.54 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "DGND")
				(number "C6")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "AVDD")
				(number "A4")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "AGND")
				(number "C4")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "D5")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "E5")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VBAT")
				(number "D4")
			)
			(pin passive line
				(at 2.54 25.4 270)
				(length 2.54)
				(hide yes)
				(name "VBAT")
				(number "E4")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "PGND")
				(number "C1")
			)
			(pin passive line
				(at 2.54 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "C2")
			)
			(pin passive line
				(at 2.54 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "C3")
			)
			(pin power_in line
				(at 5.08 25.4 270)
				(length 2.54)
				(name "PVDD")
				(number "A1")
			)
			(pin passive line
				(at 5.08 25.4 270)
				(length 2.54)
				(hide yes)
				(name "PVDD")
				(number "A2")
			)
			(pin passive line
				(at 5.08 25.4 270)
				(length 2.54)
				(hide yes)
				(name "PVDD")
				(number "E1")
			)
			(pin passive line
				(at 5.08 25.4 270)
				(length 2.54)
				(hide yes)
				(name "PVDD")
				(number "E2")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "OUTP")
				(number "D1")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(hide yes)
				(name "OUTP")
				(number "D2")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "OUTPSNS")
				(number "D3")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OUTN")
				(number "B1")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(hide yes)
				(name "OUTN")
				(number "B2")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "OUTNSNS")
				(number "B3")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "DOUT")
				(number "C7")
			)
			(pin passive line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "VREFC")
				(number "E3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX9850xTI"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 19.05 25.4 0)
		)
		(property "Value" "MAX9850xTI"
			(at 16.51 27.94 0)
		)
		(property "Footprint" "Package_DFN_QFN:TQFN-28-1EP_5x5mm_P0.5mm_EP3.25x3.25mm_ThermalVias"
			(at 0 0 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX9850.pdf"
			(at 0 0 0)
		)
		(property "Description" "Stereo audio DAC with headphone amplifier, TQFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio ampflifier stereo i2s"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MAX9850xTI_0_1")
		(symbol "MAX9850xTI_1_1"
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "MCLK")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "BCLK")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "LRCLK")
				(number "1")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "SDIN")
				(number "3")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "INL")
				(number "10")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "INR")
				(number "9")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "SDA")
				(number "28")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "SCL")
				(number "27")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "ADD")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "GPIO")
				(number "8")
			)
			(pin power_in line
				(at -5.08 -25.4 90)
				(length 2.54)
				(name "DGND")
				(number "6")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "DVDD")
				(number "4")
			)
			(pin power_in line
				(at -2.54 -25.4 90)
				(length 2.54)
				(name "PGND")
				(number "24")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "PVDD")
				(number "26")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "AGND")
				(number "14")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "29")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "AVDD")
				(number "17")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "PVSS")
				(number "22")
			)
			(pin power_in line
				(at 5.08 -25.4 90)
				(length 2.54)
				(name "SVSS")
				(number "20")
			)
			(pin power_out line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "REF")
				(number "13")
			)
			(pin power_out line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PREG")
				(number "16")
			)
			(pin power_out line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "NREG")
				(number "15")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "OUTL")
				(number "12")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "OUTR")
				(number "11")
			)
			(pin passive line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "C1P")
				(number "25")
			)
			(pin passive line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "C1N")
				(number "23")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "HPL")
				(number "19")
			)
			(pin input line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "HPS")
				(number "21")
			)
			(pin output line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "HPR")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "OPA1622"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "OPA1622"
			(at 3.81 3.81 0)
		)
		(property "Footprint" "Package_SON:Texas_S-PVSON-N10"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa1622.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Fidelity, Bipolar-Input, Audio Operational Amplifier, VSON-10"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp audio"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*PVSON*"
			(at 0 0 0)
		)
		(symbol "OPA1622_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "10")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "EN")
				(number "8")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "9")
			)
		)
		(symbol "OPA1622_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "OPA1622_3_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "2")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "V-")
				(number "11")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 5.08)
				(name "GND")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PAM8301"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 8.89 0)
		)
		(property "Value" "PAM8301"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/products_inactive_data/PAM8301.pdf"
			(at 0 0 0)
		)
		(property "Description" "Filterless Class-D Mono Audio Amplifier, 1.5W, TSOT-26"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier class d"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "PAM8301_0_1")
		(symbol "PAM8301_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{SD}")
				(number "4")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT+")
				(number "6")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUT-")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PAM8302AAD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 11.43 0)
		)
		(property "Value" "PAM8302AAD"
			(at 7.62 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/PAM8302A.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.5W Filterless Class-D Mono Audio Amplifier, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier class d"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "PAM8302AAD_0_1")
		(symbol "PAM8302AAD_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IN+")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN-")
				(number "4")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{SD}")
				(number "1")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin no_connect line
				(at 7.62 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OUT+")
				(number "5")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT-")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PAM8302AAY"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 11.43 0)
		)
		(property "Value" "PAM8302AAY"
			(at 7.62 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.65mm_EP1.55x2.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/PAM8302A.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.5W Filterless Class-D Mono Audio Amplifier, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier class d"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PAM8302AAY_0_1")
		(symbol "PAM8302AAY_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IN+")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN-")
				(number "4")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{SD}")
				(number "1")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin no_connect line
				(at 7.62 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OUT+")
				(number "5")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT-")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PAM8403D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 16.51 0)
		)
		(property "Value" "PAM8403D"
			(at 6.096 14.224 0)
		)
		(property "Footprint" "Package_SO:SOP-16_3.9x9.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/products_inactive_data/PAM8403.pdf"
			(at -5.08 5.08 0)
		)
		(property "Description" "3W Filterless Class-D Stereo Audio Amplifier, SOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier class d"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "PAM8403D_0_1")
		(symbol "PAM8403D_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "INL")
				(number "7")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VREF")
				(number "8")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "INR")
				(number "10")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "12")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "~{MUTE}")
				(number "5")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 2.54)
				(hide yes)
				(name "PVDD")
				(number "13")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "PVDD")
				(number "4")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "15")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "PGND")
				(number "2")
			)
			(pin no_connect line
				(at 10.16 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "LOUT+")
				(number "1")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "LOUT-")
				(number "3")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "ROUT-")
				(number "14")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "ROUT+")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PAM8406D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 -15.24 0)
		)
		(property "Value" "PAM8406D"
			(at -10.16 -17.78 0)
		)
		(property "Footprint" "Package_SO:SOP-16_3.9x9.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/PAM8406.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Filterless Class-D / Class-AB Stereo Audio Amplifier, 5.0W, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier class d or class ab"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "PAM8406D_0_1")
		(symbol "PAM8406D_1_1"
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "INL")
				(number "7")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "INR")
				(number "10")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "~{SHND}")
				(number "12")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "~{MUTE}")
				(number "5")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "MODE")
				(number "9")
			)
			(pin passive line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "VREF")
				(number "8")
			)
			(pin power_in line
				(at -5.08 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at -5.08 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "PVDDL")
				(number "4")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "PGNDL")
				(number "2")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "PVDDR")
				(number "13")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "PGNDR")
				(number "15")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "+OUT_L")
				(number "1")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "-OUT_L")
				(number "3")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "-OUT_R")
				(number "14")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "+OUT_R")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SSM2017P"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 5.08 0)
		)
		(property "Value" "SSM2017P"
			(at 7.62 2.54 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/obsolete-data-sheets/139484016SSM2017.pdf"
			(at 0 0 0)
		)
		(property "Description" "Self-Contained Audio Preamplifier, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio preamplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "SSM2017P_0_1")
		(symbol "SSM2017P_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "RG1")
				(number "1")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "REF")
				(number "5")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 6.35)
				(name "RG2")
				(number "8")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SSM2018"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 11.43 0)
		)
		(property "Value" "SSM2018"
			(at 6.35 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/SSM2018.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Trimless Voltage Controlled Amplifier, DIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio VCA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "SSM2018_0_0"
			(text "+"
				(at -5.08 1.905 0)
			)
			(text "-"
				(at -5.08 0.635 0)
			)
			(text "+"
				(at 1.905 5.715 0)
			)
			(text "-"
				(at 1.905 4.445 0)
			)
			(text "+"
				(at 1.905 -1.905 0)
			)
			(text "-"
				(at 1.905 -3.175 0)
			)
		)
		(symbol "SSM2018_0_1"
			(text "GAIN CORE"
				(at -1.27 0 900)
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "COMP3")
				(number "9")
			)
		)
		(symbol "SSM2018_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "VC")
				(number "11")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "+IN")
				(number "6")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "-IN")
				(number "7")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "COMP1")
				(number "5")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "COMP2")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "2")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "10")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "MODE")
				(number "12")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "VG")
				(number "14")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "-IG")
				(number "3")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "BAL")
				(number "15")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "V1-G")
				(number "16")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "-I1-G")
				(number "4")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "+I1-G")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SSM2120"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.89 5.08 0)
		)
		(property "Value" "SSM2120"
			(at 10.16 2.54 0)
		)
		(property "Footprint" "Package_DIP:DIP-22_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/obsolete-data-sheets/105738070SSM2120.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dynamic Range Pprocessor/Dual VCA, DIP-22"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "audio VCA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "SSM2120_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "5")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "8")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "7")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "CFT")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(symbol "SSM2120_2_1"
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "THRESH")
				(number "1")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "LOGAV")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "RECIN")
				(number "9")
			)
			(pin input line
				(at 7.62 0 180)
				(length 2.54)
				(name "CONOUT")
				(number "3")
			)
		)
		(symbol "SSM2120_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "19")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "16")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "17")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "CFT")
				(number "18")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "20")
			)
		)
		(symbol "SSM2120_4_1"
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "THRESH")
				(number "12")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "LOGAV")
				(number "13")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "RECIN")
				(number "15")
			)
			(pin input line
				(at 7.62 0 180)
				(length 2.54)
				(name "CONOUT")
				(number "14")
			)
		)
		(symbol "SSM2120_5_0"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "21")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "11")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 5.08)
				(name "GND")
				(number "22")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 6.35)
				(name "IREF")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SSM2122"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 5.08 0)
		)
		(property "Value" "SSM2122"
			(at 7.62 2.54 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/obsolete-data-sheets/105738070SSM2120.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dynamic Range Pprocessor/Dual VCA, DIP-16"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "audio VCA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "SSM2122_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "6")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "5")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "CFT")
				(number "4")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(symbol "SSM2122_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "13")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "10")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "11")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "CFT")
				(number "12")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(symbol "SSM2122_3_0"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "15")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 5.08)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 6.35)
				(name "IREF")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SSM2165"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "SSM2165"
			(at 5.08 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/obsolete-data-sheets/SSM2165.PDF"
			(at 0 0 0)
		)
		(property "Description" "Microphone Preamplifier with Variable Compression and Noise Gating, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio microphone preamplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "SSM2165_0_1")
		(symbol "SSM2165_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IN+")
				(number "4")
			)
			(pin output line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "BUFOUT")
				(number "3")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "VCAIN")
				(number "2")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "7")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "AVG")
				(number "5")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "COMP")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SSM2167"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "SSM2167"
			(at 5.08 11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/SSM2167.pdf"
			(at -8.89 11.43 0)
		)
		(property "Description" "Low Voltage Microphone Preamplifier with Variable Compression and Noise Gating, MSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio microphone amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "SSM2167_0_1")
		(symbol "SSM2167_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "IN+")
				(number "5")
			)
			(pin output line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "BUFOUT")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "VCAIN")
				(number "2")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "~{SD}")
				(number "3")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "10")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VOUT")
				(number "9")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "AVG")
				(number "6")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "GATE")
				(number "7")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "COMP")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SSM2211CP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 12.7 0)
		)
		(property "Value" "SSM2211CP"
			(at 5.08 12.7 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-8-1EP_3x3mm_P0.5mm_EP1.45x1.74mm"
			(at 2.54 -22.86 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/SSM2211.pdf"
			(at -2.54 7.62 0)
		)
		(property "Description" "1.5W BTL or 250mW SE 4MHz-bandwidth high performance amplifier, LFCSP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "SSM2211CP_0_1")
		(symbol "SSM2211CP_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IN-")
				(number "4")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SHUTDOWN")
				(number "1")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "BYPASS")
				(number "2")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "IN+")
				(number "3")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "V+")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "V-")
				(number "7")
			)
			(pin passive line
				(at -2.54 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "V-")
				(number "9")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VoutA")
				(number "5")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "VoutB")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SSM2211S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 12.7 0)
		)
		(property "Value" "SSM2211S"
			(at 5.08 12.7 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/SSM2211.pdf"
			(at -2.54 7.62 0)
		)
		(property "Description" "1.5W BTL or 250mW SE 4MHz-bandwidth high performance amplifier, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "SSM2211S_0_1")
		(symbol "SSM2211S_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IN-")
				(number "4")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SHUTDOWN")
				(number "1")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "BYPASS")
				(number "2")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "IN+")
				(number "3")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "V+")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "V-")
				(number "7")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VoutA")
				(number "5")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "VoutB")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "STK433_Sanyo"
		(pin_names
			(offset 0.0254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 5.08 0)
		)
		(property "Value" "STK433_Sanyo"
			(at 3.81 2.54 0)
		)
		(property "Footprint" "Package_SIP:Sanyo_STK4xx-15_59.2x8.0mm_P2.54mm"
			(at 7.62 -8.89 0)
		)
		(property "Datasheet" "http://datasheet.octopart.com/STK430-Sanyo-datasheet-107060.pdf"
			(at 0 0 0)
		)
		(property "Description" "2-Channel 5 Wmin Audio Frequency Power Amplifier, 4010, SIP-15"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier 2ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Sanyo*59.2x8.0mm*P2.54mm*"
			(at 0 0 0)
		)
		(symbol "STK433_Sanyo_0_1")
		(symbol "STK433_Sanyo_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "9")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 5.08)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 5.08)
				(name "V-")
				(number "4")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 3.81)
				(name "~")
				(number "6")
			)
			(pin power_in line
				(at 2.54 -5.08 90)
				(length 3.81)
				(name "~")
				(number "8")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(symbol "STK433_Sanyo_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "15")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "14")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "13")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 5.08)
				(name "V-")
				(number "12")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 3.81)
				(name "~")
				(number "10")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "STK437_Sanyo"
		(pin_names
			(offset 0.0254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 5.08 0)
		)
		(property "Value" "STK437_Sanyo"
			(at 3.81 2.54 0)
		)
		(property "Footprint" "Package_SIP:Sanyo_STK4xx-15_78.0x8.0mm_P2.54mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://datasheet.octopart.com/STK430-Sanyo-datasheet-107060.pdf"
			(at 0 0 0)
		)
		(property "Description" "2-Channel 12 Wmin Audio Frequency Power Amplifier, 4010, SIP-15"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier 2ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Sanyo*78.0x8.0mm*P2.54mm*"
			(at 0 0 0)
		)
		(symbol "STK437_Sanyo_0_1")
		(symbol "STK437_Sanyo_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "9")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 5.08)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 5.08)
				(name "V-")
				(number "4")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 3.81)
				(name "~")
				(number "6")
			)
			(pin power_in line
				(at 2.54 -5.08 90)
				(length 3.81)
				(name "~")
				(number "8")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(symbol "STK437_Sanyo_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "15")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "14")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "13")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 5.08)
				(name "V-")
				(number "12")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 3.81)
				(name "~")
				(number "10")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Si8241BB"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 11.43 0)
		)
		(property "Value" "Si8241BB"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/Si824x.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Class D Audio Driver With Precision Dead-Time Generator, 8V UVLO, ±750V, ±0.5A, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "class d gate driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "Si8241BB_0_1")
		(symbol "Si8241BB_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "PWM")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "DISABLE")
				(number "5")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "DT")
				(number "6")
			)
			(pin no_connect line
				(at -7.62 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin no_connect line
				(at -7.62 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDDI")
				(number "3")
			)
			(pin passive line
				(at 0 12.7 270)
				(length 2.54)
				(hide yes)
				(name "VDDI")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GNDI")
				(number "4")
			)
			(pin power_in line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "VDDA")
				(number "16")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VOA")
				(number "15")
			)
			(pin power_in line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "GNDA")
				(number "14")
			)
			(pin power_in line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "VDDB")
				(number "11")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "VOB")
				(number "10")
			)
			(pin power_in line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "GNDB")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TAS5825MRHB"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 24.13 0)
		)
		(property "Value" "TAS5825MRHB"
			(at 13.97 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 -34.29 0)
		)
		(property "Datasheet" "www.ti.com/lit/ds/symlink/tas5825m.pdf"
			(at 0 0 0)
		)
		(property "Description" "38-W Stereo, Inductor-Less, Digital Input, Closed-Loop Class-D Audio Amplifier with 192-kHz Extended Audio Processing, VQFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Class-D Stereo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TAS5825MRHB_0_1")
		(symbol "TAS5825MRHB_1_1"
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "~{PDN}")
				(number "17")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "LRCLK")
				(number "12")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "SCLK")
				(number "13")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "SDIN")
				(number "14")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "SDA")
				(number "15")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "SCL")
				(number "16")
			)
			(pin passive line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "ADR")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "GPIO0")
				(number "9")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "GPIO1")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "GPIO2")
				(number "11")
			)
			(pin passive line
				(at -5.08 25.4 270)
				(length 2.54)
				(name "VR_DIG")
				(number "7")
			)
			(pin passive line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "AVDD")
				(number "19")
			)
			(pin power_in line
				(at -2.54 -25.4 90)
				(length 2.54)
				(name "AGND")
				(number "20")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "DVDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "DGND")
				(number "5")
			)
			(pin passive line
				(at 2.54 25.4 270)
				(length 2.54)
				(hide yes)
				(name "PVDD")
				(number "21")
			)
			(pin passive line
				(at 2.54 25.4 270)
				(length 2.54)
				(hide yes)
				(name "PVDD")
				(number "22")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "PVDD")
				(number "3")
			)
			(pin passive line
				(at 2.54 25.4 270)
				(length 2.54)
				(hide yes)
				(name "PVDD")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "PGND")
				(number "25")
			)
			(pin passive line
				(at 2.54 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "26")
			)
			(pin passive line
				(at 2.54 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "31")
			)
			(pin passive line
				(at 2.54 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "32")
			)
			(pin passive line
				(at 5.08 25.4 270)
				(length 2.54)
				(name "GVDD")
				(number "18")
			)
			(pin passive line
				(at 5.08 -25.4 90)
				(length 2.54)
				(name "EP")
				(number "33")
			)
			(pin passive line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "BST_A+")
				(number "1")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "OUT_A+")
				(number "2")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "OUT_A-")
				(number "30")
			)
			(pin passive line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "BST_A-")
				(number "29")
			)
			(pin passive line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "BST_B+")
				(number "24")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "OUT_B+")
				(number "23")
			)
			(pin output line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "OUT_B-")
				(number "27")
			)
			(pin passive line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "BST_B-")
				(number "28")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TDA1308"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 6.35 0)
		)
		(property "Value" "TDA1308"
			(at 5.08 3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/TDA1308.pdf"
			(at 0 0 0)
		)
		(property "Description" "Class-AB Stereo Headphone Driver, SOIC-8/TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* TSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TDA1308_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "TDA1308_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "TDA1308_3_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "VSS")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TDA2003"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "TDA2003"
			(at 3.81 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-5_P3.4x3.7mm_StaggerOdd_Lead3.8mm_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/cd00000123.pdf"
			(at 0 0 0)
		)
		(property "Description" "10W Car Radio Audio Amplifier, TO-220-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*220*StaggerOdd*"
			(at 0 0 0)
		)
		(symbol "TDA2003_0_1")
		(symbol "TDA2003_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TDA2005"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 6.35 0)
		)
		(property "Value" "TDA2005"
			(at 7.62 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-11_P3.4x5.08mm_StaggerOdd_Lead4.85mm_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/cd00000124.pdf"
			(at 0 0 0)
		)
		(property "Description" "20W Bridge/Stereo Amplifier for Car Radio, TO-220-11"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*StaggerOdd*"
			(at 0 0 0)
		)
		(symbol "TDA2005_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 5.08)
				(name "SVRR")
				(number "3")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 3.81)
				(name "BOOT")
				(number "11")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "10")
			)
		)
		(symbol "TDA2005_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 3.81)
				(name "BOOT")
				(number "7")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(symbol "TDA2005_3_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "9")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TDA2030"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "TDA2030"
			(at 3.81 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-5_P3.4x3.7mm_StaggerOdd_Lead3.8mm_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/cd00000128.pdf"
			(at 0 0 0)
		)
		(property "Description" "14W Hi-Fi Audio Amplifier, TO-220-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*220*StaggerOdd*"
			(at 0 0 0)
		)
		(symbol "TDA2030_0_1")
		(symbol "TDA2030_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "+Vs")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "-Vs")
				(number "3")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TDA7052A"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 7.62 0)
		)
		(property "Value" "TDA7052A"
			(at 5.08 5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/TDA7052A_AT.pdf"
			(at 0 0 0)
		)
		(property "Description" "1W BTL mono audio amplifier with DC volume control, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "TDA7052A_0_1")
		(symbol "TDA7052A_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "V")
				(number "4")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "VP")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "3")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 5.08)
				(name "GND")
				(number "6")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 5.08)
				(name "~")
				(number "5")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 5.08)
				(name "~")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TDA7264"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "TDA7264"
			(at 5.08 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-8_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/tda7264.pdf"
			(at 0 0 0)
		)
		(property "Description" "25W + 25W stereo amplifier with mute and standby, TO-220-8"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier 2ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
		(symbol "TDA7264_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "8")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "MUTE")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "TDA7264_2_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(symbol "TDA7264_3_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TDA7265"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "TDA7265"
			(at 5.08 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-11_P3.4x5.08mm_StaggerOdd_Lead4.85mm_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/tda7265.pdf"
			(at 0 0 0)
		)
		(property "Description" "25W +25W Stereo Amplifier with Mute & St-by, TO-220-11"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier 2ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*StaggerOdd*"
			(at 0 0 0)
		)
		(symbol "TDA7265_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "11")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "10")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "MUTE")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 5.08)
				(name "GND")
				(number "9")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(symbol "TDA7265_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "7")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "8")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(symbol "TDA7265_3_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "1")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "V-")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TDA7266"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 5.08 0)
		)
		(property "Value" "TDA7266"
			(at 5.08 -5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-15_P2.54x2.54mm_StaggerOdd_Lead4.58mm_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/tda7266.pdf"
			(at 0 0 0)
		)
		(property "Description" "7+7W Dual Bridge Amplifier, TO-220-15"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier 2ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*StaggerOdd*"
			(at 0 0 0)
		)
		(symbol "TDA7266_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "+")
				(number "4")
			)
			(pin no_connect line
				(at -5.08 5.08 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin no_connect line
				(at -5.08 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at -2.54 3.81 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "MUTE")
				(number "6")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 6.35)
				(name "STBY")
				(number "7")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 3.81)
				(name "~")
				(number "2")
			)
		)
		(symbol "TDA7266_2_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "+")
				(number "12")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 3.81)
				(name "~")
				(number "15")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 3.81)
				(name "~")
				(number "14")
			)
		)
		(symbol "TDA7266_3_1"
			(pin passive line
				(at -2.54 7.62 270)
				(length 3.81)
				(hide yes)
				(name "V+")
				(number "13")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "SG")
				(number "9")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 5.08)
				(name "PG")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TDA7266D"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 5.08 0)
		)
		(property "Value" "TDA7266D"
			(at 5.08 -5.08 0)
		)
		(property "Footprint" "Package_SO:HSOP-20-1EP_11.0x15.9mm_P1.27mm_SlugDown"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/tda7266d.pdf"
			(at 0 0 0)
		)
		(property "Description" "5W+5W Dual Bridge Amplifier, PowerSO-20"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier 2ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HSOP*EP*11.0x15.9mm*P1.27mm*SlugDown*"
			(at 0 0 0)
		)
		(symbol "TDA7266D_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "+")
				(number "7")
			)
			(pin no_connect line
				(at -5.08 5.08 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at -5.08 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin no_connect line
				(at -2.54 3.81 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "MUTE")
				(number "8")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at 0 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "18")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 6.35)
				(name "STBY")
				(number "9")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 3.81)
				(name "~")
				(number "5")
			)
		)
		(symbol "TDA7266D_2_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "+")
				(number "14")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 3.81)
				(name "~")
				(number "19")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 3.81)
				(name "~")
				(number "16")
			)
		)
		(symbol "TDA7266D_3_1"
			(pin passive line
				(at -2.54 7.62 270)
				(length 3.81)
				(hide yes)
				(name "V+")
				(number "15")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "SG")
				(number "13")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 5.08)
				(name "PG")
				(number "1")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 5.08)
				(hide yes)
				(name "PG")
				(number "10")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 5.08)
				(hide yes)
				(name "PG")
				(number "11")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 5.08)
				(hide yes)
				(name "PG")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TDA7266M"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 5.08 0)
		)
		(property "Value" "TDA7266M"
			(at 5.08 -5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-15_P2.54x2.54mm_StaggerOdd_Lead4.58mm_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/tda7266m.pdf"
			(at 0 0 0)
		)
		(property "Description" "7W Mono Bridge Amplifier, TO-220-15"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*StaggerOdd*"
			(at 0 0 0)
		)
		(symbol "TDA7266M_0_1")
		(symbol "TDA7266M_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "+")
				(number "4")
			)
			(pin no_connect line
				(at -5.08 5.08 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at -5.08 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 3.81)
				(hide yes)
				(name "V+")
				(number "13")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "SG")
				(number "9")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "MUTE")
				(number "6")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at 0 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 5.08)
				(name "PG")
				(number "8")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 6.35)
				(name "STBY")
				(number "7")
			)
			(pin no_connect line
				(at 2.54 1.27 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin no_connect line
				(at 2.54 -1.27 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 3.81)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TDA7266P"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 5.08 0)
		)
		(property "Value" "TDA7266P"
			(at 5.08 -5.08 0)
		)
		(property "Footprint" "Package_SO:ST_PowerSSO-24_SlugDown"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/tda7266p.pdf"
			(at 0 0 0)
		)
		(property "Description" "3W+3W Dual Bridge Amplifier, PowerSSO-24"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier 2ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*PowerSSO*SlugDown*"
			(at 0 0 0)
		)
		(symbol "TDA7266P_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "+")
				(number "8")
			)
			(pin no_connect line
				(at -5.08 5.08 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at -5.08 -1.27 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin no_connect line
				(at -5.08 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin no_connect line
				(at -2.54 3.81 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin no_connect line
				(at -2.54 -3.81 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "21")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "MUTE")
				(number "10")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at 0 0 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at 0 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "22")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 6.35)
				(name "STBY")
				(number "11")
			)
			(pin no_connect line
				(at 2.54 1.27 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at 2.54 -1.27 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "23")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "TDA7266P_2_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "+")
				(number "17")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 3.81)
				(name "~")
				(number "20")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 3.81)
				(name "~")
				(number "19")
			)
		)
		(symbol "TDA7266P_3_1"
			(pin passive line
				(at -2.54 7.62 270)
				(length 3.81)
				(hide yes)
				(name "V+")
				(number "18")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "SG")
				(number "14")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 5.08)
				(name "PG")
				(number "1")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 5.08)
				(hide yes)
				(name "PG")
				(number "24")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TDA7293"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 10.16 6.35 0)
		)
		(property "Value" "TDA7293"
			(at 10.16 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-15_P2.54x2.54mm_StaggerOdd_Lead4.58mm_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/tda7293.pdf"
			(at 0 0 0)
		)
		(property "Description" "120-volt, 100-watt, DMOS Audio Amplifier with Mute and Standby, TO-220-15"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*StaggerOdd*"
			(at 0 0 0)
		)
		(symbol "TDA7293_0_1")
		(symbol "TDA7293_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin power_in line
				(at -5.08 10.16 270)
				(length 3.81)
				(name "+Vs")
				(number "7")
			)
			(pin power_in line
				(at -5.08 -10.16 90)
				(length 3.81)
				(name "-Vs")
				(number "8")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 5.08)
				(name "+Vs")
				(number "13")
			)
			(pin no_connect line
				(at -2.54 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 5.08)
				(name "-Vs")
				(number "15")
			)
			(pin input line
				(at 0 7.62 270)
				(length 3.81)
				(name "MUTE")
				(number "10")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 3.81)
				(name "SIG_GND")
				(number "4")
			)
			(pin input line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "STBY")
				(number "9")
			)
			(pin no_connect line
				(at 2.54 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin power_in line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "SGND")
				(number "1")
			)
			(pin passive line
				(at 5.08 5.08 270)
				(length 3.81)
				(name "BOOT")
				(number "6")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TDA7496"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 3.81 0)
		)
		(property "Value" "TDA7496"
			(at 7.62 -3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-15_P2.54x2.54mm_StaggerOdd_Lead4.58mm_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/tda7297.pdf"
			(at 0 0 0)
		)
		(property "Description" "5W+5W Amplifier with DC Volume Control, TO-220-15"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier 2ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*StaggerOdd*"
			(at 0 0 0)
		)
		(symbol "TDA7496_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "V")
				(number "3")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "+")
				(number "5")
			)
			(pin output line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "O")
				(number "4")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "MUTE")
				(number "10")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 6.35)
				(name "STBY")
				(number "9")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "12")
			)
		)
		(symbol "TDA7496_2_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "+")
				(number "1")
			)
			(pin output line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "O")
				(number "2")
			)
			(pin passive line
				(at 2.54 -7.62 90)
				(length 6.35)
				(name "SVR")
				(number "7")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(symbol "TDA7496_3_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "13")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "SG")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 5.08)
				(name "PG")
				(number "11")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 5.08)
				(hide yes)
				(name "PG")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TFA9879HN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 27.94 0)
		)
		(property "Value" "TFA9879HN"
			(at -12.7 25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:HVQFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm_ThermalVias"
			(at 7.62 -38.1 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/TFA9879.pdf"
			(at -12.7 27.94 0)
		)
		(property "Description" "Mono BTL class-D audio amplifier for portable applications with digital input, HVQFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Audio Amplifier Class D NXP Semiconductors"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HVQFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TFA9879HN_0_1")
		(symbol "TFA9879HN_1_1"
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "LRCK1")
				(number "22")
			)
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "SCK1")
				(number "21")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "SDI1")
				(number "20")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "LRCK2")
				(number "19")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "SCK2")
				(number "18")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SDI2")
				(number "17")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "SCL")
				(number "2")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SDA")
				(number "1")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "ADSEL1")
				(number "16")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "ADSEL2")
				(number "4")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "TEST1")
				(number "3")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "TEST2")
				(number "15")
			)
			(pin input line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "TEST3")
				(number "5")
			)
			(pin passive line
				(at -2.54 -25.4 90)
				(length 2.54)
				(name "EP")
				(number "25")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "23")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GNDD")
				(number "24")
			)
			(pin passive line
				(at 2.54 25.4 270)
				(length 2.54)
				(hide yes)
				(name "VDDP")
				(number "7")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VDDP")
				(number "8")
			)
			(pin passive line
				(at 2.54 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GNDP")
				(number "11")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "GNDP")
				(number "12")
			)
			(pin no_connect line
				(at 10.16 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin no_connect line
				(at 10.16 -12.7 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "OUTA")
				(number "10")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OUTB")
				(number "9")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "STABA")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "THAT151xx08"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" "THAT151xx08"
			(at 0 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.thatcorp.com/datashts/THAT_1510-1512_Datasheet.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "Low-Noise, High Performance Audio Preamplifier IC"
			(at 0 0 0)
		)
		(property "ki_keywords" "Audio Preamplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "THAT151xx08_0_1")
		(symbol "THAT151xx08_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 5.08)
				(name "+In")
				(number "3")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 5.08)
				(name "Rg1")
				(number "1")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 5.08)
				(name "Rg2")
				(number "8")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 5.08)
				(name "-In")
				(number "2")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "V-")
				(number "4")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 5.08)
				(name "Out")
				(number "6")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 5.08)
				(name "Ref")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "THAT2180"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 6.35 0)
		)
		(property "Value" "THAT2180"
			(at 7.62 3.81 0)
		)
		(property "Footprint" "Package_SIP:SIP-8_19x3mm_P2.54mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.thatcorp.com/datashts/THAT_2180-Series_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "Blackmer Pre-Trimmed IC Voltage Controlled Amplifiers, SIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio vca"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SIP*19x3mm*P2.54mm*"
			(at 0 0 0)
		)
		(symbol "THAT2180_0_0"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 5.08)
				(name "GND")
				(number "6")
			)
		)
		(symbol "THAT2180_0_1")
		(symbol "THAT2180_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "-")
				(number "1")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "SYM")
				(number "4")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 6.35)
				(name "E+")
				(number "2")
			)
			(pin input line
				(at 2.54 -7.62 90)
				(length 6.35)
				(name "E-")
				(number "3")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "THAT2181"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 6.35 0)
		)
		(property "Value" "THAT2181"
			(at 7.62 3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.thatcorp.com/datashts/THAT_2181-Series_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "Blackmer Trimmable IC Voltage Controlled Amplifiers, SIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio vca"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SIP*19x3mm*P2.54mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "THAT2181_0_0"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 5.08)
				(name "GND")
				(number "6")
			)
		)
		(symbol "THAT2181_0_1")
		(symbol "THAT2181_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "-")
				(number "1")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "SYM")
				(number "4")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 6.35)
				(name "E+")
				(number "2")
			)
			(pin input line
				(at 2.54 -7.62 90)
				(length 6.35)
				(name "E-")
				(number "3")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPA3251"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 19.05 0)
		)
		(property "Value" "TPA3251"
			(at 3.81 19.05 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-44_6.1x14mm_P0.635mm_TopEP4.14x7.01mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tpa3251.pdf"
			(at 0 0 0)
		)
		(property "Description" "175-W Stereo, 350-W Mono PurePath Ultra-HD Analog-Input Class-D Amplifier, HTSSOP-44"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "stereo class d amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*6.1x14mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "TPA3251_0_1")
		(symbol "TPA3251_1_1"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "INPUT_A")
				(number "5")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "INPUT_B")
				(number "6")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "OSC_IOM")
				(number "9")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "OSC_IOP")
				(number "10")
			)
			(pin passive line
				(at -12.7 0 0)
				(length 2.54)
				(name "OC_ADJ")
				(number "7")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "FREQ_ADJ")
				(number "8")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "DVDD")
				(number "11")
			)
			(pin passive line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "AVDD")
				(number "14")
			)
			(pin passive line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "C_START")
				(number "15")
			)
			(pin passive line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "VBG")
				(number "20")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "GVDD_AB")
				(number "1")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "26")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "34")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "41")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "42")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "PVDD_AB")
				(number "36")
			)
			(pin passive line
				(at 2.54 20.32 270)
				(length 2.54)
				(hide yes)
				(name "PVDD_AB")
				(number "37")
			)
			(pin passive line
				(at 2.54 20.32 270)
				(length 2.54)
				(hide yes)
				(name "PVDD_AB")
				(number "38")
			)
			(pin passive line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "BST_A")
				(number "44")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "OUT_A")
				(number "39")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 2.54)
				(hide yes)
				(name "OUT_A")
				(number "40")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "OUT_B")
				(number "35")
			)
			(pin passive line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "BST_B")
				(number "43")
			)
		)
		(symbol "TPA3251_2_1"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "INPUT_C")
				(number "16")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "INPUT_D")
				(number "17")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "M1")
				(number "3")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "M2")
				(number "4")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "~{RESET}")
				(number "18")
			)
			(pin open_collector line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "~{FAULT}")
				(number "19")
			)
			(pin open_collector line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "~{CLIP_OTW}")
				(number "21")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "GVDD_CD")
				(number "22")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "PVDD_CD")
				(number "29")
			)
			(pin passive line
				(at 2.54 20.32 270)
				(length 2.54)
				(hide yes)
				(name "PVDD_CD")
				(number "30")
			)
			(pin passive line
				(at 2.54 20.32 270)
				(length 2.54)
				(hide yes)
				(name "PVDD_CD")
				(number "31")
			)
			(pin passive line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "BST_C")
				(number "24")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "OUT_C")
				(number "32")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "OUT_D")
				(number "27")
			)
			(pin passive line
				(at 12.7 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "OUT_D")
				(number "28")
			)
			(pin passive line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "BST_D")
				(number "23")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPA6110A2DGN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "TPA6110A2DGN"
			(at 6.35 11.43 0)
		)
		(property "Footprint" "Package_SO:HVSSOP-8-1EP_3x3mm_P0.65mm_EP1.57x1.89mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tpa6110a2.pdf"
			(at 0 0 0)
		)
		(property "Description" "150-mW Stereo Audio Power Amplifier, HVSSOP"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier headphone"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HVSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TPA6110A2DGN_0_1")
		(symbol "TPA6110A2DGN_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IN1-")
				(number "8")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN2-")
				(number "4")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SHDN")
				(number "3")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VO1")
				(number "7")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "VO2")
				(number "5")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "BYPASS")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPA6132A2RTE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "TPA6132A2RTE"
			(at 8.89 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:WQFN-16-1EP_3x3mm_P0.5mm_EP1.6x1.6mm_ThermalVias"
			(at 2.54 -13.97 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tpa6132a2.pdf"
			(at -7.62 13.97 0)
		)
		(property "Description" "25mW, Stereo, DirectPath Audio Amplifier, WQFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "DirectPath audio amplifier Stereo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WQFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TPA6132A2RTE_0_1")
		(symbol "TPA6132A2RTE_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "INR+")
				(number "3")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "INR-")
				(number "4")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "INL+")
				(number "2")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "INL-")
				(number "1")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "G0")
				(number "6")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "G1")
				(number "7")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "EN")
				(number "13")
			)
			(pin power_in line
				(at -5.08 -15.24 90)
				(length 2.54)
				(name "SGND")
				(number "15")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "PGND")
				(number "10")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "HPVDD")
				(number "12")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "HPVSS")
				(number "8")
			)
			(pin passive line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "EP")
				(number "17")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "OUTR")
				(number "5")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OUTL")
				(number "16")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "CPP")
				(number "11")
			)
			(pin passive line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "CPN")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPA6203A1DGN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "TPA6203A1DGN"
			(at 8.89 -11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-8-1EP_3x3mm_P0.65mm_EP1.95x2.15mm_ThermalVias"
			(at 0 -25.4 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tpa6203a1.pdf"
			(at 0 23.368 0)
		)
		(property "Description" "1.25W, Mono, Differential Audio Amplifier, MSOP-8"
			(at 0 25.4 0)
		)
		(property "ki_keywords" "Differential audio amplifier Mono"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TPA6203A1DGN_0_1")
		(symbol "TPA6203A1DGN_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "IN-")
				(number "4")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IN+")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHUTDOWN}")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "BYPASS")
				(number "2")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V_{DD}")
				(number "6")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "V_{O+}")
				(number "5")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "V_{O-}")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IR4311"
		(extends "IR4301")
		(property "Reference" "U"
			(at -7.62 20.955 0)
		)
		(property "Value" "IR4311"
			(at -7.62 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:Infineon_PQFN-22-15-4EP_6x5mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir4301.pdf?fileId=5546d462533600a4015355d5fc691819"
			(at 0 0 0)
		)
		(property "Description" "PowIRaudio Integrated Analog Input Class D Audio Amplifier, 90W/4ohm, 60V, PQFN-22"
			(at 0 0 0)
		)
		(property "ki_keywords" "integrated class d amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*PQFN*4EP*6x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "IR4312"
		(extends "IR4302")
		(property "Reference" "U"
			(at -7.62 20.955 0)
		)
		(property "Value" "IR4312"
			(at -7.62 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:Infineon_PQFN-44-31-5EP_7x7mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir4302.pdf?fileId=5546d462533600a4015355d602a9181d"
			(at 0 0 0)
		)
		(property "Description" "PowIRaudio 2 Channel Integrated Analog Input Class D Audio Amplifier, 100W/4ohm, 60V, PQFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "integrated class d amplifier 2ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*PQFN*5EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "IR4321"
		(extends "IR4301")
		(property "Reference" "U"
			(at -7.62 20.955 0)
		)
		(property "Value" "IR4321"
			(at -7.62 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:Infineon_PQFN-22-15-4EP_6x5mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir4301.pdf?fileId=5546d462533600a4015355d5fc691819"
			(at 0 0 0)
		)
		(property "Description" "PowIRaudio Integrated Analog Input Class D Audio Amplifier, 35W/4ohm, 40V, PQFN-22"
			(at 0 0 0)
		)
		(property "ki_keywords" "integrated class d amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*PQFN*4EP*6x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "IR4322"
		(extends "IR4302")
		(property "Reference" "U"
			(at -7.62 20.955 0)
		)
		(property "Value" "IR4322"
			(at -7.62 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:Infineon_PQFN-44-31-5EP_7x7mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir4302.pdf?fileId=5546d462533600a4015355d602a9181d"
			(at 0 0 0)
		)
		(property "Description" "PowIRaudio 2 Channel Integrated Analog Input Class D Audio Amplifier, 35W/4ohm, 40V, PQFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "integrated class d amplifier 2ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*PQFN*5EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MA12070"
		(extends "MA12040")
		(property "Reference" "U"
			(at -10.16 44.45 0)
		)
		(property "Value" "MA12070"
			(at 3.81 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.45x5.45mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-MA12070-DS-v01_00-EN.pdf?fileId=5546d46264a8de7e0164b750002861a5"
			(at 0 0 0)
		)
		(property "Description" "Filterless and High-Efficiency +4V to +26V Audio Amplifier with Analog Input, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "integrated class d amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MA12070P"
		(extends "MA12040P")
		(property "Reference" "U"
			(at -10.16 44.45 0)
		)
		(property "Value" "MA12070P"
			(at 3.81 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.45x5.45mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-MA12070P-DS-v01_00-EN.pdf?fileId=5546d46264a8de7e0164b761f2f261e4"
			(at 0 0 0)
		)
		(property "Description" "Filterless and High-Efficiency +4V to +26V Audio Amplifier with I2S Digital Input, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "integrated class d amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PAM8302AAS"
		(extends "PAM8302AAD")
		(property "Reference" "U"
			(at 7.62 11.43 0)
		)
		(property "Value" "PAM8302AAS"
			(at 7.62 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/PAM8302A.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.5W Filterless Class-D Mono Audio Amplifier, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier class d"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "STK435_Sanyo"
		(extends "STK433_Sanyo")
		(property "Reference" "U"
			(at 3.81 5.08 0)
		)
		(property "Value" "STK435_Sanyo"
			(at 3.81 2.54 0)
		)
		(property "Footprint" "Package_SIP:Sanyo_STK4xx-15_59.2x8.0mm_P2.54mm"
			(at 7.62 -8.89 0)
		)
		(property "Datasheet" "http://datasheet.octopart.com/STK430-Sanyo-datasheet-107060.pdf"
			(at 0 0 0)
		)
		(property "Description" "2-Channel 7 Wmin Audio Frequency Power Amplifier, 4010, SIP-15"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier 2ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Sanyo*59.2x8.0mm*P2.54mm*"
			(at 0 0 0)
		)
	)
	(symbol "STK436_Sanyo"
		(extends "STK433_Sanyo")
		(property "Reference" "U"
			(at 3.81 5.08 0)
		)
		(property "Value" "STK436_Sanyo"
			(at 3.81 2.54 0)
		)
		(property "Footprint" "Package_SIP:Sanyo_STK4xx-15_59.2x8.0mm_P2.54mm"
			(at 7.62 -8.89 0)
		)
		(property "Datasheet" "http://datasheet.octopart.com/STK430-Sanyo-datasheet-107060.pdf"
			(at 0 0 0)
		)
		(property "Description" "2-Channel 10 Wmin Audio Frequency Power Amplifier, 4010, SIP-15"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier 2ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Sanyo*59.2x8.0mm*P2.54mm*"
			(at 0 0 0)
		)
	)
	(symbol "STK439_Sanyo"
		(extends "STK437_Sanyo")
		(property "Reference" "U"
			(at 3.81 5.08 0)
		)
		(property "Value" "STK439_Sanyo"
			(at 3.81 2.54 0)
		)
		(property "Footprint" "Package_SIP:Sanyo_STK4xx-15_78.0x8.0mm_P2.54mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://datasheet.octopart.com/STK430-Sanyo-datasheet-107060.pdf"
			(at 0 0 0)
		)
		(property "Description" "2-Channel 16 Wmin Audio Frequency Power Amplifier, 4010, SIP-15"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier 2ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Sanyo*78.0x8.0mm*P2.54mm*"
			(at 0 0 0)
		)
	)
	(symbol "STK441_Sanyo"
		(extends "STK437_Sanyo")
		(property "Reference" "U"
			(at 3.81 5.08 0)
		)
		(property "Value" "STK441_Sanyo"
			(at 3.81 2.54 0)
		)
		(property "Footprint" "Package_SIP:Sanyo_STK4xx-15_78.0x8.0mm_P2.54mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://datasheet.octopart.com/STK430-Sanyo-datasheet-107060.pdf"
			(at 0 0 0)
		)
		(property "Description" "2-Channel 24 Wmin Audio Frequency Power Amplifier, 4010, SIP-15"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier 2ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Sanyo*78.0x8.0mm*P2.54mm*"
			(at 0 0 0)
		)
	)
	(symbol "STK443_Sanyo"
		(extends "STK437_Sanyo")
		(property "Reference" "U"
			(at 3.81 5.08 0)
		)
		(property "Value" "STK443_Sanyo"
			(at 3.81 2.54 0)
		)
		(property "Footprint" "Package_SIP:Sanyo_STK4xx-15_78.0x8.0mm_P2.54mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://datasheet.octopart.com/STK430-Sanyo-datasheet-107060.pdf"
			(at 0 0 0)
		)
		(property "Description" "2-Channel 28 Wmin Audio Frequency Power Amplifier, 4010, SIP-15"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier 2ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Sanyo*78.0x8.0mm*P2.54mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8241CB"
		(extends "Si8241BB")
		(property "Reference" "U"
			(at -5.08 11.43 0)
		)
		(property "Value" "Si8241CB"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCD5702-D.PDF"
			(at 0 2.54 0)
		)
		(property "Description" "Class D Audio Driver With Precision Dead-Time Generator, 10V UVLO, ±750V, ±0.5A, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "class d gate driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8244BB"
		(extends "Si8241BB")
		(property "Reference" "U"
			(at -5.08 11.43 0)
		)
		(property "Value" "Si8244BB"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCD5702-D.PDF"
			(at 0 2.54 0)
		)
		(property "Description" "Class D Audio Driver With Precision Dead-Time Generator, 8V UVLO, ±750V, ±4A, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "class d gate driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8244CB"
		(extends "Si8241BB")
		(property "Reference" "U"
			(at -5.08 11.43 0)
		)
		(property "Value" "Si8244CB"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCD5702-D.PDF"
			(at 0 2.54 0)
		)
		(property "Description" "Class D Audio Driver With Precision Dead-Time Generator, 10V UVLO, ±750V, ±4A, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "class d gate driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TDA2050"
		(extends "TDA2030")
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "TDA2050"
			(at 3.81 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-5_P3.4x3.7mm_StaggerOdd_Lead3.8mm_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/cd00000131.pdf"
			(at 0 0 0)
		)
		(property "Description" "32W Hi-Fi Audio Amplifier, TO-220-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*220*StaggerOdd*"
			(at 0 0 0)
		)
	)
	(symbol "TDA7265B"
		(extends "TDA7265")
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "TDA7265B"
			(at 5.08 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-11_P3.4x5.08mm_StaggerOdd_Lead4.85mm_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/tda7265b.pdf"
			(at 0 0 0)
		)
		(property "Description" "30W + 30W Stereo Amplifier with Mute and Standby, TO-220-11"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier 2ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*StaggerOdd*"
			(at 0 0 0)
		)
	)
	(symbol "TDA7269A"
		(extends "TDA7265")
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "TDA7269A"
			(at 5.08 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-11_P3.4x5.08mm_StaggerOdd_Lead4.85mm_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/tda7269a.pdf"
			(at 0 0 0)
		)
		(property "Description" "14W+14W Stereo Amplifier with Mute & St-by, TO-220-11"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplfier 2ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*StaggerOdd*"
			(at 0 0 0)
		)
	)
	(symbol "TDA7292"
		(extends "TDA7265")
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "TDA7292"
			(at 5.08 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-11_P3.4x5.08mm_StaggerOdd_Lead4.85mm_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/tda7292.pdf"
			(at 0 0 0)
		)
		(property "Description" "40W + 40W stereo amplifier with mute and standby, TO-220-11"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier 2ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*StaggerOdd*"
			(at 0 0 0)
		)
	)
	(symbol "TDA7294"
		(extends "TDA7293")
		(property "Reference" "U"
			(at 10.16 6.35 0)
		)
		(property "Value" "TDA7294"
			(at 10.16 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-15_P2.54x2.54mm_StaggerOdd_Lead4.58mm_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/tda7294.pdf"
			(at 0 0 0)
		)
		(property "Description" "100V - 100W DMOS Audio Amplifier with Mute/St-by, TO-220-15"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*StaggerOdd*"
			(at 0 0 0)
		)
	)
	(symbol "TDA7295"
		(extends "TDA7293")
		(property "Reference" "U"
			(at 10.16 6.35 0)
		)
		(property "Value" "TDA7295"
			(at 10.16 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-15_P2.54x2.54mm_StaggerOdd_Lead4.58mm_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/tda7295.pdf"
			(at 0 0 0)
		)
		(property "Description" "80V - 80W DMOS Audio Amplifier with Mute/St-by, TO-220-15"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*StaggerOdd*"
			(at 0 0 0)
		)
	)
	(symbol "TDA7296"
		(extends "TDA7293")
		(property "Reference" "U"
			(at 10.16 6.35 0)
		)
		(property "Value" "TDA7296"
			(at 10.16 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-15_P2.54x2.54mm_StaggerOdd_Lead4.58mm_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/tda7296.pdf"
			(at 0 0 0)
		)
		(property "Description" "70V - 60W DMOS Audio Amplifier with Mute/St-by, TO-220-15"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*StaggerOdd*"
			(at 0 0 0)
		)
	)
	(symbol "TDA7297"
		(extends "TDA7266")
		(property "Reference" "U"
			(at 5.08 5.08 0)
		)
		(property "Value" "TDA7297"
			(at 5.08 -5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-15_P2.54x2.54mm_StaggerOdd_Lead4.58mm_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/tda7297.pdf"
			(at 0 0 0)
		)
		(property "Description" "15+15W Dual Bridge Amplifier, TO-220-15"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio amplifier 2ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*StaggerOdd*"
			(at 0 0 0)
		)
	)
	(symbol "TPA6203A1DRB"
		(extends "TPA6203A1DGN")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "TPA6203A1DRB"
			(at 8.89 -11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_DRB0008A"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tpa6203a1.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.25W, Mono, Differential Audio Amplifier, VSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Differential audio amplifier Mono"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DRB*"
			(at 0 0 0)
		)
	)
)
