(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "BUF602xD"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 2.54 0)
		)
		(property "Value" "BUF602xD"
			(at 7.62 -2.54 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/buf602.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed, 1000 MHz, Closed-Loop Buffer, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "buffer amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "BUF602xD_0_1")
		(symbol "BUF602xD_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "4")
			)
			(pin no_connect line
				(at -5.08 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at -5.08 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "5")
			)
			(pin output line
				(at 0 -7.62 90)
				(length 5.08)
				(name "VREF")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BUF602xDBV"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 2.54 0)
		)
		(property "Value" "BUF602xDBV"
			(at 7.62 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/buf602.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed, 1000 MHz, Closed-Loop Buffer, SOT23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "buffer amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "BUF602xDBV_0_1")
		(symbol "BUF602xDBV_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "4")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "2")
			)
			(pin output line
				(at 0 -7.62 90)
				(length 5.08)
				(name "VREF")
				(number "3")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BUF634AxDDA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 2.54 0)
		)
		(property "Value" "BUF634AxDDA"
			(at 10.414 -2.54 0)
		)
		(property "Footprint" "Package_SO:TI_SO-PowerPAD-8_ThermalVias"
			(at 3.81 -5.08 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/buf634.pdf"
			(at 3.81 -7.62 0)
		)
		(property "Description" "250mA High-Speed Buffer, PowerPAD SOIC-8"
			(at 3.81 -10.16 0)
		)
		(property "ki_keywords" "buffer amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TI*SO*PowerPAD*"
			(at 0 0 0)
		)
		(symbol "BUF634AxDDA_0_1")
		(symbol "BUF634AxDDA_1_0"
			(pin power_in line
				(at 0 -7.62 90)
				(length 5.08)
				(name "THPAD")
				(number "9")
			)
		)
		(symbol "BUF634AxDDA_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "V_{IN}")
				(number "3")
			)
			(pin no_connect line
				(at -5.08 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at -5.08 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin input line
				(at 2.54 -7.62 90)
				(length 6.35)
				(name "BW")
				(number "1")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BUF634U"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 2.54 0)
		)
		(property "Value" "BUF634U"
			(at 7.62 -2.54 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -5.08 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/buf634.pdf"
			(at 1.27 -7.62 0)
		)
		(property "Description" "250mA High-Speed Buffer, SOIC-8"
			(at 1.27 -10.16 0)
		)
		(property "ki_keywords" "buffer amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "BUF634U_0_1")
		(symbol "BUF634U_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "V_{IN}")
				(number "3")
			)
			(pin no_connect line
				(at -5.08 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at -5.08 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "BW")
				(number "1")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EL2001CN"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 5.08 0)
		)
		(property "Value" "EL2001CN"
			(at 7.62 2.54 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://www.datasheetlib.com/datasheet/677973/el2001_intersil.html#datasheet"
			(at 0 0 0)
		)
		(property "Description" "Monolithic high slew rate, buffer amplifier, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Monolithic high slew rate, buffer amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "EL2001CN_0_1")
		(symbol "EL2001CN_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at -5.08 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at -5.08 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at -5.08 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LH0002H"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 2.54 0)
		)
		(property "Value" "LH0002H"
			(at 7.62 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-5-8"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.calogic.net/pdf/LH0002_Datasheet_Rev_A.pdf"
			(at 0 0 0)
		)
		(property "Description" "Wide-Band, High Current, Unity Gain Buffer Amplifier, TO-5-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Buffer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?5*"
			(at 0 0 0)
		)
		(symbol "LH0002H_0_1")
		(symbol "LH0002H_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "8")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V1+")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V1-")
				(number "7")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 5.08)
				(name "V2+")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 5.08)
				(name "V2-")
				(number "6")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 6.35)
				(name "E3")
				(number "3")
			)
			(pin passive line
				(at 2.54 -7.62 90)
				(length 6.35)
				(name "E4")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM6321H"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 3.81 0)
		)
		(property "Value" "LM6321H"
			(at 5.08 -3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-5-8"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.electronica60norte.com/mwfls/pdf/LM6221.pdf"
			(at 0 0 0)
		)
		(property "Description" "High Speed Buffer, TO-5-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single buffer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?5*"
			(at 0 0 0)
		)
		(symbol "LM6321H_0_1")
		(symbol "LM6321H_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "8")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "2")
			)
			(pin no_connect line
				(at -2.54 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -2.54 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "6")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at 0 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM6321M"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 3.81 0)
		)
		(property "Value" "LM6321M"
			(at 5.08 -3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.electronica60norte.com/mwfls/pdf/LM6221.pdf"
			(at 0 0 0)
		)
		(property "Description" "High Speed Buffer, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "single buffer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LM6321M_0_1")
		(symbol "LM6321M_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "5")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "11")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "V-")
				(number "1")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "V-")
				(number "13")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "V-")
				(number "14")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "V-")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "3")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "V-")
				(number "6")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "V-")
				(number "7")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "V-")
				(number "8")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "V-")
				(number "9")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at 0 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM6321N"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 3.81 0)
		)
		(property "Value" "LM6321N"
			(at 5.08 -3.81 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 5.08 -10.16 0)
		)
		(property "Datasheet" "http://www.electronica60norte.com/mwfls/pdf/LM6221.pdf"
			(at 0 0 0)
		)
		(property "Description" "High Speed Buffer, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single buffer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "LM6321N_0_1")
		(symbol "LM6321N_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "8")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "2")
			)
			(pin no_connect line
				(at -2.54 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at -2.54 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "6")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at 0 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BUF634AxD"
		(extends "BUF634U")
		(property "Reference" "U"
			(at 6.35 2.54 0)
		)
		(property "Value" "BUF634AxD"
			(at 7.62 -2.54 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -5.08 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/buf634a.pdf"
			(at 1.27 -7.62 0)
		)
		(property "Description" "36-V, 210-MHz, 250-mA Output, High-Speed Buffer, SOIC-8"
			(at 1.27 -10.16 0)
		)
		(property "ki_keywords" "buffer amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "BUF634AxDRB"
		(extends "BUF634AxDDA")
		(property "Reference" "U"
			(at 6.35 2.54 0)
		)
		(property "Value" "BUF634AxDRB"
			(at 10.414 -2.54 0)
		)
		(property "Footprint" "Package_SON:Texas_S-PVSON-N8_ThermalVias"
			(at 3.81 -5.08 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/buf634a.pdf"
			(at 3.81 -7.62 0)
		)
		(property "Description" "250mA High-Speed Buffer, VSON-8"
			(at 3.81 -10.16 0)
		)
		(property "ki_keywords" "buffer amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*S*PVSON*"
			(at 0 0 0)
		)
	)
)
