(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "AD8202"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 10.795 0)
		)
		(property "Value" "AD8202"
			(at -7.62 8.89 0)
		)
		(property "Footprint" ""
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8202.pdf"
			(at 16.51 -17.78 0)
		)
		(property "Description" "28V High Common-Mode Voltage, Single-Supply Difference Amplifier, 10V/V x 2V/V adjustable gain, bandwidth 50kHz, Vcc=3.5V~12V, unidirectional, SOIC-8/MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "highside HS current sense amplifier linear buffered monitor preamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*P1.27mm* MSOP*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AD8202_0_1")
		(symbol "AD8202_1_1"
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "A1")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A2")
				(number "4")
			)
			(pin power_in line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "+Vs")
				(number "6")
			)
			(pin input line
				(at -5.08 10.16 270)
				(length 2.54)
				(name "+IN")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin no_connect line
				(at 2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin input line
				(at 5.08 10.16 270)
				(length 2.54)
				(name "-IN")
				(number "1")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD8203"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 10.795 0)
		)
		(property "Value" "AD8203"
			(at -7.62 8.89 0)
		)
		(property "Footprint" ""
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8203.pdf"
			(at 16.51 -17.78 0)
		)
		(property "Description" "30V High Common-Mode Voltage, Single-Supply Difference Amplifier, 7V/V x 2V/V adjustable gain, bandwidth 60kHz, Vcc=3.5V~12V, unidirectional, SOIC-8/MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "highside HS current sense amplifier linear buffered monitor preamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*P1.27mm* MSOP*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AD8203_0_1")
		(symbol "AD8203_1_1"
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "A1")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A2")
				(number "4")
			)
			(pin power_in line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "+Vs")
				(number "7")
			)
			(pin input line
				(at -5.08 10.16 270)
				(length 2.54)
				(name "+IN")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin no_connect line
				(at 2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin input line
				(at 5.08 10.16 270)
				(length 2.54)
				(name "-IN")
				(number "1")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD8210"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 10.795 0)
		)
		(property "Value" "AD8210"
			(at -7.62 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8210.pdf"
			(at 16.51 -17.78 0)
		)
		(property "Description" "65V High Voltage, Bidirectional Current Shunt Monitor, 20V/V gain, bandwidth 450kHz, Vcc=5V, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "highside HS current sense amplifier linear buffered"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "AD8210_0_1")
		(symbol "AD8210_1_1"
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "Vref1")
				(number "7")
			)
			(pin power_in line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "V+")
				(number "6")
			)
			(pin input line
				(at -5.08 10.16 270)
				(length 2.54)
				(name "+IN")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin no_connect line
				(at 2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin input line
				(at 5.08 10.16 270)
				(length 2.54)
				(name "-IN")
				(number "1")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "Vref2")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD8211"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 10.795 0)
		)
		(property "Value" "AD8211"
			(at -7.62 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8211.pdf"
			(at 16.51 -17.78 0)
		)
		(property "Description" "65V High Voltage, Current Shunt Monitor, 20V/V gain, bandwidth 500kHz, Vcc=5V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "highside HS current sense amplifier linear buffered"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "AD8211_0_1")
		(symbol "AD8211_1_1"
			(pin power_in line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "V+")
				(number "5")
			)
			(pin input line
				(at -5.08 10.16 270)
				(length 2.54)
				(name "Vin+")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at 5.08 10.16 270)
				(length 2.54)
				(name "Vin-")
				(number "4")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD8212"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 10.795 0)
		)
		(property "Value" "AD8212"
			(at -7.62 8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8212.pdf"
			(at 16.51 -17.78 0)
		)
		(property "Description" "65V High Voltage Current, Shunt Monitor, adjustable gain, bandwidth 1000kHz, Vcc=7V~65V, current output, unidirectional, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "highside HS current sense shunt monitor amplifier linear"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AD8212_0_1")
		(symbol "AD8212_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "BIAS")
				(number "3")
			)
			(pin output line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "ALPHA")
				(number "6")
			)
			(pin power_in line
				(at -5.08 10.16 270)
				(length 2.54)
				(name "V+")
				(number "1")
			)
			(pin no_connect line
				(at -2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin input line
				(at 5.08 10.16 270)
				(length 2.54)
				(name "Vsns")
				(number "8")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "Iout")
				(number "5")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "COM")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD8213"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 10.795 0)
		)
		(property "Value" "AD8213"
			(at -7.62 8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8213.pdf"
			(at 0 0 0)
		)
		(property "Description" "65V Dual, High Voltage, Current Shunt Monitor, 20V/V gain, bandwidth 500kHz, Vcc=5V, MSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "highside HS current sense amplifier linear buffered dual monitor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AD8213_0_1")
		(symbol "AD8213_1_1"
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "CF")
				(number "6")
			)
			(pin power_in line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "V+")
				(number "8")
			)
			(pin input line
				(at -5.08 10.16 270)
				(length 2.54)
				(name "+IN")
				(number "9")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin input line
				(at 5.08 10.16 270)
				(length 2.54)
				(name "-IN")
				(number "10")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "7")
			)
		)
		(symbol "AD8213_2_1"
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "CF")
				(number "5")
			)
			(pin input line
				(at -5.08 10.16 270)
				(length 2.54)
				(name "+IN")
				(number "2")
			)
			(pin input line
				(at 5.08 10.16 270)
				(length 2.54)
				(name "-IN")
				(number "1")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD8215"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 10.795 0)
		)
		(property "Value" "AD8215"
			(at -7.62 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8215.pdf"
			(at 16.51 -17.78 0)
		)
		(property "Description" "65V High Voltage, Current Shunt Monitor, 20V/V gain, bandwidth 450kHz, Vcc=5V, unidirectional, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "highside HS current sense amplifier linear buffered monitor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "AD8215_0_1")
		(symbol "AD8215_1_1"
			(pin power_in line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "V+")
				(number "6")
			)
			(pin input line
				(at -5.08 10.16 270)
				(length 2.54)
				(name "+IN")
				(number "8")
			)
			(pin no_connect line
				(at -2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin no_connect line
				(at 2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin input line
				(at 5.08 10.16 270)
				(length 2.54)
				(name "-IN")
				(number "1")
			)
			(pin no_connect line
				(at 5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD8217"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 10.795 0)
		)
		(property "Value" "AD8217"
			(at -7.62 8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8217.pdf"
			(at 16.51 -17.78 0)
		)
		(property "Description" "80V High Resolution, Zero-Drift, Current Shunt Monitor, 20V/V gain, bandwidth 500kHz, internal LDO, unidirectional, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "highside HS current sense amplifier linear buffered monitor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AD8217_0_1")
		(symbol "AD8217_1_1"
			(pin power_in line
				(at -5.08 10.16 270)
				(length 2.54)
				(name "+IN")
				(number "1")
			)
			(pin no_connect line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin no_connect line
				(at 2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin input line
				(at 5.08 10.16 270)
				(length 2.54)
				(name "-IN")
				(number "8")
			)
			(pin no_connect line
				(at 5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD8218xCP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 10.795 0)
		)
		(property "Value" "AD8218xCP"
			(at -7.62 8.89 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-8-1EP_3x2mm_P0.5mm_EP1.6x1.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8218.pdf"
			(at 16.51 -17.78 0)
		)
		(property "Description" "80V Zero Drift, Bidirectional, Current Shunt Monitor, 20V/V gain, bandwidth 450kHz, Vcc=5V, LFCSP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "highside HS current sense amplifier linear buffered"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AD8218xCP_0_1")
		(symbol "AD8218xCP_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "ENB")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "REF")
				(number "7")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "Vs")
				(number "2")
			)
			(pin input line
				(at -5.08 10.16 270)
				(length 2.54)
				(name "+IN")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin no_connect line
				(at 2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin input line
				(at 5.08 10.16 270)
				(length 2.54)
				(name "-IN")
				(number "8")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD8218xRM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 10.795 0)
		)
		(property "Value" "AD8218xRM"
			(at -7.62 8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8218.pdf"
			(at 16.51 -17.78 0)
		)
		(property "Description" "80V Zero Drift, Bidirectional, Current Shunt Monitor, 20V/V gain, bandwidth 450kHz, Vcc=5V, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "highside HS current sense amplifier linear buffered"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AD8218xRM_0_1")
		(symbol "AD8218xRM_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "ENB")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "REF")
				(number "7")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "Vs")
				(number "2")
			)
			(pin input line
				(at -5.08 10.16 270)
				(length 2.54)
				(name "+IN")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin no_connect line
				(at 2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin input line
				(at 5.08 10.16 270)
				(length 2.54)
				(name "-IN")
				(number "8")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD8219"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 10.795 0)
		)
		(property "Value" "AD8219"
			(at -7.62 8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8219.pdf"
			(at 16.51 -17.78 0)
		)
		(property "Description" "80V Zero Drift, Unidirectional, Current Shunt Monitor, 60V/V gain, bandwidth 500kHz, Vcc=4V~80V, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "highside HS current sense amplifier linear buffered monitor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AD8219_0_1")
		(symbol "AD8219_1_1"
			(pin power_in line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "Vs")
				(number "2")
			)
			(pin input line
				(at -5.08 10.16 270)
				(length 2.54)
				(name "+IN")
				(number "1")
			)
			(pin no_connect line
				(at -2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin no_connect line
				(at 2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin input line
				(at 5.08 10.16 270)
				(length 2.54)
				(name "-IN")
				(number "8")
			)
			(pin no_connect line
				(at 5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD8417"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 10.795 0)
		)
		(property "Value" "AD8417"
			(at -7.62 8.89 0)
		)
		(property "Footprint" ""
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8417.pdf"
			(at 16.51 -17.78 0)
		)
		(property "Description" "70V Bidirectional, Zero Drift, Current Sense Amplifier, 60V/V gain, bandwidth 250kHz, VS=2.7V~5.5V, SOIC-8/MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "highside HS current sense amplifier linear"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AD8417_0_1")
		(symbol "AD8417_1_1"
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "REF1")
				(number "7")
			)
			(pin power_in line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "VS")
				(number "6")
			)
			(pin input line
				(at -5.08 10.16 270)
				(length 2.54)
				(name "IN+")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin no_connect line
				(at 2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin input line
				(at 5.08 10.16 270)
				(length 2.54)
				(name "IN-")
				(number "1")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "REF2")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BQ500100DCK"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "BQ500100DCK"
			(at 3.81 -3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/bq500100.pdf"
			(at 0 0 0)
		)
		(property "Description" "20V High side current sensor, Voltage Output, 50V/V Gain, SC-70-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Current shunt monitor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
		(symbol "BQ500100DCK_0_1")
		(symbol "BQ500100DCK_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "5")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "3")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "INA138"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 5.08 0)
		)
		(property "Value" "INA138"
			(at 3.81 2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina138.pdf"
			(at 0 0.127 0)
		)
		(property "Description" "High-Side Measurement Current Shunt Monitor, 36V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "current sense shunt monitor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "INA138_0_1")
		(symbol "INA138_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "INA180A1"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA180A1"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina180.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Current Sense Amplifier, 1 Circuit, Rail-to-Rail, 26V, Gain 20 V/V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "INA180A1_0_1")
		(symbol "INA180A1_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "INA180B1"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA180B1"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina180.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Current Sense Amplifier, 1 Circuit, Rail-to-Rail, 26V, Gain 20 V/V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "INA180B1_0_1")
		(symbol "INA180B1_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "3")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "INA181"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA181"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina181.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Bidirectional, Low- and High-Side Voltage Output, Current-Sense Amplifier, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor bidirectional"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "INA181_0_1")
		(symbol "INA181_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at 2.54 -7.62 90)
				(length 6.35)
				(name "REF")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "INA193"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA193"
			(at 3.81 -3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina193.pdf"
			(at 0 0 0)
		)
		(property "Description" "Current Shunt Monitor −16V to +80V Common-Mode Range, 20V/V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "current sense shunt monitor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "INA193_0_1")
		(symbol "INA193_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "INA196"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA196"
			(at 3.81 -3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina193.pdf"
			(at 0 0 0)
		)
		(property "Description" "Current Shunt Monitor −16V to +80V Common-Mode Range, 20V/V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "current sense shunt monitor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "INA196_0_1")
		(symbol "INA196_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "5")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "INA199xxDCK"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA199xxDCK"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina199.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "INA199 26-V, Bidirectional, Zero-Drift, Low- or High-Side, Voltage-Output, Current-Shunt Monitor, SOT-363, SC-70"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor bidirectional"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
		(symbol "INA199xxDCK_0_1")
		(symbol "INA199xxDCK_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "5")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at 2.54 -7.62 90)
				(length 6.35)
				(name "REF")
				(number "1")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "INA200D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 17.78 0)
		)
		(property "Value" "INA200D"
			(at 8.89 17.78 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 5.08 -24.13 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina201.pdf"
			(at 5.08 -21.59 0)
		)
		(property "Description" "Current Shunt Monitor, integrated comparator and reference, -16V to +80V Common-Mode Range, 20V/V, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current-sense amplifier fixed-gain high-side low-side"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "INA200D_0_0"
			(text "Ref"
				(at -8.89 -8.636 0)
			)
			(text "+"
				(at -2.794 -2.54 0)
			)
			(text "-"
				(at -2.794 -7.62 0)
			)
			(text "G"
				(at 0.762 5.08 0)
			)
			(text "+"
				(at 2.54 7.62 0)
			)
			(text "-"
				(at 2.54 2.54 0)
			)
		)
		(symbol "INA200D_0_1")
		(symbol "INA200D_1_0"
			(text "0.6V"
				(at -8.89 -6.604 0)
			)
		)
		(symbol "INA200D_1_1"
			(pin output line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "OUT")
				(number "2")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "CMP_{IN}")
				(number "3")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "~{RESET}")
				(number "5")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "V_{s}")
				(number "1")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "V_{IN+}")
				(number "8")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "V_{IN-}")
				(number "7")
			)
			(pin open_collector line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "CMP_{OUT}")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "INA225"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 7.62 0)
		)
		(property "Value" "INA225"
			(at 5.08 7.62 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina225-q1.pdf"
			(at -2.54 -5.08 0)
		)
		(property "Description" "36-V, Bidirectional Current Sense Amplifier, With Four Pin-Selectable Gain Settings, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage-output current-sense amplifier shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "INA225_0_0"
			(text ""
				(at -10.16 -5.08 0)
			)
		)
		(symbol "INA225_0_1")
		(symbol "INA225_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN+")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "GS0")
				(number "5")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "GS1")
				(number "6")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V_{S}")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "IN-")
				(number "8")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "REF")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "INA240A1D"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA240A1D"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina240.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "High- and Low-Side, Bidirectional, Zero-Drift, Current-Sense Amplifier With Enhanced PWM Rejection, 20V/V, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor bidirectional high low"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "INA240A1D_0_1")
		(symbol "INA240A1D_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "8")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "1")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 5.08)
				(name "REF2")
				(number "3")
			)
			(pin passive line
				(at 2.54 -7.62 90)
				(length 6.35)
				(name "REF1")
				(number "7")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "INA240A1PW"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA240A1PW"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_SO:TSSOP-8_4.4x3mm_P0.65mm"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina240.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "High- and Low-Side, Bidirectional, Zero-Drift, Current-Sense Amplifier With Enhanced PWM Rejection, 20V/V, TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor bidirectional high low"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "INA240A1PW_0_1")
		(symbol "INA240A1PW_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "3")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "5")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 5.08)
				(name "REF2")
				(number "6")
			)
			(pin passive line
				(at 2.54 -7.62 90)
				(length 6.35)
				(name "REF1")
				(number "7")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "INA253"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 13.97 0)
		)
		(property "Value" "INA253"
			(at 6.35 13.97 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina253.pdf"
			(at 0 -25.4 0)
		)
		(property "Description" "High Voltage, Bidirectional, Zero-Drift, Current-ShuntMonitor With Integrated, 2-mΩ, Precision, Low Inductive Shunt Resistor, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "shunt current amplifier bidirectional"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "INA253_0_1")
		(symbol "INA253_1_1"
			(pin passive line
				(at -10.16 10.16 0)
				(length 2.54)
				(hide yes)
				(name "IS+")
				(number "18")
			)
			(pin passive line
				(at -10.16 10.16 0)
				(length 2.54)
				(hide yes)
				(name "IS+")
				(number "19")
			)
			(pin passive line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "IS+")
				(number "20")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SH+")
				(number "17")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN+")
				(number "16")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IN-")
				(number "5")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SH-")
				(number "4")
			)
			(pin passive line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "IS-")
				(number "1")
			)
			(pin passive line
				(at -10.16 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "IS-")
				(number "2")
			)
			(pin passive line
				(at -10.16 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "IS-")
				(number "3")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VS")
				(number "9")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin no_connect line
				(at 7.62 10.16 180)
				(length 2.54)
				(hide yes)
				(name "DNC2")
				(number "14")
			)
			(pin no_connect line
				(at 7.62 7.62 180)
				(length 2.54)
				(hide yes)
				(name "DNC1")
				(number "7")
			)
			(pin no_connect line
				(at 7.62 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OUT")
				(number "13")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "REF2")
				(number "10")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "REF1")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "INA282"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA282"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina282.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Accuracy, Wide Common-Mode Range, Bidirectional Current Shunt Monitors, Zero-Drift Series, 50V/V, SOIC-8/VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor bidirectional"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "INA282_0_1")
		(symbol "INA282_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "8")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "1")
			)
			(pin no_connect line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin input line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "REF2")
				(number "3")
			)
			(pin input line
				(at 2.54 -7.62 90)
				(length 6.35)
				(name "REF1")
				(number "7")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "INA293A1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.382 6.858 0)
		)
		(property "Value" "INA293A1"
			(at 5.08 6.858 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina293.pdf"
			(at 0 0 0)
		)
		(property "Description" "-4-V to 110-V, 1.3-MHz bandwidth, Current Sense Amplifier, 20V/V gain, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "highside high lowside low HS LS linear buffered texas shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "INA293A1_0_1")
		(symbol "INA293A1_1_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "IN+")
				(number "3")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "IN-")
				(number "4")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vs")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "INA293B1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.382 6.858 0)
		)
		(property "Value" "INA293B1"
			(at 5.08 6.858 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina293.pdf"
			(at 0 0 0)
		)
		(property "Description" "-4-V to 110-V, 1.3-MHz bandwidth, Current Sense Amplifier, 20V/V gain, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "highside high lowside low HS LS linear buffered texas shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "INA293B1_0_1")
		(symbol "INA293B1_1_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "IN+")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "IN-")
				(number "5")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vs")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "INA4180A1"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 5.08 0)
		)
		(property "Value" "INA4180A1"
			(at 2.54 -5.08 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at 1.27 2.54 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina4180.pdf"
			(at 3.81 5.08 0)
		)
		(property "Description" "Quad current sense amplifier, Rail-to-Rail, 26V, Gain 20 V/V, TSSOP-14"
			(at 2.54 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor texas"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "INA4180A1_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "INA4180A1_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "INA4180A1_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "10")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "9")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(symbol "INA4180A1_4_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "12")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "13")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(symbol "INA4180A1_5_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 3.81)
				(name "VS")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LMP8640"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 5.08 0)
		)
		(property "Value" "LMP8640"
			(at 3.81 2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 3.81 -2.54 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmp8640.pdf"
			(at 0 0.127 0)
		)
		(property "Description" "Precision High Voltage Current Sense Amplifiers, 42V/76V, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "LMP8640_0_1")
		(symbol "LMP8640_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT6106"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 5.08 0)
		)
		(property "Value" "LT6106"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/6106fb.pdf"
			(at 1.27 5.08 0)
		)
		(property "Description" "36V Low Cost, High Side Current Sense, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "current sense"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "LT6106_0_1")
		(symbol "LT6106_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "3")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "2")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC6102xDD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "LTC6102xDD"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.5mm_EP1.66x2.38mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/6102fe.pdf"
			(at 0 0 0)
		)
		(property "Description" "Precision Zero Drift Current Sense Amplifier, 60V, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current sense amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC6102xDD_0_1")
		(symbol "LTC6102xDD_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "-INS")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "-INF")
				(number "2")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "+IN")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "V-")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "V-")
				(number "5")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "V-")
				(number "9")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "VREG")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC6102xDD-1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "LTC6102xDD-1"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.5mm_EP1.66x2.38mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/6102fe.pdf"
			(at 0 0 0)
		)
		(property "Description" "Precision Zero Drift Current Sense Amplifier, 60V, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current sense amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC6102xDD-1_0_1")
		(symbol "LTC6102xDD-1_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "-INS")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "-INF")
				(number "2")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "+IN")
				(number "8")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "V-")
				(number "5")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "V-")
				(number "9")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "VREG")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC6102xMS8"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "LTC6102xMS8"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/6102fe.pdf"
			(at 0 0 0)
		)
		(property "Description" "Precision Zero Drift Current Sense Amplifier, 60V, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current sense amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LTC6102xMS8_0_1")
		(symbol "LTC6102xMS8_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "-INS")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "-INF")
				(number "2")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "+IN")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "V-")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "V-")
				(number "5")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "VREG")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC6102xMS8-1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "LTC6102xMS8-1"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/6102fe.pdf"
			(at 0 0 0)
		)
		(property "Description" "Precision Zero Drift Current Sense Amplifier, 60V, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current sense amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LTC6102xMS8-1_0_1")
		(symbol "LTC6102xMS8-1_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "-INS")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "-INF")
				(number "2")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "+IN")
				(number "8")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "V-")
				(number "5")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "VREG")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX4080F"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MAX4080F"
			(at 2.54 6.35 0)
		)
		(property "Footprint" ""
			(at 16.51 -17.78 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX4080-MAX4081.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "76V, High-Side, Current-Sense Amplifiers with Voltage Output, Unidirectional, 5V/V Gain, SOIC-8/uMAX-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current sense amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MAX4080F_0_1")
		(symbol "MAX4080F_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "RS+")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "RS-")
				(number "8")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vcc")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin no_connect line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at 5.08 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 7.62 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX4081F"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MAX4081F"
			(at 2.54 8.89 0)
		)
		(property "Footprint" ""
			(at 16.51 -17.78 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX4080-MAX4081.pdf"
			(at 16.51 -17.78 0)
		)
		(property "Description" "76V, High-Side, Current-Sense Amplifiers with Voltage Output, Bidirectional, 5V/V Gain, SOIC-8/uMAX-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current sense amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MAX4081F_0_1")
		(symbol "MAX4081F_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "RS+")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "RS-")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "Vcc")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin no_connect line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "REF1A")
				(number "7")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "REF1B")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX471"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MAX471"
			(at 0 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://pdfserv.maximintegrated.com/en/ds/MAX471-MAX472.pdf"
			(at 0 0 0)
		)
		(property "Description" "Precision, High-Side, Current-Sense Amplifiers, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current sense amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MAX471_0_1")
		(symbol "MAX471_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "RS+")
				(number "2")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "RS+")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SHDN")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "RS-")
				(number "6")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "RS-")
				(number "7")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SIGN")
				(number "5")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "OUT")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX472"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 11.43 0)
		)
		(property "Value" "MAX472"
			(at 3.81 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://pdfserv.maximintegrated.com/en/ds/MAX471-MAX472.pdf"
			(at 0 0 0)
		)
		(property "Description" "Precision, High-Side, Current-Sense Amplifiers, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current sense amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MAX472_0_1")
		(symbol "MAX472_1_1"
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SHDN")
				(number "1")
			)
			(pin input line
				(at -5.08 10.16 270)
				(length 2.54)
				(name "SENSE+")
				(number "3")
			)
			(pin input line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "SENSE-")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "7")
			)
			(pin no_connect line
				(at 7.62 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SIGN")
				(number "5")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "OUT")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NCS210"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "NCS210"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCS210R-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Current-Shunt Monitor, Voltage Output, Bi-Directional Zero-Drift, 200V/V Gain, SC-70-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Current shunt monitor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
		(symbol "NCS210_0_1")
		(symbol "NCS210_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "+IN")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "-IN")
				(number "5")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "Vs")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "OUT")
				(number "6")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "REF")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ZXCT1009F"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 1.27 0)
		)
		(property "Value" "ZXCT1009F"
			(at 7.62 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/ZXCT1009.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "High-Side Current Monitor, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "High side current monitor shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "ZXCT1009F_0_1")
		(symbol "ZXCT1009F_1_1"
			(pin input line
				(at -5.08 5.08 270)
				(length 2.54)
				(name "Vs+")
				(number "2")
			)
			(pin output line
				(at 0 -5.08 90)
				(length 2.54)
				(name "Iout")
				(number "3")
			)
			(pin input line
				(at 5.08 5.08 270)
				(length 2.54)
				(name "Vs-")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ZXCT1009T8"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 1.27 0)
		)
		(property "Value" "ZXCT1009T8"
			(at 7.62 -1.27 0)
		)
		(property "Footprint" "Package_SO:Zetex_SM8"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/ZXCT1009.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "High-Side Current Monitor, SM8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High side current monitor shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Zetex*SM8*"
			(at 0 0 0)
		)
		(symbol "ZXCT1009T8_0_1")
		(symbol "ZXCT1009T8_1_1"
			(pin input line
				(at -5.08 5.08 270)
				(length 2.54)
				(name "Vs+")
				(number "3")
			)
			(pin no_connect line
				(at -2.54 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -2.54 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin output line
				(at 0 -5.08 90)
				(length 2.54)
				(name "Iout")
				(number "4")
			)
			(pin no_connect line
				(at 2.54 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 2.54 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin input line
				(at 5.08 5.08 270)
				(length 2.54)
				(name "Vs-")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ZXCT1010"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 1.27 0)
		)
		(property "Value" "ZXCT1010"
			(at 7.62 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/ZXCT1010.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Enhanced High-Side Current Monitors, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "High side current monitor shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "ZXCT1010_0_1")
		(symbol "ZXCT1010_1_1"
			(pin input line
				(at -5.08 5.08 270)
				(length 2.54)
				(name "Vs+")
				(number "4")
			)
			(pin power_in line
				(at -2.54 -5.08 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin output line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
			(pin input line
				(at 5.08 5.08 270)
				(length 2.54)
				(name "Vs-")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ZXCT1107"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 1.27 0)
		)
		(property "Value" "ZXCT1107"
			(at 7.62 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/ZXCT1107_10.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Low Power High-Side Current Monitors, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "High side current monitor shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "ZXCT1107_0_1")
		(symbol "ZXCT1107_1_1"
			(pin input line
				(at -5.08 5.08 270)
				(length 2.54)
				(name "Vs+")
				(number "1")
			)
			(pin output line
				(at 0 -5.08 90)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
			(pin input line
				(at 5.08 5.08 270)
				(length 2.54)
				(name "Vs-")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ZXCT1109"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 1.27 0)
		)
		(property "Value" "ZXCT1109"
			(at 7.62 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/ZXCT1107_10.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Low Power High-Side Current Monitors, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "High side current monitor shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "ZXCT1109_0_1")
		(symbol "ZXCT1109_1_1"
			(pin input line
				(at -5.08 5.08 270)
				(length 2.54)
				(name "Vs+")
				(number "2")
			)
			(pin output line
				(at 0 -5.08 90)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
			(pin input line
				(at 5.08 5.08 270)
				(length 2.54)
				(name "Vs-")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ZXCT1110"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 1.27 0)
		)
		(property "Value" "ZXCT1110"
			(at 7.62 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/ZXCT1107_10.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Low Power High-Side Current Monitors, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "High side current monitor shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "ZXCT1110_0_1")
		(symbol "ZXCT1110_1_1"
			(pin input line
				(at -5.08 5.08 270)
				(length 2.54)
				(name "Vs+")
				(number "4")
			)
			(pin power_in line
				(at -2.54 -5.08 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin output line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
			(pin input line
				(at 5.08 5.08 270)
				(length 2.54)
				(name "Vs-")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD8205"
		(extends "AD8210")
		(property "Reference" "U"
			(at -7.62 10.795 0)
		)
		(property "Value" "AD8205"
			(at -7.62 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8205.pdf"
			(at 16.51 -17.78 0)
		)
		(property "Description" "65V Single-Supply, System Difference Amplifier, 50V/V gain, bandwidth 50kHz, Vcc=5V, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "highside HS difference amplifier linear buffered"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "AD8206"
		(extends "AD8210")
		(property "Reference" "U"
			(at -7.62 10.795 0)
		)
		(property "Value" "AD8206"
			(at -7.62 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8206.pdf"
			(at 16.51 -17.78 0)
		)
		(property "Description" "65V High Common-Mode Voltage, Bidirectional, Current Shunt Amplifier, 20V/V gain, bandwidth 100kHz, Vcc=5V, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "highside HS current sense amplifier linear buffered"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "AD8208"
		(extends "AD8202")
		(property "Reference" "U"
			(at -7.62 10.795 0)
		)
		(property "Value" "AD8208"
			(at -7.62 8.89 0)
		)
		(property "Footprint" ""
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8208.pdf"
			(at 16.51 -17.78 0)
		)
		(property "Description" "45V High Voltage, Precision Difference Amplifier, 10V/V x 2V/V adjustable gain, bandwidth 70kHz, Vcc=5V, unidirectional, SOIC-8/MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "highside HS current sense amplifier linear buffered monitor preamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*P1.27mm* MSOP*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "AD8209"
		(extends "AD8203")
		(property "Reference" "U"
			(at -7.62 10.795 0)
		)
		(property "Value" "AD8209"
			(at -7.62 8.89 0)
		)
		(property "Footprint" ""
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8209.pdf"
			(at 16.51 -17.78 0)
		)
		(property "Description" "45V High Voltage, Precision Difference Amplifier, 7V/V x 2V/V adjustable gain, bandwidth 80kHz, Vcc=5V, unidirectional, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "highside HS current sense amplifier linear buffered monitor preamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*P1.27mm* MSOP*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "AD8216"
		(extends "AD8210")
		(property "Reference" "U"
			(at -7.62 10.795 0)
		)
		(property "Value" "AD8216"
			(at -7.62 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8216.pdf"
			(at 16.51 -17.78 0)
		)
		(property "Description" "65V High Bandwidth, Bidirectional Difference Amplifier, 3V/V gain, bandwidth 3MHz, Vcc=5V, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "HS difference amplifier linear"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "AD8418"
		(extends "AD8417")
		(property "Reference" "U"
			(at -7.62 10.795 0)
		)
		(property "Value" "AD8418"
			(at -7.62 8.89 0)
		)
		(property "Footprint" ""
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8418.pdf"
			(at 16.51 -17.78 0)
		)
		(property "Description" "70V Bidirectional, Zero Drift, Current Sense Amplifier, 20V/V gain, bandwidth 250kHz, VS=2.7V~5.5V, SOIC-8/MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "highside HS current sense amplifier linear"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "INA139"
		(extends "INA138")
		(property "Reference" "U"
			(at 3.81 5.08 0)
		)
		(property "Value" "INA139"
			(at 3.81 2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina169.pdf"
			(at 0 0.127 0)
		)
		(property "Description" "High-Side Measurement Current Shunt Monitor, 40V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "current sense shunt monitor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "INA168"
		(extends "INA138")
		(property "Reference" "U"
			(at 3.81 5.08 0)
		)
		(property "Value" "INA168"
			(at 3.81 2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina138.pdf"
			(at 0 0.127 0)
		)
		(property "Description" "High-Side Measurement Current Shunt Monitor, 60V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "current sense shunt monitor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "INA169"
		(extends "INA138")
		(property "Reference" "U"
			(at 3.81 5.08 0)
		)
		(property "Value" "INA169"
			(at 3.81 2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina169.pdf"
			(at 0 0.127 0)
		)
		(property "Description" "High-Side Measurement Current Shunt Monitor, 60V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "current sense shunt monitor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "INA180A2"
		(extends "INA180A1")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA180A2"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina180.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Current Sense Amplifier, 1 Circuit, Rail-to-Rail, 26V, Gain 50 V/V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "INA180A3"
		(extends "INA180A1")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA180A3"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina180.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Current Sense Amplifier, 1 Circuit, Rail-to-Rail, 26V, Gain 100 V/V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "INA180A4"
		(extends "INA180A1")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA180A4"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina180.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Current Sense Amplifier, 1 Circuit, Rail-to-Rail, 26V, Gain 200 V/V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "INA180B2"
		(extends "INA180B1")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA180B2"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina180.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Current Sense Amplifier, 1 Circuit, Rail-to-Rail, 26V, Gain 50 V/V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "INA180B3"
		(extends "INA180B1")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA180B3"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina180.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Current Sense Amplifier, 1 Circuit, Rail-to-Rail, 26V, Gain 100 V/V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "INA180B4"
		(extends "INA180B1")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA180B4"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina180.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Current Sense Amplifier, 1 Circuit, Rail-to-Rail, 26V, Gain 200 V/V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "INA185"
		(extends "INA181")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA185"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-563"
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina185.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Ultra-small, bidirectional, precision low-side and high-side, voltage output current-sense amplifier (SOT-563)"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor bidirectional"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*563*"
			(at 0 0 0)
		)
	)
	(symbol "INA194"
		(extends "INA193")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA194"
			(at 3.81 -3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina193.pdf"
			(at 0 0 0)
		)
		(property "Description" "Current Shunt Monitor −16V to +80V Common-Mode Range, 50V/V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "current sense shunt monitor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "INA195"
		(extends "INA193")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA195"
			(at 3.81 -3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina193.pdf"
			(at 0 0 0)
		)
		(property "Description" "Current Shunt Monitor −16V to +80V Common-Mode Range, 100V/V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "current sense shunt monitor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "INA197"
		(extends "INA196")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA197"
			(at 3.81 -3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina193.pdf"
			(at 0 0 0)
		)
		(property "Description" "Current Shunt Monitor −16V to +80V Common-Mode Range, 50V/V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "current sense shunt monitor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "INA198"
		(extends "INA196")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA198"
			(at 3.81 -3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina193.pdf"
			(at 0 0 0)
		)
		(property "Description" "Current Shunt Monitor −16V to +80V Common-Mode Range, 100V/V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "current sense shunt monitor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "INA200DGK"
		(extends "INA200D")
		(property "Reference" "U"
			(at -10.16 17.78 0)
		)
		(property "Value" "INA200DGK"
			(at 10.16 17.78 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina201.pdf"
			(at 0 0 0)
		)
		(property "Description" "Current Shunt Monitor, integrated comparator and reference, -16V to +80V Common-Mode Range, 20V/V, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current-sense amplifier fixed-gain high-side low-side"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "INA201D"
		(extends "INA200D")
		(property "Reference" "U"
			(at -10.16 17.78 0)
		)
		(property "Value" "INA201D"
			(at 10.16 17.78 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina201.pdf"
			(at 0 0 0)
		)
		(property "Description" "Current Shunt Monitor, integrated comparator and reference, -16V to +80V Common-Mode Range, 50V/V, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current-sense amplifier fixed-gain high-side low-side"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "INA201DGK"
		(extends "INA200D")
		(property "Reference" "U"
			(at -10.16 17.78 0)
		)
		(property "Value" "INA201DGK"
			(at 10.16 17.78 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina201.pdf"
			(at 0 0 0)
		)
		(property "Description" "Current Shunt Monitor, integrated comparator and reference, -16V to +80V Common-Mode Range, 50V/V, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current-sense amplifier fixed-gain high-side low-side"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "INA202D"
		(extends "INA200D")
		(property "Reference" "U"
			(at -10.16 17.78 0)
		)
		(property "Value" "INA202D"
			(at 10.16 17.78 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina201.pdf"
			(at 0 0 0)
		)
		(property "Description" "Current Shunt Monitor, integrated comparator and reference, -16V to +80V Common-Mode Range, 100V/V, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current-sense amplifier fixed-gain high-side low-side"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "INA202DGK"
		(extends "INA200D")
		(property "Reference" "U"
			(at -10.16 17.78 0)
		)
		(property "Value" "INA202DGK"
			(at 10.16 17.78 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina201.pdf"
			(at 0 0 0)
		)
		(property "Description" "Current Shunt Monitor, integrated comparator and reference, -16V to +80V Common-Mode Range, 100V/V, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current-sense amplifier fixed-gain high-side low-side"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "INA240A2D"
		(extends "INA240A1D")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA240A2D"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina240.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "High- and Low-Side, Bidirectional, Zero-Drift, Current-Sense Amplifier With Enhanced PWM Rejection, 50V/V, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor bidirectional high low"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "INA240A2PW"
		(extends "INA240A1PW")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA240A2PW"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_SO:TSSOP-8_4.4x3mm_P0.65mm"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina240.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "High- and Low-Side, Bidirectional, Zero-Drift, Current-Sense Amplifier With Enhanced PWM Rejection, 50V/V, TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor bidirectional high low"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "INA240A3D"
		(extends "INA240A1D")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA240A3D"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina240.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "High- and Low-Side, Bidirectional, Zero-Drift, Current-Sense Amplifier With Enhanced PWM Rejection, 100V/V, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor bidirectional high low"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "INA240A3PW"
		(extends "INA240A1PW")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA240A3PW"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_SO:TSSOP-8_4.4x3mm_P0.65mm"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina240.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "High- and Low-Side, Bidirectional, Zero-Drift, Current-Sense Amplifier With Enhanced PWM Rejection, 100V/V, TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor bidirectional high low"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "INA240A4D"
		(extends "INA240A1D")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA240A4D"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina240.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "High- and Low-Side, Bidirectional, Zero-Drift, Current-Sense Amplifier With Enhanced PWM Rejection, 200V/V, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor bidirectional high low"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "INA240A4PW"
		(extends "INA240A1PW")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA240A4PW"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_SO:TSSOP-8_4.4x3mm_P0.65mm"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina240.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "High- and Low-Side, Bidirectional, Zero-Drift, Current-Sense Amplifier With Enhanced PWM Rejection, 200V/V, TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor bidirectional high low"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "INA241A1xD"
		(extends "INA240A1D")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA241A1xD"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina241b.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "High- and Low-Side, Bidirectional, Zero-Drift, Current-Sense Amplifier With Enhanced PWM Rejection, 10V/V, ±0.01% Gain Accuracy, ±10 μV Offset Voltage, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor bidirectional high low"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "INA241A1xDDF"
		(extends "INA240A1D")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA241A1xDDF"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-8"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina241b.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "High- and Low-Side, Bidirectional, Zero-Drift, Current-Sense Amplifier With Enhanced PWM Rejection, 10V/V, ±0.01% Gain Accuracy, ±10 μV Offset Voltage, SOT-23-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor bidirectional high low"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "INA241A1xDGK"
		(extends "INA240A1D")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA241A1xDGK"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina241b.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "High- and Low-Side, Bidirectional, Zero-Drift, Current-Sense Amplifier With Enhanced PWM Rejection, 10V/V, ±0.01% Gain Accuracy, ±10 μV Offset Voltage, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor bidirectional high low"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "INA241A2xD"
		(extends "INA240A1D")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA241A2xD"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina241b.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "High- and Low-Side, Bidirectional, Zero-Drift, Current-Sense Amplifier With Enhanced PWM Rejection, 20V/V, ±0.01% Gain Accuracy, ±10 μV Offset Voltage, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor bidirectional high low"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "INA241A2xDDF"
		(extends "INA240A1D")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA241A2xDDF"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-8"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina241b.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "High- and Low-Side, Bidirectional, Zero-Drift, Current-Sense Amplifier With Enhanced PWM Rejection, 20V/V, ±0.01% Gain Accuracy, ±10 μV Offset Voltage, SOT-23-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor bidirectional high low"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "INA241A2xDGK"
		(extends "INA240A1D")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA241A2xDGK"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina241b.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "High- and Low-Side, Bidirectional, Zero-Drift, Current-Sense Amplifier With Enhanced PWM Rejection, 20V/V, ±0.01% Gain Accuracy, ±10 μV Offset Voltage, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor bidirectional high low"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "INA241A3xD"
		(extends "INA240A1D")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA241A3xD"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina241b.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "High- and Low-Side, Bidirectional, Zero-Drift, Current-Sense Amplifier With Enhanced PWM Rejection, 50V/V, ±0.01% Gain Accuracy, ±10 μV Offset Voltage, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor bidirectional high low"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "INA241A3xDDF"
		(extends "INA240A1D")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA241A3xDDF"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-8"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina241b.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "High- and Low-Side, Bidirectional, Zero-Drift, Current-Sense Amplifier With Enhanced PWM Rejection, 50V/V, ±0.01% Gain Accuracy, ±10 μV Offset Voltage, SOT-23-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor bidirectional high low"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "INA241A3xDGK"
		(extends "INA240A1D")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA241A3xDGK"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina241b.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "High- and Low-Side, Bidirectional, Zero-Drift, Current-Sense Amplifier With Enhanced PWM Rejection, 50V/V, ±0.01% Gain Accuracy, ±10 μV Offset Voltage, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor bidirectional high low"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "INA241A4xD"
		(extends "INA240A1D")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA241A4xD"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina241b.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "High- and Low-Side, Bidirectional, Zero-Drift, Current-Sense Amplifier With Enhanced PWM Rejection, 100V/V, ±0.01% Gain Accuracy, ±10 μV Offset Voltage, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor bidirectional high low"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "INA241A4xDDF"
		(extends "INA240A1D")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA241A4xDDF"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-8"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina241b.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "High- and Low-Side, Bidirectional, Zero-Drift, Current-Sense Amplifier With Enhanced PWM Rejection, 100V/V, ±0.01% Gain Accuracy, ±10 μV Offset Voltage, SOT-23-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor bidirectional high low"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "INA241A4xDGK"
		(extends "INA240A1D")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA241A4xDGK"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina241b.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "High- and Low-Side, Bidirectional, Zero-Drift, Current-Sense Amplifier With Enhanced PWM Rejection, 100V/V, ±0.01% Gain Accuracy, ±10 μV Offset Voltage, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor bidirectional high low"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "INA241A5xD"
		(extends "INA240A1D")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA241A5xD"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina241b.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "High- and Low-Side, Bidirectional, Zero-Drift, Current-Sense Amplifier With Enhanced PWM Rejection, 200V/V, ±0.01% Gain Accuracy, ±10 μV Offset Voltage, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor bidirectional high low"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "INA241A5xDDF"
		(extends "INA240A1D")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA241A5xDDF"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-8"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina241b.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "High- and Low-Side, Bidirectional, Zero-Drift, Current-Sense Amplifier With Enhanced PWM Rejection, 200V/V, ±0.01% Gain Accuracy, ±10 μV Offset Voltage, SOT-23-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor bidirectional high low"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "INA241A5xDGK"
		(extends "INA240A1D")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA241A5xDGK"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina241b.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "High- and Low-Side, Bidirectional, Zero-Drift, Current-Sense Amplifier With Enhanced PWM Rejection, 200V/V, ±0.01% Gain Accuracy, ±10 μV Offset Voltage, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor bidirectional high low"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "INA241B1xD"
		(extends "INA240A1D")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA241B1xD"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina241b.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "High- and Low-Side, Bidirectional, Zero-Drift, Current-Sense Amplifier With Enhanced PWM Rejection, 10V/V, ±0.1% Gain Accuracy, ±150 μV Offset Voltage, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor bidirectional high low"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "INA241B1xDDF"
		(extends "INA240A1D")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA241B1xDDF"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-8"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina241b.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "High- and Low-Side, Bidirectional, Zero-Drift, Current-Sense Amplifier With Enhanced PWM Rejection, 10V/V, ±0.1% Gain Accuracy, ±150 μV Offset Voltage, SOT-23-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor bidirectional high low"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "INA241B1xDGK"
		(extends "INA240A1D")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA241B1xDGK"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina241b.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "High- and Low-Side, Bidirectional, Zero-Drift, Current-Sense Amplifier With Enhanced PWM Rejection, 10V/V, ±0.1% Gain Accuracy, ±150 μV Offset Voltage, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor bidirectional high low"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "INA241B2xD"
		(extends "INA240A1D")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA241B2xD"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina241b.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "High- and Low-Side, Bidirectional, Zero-Drift, Current-Sense Amplifier With Enhanced PWM Rejection, 20V/V, ±0.1% Gain Accuracy, ±150 μV Offset Voltage, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor bidirectional high low"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "INA241B2xDDF"
		(extends "INA240A1D")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA241B2xDDF"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-8"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina241b.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "High- and Low-Side, Bidirectional, Zero-Drift, Current-Sense Amplifier With Enhanced PWM Rejection, 20V/V, ±0.1% Gain Accuracy, ±150 μV Offset Voltage, SOT-23-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor bidirectional high low"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "INA241B2xDGK"
		(extends "INA240A1D")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA241B2xDGK"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina241b.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "High- and Low-Side, Bidirectional, Zero-Drift, Current-Sense Amplifier With Enhanced PWM Rejection, 20V/V, ±0.1% Gain Accuracy, ±150 μV Offset Voltage, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor bidirectional high low"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "INA241B3xD"
		(extends "INA240A1D")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA241B3xD"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina241b.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "High- and Low-Side, Bidirectional, Zero-Drift, Current-Sense Amplifier With Enhanced PWM Rejection, 50V/V, ±0.1% Gain Accuracy, ±150 μV Offset Voltage, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor bidirectional high low"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "INA241B3xDDF"
		(extends "INA240A1D")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA241B3xDDF"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-8"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina241b.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "High- and Low-Side, Bidirectional, Zero-Drift, Current-Sense Amplifier With Enhanced PWM Rejection, 50V/V, ±0.1% Gain Accuracy, ±150 μV Offset Voltage, SOT-23-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor bidirectional high low"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "INA241B3xDGK"
		(extends "INA240A1D")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA241B3xDGK"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina241b.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "High- and Low-Side, Bidirectional, Zero-Drift, Current-Sense Amplifier With Enhanced PWM Rejection, 50V/V, ±0.1% Gain Accuracy, ±150 μV Offset Voltage, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor bidirectional high low"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "INA241B4xD"
		(extends "INA240A1D")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA241B4xD"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina241b.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "High- and Low-Side, Bidirectional, Zero-Drift, Current-Sense Amplifier With Enhanced PWM Rejection, 100V/V, ±0.1% Gain Accuracy, ±150 μV Offset Voltage, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor bidirectional high low"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "INA241B4xDDF"
		(extends "INA240A1D")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA241B4xDDF"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-8"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina241b.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "High- and Low-Side, Bidirectional, Zero-Drift, Current-Sense Amplifier With Enhanced PWM Rejection, 100V/V, ±0.1% Gain Accuracy, ±150 μV Offset Voltage, SOT-23-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor bidirectional high low"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "INA241B4xDGK"
		(extends "INA240A1D")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA241B4xDGK"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina241b.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "High- and Low-Side, Bidirectional, Zero-Drift, Current-Sense Amplifier With Enhanced PWM Rejection, 100V/V, ±0.1% Gain Accuracy, ±150 μV Offset Voltage, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor bidirectional high low"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "INA241B5xD"
		(extends "INA240A1D")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA241B5xD"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina241b.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "High- and Low-Side, Bidirectional, Zero-Drift, Current-Sense Amplifier With Enhanced PWM Rejection, 200V/V, ±0.1% Gain Accuracy, ±150 μV Offset Voltage, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor bidirectional high low"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "INA241B5xDDF"
		(extends "INA240A1D")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA241B5xDDF"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-8"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina241b.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "High- and Low-Side, Bidirectional, Zero-Drift, Current-Sense Amplifier With Enhanced PWM Rejection, 200V/V, ±0.1% Gain Accuracy, ±150 μV Offset Voltage, SOT-23-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor bidirectional high low"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "INA241B5xDGK"
		(extends "INA240A1D")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA241B5xDGK"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina241b.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "High- and Low-Side, Bidirectional, Zero-Drift, Current-Sense Amplifier With Enhanced PWM Rejection, 200V/V, ±0.1% Gain Accuracy, ±150 μV Offset Voltage, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor bidirectional high low"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "INA281A1"
		(extends "AD8211")
		(property "Reference" "U"
			(at -7.62 10.795 0)
		)
		(property "Value" "INA281A1"
			(at -7.62 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina281.pdf"
			(at 16.51 -17.78 0)
		)
		(property "Description" "-4...+110V High Voltage Current Shunt Monitor, 20V/V gain, 1.3 MHz bandwidth,  2.7..20Vcc, 55uV offset voltage, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "highside HS current sense amplifier linear buffered texas"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "INA283"
		(extends "INA282")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA283"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina282.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Accuracy, Wide Common-Mode Range, Bidirectional Current Shunt Monitors, Zero-Drift Series, 200V/V, SOIC-8/VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor bidirectional"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "INA284"
		(extends "INA282")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA284"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina282.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Accuracy, Wide Common-Mode Range, Bidirectional Current Shunt Monitors, Zero-Drift Series, 500V/V, SOIC-8/VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor bidirectional"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "INA285"
		(extends "INA282")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA285"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina282.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Accuracy, Wide Common-Mode Range, Bidirectional Current Shunt Monitors, Zero-Drift Series, 1000V/V, SOIC-8/VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor bidirectional"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "INA286"
		(extends "INA282")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "INA286"
			(at 3.81 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina282.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Accuracy, Wide Common-Mode Range, Bidirectional Current Shunt Monitors, Zero-Drift Series, 100V/V, SOIC-8/VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current monitor shunt sensor bidirectional"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "INA293A2"
		(extends "INA293A1")
		(property "Reference" "U"
			(at -8.382 6.858 0)
		)
		(property "Value" "INA293A2"
			(at 5.08 6.858 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina293.pdf"
			(at 0 0 0)
		)
		(property "Description" "-4-V to 110-V, 1.3-MHz bandwidth, Current Sense Amplifier, 50V/V gain, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "highside high lowside low HS LS linear buffered texas shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "INA293A3"
		(extends "INA293A1")
		(property "Reference" "U"
			(at -8.382 6.858 0)
		)
		(property "Value" "INA293A3"
			(at 5.08 6.858 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina293.pdf"
			(at 0 0 0)
		)
		(property "Description" "-4-V to 110-V, 1-MHz bandwidth, Current Sense Amplifier, 100V/V gain, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "highside high lowside low HS LS linear buffered texas shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "INA293A4"
		(extends "INA293A1")
		(property "Reference" "U"
			(at -8.382 6.858 0)
		)
		(property "Value" "INA293A4"
			(at 5.08 6.858 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina293.pdf"
			(at 0 0 0)
		)
		(property "Description" "-4-V to 110-V, 900-KHz bandwidth, Current Sense Amplifier, 200V/V gain, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "highside high lowside low HS LS linear buffered texas shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "INA293A5"
		(extends "INA293A1")
		(property "Reference" "U"
			(at -8.382 6.858 0)
		)
		(property "Value" "INA293A5"
			(at 5.08 6.858 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina293.pdf"
			(at 0 0 0)
		)
		(property "Description" "-4-V to 110-V, 900-KHz bandwidth, Current Sense Amplifier, 500V/V gain, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "highside high lowside low HS LS linear buffered texas shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "INA293B2"
		(extends "INA293B1")
		(property "Reference" "U"
			(at -8.382 6.858 0)
		)
		(property "Value" "INA293B2"
			(at 5.08 6.858 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina293.pdf"
			(at 0 0 0)
		)
		(property "Description" "-4-V to 110-V, 1.3-MHz bandwidth, Current Sense Amplifier, 50V/V gain, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "highside high lowside low HS LS linear buffered texas shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "INA293B3"
		(extends "INA293B1")
		(property "Reference" "U"
			(at -8.382 6.858 0)
		)
		(property "Value" "INA293B3"
			(at 5.08 6.858 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina293.pdf"
			(at 0 0 0)
		)
		(property "Description" "-4-V to 110-V, 1-MHz bandwidth, Current Sense Amplifier, 100V/V gain, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "highside high lowside low HS LS linear buffered texas shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "INA293B4"
		(extends "INA293B1")
		(property "Reference" "U"
			(at -8.382 6.858 0)
		)
		(property "Value" "INA293B4"
			(at 5.08 6.858 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina293.pdf"
			(at 0 0 0)
		)
		(property "Description" "-4-V to 110-V, 900-KHz bandwidth, Current Sense Amplifier, 200V/V gain, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "highside high lowside low HS LS linear buffered texas shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "INA293B5"
		(extends "INA293B1")
		(property "Reference" "U"
			(at -8.382 6.858 0)
		)
		(property "Value" "INA293B5"
			(at 5.08 6.858 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina293.pdf"
			(at 0 0 0)
		)
		(property "Description" "-4-V to 110-V, 900-KHz bandwidth, Current Sense Amplifier, 500V/V gain, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "highside high lowside low HS LS linear buffered texas shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "INA4180A2"
		(extends "INA4180A1")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "INA4180A2"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -1.27 2.54 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina4180.pdf"
			(at 1.27 5.08 0)
		)
		(property "Description" "Quad current sense amplifier, Rail-to-Rail, 26V, Gain 50 V/V, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "monitor shunt sensor texas"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "INA4180A3"
		(extends "INA4180A1")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "INA4180A3"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -1.27 2.54 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina4180.pdf"
			(at 1.27 5.08 0)
		)
		(property "Description" "Quad current sense amplifier, Rail-to-Rail, 26V, Gain 100 V/V, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "monitor shunt sensor texas"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "INA4180A4"
		(extends "INA4180A1")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "INA4180A4"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -1.27 2.54 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina4180.pdf"
			(at 1.27 5.08 0)
		)
		(property "Description" "Quad current sense amplifier, Rail-to-Rail, 26V, Gain 200 V/V, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "monitor shunt sensor texas"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC6102HVxDD"
		(extends "LTC6102xDD")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "LTC6102HVxDD"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.5mm_EP1.66x2.38mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/6102fe.pdf"
			(at 0 0 0)
		)
		(property "Description" "Precision Zero Drift Current Sense Amplifier, 100V, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current sense amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC6102HVxMS8"
		(extends "LTC6102xMS8")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "LTC6102HVxMS8"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/6102fe.pdf"
			(at 0 0 0)
		)
		(property "Description" "Precision Zero Drift Current Sense Amplifier, 100V, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current sense amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX4080S"
		(extends "MAX4080F")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MAX4080S"
			(at 2.54 6.35 0)
		)
		(property "Footprint" ""
			(at 16.51 -17.78 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX4080-MAX4081.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "76V, High-Side, Current-Sense Amplifiers with Voltage Output, Undirectional, 60V/V Gain, SOIC-8/uMAX-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current sense amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX4080T"
		(extends "MAX4080F")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MAX4080T"
			(at 2.54 6.35 0)
		)
		(property "Footprint" ""
			(at 16.51 -17.78 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX4080-MAX4081.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "76V, High-Side, Current-Sense Amplifiers with Voltage Output, Unidirectional, 20V/V Gain, SOIC-8/uMAX-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current sense amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX4081S"
		(extends "MAX4081F")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MAX4081S"
			(at 2.54 8.89 0)
		)
		(property "Footprint" ""
			(at 16.51 -17.78 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX4080-MAX4081.pdf"
			(at 16.51 -17.78 0)
		)
		(property "Description" "76V, High-Side, Current-Sense Amplifiers with Voltage Outpute, Bidirectional, 60V/V Gain, SOIC-8/uMAX-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current sense amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX4081T"
		(extends "MAX4081F")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MAX4081T"
			(at 2.54 8.89 0)
		)
		(property "Footprint" ""
			(at 16.51 -17.78 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX4080-MAX4081.pdf"
			(at 16.51 -17.78 0)
		)
		(property "Description" "76V, High-Side, Current-Sense Amplifiers with Voltage Output, Bidirectional, 20V/V Gain, SOIC-8/uMAX-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current sense amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCS211"
		(extends "NCS210")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "NCS211"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCS210R-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Current-Shunt Monitor, Voltage Output, Bi-Directional Zero-Drift, 500V/V Gain, SC-70-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Current shunt monitor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "NCS213"
		(extends "NCS210")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "NCS213"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCS210R-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Current-Shunt Monitor, Voltage Output, Bi-Directional Zero-Drift, 50V/V Gain, SC-70-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Current shunt monitor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "NCS214"
		(extends "NCS210")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "NCS214"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCS210R-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Current-Shunt Monitor, Voltage Output, Bi-Directional Zero-Drift, 100V/V Gain, SC-70-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Current shunt monitor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "NCV210"
		(extends "NCS210")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "NCV210"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCS210R-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Current-Shunt Monitor, Voltage Output, Bi-Directional Zero-Drift, 200V/V Gain, SC-70-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Current shunt monitor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "NCV211"
		(extends "NCS210")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "NCV211"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCS210R-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Current-Shunt Monitor, Voltage Output, Bi-Directional Zero-Drift, 500V/V Gain, SC-70-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Current shunt monitor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "NCV213"
		(extends "NCS210")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "NCV213"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCS210R-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Current-Shunt Monitor, Voltage Output, Bi-Directional Zero-Drift, 50V/V Gain, SC-70-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Current shunt monitor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "NCV214"
		(extends "NCS210")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "NCV214"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCS210R-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Current-Shunt Monitor, Voltage Output, Bi-Directional Zero-Drift, 100V/V Gain, SC-70-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Current shunt monitor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "INA281A2"
		(extends "INA281A1")
		(property "Reference" "U"
			(at -7.62 10.795 0)
		)
		(property "Value" "INA281A2"
			(at -7.62 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina281.pdf"
			(at 16.51 -17.78 0)
		)
		(property "Description" "-4...+110V High Voltage Current Shunt Monitor, 50V/V gain, 1.3 MHz bandwidth,  2.7..20Vcc, 55uV offset voltage, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "highside HS current sense amplifier linear buffered texas"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "INA281A3"
		(extends "INA281A1")
		(property "Reference" "U"
			(at -7.62 10.795 0)
		)
		(property "Value" "INA281A3"
			(at -7.62 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina281.pdf"
			(at 16.51 -17.78 0)
		)
		(property "Description" "-4...+110V High Voltage Current Shunt Monitor, 100V/V gain, 1.3 MHz bandwidth,  2.7..20Vcc, 55uV offset voltage, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "highside HS current sense amplifier linear buffered texas"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "INA281A4"
		(extends "INA281A1")
		(property "Reference" "U"
			(at -7.62 10.795 0)
		)
		(property "Value" "INA281A4"
			(at -7.62 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina281.pdf"
			(at 16.51 -17.78 0)
		)
		(property "Description" "-4...+110V High Voltage Current Shunt Monitor, 200V/V gain, 1.3 MHz bandwidth,  2.7..20Vcc, 55uV offset voltage, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "highside HS current sense amplifier linear buffered texas"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "INA281A5"
		(extends "INA281A1")
		(property "Reference" "U"
			(at -7.62 10.795 0)
		)
		(property "Value" "INA281A5"
			(at -7.62 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina281.pdf"
			(at 16.51 -17.78 0)
		)
		(property "Description" "-4...+110V High Voltage Current Shunt Monitor, 500V/V gain, 1.3 MHz bandwidth,  2.7..20Vcc, 55uV offset voltage, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "highside HS current sense amplifier linear buffered texas"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
)
