(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "AD628"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 3.175 0)
		)
		(property "Value" "AD628"
			(at 3.81 -3.175 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD628.pdf"
			(at 0 0 0)
		)
		(property "Description" "High Common-Mode Voltage, Programmable Gain Difference Amplifier, ±120V, Gain = 0.1 to 100, SOIC-8/MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "difference amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AD628_0_1")
		(symbol "AD628_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "8")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "2")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 5.08)
				(name "RG")
				(number "6")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 5.08)
				(name "VREF")
				(number "3")
			)
			(pin passive line
				(at 2.54 -7.62 90)
				(length 6.35)
				(name "CFILT")
				(number "4")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD8207"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 10.795 0)
		)
		(property "Value" "AD8207"
			(at -7.62 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8207.pdf"
			(at 16.51 -17.78 0)
		)
		(property "Description" "65V (35V) Zero-Drift, High Voltage, Bidirectional, Difference Amplifier, 20V/V gain, bandwidth 150kHz, Vcc=5V (3.3V), SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "highside HS current sense difference amplifier linear buffered"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "AD8207_0_1")
		(symbol "AD8207_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "RANGE")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "Vref1")
				(number "7")
			)
			(pin power_in line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "V+")
				(number "6")
			)
			(pin input line
				(at -5.08 10.16 270)
				(length 2.54)
				(name "+IN")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at 5.08 10.16 270)
				(length 2.54)
				(name "-IN")
				(number "1")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "Vref2")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD8276"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 5.08 0)
		)
		(property "Value" "AD8276"
			(at 7.62 2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8276_8277.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low Power, Wide Supply Range, Low Cost Unity-Gain Difference Amplifier, SOIC-8/MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "difference amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AD8276_0_1")
		(symbol "AD8276_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "8")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 5.08)
				(name "SENSE")
				(number "5")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 5.08)
				(name "REF")
				(number "1")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD8475ACPZ"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "AD8475ACPZ"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-16-1EP_3x3mm_P0.5mm_EP1.6x1.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8475.pdf"
			(at 10.16 5.08 0)
		)
		(property "Description" "Precision, Selectable Gain, Fully Differential Funnel Amplifier, LFCSP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "selectable gain ADC driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AD8475ACPZ_0_1")
		(symbol "AD8475ACPZ_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "+IN0.4x")
				(number "1")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "+IN0.4x")
				(number "16")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "+IN0.8x")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "-IN0.8x")
				(number "3")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "-IN0.4x")
				(number "4")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "-IN0.4x")
				(number "5")
			)
			(pin no_connect line
				(at -7.62 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "+Vs")
				(number "6")
			)
			(pin passive line
				(at 0 10.16 270)
				(length 5.08)
				(hide yes)
				(name "+Vs")
				(number "7")
			)
			(pin passive line
				(at 0 10.16 270)
				(length 5.08)
				(hide yes)
				(name "+Vs")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "-Vs")
				(number "13")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 5.08)
				(hide yes)
				(name "-Vs")
				(number "14")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 5.08)
				(hide yes)
				(name "-Vs")
				(number "15")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 6.35)
				(name "VOCM")
				(number "9")
			)
			(pin passive line
				(at 2.54 -10.16 90)
				(length 6.35)
				(name "EP")
				(number "17")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 5.08)
				(name "-")
				(number "11")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 5.08)
				(name "+")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD8475xRMZ"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "AD8475xRMZ"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at -1.27 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8475.pdf"
			(at 12.7 5.08 0)
		)
		(property "Description" "Precision, Selectable Gain, Fully Differential Funnel Amplifier, MSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "selectable gain ADC driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AD8475xRMZ_0_1")
		(symbol "AD8475xRMZ_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "+IN0.4x")
				(number "9")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "+IN0.8x")
				(number "10")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "-IN0.8x")
				(number "1")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "-IN0.4x")
				(number "2")
			)
			(pin no_connect line
				(at -7.62 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "+Vs")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "-Vs")
				(number "8")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 6.35)
				(name "VOCM")
				(number "4")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 5.08)
				(name "-")
				(number "6")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 5.08)
				(name "+")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADA4938-1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "ADA4938-1"
			(at 7.62 -6.35 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-16-1EP_3x3mm_P0.5mm_EP1.3x1.3mm_ThermalVias"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADA4938-1_4938-2.pdf"
			(at -1.27 -11.43 0)
		)
		(property "Description" "Ultralow distortion, high speed fully-differential amplifier, ADC Driver, 1GHz GBP, 3x3mm LFCSP-16"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "Fully-Differential Amplifier ADC Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*EP?3x3mm?P0.5mm?EP1.3x1.3mm*"
			(at 0 0 0)
		)
		(symbol "ADA4938-1_0_1")
		(symbol "ADA4938-1_1_1"
			(pin output line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "FB-")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "+")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "-")
				(number "3")
			)
			(pin output line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "FB+")
				(number "4")
			)
			(pin input line
				(at 0 7.62 270)
				(length 3.8)
				(name "V_{OCM}")
				(number "9")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 3.175)
				(name "")
				(number "11")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 3.175)
				(name "")
				(number "10")
			)
		)
		(symbol "ADA4938-1_2_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "~{PD}")
				(number "12")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V+")
				(number "5")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(hide yes)
				(name "V+")
				(number "6")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(hide yes)
				(name "V+")
				(number "7")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(hide yes)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "V-")
				(number "13")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "V-")
				(number "14")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "V-")
				(number "15")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "V-")
				(number "16")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "PAD")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADA4940-1xCP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 5.08 0)
		)
		(property "Value" "ADA4940-1xCP"
			(at 11.43 -5.08 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-16-1EP_3x3mm_P0.5mm_EP1.3x1.3mm_ThermalVias"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADA4940-1_4940-2.pdf"
			(at -43.18 30.48 0)
		)
		(property "Description" "Ultralow Power, Low Distortion, Fully Differential ADC Drivers, LFCSP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "differential amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ADA4940-1xCP_1_1"
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "-IN")
				(number "3")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~{DISABLE}")
				(number "12")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "VOCM")
				(number "9")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "+IN")
				(number "2")
			)
			(pin input line
				(at 0 7.62 270)
				(length 2.54)
				(name "+FB")
				(number "4")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "-FB")
				(number "1")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 5.08)
				(name "+OUT")
				(number "10")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 5.08)
				(name "-OUT")
				(number "11")
			)
		)
		(symbol "ADA4940-1xCP_2_1"
			(pin power_in line
				(at 0 6.35 270)
				(length 2.54)
				(name "+Vs")
				(number "5")
			)
			(pin passive line
				(at 0 6.35 270)
				(length 2.54)
				(hide yes)
				(name "+Vs")
				(number "6")
			)
			(pin passive line
				(at 0 6.35 270)
				(length 2.54)
				(hide yes)
				(name "+Vs")
				(number "7")
			)
			(pin passive line
				(at 0 6.35 270)
				(length 2.54)
				(hide yes)
				(name "+Vs")
				(number "8")
			)
			(pin power_in line
				(at 0 -6.35 90)
				(length 2.54)
				(name "-Vs")
				(number "13")
			)
			(pin passive line
				(at 0 -6.35 90)
				(length 2.54)
				(hide yes)
				(name "-Vs")
				(number "14")
			)
			(pin passive line
				(at 0 -6.35 90)
				(length 2.54)
				(hide yes)
				(name "-Vs")
				(number "15")
			)
			(pin passive line
				(at 0 -6.35 90)
				(length 2.54)
				(hide yes)
				(name "-Vs")
				(number "16")
			)
			(pin passive line
				(at 2.54 -6.35 90)
				(length 2.54)
				(name "EP")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADA4940-2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 5.08 0)
		)
		(property "Value" "ADA4940-2"
			(at 8.89 -5.08 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-24-1EP_4x4mm_P0.5mm_EP2.5x2.5mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADA4940-1_4940-2.pdf"
			(at -43.18 30.48 0)
		)
		(property "Description" "Ultralow Power, Low Distortion, Fully Differential ADC Drivers, Dual-Channel, LFCSP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "differential amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ADA4940-2_0_1")
		(symbol "ADA4940-2_1_1"
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "-IN1")
				(number "1")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~{DISABLE1}")
				(number "20")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "VOCM1")
				(number "17")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "+IN1")
				(number "24")
			)
			(pin input line
				(at 0 7.62 270)
				(length 2.54)
				(name "+FB1")
				(number "2")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "-FB1")
				(number "23")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 5.08)
				(name "+1")
				(number "18")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 5.08)
				(name "-1")
				(number "19")
			)
		)
		(symbol "ADA4940-2_2_1"
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "-IN2")
				(number "7")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~{DISABLE2}")
				(number "14")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "VOCM2")
				(number "11")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "+IN2")
				(number "6")
			)
			(pin input line
				(at 0 7.62 270)
				(length 2.54)
				(name "+FB2")
				(number "8")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "-FB2")
				(number "5")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 5.08)
				(name "+2")
				(number "12")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 5.08)
				(name "-2")
				(number "13")
			)
		)
		(symbol "ADA4940-2_3_1"
			(pin input line
				(at 2.54 7.62 270)
				(length 3.81)
				(name "+FB2")
				(number "3")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 3.81)
				(hide yes)
				(name "+FB2")
				(number "4")
			)
			(pin input line
				(at 2.54 -7.62 90)
				(length 3.81)
				(name "-FB2")
				(number "21")
			)
			(pin input line
				(at 2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "-FB2")
				(number "22")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 4.445)
				(name "EP")
				(number "25")
			)
		)
		(symbol "ADA4940-2_4_1"
			(pin input line
				(at 2.54 7.62 270)
				(length 3.81)
				(hide yes)
				(name "+FB2")
				(number "10")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 3.81)
				(name "+FB2")
				(number "9")
			)
			(pin input line
				(at 2.54 -7.62 90)
				(length 3.81)
				(name "-FB2")
				(number "15")
			)
			(pin input line
				(at 2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "-FB2")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AMC1100DWV"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 8.89 0)
		)
		(property "Value" "AMC1100DWV"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_7.5x5.85mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/amc1100.pdf"
			(at 16.51 -17.78 0)
		)
		(property "Description" "Fully-differential isolated amplifier, fixed gain = 8, peak isolation voltage 4250V, transient immunity 2.5kV/us, UL1577/IEC60747-5-2 approved, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "isolated difference amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x5.85mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "AMC1100DWV_0_1")
		(symbol "AMC1100DWV_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "+")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "-")
				(number "3")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "V+")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "V-")
				(number "4")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 3.81)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "5")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 5.08)
				(name "+")
				(number "7")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 5.08)
				(name "-")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM733CH"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "LM733CH"
			(at 3.81 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-5-10"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.soemtron.org/downloads/disposals/lm733cn.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Differential Amplifier, TO-5-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "single differential video opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?5*"
			(at 0 0 0)
		)
		(symbol "LM733CH_0_1")
		(symbol "LM733CH_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "5")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 5.08)
				(name "1A")
				(number "9")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 5.08)
				(name "2A")
				(number "10")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 6.35)
				(name "1B")
				(number "4")
			)
			(pin passive line
				(at 2.54 -7.62 90)
				(length 6.35)
				(name "2B")
				(number "3")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM733CN"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "LM733CN"
			(at 3.81 -6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.soemtron.org/downloads/disposals/lm733cn.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Differential Amplifier, DIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "single differential video opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "LM733CN_0_1")
		(symbol "LM733CN_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "14")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "10")
			)
			(pin no_connect line
				(at -2.54 -3.81 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "5")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 5.08)
				(name "1A")
				(number "11")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 0 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 5.08)
				(name "2A")
				(number "12")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 6.35)
				(name "1B")
				(number "4")
			)
			(pin no_connect line
				(at 2.54 1.27 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin passive line
				(at 2.54 -7.62 90)
				(length 6.35)
				(name "2B")
				(number "3")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC1992-x-xMS8"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "LTC1992-x-xMS8"
			(at 10.16 -6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1992fb.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise Precision Fully Differential Amplifier, fixed or variable gain, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "fully differential amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LTC1992-x-xMS8_0_1")
		(symbol "LTC1992-x-xMS8_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "+")
				(number "8")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "V_{Mid}")
				(number "7")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "V_{OCM}")
				(number "2")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "-")
				(number "1")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "+V_{S}")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "-V_{S}")
				(number "6")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 3.175)
				(name "")
				(number "5")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 3.175)
				(name "")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "THS4521IDGK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "THS4521IDGK"
			(at 10.16 -6.35 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 0 -19.05 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ths4521.pdf"
			(at 0 -16.51 0)
		)
		(property "Description" "Very Low Power, Negative Rail Input, Rail to Rail Output, Fully Differential Amplifier, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "differential amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "THS4521IDGK_0_1")
		(symbol "THS4521IDGK_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "+")
				(number "8")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{PD}")
				(number "7")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "V_{OCM}")
				(number "2")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "-")
				(number "1")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "V_{S+}")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "V_{S-}")
				(number "6")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 3.175)
				(name "")
				(number "5")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 3.175)
				(name "")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "THS4551xRGT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "THS4551xRGT"
			(at 10.16 -6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.68x1.68mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ths4551.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise Precision Fully Differential Amplifier, VQFN-16"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "differential amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "THS4551xRGT_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IN+")
				(number "2")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{PD}")
				(number "12")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "VOCM")
				(number "9")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "IN-")
				(number "3")
			)
			(pin output line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "FB+")
				(number "4")
			)
			(pin output line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "FB-")
				(number "1")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 5.08)
				(name "OUT+")
				(number "10")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 5.08)
				(name "OUT-")
				(number "11")
			)
		)
		(symbol "THS4551xRGT_2_1"
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "VS-")
				(number "13")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "VS-")
				(number "14")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "VS-")
				(number "15")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "VS-")
				(number "16")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VS+")
				(number "5")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(hide yes)
				(name "VS+")
				(number "6")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(hide yes)
				(name "VS+")
				(number "7")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(hide yes)
				(name "VS+")
				(number "8")
			)
			(pin passive line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "EP")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AMC1200BDWV"
		(extends "AMC1100DWV")
		(property "Reference" "U"
			(at 7.62 8.89 0)
		)
		(property "Value" "AMC1200BDWV"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_7.5x5.85mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/amc1200.pdf"
			(at 16.51 -17.78 0)
		)
		(property "Description" "Fully-differential isolated amplifier, ±250-mV input, fixed gain = 8, peak isolation voltage 4250V, transient immunity 10kV/us, UL1577/VDE V 0884-10 approved, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "isolated difference amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x5.85mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "AMC1300BDWV"
		(extends "AMC1100DWV")
		(property "Reference" "U"
			(at 7.62 8.89 0)
		)
		(property "Value" "AMC1300BDWV"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_7.5x5.85mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/amc1300.pdf"
			(at 16.51 -17.78 0)
		)
		(property "Description" "Fully-differental precision isolated amplifier, ±250-mV Input, reinforced isloation, fixed Gain = 8.2, peak isolation voltage 7071V, transient immunity 100kV/us, UL1577/VDE V 0884-11 approved, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "isolated difference amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x5.85mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "AMC1300DWV"
		(extends "AMC1100DWV")
		(property "Reference" "U"
			(at 7.62 8.89 0)
		)
		(property "Value" "AMC1300DWV"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_7.5x5.85mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/amc1300.pdf"
			(at 16.51 -17.78 0)
		)
		(property "Description" "Fully-differental isolated amplifier, ±250-mV Input, reinforced isloation, fixed gain = 8.2, peak isolation voltage 7071V, transient immunity 15kV/us, UL1577/VDE V 0884-11 approved, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "isolated difference amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x5.85mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "INA105KP"
		(extends "AD8276")
		(property "Reference" "U"
			(at 7.62 5.08 0)
		)
		(property "Value" "INA105KP"
			(at 7.62 2.54 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina105.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low Power, Wide Supply Range, Low Cost Unity-Gain Difference Amplifier, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "difference amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "INA105KU"
		(extends "AD8276")
		(property "Reference" "U"
			(at 7.62 5.08 0)
		)
		(property "Value" "INA105KU"
			(at 7.62 2.54 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina105.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low Power, Wide Supply Range, Low Cost Unity-Gain Difference Amplifier, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "difference amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM733H"
		(extends "LM733CH")
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "LM733H"
			(at 3.81 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-5-10"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.soemtron.org/downloads/disposals/lm733cn.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Differential Amplifier, TO-5-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "single differential video opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?5*"
			(at 0 0 0)
		)
	)
	(symbol "THS4521ID"
		(extends "THS4521IDGK")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "THS4521ID"
			(at 10.16 -6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ths4521.pdf"
			(at 0 0 0)
		)
		(property "Description" "Very Low Power, Negative Rail Input, Rail to Rail Output, Fully Differential Amplifier, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "differential amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
)
