(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "AD620"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 7.62 0)
		)
		(property "Value" "AD620"
			(at 5.08 5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD620.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low Cost, Low Power, Instrumentation Amplifier, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Instrumentation amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "AD620_0_1")
		(symbol "AD620_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "Rg")
				(number "1")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "Rg")
				(number "8")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "Vs+")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "Vs-")
				(number "4")
			)
			(pin passive line
				(at 2.54 -7.62 90)
				(length 5.08)
				(name "Ref")
				(number "5")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD623AN"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.556 7.366 0)
		)
		(property "Value" "AD623AN"
			(at 6.604 5.334 0)
		)
		(property "Footprint" ""
			(at -2.54 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD623.pdf"
			(at 11.43 -10.16 0)
		)
		(property "Description" "Single Supply, Rail to Rail, Instumentation Amplifier, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "ad623 instumentation amplifier dip-8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP-8*"
			(at 0 0 0)
		)
		(symbol "AD623AN_0_1")
		(symbol "AD623AN_1_1"
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "Rg")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "Rg")
				(number "8")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vs+")
				(number "7")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "Vs-")
				(number "4")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 5.08)
				(name "Ref")
				(number "5")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD623AR"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.556 7.366 0)
		)
		(property "Value" "AD623AR"
			(at 6.604 5.334 0)
		)
		(property "Footprint" ""
			(at -2.54 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD623.pdf"
			(at 11.43 -10.16 0)
		)
		(property "Description" "Single Supply, Rail to Rail, Instumentation Amplifier, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "ad623 instumentation amplifier soic-8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC-8*"
			(at 0 0 0)
		)
		(symbol "AD623AR_0_1")
		(symbol "AD623AR_1_1"
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "Rg")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "Rg")
				(number "8")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vs+")
				(number "7")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "Vs-")
				(number "4")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 5.08)
				(name "Ref")
				(number "5")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD623ARM"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.556 7.366 0)
		)
		(property "Value" "AD623ARM"
			(at 7.112 5.334 0)
		)
		(property "Footprint" ""
			(at -2.54 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD623.pdf"
			(at 11.43 -10.16 0)
		)
		(property "Description" "Single Supply, Rail to Rail, Instumentation Amplifier, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "ad623 instumentation amplifier msop-8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP-8*"
			(at 0 0 0)
		)
		(symbol "AD623ARM_0_1")
		(symbol "AD623ARM_1_1"
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "Rg")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "Rg")
				(number "8")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vs+")
				(number "7")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "Vs-")
				(number "4")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 5.08)
				(name "Ref")
				(number "5")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD8230"
		(pin_names
			(offset 0.0762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 7.62 0)
		)
		(property "Value" "AD8230"
			(at 7.62 5.08 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 3.81 -13.97 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8230.pdf"
			(at -2.54 2.54 0)
		)
		(property "Description" "16V Rail-to-Rail, Zero-Drift, Precision Instrumentation Amplifier, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single instrumentation amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "AD8230_0_1")
		(symbol "AD8230_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "5")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "1")
			)
			(pin output line
				(at 0 7.62 270)
				(length 5.08)
				(name "Rg")
				(number "7")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "Vr1")
				(number "3")
			)
			(pin input line
				(at 2.54 -7.62 90)
				(length 6.35)
				(name "Vr2")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD8231"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "AD8231"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_CSP:Analog_LFCSP-16-1EP_4x4mm_P0.65mm_EP2.1x2.1mm"
			(at 0 -21.59 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ad8231.pdf"
			(at 0 -24.13 0)
		)
		(property "Description" "Zero Drift, Digitally programmable instrumentation amplifier, 2.7MHz bandwidth, LFCSP-16"
			(at 0 -26.67 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "Analog extra op amp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Analog*LFCSP*4x4mm*P0.65mm*EP2.1x2.1mm*"
			(at 0 0 0)
		)
		(symbol "AD8231_1_0"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "")
				(number "10")
			)
		)
		(symbol "AD8231_1_1"
			(text "In-Amp"
				(at -1.524 0 0)
			)
			(pin input line
				(at 0 -7.62 90)
				(length 3.8)
				(name "REF")
				(number "9")
			)
		)
		(symbol "AD8231_2_0"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "6")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "7")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "")
				(number "8")
			)
		)
		(symbol "AD8231_2_1")
		(symbol "AD8231_3_0"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "A0")
				(number "14")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A1")
				(number "15")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A2")
				(number "16")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{CS}")
				(number "13")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "~{SDN}")
				(number "5")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V+")
				(number "12")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "11")
			)
			(pin no_connect line
				(at 7.62 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at 7.62 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "EP")
				(number "17")
			)
		)
		(symbol "AD8231_3_1")
		(embedded_fonts no)
	)
	(symbol "AD8236"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 7.62 0)
		)
		(property "Value" "AD8236"
			(at 3.81 5.08 0)
		)
		(property "Footprint" ""
			(at -7.62 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8236.pdf"
			(at 8.89 -10.16 0)
		)
		(property "Description" "Single 40 μA Micropower Instrumentation Amplifier with Zero Crossover Distortion, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single instumentation amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AD8236_0_1")
		(symbol "AD8236_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "-")
				(number "1")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "Rg")
				(number "2")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "Rg")
				(number "3")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "+")
				(number "4")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "Vs+")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "Vs-")
				(number "5")
			)
			(pin passive line
				(at 2.54 -7.62 90)
				(length 5.08)
				(name "Ref")
				(number "6")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD8422ARMZ"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.556 7.366 0)
		)
		(property "Value" "AD8422ARMZ"
			(at 7.366 5.334 0)
		)
		(property "Footprint" ""
			(at -5.08 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8422.pdf"
			(at 8.89 -10.16 0)
		)
		(property "Description" "Low Power, Rail to Rail, Instumentation Amplifier, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "ad8422 instumentation amplifier msop-8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP-8*"
			(at 0 0 0)
		)
		(symbol "AD8422ARMZ_0_1")
		(symbol "AD8422ARMZ_1_1"
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "-")
				(number "1")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "Rg")
				(number "2")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "Rg")
				(number "3")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "+")
				(number "4")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vs+")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "Vs-")
				(number "5")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 5.08)
				(name "Ref")
				(number "6")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD8422ARZ"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.556 7.366 0)
		)
		(property "Value" "AD8422ARZ"
			(at 7.366 5.334 0)
		)
		(property "Footprint" ""
			(at -2.54 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8422.pdf"
			(at 11.43 -10.16 0)
		)
		(property "Description" "Low Power, Rail to Rail, Instumentation Amplifier, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "ad8422 instumentation amplifier soic-8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC-8*"
			(at 0 0 0)
		)
		(symbol "AD8422ARZ_0_1")
		(symbol "AD8422ARZ_1_1"
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "-")
				(number "1")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "Rg")
				(number "2")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "Rg")
				(number "3")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "+")
				(number "4")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vs+")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "Vs-")
				(number "5")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 5.08)
				(name "Ref")
				(number "6")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "INA128"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 3.175 0)
		)
		(property "Value" "INA128"
			(at 3.81 -3.175 0)
		)
		(property "Footprint" ""
			(at 2.54 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina128.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "Precision, Low Power Instrumentation Amplifier G = 1 + 50kOhm/Rg, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "instrumentation opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "INA128_0_1")
		(symbol "INA128_1_1"
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "Rg")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "Rg")
				(number "8")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin input line
				(at 2.54 -7.62 90)
				(length 5.08)
				(name "Ref")
				(number "5")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "INA326"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 3.175 0)
		)
		(property "Value" "INA326"
			(at 3.81 -3.175 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina326.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "Precision, Rail-to-Rail I/O Instrumentation Amplifier, MSOP-8 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "instrumentation opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "INA326_0_1")
		(symbol "INA326_1_1"
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "R1")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "R1")
				(number "8")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin input line
				(at 2.54 -7.62 90)
				(length 5.08)
				(name "R2")
				(number "5")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "INA327"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 3.175 0)
		)
		(property "Value" "INA327"
			(at 3.81 -3.175 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina326.pdf"
			(at 0 0 0)
		)
		(property "Description" "Precision, Rail-to-Rail I/O Instrumentation Amplifier, MSOP-10 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "instrumentation opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "INA327_0_1")
		(symbol "INA327_1_1"
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "R1")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "R1")
				(number "10")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 3.81)
				(name "V+")
				(number "5")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 3.81)
				(hide yes)
				(name "V+")
				(number "9")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 5.08)
				(name "EN")
				(number "6")
			)
			(pin input line
				(at 2.54 -7.62 90)
				(length 5.08)
				(name "R2")
				(number "7")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "INA333xxDGK"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 3.175 0)
		)
		(property "Value" "INA333xxDGK"
			(at 3.81 -3.175 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina333.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "Zero Drift, Micropower Instrumentation Amplifier G = 1 + 100kOhm/Rg, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "instrumentation opamp amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "INA333xxDGK_0_1")
		(symbol "INA333xxDGK_1_1"
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "Rg")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "Rg")
				(number "8")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin input line
				(at 2.54 -7.62 90)
				(length 5.08)
				(name "Ref")
				(number "5")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "INA333xxDRG"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 3.175 0)
		)
		(property "Value" "INA333xxDRG"
			(at 3.81 -3.175 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_3x3mm_P0.5mm_EP1.45x2.4mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina333.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "Zero Drift, Micropower Instrumentation Amplifier G = 1 + 100kOhm/Rg, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "instrumentation opamp amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "INA333xxDRG_0_1")
		(symbol "INA333xxDRG_1_1"
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "Rg")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "Rg")
				(number "8")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 5.08)
				(name "Ref")
				(number "5")
			)
			(pin passive line
				(at 2.54 -7.62 90)
				(length 5.08)
				(name "EP")
				(number "9")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC1100xN8"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 6.35 0)
		)
		(property "Value" "LTC1100xN8"
			(at 1.27 3.81 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1100fc.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Precision, Zero-Drift Instrumentation Amplifier, Gain = 100, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single instrumentation amp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "LTC1100xN8_0_1")
		(symbol "LTC1100xN8_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "6")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "3")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "COMP")
				(number "7")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "CMRR")
				(number "2")
			)
			(pin input line
				(at 2.54 -7.62 90)
				(length 6.35)
				(name "GND")
				(number "1")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC1100xSW"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 3.81 0)
		)
		(property "Value" "LTC1100xSW"
			(at 6.35 -2.54 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1100fc.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Precision, Zero-Drift Instrumentation Amplifier, Gain = 10/100, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "single instrumentation amp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LTC1100xSW_0_1")
		(symbol "LTC1100xSW_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "11")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "6")
			)
			(pin no_connect line
				(at -5.08 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -5.08 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "10")
			)
			(pin no_connect line
				(at -2.54 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at -2.54 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "7")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "COMP")
				(number "13")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at 0 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "CMRR")
				(number "4")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 3.81)
				(name "~")
				(number "14")
			)
			(pin input line
				(at 2.54 -7.62 90)
				(length 6.35)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 5.08 7.62 270)
				(length 3.81)
				(name "~")
				(number "3")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD623"
		(extends "AD620")
		(property "Reference" "U"
			(at 3.81 7.62 0)
		)
		(property "Value" "AD623"
			(at 5.08 5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD623.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Rail-to-Rail, Low Cost Instrumentation Amplifier, DIP-8/SOIC-8/MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single instumentation amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "AD623ANZ"
		(extends "AD623AN")
		(property "Reference" "U"
			(at 3.556 7.366 0)
		)
		(property "Value" "AD623ANZ"
			(at 6.604 5.334 0)
		)
		(property "Footprint" ""
			(at -2.54 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD623.pdf"
			(at 11.43 -10.16 0)
		)
		(property "Description" "Single Supply, Rail to Rail, Instumentation Amplifier, RoHS, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "ad623 instumentation amplifier dip-8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP-8*"
			(at 0 0 0)
		)
	)
	(symbol "AD623ARMZ"
		(extends "AD623ARM")
		(property "Reference" "U"
			(at 3.556 7.366 0)
		)
		(property "Value" "AD623ARMZ"
			(at 7.112 5.334 0)
		)
		(property "Footprint" ""
			(at -2.54 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD623.pdf"
			(at 11.43 -10.16 0)
		)
		(property "Description" "Single Supply, Rail to Rail, Instumentation Amplifier, RoHS, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "ad623 instumentation amplifier msop-8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP-8*"
			(at 0 0 0)
		)
	)
	(symbol "AD623ARZ"
		(extends "AD623AR")
		(property "Reference" "U"
			(at 3.556 7.366 0)
		)
		(property "Value" "AD623ARZ"
			(at 6.604 5.334 0)
		)
		(property "Footprint" ""
			(at -2.54 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD623.pdf"
			(at 11.43 -10.16 0)
		)
		(property "Description" "Single Supply, Rail to Rail, Instumentation Amplifier, RoHS, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "ad623 instumentation amplifier soic-8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC-8*"
			(at 0 0 0)
		)
	)
	(symbol "AD623BN"
		(extends "AD623AN")
		(property "Reference" "U"
			(at 3.556 7.366 0)
		)
		(property "Value" "AD623BN"
			(at 6.604 5.334 0)
		)
		(property "Footprint" ""
			(at -2.54 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD623.pdf"
			(at 11.43 -10.16 0)
		)
		(property "Description" "Single Supply, Rail to Rail, Instumentation Amplifier, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "ad623 instumentation amplifier dip-8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP-8*"
			(at 0 0 0)
		)
	)
	(symbol "AD623BNZ"
		(extends "AD623AN")
		(property "Reference" "U"
			(at 3.556 7.366 0)
		)
		(property "Value" "AD623BNZ"
			(at 6.604 5.334 0)
		)
		(property "Footprint" ""
			(at -2.54 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD623.pdf"
			(at 11.43 -10.16 0)
		)
		(property "Description" "Single Supply, Rail to Rail, Instumentation Amplifier, RoHS, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "ad623 instumentation amplifier dip-8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP-8*"
			(at 0 0 0)
		)
	)
	(symbol "AD623BR"
		(extends "AD623AR")
		(property "Reference" "U"
			(at 3.556 7.366 0)
		)
		(property "Value" "AD623BR"
			(at 6.604 5.334 0)
		)
		(property "Footprint" ""
			(at -2.54 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD623.pdf"
			(at 11.43 -10.16 0)
		)
		(property "Description" "Single Supply, Rail to Rail, Instumentation Amplifier, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "ad623 instumentation amplifier soic-8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC-8*"
			(at 0 0 0)
		)
	)
	(symbol "AD623BRZ"
		(extends "AD623AR")
		(property "Reference" "U"
			(at 3.556 7.366 0)
		)
		(property "Value" "AD623BRZ"
			(at 6.604 5.334 0)
		)
		(property "Footprint" ""
			(at -2.54 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD623.pdf"
			(at 11.43 -10.16 0)
		)
		(property "Description" "Single Supply, Rail to Rail, Instumentation Amplifier, RoHS, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "ad623 instumentation amplifier soic-8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC-8*"
			(at 0 0 0)
		)
	)
	(symbol "AD8236ARMZ"
		(extends "AD8422ARMZ")
		(property "Reference" "U"
			(at 3.556 7.366 0)
		)
		(property "Value" "AD8236ARMZ"
			(at 7.366 5.334 0)
		)
		(property "Footprint" ""
			(at -5.08 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8236.pdf"
			(at 8.89 -10.16 0)
		)
		(property "Description" "Micropower Instumentation Amplifier with Zero Crossover Distortion, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "ad8236 instumentation amplifier msop-8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP-8*"
			(at 0 0 0)
		)
	)
	(symbol "AD8421"
		(extends "AD8236")
		(property "Reference" "U"
			(at 3.81 7.62 0)
		)
		(property "Value" "AD8421"
			(at 3.81 5.08 0)
		)
		(property "Footprint" ""
			(at -7.62 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8421.pdf"
			(at 8.89 -10.16 0)
		)
		(property "Description" "Single Low Power Instrumentation Amplifier, SOIC-8/MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single instumentation amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "AD8421ARMZ"
		(extends "AD8422ARMZ")
		(property "Reference" "U"
			(at 3.556 7.366 0)
		)
		(property "Value" "AD8421ARMZ"
			(at 7.366 5.334 0)
		)
		(property "Footprint" ""
			(at -5.08 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8421.pdf"
			(at 8.89 -10.16 0)
		)
		(property "Description" "Low Power,  Instumentation Amplifier, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "ad8421 instumentation amplifier msop-8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP-8*"
			(at 0 0 0)
		)
	)
	(symbol "AD8421ARZ"
		(extends "AD8422ARZ")
		(property "Reference" "U"
			(at 3.556 7.366 0)
		)
		(property "Value" "AD8421ARZ"
			(at 7.366 5.334 0)
		)
		(property "Footprint" ""
			(at -2.54 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8421.pdf"
			(at 11.43 -10.16 0)
		)
		(property "Description" "Low Power, Instumentation Amplifier, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "ad8421 instumentation amplifier soic-8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC-8*"
			(at 0 0 0)
		)
	)
	(symbol "AD8421BRMZ"
		(extends "AD8422ARMZ")
		(property "Reference" "U"
			(at 3.556 7.366 0)
		)
		(property "Value" "AD8421BRMZ"
			(at 7.366 5.334 0)
		)
		(property "Footprint" ""
			(at -5.08 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8421.pdf"
			(at 8.89 -10.16 0)
		)
		(property "Description" "Low Power, Instumentation Amplifier, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "ad8421 instumentation amplifier msop-8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP-8*"
			(at 0 0 0)
		)
	)
	(symbol "AD8421BRZ"
		(extends "AD8422ARZ")
		(property "Reference" "U"
			(at 3.556 7.366 0)
		)
		(property "Value" "AD8421BRZ"
			(at 7.366 5.334 0)
		)
		(property "Footprint" ""
			(at -2.54 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8421.pdf"
			(at 11.43 -10.16 0)
		)
		(property "Description" "Low Power, Instumentation Amplifier, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "ad8421 instumentation amplifier soic-8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC-8*"
			(at 0 0 0)
		)
	)
	(symbol "AD8422"
		(extends "AD8236")
		(property "Reference" "U"
			(at 3.81 7.62 0)
		)
		(property "Value" "AD8422"
			(at 3.81 5.08 0)
		)
		(property "Footprint" ""
			(at -7.62 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8422.pdf"
			(at 8.89 -10.16 0)
		)
		(property "Description" "Single High Performance, Low Power, Rail-to-Rail Precision Instrumentation Amplifier, SOIC-8/MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single instumentation amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "AD8422BRMZ"
		(extends "AD8422ARMZ")
		(property "Reference" "U"
			(at 3.556 7.366 0)
		)
		(property "Value" "AD8422BRMZ"
			(at 7.366 5.334 0)
		)
		(property "Footprint" ""
			(at -5.08 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8422.pdf"
			(at 8.89 -10.16 0)
		)
		(property "Description" "Low Power, Rail to Rail, Instumentation Amplifier, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "ad8422 instumentation amplifier msop-8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP-8*"
			(at 0 0 0)
		)
	)
	(symbol "AD8422BRZ"
		(extends "AD8422ARZ")
		(property "Reference" "U"
			(at 3.556 7.366 0)
		)
		(property "Value" "AD8422BRZ"
			(at 7.366 5.334 0)
		)
		(property "Footprint" ""
			(at -2.54 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8422.pdf"
			(at 11.43 -10.16 0)
		)
		(property "Description" "Low Power, Rail to Rail, Instumentation Amplifier, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "ad8422 instumentation amplifier soic-8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC-8*"
			(at 0 0 0)
		)
	)
	(symbol "AD8429"
		(extends "AD8236")
		(property "Reference" "U"
			(at 3.81 7.62 0)
		)
		(property "Value" "AD8429"
			(at 3.81 5.08 0)
		)
		(property "Footprint" ""
			(at -7.62 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8429.pdf"
			(at 8.89 -10.16 0)
		)
		(property "Description" "Single Low Noise Instrumentation Amplifier, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single instumentation amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "AD8429ARZ"
		(extends "AD8422ARZ")
		(property "Reference" "U"
			(at 3.556 7.366 0)
		)
		(property "Value" "AD8429ARZ"
			(at 7.366 5.334 0)
		)
		(property "Footprint" ""
			(at -2.54 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8429.pdf"
			(at 11.43 -10.16 0)
		)
		(property "Description" "Low Noise, Instumentation Amplifier, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "ad8429 instumentation amplifier soic-8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC-8*"
			(at 0 0 0)
		)
	)
	(symbol "AD8429BRZ"
		(extends "AD8422ARZ")
		(property "Reference" "U"
			(at 3.556 7.366 0)
		)
		(property "Value" "AD8429BRZ"
			(at 7.366 5.334 0)
		)
		(property "Footprint" ""
			(at -2.54 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8429.pdf"
			(at 11.43 -10.16 0)
		)
		(property "Description" "Low Noise, Instumentation Amplifier, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "ad8429 instumentation amplifier soic-8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC-8*"
			(at 0 0 0)
		)
	)
	(symbol "INA129"
		(extends "INA128")
		(property "Reference" "U"
			(at 3.81 3.175 0)
		)
		(property "Value" "INA129"
			(at 3.81 -3.175 0)
		)
		(property "Footprint" ""
			(at 2.54 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina128.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "Precision, Low Power Instrumentation Amplifier G = 1 + 49.4kOhm/Rg, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "instrumentation opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "INA849D"
		(extends "AD8422ARMZ")
		(property "Reference" "U"
			(at 3.556 7.366 0)
		)
		(property "Value" "INA849D"
			(at 7.366 5.334 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0.254 -27.432 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina849.pdf"
			(at 0.508 -29.972 0)
		)
		(property "Description" "Ultra-Low-Noise (1 nV/√Hz), 28 MHz Bandwidth, Instrumentation Amplifier, Supply Range 8V to 36V, SOIC-8"
			(at 0 -24.892 0)
		)
		(property "ki_keywords" "high-common-mode-rejection low-offset-drift low-gain-drift"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "INA849DGK"
		(extends "AD8422ARMZ")
		(property "Reference" "U"
			(at 3.556 7.366 0)
		)
		(property "Value" "INA849DGK"
			(at 7.366 5.334 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 0.254 -27.432 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina849.pdf"
			(at 0.508 -29.972 0)
		)
		(property "Description" "Ultra-Low-Noise (1 nV/√Hz), 28 MHz Bandwidth, Instrumentation Amplifier, Supply Range 8V to 36V, VSSOP-8"
			(at 0 -24.892 0)
		)
		(property "ki_keywords" "high-common-mode-rejection low-offset-drift low-gain-drift"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
)
