(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "AD8015"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "AD8015"
			(at 3.81 -5.08 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -15.24 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8015.pdf"
			(at 25.4 -7.62 0)
		)
		(property "Description" "Wideband/Differential Output Transimpedance Amplifier, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "amplifier transimpedance differential optical receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "AD8015_0_1")
		(symbol "AD8015_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "Iin")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -5.08 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "+V")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "-V")
				(number "5")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 3.81)
				(name "Vbyp")
				(number "4")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 5.08)
				(name "+")
				(number "7")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 5.08)
				(name "-")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD8021AR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 7.62 0)
		)
		(property "Value" "AD8021AR"
			(at 1.27 5.08 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8021.pdf"
			(at 3.81 -1.27 0)
		)
		(property "Description" "Operational Amplifier, 4.5-24V single/dual supply, low noise, high speed, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "AD8021AR_0_1")
		(symbol "AD8021AR_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin power_in line
				(at -5.08 10.16 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at -5.08 -10.16 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin input line
				(at -2.54 10.16 270)
				(length 5.08)
				(name "LOGIC_REFERENCE")
				(number "1")
			)
			(pin input line
				(at 0 10.16 270)
				(length 6.35)
				(name "~{DISABLE}")
				(number "8")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 6.35)
				(name "C_{COMP}")
				(number "5")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD817"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 6.35 0)
		)
		(property "Value" "AD817"
			(at 1.27 3.81 0)
		)
		(property "Footprint" ""
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ad817.pdf"
			(at 1.27 3.81 0)
		)
		(property "Description" "High Speed, Low Power Wide Supply Range Operational Amplifier, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?8?W7.62mm* SO?8?3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "AD817_0_1")
		(symbol "AD817_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "NULL")
				(number "1")
			)
			(pin input line
				(at 2.54 -7.62 90)
				(length 6.35)
				(name "NULL")
				(number "8")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD8603"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "AD8603"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8603_8607_8609.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Precision Micropower, Low Noise CMOS, Rail-to-Rail Input/Output Operational Amplifier, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT*23*"
			(at 0 0 0)
		)
		(symbol "AD8603_0_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "2")
			)
		)
		(symbol "AD8603_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADA4099-1xUJ"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 3.81 0)
		)
		(property "Value" "ADA4099-1xUJ"
			(at 1.27 -3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ada4099-1_ada4099-2.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "3.15..50V supply, 8MHz GBW, Rail-to-Rail input/output, over-the-top opamp with shutdown, TSOT-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "single operational amplifier analog-devices high-voltage rrio"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "ADA4099-1xUJ_0_1")
		(symbol "ADA4099-1xUJ_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "2")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "~{SHDN}")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADA4099-2xCP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "ADA4099-2xCP"
			(at 2.54 3.81 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-WD-10-1EP_3x3mm_P0.5mm_EP1.64x2.38mm"
			(at 2.54 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ada4099-1_ada4099-2.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "3.15..50V supply, 8MHz GBW, Rail-to-Rail input/output, over-the-top dual opamp with shutdown, LFCSP-10"
			(at 2.54 0 0)
		)
		(property "ki_keywords" "operational amplifier analog-devices high-voltage rrio enable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ADA4099-2xCP_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "SHDN")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "ADA4099-2xCP_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "7")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "8")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "SHDN")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "9")
			)
		)
		(symbol "ADA4099-2xCP_3_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 3.81)
				(name "V+")
				(number "10")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "V-")
				(number "11")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADA4530-1"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 5.08 0)
		)
		(property "Value" "ADA4530-1"
			(at 3.81 3.175 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADA4530-1.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "Femtoampere Input Bias Current Electrometer Amplifier, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ADA4530-1_0_1")
		(symbol "ADA4530-1_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "8")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 5.08)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 5.08)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 2.54 -7.62 90)
				(length 6.35)
				(name "IC")
				(number "3")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADA4610-2xCP"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "ADA4610-2xCP"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-8-1EP_3x3mm_P0.5mm_EP1.6x2.34mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADA4610-1_4610-2_4610-4.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Low Noise, Precision, Rail-to-Rail Output, JFET Op Amp, LFCSP-8"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ADA4610-2xCP_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "ADA4610-2xCP_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "ADA4610-2xCP_3_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "V-")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADA4610-4xCP"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "ADA4610-4xCP"
			(at 2.54 3.81 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-16-1EP_4x4mm_P0.65mm_EP2.1x2.1mm"
			(at 2.54 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADA4610-1_4610-2_4610-4.pdf"
			(at 6.35 3.81 0)
		)
		(property "Description" "Quad Low Noise, Precision, Rail-to-Rail Output, JFET Op Amp, LFCSP-16"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "quad opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*4x4mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADA4610-4xCP_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "1")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NIC")
				(number "13")
			)
			(pin no_connect line
				(at 0 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NIC")
				(number "16")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "15")
			)
		)
		(symbol "ADA4610-4xCP_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(symbol "ADA4610-4xCP_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "9")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "8")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "ADA4610-4xCP_4_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "11")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "12")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(symbol "ADA4610-4xCP_5_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 3.81)
				(name "V+")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "10")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "V-")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADA4622-2xCP"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "ADA4622-2xCP"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-8-1EP_3x3mm_P0.5mm_EP1.45x1.74mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ada4622-1-4622-2-4622-4.pdf"
			(at 0 0 0)
		)
		(property "Description" "Analog Devices Dual 30V, 8MHz, Low Bias Current, Single Supply, RRO, Precision Op Amp, LFCSP-8"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*LFCSP*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ADA4622-2xCP_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "ADA4622-2xCP_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "ADA4622-2xCP_3_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "8")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 3.81)
				(hide yes)
				(name "V+")
				(number "9")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADA4622-4xCP"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "ADA4622-4xCP"
			(at 2.54 3.81 0)
		)
		(property "Footprint" "Package_CSP:Analog_LFCSP-16-1EP_4x4mm_P0.65mm_EP2.35x2.35mm"
			(at 2.54 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ada4622-1-4622-2-4622-4.pdf"
			(at 6.35 3.81 0)
		)
		(property "Description" "Analog Devices Quad 30V, 8MHz, Low Bias Current, Single Supply, RRO, Precision Op Amp, LFCSP-16"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "quad opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*LFCSP*1EP*4x4mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADA4622-4xCP_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "1")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "15")
			)
		)
		(symbol "ADA4622-4xCP_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(symbol "ADA4622-4xCP_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "9")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "8")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "ADA4622-4xCP_4_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "11")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "12")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(symbol "ADA4622-4xCP_5_1"
			(pin passive line
				(at 0 7.62 270)
				(length 3.81)
				(hide yes)
				(name "V+")
				(number "17")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 3.81)
				(name "V+")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "10")
			)
			(pin free line
				(at 2.54 2.54 180)
				(length 3.81)
				(hide yes)
				(name "NIC")
				(number "16")
			)
			(pin free line
				(at 2.54 0 180)
				(length 3.81)
				(hide yes)
				(name "NIC")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADA4625-1ARDZ"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "ADA4625-1ARDZ"
			(at 2.54 -3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.29x3mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADA4625-1-4625-2.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single 5V..36V/±2.5V..±18V supply, 18 MHz, 48V/µs slew rate, ±80 µV offset, RRO, Fast-settling single JFET Op Amp, SOIC-8-1EP"
			(at 0 0 0)
		)
		(property "ki_keywords" "analog-devices adi operational amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ADA4625-1ARDZ_0_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
		)
		(symbol "ADA4625-1ARDZ_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -2.54 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at 0 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 5.08)
				(name "EP")
				(number "9")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADA4807-1"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 3.81 0)
		)
		(property "Value" "ADA4807-1"
			(at 1.27 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADA4807-1_4807-2_4807-4.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "Single Rail-to-Rail Input/Output Amplifiers, with disable, SC-70-6/SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC*70* SOT?23*"
			(at 0 0 0)
		)
		(symbol "ADA4807-1_0_1")
		(symbol "ADA4807-1_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "2")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "~{DISABLE}")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADA4807-2ACP"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 5.08 0)
		)
		(property "Value" "ADA4807-2ACP"
			(at 3.81 -5.08 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-WD-10-1EP_3x3mm_P0.5mm_EP1.64x2.38mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADA4807-1_4807-2_4807-4.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Rail-to-Rail Input/Output Amplifiers, with disable, SC-70-6/SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*LFCSP*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ADA4807-2ACP_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "~{DISABLE1}")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "ADA4807-2ACP_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "7")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "8")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "~{DISABLE2}")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "9")
			)
		)
		(symbol "ADA4807-2ACP_3_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "10")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -7.62 90)
				(length 6.35)
				(name "EPAD")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADA4817-1ACP"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 3.81 0)
		)
		(property "Value" "ADA4817-1ACP"
			(at 1.27 -3.81 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-8-1EP_3x3mm_P0.5mm_EP1.45x1.74mm"
			(at 0 1.27 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADA4817-1_4817-2.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Single Low Noise, 1 GHz, Unity-gain stable, FastFET Op Amp, with power down, LFCSP-8-1EP"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ADA4817-1ACP_0_1")
		(symbol "ADA4817-1ACP_1_0"
			(pin no_connect line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "")
				(number "6")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 5.08)
				(name "EP")
				(number "9")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "FB")
				(number "2")
			)
		)
		(symbol "ADA4817-1ACP_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "-")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "+")
				(number "4")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "+V_{S}")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "-V_{S}")
				(number "5")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "~{PD}")
				(number "1")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADA4817-1ARD"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 3.81 0)
		)
		(property "Value" "ADA4817-1ARD"
			(at 1.27 -3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.29x3mm"
			(at 0 1.27 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADA4817-1_4817-2.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Single Low Noise, 1 GHz, Unity-gain stable, FastFET Op Amp, with power down, SOIC-8-1EP"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ADA4817-1ARD_0_1")
		(symbol "ADA4817-1ARD_1_0"
			(pin no_connect line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 5.08)
				(name "EP")
				(number "9")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "FB")
				(number "1")
			)
		)
		(symbol "ADA4817-1ARD_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "+V_{S}")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "-V_{S}")
				(number "4")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "~{PD}")
				(number "8")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADA4817-2ACP"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 3.81 0)
		)
		(property "Value" "ADA4817-2ACP"
			(at 1.27 -3.81 0)
		)
		(property "Footprint" "Package_CSP:Analog_LFCSP-16-1EP_4x4mm_P0.65mm_EP2.35x2.35mm"
			(at 0 1.27 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADA4817-1_4817-2.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Dual Low Noise, 1 GHz, Unity-gain stable, FastFET Op Amp, with power down, LFCSP-16-1EP"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*LFCSP*1EP*4x4mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADA4817-2ACP_1_0"
			(pin no_connect line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "")
				(number "11")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 5.08)
				(name "EP")
				(number "17")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "FB")
				(number "16")
			)
		)
		(symbol "ADA4817-2ACP_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "-")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "+")
				(number "2")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "+V_{S}")
				(number "14")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "-V_{S}")
				(number "12")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "~{PD}")
				(number "15")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "13")
			)
		)
		(symbol "ADA4817-2ACP_2_0"
			(pin no_connect line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "")
				(number "3")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "FB")
				(number "8")
			)
		)
		(symbol "ADA4817-2ACP_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "-")
				(number "9")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "+")
				(number "10")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "+V_{S}")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "-V_{S}")
				(number "4")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "~{PD}")
				(number "7")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADA4841-1YRJ"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "ADA4841-1YRJ"
			(at 8.89 -3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADA4841-1_4841-2.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low Power, Low Noise and Distorsion, Rail-to-Rail Output Amplifier, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp low-noise rail-to-rail"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "ADA4841-1YRJ_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "2")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "~{PD}")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADA4870ARRZ"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 5.08 0)
		)
		(property "Value" "ADA4870ARRZ"
			(at 3.81 2.54 0)
		)
		(property "Footprint" "Package_SO:HSOP-20-1EP_11.0x15.9mm_P1.27mm_SlugDown_ThermalVias"
			(at 0 0 0)
		)
		(property "Datasheet" "www.analog.com/media/en/technical-documentation/data-sheets/ADA4870.pdf"
			(at 0 0 0)
		)
		(property "Description" "High Speed, High Voltage, 1A Output Drive Amplifier, PSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HSOP*1EP*11.0x15.9mm*P1.27mm*SlugDown*"
			(at 0 0 0)
		)
		(symbol "ADA4870ARRZ_0_1")
		(symbol "ADA4870ARRZ_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "6")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "7")
			)
			(pin no_connect line
				(at -5.08 5.08 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at -5.08 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "1")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 3.81)
				(hide yes)
				(name "V+")
				(number "18")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 3.81)
				(hide yes)
				(name "V+")
				(number "19")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 3.81)
				(hide yes)
				(name "V+")
				(number "20")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "10")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "V-")
				(number "11")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "V-")
				(number "12")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "V-")
				(number "13")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 5.08)
				(name "TFL")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 5.08)
				(name "PAD")
				(number "21")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 6.35)
				(name "~{ON}")
				(number "4")
			)
			(pin input line
				(at 2.54 -7.62 90)
				(length 6.35)
				(name "~{SD}")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "15")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "16")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "17")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADA4898-1YRDZ"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "ADA4898-1YRDZ"
			(at 11.43 -2.54 0)
		)
		(property "Footprint" "Package_SO:SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.29x3mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ada4898-1_4898-2.pdf"
			(at 0 0 0)
		)
		(property "Description" "High Voltage, Low Noise, Low Distortion, Unity-Gain Stable, High Speed Op Amp, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "opamp single low noise low distortion"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ADA4898-1YRDZ_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "~{PD}")
				(number "8")
			)
			(pin passive line
				(at 2.54 -7.62 90)
				(length 6.35)
				(name "EP")
				(number "9")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADA4898-2"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "ADA4898-2"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.41x3.81mm"
			(at -1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ada4898-1_4898-2.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual High Voltage, Low Noise, Low Distortion, Unity-Gain Stable, High Speed Op Amp, SOIC-8-1EP"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "opamp dual low noise low distortion"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ADA4898-2_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "ADA4898-2_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "ADA4898-2_3_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 5.08)
				(name "EP")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AS13704"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 5.08 0)
		)
		(property "Value" "AS13704"
			(at 5.08 -5.08 0)
		)
		(property "Footprint" "Package_SO:SSOP-24_3.9x8.7mm_P0.635mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://www.alfarzpp.lv/eng/sc/AS13704.pdf"
			(at 0 -11.43 0)
		)
		(property "Description" "Quad Operational Transconductance Amplifiers (OTA), with linearizing diodes, SSOP24"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "operational transconductance amplifier OTA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*3.9x8.7mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "AS13704_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "DIODE_BIAS")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin no_connect line
				(at 0 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at 0 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "18")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "AS13704_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "-")
				(number "9")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "DIODE_BIAS")
				(number "11")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "+")
				(number "10")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "12")
			)
		)
		(symbol "AS13704_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "-")
				(number "16")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "DIODE_BIAS")
				(number "14")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "+")
				(number "15")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "17")
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "13")
			)
		)
		(symbol "AS13704_4_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "-")
				(number "21")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "DIODE_BIAS")
				(number "23")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "+")
				(number "22")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "20")
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "24")
			)
		)
		(symbol "AS13704_5_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 3.81)
				(name "V+")
				(number "19")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CA3080"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 3.81 0)
		)
		(property "Value" "CA3080"
			(at 1.27 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/ca30/ca3080-a.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "2MHz, Operational Transconductance Amplifier (OTA), gM spread 2:1, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "operational transconductance amplifier ota"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "CA3080_0_1")
		(symbol "CA3080_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin no_connect line
				(at -2.54 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 5.08)
				(name "BIAS")
				(number "5")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CA3130"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 5.08 0)
		)
		(property "Value" "CA3130"
			(at 6.35 2.54 0)
		)
		(property "Footprint" ""
			(at -2.54 -2.54 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/intersil/documents/ca31/ca3130-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "15MHz, BiMOS Operational Amplifier with MOSFET Input/CMOS Output, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "CA3130_0_1")
		(symbol "CA3130_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 5.08)
				(name "NULL")
				(number "1")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 5.08)
				(name "STRB")
				(number "8")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 6.35)
				(name "NULL")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HMC799LP3E"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 2.54 0)
		)
		(property "Value" "HMC799LP3E"
			(at 7.62 -2.54 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_3x3mm_P0.5mm_EP1.75x1.75mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/hmc799.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC - 700 MHz, 10 kOhm Transimpedance amplifier, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "amplifier transimpedance"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "HMC799LP3E_0_0"
			(pin no_connect line
				(at -5.08 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at -5.08 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -5.08 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at -5.08 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "12")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "14")
			)
			(pin no_connect line
				(at -2.54 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin no_connect line
				(at -2.54 0 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at -2.54 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin no_connect line
				(at 0 0 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin no_connect line
				(at 2.54 0 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
		)
		(symbol "HMC799LP3E_0_1")
		(symbol "HMC799LP3E_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "3")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 5.08)
				(name "CFILT")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 5.08)
				(name "CEXT")
				(number "4")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "L272"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "L272"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "www.st.com/resource/en/datasheet/l272.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Power Operation Amplifier, DIP-16"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "dual power opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "L272_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "7")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "8")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "L272_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "6")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(symbol "L272_3_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "Vs")
				(number "2")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "16")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "L272D"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "L272D"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "www.st.com/resource/en/datasheet/l272.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Power Operation Amplifier, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "dual power opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "L272D_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "13")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "14")
			)
			(pin no_connect line
				(at -2.54 2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at -2.54 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at 0 2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at 0 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(symbol "L272D_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "12")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "11")
			)
			(pin no_connect line
				(at -2.54 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin no_connect line
				(at -2.54 -2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin no_connect line
				(at 0 -2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(symbol "L272D_3_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "L272M"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "L272M"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm_LongPads"
			(at 0 0 0)
		)
		(property "Datasheet" "www.st.com/resource/en/datasheet/l272.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Power Operation Amplifier, DIP-8"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "dual power opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "L272M_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "7")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "8")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "L272M_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "6")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(symbol "L272M_3_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LF351D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "LF351D"
			(at 0 3.81 0)
		)
		(property "Footprint" ""
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/lf351.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Wide bandwidth single JFET operational amplifier, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single OpAmp JFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LF351D_0_1")
		(symbol "LF351D_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "NULL")
				(number "1")
			)
			(pin input line
				(at 2.54 -7.62 90)
				(length 6.35)
				(name "NULL")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LF351N"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "LF351N"
			(at 0 3.81 0)
		)
		(property "Footprint" ""
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/lf351.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Wide bandwidth single JFET operational amplifier, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single OpAmp JFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "LF351N_0_1")
		(symbol "LF351N_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "NULL")
				(number "1")
			)
			(pin input line
				(at 2.54 -7.62 90)
				(length 6.35)
				(name "NULL")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM13700"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 5.08 0)
		)
		(property "Value" "LM13700"
			(at 5.08 -5.08 0)
		)
		(property "Footprint" ""
			(at -7.62 0.635 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm13700.pdf"
			(at -7.62 0.635 0)
		)
		(property "Description" "Dual Operational Transconductance Amplifiers with Linearizing Diodes and Buffers, DIP-16/SOIC-16"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "operational transconductance amplifier OTA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "LM13700_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "-")
				(number "13")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "DIODE_BIAS")
				(number "15")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "+")
				(number "14")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "16")
			)
		)
		(symbol "LM13700_2_0")
		(symbol "LM13700_2_1"
			(text "V+"
				(at -2.54 3.81 0)
			)
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "10")
			)
			(pin output line
				(at 2.54 -2.54 180)
				(length 3.81)
				(name "~")
				(number "9")
			)
		)
		(symbol "LM13700_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "DIODE_BIAS")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "LM13700_4_0"
			(text "V+"
				(at -2.54 3.81 0)
			)
		)
		(symbol "LM13700_4_1"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "7")
			)
			(pin output line
				(at 2.54 -2.54 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "LM13700_5_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "11")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM2902"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "LM2902"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at -1.27 2.54 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2902-n.pdf"
			(at 1.27 5.08 0)
		)
		(property "Description" "Low-Power, Quad-Operational Amplifiers, DIP-14/SOIC-14/SSOP-14"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "quad opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* DIP*W7.62mm* TSSOP*4.4x5mm*P0.65mm* SSOP*5.3x6.2mm*P0.65mm* MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LM2902_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "LM2902_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "LM2902_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "10")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "9")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(symbol "LM2902_4_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "12")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "13")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(symbol "LM2902_5_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM2904"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "LM2904"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm358.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Operational Amplifiers, DIP-8/SOIC-8/TSSOP-8/VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LM2904_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "LM2904_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "LM2904_3_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM318J"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "LM318J"
			(at 3.81 -3.81 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm318-n.pdf"
			(at 0 0 0)
		)
		(property "Description" "Operational Amplifier, DIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "LM318J_0_1")
		(symbol "LM318J_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin no_connect line
				(at -5.08 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -5.08 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "11")
			)
			(pin no_connect line
				(at -2.54 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -2.54 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "6")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 5.08)
				(name "BAL2")
				(number "12")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at 0 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 5.08)
				(name "BAL1")
				(number "3")
			)
			(pin passive line
				(at 2.54 -7.62 90)
				(length 6.35)
				(name "BAL3")
				(number "9")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM318M"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "LM318M"
			(at 3.81 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm318-n.pdf"
			(at 0 0 0)
		)
		(property "Description" "Operational Amplifier, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99*"
			(at 0 0 0)
		)
		(symbol "LM318M_0_1")
		(symbol "LM318M_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 5.08)
				(name "BAL2")
				(number "8")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 5.08)
				(name "BAL1")
				(number "1")
			)
			(pin passive line
				(at 2.54 -7.62 90)
				(length 6.35)
				(name "BAL3")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM321"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "LM321"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm321.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low Power Single Operational Amplifier, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "LM321_0_1")
		(symbol "LM321_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "3")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM4250"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 6.35 0)
		)
		(property "Value" "LM4250"
			(at 5.08 3.81 0)
		)
		(property "Footprint" ""
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4250.pdf"
			(at 1.27 3.81 0)
		)
		(property "Description" "Programmable Operational Amplifier, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Programmable opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm* TO?5*"
			(at 0 0 0)
		)
		(symbol "LM4250_0_1")
		(symbol "LM4250_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "NULL")
				(number "1")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "IQ")
				(number "8")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 6.35)
				(name "NULL")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM6361"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "LM6361"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at 1.27 5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm6161.pdf"
			(at 3.81 7.62 0)
		)
		(property "Description" "Single High Speed Operational Amplifier, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "LM6361_0_1"
			(pin no_connect line
				(at 0 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
		)
		(symbol "LM6361_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 5.08)
				(name "VOS")
				(number "8")
			)
			(pin passive line
				(at 2.54 -7.62 90)
				(length 6.35)
				(name "VOS")
				(number "1")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM675"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "LM675"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-5_P3.4x3.7mm_StaggerOdd_Lead3.8mm_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm675.pdf"
			(at 0 0 0)
		)
		(property "Description" "Power Operational Amplifier, TO-220-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220?5*StaggerOdd*"
			(at 0 0 0)
		)
		(symbol "LM675_0_1")
		(symbol "LM675_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "3")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM7171xIM"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "LM7171xIM"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm7171.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Very High Speed High Output Current Voltage Feedback Amplifier, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LM7171xIM_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at 0 -2.54 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at 2.54 -1.27 90)
				(length 6.35)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM7171xIN"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "LM7171xIN"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm7171.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Very High Speed High Output Current Voltage Feedback Amplifier, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "LM7171xIN_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at 0 -2.54 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at 2.54 -1.27 90)
				(length 6.35)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM741"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "LM741"
			(at 0 3.81 0)
		)
		(property "Footprint" ""
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm741.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Operational Amplifier, DIP-8/TO-99-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LM741_0_1")
		(symbol "LM741_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "NULL")
				(number "1")
			)
			(pin input line
				(at 2.54 -7.62 90)
				(length 6.35)
				(name "NULL")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LMH6551MA"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "LMH6551MA"
			(at 3.81 -5.08 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -15.24 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmh6551.pdf"
			(at 25.4 -7.62 0)
		)
		(property "Description" "Differential, High-Speed, Op Amp, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "differential opamp operational amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LMH6551MA_0_1")
		(symbol "LMH6551MA_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "8")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "VCM")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "1")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "V+")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "V-")
				(number "6")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 5.08)
				(name "-")
				(number "5")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 5.08)
				(name "+")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LMH6551MM"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "LMH6551MM"
			(at 3.81 -5.08 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 2.54 -15.24 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmh6551.pdf"
			(at 25.4 -7.62 0)
		)
		(property "Description" "Differential, High-Speed, Op Amp, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "differential opamp operational amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LMH6551MM_0_1")
		(symbol "LMH6551MM_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "8")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "VCM")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "1")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "V+")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "V-")
				(number "6")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 5.08)
				(name "-")
				(number "5")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 5.08)
				(name "+")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LMH6611"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 3.81 0)
		)
		(property "Value" "LMH6611"
			(at 2.54 -3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 2.54 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmh6612.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Single Supply, 345 MHz, Rail-to-Rail Output, Amplifier, TSOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "opamp operational amplifier single"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT*23*"
			(at 0 0 0)
		)
		(symbol "LMH6611_0_1")
		(symbol "LMH6611_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "2")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "~{DISABLE}")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LMH6733"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 4.445 2.54 0)
		)
		(property "Value" "LMH6733"
			(at 7.62 -2.54 0)
		)
		(property "Footprint" "Package_SO:SSOP-16_3.9x4.9mm_P0.635mm"
			(at 2.54 -10.16 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lmh6733.pdf"
			(at 2.54 -7.62 0)
		)
		(property "Description" "1.0 GHz GBW Triple Operational Amplifier, 3..12V single supply or ±1.5V...6V dual supply , SSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "opamp rf hf "
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "LMH6733_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "1")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "~{DIS}")
				(number "16")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "")
				(number "14")
			)
		)
		(symbol "LMH6733_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "~{DIS}")
				(number "3")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "")
				(number "12")
			)
		)
		(symbol "LMH6733_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "8")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "7")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "~{DIS}")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "")
				(number "10")
			)
		)
		(symbol "LMH6733_4_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "+VS")
				(number "11")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(hide yes)
				(name "+VS")
				(number "15")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "-VS")
				(number "13")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "-VS")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LMV321"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "LMV321"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmv324.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Voltage Rail-to-Rail Output Operational Amplifiers, SOT-23-5/SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* *SC*70*"
			(at 0 0 0)
		)
		(symbol "LMV321_0_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "2")
			)
		)
		(symbol "LMV321_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "3")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LMV601"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "LMV601"
			(at 3.81 -3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmv601.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "1MHz, Low-Power, General-Purpose, 2.7V Operational Amplifiers, SC-70-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC*70*"
			(at 0 0 0)
		)
		(symbol "LMV601_0_1")
		(symbol "LMV601_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "3")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "2")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "~{SHDN}")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LOG114AxRGV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -21.59 21.59 0)
		)
		(property "Value" "LOG114AxRGV"
			(at 17.78 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGV0016A_VQFN-16-1EP_4x4mm_P0.65mm_EP2.1x2.1mm"
			(at 7.62 -36.83 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/log114.pdf"
			(at 7.62 -34.036 0)
		)
		(property "Description" "Logarithmic difference amplifer, Transimpedance input, 100pA to 10mA, integrated 2.5V reference, single or dual supply: +-5V, +5V, VQFN-16"
			(at 7.366 -31.75 0)
		)
		(property "ki_keywords" "logamp texas ti tia"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGV0016A*"
			(at 0 0 0)
		)
		(symbol "LOG114AxRGV_0_0"
			(pin input line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "I_{1}")
				(number "4")
			)
			(pin input line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "V_{CMIN}")
				(number "5")
			)
			(pin input line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "I_{2}")
				(number "3")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "COM")
				(number "7")
			)
			(pin output line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "V_{REF}")
				(number "16")
			)
			(pin power_in line
				(at -10.16 -25.4 90)
				(length 2.54)
				(name "V_{REFGND}")
				(number "1")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "V-")
				(number "6")
			)
			(pin output line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "V_{O4}")
				(number "12")
			)
			(pin input line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "-IN_{4}")
				(number "11")
			)
			(pin input line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "+IN_{4}")
				(number "10")
			)
			(pin output line
				(at 25.4 0 180)
				(length 2.54)
				(name "V_{LOGOUT}")
				(number "9")
			)
			(pin output line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "V_{O5}")
				(number "15")
			)
			(pin input line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "-IN_{5}")
				(number "14")
			)
			(pin input line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "+IN_{5}")
				(number "13")
			)
		)
		(symbol "LOG114AxRGV_0_1")
		(symbol "LOG114AxRGV_1_0"
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "V-")
				(number "17")
			)
			(pin no_connect line
				(at 5.08 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
		)
		(symbol "LOG114AxRGV_1_1"
			(text "-"
				(at -12.319 7.62 0)
			)
			(text "+"
				(at -12.319 5.207 0)
			)
			(text "-"
				(at -12.192 -5.08 0)
			)
			(text "+"
				(at -12.192 -7.62 0)
			)
			(text "A_{1}"
				(at -10.541 6.477 0)
			)
			(text "A_{2}"
				(at -10.414 -6.223 0)
			)
			(text "2.5 V_{REF}"
				(at -10.033 -12.827 0)
			)
			(text "-"
				(at 1.397 1.27 0)
			)
			(text "+"
				(at 1.397 -1.27 0)
			)
			(text "A_{3}"
				(at 3.175 0.127 0)
			)
			(text "+"
				(at 11.176 16.51 0)
			)
			(text "-"
				(at 11.176 13.97 0)
			)
			(text "+"
				(at 11.176 -3.81 0)
			)
			(text "-"
				(at 11.176 -6.35 0)
			)
			(text "A_{4}"
				(at 12.954 15.24 0)
			)
			(text "A_{5}"
				(at 12.954 -5.08 0)
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT6230xS6"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "LT6230xS6"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at -1.27 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/623012fc.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "215 MHz, Rail-to-Rail Output, Amplifier, TSOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "opamp operational amplifier single"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT*23*"
			(at 0 0 0)
		)
		(symbol "LT6230xS6_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "2")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "~{ENABLE}")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC1151CN8"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 7.62 0)
		)
		(property "Value" "LTC1151CN8"
			(at 5.08 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1151fa.pdf"
			(at -53.34 19.05 0)
		)
		(property "Description" "Dual ±15V, Zero-Drift, Operational Amplifier, DIP-8"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "LTC1151CN8_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "LTC1151CN8_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "LTC1151CN8_3_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC1151CSW"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 7.62 0)
		)
		(property "Value" "LTC1151CSW"
			(at 5.08 5.08 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1151fa.pdf"
			(at -53.34 19.05 0)
		)
		(property "Description" "Dual ±15V, Zero-Drift, Operational Amplifier, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LTC1151CSW_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin no_connect line
				(at -2.54 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at -2.54 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at 0 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(symbol "LTC1151CSW_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "11")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "12")
			)
			(pin no_connect line
				(at -2.54 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin no_connect line
				(at -2.54 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin no_connect line
				(at 0 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "13")
			)
		)
		(symbol "LTC1151CSW_3_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "14")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC1152"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 7.62 0)
		)
		(property "Value" "LTC1152"
			(at 5.08 5.08 0)
		)
		(property "Footprint" ""
			(at -20.32 8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/lt1152.pdf"
			(at -20.32 8.89 0)
		)
		(property "Description" "Rail-to-Rail Input, Rail-to-Rail Output, Zero-Drift Op Amp, DIP-8, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "LTC1152_0_1")
		(symbol "LTC1152_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "SHDN")
				(number "1")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "COMP")
				(number "5")
			)
			(pin output line
				(at 2.54 -7.62 90)
				(length 6.35)
				(name "CP")
				(number "8")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC6081xDD"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 5.08 0)
		)
		(property "Value" "LTC6081xDD"
			(at 6.35 -5.08 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-10-1EP_3x3mm_P0.5mm_EP1.55x2.48mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/60812fd.pdf"
			(at 0 0 0)
		)
		(property "Description" "Precision Dual CMOS Rail-to-Rail Input/Output Amplifiers, DFN-10"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC6081xDD_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "~{SHDN_A}")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "LTC6081xDD_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "7")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "8")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "~{SHDN_B}")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "9")
			)
		)
		(symbol "LTC6081xDD_3_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "10")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "V-")
				(number "11")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC6082xDHC"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 5.08 0)
		)
		(property "Value" "LTC6082xDHC"
			(at 5.08 -5.08 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-16-1EP_3x5mm_P0.5mm_EP1.66x4.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/60812fd.pdf"
			(at 0 0 0)
		)
		(property "Description" "Precision Quad CMOS Rail-to-Rail Input/Output Amplifiers, DFN-16"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "quad opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC6082xDHC_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin no_connect line
				(at -2.54 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at 0 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "LTC6082xDHC_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "LTC6082xDHC_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "12")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "11")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "10")
			)
		)
		(symbol "LTC6082xDHC_4_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "14")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "15")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "16")
			)
		)
		(symbol "LTC6082xDHC_5_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "13")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "V-")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC6082xGN"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 5.08 0)
		)
		(property "Value" "LTC6082xGN"
			(at 5.08 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/60812fd.pdf"
			(at 0 0 0)
		)
		(property "Description" "Precision Quad CMOS Rail-to-Rail Input/Output Amplifiers, SSOP-16"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "quad opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*3.9x4.9mm*P0.635mm* SOIC*3.9x9.9mm*P1.27mm* QSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "LTC6082xGN_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin no_connect line
				(at -2.54 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at 0 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "LTC6082xGN_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "LTC6082xGN_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "12")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "11")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "10")
			)
		)
		(symbol "LTC6082xGN_4_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "14")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "15")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "16")
			)
		)
		(symbol "LTC6082xGN_5_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC6228xDC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "LTC6228xDC"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6-1EP_2x2mm_P0.5mm_EP0.6x1.37mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LTC6228-6229.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low Distortion Rail-to-Rail Output Op Amp with Shutdown, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC6228xDC_0_1")
		(symbol "LTC6228xDC_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "5")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "3")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "V-")
				(number "7")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "~{SHDN}")
				(number "4")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC6228xS6"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "LTC6228xS6"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LTC6228-6229.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low Distortion Rail-to-Rail Output Op Amp with Shutdown, TSOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "LTC6228xS6_0_1")
		(symbol "LTC6228xS6_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "2")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "~{SHDN}")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC6228xS8"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LTC6228xS8"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:SO-8_3.9x4.9mm_P1.27mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LTC6228-6229.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low Distortion Rail-to-Rail Output Op Amp with Shutdown, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LTC6228xS8_0_1")
		(symbol "LTC6228xS8_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "V-")
				(number "5")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "~{SHDN}")
				(number "8")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "FB")
				(number "1")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC6229xDD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "LTC6229xDD"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-10-1EP_3x3mm_P0.5mm_EP1.65x2.38mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LTC6228-6229.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low Distortion Rail-to-Rail Output Op Amps with Shutdown, DFN-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DFN*1EP*3x3mm*P0.5mm*EP1.65x2.38mm*"
			(at 0 0 0)
		)
		(symbol "LTC6229xDD_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~{SHDN}")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "LTC6229xDD_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "7")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "8")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~{SHDN}")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "9")
			)
		)
		(symbol "LTC6229xDD_3_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "10")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "V-")
				(number "11")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC6229xMS8E"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "LTC6229xMS8E"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:MSOP-8-1EP_3x3mm_P0.65mm_EP1.68x1.88mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LTC6228-6229.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low Distortion Rail-to-Rail Output Op Amps with Shutdown, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LTC6229xMS8E_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "LTC6229xMS8E_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "LTC6229xMS8E_3_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "V-")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC6268xS6-10"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 10.795 0)
		)
		(property "Value" "LTC6268xS6-10"
			(at 0 13.335 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0 -13.335 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/626810f.pdf"
			(at -50.165 18.415 0)
		)
		(property "Description" "500Mhz, Ultra-Low Bias Current, FET Input, Op Amp, TSOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp transimpedance"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "LTC6268xS6-10_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "2")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "~{SHDN}")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC6268xS8-10"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 10.795 0)
		)
		(property "Value" "LTC6268xS8-10"
			(at 0 13.335 0)
		)
		(property "Footprint" "Package_SO:SO-8_3.9x4.9mm_P1.27mm"
			(at 0 -13.335 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/626810f.pdf"
			(at -50.165 18.415 0)
		)
		(property "Description" "500Mhz, Ultra-Low Bias Current, FET Input, Op Amp, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp transimpedance"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LTC6268xS8-10_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "5")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "~{SHDN}")
				(number "8")
			)
			(pin no_connect line
				(at 0 -2.54 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at 0 -2.54 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC6362xDD"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 5.08 0)
		)
		(property "Value" "LTC6362xDD"
			(at 2.54 -5.08 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.5mm_EP1.66x2.38mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/6362fa.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "Precision, Low Power, Rail-to-Rail Input/Output, Differential Op Amp/SAR ADC Driver, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single differential opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC6362xDD_0_1")
		(symbol "LTC6362xDD_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "8")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "VOCM")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "1")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "V+")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "V-")
				(number "6")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "V-")
				(number "9")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 3.81)
				(name "~{SHDN}")
				(number "7")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 5.08)
				(name "-")
				(number "5")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 5.08)
				(name "+")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC6362xMS8"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 5.08 0)
		)
		(property "Value" "LTC6362xMS8"
			(at 2.54 -5.08 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/6362fa.pdf"
			(at 0 0 0)
		)
		(property "Description" "Precision, Low Power, Rail-to-Rail Input/Output, Differential Op Amp/SAR ADC Driver, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single differential opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LTC6362xMS8_0_1")
		(symbol "LTC6362xMS8_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "8")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "VOCM")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "1")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "V+")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "V-")
				(number "6")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 3.81)
				(name "~{SHDN}")
				(number "7")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 5.08)
				(name "-")
				(number "5")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 5.08)
				(name "+")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX4238ASA"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "MAX4238ASA"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX4238-MAX4239.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Ultra-Low Offset/Drift, Low-Noise, Precision Amplifiers, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MAX4238ASA_0_1")
		(symbol "MAX4238ASA_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at 0 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "~{SHDN}")
				(number "1")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX4238AUT"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "MAX4238AUT"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX4238-MAX4239.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Ultra-Low Offset/Drift, Low-Noise, Precision Amplifiers, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MAX4238AUT_0_1")
		(symbol "MAX4238AUT_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "2")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "~{SHDN}")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP6001R"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "MCP6001R"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/MCP6001-1R-1U-2-4-1-MHz-Low-Power-Op-Amp-DS20001733L.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "1MHz, Low-Power Op Amp, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MCP6001R_0_1")
		(symbol "MCP6001R_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP6001x-LT"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "MCP6001x-LT"
			(at -1.27 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/MCP6001-1R-1U-2-4-1-MHz-Low-Power-Op-Amp-DS20001733L.pdf"
			(at 0 0 0)
		)
		(property "Description" "1 MHz, Low-Power Op Amp, SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
		(symbol "MCP6001x-LT_0_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "2")
			)
		)
		(symbol "MCP6001x-LT_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP6002-xMC"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "MCP6002-xMC"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.75x1.45mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21733j.pdf"
			(at 0 0 0)
		)
		(property "Description" "1MHz, Low-Power Op Amp, DFN-8"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MCP6002-xMC_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "MCP6002-xMC_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "MCP6002-xMC_3_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "V-")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP601-xP"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "MCP601-xP"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21314g.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Single 2.7V to 6.0V Single Supply CMOS Op Amps, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MCP601-xP_0_1")
		(symbol "MCP601-xP_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin no_connect line
				(at -2.54 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin no_connect line
				(at 0 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP601-xST"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "MCP601-xST"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:TSSOP-8_4.4x3mm_P0.65mm"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21314g.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Single 2.7V to 6.0V Single Supply CMOS Op Amps, TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP601-xST_0_1")
		(symbol "MCP601-xST_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin no_connect line
				(at -2.54 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at 0 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP603-xCH"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "MCP603-xCH"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21314g.pdf"
			(at 1.27 5.08 0)
		)
		(property "Description" "Single 2.7V to 6.0V Single Supply CMOS Op Amps, with Chip Select, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MCP603-xCH_0_1")
		(symbol "MCP603-xCH_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "2")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "~{CS}")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP603-xP"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "MCP603-xP"
			(at 0 3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21314g.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Single 2.7V to 6.0V Single Supply CMOS Op Amps, with Chip Select, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm* TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP603-xP_0_1")
		(symbol "MCP603-xP_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin no_connect line
				(at -2.54 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin no_connect line
				(at 0 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "~{CS}")
				(number "8")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP6L91T-EOT"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "MCP6L91T-EOT"
			(at -1.27 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22141b.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "10 MHz, 850 µA Op Amps, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MCP6L91T-EOT_0_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "2")
			)
		)
		(symbol "MCP6L91T-EOT_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP6V67xMNY"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "MCP6V67xMNY"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_DFN_QFN:TDFN-8-1EP_3x2mm_P0.5mm_EP1.3x1.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MCP6V66-Family-Data-Sheet-DS20006266A.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Operational Amplifiers, Zero-Drift, 80 kHz Bandwidth, 1.8V to 5.5V, Rail-to-Rail, TDFN-8"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp zero drift"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MCP6V67xMNY_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "MCP6V67xMNY_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "MCP6V67xMNY_3_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "V-")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NCS20071SN"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 10.16 0)
		)
		(property "Value" "NCS20071SN"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_SO:TSOP-5_1.65x3.05mm_P0.95mm"
			(at 1.27 30.48 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCS20071-D.PDF"
			(at 1.27 30.48 0)
		)
		(property "Description" "Single, 2.8V/µs, Rail-to-Rail Output, TSOP-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "OpAmp Rail-to-rail Output Single vfa"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOP*1.65x3.05mm*P0.95mm*"
			(at 0 0 0)
		)
		(symbol "NCS20071SN_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NCS20071XV"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 10.16 0)
		)
		(property "Value" "NCS20071XV"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-553"
			(at 1.27 30.48 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCS20071-D.PDF"
			(at 1.27 30.48 0)
		)
		(property "Description" "Single, 2.8V/µs, Rail-to-Rail Output, SOT-553"
			(at 0 0 0)
		)
		(property "ki_keywords" "OpAmp Rail-to-rail Output Single vfa"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?553*"
			(at 0 0 0)
		)
		(symbol "NCS20071XV_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "3")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NCS20072DTB"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "NCS20072DTB"
			(at 2.54 3.81 0)
		)
		(property "Footprint" "Package_SO:TSSOP-8_4.4x3mm_P0.65mm"
			(at 2.54 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCS20071-D.PDF"
			(at 6.35 3.81 0)
		)
		(property "Description" "Dual, 2.8V/µs, Rail-to-Rail Output, TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "dual rail-to-rail output opamp vfa"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "NCS20072DTB_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "NCS20072DTB_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "NCS20072DTB_3_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 3.81)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NCS20074DTB"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "NCS20074DTB"
			(at 2.54 3.81 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at 2.54 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCS20071-D.PDF"
			(at 6.35 3.81 0)
		)
		(property "Description" "Quad, 2.8V/µs, Rail-to-Rail Output, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "quad rail-to-rail output opamp vfa"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "NCS20074DTB_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "NCS20074DTB_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "NCS20074DTB_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "10")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "9")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(symbol "NCS20074DTB_4_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "12")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "13")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(symbol "NCS20074DTB_5_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 3.81)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NCS2325D"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "NCS2325D"
			(at 2.54 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/PowerSolutions/document/NCS325-D.PDF"
			(at 6.35 3.81 0)
		)
		(property "Description" "Dual operational amplifier, 50uV Offset, 0.25uV/C, 35uA Zero-Drift, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp low-power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "NCS2325D_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "NCS2325D_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "NCS2325D_3_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 3.81)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NCS2325DM"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "NCS2325DM"
			(at 2.54 3.81 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 2.54 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/PowerSolutions/document/NCS325-D.PDF"
			(at 6.35 3.81 0)
		)
		(property "Description" "Dual operational amplifier, 50uV Offset, 0.25uV/C, 35uA Zero-Drift, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp low-power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "NCS2325DM_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "NCS2325DM_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "NCS2325DM_3_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 3.81)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NCS325"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "NCS325"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCS325-D.PDF"
			(at 3.81 3.81 0)
		)
		(property "Description" "Single operational amplifier, 50uV Offset, 0.25uV/C, 35uA Zero-Drift, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp low-power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "NCS325_0_1")
		(symbol "NCS325_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NCS4325"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "NCS4325"
			(at 2.54 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 2.54 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCS325-D.PDF"
			(at 6.35 3.81 0)
		)
		(property "Description" "Quad operational amplifier, 50uV Offset, 0.25uV/C, 35uA Zero-Drift, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "quad opamp low-power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "NCS4325_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "NCS4325_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "NCS4325_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "10")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "9")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(symbol "NCS4325_4_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "12")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "13")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(symbol "NCS4325_5_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 3.81)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NE5534"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 6.35 0)
		)
		(property "Value" "NE5534"
			(at 1.27 3.81 0)
		)
		(property "Footprint" ""
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ne5534.pdf"
			(at 1.27 3.81 0)
		)
		(property "Description" "Single Low-Noise Operational Amplifiers, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm* TO?5*"
			(at 0 0 0)
		)
		(symbol "NE5534_0_1")
		(symbol "NE5534_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "C/B")
				(number "8")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "BAL")
				(number "1")
			)
			(pin input line
				(at 2.54 -7.62 90)
				(length 6.35)
				(name "COMP")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "OP07"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 6.35 0)
		)
		(property "Value" "OP07"
			(at 1.27 3.81 0)
		)
		(property "Footprint" ""
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/OP07.pdf"
			(at 1.27 3.81 0)
		)
		(property "Description" "Single Ultra-Low Offset Voltage Operational Amplifier, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm* TO*99*"
			(at 0 0 0)
		)
		(symbol "OP07_0_1")
		(symbol "OP07_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "VOS")
				(number "1")
			)
			(pin input line
				(at 2.54 -7.62 90)
				(length 6.35)
				(name "VOS")
				(number "8")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "OP1177AR"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 5.08 0)
		)
		(property "Value" "OP1177AR"
			(at 7.62 2.54 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/OP1177_2177_4177.pdf"
			(at 0 0 0)
		)
		(property "Description" "Precision Low Noise, Low Input Bias Current Operational Amplifier, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single operational amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "OP1177AR_0_1")
		(symbol "OP1177AR_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 0 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at 0 -2.54 90)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "OP1177ARM"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 5.08 0)
		)
		(property "Value" "OP1177ARM"
			(at 7.62 2.54 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/OP1177_2177_4177.pdf"
			(at 0 0 0)
		)
		(property "Description" "Precision Low Noise, Low Input Bias Current Operational Amplifier, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single operational amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "OP1177ARM_0_1")
		(symbol "OP1177ARM_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 0 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at 0 -2.54 90)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "OP179GRT"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "OP179GRT"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/OP179_279.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Single Rail-to-Rail High Output Current Operational Amplifiers, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "OP179GRT_0_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "5")
			)
		)
		(symbol "OP179GRT_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "OP179GS"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "OP179GS"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/OP179_279.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Single Rail-to-Rail High Output Current Operational Amplifiers, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "OP179GS_0_1")
		(symbol "OP179GS_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin no_connect line
				(at -2.54 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin no_connect line
				(at 0 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "OP249GS"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "OP249GS"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/OP249.pdf"
			(at 0 0 0)
		)
		(property "Description" "Precision JFET, High Speed, Dual Operational Amplifier, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "OP249GS_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "8")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "OP249GS_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(symbol "OP249GS_3_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "OP279"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "OP279"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/OP179_279.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Rail-to-Rail High Output Current Operational Amplifiers, SOIC-8/TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "OP279_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "OP279_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "OP279_3_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "OPA121KU"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "OPA121KU"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "https://www.alldatasheet.com/datasheet-pdf/pdf/56725/BURR-BROWN/OPA121.html"
			(at 3.81 3.81 0)
		)
		(property "Description" "Operational Amplifier, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp BURR-BROWN Texas Instruments"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "OPA121KU_0_1")
		(symbol "OPA121KU_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "Subst.")
				(number "8")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "NULL")
				(number "1")
			)
			(pin input line
				(at 2.54 -7.62 90)
				(length 6.35)
				(name "NULL")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "OPA1641"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "OPA1641"
			(at 3.81 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa1641.pdf"
			(at 0 0 0)
		)
		(property "Description" "JFET input, ultralow distortion, low-noise operational amplifier, SOIC-8/VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "OPA1641_0_1")
		(symbol "OPA1641_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin no_connect line
				(at -2.54 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin no_connect line
				(at 0 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "OPA197xDGK"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "OPA197xDGK"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa197.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Single 36V, Precision, Rail-to-Rail Input/Output, Low Offset Voltage, Operational Amplifier, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp rtor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "OPA197xDGK_0_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at 0 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at 2.54 0 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
		)
		(symbol "OPA197xDGK_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "OPA2197xDGK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "OPA2197xDGK"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa2197.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual 36V, Precision, Rail-to-Rail Input/Output, Low Offset Voltage, Operational Amplifier, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp rtor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "OPA2197xDGK_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "OPA2197xDGK_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "OPA2197xDGK_3_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "OPA2325"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "OPA2325"
			(at -1.27 -5.08 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa2325.pdf"
			(at 0 0 0)
		)
		(property "Description" "Precision, 10-MHz, Low-Noise, Low-Power, RRIO, CMOS Operational Amplifier, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "OPA2325_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "OPA2325_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "OPA2325_3_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "OPA2333xxDRB"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "OPA2333xxDRB"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SON:Texas_S-PVSON-N8"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa333.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual 1.8V, microPower, CMOS Operational Amplifiers, Zero-Drift Series, SON-8"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*PVSON*"
			(at 0 0 0)
		)
		(symbol "OPA2333xxDRB_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "OPA2333xxDRB_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "OPA2333xxDRB_3_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 5.08)
				(name "PAD")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "OPA2376xxYZD"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "OPA2376xxYZD"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_BGA:Texas_DSBGA-8_0.9x1.9mm_Layout2x4_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa376.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Low-Noise, Low Quiescent Current, Precision Operational Amplifier e-trim Series, DSBGA-8"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DSBGA*0.9x1.9mm*0.5mm*"
			(at 0 0 0)
		)
		(symbol "OPA2376xxYZD_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "C1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "B1")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "A1")
			)
		)
		(symbol "OPA2376xxYZD_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "D2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "C2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "B2")
			)
		)
		(symbol "OPA2376xxYZD_3_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "A2")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "D1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "OPA2691-14"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "OPA2691-14"
			(at 6.35 -2.54 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/sbos224d/sbos224d.pdf"
			(at 2.54 -15.24 0)
		)
		(property "Description" "Dual Wideband, Current-Feedback Operational Amplifier With Disable, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "dual current feedback opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "OPA2691-14_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "1")
			)
			(pin no_connect line
				(at -2.54 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at 0 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "~{DIS_A}")
				(number "3")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(symbol "OPA2691-14_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "6")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "7")
			)
			(pin no_connect line
				(at -2.54 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin no_connect line
				(at 0 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "~{DIS_B}")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(symbol "OPA2691-14_3_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "11")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "OPA2695xD"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "OPA2695xD"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/sbos354a/sbos354a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual, Ultra-Wideband, Current-Feedback Operational Amplifier with Disable, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "OPA2695xD_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "1")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(symbol "OPA2695xD_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(symbol "OPA2695xD_3_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "OPA2695xRGT"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "OPA2695xRGT"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.45x1.45mm_ThermalVias"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/sbos354a/sbos354a.pdf"
			(at 2.54 -15.24 0)
		)
		(property "Description" "Dual, Ultra-Wideband, Current-Feedback Operational Amplifier with Disable, QFN-16"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "OPA2695xRGT_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "15")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at 0 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "~{DIS_A}")
				(number "1")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "13")
			)
		)
		(symbol "OPA2695xRGT_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "6")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at 0 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "~{DIS_B}")
				(number "4")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(symbol "OPA2695xRGT_3_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "10")
			)
			(pin passive line
				(at -2.54 7.62 90)
				(length 3.81)
				(hide yes)
				(name "V+")
				(number "11")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "V-")
				(number "12")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "OPA2890IDGS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 -7.62 0)
		)
		(property "Value" "OPA2890IDGS"
			(at 2.54 -10.16 0)
		)
		(property "Footprint" "Package_SO:VSSOP-10_3x3mm_P0.5mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/opa2890.pdf"
			(at 0 -17.78 0)
		)
		(property "Description" "Low-Power, Wideband, Voltage-Feedback Operational Amplifier with Disable, VSSOP-10"
			(at 0 -12.7 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*VSSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "OPA2890IDGS_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "+")
				(number "1")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "-")
				(number "10")
			)
			(pin input line
				(at 0 5.08 270)
				(length 5.08)
				(name "~{DIS}")
				(number "2")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "9")
			)
		)
		(symbol "OPA2890IDGS_2_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "+")
				(number "5")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "-")
				(number "6")
			)
			(pin input line
				(at 0 5.08 270)
				(length 5.08)
				(name "~{DIS}")
				(number "4")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "OPA2890IDGS_3_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 3.81)
				(name "+VS")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 3.81)
				(name "-VS")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "OPA310SxDCK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "OPA310SxDCK"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Texas_R-PDSO-G6"
			(at 3.175 -6.985 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/opa310.pdf"
			(at 3.175 -4.445 0)
		)
		(property "Description" "Single Rail-to-Rail Input/Output Operational Amplifier with Shutdown, 1.5..5.5V supply, 3MHz GBW, 250uV offset voltage, 150mA output current,  SC-70-6"
			(at 3.302 -9.652 0)
		)
		(property "ki_keywords" "single opamp "
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*R*PDSO*G6*"
			(at 0 0 0)
		)
		(symbol "OPA310SxDCK_0_1")
		(symbol "OPA310SxDCK_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "3")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "2")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "~{SHDN}")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "OPA330xxYFF"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "OPA330xxYFF"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_BGA:Texas_DSBGA-5_0.822x1.116mm_Layout2x1x2_P0.4mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa330.pdf"
			(at 0 0 0)
		)
		(property "Description" "50μV V OS, 0.25μV/°C, 35μA CMOS OPERATIONAL AMPLIFIERS, Zerø-Drift Series, DSBGA"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DSBGA*0.822x1.116mm*2x1x2*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "OPA330xxYFF_0_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "A3")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "B2")
			)
		)
		(symbol "OPA330xxYFF_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "A1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "C1")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "C3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "OPA333xxD"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "OPA333xxD"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa333.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Single 1.8V, microPower, CMOS Operational Amplifiers, Zero-Drift Series, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "OPA333xxD_0_1")
		(symbol "OPA333xxD_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin no_connect line
				(at -2.54 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at 0 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "OPA355NA"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "OPA355NA"
			(at 3.81 -3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 3.81 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa355.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "200MHz, CMOS, Operational amplifier, with shutdown, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "operational amplifier opamp shutdown high-speed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "OPA355NA_0_1")
		(symbol "OPA355NA_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "2")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "ENABLE")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "OPA4197xD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 3.81 0)
		)
		(property "Value" "OPA4197xD"
			(at 0 -3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa4197.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad 36V, Precision, Rail-to-Rail Input/Output, Low Offset Voltage, Operational Amplifier, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "quad opamp rtor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "OPA4197xD_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "OPA4197xD_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "OPA4197xD_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "10")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "9")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(symbol "OPA4197xD_4_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "12")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "13")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(symbol "OPA4197xD_5_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "OPA4197xPW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 3.81 0)
		)
		(property "Value" "OPA4197xPW"
			(at 0 -3.81 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa4197.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad 36V, Precision, Rail-to-Rail Input/Output, Low Offset Voltage, Operational Amplifier, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "quad opamp rtor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "OPA4197xPW_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "OPA4197xPW_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "OPA4197xPW_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "10")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "9")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(symbol "OPA4197xPW_4_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "12")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "13")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(symbol "OPA4197xPW_5_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "OPA551P"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 7.62 0)
		)
		(property "Value" "OPA551P"
			(at 5.08 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 5.08 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa551.pdf"
			(at 31.75 -2.54 0)
		)
		(property "Description" "High-Voltage High-Current Operational Amplifier, bandwidth 3MHz, slew-rate 15V/us, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "OPA551P_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at 0 -2.54 90)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin output line
				(at 0 -7.62 90)
				(length 5.08)
				(name "Flag")
				(number "8")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "OPA551U"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 7.62 0)
		)
		(property "Value" "OPA551U"
			(at 5.08 5.08 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 5.08 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa551.pdf"
			(at 30.48 -2.54 0)
		)
		(property "Description" "High-Voltage High-Current Operational Amplifier, bandwidth 3MHz, slew-rate 15V/us, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "OPA551U_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "1")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "V-")
				(number "4")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "V-")
				(number "5")
			)
			(pin output line
				(at 0 -7.62 90)
				(length 5.08)
				(name "Flag")
				(number "8")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "OPA569DWP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 11.43 0)
		)
		(property "Value" "OPA569DWP"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Package_SO:SO-20-1EP_7.52x12.825mm_P1.27mm_EP6.045x12.09mm_Mask3.56x4.47mm"
			(at -7.62 25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa569.pdf"
			(at -5.08 0 0)
		)
		(property "Description" "Rail-to-Rail I/O, 2A, Power Amplifier, SO-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "opamp single high current"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*1EP*7.52x12.825mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "OPA569DWP_0_0"
			(pin no_connect line
				(at -12.7 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin passive line
				(at -10.16 -15.24 90)
				(length 3.048)
				(hide yes)
				(name "PAD")
				(number "21")
			)
		)
		(symbol "OPA569DWP_0_1")
		(symbol "OPA569DWP_1_1"
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "-IN")
				(number "5")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "+IN")
				(number "6")
			)
			(pin power_in line
				(at -10.16 -15.24 90)
				(length 3.048)
				(name "PAD")
				(number "1")
			)
			(pin passive line
				(at -10.16 -15.24 90)
				(length 3.048)
				(hide yes)
				(name "PAD")
				(number "10")
			)
			(pin passive line
				(at -10.16 -15.24 90)
				(length 3.048)
				(hide yes)
				(name "PAD")
				(number "11")
			)
			(pin passive line
				(at -10.16 -15.24 90)
				(length 3.048)
				(hide yes)
				(name "PAD")
				(number "20")
			)
			(pin power_in line
				(at -7.62 15.24 270)
				(length 4.572)
				(name "V+")
				(number "12")
			)
			(pin passive line
				(at -7.62 15.24 270)
				(length 4.572)
				(hide yes)
				(name "V+")
				(number "13")
			)
			(pin power_in line
				(at -7.62 -15.24 90)
				(length 4.572)
				(name "V-")
				(number "17")
			)
			(pin passive line
				(at -7.62 -15.24 90)
				(length 4.572)
				(hide yes)
				(name "V-")
				(number "18")
			)
			(pin output line
				(at -5.08 15.24 270)
				(length 6.096)
				(name "~{TFLAG}")
				(number "7")
			)
			(pin output line
				(at -2.54 15.24 270)
				(length 7.62)
				(name "~{IFLAG}")
				(number "4")
			)
			(pin output line
				(at -2.54 -15.24 90)
				(length 7.62)
				(name "ISET")
				(number "3")
			)
			(pin input line
				(at 0 15.24 270)
				(length 9.144)
				(name "ENA")
				(number "8")
			)
			(pin output line
				(at 0 -15.24 90)
				(length 9.144)
				(name "IMON")
				(number "19")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 5.08)
				(name "POUT1")
				(number "2")
			)
			(pin output line
				(at 15.24 0 180)
				(length 5.08)
				(name "OUT")
				(number "14")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 5.08)
				(hide yes)
				(name "OUT")
				(number "15")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 5.08)
				(name "POUT2")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "OPA818xDRG"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "OPA818xDRG"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_3x3mm_P0.5mm_EP1.45x2.4mm"
			(at -2.54 15.24 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/opa818.pdf"
			(at 10.16 10.16 0)
		)
		(property "Description" "2.7 GHz, High-Voltage, FET-Input, Low Noise, Operational Amplifier, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "opamp VFA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*3x3mm*EP1.45x2.4mm*"
			(at 0 0 0)
		)
		(symbol "OPA818xDRG_0_0"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "8")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "~{PD}")
				(number "1")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 5.08)
				(name "EP")
				(number "9")
			)
		)
		(symbol "OPA818xDRG_0_1"
			(pin no_connect line
				(at -5.08 -5.08 90)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "OPA818xDRG_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "5")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "FB")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "OPA858xDSG"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "OPA858xDSG"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm"
			(at -2.54 15.24 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa858.pdf"
			(at 10.16 10.16 0)
		)
		(property "Description" "5.5-GHz Gain Bandwidth Product, Gain of 7 V/V Stable, FET Input Amplifier, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "opamp VFA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "OPA858xDSG_0_0"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "V-")
				(number "9")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "~{PD}")
				(number "8")
			)
		)
		(symbol "OPA858xDSG_0_1"
			(pin no_connect line
				(at -5.08 -5.08 90)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(symbol "OPA858xDSG_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "-")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "+")
				(number "4")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "5")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "FB")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "OPA890xD"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "OPA890xD"
			(at -1.27 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/opa890.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Single Low-Power, Wideband, Voltage-Feedback Operational Amplifier with Disable, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp wideband low-power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "OPA890xD_0_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
		)
		(symbol "OPA890xD_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 5.08 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -5.08 -5.08 90)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "~{DIS}")
				(number "8")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "OPA890xDBV"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "OPA890xDBV"
			(at -1.27 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/opa890.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Single Low-Power, Wideband, Voltage-Feedback Operational Amplifier with Disable, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp wideband low-power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "OPA890xDBV_0_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "2")
			)
		)
		(symbol "OPA890xDBV_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "~{DIS}")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "THS3491xDDA"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "THS3491xDDA"
			(at 10.16 -2.54 0)
		)
		(property "Footprint" "Package_SO:Texas_R-PDSO-G8_EP2.95x4.9mm_Mask2.4x3.1mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ths3491.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "900-MHz, 500-mA High-Power Output Current Feedback Operational Amplifier, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "opamp single current feedback wideband"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*R*PDSO*G8*EP*"
			(at 0 0 0)
		)
		(symbol "THS3491xDDA_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "~{PD}")
				(number "8")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "REF")
				(number "1")
			)
			(pin passive line
				(at 2.54 -7.62 90)
				(length 6.35)
				(name "EP")
				(number "9")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "THS4631DDA"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "THS4631DDA"
			(at 0 3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "www.ti.com/lit/ds/symlink/ths4631.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Single High-voltage, High Slew Rate, Wideband, FET-input Operational Amplifier, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*1EP*3.9x4.9mm*P1.27mm* MSOP*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "THS4631DDA_0_1")
		(symbol "THS4631DDA_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin no_connect line
				(at -2.54 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at 0 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 5.08)
				(name "PAD")
				(number "9")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLV172IDCK"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 2.54 0)
		)
		(property "Value" "TLV172IDCK"
			(at 11.43 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 5.08 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv172.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-power Operational Amplifier, SOT-353"
			(at 0 0 0)
		)
		(property "ki_keywords" "op amp operational amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*353*SC*70*"
			(at 0 0 0)
		)
		(symbol "TLV172IDCK_0_1")
		(symbol "TLV172IDCK_1_1"
			(pin input line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "+")
				(number "1")
			)
			(pin input line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "-")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 3.81)
				(name "V+")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLV9004xRUCR"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TLV9004xRUCR"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_S-PX2QFN-14"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv9004.pdf"
			(at 1.27 5.08 0)
		)
		(property "Description" "Low-Power, Quad-Operational Amplifiers, Texas S-PX2QFN-14"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "quad opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*S*PX2QFN*"
			(at 0 0 0)
		)
		(symbol "TLV9004xRUCR_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "1")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(symbol "TLV9004xRUCR_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(symbol "TLV9004xRUCR_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "9")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "8")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "TLV9004xRUCR_4_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "11")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "12")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "13")
			)
		)
		(symbol "TLV9004xRUCR_5_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLV9061xDPW"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "TLV9061xDPW"
			(at -1.27 3.81 0)
		)
		(property "Footprint" "Package_SON:Texas_X2SON-5_0.8x0.8mm_P0.48mm"
			(at -23.114 -24.892 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv9061.pdf"
			(at 0 -27.686 0)
		)
		(property "Description" "10-MHz, RRIO, CMOS Operational Amplifiers for Cost-Sensitive Systems, X2SON"
			(at -0.254 -22.098 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas?X2SON*0.8x0.8mm*P0.48mm*"
			(at 0 0 0)
		)
		(symbol "TLV9061xDPW_0_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "3")
			)
		)
		(symbol "TLV9061xDPW_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLV9064xRTE"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 5.08 0)
		)
		(property "Value" "TLV9064xRTE"
			(at 8.89 -5.08 0)
		)
		(property "Footprint" "Package_DFN_QFN:WQFN-16-1EP_3x3mm_P0.5mm_EP1.68x1.68mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv9064.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad 10-MHz RRIO CMOS Operational Amplifier, WQFN-N16"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "quad opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WQFN*16*EP1.68x1.68mm*"
			(at 0 0 0)
		)
		(symbol "TLV9064xRTE_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "-")
				(number "16")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "+")
				(number "1")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~{SHDN_12}")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "15")
			)
		)
		(symbol "TLV9064xRTE_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(symbol "TLV9064xRTE_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "-")
				(number "9")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "+")
				(number "10")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~{SHDN_34}")
				(number "7")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(symbol "TLV9064xRTE_4_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "-")
				(number "13")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "+")
				(number "12")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(symbol "TLV9064xRTE_5_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V+")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "V-")
				(number "11")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "V-")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TSV524xIQ4T"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 5.08 0)
		)
		(property "Value" "TSV524xIQ4T"
			(at 5.08 -5.08 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_3x3mm_P0.5mm_EP1.7x1.7mm"
			(at 0 7.62 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/tsv521.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad CMOS Rail-to-Rail Input/Output Amplifier, 1.15MHz GBP, QFN-16"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "quad opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TSV524xIQ4T_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "16")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "15")
			)
		)
		(symbol "TSV524xIQ4T_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(symbol "TSV524xIQ4T_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "9")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "8")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "TSV524xIQ4T_4_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "12")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "13")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(symbol "TSV524xIQ4T_5_1"
			(pin no_connect line
				(at -2.54 2.54 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at -2.54 0 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "EP")
				(number "17")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 3.81)
				(name "V+")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TSV912IQ2T"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TSV912IQ2T"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_2x2mm_P0.5mm_EP1.05x1.75mm"
			(at 0 0 0)
		)
		(property "Datasheet" "www.st.com/resource/en/datasheet/tsv911.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual rail-to-rail input/output 8 MHz operational amplifiers, DFN-8"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TSV912IQ2T_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "TSV912IQ2T_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "TSV912IQ2T_3_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 5.08)
				(name "PAD")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TSV991AILT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 -5.08 0)
		)
		(property "Value" "TSV991AILT"
			(at 2.54 -7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "www.st.com/resource/en/datasheet/tsv991.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "20MHz GBW, RRIO, 2.5..5.5V supply, 820uA single OpAmp, SOT-23-5"
			(at 0 -15.24 0)
		)
		(property "ki_keywords" "low-power micropower st"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TSV991AILT_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "TSV991AILT_2_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 3.81)
				(name "V+")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TSV991AIQ1T"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 -5.08 0)
		)
		(property "Value" "TSV991AIQ1T"
			(at 2.54 -7.62 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6_1.6x1.3mm_P0.4mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "www.st.com/resource/en/datasheet/tsv991.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "20MHz GBW, RRIO, 2.5..5.5V supply, 820uA single OpAmp, DFN-6"
			(at 0 -15.24 0)
		)
		(property "ki_keywords" "low-power micropower st"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DFN*1.6x1.3mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "TSV991AIQ1T_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "1")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(symbol "TSV991AIQ1T_2_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 3.81)
				(name "V+")
				(number "6")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD797"
		(extends "NE5534")
		(property "Reference" "U"
			(at 1.27 6.35 0)
		)
		(property "Value" "AD797"
			(at 1.27 3.81 0)
		)
		(property "Footprint" ""
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD797.pdf"
			(at 1.27 3.81 0)
		)
		(property "Description" "Ultralow Distortion, Ultralow Noise Op Amp, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "AD8001AN"
		(extends "MCP601-xP")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "AD8001AN"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ad8001.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Current Feedback Amplifier, 800 MHz, 50mW, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "AD8001AR"
		(extends "OPA333xxD")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "AD8001AR"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ad8001.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Current Feedback Amplifier, 800 MHz, 50mW, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "AD8021ARM"
		(extends "AD8021AR")
		(property "Reference" "U"
			(at 1.27 7.62 0)
		)
		(property "Value" "AD8021ARM"
			(at 1.27 5.08 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8021.pdf"
			(at 3.81 -1.27 0)
		)
		(property "Description" "Operational Amplifier, 4.5-24V single/dual supply, low noise, high speed, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "AD8606ARM"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "AD8606ARM"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8605_8606_8608.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Precision Low Noise, Low Input Bias Current, Wide Bandwidth Operational Amplifiers, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "AD8606ARZ"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "AD8606ARZ"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8605_8606_8608.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Precision Low Noise, Low Input Bias Current, Wide Bandwidth Operational Amplifiers, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "AD8610xR"
		(extends "LM741")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "AD8610xR"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8610_8620.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Single Precision, Very Low Noise, Low Input Bias Current, Wide Bandwidth JFET Operational Amplifiers, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "AD8610xRM"
		(extends "LM741")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "AD8610xRM"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8610_8620.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Single Precision, Very Low Noise, Low Input Bias Current, Wide Bandwidth JFET Operational Amplifiers, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "AD8620"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "AD8620"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8610_8620.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Precision, Very Low Noise, Low Input Bias Current, Wide Bandwidth JFET Operational Amplifiers, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "AD8620xRM"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "AD8620xRM"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8610_8620.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Precision, Very Low Noise, Low Input Bias Current, Wide Bandwidth JFET Operational Amplifiers, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "AD8655"
		(extends "LM741")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "AD8655"
			(at 0 3.81 0)
		)
		(property "Footprint" ""
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ad8655_8656.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Single Low Noise, Precision CMOS Amplifier"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "AD8656"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "AD8656"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ad8655_8656.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Low Noise, Precision CMOS Amplifier"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "AD8676xR"
		(extends "NCS2325D")
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "AD8676xR"
			(at 2.54 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8676.pdf"
			(at 6.35 3.81 0)
		)
		(property "Description" "Dual operational amplifier, Ultra-precision, 36V, Rail-to-rail output, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp precision high-voltage RRO RTR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADA4075-2"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "ADA4075-2"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/ADA4075-2.pdf"
			(at 0 0 0)
		)
		(property "Description" "Ultralow Noise Amplifier at Lower Power, SOIC-8/LFCSP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual low-power opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADA4077-1xR"
		(extends "OPA333xxD")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "ADA4077-1xR"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADA4077-1_4077-2_4077-4.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "4MHz, 7nV/sqrtHz, Low Offset and Drift, High Precision Amplifier, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADA4077-1xRM"
		(extends "OPA333xxD")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "ADA4077-1xRM"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADA4077-1_4077-2_4077-4.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "4MHz, 7nV/sqrtHz, Low Offset and Drift, High Precision Amplifier, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADA4084-4xCP"
		(extends "ADA4610-4xCP")
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "ADA4084-4xCP"
			(at 2.54 3.81 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-16-1EP_4x4mm_P0.65mm_EP2.6x2.6mm"
			(at 2.54 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADA4084-1_4084-2_4084-4.pdf"
			(at 6.35 3.81 0)
		)
		(property "Description" "30V Quad Low Noise, Rail-to-Rail Input/Output, Low Power Operational Amplifier, LFCSP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "quad opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*4x4mm*P0.65mm*EP2.6x2.6mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADA4099-2xR"
		(extends "NCS2325DM")
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "ADA4099-2xR"
			(at 2.54 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ada4099-1_ada4099-2.pdf"
			(at 6.35 3.81 0)
		)
		(property "Description" "3.15..50V supply, 8MHz GBW, Rail-to-Rail input/output, over-the-top dual opamp, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "operational amplifier analog-devices high-voltage rrio"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADA4099-2xRM"
		(extends "NCS2325DM")
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "ADA4099-2xRM"
			(at 2.54 3.81 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 2.54 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ada4099-1_ada4099-2.pdf"
			(at 6.35 3.81 0)
		)
		(property "Description" "3.15..50V supply, 8MHz GBW, Rail-to-Rail input/output, over-the-top dual opamp, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "operational amplifier analog-devices high-voltage rrio"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADA4522-1"
		(extends "OPA333xxD")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "ADA4522-1"
			(at 0 3.81 0)
		)
		(property "Footprint" ""
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ada4522-1_4522-2_4522-4.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "55 V supply, 5uV max Vos, 3MHz GBW, EMI Enhanced, Zero Drift, 5.8 nV/√Hz, RRO single operational amplifier"
			(at 0 0 0)
		)
		(property "ki_keywords" "analog-devices opamp chopper"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADA4522-2"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "ADA4522-2"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ada4522-1_4522-2_4522-4.pdf"
			(at 0 0 0)
		)
		(property "Description" "55 V supply, 5uV max Vos, 3MHz GBW, EMI Enhanced, Zero Drift, 5.8 nV/√Hz, RRO dual operational amplifiers"
			(at 0 0 0)
		)
		(property "ki_keywords" "analog-devices opamp chopper"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADA4522-4"
		(extends "LM2902")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "ADA4522-4"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at -1.27 2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ada4522-1_4522-2_4522-4.pdf"
			(at 1.27 5.08 0)
		)
		(property "Description" "55 V supply, 5uV max Vos, 3MHz GBW, EMI Enhanced, Zero Drift, 5.8 nV/√Hz, RRO quad operational amplifiers"
			(at 0 0 0)
		)
		(property "ki_keywords" "analog-devices opamp chopper"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADA4610-1xR"
		(extends "OPA333xxD")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "ADA4610-1xR"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADA4610-1_4610-2_4610-4.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Low Noise, Precision, Rail-to-Rail Output, JFET Single Op Amp, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADA4610-1xRJ"
		(extends "MCP6L91T-EOT")
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "ADA4610-1xRJ"
			(at -1.27 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADA4610-1_4610-2_4610-4.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Low Noise, Precision, Rail-to-Rail Output, JFET Single Op Amp, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "ADA4610-2xR"
		(extends "NCS2325D")
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "ADA4610-2xR"
			(at 2.54 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADA4610-1_4610-2_4610-4.pdf"
			(at 6.35 3.81 0)
		)
		(property "Description" "Dual Low Noise, Precision, Rail-to-Rail Output, JFET Op Amp, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADA4610-2xRM"
		(extends "NCS2325DM")
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "ADA4610-2xRM"
			(at 2.54 3.81 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 2.54 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADA4610-1_4610-2_4610-4.pdf"
			(at 6.35 3.81 0)
		)
		(property "Description" "Dual Low Noise, Precision, Rail-to-Rail Output, JFET Op Amp, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADA4610-4xR"
		(extends "OPA4197xD")
		(property "Reference" "U"
			(at 0 3.81 0)
		)
		(property "Value" "ADA4610-4xR"
			(at 0 -3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADA4610-1_4610-2_4610-4.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad Low Noise, Precision, Rail-to-Rail Output, JFET Single Op Amp, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "quad opamp low-power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADA4625-2ARDZ"
		(extends "ADA4898-2")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "ADA4625-2ARDZ"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.29x3mm"
			(at -1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADA4625-1-4625-2.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual 5V..36V/±2.5V..±18V supply, 18 MHz, 48V/µs slew rate, ±80 µV offset, RRO, Fast-settling JFET Op Amp, SOIC-8-1EP"
			(at 0 0 0)
		)
		(property "ki_keywords" "analog-devices adi operational amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADA4807-2ARM"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "ADA4807-2ARM"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADA4807-1_4807-2_4807-4.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Rail-to-Rail Input/Output Amplifiers, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADA4807-4ARUZ"
		(extends "LM2902")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "ADA4807-4ARUZ"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -1.27 2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADA4807-1_4807-2_4807-4.pdf"
			(at 1.27 5.08 0)
		)
		(property "Description" "Quad Rail-to-Rail Input/Output Amplifiers, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "quad opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "CA3080A"
		(extends "CA3080")
		(property "Reference" "U"
			(at 1.27 3.81 0)
		)
		(property "Value" "CA3080A"
			(at 1.27 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/ca30/ca3080-a.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "2MHz, Operational Transconductance Amplifier (OTA), gM spread 1.6:1, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "operational transconductance amplifier ota"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "CA3140"
		(extends "CA3130")
		(property "Reference" "U"
			(at 6.35 5.08 0)
		)
		(property "Value" "CA3140"
			(at 6.35 2.54 0)
		)
		(property "Footprint" ""
			(at -2.54 -2.54 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/intersil/documents/ca31/ca3140-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "4.5MHz, BiMOS Operational Amplifier with MOSFET Input/Bipolar Output, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LF155"
		(extends "LM741")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "LF155"
			(at 0 3.81 0)
		)
		(property "Footprint" ""
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lf357.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Single JFET Input Operational Amplifiers, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single jfet opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LF156"
		(extends "LM741")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "LF156"
			(at 0 3.81 0)
		)
		(property "Footprint" ""
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lf357.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Single JFET Input Operational Amplifiers, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single jfet opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LF256"
		(extends "LM741")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "LF256"
			(at 0 3.81 0)
		)
		(property "Footprint" ""
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lf357.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Single JFET Input Operational Amplifiers, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single jfet opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LF257"
		(extends "LM741")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "LF257"
			(at 0 3.81 0)
		)
		(property "Footprint" ""
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lf357.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Single JFET Input Operational Amplifiers, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single jfet opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LF355"
		(extends "LM741")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "LF355"
			(at 0 3.81 0)
		)
		(property "Footprint" ""
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lf357.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Single JFET Input Operational Amplifiers, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single jfet opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LF356"
		(extends "LM741")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "LF356"
			(at 0 3.81 0)
		)
		(property "Footprint" ""
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lf357.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Single JFET Input Operational Amplifiers, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single jfet opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LF357"
		(extends "LM741")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "LF357"
			(at 0 3.81 0)
		)
		(property "Footprint" ""
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lf357.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Single JFET Input Operational Amplifiers, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single jfet opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM101"
		(extends "NE5534")
		(property "Reference" "U"
			(at 1.27 6.35 0)
		)
		(property "Value" "LM101"
			(at 1.27 3.81 0)
		)
		(property "Footprint" ""
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm101a-n.pdf"
			(at 1.27 3.81 0)
		)
		(property "Description" "Operational Amplifier, DIP-8/TO-99-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm* TO?5*"
			(at 0 0 0)
		)
	)
	(symbol "LM13600"
		(extends "LM13700")
		(property "Reference" "U"
			(at 3.81 5.08 0)
		)
		(property "Value" "LM13600"
			(at 5.08 -5.08 0)
		)
		(property "Footprint" ""
			(at -7.62 0.635 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheet/nationalsemiconductor/DS007980.PDF"
			(at -7.62 0.635 0)
		)
		(property "Description" "Dual Operational Transconductance Amplifiers with Linearizing Diodes and Buffers, DIP-16/SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "operational transconductance amplifier OTA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM201"
		(extends "NE5534")
		(property "Reference" "U"
			(at 1.27 6.35 0)
		)
		(property "Value" "LM201"
			(at 1.27 3.81 0)
		)
		(property "Footprint" ""
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm101a-n.pdf"
			(at 1.27 3.81 0)
		)
		(property "Description" "Operational Amplifier, DIP-8/TO-99-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm* TO?5*"
			(at 0 0 0)
		)
	)
	(symbol "LM301"
		(extends "NE5534")
		(property "Reference" "U"
			(at 1.27 6.35 0)
		)
		(property "Value" "LM301"
			(at 1.27 3.81 0)
		)
		(property "Footprint" ""
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm101a-n.pdf"
			(at 1.27 3.81 0)
		)
		(property "Description" "Operational Amplifier, DIP-8/TO-99-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm* TO?5*"
			(at 0 0 0)
		)
	)
	(symbol "LM318H"
		(extends "LM318M")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "LM318H"
			(at 3.81 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm318-n.pdf"
			(at 0 0 0)
		)
		(property "Description" "Operational Amplifier, TO-99-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99*"
			(at 0 0 0)
		)
	)
	(symbol "LM318N"
		(extends "LM318M")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "LM318N"
			(at 3.81 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm318-n.pdf"
			(at 0 0 0)
		)
		(property "Description" "Operational Amplifier, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99*"
			(at 0 0 0)
		)
	)
	(symbol "LM324"
		(extends "LM2902")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "LM324"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at -1.27 2.54 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2902-n.pdf"
			(at 1.27 5.08 0)
		)
		(property "Description" "Low-Power, Quad-Operational Amplifiers, DIP-14/SOIC-14/SSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "quad opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* DIP*W7.62mm* TSSOP*4.4x5mm*P0.65mm* SSOP*5.3x6.2mm*P0.65mm* MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM324A"
		(extends "LM2902")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "LM324A"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at -1.27 2.54 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2902-n.pdf"
			(at 1.27 5.08 0)
		)
		(property "Description" "Low-Power, Quad-Operational Amplifiers, DIP-14/SOIC-14/SSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "quad opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* DIP*W7.62mm* TSSOP*4.4x5mm*P0.65mm* SSOP*5.3x6.2mm*P0.65mm* MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM358"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "LM358"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2904-n.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Power, Dual Operational Amplifiers, DIP-8/SOIC-8/TO-99-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM358_DFN"
		(extends "TSV912IQ2T")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "LM358_DFN"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_2x2mm_P0.5mm_EP1.05x1.75mm"
			(at 0 0 0)
		)
		(property "Datasheet" "www.st.com/resource/en/datasheet/lm358.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Power, Dual Operational Amplifiers, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM4562"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "LM4562"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4562.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual High-Performance, High-Fidelity Audio Operational Amplifier, DIP-8/SOIC-8/TO-99-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM6142xIx"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "LM6142xIx"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm6142.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Operational Amplifiers, 17MHz, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp rail"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM6144xIx"
		(extends "LM2902")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "LM6144xIx"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at -1.27 2.54 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm6142.pdf"
			(at 1.27 5.08 0)
		)
		(property "Description" "Low-Power, Quad-Operational Amplifiers, 17MHz, DIP-14/SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "quad opamp rail"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM6171D"
		(extends "OPA333xxD")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "LM6171D"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm6171.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "High Speed Low Power Low Distortion Voltage Feedback Amplifier, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM6171xxN"
		(extends "MCP601-xP")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "LM6171xxN"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm6171.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Single High Speed Low Power Low Distortion Voltage Feedback Amplifier, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM6172"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "LM6172"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm6172.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual High Speed, Low Power, Low Distortion, Voltage Feedback Amplifiers, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM7332"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "LM7332"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm7332.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Rail-to-Rail Input and Output 30-V, Wide Voltage Range, High Output, Operational Amplifier, SOIC-8/SSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM8261"
		(extends "MCP6L91T-EOT")
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "LM8261"
			(at -1.27 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm8261.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Single Opamp, Rail-to-Rail Input/Output, Unlimited Capacitive Load Drive, +53mA/-75mA Output Current, 2.5-30V, 350uV offset, 12MHz GBW, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "RRIO CapLoad gate driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LMC6062"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "LMC6062"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmc6062.pdf"
			(at 0 0 0)
		)
		(property "Description" "Precision CMOS Dual Micropower Operational Amplifier, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LMC6082"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "LMC6082"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmc6082.pdf"
			(at 0 0 0)
		)
		(property "Description" "Precision CMOS Dual Operational Amplifier, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LMC6482"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "LMC6482"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmc6482.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual CMOS Rail-to-Rail Input and Output Operational Amplifier, DIP-8/SOIC-8, SSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LMC6484"
		(extends "LM2902")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "LMC6484"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at -1.27 2.54 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmc6484.pdf"
			(at 1.27 5.08 0)
		)
		(property "Description" "Quad CMOS Rail-to-Rail Input and Output Operational Amplifier, DIP-14/SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "quad opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* DIP*W7.62mm* TSSOP*4.4x5mm*P0.65mm* SSOP*5.3x6.2mm*P0.65mm* MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LMH6609MA"
		(extends "OPA333xxD")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "LMH6609MA"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmh6609.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "900MHz Voltage Feedback Op Amp, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "opamp single wideband unity-gain stable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LMH6609MF"
		(extends "MCP6L91T-EOT")
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "LMH6609MF"
			(at -1.27 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmh6609.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "900MHz Voltage Feedback Op Amp, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "opamp single wideband unity-gain stable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LMH6702MA"
		(extends "OPA333xxD")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "LMH6702MA"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmh6702.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "1.7 GHz Ultra-Low Distortion Wideband Op Amp, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "opamp single low distortion wideband"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LMH6702MF"
		(extends "MCP6L91T-EOT")
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "LMH6702MF"
			(at -1.27 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmh6702.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "1.7 GHz Ultra-Low Distortion Wideband Op Amp, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "opamp single low distortion wideband"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LMV324"
		(extends "LM2902")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "LMV324"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at -1.27 2.54 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmv324.pdf"
			(at 1.27 5.08 0)
		)
		(property "Description" "Quad Low-Voltage Rail-to-Rail Output Operational Amplifier, SOIC-14/SSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "quad opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* DIP*W7.62mm* TSSOP*4.4x5mm*P0.65mm* SSOP*5.3x6.2mm*P0.65mm* MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LMV358"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "LMV358"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmv324.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Low-Voltage Rail-to-Rail Output Operational Amplifiers, SOIC-8/SSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPV811DBV"
		(extends "MCP6L91T-EOT")
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "LPV811DBV"
			(at -1.27 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lpv812.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Single operational amplifier, 8kHz GBW, 425 nA/channel quiescent, 100 fA input bias, 300 uV offset max, 1 uV/C, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp low-power rail-to-rail"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LPV812DGK"
		(extends "OPA2197xDGK")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "LPV812DGK"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lpv812.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual operational amplifier, 8kHz GBW, 425 nA/channel quiescent, 100 fA input bias, 300 uV offset max, 1 uV/C, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp low-power rail-to-rail"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1012"
		(extends "NE5534")
		(property "Reference" "U"
			(at 1.27 6.35 0)
		)
		(property "Value" "LT1012"
			(at 1.27 3.81 0)
		)
		(property "Footprint" ""
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/lt1012.pdf"
			(at 1.27 3.81 0)
		)
		(property "Description" "Single Picoamp Input Current, Microvolt Offset, Low Noise Op Amp, DIP-8/SOIC-8/TO-5-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm* TO?5*"
			(at 0 0 0)
		)
	)
	(symbol "LT1363"
		(extends "OP07")
		(property "Reference" "U"
			(at 1.27 6.35 0)
		)
		(property "Value" "LT1363"
			(at 1.27 3.81 0)
		)
		(property "Footprint" ""
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1363fa.pdf"
			(at 1.27 3.81 0)
		)
		(property "Description" "70MHz, 1000V/µs Operational Amplifier, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm* TO*99*"
			(at 0 0 0)
		)
	)
	(symbol "LT1492"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "LT1492"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/14923f.pdf"
			(at 0 0 0)
		)
		(property "Description" "5MHz, 3V/µs, Low Power, Single Supply, Dual Precision Op Amps, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1493"
		(extends "LTC6082xGN")
		(property "Reference" "U"
			(at 2.54 5.08 0)
		)
		(property "Value" "LT1493"
			(at 5.08 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/14923f.pdf"
			(at 0 0 0)
		)
		(property "Description" "5MHz, 3V/µs, Low Power, Single Supply, Quad Precision Op Amps, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "quad opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*3.9x4.9mm*P0.635mm* SOIC*3.9x9.9mm*P1.27mm* QSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT6015xS5"
		(extends "MCP6L91T-EOT")
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "LT6015xS5"
			(at -1.27 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/601567ff.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "3.2MHz, 0.8V/us, Low Power, Over-The-Top Precision Op Amp, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LT6234"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "LT6234"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/623345fc.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual 60MHz, Rail-to-Rail Output, 1.9nV/√Hz, 1.2mA, Operational Amplifier, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT6237"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "LT6237"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/623637fb.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual 215MHz, Rail-to-Rail Output, 1.1nV/√Hz, 3.5mA, Operational Amplifier, MSOP-8/DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC6081xMS8"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "LTC6081xMS8"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/60812fd.pdf"
			(at 0 0 0)
		)
		(property "Description" "Precision Dual CMOS Rail-to-Rail Input/Output Amplifiers, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC6253xMS8"
		(extends "NCS2325DM")
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "LTC6253xMS8"
			(at 2.54 3.81 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 2.54 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/625234fc.pdf"
			(at 6.35 3.81 0)
		)
		(property "Description" "720MHz, 3.5mA Power Efficient, Rail-to-Rail Op Amp, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp low-power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC6269xDD"
		(extends "LTC6229xDD")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "LTC6269xDD"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-10-1EP_3x3mm_P0.5mm_EP1.65x2.38mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/62689f.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual 500MHz Ultra-Low Bias  Current FET Input Op Amps with Shutdown, DFN-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DFN*1EP*3x3mm*P0.5mm*EP1.65x2.38mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC6269xMS8E"
		(extends "LTC6229xMS8E")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "LTC6269xMS8E"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:MSOP-8-1EP_3x3mm_P0.65mm_EP1.68x1.88mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/62689f.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual 500MHz Ultra-Low Bias  Current FET Input Op Amps, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX4239ASA"
		(extends "MAX4238ASA")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "MAX4239ASA"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX4238-MAX4239.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Ultra-Low Offset/Drift, Low-Noise, Precision Amplifiers, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX4239AUT"
		(extends "MAX4238AUT")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "MAX4239AUT"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX4238-MAX4239.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Ultra-Low Offset/Drift, Low-Noise, Precision Amplifiers, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX4395ESD"
		(extends "LM2902")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "MAX4395ESD"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:SO-14_3.9x8.65mm_P1.27mm"
			(at -1.27 2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX4389-MAX4396.pdf"
			(at 1.27 5.08 0)
		)
		(property "Description" "Ultra-Small, Low-Cost, 85MHz Quad Op Amp with Rail-to-Rail Outputs"
			(at 0 0 0)
		)
		(property "ki_keywords" "quad opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*3.9x8.65mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX4395EUD"
		(extends "LM2902")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "MAX4395EUD"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -1.27 2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX4389-MAX4396.pdf"
			(at 1.27 5.08 0)
		)
		(property "Description" "Ultra-Small, Low-Cost, 85MHz Quad Op Amp with Rail-to-Rail Outputs"
			(at 0 0 0)
		)
		(property "ki_keywords" "quad opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC33078"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "MC33078"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC33078-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Low Noise, Dual Operational Amplifiers, DIP-8/SOIC-8/SSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC33079"
		(extends "LM2902")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "MC33079"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at -1.27 2.54 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC33078-D.PDF"
			(at 1.27 5.08 0)
		)
		(property "Description" "Low Noise, Quad Operational Amplifiers, DIP-14/SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "quad opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* DIP*W7.62mm* TSSOP*4.4x5mm*P0.65mm* SSOP*5.3x6.2mm*P0.65mm* MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC33172"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "MC33172"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/MC33171-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Dual Single Supply 3.0V to 44V, Low Power Operational Amplifiers, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC33174"
		(extends "LM2902")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "MC33174"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at -1.27 2.54 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/MC33171-D.PDF"
			(at 1.27 5.08 0)
		)
		(property "Description" "Quad Single Supply 3.0V to 44V, Low Power Operational Amplifiers, DIP-14/SOIC-14/TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "quad opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* DIP*W7.62mm* TSSOP*4.4x5mm*P0.65mm* SSOP*5.3x6.2mm*P0.65mm* MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC33178"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "MC33178"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC33178-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Dual Low Power, Low Noise Operational Amplifiers, DIP-8/SOIC-8/SSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC33179"
		(extends "LM2902")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "MC33179"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at -1.27 2.54 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC33178-D.PDF"
			(at 1.27 5.08 0)
		)
		(property "Description" "Quad Low Power, Low Noise Operational Amplifiers, DIP-14/SOIC-14/SSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "quad opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* DIP*W7.62mm* TSSOP*4.4x5mm*P0.65mm* SSOP*5.3x6.2mm*P0.65mm* MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP6001-OT"
		(extends "MCP6L91T-EOT")
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "MCP6001-OT"
			(at -1.27 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/MCP6001-1R-1U-2-4-1-MHz-Low-Power-Op-Amp-DS20001733L.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "1MHz, Low-Power Op Amp, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP6001U"
		(extends "LMV321")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "MCP6001U"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/MCP6001-1R-1U-2-4-1-MHz-Low-Power-Op-Amp-DS20001733L.pdf"
			(at 0 0 0)
		)
		(property "Description" "1MHz, Low-Power Op Amp, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* *SC*70*"
			(at 0 0 0)
		)
	)
	(symbol "MCP6002-xMS"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "MCP6002-xMS"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21733j.pdf"
			(at 0 0 0)
		)
		(property "Description" "1MHz, Low-Power Op Amp, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP6002-xP"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "MCP6002-xP"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21733j.pdf"
			(at 0 0 0)
		)
		(property "Description" "1MHz, Low-Power Op Amp, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP6002-xSN"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "MCP6002-xSN"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21733j.pdf"
			(at 0 0 0)
		)
		(property "Description" "1MHz, Low-Power Op Amp, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP6004"
		(extends "LM2902")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "MCP6004"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at -1.27 2.54 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21733j.pdf"
			(at 1.27 5.08 0)
		)
		(property "Description" "1MHz, Low-Power Op Amp, DIP-14/SOIC-14/TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "quad opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* DIP*W7.62mm* TSSOP*4.4x5mm*P0.65mm* SSOP*5.3x6.2mm*P0.65mm* MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP601-xOT"
		(extends "MCP6L91T-EOT")
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "MCP601-xOT"
			(at -1.27 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21314g.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Single 2.7V to 6.0V Single Supply CMOS Op Amps, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP601-xSN"
		(extends "OPA333xxD")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "MCP601-xSN"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21314g.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Single 2.7V to 6.0V Single Supply CMOS Op Amps, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP601R"
		(extends "MCP6001R")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "MCP601R"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/21314g.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Single 2.7V to 6.0V Single Supply CMOS Op Amps, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP602"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "MCP602"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21314g.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual 2.7V to 6.0V Single Supply CMOS Op Amps, DIP-8/SOIC-8/TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP6022"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "MCP6022"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/20001685e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Operational Amplifiers, Rail-to-Rail Input/Output, DIP-8/SOIC-8/TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp rail-to-rail"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP603-xSN"
		(extends "MCP603-xP")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "MCP603-xSN"
			(at 0 3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21314g.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Single 2.7V to 6.0V Single Supply CMOS Op Amps, with Chip Select, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm* TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP603-xST"
		(extends "MCP603-xP")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "MCP603-xST"
			(at 0 3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21314g.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Single 2.7V to 6.0V Single Supply CMOS Op Amps, with Chip Select, TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm* TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP604"
		(extends "LM2902")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "MCP604"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at -1.27 2.54 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21314g.pdf"
			(at 1.27 5.08 0)
		)
		(property "Description" "Quad 2.7V to 6.0V Single Supply CMOS Op Amps, DIP-14/SOIC-14/TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "quad opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* DIP*W7.62mm* TSSOP*4.4x5mm*P0.65mm* SSOP*5.3x6.2mm*P0.65mm* MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP6401RT-xOT"
		(extends "MCP6001R")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "MCP6401RT-xOT"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/22229d.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "1 MHz, 45 µA Op Amps, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP6401T-xLT"
		(extends "MCP6001x-LT")
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "MCP6401T-xLT"
			(at -1.27 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/22229d.pdf"
			(at 0 0 0)
		)
		(property "Description" "1 MHz, 45 µA Op Amps, SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "MCP6401T-xOT"
		(extends "MCP6L91T-EOT")
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "MCP6401T-xOT"
			(at -1.27 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/22229d.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "1 MHz, 45 µA Op Amps, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP6401UT-xOT"
		(extends "LMV321")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "MCP6401UT-xOT"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/22229d.pdf"
			(at 0 0 0)
		)
		(property "Description" "1 MHz, 45 µA Op Amps, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* *SC*70*"
			(at 0 0 0)
		)
	)
	(symbol "MCP6L01Rx-xOT"
		(extends "MCP6001R")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "MCP6L01Rx-xOT"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/MSLD/ProductDocuments/DataSheets/MCP6L01-1R-1U-2-4-1-MHz-85-uA-Op-Amps-DS20002140D.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Single, 1 MHz, 85µA, Rail-to-Rail input and output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "opamp vfa r2r rtr"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP6L01Ux-xOT"
		(extends "LM321")
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "MCP6L01Ux-xOT"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/22140b.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single, 1 MHz, 85µA, Rail-to-Rail input and output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "opamp vfa r2r rtr"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP6L01x-xLT"
		(extends "MCP6001x-LT")
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "MCP6L01x-xLT"
			(at -1.27 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/22140b.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single, 1 MHz, Rail-to-Rail input and output, SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "opamp vfa r2r rtr"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "MCP6L01x-xOT"
		(extends "MCP6L91T-EOT")
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "MCP6L01x-xOT"
			(at -1.27 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/22140b.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Single, 1 MHz, 85µA, Rail-to-Rail input and output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "opamp vfa rtr r2r"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP6L02x-xMS"
		(extends "NCS2325DM")
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "MCP6L02x-xMS"
			(at 2.54 3.81 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 2.54 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/22140b.pdf"
			(at 6.35 3.81 0)
		)
		(property "Description" "Dual, 1 MHz, 85µA, Rail-to-Rail input and output, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "opamp vfa r2r rtr"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP6L02x-xSN"
		(extends "NCS2325D")
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "MCP6L02x-xSN"
			(at 2.54 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/22140b.pdf"
			(at 6.35 3.81 0)
		)
		(property "Description" "Dual, 1 MHz, 85µA, Rail-to-Rail input and output SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "opamp vfa r2r rtr"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP6L04-xST"
		(extends "OPA4197xPW")
		(property "Reference" "U"
			(at 0 3.81 0)
		)
		(property "Value" "MCP6L04-xST"
			(at 0 -3.81 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/22140b.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad, 1 MHz, 85µA, Rail-to-Rail input and output, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "opamp vfa r2r rtr"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP6L04x-xSL"
		(extends "OPA4197xD")
		(property "Reference" "U"
			(at 0 3.81 0)
		)
		(property "Value" "MCP6L04x-xSL"
			(at 0 -3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/22140b.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad, 1 MHz, 85µA, Rail-to-Rail input and output, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "opamp vfa r2r rtr"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP6L91RT-EOT"
		(extends "MCP6001R")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "MCP6L91RT-EOT"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/MSLD/ProductDocuments/DataSheets/MCP6L91-1R-2-4-Data-Sheet-DS20002141C.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "10 MHz, 850 µA Op Amps, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP6L92"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "MCP6L92"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22141b.pdf"
			(at 0 0 0)
		)
		(property "Description" "10 MHz, 850 µA Op Amps, SOIC-8/MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP6L94"
		(extends "LM2902")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "MCP6L94"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at -1.27 2.54 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22141b.pdf"
			(at 1.27 5.08 0)
		)
		(property "Description" "10 MHz, 850 µA Op Amps, SOIC-14/TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "quad opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* DIP*W7.62mm* TSSOP*4.4x5mm*P0.65mm* SSOP*5.3x6.2mm*P0.65mm* MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP6V67EMS"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "MCP6V67EMS"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MCP6V66-Family-Data-Sheet-DS20006266A.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Operational Amplifiers, Zero-Drift, 80 kHz Bandwidth, 1.8V to 5.5V, Rail-to-Rail, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp zero drift"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCS20072D"
		(extends "NCS2325D")
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "NCS20072D"
			(at 2.54 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCS20071-D.PDF"
			(at 6.35 3.81 0)
		)
		(property "Description" "Dual, 2.8V/µs, Rail-to-Rail Output, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual rail-to-rail output opamp vfa"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCS20072DM"
		(extends "NCS2325DM")
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "NCS20072DM"
			(at 2.54 3.81 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 2.54 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCS20071-D.PDF"
			(at 6.35 3.81 0)
		)
		(property "Description" "Dual, 2.8V/µs, Rail-to-Rail Output, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual rail-to-rail output opamp vfa"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCS20074D"
		(extends "NCS4325")
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "NCS20074D"
			(at 2.54 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 2.54 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCS20071-D.PDF"
			(at 6.35 3.81 0)
		)
		(property "Description" "Quad, 2.8V/µs, Rail-to-Rail Output, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "quad rail-to-rail output opamp vfa"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "NE5532"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "NE5532"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ne5532.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Low-Noise Operational Amplifiers, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "NJM2043"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "NJM2043"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.njr.com/semicon/PDF/NJM2043_E.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Low Noise Pre-Amplifier, DIP-8/DMP-8/SIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "NJM2114"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "NJM2114"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.njr.com/semicon/PDF/NJM2114_E.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual High Performance Low Noise Operational Amplifier, DIP-8/DMP-8/SIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "NJM4556A"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "NJM4556A"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.njr.com/semicon/PDF/NJM4556A_E.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual High Current Operational Amplifier, DIP-8/DMP-8/SIP-8/SSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "NJM4558"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "NJM4558"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.njr.com/semicon/PDF/NJM4558_NJM4559_E.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Operational Amplifier, DIP-8/DMP-8/SIP-8/SOP-8/SSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "NJM4559"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "NJM4559"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.njr.com/semicon/PDF/NJM4558_NJM4559_E.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Operational Amplifier, DIP-8/DMP-8/SIP-8/SOP-8/SSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "NJM4560"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "NJM4560"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.njr.com/semicon/PDF/NJM4560_E.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Operational Amplifier, DIP-8/DMP-8/SIP-8/SOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "NJM4580"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "NJM4580"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.njr.com/semicon/PDF/NJM4580_E.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Operational Amplifier, DIP-8/DMP-8/SIP-8/MSOP-8/SOP-8/SSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "NJM5532"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "NJM5532"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.njr.com/semicon/PDF/NJM5532_E.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Low-Noise Operational Amplifier, DIP-8/DMP-8/SIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "OP249"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "OP249"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/OP249.pdf"
			(at 0 0 0)
		)
		(property "Description" "Precision JFET, High Speed, Dual Operational Amplifier, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "OP275"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "OP275"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/OP275.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Bipolar/JFET, Audio Operational Amplifier, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "OP77"
		(extends "OP07")
		(property "Reference" "U"
			(at 1.27 6.35 0)
		)
		(property "Value" "OP77"
			(at 1.27 3.81 0)
		)
		(property "Footprint" ""
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/OP77.pdf"
			(at 1.27 3.81 0)
		)
		(property "Description" "Next Generation OP07 Ultralow Offset Voltage Operational Amplifier, DIP-8/TO-99-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm* TO*99*"
			(at 0 0 0)
		)
	)
	(symbol "OPA121KM"
		(extends "OPA121KU")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "OPA121KM"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-99-8"
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "https://www.alldatasheet.com/datasheet-pdf/pdf/56725/BURR-BROWN/OPA121.html"
			(at 3.81 3.81 0)
		)
		(property "Description" "Operational Amplifier, TO-99"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp BURR-BROWN Texas Instruments"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TO*99*"
			(at 0 0 0)
		)
	)
	(symbol "OPA121KP"
		(extends "OPA121KU")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "OPA121KP"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "https://www.alldatasheet.com/datasheet-pdf/pdf/56725/BURR-BROWN/OPA121.html"
			(at 3.81 3.81 0)
		)
		(property "Description" "Operational Amplifier, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp BURR-BROWN Texas Instruments"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA134"
		(extends "OP07")
		(property "Reference" "U"
			(at 1.27 6.35 0)
		)
		(property "Value" "OPA134"
			(at 1.27 3.81 0)
		)
		(property "Footprint" ""
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa134.pdf"
			(at 1.27 3.81 0)
		)
		(property "Description" "Single SoundPlus High Performance Audio Operational Amplifiers, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm* TO*99*"
			(at 0 0 0)
		)
	)
	(symbol "OPA1602"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "OPA1602"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa1604.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual SoundPlus High Performance, Bipolar-Input Audio Operational Amplifiers, SOIC-8/MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA1604"
		(extends "LM2902")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "OPA1604"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at -1.27 2.54 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa1604.pdf"
			(at 1.27 5.08 0)
		)
		(property "Description" "Quad SoundPlus High Performance, Bipolar-Input Audio Operational Amplifiers, SOIC-14/TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "quad opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* DIP*W7.62mm* TSSOP*4.4x5mm*P0.65mm* SSOP*5.3x6.2mm*P0.65mm* MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA1612AxD"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "OPA1612AxD"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa1612.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual SoundPlus High Performance, Bipolar-Input Audio Operational Amplifiers, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA1655D"
		(extends "OPA333xxD")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "OPA1655D"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/opa1655.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Single Ultra-Low-Noise, Low-Distortion, FET-Input, Burr-Brown Audio Operational Amplifiers, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA1655DBV"
		(extends "MCP6L91T-EOT")
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "OPA1655DBV"
			(at -1.27 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/opa1655.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Single Ultra-Low-Noise, Low-Distortion, FET-Input, Burr-Brown Audio Operational Amplifiers, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "OPA1656ID"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "OPA1656ID"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/opa1656.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Ultra-Low-Noise, Low-Distortion, FET-Input, Burr-Brown Audio Operational Amplifiers, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA1678"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "OPA1678"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa1678.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Distortion Audio Operational Amplifiers, SOIC-8/VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA1679"
		(extends "LM2902")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "OPA1679"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at -1.27 2.54 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa1678.pdf"
			(at 1.27 5.08 0)
		)
		(property "Description" "Low-Distortion Audio Operational Amplifiers, SOIC-14/TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "quad opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* DIP*W7.62mm* TSSOP*4.4x5mm*P0.65mm* SSOP*5.3x6.2mm*P0.65mm* MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA1692xD"
		(extends "NCS2325D")
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "OPA1692xD"
			(at 2.54 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/opa1692.pdf"
			(at 6.35 3.81 0)
		)
		(property "Description" "Dual SoundPlus Low Power, Low Noise & Low Distortion Audio Operational Amplifiers, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "VFA opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA1692xDGK"
		(extends "OPA2197xDGK")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "OPA1692xDGK"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/opa1692.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual SoundPlus Low Power, Low Noise & Low Distortion Audio Operational Amplifiers, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "VFA opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA188xxD"
		(extends "OPA333xxD")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "OPA188xxD"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa188.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Precision, Low-Noise, Rail-to-Rail Output, 36-V, Zero-Drift Operational Amplifier, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp zero-drift"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA188xxDBV"
		(extends "AD8603")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "OPA188xxDBV"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa188.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Zero-Drift, Precision, Low-Noise, Rail-to-Rail Output, 36-V Operational Amplifier, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp zero-drift"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT*23*"
			(at 0 0 0)
		)
	)
	(symbol "OPA196xD"
		(extends "OPA333xxD")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "OPA196xD"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa4196.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Sing, Low-Power, Low Offset Voltage, Rail-to-Rail Operational Amplifier, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA196xDBV"
		(extends "MCP6L91T-EOT")
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "OPA196xDBV"
			(at -1.27 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa4196.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Single, Low-Power, Low Offset Voltage, Rail-to-Rail Operational Amplifier, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "OPA196xDGK"
		(extends "OPA197xDGK")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "OPA196xDGK"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa4196.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Single, Low-Power, Low Offset Voltage, Rail-to-Rail Operational Amplifier, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp rtor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA197xD"
		(extends "OPA333xxD")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "OPA197xD"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa197.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Single 36V, Precision, Rail-to-Rail Input/Output, Low Offset Voltage, Operational Amplifier, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp rtor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA197xDBV"
		(extends "MCP6L91T-EOT")
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "OPA197xDBV"
			(at -1.27 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa197.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Single 36V, Precision, Rail-to-Rail Input/Output, Low Offset Voltage, Operational Amplifier, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp rtor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "OPA2134"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "OPA2134"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa134.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual SoundPlus High Performance Audio Operational Amplifiers, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA2156xD"
		(extends "NCS2325D")
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "OPA2156xD"
			(at 2.54 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/opa2156.pdf"
			(at 6.35 3.81 0)
		)
		(property "Description" "Dual 36V, Ultra Low Noise, Rail-to-Rail Input/Output, Low Offset Voltage, Operational Amplifier, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp low-noise r2r"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA2156xDGK"
		(extends "OPA2197xDGK")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "OPA2156xDGK"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa2156.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual 36V, Ultra Low Noise, Rail-to-Rail Input/Output, Low Offset Voltage, Operational Amplifier, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp low-noise r2r"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA2196xD"
		(extends "NCS2325D")
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "OPA2196xD"
			(at 2.54 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa4196.pdf"
			(at 6.35 3.81 0)
		)
		(property "Description" "Dual, Low-Power, Low Offset Voltage, Rail-to-Rail Operational Amplifier, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp low-power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA2196xDGK"
		(extends "OPA2197xDGK")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "OPA2196xDGK"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa4196.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual, Low-Power, Low Offset Voltage, Rail-to-Rail Operational Amplifier, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp rtor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA2197xD"
		(extends "NCS2325D")
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "OPA2197xD"
			(at 2.54 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa2197.pdf"
			(at 6.35 3.81 0)
		)
		(property "Description" "Dual 36V, Precision, Rail-to-Rail Input/Output, Low Offset Voltage, Operational Amplifier, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp rtor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA2277"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "OPA2277"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/opa2277.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual High Precision Operational Amplifiers, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA2333xxD"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "OPA2333xxD"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa333.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual 1.8V, microPower, CMOS Operational Amplifiers, Zero-Drift Series, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA2333xxDGK"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "OPA2333xxDGK"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa333.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual 1.8V, microPower, CMOS Operational Amplifiers, Zero-Drift Series, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA2340"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "OPA2340"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa4340.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Single-Supply, Rail-to-Rail Operational Amplifiers, MicroAmplifier Series, DIP-8/SOIC-8/SSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA2356xxD"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "OPA2356xxD"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa2356.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual High Speed CMOS Operational Amplifiers, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA2356xxDGK"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "OPA2356xxDGK"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa2356.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual High Speed CMOS Operational Amplifiers, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA2376xxD"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "OPA2376xxD"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa376.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Low-Noise, Low Quiescent Current, Precision Operational Amplifier e-trim Series, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA2376xxDGK"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "OPA2376xxDGK"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa376.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Low-Noise, Low Quiescent Current, Precision Operational Amplifier e-trim Series, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA2691"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "OPA2691"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/sbos224d/sbos224d.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Wideband, Current-Feedback Operational Amplifier, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual current feedback opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA2890ID"
		(extends "OPA2197xDGK")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "OPA2890ID"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:SO-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/opa2890.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Power, Wideband, Voltage-Feedback Operational Amplifier, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SO*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA2994xD"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "OPA2994xD"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -1.27 2.54 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/opa2994.pdf"
			(at 1.27 5.08 0)
		)
		(property "Description" "Dual Opamp, Rail-to-Rail Input/Output, Unlimited Capacitive Load Drive, 125mA Output Current, 2-32V, 350uV offset, 24MHz GBW, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "high-output-current rrio"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA310SxDBV"
		(extends "LTC6228xS6")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "OPA310SxDBV"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/opa310.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Rail-to-Rail Input/Output Operational Amplifier with Shutdown, 1.5..5.5V supply, 3MHz GBW, 250uV offset voltage, 150mA output current, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp "
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "OPA310xDBV"
		(extends "MCP6L91T-EOT")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "OPA310xDBV"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/opa2310.pdf"
			(at 0 0 0)
		)
		(property "Description" "High output current, Rail-to-Rail Input/Output, 3MHz GBW, Operational Amplifiers, integrated RFI/EMI filter, 1.5V to 5.5V supply, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp rrio"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "OPA310xDCK"
		(extends "LMV321")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "OPA310xDCK"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/opa2310.pdf"
			(at 0 0 0)
		)
		(property "Description" "High output current, Rail-to-Rail Input/Output, 3MHz GBW, Operational Amplifiers, integrated RFI/EMI filter, 1.5V to 5.5V supply, SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp rrio"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC*70*"
			(at 0 0 0)
		)
	)
	(symbol "OPA330xxD"
		(extends "OPA333xxD")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "OPA330xxD"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa330.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "50μV V OS, 0.25μV/°C, 35μA CMOS OPERATIONAL AMPLIFIERS, Zerø-Drift Series, SOIC"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA330xxDBV"
		(extends "MCP6L91T-EOT")
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "OPA330xxDBV"
			(at -1.27 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa330.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "50μV V OS, 0.25μV/°C, 35μA CMOS OPERATIONAL AMPLIFIERS, Zerø-Drift Series, SOT"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "OPA330xxDCK"
		(extends "LMV321")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "OPA330xxDCK"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa330.pdf"
			(at 0 0 0)
		)
		(property "Description" "50μV V OS, 0.25μV/°C, 35μA CMOS OPERATIONAL AMPLIFIERS, Zerø-Drift Series, SC70"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* *SC*70*"
			(at 0 0 0)
		)
	)
	(symbol "OPA333xxDBV"
		(extends "MCP6L91T-EOT")
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "OPA333xxDBV"
			(at -1.27 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa333.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Single 1.8V, microPower, CMOS Operational Amplifiers, Zero-Drift Series, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "OPA333xxDCK"
		(extends "LMV321")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "OPA333xxDCK"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa333.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single 1.8V, microPower, CMOS Operational Amplifiers, Zero-Drift Series, SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC*70*"
			(at 0 0 0)
		)
	)
	(symbol "OPA336Nx"
		(extends "MCP6L91T-EOT")
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "OPA336Nx"
			(at -1.27 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/opa2336.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "100 KHz, microPower CMOS, Op Amps, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp rail"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "OPA336Ux"
		(extends "OPA333xxD")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "OPA336Ux"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:SO-8_3.9x4.9mm_P1.27mm"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/opa2336.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "100 KHz, microPower CMOS, Op Amps, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp rail"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA340NA"
		(extends "MCP6L91T-EOT")
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "OPA340NA"
			(at -1.27 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa340.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Single Single-Supply, Rail-to-Rail Operational Amplifier, MicroAmplifier Series, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "OPA340P"
		(extends "MCP601-xP")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "OPA340P"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa340.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Single Single-Supply, Rail-to-Rail Operational Amplifier, MicroAmplifier Series, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA340UA"
		(extends "OPA333xxD")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "OPA340UA"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa340.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Single Single-Supply, Rail-to-Rail Operational Amplifier, MicroAmplifier Series, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA356xxD"
		(extends "OPA333xxD")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "OPA356xxD"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa356.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Single High Speed CMOS Operational Amplifier, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA356xxDBV"
		(extends "MCP6L91T-EOT")
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "OPA356xxDBV"
			(at -1.27 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa356.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Single High Speed CMOS Operational Amplifier, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "OPA365xxD"
		(extends "OPA333xxD")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "OPA365xxD"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa365.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "50-MHz, Zero-Crossover, Low-Distortion, High CMRR, RRI/O, Single-Supply, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA365xxDBV"
		(extends "MCP6L91T-EOT")
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "OPA365xxDBV"
			(at -1.27 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/opa365.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "50-MHz, Zero-Crossover, Low-Distortion, High CMRR, RRI/O, Single-Supply, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "OPA376xxD"
		(extends "OPA333xxD")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "OPA376xxD"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa376.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Single Low-Noise, Low Quiescent Current, Precision Operational Amplifier e-trim Series, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA376xxDBV"
		(extends "MCP6L91T-EOT")
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "OPA376xxDBV"
			(at -1.27 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa376.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Single Low-Noise, Low Quiescent Current, Precision Operational Amplifier e-trim Series, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "OPA376xxDCK"
		(extends "LMV321")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "OPA376xxDCK"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa376.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Low-Noise, Low Quiescent Current, Precision Operational Amplifier e-trim Series, SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* *SC*70*"
			(at 0 0 0)
		)
	)
	(symbol "OPA4134"
		(extends "LM2902")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "OPA4134"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at -1.27 2.54 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa134.pdf"
			(at 1.27 5.08 0)
		)
		(property "Description" "Quad SoundPlus High Performance Audio Operational Amplifiers, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "quad opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* DIP*W7.62mm* TSSOP*4.4x5mm*P0.65mm* SSOP*5.3x6.2mm*P0.65mm* MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA4196xD"
		(extends "OPA4197xD")
		(property "Reference" "U"
			(at 0 3.81 0)
		)
		(property "Value" "OPA4196xD"
			(at 0 -3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa4196.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad, Low-Power, Low Offset Voltage, Rail-to-Rail Operational Amplifier, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "quad opamp rtor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA4196xPW"
		(extends "OPA4197xPW")
		(property "Reference" "U"
			(at 0 3.81 0)
		)
		(property "Value" "OPA4196xPW"
			(at 0 -3.81 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa4196.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad, Low-Power, Low Offset Voltage, Rail-to-Rail Operational Amplifier, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "quad opamp rtor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA4340EA"
		(extends "LTC6082xGN")
		(property "Reference" "U"
			(at 2.54 5.08 0)
		)
		(property "Value" "OPA4340EA"
			(at 5.08 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa340.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad Single-Supply, Rail-to-Rail Operational Amplifier, MicroAmplifier Series, SSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "quad opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*3.9x4.9mm*P0.635mm* SOIC*3.9x9.9mm*P1.27mm* QSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA4340UA"
		(extends "LM2902")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "OPA4340UA"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at -1.27 2.54 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa340.pdf"
			(at 1.27 5.08 0)
		)
		(property "Description" "Quad Single-Supply, Rail-to-Rail Operational Amplifier, MicroAmplifier Series, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "quad opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* DIP*W7.62mm* TSSOP*4.4x5mm*P0.65mm* SSOP*5.3x6.2mm*P0.65mm* MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA4376"
		(extends "LM2902")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "OPA4376"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at -1.27 2.54 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa376.pdf"
			(at 1.27 5.08 0)
		)
		(property "Description" "Quad Low-Noise, Low Quiescent Current, Precision Operational Amplifier e-trim Series, SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "quad opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* DIP*W7.62mm* TSSOP*4.4x5mm*P0.65mm* SSOP*5.3x6.2mm*P0.65mm* MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA552P"
		(extends "OPA551P")
		(property "Reference" "U"
			(at 5.08 7.62 0)
		)
		(property "Value" "OPA552P"
			(at 5.08 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 5.08 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa552.pdf"
			(at 31.75 -2.54 0)
		)
		(property "Description" "High-Voltage High-Current Operational Amplifier, bandwidth 12MHz, slew-rate 24V/us, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA552U"
		(extends "OPA551U")
		(property "Reference" "U"
			(at 5.08 7.62 0)
		)
		(property "Value" "OPA552U"
			(at 5.08 5.08 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 5.08 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa552.pdf"
			(at 30.48 -2.54 0)
		)
		(property "Description" "High-Voltage High-Current Operational Amplifier, bandwidth 12MHz, slew-rate 24V/us, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA690xD"
		(extends "OPA890xD")
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "OPA690xD"
			(at -1.27 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/opa690.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Single Low-Power, 500 MHz GBW, ±2.5V to ±5V Dual Supply, 5V to 12V Single Supply, 190mA output current, 1.8kV/us slew rate, Voltage-Feedback Operational Amplifier with Disable, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "opamp texas"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA690xDBV"
		(extends "OPA890xDBV")
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "OPA690xDBV"
			(at -1.27 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/opa690.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Single Low-Power, 500 MHz GBW, ±2.5V to ±5V Dual Supply, 5V to 12V Single Supply, 190mA output current, 1.8kV/us slew rate, Voltage-Feedback Operational Amplifier with Disable, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "opamp texas"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "OPA810xD"
		(extends "OPA333xxD")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "OPA810xD"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -17.526 -21.59 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/opa810.pdf"
			(at 0.508 -24.13 0)
		)
		(property "Description" "140-MHz, Rail-to-Rail Input and Output, FET-Input Operational Amplifier, SOIC-8"
			(at 0 -18.796 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA810xDBV"
		(extends "MCP6L91T-EOT")
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "OPA810xDBV"
			(at -1.27 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -16.764 -22.098 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/opa810.pdf"
			(at 0 -25.4 0)
		)
		(property "Description" "140-MHz, Rail-to-Rail Input and Output, FET-Input Operational Amplifier, SOT-23-5"
			(at 0 -19.05 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "OPA842xD"
		(extends "OPA333xxD")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "OPA842xD"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa842.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "200MHz, Low Distortion, Unity-Gain Stable, Voltage Feedback Operational Amplifier, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA842xDBV"
		(extends "MCP6L91T-EOT")
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "OPA842xDBV"
			(at -1.27 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa842.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "200MHz, Low Distortion, Unity-Gain Stable, Voltage Feedback Operational Amplifier, SOT23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "OPA843xD"
		(extends "OPA333xxD")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "OPA843xD"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa843.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "800MHz, Wideband, Low Distortion, Medium Gain, Voltage-Feedback Operational Amplifier, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp low distortion"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA843xDBV"
		(extends "MCP6L91T-EOT")
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "OPA843xDBV"
			(at -1.27 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa843.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "800MHz, Wideband, Low Distortion, Medium Gain, Voltage-Feedback Operational Amplifier, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp low distortion"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "OPA846xD"
		(extends "OPA333xxD")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "OPA846xD"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa846.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "1750MHz, Wideband, Low-Noise, Voltage Feedback Operational Amplifier, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA846xDBV"
		(extends "MCP6L91T-EOT")
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "OPA846xDBV"
			(at -1.27 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa846.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "1750MHz, Wideband, Low-Noise, Voltage Feedback Operational Amplifier, SOT23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "OPA847xD"
		(extends "OPA890xD")
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "OPA847xD"
			(at -1.27 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa847.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Single Low-Power, 3.9GHz, Wideband, Ultra-Low Noise, Voltage-Feedback Operational Amplifier with Disable, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp wideband low-power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA847xDBV"
		(extends "OPA890xDBV")
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "OPA847xDBV"
			(at -1.27 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa847.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Single Low-Power, 3.9GHz, Wideband, Ultra-Low Noise, Voltage-Feedback Operational Amplifier with Disable, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp wideband low-power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "OPA855xDSG"
		(extends "OPA858xDSG")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "OPA855xDSG"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm"
			(at -2.54 15.24 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa855.pdf"
			(at 10.16 10.16 0)
		)
		(property "Description" "8-GHz Gain Bandwidth Product, Gain of 7-V/V Stable, Bipolar Input Amplifier, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "opamp VFA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA859xDSG"
		(extends "OPA858xDSG")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "OPA859xDSG"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm"
			(at -2.54 15.24 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa859.pdf"
			(at 10.16 10.16 0)
		)
		(property "Description" "1.8 GHz Unity-Gain Bandwidth FET Input Amplifier, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "opamp VFA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "RC4558"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "RC4558"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/rc4558.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual General Purpose, Operational Amplifier, DIP-8/SOIC-8/SSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "RC4560"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "RC4560"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/rc4560.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Audio Operational Amplifier, DIP-8/SOIC-8/SSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "RC4580"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "RC4580"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/rc4580.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Audio Operational Amplifier, SOIC-8/SSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "SA5532"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "SA5532"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ne5532.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Low-Noise Operational Amplifiers, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "SA5534"
		(extends "NE5534")
		(property "Reference" "U"
			(at 1.27 6.35 0)
		)
		(property "Value" "SA5534"
			(at 1.27 3.81 0)
		)
		(property "Footprint" ""
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ne5534.pdf"
			(at 1.27 3.81 0)
		)
		(property "Description" "Single Low-Noise Operational Amplifiers, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm* TO?5*"
			(at 0 0 0)
		)
	)
	(symbol "THS4631D"
		(extends "OPA333xxD")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "THS4631D"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "www.ti.com/lit/ds/symlink/ths4631.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Single High-voltage, High Slew Rate, Wideband, FET-input Operational Amplifier, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "THS4631DGN"
		(extends "THS4631DDA")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "THS4631DGN"
			(at 0 3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "www.ti.com/lit/ds/symlink/ths4631.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Single High-voltage, High Slew Rate, Wideband, FET-input Operational Amplifier, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*1EP*3.9x4.9mm*P1.27mm* MSOP*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TL061"
		(extends "LM741")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "TL061"
			(at 0 3.81 0)
		)
		(property "Footprint" ""
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tl061.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Single Low-Power JFET-Input Operational Amplifiers, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TL062"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TL062"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tl061.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Low-Power JFET-Input Operational Amplifiers, DIP-8/SOIC-8/SSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TL064"
		(extends "LM2902")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TL064"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at -1.27 2.54 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tl061.pdf"
			(at 1.27 5.08 0)
		)
		(property "Description" "Quad Low-Power JFET-Input Operational Amplifiers, DIP-14/SOIC-14/SSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "quad opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* DIP*W7.62mm* TSSOP*4.4x5mm*P0.65mm* SSOP*5.3x6.2mm*P0.65mm* MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TL071"
		(extends "LM741")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "TL071"
			(at 0 3.81 0)
		)
		(property "Footprint" ""
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tl071.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Single Low-Noise JFET-Input Operational Amplifiers, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "singel opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TL072"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TL072"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tl071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Low-Noise JFET-Input Operational Amplifiers, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TL074"
		(extends "LM2902")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TL074"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at -1.27 2.54 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tl071.pdf"
			(at 1.27 5.08 0)
		)
		(property "Description" "Quad Low-Noise JFET-Input Operational Amplifiers, DIP-14/SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "quad opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* DIP*W7.62mm* TSSOP*4.4x5mm*P0.65mm* SSOP*5.3x6.2mm*P0.65mm* MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TL081"
		(extends "LM741")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "TL081"
			(at 0 3.81 0)
		)
		(property "Footprint" ""
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tl081.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Single JFET-Input Operational Amplifiers, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TL082"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TL082"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tl081.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual JFET-Input Operational Amplifiers, DIP-8/SOIC-8/SSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TL084"
		(extends "LM2902")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TL084"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at -1.27 2.54 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tl081.pdf"
			(at 1.27 5.08 0)
		)
		(property "Description" "Quad JFET-Input Operational Amplifiers, DIP-14/SOIC-14/SSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "quad opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* DIP*W7.62mm* TSSOP*4.4x5mm*P0.65mm* SSOP*5.3x6.2mm*P0.65mm* MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLC272"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TLC272"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlc272.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual LinCMOS Precision Dual Operational Amplifiers, DIP-8/SOIC-8/SSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLC274"
		(extends "LM2902")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TLC274"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at -1.27 2.54 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlc274.pdf"
			(at 1.27 5.08 0)
		)
		(property "Description" "Quad LinCMOS Precision Quad Operational Amplifiers, DIP-14/SOIC-14/SSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "quad opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* DIP*W7.62mm* TSSOP*4.4x5mm*P0.65mm* SSOP*5.3x6.2mm*P0.65mm* MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLC277"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TLC277"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlc272.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual LinCMOS Precision Dual Operational Amplifiers, DIP-8/SOIC-8/SSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLC279"
		(extends "LM2902")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TLC279"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at -1.27 2.54 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlc274.pdf"
			(at 1.27 5.08 0)
		)
		(property "Description" "Quad LinCMOS Precision Quad Operational Amplifiers, DIP-14/SOIC-14/SSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "quad opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* DIP*W7.62mm* TSSOP*4.4x5mm*P0.65mm* SSOP*5.3x6.2mm*P0.65mm* MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLE2141ACD"
		(extends "LM741")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "TLE2141ACD"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tle2141a.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Operational Amplifier, 500 uV offset voltage, 0-70°C, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLE2141ACP"
		(extends "LM741")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "TLE2141ACP"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tle2141a.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Operational Amplifier, 500 uV offset voltage, 0-70°C, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLE2141AID"
		(extends "LM741")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "TLE2141AID"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tle2141a.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Operational Amplifier, 500 uV offset voltage, -40 to 105°C, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLE2141AIP"
		(extends "LM741")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "TLE2141AIP"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tle2141a.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Operational Amplifier, 500 uV offset voltage, -40 to 105°C, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLE2141CD"
		(extends "LM741")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "TLE2141CD"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tle2141a.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Operational Amplifier, 900 uV offset voltage, 0-70°C, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLE2141CP"
		(extends "LM741")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "TLE2141CP"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tle2141a.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Operational Amplifier, 900 uV offset voltage, 0-70°C, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLE2141ID"
		(extends "LM741")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "TLE2141ID"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tle2141a.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Operational Amplifier, 900 uV offset voltage, -40 to 105°C, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLE2141IP"
		(extends "LM741")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "TLE2141IP"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tle2141a.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Operational Amplifier, 900 uV offset voltage, -40 to 105°C, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLE2141MD"
		(extends "LM741")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "TLE2141MD"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tle2141a.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Operational Amplifier, 900 uV offset voltage, -55 to 125°C, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLV2371D"
		(extends "OPA333xxD")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "TLV2371D"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv2375.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Rail-to-Rail Input/Output Operational Amplifier, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLV2371DBV"
		(extends "MCP6L91T-EOT")
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "TLV2371DBV"
			(at -1.27 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv2375.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Rail-to-Rail Input/Output Operational Amplifier, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV2371P"
		(extends "MCP601-xP")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "TLV2371P"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv2375.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Rail-to-Rail Input/Output Operational Amplifier, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLV2372"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TLV2372"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv2375.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Rail-to-Rail Input/Output Operational Amplifier, DIP-8/SOIC-8/VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLV6001DCK"
		(extends "TLV172IDCK")
		(property "Reference" "U"
			(at 7.62 2.54 0)
		)
		(property "Value" "TLV6001DCK"
			(at 11.43 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 5.08 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv6001.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-power, Rail-to-rail, 1MHz Operational Amplifier, SOT-353"
			(at 0 0 0)
		)
		(property "ki_keywords" "op amp operational amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*353*SC*70*"
			(at 0 0 0)
		)
	)
	(symbol "TLV9001IDCK"
		(extends "TLV172IDCK")
		(property "Reference" "U"
			(at 7.62 2.54 0)
		)
		(property "Value" "TLV9001IDCK"
			(at 11.43 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 5.08 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv9001.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-power, Rail-to-Rail, 1MHz Operational Amplifier, SOT-353"
			(at 0 0 0)
		)
		(property "ki_keywords" "op amp operational amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*353*SC*70*"
			(at 0 0 0)
		)
	)
	(symbol "TLV9061xDBV"
		(extends "MCP6L91T-EOT")
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "TLV9061xDBV"
			(at -1.27 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -15.24 -19.05 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv9061.pdf"
			(at 0 20.32 0)
		)
		(property "Description" "10-MHz, RRIO, CMOS Operational Amplifiers for Cost-Sensitive Systems, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp rail to rail input output"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV9061xDCK"
		(extends "TLV172IDCK")
		(property "Reference" "U"
			(at 7.62 2.54 0)
		)
		(property "Value" "TLV9061xDCK"
			(at 11.43 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv9061.pdf"
			(at 0 17.78 0)
		)
		(property "Description" "10-MHz, RRIO, CMOS Operational Amplifiers for Cost-Sensitive Systems, SC-70"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp rail to rail input output"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*353*SC*70*"
			(at 0 0 0)
		)
	)
	(symbol "TLV9062"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TLV9062"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv9062.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Operational Amplifiers, SOIC-8/TSSOP-8/VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* TSSOP*4.4x3mm*P0.65mm* VSSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLV9062xD"
		(extends "NCS2325D")
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "TLV9062xD"
			(at 2.54 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv9062.pdf"
			(at 6.35 3.81 0)
		)
		(property "Description" "Dual operational amplifier, 300 uV Offset, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual op-amp low power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLV9062xDSG"
		(extends "OPA2333xxDRB")
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "TLV9062xDSG"
			(at 2.54 3.81 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm_ThermalVias"
			(at 2.54 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv9062.pdf"
			(at 6.35 3.81 0)
		)
		(property "Description" "Dual operational amplifier, 210uV Offset, 0.25uV/C, low-noise, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp low-power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP?2x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLV9064"
		(extends "LM2902")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TLV9064"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at -1.27 2.54 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv9064.pdf"
			(at 1.27 5.08 0)
		)
		(property "Description" "Quad Rail-to-Rail, Operational Amplifiers, 10MHz, SOIC-14/TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "quad opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLV9301xDBV"
		(extends "MCP6L91T-EOT")
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "TLV9301xDBV"
			(at -1.27 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv9301.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "40-V, 1-MHz, RRO Operational Amplifiers for Cost-Sensitive Systems, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp 40V rail to rail output"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV9301xDCK"
		(extends "TLV172IDCK")
		(property "Reference" "U"
			(at 7.62 2.54 0)
		)
		(property "Value" "TLV9301xDCK"
			(at 11.43 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 5.08 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv9301.pdf"
			(at 0 0 0)
		)
		(property "Description" "40-V, 1-MHz, RRO Operational Amplifiers for Cost-Sensitive Systems, SC-70"
			(at 0 0 0)
		)
		(property "ki_keywords" "op amp operational amplifier 40V rail to rail output"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*353*SC*70*"
			(at 0 0 0)
		)
	)
	(symbol "TLV9302xD"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TLV9302xD"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 10.16 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv9302.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "40-V, 1-MHz, RRO Operational Amplifiers for Cost-Sensitive Systems, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp 40V rail to rail output"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLV9302xDDF"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TLV9302xDDF"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-8"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv9302.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "40-V, 1-MHz, RRO Operational Amplifiers for Cost-Sensitive Systems, SOT-23-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp 40V rail to rail output"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV9302xDGK"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TLV9302xDGK"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 10.16 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv9302.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "40-V, 1-MHz, RRO Operational Amplifiers for Cost-Sensitive Systems, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp 40V rail to rail output"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLV9302xPW"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TLV9302xPW"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:TSSOP-8_4.4x3mm_P0.65mm"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv9302.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "40-V, 1-MHz, RRO Operational Amplifiers for Cost-Sensitive Systems, TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp 40V rail to rail output"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLV9304xD"
		(extends "LM2902")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TLV9304xD"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:SO-14_3.9x8.65mm_P1.27mm"
			(at -1.27 2.54 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv9304.pdf"
			(at 1.27 5.08 0)
		)
		(property "Description" "40-V, 1-MHz, RRO Operational Amplifiers for Cost-Sensitive Systems, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "quad opamp 40V rail to rail output"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*3.9x8.65mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLV9304xPW"
		(extends "LM2902")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TLV9304xPW"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -1.27 2.54 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv9304.pdf"
			(at 1.27 5.08 0)
		)
		(property "Description" "40-V, 1-MHz, RRO Operational Amplifiers for Cost-Sensitive Systems, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "quad opamp 40V rail to rail output"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TS881xCx"
		(extends "MCP6001x-LT")
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "TS881xCx"
			(at -1.27 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/a2/60/3e/5d/b2/c1/4a/e9/DM00057901.pdf/files/DM00057901.pdf/jcr:content/translations/en.DM00057901.pdf"
			(at 0 0 0)
		)
		(property "Description" "Rail-to-rail 0.9V nanopower comparator, SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single comparator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "TS881xLx"
		(extends "MCP6L91T-EOT")
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "TS881xLx"
			(at -1.27 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "www.st.com/resource/en/datasheet/ts881.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Rail-to-rail 0.9V nanopower comparator, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single comparator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TS912"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TS912"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "www.st.com/resource/en/datasheet/ts912.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Rail-to-rail CMOS Operational Amplifier, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TSV911IDT"
		(extends "OPA333xxD")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "TSV911IDT"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "www.st.com/resource/en/datasheet/tsv911.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "Single rail-to-rail input/output 8 MHz operational amplifiers, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TSV911RILT"
		(extends "OP179GRT")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TSV911RILT"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "www.st.com/resource/en/datasheet/tsv911.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Single rail-to-rail input/output 8 MHz operational amplifiers, reversed power pins, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TSV911xxLx"
		(extends "MCP6L91T-EOT")
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "TSV911xxLx"
			(at -1.27 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "www.st.com/resource/en/datasheet/tsv911.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Single rail-to-rail input/output 8 MHz operational amplifiers, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TSV912IDT"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TSV912IDT"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "www.st.com/resource/en/datasheet/tsv911.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual rail-to-rail input/output 8 MHz operational amplifiers, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TSV912IST"
		(extends "LM2904")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TSV912IST"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "www.st.com/resource/en/datasheet/tsv911.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual rail-to-rail input/output 8 MHz operational amplifiers, MiniSO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TSV914"
		(extends "LM2902")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TSV914"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at -1.27 2.54 0)
		)
		(property "Datasheet" "www.st.com/resource/en/datasheet/tsv911.pdf"
			(at 1.27 5.08 0)
		)
		(property "Description" "Quad rail-to-rail input/output 8 MHz operational amplifiers, SOIC-14/TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "quad opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* DIP*W7.62mm* TSSOP*4.4x5mm*P0.65mm* SSOP*5.3x6.2mm*P0.65mm* MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TSV994"
		(extends "LM2902")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TSV994"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at -1.27 2.54 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/tsv994.pdf"
			(at 1.27 5.08 0)
		)
		(property "Description" "Quad Rail-to-rail, 20 MHz GBP, operational amplifiers, SOIC-14/TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "quad opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* DIP*W7.62mm* TSSOP*4.4x5mm*P0.65mm* SSOP*5.3x6.2mm*P0.65mm* MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA2604AP"
		(extends "NE5532")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "OPA2604AP"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at -2.54 -16.51 0)
		)
		(property "Datasheet" "https://pdf1.alldatasheetcn.com/datasheet-pdf/view/785955/TI1/OPA2604AP.html"
			(at -2.54 -21.59 0)
		)
		(property "Description" "Dual FET-Input, Low-Distortion Operational Amplifier, DIP-8"
			(at -2.54 -19.05 0)
		)
		(property "ki_keywords" "dual opamp fet-input"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*8*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "OPA810xDCK"
		(extends "OPA810xDBV")
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "OPA810xDCK"
			(at -1.27 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Texas_R-PDSO-G5_DCK-5"
			(at -16.764 -22.098 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/opa810.pdf"
			(at 0 -25.4 0)
		)
		(property "Description" "140-MHz, Rail-to-Rail Input and Output, FET-Input Operational Amplifier, SC-70-5"
			(at 0 -19.05 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas?R?PDSO?G5?DCK*"
			(at 0 0 0)
		)
	)
	(symbol "TLC27M2xD"
		(extends "TLC272")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TLC27M2xD"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlc27m2.pdf"
			(at 0 -8.128 0)
		)
		(property "Description" "LinCMOS Precision Dual Operational Amplifiers, VIO_max = 10mV (at 25°C), VDD = 3..16V (C suffix) / VDD = 4..16V (I / M suffix), 525kHz unity-gain bandwidth (VDD = 5V, TA = 25°C), SOIC-8 (150 mil)"
			(at 0 -12.192 0)
		)
		(property "ki_keywords" "opamp operational-amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLC27M7xD"
		(extends "TLC277")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TLC27M7xD"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.192 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlc27m2.pdf"
			(at 0 -8.128 0)
		)
		(property "Description" "LinCMOS Precision Dual Operational Amplifiers, VIO_max = 500μV (at 25°C), VDD = 3..16V (C suffix) / VDD = 4..16V (I / M suffix), 525kHz unity-gain bandwidth (VDD = 5V, TA = 25°C), SOIC-8 (150 mil)"
			(at 0 -10.16 0)
		)
		(property "ki_keywords" "opamp operational-amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLC27M2xPS"
		(extends "TLC27M2xD")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TLC27M2xPS"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_5.3x6.2mm_P1.27mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlc27m2.pdf"
			(at 0 -8.128 0)
		)
		(property "Description" "LinCMOS Precision Dual Operational Amplifiers, VIO_max = 10mV (at 25°C), VDD = 3..16V (C suffix) / VDD = 4..16V (I / M suffix), 525kHz unity-gain bandwidth (VDD = 5V, TA = 25°C), SOIC-8 (208 mil)"
			(at 0 -12.192 0)
		)
		(property "ki_keywords" "opamp operational-amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLC27M2xPW"
		(extends "TLC27M2xD")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TLC27M2xPW"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:TSSOP-8_4.4x3mm_P0.65mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlc27m2.pdf"
			(at 0 -8.128 0)
		)
		(property "Description" "LinCMOS Precision Dual Operational Amplifiers, VIO_max = 10mV (at 25°C), VDD = 3..16V (C suffix) / VDD = 4..16V (I / M suffix), 525kHz unity-gain bandwidth (VDD = 5V, TA = 25°C), TSSOP-8"
			(at 0 -12.192 0)
		)
		(property "ki_keywords" "opamp operational-amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLC27M7xPS"
		(extends "TLC27M7xD")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TLC27M7xPS"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_5.3x6.2mm_P1.27mm"
			(at 0 -12.192 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlc27m2.pdf"
			(at 0 -8.128 0)
		)
		(property "Description" "LinCMOS Precision Dual Operational Amplifiers, VIO_max = 500μV (at 25°C), VDD = 3..16V (C suffix) / VDD = 4..16V (I / M suffix), 525kHz unity-gain bandwidth (VDD = 5V, TA = 25°C), SOIC-8 (208 mil)"
			(at 0 -10.16 0)
		)
		(property "ki_keywords" "opamp operational-amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
)
