(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "AD813"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 2.54 0)
		)
		(property "Value" "AD813"
			(at 5.08 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD813.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Supply, Low Power, Triple Video Amplifier, DIP-14/SOIC-14"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "triple opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "AD813_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "6")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~{DISABLE}")
				(number "1")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "AD813_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "12")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "13")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~{DISABLE}")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(symbol "AD813_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "10")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "9")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~{DISABLE}")
				(number "3")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(symbol "AD813_4_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX453"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 8.89 0)
		)
		(property "Value" "MAX453"
			(at -6.35 8.89 0)
		)
		(property "Footprint" ""
			(at -3.81 0 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX452-MAX455.pdf"
			(at -3.81 0 0)
		)
		(property "Description" "CMOS video amplifier with input multiplexer, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MAX453_0_0"
			(text "MUX"
				(at -3.81 3.556 0)
			)
			(text "+"
				(at 2.794 1.27 0)
			)
			(text "-"
				(at 2.794 -1.016 0)
			)
		)
		(symbol "MAX453_0_1")
		(symbol "MAX453_1_1"
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "IN0")
				(number "4")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "IN1")
				(number "5")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "A0")
				(number "1")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "IN-")
				(number "7")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "V+")
				(number "6")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "V-")
				(number "3")
			)
			(pin power_in line
				(at 7.62 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "VOUT")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "THS7374"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 11.43 0)
		)
		(property "Value" "THS7374"
			(at 5.08 11.43 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ths7374.pdf"
			(at 0 0 0)
		)
		(property "Description" "4 channel SDTV Video Amplifier, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "video amplifier sdtv cvbs rgb ypbpr"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "THS7374_0_1")
		(symbol "THS7374_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "CH1_IN")
				(number "1")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "CH2_IN")
				(number "2")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "CH3_IN")
				(number "3")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "CH4_IN")
				(number "4")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "DISABLE")
				(number "6")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "BYPASS")
				(number "9")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V_{S+}")
				(number "10")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin no_connect line
				(at 10.16 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at 10.16 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "CH1_OUT")
				(number "14")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "CH2_OUT")
				(number "13")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CH3_OUT")
				(number "12")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "CH4_OUT")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
)
