(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "AD5593R"
		(pin_names
			(offset 1.27)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 15.24 0)
		)
		(property "Value" "AD5593R"
			(at 3.81 15.24 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 25.4 -12.7 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD5593R.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "8-channel 12bits configurable ADC/DAC/GPIO Internal Reference, I2C interface Integrated temperature sensor,Single Supply, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "8channel 12bit ADC DAC GPIO I2C Temperature"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AD5593R_0_1")
		(symbol "AD5593R_1_1"
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 3.81)
				(name "SDA")
				(number "15")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 3.81)
				(name "SCL")
				(number "16")
			)
			(pin passive line
				(at -12.7 2.54 0)
				(length 3.81)
				(name "V_{REF}")
				(number "8")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 3.81)
				(name "~{RESET}")
				(number "1")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 3.81)
				(name "A0")
				(number "2")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 3.81)
				(name "V_{DD}")
				(number "3")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 3.81)
				(name "GND")
				(number "14")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 3.81)
				(name "V_{LOGIC}")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 3.81)
				(name "IO0")
				(number "4")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 3.81)
				(name "IO1")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 3.81)
				(name "IO2")
				(number "6")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 3.81)
				(name "IO3")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 3.81)
				(name "IO4")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 3.81)
				(name "IO5")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 3.81)
				(name "IO6")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 3.81)
				(name "IO7")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD630ARZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 19.05 0)
		)
		(property "Value" "AD630ARZ"
			(at 6.35 19.05 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 -26.67 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ad630.pdf"
			(at -10.16 27.94 0)
		)
		(property "Description" "High precision Balanced Modulator/Demodulator, 2 MHz, SOIC-20W"
			(at 0 0 0)
		)
		(property "ki_keywords" "modulator demodulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "AD630ARZ_0_0"
			(text "R_{in}A"
				(at -11.176 15.875 0)
			)
			(text "R_{in}B"
				(at -11.176 5.842 0)
			)
			(text "CHA+"
				(at -10.922 13.335 0)
			)
			(text "CHA-"
				(at -10.922 10.922 0)
			)
			(text "CHB+"
				(at -10.795 3.175 0)
			)
			(text "CHB-"
				(at -10.668 0.762 0)
			)
			(text "SEL_B"
				(at -10.541 -4.445 0)
			)
			(text "SEL_A"
				(at -10.541 -6.985 0)
			)
			(text "2k5"
				(at -8.255 15.24 0)
			)
			(text "2k5"
				(at -8.255 5.08 0)
			)
			(text "+"
				(at -4.445 12.7 0)
			)
			(text "-"
				(at -4.445 10.16 0)
			)
			(text "+"
				(at -4.445 2.54 0)
			)
			(text "-"
				(at -4.445 0 0)
			)
			(text "-"
				(at -4.445 -5.08 0)
			)
			(text "+"
				(at -4.445 -7.493 0)
			)
			(text "A"
				(at -3.683 11.43 0)
			)
			(text "B"
				(at -3.683 1.27 0)
			)
			(text "-"
				(at 4.445 6.477 0)
			)
			(text "+"
				(at 4.445 3.937 0)
			)
			(text "10k"
				(at 7.62 2.54 900)
			)
			(text "10k"
				(at 9.525 0 0)
			)
			(text "5k"
				(at 9.525 -2.54 0)
			)
			(text "COMP"
				(at 10.668 13.462 0)
			)
			(text "V_{OUT}"
				(at 10.922 5.842 0)
			)
			(text "B/~{A}"
				(at 11.176 -6.858 0)
			)
			(text "R_{B}"
				(at 11.684 0.762 0)
			)
			(text "R_{A}"
				(at 11.684 -1.778 0)
			)
			(text "R_{F}"
				(at 11.684 -4.318 0)
			)
		)
		(symbol "AD630ARZ_0_1")
		(symbol "AD630ARZ_1_1"
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "R_{in}A")
				(number "1")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "CHA+")
				(number "2")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "CHA-")
				(number "20")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "R_{in}B")
				(number "17")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "CHB+")
				(number "18")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "CHB-")
				(number "19")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "SEL_B")
				(number "9")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "SEL_A")
				(number "10")
			)
			(pin passive line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "DIFF_OFF_ADJ1")
				(number "3")
			)
			(pin passive line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "DIFF_OFF_ADJ2")
				(number "4")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "+V_{S}")
				(number "11")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "-V_{S}")
				(number "8")
			)
			(pin passive line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "COMP")
				(number "12")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "V_{OUT}")
				(number "13")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "R_{B}")
				(number "14")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "R_{A}")
				(number "16")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "R_{F}")
				(number "15")
			)
			(pin open_collector line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "B/~{A}")
				(number "7")
			)
			(pin passive line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "CM_OFF_ADJ1")
				(number "5")
			)
			(pin passive line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "CM_OFF_ADJ2")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD637xQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 13.97 0)
		)
		(property "Value" "AD637xQ"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD637.pdf"
			(at -6.35 17.78 0)
		)
		(property "Description" "High Precision, Wideband RMS-to-DC Converter, DIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "rms-to-dc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "AD637xQ_0_1")
		(symbol "AD637xQ_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "CS")
				(number "5")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "V_{IN}")
				(number "13")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "OUTPUT_OFFSET")
				(number "4")
			)
			(pin no_connect line
				(at -10.16 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NIC")
				(number "2")
			)
			(pin no_connect line
				(at -10.16 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NIC")
				(number "12")
			)
			(pin power_in line
				(at -5.08 -15.24 90)
				(length 2.54)
				(name "COM")
				(number "3")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "+V_{S}")
				(number "11")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "-V_{S}")
				(number "10")
			)
			(pin passive line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "C_{AV}")
				(number "8")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "RMS_OUT")
				(number "9")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "DEN_INPUT")
				(number "6")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "dB_OUTPUT")
				(number "7")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "BUFF_IN")
				(number "1")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "BUFF_OUT")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD637xRZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 13.97 0)
		)
		(property "Value" "AD637xRZ"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD637.pdf"
			(at -6.35 17.78 0)
		)
		(property "Description" "High Precision, Wideband RMS-to-DC Converter, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "rms-to-dc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "AD637xRZ_0_1")
		(symbol "AD637xRZ_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "CS")
				(number "5")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "V_{IN}")
				(number "15")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "OUTPUT_OFFSET")
				(number "4")
			)
			(pin no_connect line
				(at -10.16 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NIC")
				(number "2")
			)
			(pin no_connect line
				(at -10.16 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NIC")
				(number "8")
			)
			(pin no_connect line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NIC")
				(number "9")
			)
			(pin no_connect line
				(at -10.16 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NIC")
				(number "14")
			)
			(pin power_in line
				(at -5.08 -15.24 90)
				(length 2.54)
				(name "COM")
				(number "3")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "+V_{S}")
				(number "13")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "-V_{S}")
				(number "12")
			)
			(pin passive line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "C_{AV}")
				(number "10")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "RMS_OUT")
				(number "11")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "DEN_INPUT")
				(number "6")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "dB_OUTPUT")
				(number "7")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "BUFF_IN")
				(number "1")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "BUFF_OUT")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD654JN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "AD654JN"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD654.pdf"
			(at -6.35 17.78 0)
		)
		(property "Description" "Low Cost Monolithic Voltage-to-Frequency Converter, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "v-to-f v-f"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "AD654JN_0_1")
		(symbol "AD654JN_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "+V_{IN}")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "R_{T}")
				(number "3")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "+V_{S}")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "-V_{S}")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "COM")
				(number "2")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "C_{T}1")
				(number "6")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "C_{T}2")
				(number "7")
			)
			(pin open_collector line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "F_{OUT}")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD654JR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "AD654JR"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD654.pdf"
			(at -6.35 17.78 0)
		)
		(property "Description" "Low Cost Monolithic Voltage-to-Frequency Converter, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "v-to-f v-f"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "AD654JR_0_1")
		(symbol "AD654JR_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "+V_{IN}")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "R_{T}")
				(number "3")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "+V_{S}")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "-V_{S}")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "COM")
				(number "2")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "C_{T}1")
				(number "6")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "C_{T}2")
				(number "7")
			)
			(pin open_collector line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "F_{OUT}")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LF398H"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 3.81 0)
		)
		(property "Value" "LF398H"
			(at 5.08 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-99-8"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lf398-n.pdf"
			(at 0 0 0)
		)
		(property "Description" "Sample And Hold Unity Gain Follower, TO-99-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "sample hold buffer unity gain"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TO*99*"
			(at 0 0 0)
		)
		(symbol "LF398H_0_1")
		(symbol "LF398H_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "I")
				(number "3")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "Hold")
				(number "8")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "T")
				(number "7")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V^{+}")
				(number "1")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V^{-}")
				(number "4")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "Adj")
				(number "2")
			)
			(pin passive line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "C_{h}")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LF398_DIP8"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 3.81 0)
		)
		(property "Value" "LF398_DIP8"
			(at 5.08 -2.54 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lf398-n.pdf"
			(at 0 0 0)
		)
		(property "Description" "Sample And Hold Unity Gain Follower, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "sample hold buffer unity gain"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "LF398_DIP8_0_1")
		(symbol "LF398_DIP8_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "I")
				(number "3")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "Hold")
				(number "8")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "T")
				(number "7")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V^{+}")
				(number "1")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V^{-}")
				(number "4")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "Adj")
				(number "2")
			)
			(pin passive line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "C_{h}")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LF398_SOIC14"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 3.81 0)
		)
		(property "Value" "LF398_SOIC14"
			(at 5.08 -2.54 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lf398-n.pdf"
			(at 0 0 0)
		)
		(property "Description" "Sample And Hold Unity Gain Follower, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "sample hold buffer unity gain"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LF398_SOIC14_0_1")
		(symbol "LF398_SOIC14_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "I")
				(number "1")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "Hold")
				(number "11")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "T")
				(number "10")
			)
			(pin no_connect line
				(at -5.08 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V^{+}")
				(number "12")
			)
			(pin no_connect line
				(at -2.54 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at -2.54 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V^{-}")
				(number "3")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at 0 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "Adj")
				(number "14")
			)
			(pin passive line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "C_{h}")
				(number "8")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM331N"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -9.144 12.192 0)
		)
		(property "Value" "LM331N"
			(at 6.096 12.192 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0.254 -20.066 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/lm331"
			(at 0 -17.78 0)
		)
		(property "Description" "Precision Voltage-to-Frequency Converter, 1 Hz - 100 kHz, 0.9..1.1 kHz/V Gain, PDIP-8"
			(at 1.016 -22.098 0)
		)
		(property "ki_keywords" "v-to-f v-f"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "LM331N_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "COMPIN")
				(number "7")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RC")
				(number "5")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "THRESH")
				(number "6")
			)
			(pin output line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "IOUT")
				(number "1")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VS")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin open_collector line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "FOUT")
				(number "3")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "IREF")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC1966"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 11.43 0)
		)
		(property "Value" "LTC1966"
			(at 6.35 8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 -21.59 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1966fb.pdf"
			(at 0 -24.13 0)
		)
		(property "Description" "Precision Micropower True RMS-to-DC Converter, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "rms-to-dc converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LTC1966_0_0"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN1")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN2")
				(number "3")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT_RTN")
				(number "6")
			)
		)
		(symbol "LTC1966_1_0"
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{ENABLE}")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V_{DD}")
				(number "7")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "V_{SS}")
				(number "4")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "V_{OUT}")
				(number "5")
			)
		)
		(symbol "LTC1966_1_1")
		(embedded_fonts no)
	)
	(symbol "LTC1967"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 13.97 0)
		)
		(property "Value" "LTC1967"
			(at 6.35 11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 -21.59 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1967f.pdf"
			(at 0 -24.13 0)
		)
		(property "Description" "Precision Extended Bandwidth True RMS-to-DC Converter, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "rms-to-dc converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LTC1967_0_0"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN1")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN2")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT_RTN")
				(number "6")
			)
		)
		(symbol "LTC1967_1_0"
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{ENABLE}")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V^{+}")
				(number "7")
			)
			(pin no_connect line
				(at 2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "V_{OUT}")
				(number "5")
			)
		)
		(symbol "LTC1967_1_1")
		(embedded_fonts no)
	)
	(symbol "MLX90314xDF"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 13.97 0)
		)
		(property "Value" "MLX90314xDF"
			(at 15.24 -13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at -10.16 20.32 0)
		)
		(property "Datasheet" "https://media.digikey.com/pdf/Data%20Sheets/Melexis%20PDFs/MLX90314_Rev008.pdf"
			(at -6.35 17.78 0)
		)
		(property "Description" "Programmable Sensor Interface (Signal Conditioner), SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "sensor signal conditioning"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MLX90314xDF_0_1")
		(symbol "MLX90314xDF_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "TSTB")
				(number "3")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "VBP")
				(number "7")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "VBN")
				(number "6")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "TMP")
				(number "8")
			)
			(pin passive line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "FLT")
				(number "4")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "V_{DD}")
				(number "9")
			)
			(pin output line
				(at 0 15.24 270)
				(length 2.54)
				(name "FET")
				(number "10")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "15")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "V_{DD1}")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "COMS")
				(number "16")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "IO1")
				(number "1")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "IO2")
				(number "2")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "VMO")
				(number "12")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CMO")
				(number "13")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "CMN")
				(number "14")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "OFC")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MLX90320xFR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 13.97 0)
		)
		(property "Value" "MLX90320xFR"
			(at 15.24 13.97 0)
		)
		(property "Footprint" "Package_SO:SSOP-14_5.3x6.2mm_P0.65mm"
			(at 0 20.32 0)
		)
		(property "Datasheet" "https://www.mouser.com/datasheet/2/734/MLX90320-Datasheet-Melexis-953341.pdf"
			(at -6.35 17.78 0)
		)
		(property "Description" "Programmable Automotive Sensor Interface (Signal Conditioner), SSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "sensor signal conditioning"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x6.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MLX90320xFR_0_1")
		(symbol "MLX90320xFR_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "INP")
				(number "3")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "INM")
				(number "1")
			)
			(pin passive line
				(at -12.7 0 0)
				(length 2.54)
				(name "TMP")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "ANAGND")
				(number "2")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "DIGGND")
				(number "6")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "SUB")
				(number "4")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "OUT")
				(number "12")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "FLT")
				(number "11")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 2.54)
				(name "TESTIN1")
				(number "9")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "TESTIN2")
				(number "10")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "TESTOUT")
				(number "8")
			)
			(pin passive line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "TEST1")
				(number "7")
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "TEST2")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MPY634KP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 13.97 0)
		)
		(property "Value" "MPY634KP"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/mpy634.pdf"
			(at 1.27 1.27 0)
		)
		(property "Description" "Wide Bandwidth Precision Analog Multiplier, DIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "analog multiplier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MPY634KP_0_0"
			(text "+"
				(at -5.842 2.413 0)
			)
			(text "-"
				(at -5.842 0.254 0)
			)
			(text "+"
				(at -5.842 -5.207 0)
			)
			(text "-"
				(at -5.842 -7.366 0)
			)
			(text "+"
				(at -5.715 10.033 0)
			)
			(text "-"
				(at -5.715 7.874 0)
			)
			(text "V-I"
				(at -4.445 1.27 0)
			)
			(text "V-I"
				(at -4.445 -6.35 0)
			)
			(text "V-I"
				(at -4.318 8.89 0)
			)
			(text "+"
				(at 4.445 1.016 0)
			)
			(text "-"
				(at 4.445 -1.016 0)
			)
			(text "A"
				(at 5.588 0 0)
			)
		)
		(symbol "MPY634KP_0_1")
		(symbol "MPY634KP_1_0"
			(text "MULTIPLIER"
				(at 0 3.81 900)
			)
			(text "0.75"
				(at 0 -3.175 900)
			)
			(text "CORE"
				(at 1.27 3.81 900)
			)
			(text "ATTEN"
				(at 1.27 -3.175 900)
			)
		)
		(symbol "MPY634KP_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "X_{1}")
				(number "1")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "X_{2}")
				(number "2")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "Y_{1}")
				(number "6")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "Y_{2}")
				(number "7")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "Z_{1}")
				(number "11")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "Z_{2}")
				(number "10")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "+V_{S}")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "-V_{S}")
				(number "8")
			)
			(pin no_connect line
				(at 10.16 10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at 10.16 7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "V_{O}")
				(number "12")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "SF")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MPY634KU"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 13.97 0)
		)
		(property "Value" "MPY634KU"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/mpy634.pdf"
			(at 0 0 0)
		)
		(property "Description" "Wide Bandwidth Precision Analog Multiplier, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "analog multiplier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MPY634KU_0_0"
			(text "+"
				(at -5.842 2.413 0)
			)
			(text "-"
				(at -5.842 0.254 0)
			)
			(text "+"
				(at -5.842 -5.207 0)
			)
			(text "-"
				(at -5.842 -7.366 0)
			)
			(text "+"
				(at -5.715 10.033 0)
			)
			(text "-"
				(at -5.715 7.874 0)
			)
			(text "V-I"
				(at -4.445 1.27 0)
			)
			(text "V-I"
				(at -4.445 -6.35 0)
			)
			(text "V-I"
				(at -4.318 8.89 0)
			)
			(text "+"
				(at 4.445 1.016 0)
			)
			(text "-"
				(at 4.445 -1.016 0)
			)
			(text "A"
				(at 5.588 0 0)
			)
		)
		(symbol "MPY634KU_0_1")
		(symbol "MPY634KU_1_0"
			(text "MULTIPLIER"
				(at 0 3.81 900)
			)
			(text "0.75"
				(at 0 -3.175 900)
			)
			(text "CORE"
				(at 1.27 3.81 900)
			)
			(text "ATTEN"
				(at 1.27 -3.175 900)
			)
		)
		(symbol "MPY634KU_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "X_{1}")
				(number "1")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "X_{2}")
				(number "2")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "Y_{1}")
				(number "6")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "Y_{2}")
				(number "7")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "Z_{1}")
				(number "13")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "Z_{2}")
				(number "12")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "+V_{S}")
				(number "16")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "-V_{S}")
				(number "10")
			)
			(pin no_connect line
				(at 10.16 10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at 10.16 7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at 10.16 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin no_connect line
				(at 10.16 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "V_{O}")
				(number "14")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "SF")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PGA112"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "PGA112"
			(at 7.62 8.89 0)
		)
		(property "Footprint" "Package_SO:TSSOP-10_3x3mm_P0.5mm"
			(at -10.16 20.32 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/sbos424c/sbos424c.pdf"
			(at -6.35 17.78 0)
		)
		(property "Description" "Zero-Drift Programmable Gain Amplifier With Mux, x1/x2/x4/x8/x16/x32/x64/x128 gains, VSSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "PGA SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "PGA112_0_1")
		(symbol "PGA112_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "V_{REF}")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "CH0/V_{CAL}")
				(number "3")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "CH1")
				(number "2")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "AV_{DD}")
				(number "1")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "DV_{DD}")
				(number "10")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SCLK")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "DIO")
				(number "8")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "~{CS}")
				(number "9")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "V_{OUT}")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LF398_SOIC8"
		(extends "LF398_DIP8")
		(property "Reference" "U"
			(at 5.08 3.81 0)
		)
		(property "Value" "LF398_SOIC8"
			(at 5.08 -2.54 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/lt0398s8.pdf"
			(at 0 0 0)
		)
		(property "Description" "Sample And Hold Unity Gain Follower, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "sample hold buffer unity gain"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM231N"
		(extends "LM331N")
		(property "Reference" "U"
			(at -9.144 12.192 0)
		)
		(property "Value" "LM231N"
			(at 6.096 12.192 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0.254 -20.066 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/lm331"
			(at 0 -17.78 0)
		)
		(property "Description" "Precision Voltage-to-Frequency Converter, 1 Hz - 100 kHz, 0.95..1.05 kHz/V Gain, PDIP-8"
			(at 1.016 -22.098 0)
		)
		(property "ki_keywords" "v-to-f v-f"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC1968"
		(extends "LTC1967")
		(property "Reference" "U"
			(at 6.35 13.97 0)
		)
		(property "Value" "LTC1968"
			(at 6.35 11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 1.27 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1968f.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Precision Wide Bandwidth True RMS-to-DC Converter, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "rms-to-dc converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PGA113"
		(extends "PGA112")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "PGA113"
			(at 7.62 8.89 0)
		)
		(property "Footprint" "Package_SO:TSSOP-10_3x3mm_P0.5mm"
			(at -10.16 20.32 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/sbos424c/sbos424c.pdf"
			(at -6.35 17.78 0)
		)
		(property "Description" "Zero-Drift Programmable Gain Amplifier With Mux, x1/x2/x5/x10/x20/x50/x100/x200 gains, VSSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "PGA SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
)
