(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "AD40xxBCPZ"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "AD40xxBCPZ"
			(at 10.16 -8.89 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-WD-10-1EP_3x3mm_P0.5mm_EP1.64x2.38mm"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ad4003-4007-4011.pdf"
			(at 0 -22.86 0)
		)
		(property "Description" "18-Bit, 2 MSPS/1 MSPS/500 kSPS, Differential SAR ADCs, 2.4V to 5.1V reference, 1.8V supply, 1.71 to 5.5V logic IO, 3x3mm LFCSP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC 18-bit AD4003BCPZ AD4007BCPZ AD4011BCPZ"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*LFCSP?WD*EP?3x3mm?P0.5mm?EP1.64x2.38mm*"
			(at 0 0 0)
		)
		(symbol "AD40xxBCPZ_1_1"
			(pin input line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "IN+")
				(number "3")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "IN-")
				(number "4")
			)
			(pin input line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "REF")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "VIO")
				(number "10")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "PAD")
				(number "11")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "SDI")
				(number "9")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "SCK")
				(number "8")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "SDO")
				(number "7")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CNV")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD40xxBRMZ"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "AD40xxBRMZ"
			(at 7.62 -8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ad4003-4007-4011.pdf"
			(at 0 -15.24 0)
		)
		(property "Description" "18-Bit, 2 MSPS/1 MSPS/500 kSPS, Differential SAR ADCs, 2.4V to 5.1V reference, 1.8V supply, 1.71 to 5.5V logic IO, MSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC 18-bit AD4003BRMZ AD4007BRMZ AD4011BRMZ"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*MSOP*3x3mm?P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AD40xxBRMZ_1_1"
			(pin input line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "IN+")
				(number "3")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "IN-")
				(number "4")
			)
			(pin input line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "REF")
				(number "1")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "VIO")
				(number "10")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "SDI")
				(number "9")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "SCK")
				(number "8")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "SDO")
				(number "7")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CNV")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD574A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" "AD574A"
			(at 0 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ad574a.pdf"
			(at -43.18 -3.81 0)
		)
		(property "Description" "12-Bit Successive-Approximation (SAR) ADC"
			(at -44.45 77.47 0)
		)
		(property "ki_keywords" "analog"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DIP*W15.24mm* *PLCC* *LCC*"
			(at 0 0 0)
		)
		(symbol "AD574A_1_1"
			(text "I_{REF}"
				(at -6.35 -20.32 0)
			)
			(text "+"
				(at -3.81 -27.813 0)
			)
			(text "-"
				(at -3.81 -32.893 0)
			)
			(text "I_{DAC}\nI_{DAC} = \n4x N x I_{REF}"
				(at -2.54 -10.16 0)
			)
			(text "DAC"
				(at -2.54 -38.1 0)
			)
			(text "+"
				(at -1.27 5.207 0)
			)
			(text "-"
				(at -1.27 0.127 0)
			)
			(text "COMP"
				(at 5.08 -0.762 0)
			)
			(text "12"
				(at 8.89 8.89 0)
			)
			(text "12"
				(at 8.89 -17.78 0)
			)
			(text "V_{EE}"
				(at 8.89 -37.465 0)
			)
			(text "12"
				(at 12.7 12.7 0)
			)
			(text "3\n\nS\nT\nA\nT\nE\n\nO\nU\nT\nP\nU\nT\n\nB\nU\nF\nF\nE\nR\nS"
				(at 16.51 -12.7 0)
			)
			(text_box "10V\nREF"
				(at -17.78 6.35 0)
				(size 7.62 -7.62)
				(margins 1.016 1.016 1.016 1.016)
				(fill
					(type none)
				)
			)
			(text_box "9k95"
				(at -17.78 -6.985 0)
				(size 3.81 -1.27)
				(margins 0.508 0.508 0.508 0.508)
				(fill
					(type none)
				)
			)
			(text_box "19k95"
				(at -17.78 -27.305 0)
				(size 3.81 -1.27)
				(margins 0.508 0.508 0.508 0.508)
				(fill
					(type none)
				)
			)
			(text_box "5k"
				(at -13.335 -8.89 90)
				(size 1.27 -3.81)
				(margins 0.508 0.508 0.508 0.508)
				(fill
					(type none)
				)
			)
			(text_box "5k"
				(at -13.335 -17.145 90)
				(size 1.27 -3.81)
				(margins 0.508 0.508 0.508 0.508)
				(fill
					(type none)
				)
			)
			(text_box "CONTROL"
				(at -7.62 36.83 0)
				(size 20.32 -17.78)
				(margins 1.016 1.016 1.016 1.016)
				(fill
					(type none)
				)
			)
			(text_box "CLOCK"
				(at -7.62 15.24 0)
				(size 10.16 -5.08)
				(margins 1.016 1.016 1.016 1.016)
				(fill
					(type none)
				)
			)
			(text_box "3k"
				(at -7.62 5.715 0)
				(size 3.81 -1.27)
				(margins 0.508 0.508 0.508 0.508)
				(fill
					(type none)
				)
			)
			(text_box "8k"
				(at 0 -19.05 0)
				(size 3.81 -1.27)
				(margins 0.508 0.508 0.508 0.508)
				(fill
					(type none)
				)
			)
			(text_box "SAR"
				(at 3.81 15.24 0)
				(size 7.62 -5.08)
				(margins 1.016 1.016 1.016 1.016)
				(fill
					(type none)
				)
			)
			(text_box ""
				(at 13.97 16.51 0)
				(size 13.97 -55.88)
				(margins 1.016 1.016 1.016 1.016)
				(fill
					(type none)
				)
			)
			(text_box "N\nI\nB\nB\nL\nE\n\nA"
				(at 19.05 15.24 0)
				(size 8.89 -17.78)
				(margins 1.016 1.016 1.016 1.016)
				(fill
					(type none)
				)
			)
			(text_box "N\nI\nB\nB\nL\nE\n\nB"
				(at 19.05 -2.54 0)
				(size 8.89 -17.78)
				(margins 1.016 1.016 1.016 1.016)
				(fill
					(type none)
				)
			)
			(text_box "N\nI\nB\nB\nL\nE\n\nC"
				(at 19.05 -20.32 0)
				(size 8.89 -17.78)
				(margins 1.016 1.016 1.016 1.016)
				(fill
					(type none)
				)
			)
			(pin output line
				(at -30.48 2.54 0)
				(length 2.54)
				(name "REF_OUT")
				(number "8")
			)
			(pin input line
				(at -30.48 -7.62 0)
				(length 2.54)
				(name "BIP_OFF")
				(number "12")
			)
			(pin input line
				(at -30.48 -15.24 0)
				(length 2.54)
				(name "10V_{IN}")
				(number "13")
			)
			(pin input line
				(at -30.48 -22.86 0)
				(length 2.54)
				(name "20V_{IN}")
				(number "14")
			)
			(pin input line
				(at -30.48 -27.94 0)
				(length 2.54)
				(name "REF_IN")
				(number "10")
			)
			(pin passive line
				(at -30.48 -35.56 0)
				(length 2.54)
				(name "AC")
				(number "9")
			)
			(pin power_in line
				(at -20.32 45.72 270)
				(length 2.54)
				(name "V_{CC}")
				(number "7")
			)
			(pin power_in line
				(at -20.32 -45.72 90)
				(length 2.54)
				(name "V_{EE}")
				(number "11")
			)
			(pin power_in line
				(at 15.24 45.72 270)
				(length 2.54)
				(name "V_{LOGIC}")
				(number "1")
			)
			(pin power_in line
				(at 15.24 -45.72 90)
				(length 2.54)
				(name "DC")
				(number "15")
			)
			(pin input line
				(at 30.48 35.56 180)
				(length 2.54)
				(name "12/~{8}")
				(number "2")
			)
			(pin input line
				(at 30.48 33.02 180)
				(length 2.54)
				(name "~{CS}")
				(number "3")
			)
			(pin input line
				(at 30.48 30.48 180)
				(length 2.54)
				(name "A_{0}")
				(number "4")
			)
			(pin input line
				(at 30.48 27.94 180)
				(length 2.54)
				(name "R/~{C}")
				(number "5")
			)
			(pin input line
				(at 30.48 25.4 180)
				(length 2.54)
				(name "CE")
				(number "6")
			)
			(pin output line
				(at 30.48 20.32 180)
				(length 2.54)
				(name "STS")
				(number "28")
			)
			(pin output line
				(at 30.48 10.16 180)
				(length 2.54)
				(name "D0")
				(number "16")
			)
			(pin output line
				(at 30.48 7.62 180)
				(length 2.54)
				(name "DB1")
				(number "17")
			)
			(pin output line
				(at 30.48 5.08 180)
				(length 2.54)
				(name "DB2")
				(number "18")
			)
			(pin output line
				(at 30.48 2.54 180)
				(length 2.54)
				(name "DB3")
				(number "19")
			)
			(pin output line
				(at 30.48 -7.62 180)
				(length 2.54)
				(name "DB4")
				(number "20")
			)
			(pin output line
				(at 30.48 -10.16 180)
				(length 2.54)
				(name "DB5")
				(number "21")
			)
			(pin output line
				(at 30.48 -12.7 180)
				(length 2.54)
				(name "DB6")
				(number "22")
			)
			(pin output line
				(at 30.48 -15.24 180)
				(length 2.54)
				(name "DB7")
				(number "23")
			)
			(pin output line
				(at 30.48 -25.4 180)
				(length 2.54)
				(name "DB8")
				(number "24")
			)
			(pin output line
				(at 30.48 -27.94 180)
				(length 2.54)
				(name "DB9")
				(number "25")
			)
			(pin output line
				(at 30.48 -30.48 180)
				(length 2.54)
				(name "DB10")
				(number "26")
			)
			(pin output line
				(at 30.48 -33.02 180)
				(length 2.54)
				(name "DB11")
				(number "27")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD6644"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 26.67 0)
		)
		(property "Value" "AD6644"
			(at 3.81 26.67 0)
		)
		(property "Footprint" "Package_QFP:TQFP-52-1EP_10x10mm_P0.65mm_EP6.5x6.5mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD6644.pdf"
			(at -2.54 -31.75 0)
		)
		(property "Description" "A/D Converter, 14-Bit, 40 MSPS/65 MSPS, TQFP-52"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC differential analog digital converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*1EP*10x10mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AD6644_0_1")
		(symbol "AD6644_1_1"
			(pin input line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "ENCODE")
				(number "5")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "~{ENCODE}")
				(number "6")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "AIN")
				(number "11")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{AIN}")
				(number "12")
			)
			(pin passive line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "VREF")
				(number "3")
			)
			(pin passive line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "C1")
				(number "20")
			)
			(pin passive line
				(at -10.16 -22.86 0)
				(length 2.54)
				(name "C2")
				(number "24")
			)
			(pin passive line
				(at -2.54 27.94 270)
				(length 2.54)
				(hide yes)
				(name "AVCC")
				(number "14")
			)
			(pin passive line
				(at -2.54 27.94 270)
				(length 2.54)
				(hide yes)
				(name "AVCC")
				(number "16")
			)
			(pin passive line
				(at -2.54 27.94 270)
				(length 2.54)
				(hide yes)
				(name "AVCC")
				(number "18")
			)
			(pin passive line
				(at -2.54 27.94 270)
				(length 2.54)
				(hide yes)
				(name "AVCC")
				(number "22")
			)
			(pin passive line
				(at -2.54 27.94 270)
				(length 2.54)
				(hide yes)
				(name "AVCC")
				(number "26")
			)
			(pin passive line
				(at -2.54 27.94 270)
				(length 2.54)
				(hide yes)
				(name "AVCC")
				(number "28")
			)
			(pin passive line
				(at -2.54 27.94 270)
				(length 2.54)
				(hide yes)
				(name "AVCC")
				(number "30")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "AVCC")
				(number "8")
			)
			(pin passive line
				(at -2.54 27.94 270)
				(length 2.54)
				(hide yes)
				(name "AVCC")
				(number "9")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "19")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "23")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "27")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "34")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "42")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "53")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "DVCC")
				(number "1")
			)
			(pin passive line
				(at 2.54 27.94 270)
				(length 2.54)
				(hide yes)
				(name "DVCC")
				(number "33")
			)
			(pin passive line
				(at 2.54 27.94 270)
				(length 2.54)
				(hide yes)
				(name "DVCC")
				(number "43")
			)
			(pin no_connect line
				(at 7.62 -12.7 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "31")
			)
			(pin output line
				(at 10.16 22.86 180)
				(length 2.54)
				(name "D0")
				(number "36")
			)
			(pin output line
				(at 10.16 20.32 180)
				(length 2.54)
				(name "D1")
				(number "37")
			)
			(pin output line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "D2")
				(number "38")
			)
			(pin output line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "D3")
				(number "39")
			)
			(pin output line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "D4")
				(number "40")
			)
			(pin output line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "D5")
				(number "41")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "D6")
				(number "44")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "D7")
				(number "45")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "D8")
				(number "46")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "D9")
				(number "47")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "D10")
				(number "48")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "D11")
				(number "49")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "D12")
				(number "50")
			)
			(pin output line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "D13")
				(number "51")
			)
			(pin output line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "DRY")
				(number "52")
			)
			(pin output line
				(at 10.16 -17.78 180)
				(length 2.54)
				(name "OVR")
				(number "32")
			)
			(pin output line
				(at 10.16 -22.86 180)
				(length 2.54)
				(name "DMID")
				(number "35")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD7171"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "AD7171"
			(at 2.54 7.62 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-10-1EP_3x3mm_P0.5mm_EP1.55x2.48mm"
			(at 0 -13.335 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD7171.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single channel Analog to Digital Converter, 16-bit, differential input, 125Hz, SPI interface"
			(at 0 0 0)
		)
		(property "ki_keywords" "sigma delta adc spi 1ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P0.5mm*EP1.55x2.48mm*"
			(at 0 0 0)
		)
		(symbol "AD7171_0_1")
		(symbol "AD7171_1_1"
			(pin passive line
				(at -17.78 5.08 0)
				(length 6.35)
				(name "REFIN+")
				(number "5")
			)
			(pin passive line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "AIN+")
				(number "3")
			)
			(pin passive line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "AIN-")
				(number "4")
			)
			(pin passive line
				(at -17.78 -5.08 0)
				(length 6.35)
				(name "REFIN-")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 3.81)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 3.81)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 3.81)
				(name "PAD")
				(number "11")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 3.81)
				(name "GND")
				(number "10")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 3.81)
				(name "SCK")
				(number "1")
			)
			(pin tri_state line
				(at 15.24 0 180)
				(length 3.81)
				(name "DOUT/~{RDY}")
				(number "2")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 3.81)
				(name "~{PDRST}")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD7298"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 13.97 0)
		)
		(property "Value" "AD7298"
			(at 2.54 13.97 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-20-1EP_4x4mm_P0.5mm_EP2.6x2.6mm_ThermalVias"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD7298.pdf"
			(at 0 0 0)
		)
		(property "Description" "8 channel, 1MSPS, 12-bit SAR ADC with Temperature Sensor, LFCSP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC, 3.3V, SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AD7298_0_1")
		(symbol "AD7298_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "VIN0")
				(number "18")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "VIN1")
				(number "19")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VIN2")
				(number "20")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "VIN3")
				(number "1")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "VIN4")
				(number "2")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "VIN5")
				(number "3")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "VIN6")
				(number "4")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "VIN7")
				(number "5")
			)
			(pin passive line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "VREF")
				(number "7")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "10")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 2.54)
				(name "GND1")
				(number "6")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDRIVE")
				(number "16")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "EPAD")
				(number "21")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "SCLK")
				(number "15")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "DIN")
				(number "13")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "DOUT")
				(number "14")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "~{CS}")
				(number "11")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "~{PD}/~{RST}")
				(number "17")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "TSENSE_BUSY")
				(number "12")
			)
			(pin passive line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "DCAP")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD7321"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 10.16 18.542 0)
		)
		(property "Value" "AD7321"
			(at 16.256 16.764 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at 17.084 -14.224 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD7321.pdf"
			(at 17.084 -18.796 0)
		)
		(property "Description" "2-Channel, software selectable input range ±10 V, ±5V, ±2.5V, 0 V to +10 V, true bipolar input, 12-Bit plus sign, 500 kSPS SAR ADC, TSSOP-14"
			(at 17.084 -16.51 0)
		)
		(property "ki_keywords" "Analog-Devices ADC bipolar 12-Bit SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AD7321_0_1")
		(symbol "AD7321_1_1"
			(pin power_in line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "REF_{IN/OUT}")
				(number "5")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "V_{IN}0")
				(number "7")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "V_{IN}1")
				(number "8")
			)
			(pin power_in line
				(at -5.08 17.78 270)
				(length 2.54)
				(name "V_{DD}")
				(number "9")
			)
			(pin power_in line
				(at -5.08 -17.78 90)
				(length 2.54)
				(name "V_{SS}")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 2.54)
				(name "AGND")
				(number "4")
			)
			(pin power_in line
				(at 5.08 17.78 270)
				(length 2.54)
				(name "V_{CC}")
				(number "10")
			)
			(pin passive line
				(at 5.08 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "DGND")
				(number "13")
			)
			(pin power_in line
				(at 5.08 -17.78 90)
				(length 2.54)
				(name "DGND")
				(number "3")
			)
			(pin power_in line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "V_{DRIVE}")
				(number "11")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "~{CS}")
				(number "1")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "DOUT")
				(number "12")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "DIN")
				(number "2")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "SCLK")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD7323"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 10.16 18.542 0)
		)
		(property "Value" "AD7323"
			(at 16.256 16.764 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 17.084 -14.224 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD7323.pdf"
			(at 17.084 -18.796 0)
		)
		(property "Description" "4-Channel, software selectable input range ±10 V, ±5V, ±2.5V, 0 V to +10 V, true bipolar input, 12-Bit plus sign, 500 kSPS SAR ADC, TSSOP-16"
			(at 17.084 -16.51 0)
		)
		(property "ki_keywords" "Analog-Devices ADC bipolar 12-Bit SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AD7323_0_1")
		(symbol "AD7323_1_1"
			(pin power_in line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "REF_{IN/OUT}")
				(number "5")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "V_{IN}0")
				(number "7")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "V_{IN}1")
				(number "8")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "V_{IN}2")
				(number "10")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "V_{IN}3")
				(number "9")
			)
			(pin power_in line
				(at -5.08 17.78 270)
				(length 2.54)
				(name "V_{DD}")
				(number "11")
			)
			(pin power_in line
				(at -5.08 -17.78 90)
				(length 2.54)
				(name "V_{SS}")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 2.54)
				(name "AGND")
				(number "4")
			)
			(pin power_in line
				(at 5.08 17.78 270)
				(length 2.54)
				(name "V_{CC}")
				(number "12")
			)
			(pin passive line
				(at 5.08 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "DGND")
				(number "15")
			)
			(pin power_in line
				(at 5.08 -17.78 90)
				(length 2.54)
				(name "DGND")
				(number "3")
			)
			(pin power_in line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "V_{DRIVE}")
				(number "13")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "~{CS}")
				(number "1")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "DOUT")
				(number "14")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "DIN")
				(number "2")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "SCLK")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD7327"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 10.16 21.082 0)
		)
		(property "Value" "AD7327"
			(at 16.256 19.304 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 17.084 -11.684 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ad7327.pdf"
			(at 17.084 -16.256 0)
		)
		(property "Description" "8-Channel, software selectable input range ±10 V, ±5V, ±2.5V, 0 V to +10 V, true bipolar input, 12-Bit plus sign, 500 kSPS SAR ADC, TSSOP-20"
			(at 17.084 -13.97 0)
		)
		(property "ki_keywords" "Analog-Devices ADC bipolar 12-Bit SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AD7327_0_1")
		(symbol "AD7327_1_1"
			(pin power_in line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "REF_{IN/OUT}")
				(number "5")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "V_{IN}0")
				(number "7")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "V_{IN}1")
				(number "8")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "V_{IN}2")
				(number "14")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "V_{IN}3")
				(number "13")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "V_{IN}4")
				(number "9")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "V_{IN}5")
				(number "10")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "V_{IN}6")
				(number "12")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "V_{IN}7")
				(number "11")
			)
			(pin power_in line
				(at -5.08 20.32 270)
				(length 2.54)
				(name "V_{DD}")
				(number "15")
			)
			(pin power_in line
				(at -5.08 -20.32 90)
				(length 2.54)
				(name "V_{SS}")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 2.54)
				(name "AGND")
				(number "4")
			)
			(pin power_in line
				(at 5.08 20.32 270)
				(length 2.54)
				(name "V_{CC}")
				(number "16")
			)
			(pin passive line
				(at 5.08 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "DGND")
				(number "19")
			)
			(pin power_in line
				(at 5.08 -20.32 90)
				(length 2.54)
				(name "DGND")
				(number "3")
			)
			(pin power_in line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "V_{DRIVE}")
				(number "17")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "~{CS}")
				(number "1")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "DOUT")
				(number "18")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "DIN")
				(number "2")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "SCLK")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD7329"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 10.16 26.416 0)
		)
		(property "Value" "AD7329"
			(at 16.256 24.384 0)
		)
		(property "Footprint" "Package_SO:TSSOP-24_4.4x7.8mm_P0.65mm"
			(at 17.084 -16.764 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD7329.pdf"
			(at 17.084 -22.098 0)
		)
		(property "Description" "8-Channel, software selectable input range ±10 V, ±5V, ±2.5V, 0 V to +10 V, true bipolar input, 12-Bit plus sign, 1 MSPS SAR ADC, TSSOP-24"
			(at 17.084 -19.558 0)
		)
		(property "ki_keywords" "Analog-Devices ADC bipolar 12-Bit SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x7.8mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AD7329_0_1")
		(symbol "AD7329_1_1"
			(pin power_in line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "REF_{IN/OUT}")
				(number "5")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "V_{IN}0")
				(number "9")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "V_{IN}1")
				(number "10")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "V_{IN}2")
				(number "16")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "V_{IN}3")
				(number "15")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "V_{IN}4")
				(number "11")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "V_{IN}5")
				(number "12")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "V_{IN}6")
				(number "14")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "V_{IN}7")
				(number "13")
			)
			(pin power_in line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "ADC_{IN}+")
				(number "7")
			)
			(pin power_in line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "ADC_{IN}-")
				(number "18")
			)
			(pin power_in line
				(at -5.08 25.4 270)
				(length 2.54)
				(name "V_{DD}")
				(number "19")
			)
			(pin power_in line
				(at -5.08 -25.4 90)
				(length 2.54)
				(name "V_{SS}")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -25.4 90)
				(length 2.54)
				(name "AGND")
				(number "4")
			)
			(pin power_in line
				(at 5.08 25.4 270)
				(length 2.54)
				(name "V_{CC}")
				(number "20")
			)
			(pin passive line
				(at 5.08 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "DGND")
				(number "23")
			)
			(pin power_in line
				(at 5.08 -25.4 90)
				(length 2.54)
				(name "DGND")
				(number "3")
			)
			(pin power_in line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "V_{DRIVE}")
				(number "21")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "~{CS}")
				(number "1")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "DOUT")
				(number "22")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "DIN")
				(number "2")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SCLK")
				(number "24")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "MUX_{OUT}+")
				(number "8")
			)
			(pin output line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "MUX_{OUT}-")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD7606"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "AD7606"
			(at 8.89 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 24.13 -44.45 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ad7606_7606-6_7606-4.pdf"
			(at 3.81 -82.55 90)
		)
		(property "Description" "8-Channel DAS with 16-Bit, Bipolar Input, Simultaneous Sampling ADC, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "16bit DAS ADC 8channel 200KSPS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AD7606_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "V1")
				(number "49")
			)
			(pin input line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "V1GND")
				(number "50")
			)
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "V2")
				(number "51")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "V2GND")
				(number "52")
			)
			(pin input line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "V3")
				(number "53")
			)
			(pin input line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "V3GND")
				(number "54")
			)
			(pin input line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "V4")
				(number "55")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "V4GND")
				(number "56")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "V5")
				(number "57")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "V5GND")
				(number "58")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "V6")
				(number "59")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "V6GND")
				(number "60")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "V7")
				(number "61")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "V7GND")
				(number "62")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "V8")
				(number "63")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "V8GND")
				(number "64")
			)
			(pin passive line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "REFIN/REFOUT")
				(number "42")
			)
			(pin passive line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "REGCAP")
				(number "36")
			)
			(pin passive line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "REGCAP")
				(number "39")
			)
			(pin passive line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "REFCAPA")
				(number "44")
			)
			(pin passive line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "REFCAPB")
				(number "45")
			)
			(pin power_in line
				(at -5.08 45.72 270)
				(length 2.54)
				(name "AVCC")
				(number "1")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "AVCC")
				(number "37")
			)
			(pin power_in line
				(at -2.54 -45.72 90)
				(length 2.54)
				(name "REFGND")
				(number "43")
			)
			(pin passive line
				(at -2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "REFGND")
				(number "46")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "AVCC")
				(number "38")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "AVCC")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 2.54)
				(name "AGND")
				(number "2")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "26")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "35")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "40")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "41")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "47")
			)
			(pin power_in line
				(at 7.62 45.72 270)
				(length 2.54)
				(name "Vdrive")
				(number "23")
			)
			(pin output line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "DB0")
				(number "16")
			)
			(pin output line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "DB1")
				(number "17")
			)
			(pin output line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "DB2")
				(number "18")
			)
			(pin output line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "DB3")
				(number "19")
			)
			(pin output line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "DB4")
				(number "20")
			)
			(pin output line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "DB5")
				(number "21")
			)
			(pin output line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "DB6")
				(number "22")
			)
			(pin output line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "DB7/DOUT_A")
				(number "24")
			)
			(pin output line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "DB8/DOUT_B")
				(number "25")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "DB9")
				(number "27")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "DB10")
				(number "28")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "DB11")
				(number "29")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "DB12")
				(number "30")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "DB13")
				(number "31")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "DB14/HBEN")
				(number "32")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "DB15/BYTE_SEL")
				(number "33")
			)
			(pin input line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "CONVST_A")
				(number "9")
			)
			(pin input line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "CONVST_B")
				(number "10")
			)
			(pin input line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "~{CS}")
				(number "13")
			)
			(pin input line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "~{RD}/SCLK")
				(number "12")
			)
			(pin output line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "BUSY")
				(number "14")
			)
			(pin output line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "FRSTDATA")
				(number "15")
			)
			(pin input line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "RESET")
				(number "11")
			)
			(pin input line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "REF_SELECT")
				(number "34")
			)
			(pin input line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "~{PAR}/SER/BYTE_SEL")
				(number "6")
			)
			(pin input line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "~{STBY}")
				(number "7")
			)
			(pin input line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "RANGE")
				(number "8")
			)
			(pin input line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "OS0")
				(number "3")
			)
			(pin input line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "OS1")
				(number "4")
			)
			(pin input line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "OS2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD7606-4"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "AD7606-4"
			(at 8.89 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 24.13 -44.45 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ad7606_7606-6_7606-4.pdf"
			(at 3.81 -82.55 90)
		)
		(property "Description" "4-Channel DAS with 16-Bit, Bipolar Input, Simultaneous Sampling ADC, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "16bit DAS ADC 4channel 200KSPS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AD7606-4_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "V1")
				(number "49")
			)
			(pin input line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "V1GND")
				(number "50")
			)
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "V2")
				(number "51")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "V2GND")
				(number "52")
			)
			(pin input line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "V3")
				(number "57")
			)
			(pin input line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "V3GND")
				(number "58")
			)
			(pin input line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "V4")
				(number "59")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "V4GND")
				(number "60")
			)
			(pin passive line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "REFIN/REFOUT")
				(number "42")
			)
			(pin passive line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "REGCAP")
				(number "36")
			)
			(pin passive line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "REGCAP")
				(number "39")
			)
			(pin passive line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "REFCAPA")
				(number "44")
			)
			(pin passive line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "REFCAPB")
				(number "45")
			)
			(pin power_in line
				(at -5.08 45.72 270)
				(length 2.54)
				(name "AVCC")
				(number "1")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "AVCC")
				(number "37")
			)
			(pin power_in line
				(at -2.54 -45.72 90)
				(length 2.54)
				(name "REFGND")
				(number "43")
			)
			(pin passive line
				(at -2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "REFGND")
				(number "46")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "AVCC")
				(number "38")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "AVCC")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 2.54)
				(name "AGND")
				(number "2")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "26")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "35")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "40")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "41")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "47")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "53")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "54")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "55")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "56")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "61")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "62")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "63")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "64")
			)
			(pin power_in line
				(at 7.62 45.72 270)
				(length 2.54)
				(name "Vdrive")
				(number "23")
			)
			(pin output line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "DB0")
				(number "16")
			)
			(pin output line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "DB1")
				(number "17")
			)
			(pin output line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "DB2")
				(number "18")
			)
			(pin output line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "DB3")
				(number "19")
			)
			(pin output line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "DB4")
				(number "20")
			)
			(pin output line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "DB5")
				(number "21")
			)
			(pin output line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "DB6")
				(number "22")
			)
			(pin output line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "DB7/DOUT_A")
				(number "24")
			)
			(pin output line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "DB8/DOUT_B")
				(number "25")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "DB9")
				(number "27")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "DB10")
				(number "28")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "DB11")
				(number "29")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "DB12")
				(number "30")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "DB13")
				(number "31")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "DB14/HBEN")
				(number "32")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "DB15/BYTE_SEL")
				(number "33")
			)
			(pin input line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "CONVST_A")
				(number "9")
			)
			(pin input line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "CONVST_B")
				(number "10")
			)
			(pin input line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "~{CS}")
				(number "13")
			)
			(pin input line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "~{RD}/SCLK")
				(number "12")
			)
			(pin output line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "BUSY")
				(number "14")
			)
			(pin output line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "FRSTDATA")
				(number "15")
			)
			(pin input line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "RESET")
				(number "11")
			)
			(pin input line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "REF_SELECT")
				(number "34")
			)
			(pin input line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "~{PAR}/SER/BYTE_SEL")
				(number "6")
			)
			(pin input line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "~{STBY}")
				(number "7")
			)
			(pin input line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "RANGE")
				(number "8")
			)
			(pin input line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "OS0")
				(number "3")
			)
			(pin input line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "OS1")
				(number "4")
			)
			(pin input line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "OS2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD7606-6"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "AD7606-6"
			(at 8.89 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 24.13 -44.45 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ad7606_7606-6_7606-4.pdf"
			(at 3.81 -82.55 90)
		)
		(property "Description" "6-Channel DAS with 16-Bit, Bipolar Input, Simultaneous Sampling ADC, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "16bit DAS ADC 6channel 200KSPS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AD7606-6_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "V1")
				(number "49")
			)
			(pin input line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "V1GND")
				(number "50")
			)
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "V2")
				(number "51")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "V2GND")
				(number "52")
			)
			(pin input line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "V3")
				(number "53")
			)
			(pin input line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "V3GND")
				(number "54")
			)
			(pin input line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "V4")
				(number "57")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "V4GND")
				(number "58")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "V5")
				(number "59")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "V5GND")
				(number "60")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "V6")
				(number "61")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "V6GND")
				(number "62")
			)
			(pin passive line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "REFIN/REFOUT")
				(number "42")
			)
			(pin passive line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "REGCAP")
				(number "36")
			)
			(pin passive line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "REGCAP")
				(number "39")
			)
			(pin passive line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "REFCAPA")
				(number "44")
			)
			(pin passive line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "REFCAPB")
				(number "45")
			)
			(pin power_in line
				(at -5.08 45.72 270)
				(length 2.54)
				(name "AVCC")
				(number "1")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "AVCC")
				(number "37")
			)
			(pin power_in line
				(at -2.54 -45.72 90)
				(length 2.54)
				(name "REFGND")
				(number "43")
			)
			(pin passive line
				(at -2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "REFGND")
				(number "46")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "AVCC")
				(number "38")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "AVCC")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 2.54)
				(name "AGND")
				(number "2")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "26")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "35")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "40")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "41")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "47")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "55")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "56")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "63")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "64")
			)
			(pin power_in line
				(at 7.62 45.72 270)
				(length 2.54)
				(name "Vdrive")
				(number "23")
			)
			(pin output line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "DB0")
				(number "16")
			)
			(pin output line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "DB1")
				(number "17")
			)
			(pin output line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "DB2")
				(number "18")
			)
			(pin output line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "DB3")
				(number "19")
			)
			(pin output line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "DB4")
				(number "20")
			)
			(pin output line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "DB5")
				(number "21")
			)
			(pin output line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "DB6")
				(number "22")
			)
			(pin output line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "DB7/DOUT_A")
				(number "24")
			)
			(pin output line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "DB8/DOUT_B")
				(number "25")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "DB9")
				(number "27")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "DB10")
				(number "28")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "DB11")
				(number "29")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "DB12")
				(number "30")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "DB13")
				(number "31")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "DB14/HBEN")
				(number "32")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "DB15/BYTE_SEL")
				(number "33")
			)
			(pin input line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "CONVST_A")
				(number "9")
			)
			(pin input line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "CONVST_B")
				(number "10")
			)
			(pin input line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "~{CS}")
				(number "13")
			)
			(pin input line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "~{RD}/SCLK")
				(number "12")
			)
			(pin output line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "BUSY")
				(number "14")
			)
			(pin output line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "FRSTDATA")
				(number "15")
			)
			(pin input line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "RESET")
				(number "11")
			)
			(pin input line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "REF_SELECT")
				(number "34")
			)
			(pin input line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "~{PAR}/SER/BYTE_SEL")
				(number "6")
			)
			(pin input line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "~{STBY}")
				(number "7")
			)
			(pin input line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "RANGE")
				(number "8")
			)
			(pin input line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "OS0")
				(number "3")
			)
			(pin input line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "OS1")
				(number "4")
			)
			(pin input line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "OS2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD7616"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 57.15 0)
		)
		(property "Value" "AD7616"
			(at 17.78 57.15 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_14x14mm_P0.65mm"
			(at 33.02 -57.15 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD7616.pdf"
			(at 2.54 -76.2 0)
		)
		(property "Description" "16-Channel DAS with 16-Bit, Bipolar Input, Dual Simultaneous Sampling ADC, 2x1MSPS ADC, Serial and parallel IO, LQFP-80"
			(at 0 0 0)
		)
		(property "ki_keywords" "16bit DAS ADC 16channel 1MSPS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AD7616_1_1"
			(pin input line
				(at -27.94 53.34 0)
				(length 2.54)
				(name "V0A")
				(number "28")
			)
			(pin input line
				(at -27.94 50.8 0)
				(length 2.54)
				(name "V0AGND")
				(number "27")
			)
			(pin input line
				(at -27.94 48.26 0)
				(length 2.54)
				(name "V1A")
				(number "26")
			)
			(pin input line
				(at -27.94 45.72 0)
				(length 2.54)
				(name "V1AGND")
				(number "25")
			)
			(pin input line
				(at -27.94 43.18 0)
				(length 2.54)
				(name "V2A")
				(number "24")
			)
			(pin input line
				(at -27.94 40.64 0)
				(length 2.54)
				(name "V2AGND")
				(number "23")
			)
			(pin input line
				(at -27.94 38.1 0)
				(length 2.54)
				(name "V3A")
				(number "22")
			)
			(pin input line
				(at -27.94 35.56 0)
				(length 2.54)
				(name "V3AGND")
				(number "21")
			)
			(pin input line
				(at -27.94 33.02 0)
				(length 2.54)
				(name "V4A")
				(number "19")
			)
			(pin input line
				(at -27.94 30.48 0)
				(length 2.54)
				(name "V4AGND")
				(number "20")
			)
			(pin input line
				(at -27.94 27.94 0)
				(length 2.54)
				(name "V5A")
				(number "17")
			)
			(pin input line
				(at -27.94 25.4 0)
				(length 2.54)
				(name "V5AGND")
				(number "18")
			)
			(pin input line
				(at -27.94 22.86 0)
				(length 2.54)
				(name "V6A")
				(number "14")
			)
			(pin input line
				(at -27.94 20.32 0)
				(length 2.54)
				(name "V6AGND")
				(number "13")
			)
			(pin input line
				(at -27.94 17.78 0)
				(length 2.54)
				(name "V7A")
				(number "12")
			)
			(pin input line
				(at -27.94 15.24 0)
				(length 2.54)
				(name "V7AGND")
				(number "11")
			)
			(pin input line
				(at -27.94 12.7 0)
				(length 2.54)
				(name "V0B")
				(number "73")
			)
			(pin input line
				(at -27.94 10.16 0)
				(length 2.54)
				(name "V0BGND")
				(number "74")
			)
			(pin input line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "V1B")
				(number "75")
			)
			(pin input line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "V1BGND")
				(number "76")
			)
			(pin input line
				(at -27.94 2.54 0)
				(length 2.54)
				(name "V2B")
				(number "77")
			)
			(pin input line
				(at -27.94 0 0)
				(length 2.54)
				(name "V2BGND")
				(number "78")
			)
			(pin input line
				(at -27.94 -2.54 0)
				(length 2.54)
				(name "V3B")
				(number "79")
			)
			(pin input line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "V3BGND")
				(number "80")
			)
			(pin input line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "V4B")
				(number "2")
			)
			(pin input line
				(at -27.94 -10.16 0)
				(length 2.54)
				(name "V4BGND")
				(number "1")
			)
			(pin input line
				(at -27.94 -12.7 0)
				(length 2.54)
				(name "V5B")
				(number "4")
			)
			(pin input line
				(at -27.94 -15.24 0)
				(length 2.54)
				(name "V5BGND")
				(number "3")
			)
			(pin input line
				(at -27.94 -17.78 0)
				(length 2.54)
				(name "V6B")
				(number "7")
			)
			(pin input line
				(at -27.94 -20.32 0)
				(length 2.54)
				(name "V6BGND")
				(number "8")
			)
			(pin input line
				(at -27.94 -22.86 0)
				(length 2.54)
				(name "V7B")
				(number "9")
			)
			(pin input line
				(at -27.94 -25.4 0)
				(length 2.54)
				(name "V7BGND")
				(number "10")
			)
			(pin input line
				(at -27.94 -33.02 0)
				(length 2.54)
				(name "REFINOUT")
				(number "33")
			)
			(pin power_in line
				(at -27.94 -38.1 0)
				(length 2.54)
				(name "REFINOUTGND")
				(number "34")
			)
			(pin passive line
				(at -27.94 -40.64 0)
				(length 2.54)
				(name "REFCAP")
				(number "31")
			)
			(pin power_in line
				(at -27.94 -45.72 0)
				(length 2.54)
				(name "REFGND")
				(number "32")
			)
			(pin passive line
				(at -27.94 -48.26 0)
				(length 2.54)
				(name "REGCAP")
				(number "70")
			)
			(pin power_in line
				(at -27.94 -53.34 0)
				(length 2.54)
				(name "REGGND")
				(number "69")
			)
			(pin power_in line
				(at -10.16 58.42 270)
				(length 2.54)
				(name "VCC")
				(number "6")
			)
			(pin power_in line
				(at -7.62 58.42 270)
				(length 2.54)
				(name "VCC")
				(number "15")
			)
			(pin power_in line
				(at -5.08 58.42 270)
				(length 2.54)
				(name "VCC")
				(number "30")
			)
			(pin power_in line
				(at -2.54 58.42 270)
				(length 2.54)
				(name "VCC")
				(number "71")
			)
			(pin passive line
				(at -2.54 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "16")
			)
			(pin passive line
				(at -2.54 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "29")
			)
			(pin power_in line
				(at -2.54 -58.42 90)
				(length 2.54)
				(name "AGND")
				(number "5")
			)
			(pin passive line
				(at -2.54 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "72")
			)
			(pin power_in line
				(at 2.54 58.42 270)
				(length 2.54)
				(name "VDRIVE")
				(number "49")
			)
			(pin power_in line
				(at 2.54 -58.42 90)
				(length 2.54)
				(name "DGND")
				(number "50")
			)
			(pin input line
				(at 27.94 53.34 180)
				(length 2.54)
				(name "~{RESET}")
				(number "36")
			)
			(pin input line
				(at 27.94 50.8 180)
				(length 2.54)
				(name "SEQEN")
				(number "37")
			)
			(pin input line
				(at 27.94 45.72 180)
				(length 2.54)
				(name "HW_RNGSEL0")
				(number "39")
			)
			(pin input line
				(at 27.94 43.18 180)
				(length 2.54)
				(name "HW_RNGSEL1")
				(number "38")
			)
			(pin input line
				(at 27.94 38.1 180)
				(length 2.54)
				(name "SER/~{PAR}")
				(number "40")
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 2.54)
				(name "DB0")
				(number "41")
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 2.54)
				(name "DB1")
				(number "42")
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 2.54)
				(name "DB2")
				(number "43")
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 2.54)
				(name "DB3")
				(number "44")
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 2.54)
				(name "DB4/~{SER1W}")
				(number "45")
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 2.54)
				(name "DB5/CRCEN")
				(number "46")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 2.54)
				(name "DB6")
				(number "47")
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 2.54)
				(name "DB7")
				(number "48")
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 2.54)
				(name "DB8")
				(number "53")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 2.54)
				(name "DB9")
				(number "54")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 2.54)
				(name "DB10/SDI")
				(number "55")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 2.54)
				(name "DB11/SDOB")
				(number "56")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 2.54)
				(name "DB12/SDOA")
				(number "57")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 2.54)
				(name "DB13/OS0")
				(number "58")
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "DB14/OS1")
				(number "59")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "DB15/OS2")
				(number "60")
			)
			(pin input line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "BURST/~{WR}")
				(number "61")
			)
			(pin input line
				(at 27.94 -12.7 180)
				(length 2.54)
				(name "SCLK/~{RD}")
				(number "62")
			)
			(pin input line
				(at 27.94 -15.24 180)
				(length 2.54)
				(name "~{CS}")
				(number "63")
			)
			(pin input line
				(at 27.94 -20.32 180)
				(length 2.54)
				(name "CHSEL0")
				(number "64")
			)
			(pin input line
				(at 27.94 -22.86 180)
				(length 2.54)
				(name "CHSEL1")
				(number "65")
			)
			(pin input line
				(at 27.94 -25.4 180)
				(length 2.54)
				(name "CHSEL2")
				(number "66")
			)
			(pin output line
				(at 27.94 -30.48 180)
				(length 2.54)
				(name "BUSY")
				(number "67")
			)
			(pin input line
				(at 27.94 -33.02 180)
				(length 2.54)
				(name "CONVST")
				(number "68")
			)
			(pin input line
				(at 27.94 -35.56 180)
				(length 2.54)
				(name "REFSEL")
				(number "35")
			)
			(pin passive line
				(at 27.94 -48.26 180)
				(length 2.54)
				(name "REGCAPD")
				(number "52")
			)
			(pin power_in line
				(at 27.94 -53.34 180)
				(length 2.54)
				(name "REGGNDD")
				(number "51")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD7682BCP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.89 13.97 0)
		)
		(property "Value" "AD7682BCP"
			(at -10.16 13.97 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-20-1EP_4x4mm_P0.5mm_EP2.5x2.5mm"
			(at 0 -21.59 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD7682_7689.pdf"
			(at 0 -25.4 0)
		)
		(property "Description" "16-bit, 4-Channel, 250kSPS, PulSAR ADC, Bipolar-Unipolar, LFCSP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "16-Bit 4-Channel 250kSPS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AD7682BCP_0_1")
		(symbol "AD7682BCP_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "IN0")
				(number "16")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "IN1")
				(number "18")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "IN2")
				(number "7")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "IN3")
				(number "9")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "REF")
				(number "2")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "REFIN")
				(number "3")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "COM")
				(number "10")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at -2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin passive line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "EPAD")
				(number "21")
			)
			(pin power_in line
				(at 5.08 15.24 270)
				(length 2.54)
				(name "VIO")
				(number "15")
			)
			(pin no_connect line
				(at 10.16 7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 10.16 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "19")
			)
			(pin no_connect line
				(at 10.16 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin no_connect line
				(at 10.16 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "CNV")
				(number "11")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "SCK")
				(number "13")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "DIN")
				(number "12")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SDO")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD7722"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "AD7722"
			(at 5.08 36.83 0)
		)
		(property "Footprint" "Package_QFP:MQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD7722.pdf"
			(at 0 0 0)
		)
		(property "Description" "16-Bit, 195 kSPS CMOS, Sigma-Delta ADC, MQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "adc 1ch 16bit parallel serial"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "AD7722_0_1")
		(symbol "AD7722_1_1"
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "VIN+")
				(number "18")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "VIN-")
				(number "16")
			)
			(pin power_out line
				(at -15.24 0 0)
				(length 2.54)
				(name "REF1")
				(number "22")
			)
			(pin power_out line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "REF2")
				(number "24")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "~{UNI}")
				(number "7")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "AVDD")
				(number "20")
			)
			(pin passive line
				(at -2.54 38.1 270)
				(length 2.54)
				(hide yes)
				(name "AVDD")
				(number "23")
			)
			(pin passive line
				(at -2.54 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "13")
			)
			(pin passive line
				(at -2.54 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "15")
			)
			(pin passive line
				(at -2.54 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "19")
			)
			(pin passive line
				(at -2.54 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "21")
			)
			(pin passive line
				(at -2.54 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "25")
			)
			(pin passive line
				(at -2.54 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "26")
			)
			(pin power_in line
				(at -2.54 -38.1 90)
				(length 2.54)
				(name "AGND")
				(number "9")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "AVDD1")
				(number "14")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "AGND1")
				(number "10")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "DVDD")
				(number "39")
			)
			(pin passive line
				(at 2.54 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "DGND")
				(number "28")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 2.54)
				(name "DGND")
				(number "6")
			)
			(pin output line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "DB15")
				(number "31")
			)
			(pin output line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "DB14")
				(number "32")
			)
			(pin output line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "DB13")
				(number "33")
			)
			(pin output line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "DB12")
				(number "34")
			)
			(pin output line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "DB11")
				(number "35")
			)
			(pin output line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "DB10")
				(number "36")
			)
			(pin output line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "FSO/DB9")
				(number "37")
			)
			(pin output line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "SDO/DB8")
				(number "38")
			)
			(pin input line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "SCO/DB7")
				(number "40")
			)
			(pin input line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "FSI/DB6")
				(number "41")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "SFMT/DB5")
				(number "42")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "DOE/DB4")
				(number "43")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "TSI/DB3")
				(number "44")
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "DB2")
				(number "1")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "DB1")
				(number "2")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "DB0")
				(number "3")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "CLKIN")
				(number "11")
			)
			(pin output line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "XTAL")
				(number "12")
			)
			(pin input line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "SYNC")
				(number "30")
			)
			(pin input line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "~{CS}")
				(number "29")
			)
			(pin input line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "CFMT/~{DRDY}")
				(number "4")
			)
			(pin input line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "DVAL/~{RD}")
				(number "5")
			)
			(pin input line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "RESET")
				(number "17")
			)
			(pin input line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "CAL")
				(number "27")
			)
			(pin input line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "P/~{S}")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD7745"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 18.415 0)
		)
		(property "Value" "AD7745"
			(at 10.16 18.415 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 21.59 -19.05 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD7745_7746.pdf"
			(at 0 0 0)
		)
		(property "Description" "24-bit capacitance-to-digital converter with temperature sensor, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "adc cdc capacitance"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AD7745_0_1")
		(symbol "AD7745_1_1"
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "REFIN+")
				(number "5")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "REFIN-")
				(number "6")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "VIN+")
				(number "11")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VIN-")
				(number "12")
			)
			(pin passive line
				(at -12.7 0 0)
				(length 2.54)
				(name "CIN1+")
				(number "8")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "CIN1-")
				(number "7")
			)
			(pin output line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "EXCA")
				(number "3")
			)
			(pin output line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "EXCB")
				(number "4")
			)
			(pin no_connect line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at -10.16 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin no_connect line
				(at 10.16 -15.24 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin input line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "SCL")
				(number "1")
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "SDA")
				(number "16")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "~{RDY}")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD7746"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 18.415 0)
		)
		(property "Value" "AD7746"
			(at 10.16 18.415 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 21.59 -19.05 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD7745_7746.pdf"
			(at 0 0 0)
		)
		(property "Description" "24-bit capacitance-to-digital converter with temperature sensor, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "adc cdc capacitance"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AD7746_0_1")
		(symbol "AD7746_1_1"
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "REFIN+")
				(number "5")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "REFIN-")
				(number "6")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "VIN+")
				(number "11")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VIN-")
				(number "12")
			)
			(pin passive line
				(at -12.7 0 0)
				(length 2.54)
				(name "CIN1+")
				(number "8")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "CIN1-")
				(number "7")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "CIN2+")
				(number "9")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "CIN2-")
				(number "10")
			)
			(pin output line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "EXCA")
				(number "3")
			)
			(pin output line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "EXCB")
				(number "4")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin no_connect line
				(at 10.16 -15.24 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin input line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "SCL")
				(number "1")
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "SDA")
				(number "16")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "~{RDY}")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD7794"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 24.13 0)
		)
		(property "Value" "AD7794"
			(at 7.62 24.13 0)
		)
		(property "Footprint" "Package_SO:TSSOP-24_4.4x7.8mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD7794_7795.pdf"
			(at 2.54 -7.62 0)
		)
		(property "Description" "24-Bit, 6-Channel Sigma-Delta ADC, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "adc 6ch 24bit serial"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x7.8mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AD7794_0_1")
		(symbol "AD7794_1_1"
			(pin input line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "AIN1+")
				(number "7")
			)
			(pin input line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "AIN1-")
				(number "8")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "AIN2+")
				(number "9")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "AIN2-")
				(number "10")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "AIN3+")
				(number "11")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "AIN3-")
				(number "12")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "AIN4+/REFIN2+")
				(number "17")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "AIN4-/REFIN2-")
				(number "18")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "AIN5+/IOUT2")
				(number "15")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "AIN5-/IOUT1")
				(number "16")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "AIN6+/P1")
				(number "5")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "AIN6-/P2")
				(number "6")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "REFIN1+")
				(number "13")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "REFIN1-")
				(number "14")
			)
			(pin passive line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PSW")
				(number "19")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "AVDD")
				(number "21")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "20")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "DVDD")
				(number "22")
			)
			(pin no_connect line
				(at 15.24 -20.32 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "DOUT/~{RDY}")
				(number "23")
			)
			(pin input line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "DIN")
				(number "24")
			)
			(pin input line
				(at 17.78 0 180)
				(length 2.54)
				(name "~{CS}")
				(number "3")
			)
			(pin input line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "SCLK")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "CLK")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD7819"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 17.78 0)
		)
		(property "Value" "AD7819"
			(at 3.81 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD7819.pdf"
			(at 0 0 0)
		)
		(property "Description" "Analog to Digital 8 bits converter, PDIP/SOIC/TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "CAD"
			(at 0 0 0)
		)
		(symbol "AD7819_0_1")
		(symbol "AD7819_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 3.81)
				(name "Vin")
				(number "2")
			)
			(pin input line
				(at -12.7 0 0)
				(length 3.81)
				(name "VREF")
				(number "1")
			)
			(pin input inverted_clock
				(at -12.7 -7.62 0)
				(length 3.81)
				(name "START")
				(number "4")
			)
			(pin input input_low
				(at -12.7 -10.16 0)
				(length 3.81)
				(name "CS")
				(number "5")
			)
			(pin input input_low
				(at -12.7 -12.7 0)
				(length 3.81)
				(name "OE")
				(number "6")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "GND")
				(number "3")
			)
			(pin tri_state line
				(at 12.7 12.7 180)
				(length 3.81)
				(name "DB0")
				(number "8")
			)
			(pin tri_state line
				(at 12.7 10.16 180)
				(length 3.81)
				(name "DB1")
				(number "9")
			)
			(pin tri_state line
				(at 12.7 7.62 180)
				(length 3.81)
				(name "DB2")
				(number "10")
			)
			(pin tri_state line
				(at 12.7 5.08 180)
				(length 3.81)
				(name "DB3")
				(number "11")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 3.81)
				(name "DB4")
				(number "12")
			)
			(pin tri_state line
				(at 12.7 0 180)
				(length 3.81)
				(name "DB5")
				(number "13")
			)
			(pin tri_state line
				(at 12.7 -2.54 180)
				(length 3.81)
				(name "DB6")
				(number "14")
			)
			(pin tri_state line
				(at 12.7 -5.08 180)
				(length 3.81)
				(name "DB7")
				(number "15")
			)
			(pin output output_low
				(at 12.7 -12.7 180)
				(length 3.81)
				(name "EOC")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD7949BCP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 16.51 0)
		)
		(property "Value" "AD7949BCP"
			(at 3.81 16.51 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-20-1EP_4x4mm_P0.5mm_EP2.5x2.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD7949.pdf"
			(at 0 0 0)
		)
		(property "Description" "14-Bit, 8-Channel, 250 kSPS PulSAR ADC, LFSCP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC, SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AD7949BCP_0_1")
		(symbol "AD7949BCP_1_1"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "IN0")
				(number "16")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "IN1")
				(number "17")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "IN2")
				(number "18")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "IN3")
				(number "19")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "IN4")
				(number "6")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "IN5")
				(number "7")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "IN6")
				(number "8")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "IN7")
				(number "9")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "COM")
				(number "10")
			)
			(pin passive line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "REF")
				(number "2")
			)
			(pin passive line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "REFIN")
				(number "3")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin passive line
				(at -2.54 17.78 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at -2.54 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "VIO")
				(number "15")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "EPAD")
				(number "21")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CNV")
				(number "11")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "SDO")
				(number "14")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "DIN")
				(number "12")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "SCK")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD9280ARS"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 25.4 0)
		)
		(property "Value" "AD9280ARS"
			(at 7.62 25.4 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD9280.pdf"
			(at 0 0 0)
		)
		(property "Description" "Video ADC (32 Mhz), SSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC CAN VIDEO"
			(at 0 0 0)
		)
		(symbol "AD9280ARS_0_1")
		(symbol "AD9280ARS_1_1"
			(pin input line
				(at -17.78 20.32 0)
				(length 3.81)
				(name "AIN")
				(number "27")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "CLAMPIN")
				(number "20")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "MODE")
				(number "23")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "REFTF")
				(number "22")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "REFTS")
				(number "21")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "REFBS")
				(number "25")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "REFBF")
				(number "24")
			)
			(pin output line
				(at -17.78 -10.16 0)
				(length 3.81)
				(name "VREF")
				(number "26")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 3.81)
				(name "REFSENSE")
				(number "18")
			)
			(pin power_in line
				(at -5.08 27.94 270)
				(length 3.81)
				(name "AVDD")
				(number "28")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 3.81)
				(name "AVSS")
				(number "1")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 3.81)
				(name "DRVSS")
				(number "14")
			)
			(pin power_in line
				(at 5.08 27.94 270)
				(length 3.81)
				(name "DRVDD")
				(number "2")
			)
			(pin passive line
				(at 17.78 20.32 180)
				(length 3.81)
				(name "CLAMP")
				(number "19")
			)
			(pin passive line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "STBY")
				(number "17")
			)
			(pin input line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "THREE-STATE")
				(number "16")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "OTR")
				(number "13")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "D0")
				(number "5")
			)
			(pin output line
				(at 17.78 0 180)
				(length 3.81)
				(name "D1")
				(number "6")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "D2")
				(number "7")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "D3")
				(number "8")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "D4")
				(number "9")
			)
			(pin output line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "D5")
				(number "10")
			)
			(pin output line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "D6")
				(number "11")
			)
			(pin output line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "D7")
				(number "12")
			)
			(pin input clock
				(at 17.78 -20.32 180)
				(length 3.81)
				(name "CLK")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD9283"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 17.78 0)
		)
		(property "Value" "AD9283"
			(at 6.35 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD9283.pdf"
			(at 0 0 0)
		)
		(property "Description" "ADC 50MHz 8 bits, SSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC"
			(at 0 0 0)
		)
		(symbol "AD9283_0_1")
		(symbol "AD9283_1_1"
			(pin input line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "Ain+")
				(number "7")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "Ain-")
				(number "6")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "VREFin")
				(number "3")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 3.81)
				(name "VREFout")
				(number "2")
			)
			(pin power_in line
				(at -5.08 20.32 270)
				(length 3.81)
				(name "VaD")
				(number "5")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 3.81)
				(name "VaD")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 3.81)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 3.81)
				(name "VDD")
				(number "15")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 3.81)
				(name "GND")
				(number "16")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "DO0")
				(number "20")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "DO1")
				(number "19")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "DO2")
				(number "18")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "DO3")
				(number "17")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "DO4")
				(number "14")
			)
			(pin output line
				(at 17.78 0 180)
				(length 3.81)
				(name "DO5")
				(number "13")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "DO6")
				(number "12")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "DO7")
				(number "11")
			)
			(pin input clock
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "CLK")
				(number "10")
			)
			(pin input line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "PWRDWN")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADC0800"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 17.78 0)
		)
		(property "Value" "ADC0800"
			(at 5.08 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/snas562/snas562.pdf"
			(at 0 0 0)
		)
		(property "Description" "Analog to Digital 8 bits converter, DIP-18 (Hermetic)"
			(at 0 0 0)
		)
		(property "ki_keywords" "CAD"
			(at 0 0 0)
		)
		(symbol "ADC0800_0_1")
		(symbol "ADC0800_1_1"
			(pin input clock
				(at -15.24 12.7 0)
				(length 3.81)
				(name "Clk")
				(number "11")
			)
			(pin input clock
				(at -15.24 7.62 0)
				(length 3.81)
				(name "Start")
				(number "6")
			)
			(pin input inverted
				(at -15.24 2.54 0)
				(length 3.81)
				(name "Vin")
				(number "12")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "Rtop")
				(number "15")
			)
			(pin input inverted
				(at -15.24 -5.08 0)
				(length 3.81)
				(name "Rbot")
				(number "5")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 3.81)
				(name "OE")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 3.81)
				(name "-Vgg")
				(number "8")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "VCC")
				(number "10")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 3.81)
				(name "DGND")
				(number "18")
			)
			(pin tri_state line
				(at 15.24 12.7 180)
				(length 3.81)
				(name "QA")
				(number "13")
			)
			(pin tri_state line
				(at 15.24 10.16 180)
				(length 3.81)
				(name "QB")
				(number "14")
			)
			(pin tri_state line
				(at 15.24 7.62 180)
				(length 3.81)
				(name "QC")
				(number "16")
			)
			(pin tri_state line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "QD")
				(number "17")
			)
			(pin tri_state line
				(at 15.24 2.54 180)
				(length 3.81)
				(name "QE")
				(number "1")
			)
			(pin tri_state line
				(at 15.24 0 180)
				(length 3.81)
				(name "QF")
				(number "2")
			)
			(pin tri_state line
				(at 15.24 -2.54 180)
				(length 3.81)
				(name "QG")
				(number "3")
			)
			(pin tri_state line
				(at 15.24 -5.08 180)
				(length 3.81)
				(name "QH")
				(number "4")
			)
			(pin output line
				(at 15.24 -12.7 180)
				(length 3.81)
				(name "EOC")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADC08060"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -16.51 17.78 0)
		)
		(property "Value" "ADC08060"
			(at 8.89 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/adc08060.pdf"
			(at 0 0 0)
		)
		(property "Description" "Fast ADC  (20 .. 60 Mhz), TSSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC CAN VIDEO"
			(at 0 0 0)
		)
		(symbol "ADC08060_0_1")
		(symbol "ADC08060_1_1"
			(pin input line
				(at -20.32 10.16 0)
				(length 3.81)
				(name "AIN")
				(number "6")
			)
			(pin input line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "VIN_GND")
				(number "7")
			)
			(pin input line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "VRT")
				(number "3")
			)
			(pin input line
				(at -20.32 -10.16 0)
				(length 3.81)
				(name "VRB")
				(number "9")
			)
			(pin input line
				(at -20.32 -12.7 0)
				(length 3.81)
				(name "VRB")
				(number "10")
			)
			(pin power_in line
				(at -7.62 20.32 270)
				(length 3.81)
				(name "AVDD")
				(number "1")
			)
			(pin power_in line
				(at -7.62 -20.32 90)
				(length 3.81)
				(name "AGND")
				(number "2")
			)
			(pin power_in line
				(at -5.08 20.32 270)
				(length 3.81)
				(name "AVDD")
				(number "4")
			)
			(pin power_in line
				(at -5.08 -20.32 90)
				(length 3.81)
				(name "AGND")
				(number "5")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 3.81)
				(name "AVDD")
				(number "12")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 3.81)
				(name "AGND")
				(number "11")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 3.81)
				(name "DVDD")
				(number "18")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 3.81)
				(name "DGND")
				(number "8")
			)
			(pin power_in line
				(at 5.08 -20.32 90)
				(length 3.81)
				(name "DGND")
				(number "17")
			)
			(pin tri_state line
				(at 20.32 12.7 180)
				(length 3.81)
				(name "D0")
				(number "13")
			)
			(pin tri_state line
				(at 20.32 10.16 180)
				(length 3.81)
				(name "D1")
				(number "14")
			)
			(pin tri_state line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "D2")
				(number "15")
			)
			(pin tri_state line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "D3")
				(number "16")
			)
			(pin tri_state line
				(at 20.32 2.54 180)
				(length 3.81)
				(name "D4")
				(number "19")
			)
			(pin tri_state line
				(at 20.32 0 180)
				(length 3.81)
				(name "D5")
				(number "20")
			)
			(pin tri_state line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "D6")
				(number "21")
			)
			(pin tri_state line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "D7")
				(number "22")
			)
			(pin input clock
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "CLK")
				(number "24")
			)
			(pin input line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "PWR_DWN")
				(number "23")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADC081C021CIMM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 11.43 0)
		)
		(property "Value" "ADC081C021CIMM"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 20.32 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/adc081c021.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "I2C-Compatible, 8-Bit Analog-to-Digital Converter with Alert Function, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC I2C 8-bit Alert"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADC081C021CIMM_0_1")
		(symbol "ADC081C021CIMM_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "4")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "ADR0")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "ADR1")
				(number "6")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VA")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SCL")
				(number "1")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "SDA")
				(number "8")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "ALERT")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADC0832"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 7.62 0)
		)
		(property "Value" "ADC0832"
			(at 3.81 7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/adc0831-n.pdf"
			(at 0 0 0)
		)
		(property "Description" "2 inputs AD Converter (serial output),"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC CAN"
			(at 0 0 0)
		)
		(symbol "ADC0832_0_1")
		(symbol "ADC0832_1_1"
			(pin input line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "ANALOG0")
				(number "2")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "ANALOG1")
				(number "3")
			)
			(pin input line
				(at 0 10.16 270)
				(length 3.81)
				(name "VCC")
				(number "8")
			)
			(pin input line
				(at 0 -10.16 90)
				(length 3.81)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "DOUT")
				(number "6")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 3.81)
				(name "DIN")
				(number "5")
			)
			(pin input clock
				(at 15.24 0 180)
				(length 3.81)
				(name "CLK")
				(number "7")
			)
			(pin input inverted
				(at 15.24 -2.54 180)
				(length 3.81)
				(name "CS")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADC101C021CIMK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 11.43 0)
		)
		(property "Value" "ADC101C021CIMK"
			(at 11.43 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/adc101c021.pdf"
			(at 0 0 0)
		)
		(property "Description" "10-bit I2C ADC, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "adc 10-bit i2c"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "ADC101C021CIMK_0_1")
		(symbol "ADC101C021CIMK_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "V_{IN}")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V_{A}")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "6")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "5")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "ADDR")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADC1173"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 19.05 0)
		)
		(property "Value" "ADC1173"
			(at 8.89 19.05 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/adc1173.pdf"
			(at 0 0 0)
		)
		(property "Description" "Fast ADC  (15 Mhz), TSSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC CAN VIDEO"
			(at 0 0 0)
		)
		(symbol "ADC1173_0_1")
		(symbol "ADC1173_1_1"
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "VIN")
				(number "19")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "VRTS")
				(number "16")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "VRT")
				(number "17")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "VRB")
				(number "23")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "VRBS")
				(number "22")
			)
			(pin power_in line
				(at -7.62 20.32 270)
				(length 2.54)
				(name "AVDD")
				(number "14")
			)
			(pin power_in line
				(at -5.08 20.32 270)
				(length 2.54)
				(name "AVDD")
				(number "15")
			)
			(pin power_in line
				(at -5.08 -20.32 90)
				(length 2.54)
				(name "AVSS")
				(number "20")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 2.54)
				(name "AVDD")
				(number "18")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 2.54)
				(name "AVSS")
				(number "21")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "DVDD")
				(number "11")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "DVSS")
				(number "2")
			)
			(pin power_in line
				(at 5.08 20.32 270)
				(length 2.54)
				(name "DVDD")
				(number "13")
			)
			(pin power_in line
				(at 5.08 -20.32 90)
				(length 2.54)
				(name "DVSS")
				(number "24")
			)
			(pin tri_state line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "D0")
				(number "3")
			)
			(pin tri_state line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "D1")
				(number "4")
			)
			(pin tri_state line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "D2")
				(number "5")
			)
			(pin tri_state line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "D3")
				(number "6")
			)
			(pin tri_state line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "D4")
				(number "7")
			)
			(pin tri_state line
				(at 17.78 0 180)
				(length 2.54)
				(name "D5")
				(number "8")
			)
			(pin tri_state line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "D6")
				(number "9")
			)
			(pin tri_state line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "D7")
				(number "10")
			)
			(pin input line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "CLK")
				(number "12")
			)
			(pin input line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "OE")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADC1283"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 13.97 0)
		)
		(property "Value" "ADC1283"
			(at 0 0 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/adc1283.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low power 8-channel single ended 12-bit SAR ADC, 50 ksps to 200 ksps, SPI, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC 2.7V 3.3V 5.5V SPI 12bit 8-channel"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADC1283_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "IN0")
				(number "4")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "IN1")
				(number "5")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "IN2")
				(number "6")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "IN3")
				(number "7")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "IN4")
				(number "8")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "IN5")
				(number "9")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "IN6")
				(number "10")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "IN7")
				(number "11")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "AVCC")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "AGND")
				(number "3")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "DVCC")
				(number "13")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "DGND")
				(number "12")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "~{CS}")
				(number "1")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "SCLK")
				(number "16")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "DIN")
				(number "14")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "DOUT")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADC128D818"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 19.05 0)
		)
		(property "Value" "ADC128D818"
			(at 1.27 19.05 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/adc128d818.pdf"
			(at 0 0 0)
		)
		(property "Description" "12-Bit, 8-Channel, ADC System Monitor With Temperature Sensor, I2C Interface, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC 8 Channels TSSOP I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADC128D818_0_1")
		(symbol "ADC128D818_1_1"
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "IN0")
				(number "16")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "IN1")
				(number "15")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "IN2")
				(number "14")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "IN3")
				(number "13")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "IN4")
				(number "12")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "IN5")
				(number "11")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "IN6")
				(number "10")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "IN7")
				(number "9")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "VREF")
				(number "1")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "A0")
				(number "7")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "A1")
				(number "8")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "V+")
				(number "5")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "SDA")
				(number "2")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "SCL")
				(number "3")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "~{INT}")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADS1013IDGS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 13.97 0)
		)
		(property "Value" "ADS1013IDGS"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_SO:TSSOP-10_3x3mm_P0.5mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads1015.pdf"
			(at 1.27 -17.78 0)
		)
		(property "Description" "Ultra-Small, Low-Power, I2C-Compatible, 3.3-kSPS, 12-Bit ADCs With Internal Reference and Oscillator, VSSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "12 bit single channel I2C ADC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ADS1013IDGS_0_1")
		(symbol "ADS1013IDGS_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "AIN0")
				(number "4")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "AIN1")
				(number "5")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin no_connect line
				(at 7.62 7.62 180)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "2")
			)
			(pin no_connect line
				(at 7.62 5.08 180)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "6")
			)
			(pin no_connect line
				(at 7.62 2.54 180)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "7")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "10")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SDA")
				(number "9")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "ADDR")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADS1014IDGS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 13.97 0)
		)
		(property "Value" "ADS1014IDGS"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_SO:TSSOP-10_3x3mm_P0.5mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads1015.pdf"
			(at -1.27 -22.86 0)
		)
		(property "Description" "Ultra-Small, Low-Power, I2C-Compatible, 3.3-kSPS, 12-Bit ADCs With Internal Reference, Oscillator, and Programmable Comparator, VSSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "12 bit single channel I2C ADC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ADS1014IDGS_0_1")
		(symbol "ADS1014IDGS_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "AIN0")
				(number "4")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "AIN1")
				(number "5")
			)
			(pin no_connect line
				(at -7.62 7.62 0)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "6")
			)
			(pin no_connect line
				(at -7.62 5.08 0)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "7")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "ALERT/RDY")
				(number "2")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "10")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SDA")
				(number "9")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "ADDR")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADS1015IDGS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 13.97 0)
		)
		(property "Value" "ADS1015IDGS"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_SO:TSSOP-10_3x3mm_P0.5mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads1015.pdf"
			(at -1.27 -22.86 0)
		)
		(property "Description" "Ultra-Small, Low-Power, I2C-Compatible, 3.3-kSPS, 12-Bit ADCs With Internal Reference, Oscillator, and Programmable Comparator, VSSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "12 bit 4 channel I2C ADC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ADS1015IDGS_0_1")
		(symbol "ADS1015IDGS_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "AIN0")
				(number "4")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "AIN1")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "AIN2")
				(number "6")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "AIN3")
				(number "7")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "ALERT/RDY")
				(number "2")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "10")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SDA")
				(number "9")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "ADDR")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADS1018IDGS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "ADS1018IDGS"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at -1.27 -1.27 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads1018.pdf"
			(at -22.86 10.16 0)
		)
		(property "Description" "Ultrasmall, Low-Power, SPI-Compatible, 12-Bit, Analog-to-Digital Converter With Internal Reference and Temperature Sensor, VSSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "12 bit 4 channel SPI ADC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ADS1018IDGS_0_1")
		(symbol "ADS1018IDGS_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "AIN0")
				(number "4")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "AIN1")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "AIN2")
				(number "6")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "AIN3")
				(number "7")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SCLK")
				(number "1")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "DIN")
				(number "10")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "DOUT/~{DRDY}")
				(number "9")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{CS}")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADS1110"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "ADS1110"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 11.43 8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads1110.pdf"
			(at -7.62 8.89 0)
		)
		(property "Description" "16 Bit Analog to Digital converter with on board reference"
			(at 0 0 0)
		)
		(property "ki_keywords" "16 Bit Analog to digital converter ADC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "ADS1110_0_1")
		(symbol "ADS1110_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN+")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "VIN-")
				(number "6")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SCL")
				(number "3")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SDA")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADS1120-PW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 11.43 0)
		)
		(property "Value" "ADS1120-PW"
			(at 6.35 11.43 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 6.35 13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads1120.pdf"
			(at -12.7 10.16 0)
		)
		(property "Description" "Low-power, quad-input, 16-bit analog to digital converter, integrated temperature sensor, SPI interface, TSSOP-16 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "adc spi"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADS1120-PW_0_1")
		(symbol "ADS1120-PW_1_1"
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "REFP0")
				(number "9")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "AIN0/REFP1")
				(number "11")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "AIN1")
				(number "10")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "AIN2")
				(number "7")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "AIN3/REFN1")
				(number "6")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "REFN0")
				(number "8")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "DVDD")
				(number "13")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "DGND")
				(number "4")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "AVDD")
				(number "12")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "AVSS")
				(number "5")
			)
			(pin input line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "SCLK")
				(number "1")
			)
			(pin input line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "DIN")
				(number "16")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "DOUT/~{DRDY}")
				(number "15")
			)
			(pin input line
				(at 17.78 0 180)
				(length 2.54)
				(name "~{CS}")
				(number "2")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "~{DRDY}")
				(number "14")
			)
			(pin input line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "CLK")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADS1120-RVA"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 11.43 0)
		)
		(property "Value" "ADS1120-RVA"
			(at 6.35 11.43 0)
		)
		(property "Footprint" ""
			(at -1.27 -1.27 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads1120.pdf"
			(at -21.59 10.16 0)
		)
		(property "Description" "Low-power, quad-input, 16-bit analog to digital converter, integrated temperature sensor, SPI interface, QFN-16 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "adc spi"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*3.5x3.5mm*P0.50mm*"
			(at 0 0 0)
		)
		(symbol "ADS1120-RVA_0_1")
		(symbol "ADS1120-RVA_1_1"
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "REFP0")
				(number "7")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "AIN0/REFP1")
				(number "9")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "AIN1")
				(number "8")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "AIN2")
				(number "5")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "AIN3/REFN1")
				(number "4")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "REFN0")
				(number "6")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "DVDD")
				(number "11")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "DGND")
				(number "2")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "AVDD")
				(number "10")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "AVSS")
				(number "3")
			)
			(pin passive line
				(at 5.08 -12.7 90)
				(length 2.54)
				(name "PAD")
				(number "17")
			)
			(pin input line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "SCLK")
				(number "15")
			)
			(pin input line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "DIN")
				(number "14")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "DOUT/~{DRDY}")
				(number "13")
			)
			(pin input line
				(at 17.78 0 180)
				(length 2.54)
				(name "~{CS}")
				(number "16")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "~{DRDY}")
				(number "12")
			)
			(pin input line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "CLK")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADS1232IPW"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 25.4 0)
		)
		(property "Value" "ADS1232IPW"
			(at 7.62 25.4 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads1232.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Bridge 24bit ADC for Sensors, TSSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC 24bit Sensors Dual Channel"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*"
			(at 0 0 0)
		)
		(symbol "ADS1232IPW_0_1")
		(symbol "ADS1232IPW_1_1"
			(pin input line
				(at -17.78 20.32 0)
				(length 3.81)
				(name "REFP")
				(number "16")
			)
			(pin passive line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "CAP")
				(number "9")
			)
			(pin passive line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "CAP")
				(number "10")
			)
			(pin input line
				(at -17.78 0 0)
				(length 3.81)
				(name "AINP1")
				(number "11")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "AINN1")
				(number "12")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "AINP2")
				(number "14")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 3.81)
				(name "AINN2")
				(number "13")
			)
			(pin input line
				(at -17.78 -20.32 0)
				(length 3.81)
				(name "REFN")
				(number "15")
			)
			(pin power_in line
				(at -5.08 27.94 270)
				(length 3.81)
				(name "AVDD")
				(number "18")
			)
			(pin power_in line
				(at -5.08 -27.94 90)
				(length 3.81)
				(name "AGND")
				(number "17")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 3.81)
				(name "DGND")
				(number "2")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 3.81)
				(name "DGND")
				(number "5")
			)
			(pin power_in line
				(at 5.08 27.94 270)
				(length 3.81)
				(name "DVDD")
				(number "1")
			)
			(pin power_in line
				(at 5.08 -27.94 90)
				(length 3.81)
				(name "DGND")
				(number "6")
			)
			(pin input line
				(at 17.78 20.32 180)
				(length 3.81)
				(name "GAIN0")
				(number "19")
			)
			(pin input line
				(at 17.78 17.78 180)
				(length 3.81)
				(name "GAIN1")
				(number "20")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "~{DRDY}/DOUT")
				(number "24")
			)
			(pin input line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "SCLK")
				(number "23")
			)
			(pin input line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "~{PWDN}")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 3.81)
				(name "XTAL2")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "CLKIN/XTAL1")
				(number "3")
			)
			(pin input line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "SPEED")
				(number "21")
			)
			(pin input line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "A0")
				(number "8")
			)
			(pin input line
				(at 17.78 -20.32 180)
				(length 3.81)
				(name "TEMP")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADS1234IPW"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 25.4 0)
		)
		(property "Value" "ADS1234IPW"
			(at 7.62 27.94 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads1232.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Bridge 24bit ADC for Sensors, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC 24bit Sensors Quad Channel"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*"
			(at 0 0 0)
		)
		(symbol "ADS1234IPW_0_1")
		(symbol "ADS1234IPW_1_1"
			(pin input line
				(at -17.78 22.86 0)
				(length 3.81)
				(name "REFP")
				(number "20")
			)
			(pin passive line
				(at -17.78 17.78 0)
				(length 3.81)
				(name "CAP")
				(number "9")
			)
			(pin passive line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "CAP")
				(number "10")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "AINP1")
				(number "11")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "AINN1")
				(number "12")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "AINP2")
				(number "18")
			)
			(pin input line
				(at -17.78 0 0)
				(length 3.81)
				(name "AINN2")
				(number "17")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "AINP3")
				(number "13")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "AINN3")
				(number "14")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 3.81)
				(name "AINP4")
				(number "16")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 3.81)
				(name "AINN4")
				(number "15")
			)
			(pin input line
				(at -17.78 -22.86 0)
				(length 3.81)
				(name "REFN")
				(number "19")
			)
			(pin power_in line
				(at -5.08 30.48 270)
				(length 3.81)
				(name "AVDD")
				(number "22")
			)
			(pin power_in line
				(at -5.08 -30.48 90)
				(length 3.81)
				(name "AGND")
				(number "21")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 3.81)
				(name "DGND")
				(number "2")
			)
			(pin power_in line
				(at 2.54 -30.48 90)
				(length 3.81)
				(name "DGND")
				(number "5")
			)
			(pin power_in line
				(at 5.08 30.48 270)
				(length 3.81)
				(name "DVDD")
				(number "1")
			)
			(pin power_in line
				(at 5.08 -30.48 90)
				(length 3.81)
				(name "DGND")
				(number "6")
			)
			(pin input line
				(at 17.78 22.86 180)
				(length 3.81)
				(name "GAIN0")
				(number "23")
			)
			(pin input line
				(at 17.78 20.32 180)
				(length 3.81)
				(name "GAIN1")
				(number "24")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "~{DRDY}/DOUT")
				(number "28")
			)
			(pin input line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "SCLK")
				(number "27")
			)
			(pin input line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "~{PWDN}")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 3.81)
				(name "XTAL2")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "CLKIN/XTAL1")
				(number "3")
			)
			(pin input line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "SPEED")
				(number "25")
			)
			(pin input line
				(at 17.78 -20.32 180)
				(length 3.81)
				(name "A0")
				(number "8")
			)
			(pin input line
				(at 17.78 -22.86 180)
				(length 3.81)
				(name "A1")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADS1243"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 22.86 0)
		)
		(property "Value" "ADS1243"
			(at 2.54 22.86 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 25.4 -22.86 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads1243.pdf"
			(at 0 0 0)
		)
		(property "Description" "24-bit ADC, 8 Channels, SPI compatible, PGA 1 to 128, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "24bit ADC 8 Channels PGA SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADS1243_0_1")
		(symbol "ADS1243_1_1"
			(pin input line
				(at -15.24 17.78 0)
				(length 3.81)
				(name "Ain0/D0")
				(number "7")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 3.81)
				(name "Ain1/D1")
				(number "8")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 3.81)
				(name "Ain2/D2")
				(number "13")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 3.81)
				(name "Ain3/D3")
				(number "14")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "Ain4/D4")
				(number "9")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "Ain5/D5")
				(number "10")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "Ain6/D6")
				(number "11")
			)
			(pin input line
				(at -15.24 0 0)
				(length 3.81)
				(name "Ain7/D7")
				(number "12")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 3.81)
				(name "VREF+")
				(number "5")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 3.81)
				(name "VREF-")
				(number "6")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 3.81)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "GND")
				(number "15")
			)
			(pin input clock
				(at 15.24 17.78 180)
				(length 5.08)
				(name "SCLK")
				(number "19")
			)
			(pin output line
				(at 15.24 15.24 180)
				(length 5.08)
				(name "DOUT")
				(number "18")
			)
			(pin input line
				(at 15.24 12.7 180)
				(length 5.08)
				(name "DIN")
				(number "17")
			)
			(pin input input_low
				(at 15.24 10.16 180)
				(length 5.08)
				(name "~{CS}")
				(number "16")
			)
			(pin open_collector output_low
				(at 15.24 5.08 180)
				(length 5.08)
				(name "~{DRDY}")
				(number "20")
			)
			(pin input input_low
				(at 15.24 -7.62 180)
				(length 5.08)
				(name "~{PDWN}")
				(number "4")
			)
			(pin output line
				(at 15.24 -12.7 180)
				(length 5.08)
				(name "XOUT")
				(number "3")
			)
			(pin input line
				(at 15.24 -15.24 180)
				(length 5.08)
				(name "XIN")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADS1251"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "ADS1251"
			(at 13.97 7.62 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads1251.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Single channel 24-bit Analog to Digital Converter, 5V supply, differential input, 20kHz, 2-wire serial interface, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "delta-sigma adc low-power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*"
			(at 0 0 0)
		)
		(symbol "ADS1251_0_1")
		(symbol "ADS1251_1_1"
			(pin input line
				(at -20.32 2.54 0)
				(length 6.35)
				(name "IN+")
				(number "1")
			)
			(pin input line
				(at -20.32 -2.54 0)
				(length 6.35)
				(name "IN-")
				(number "2")
			)
			(pin input line
				(at -5.08 10.16 270)
				(length 3.81)
				(name "VREF")
				(number "8")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 3.81)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 3.81)
				(name "GND")
				(number "7")
			)
			(pin input line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "SCLK")
				(number "6")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "DOUT/nDRDY")
				(number "5")
			)
			(pin input line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "CLK")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADS127L01IPBS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -16.51 26.67 0)
		)
		(property "Value" "ADS127L01IPBS"
			(at 11.43 -26.67 0)
		)
		(property "Footprint" "Package_QFP:PQFP-32_5x5mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ads127l01.pdf"
			(at 0 0 0)
		)
		(property "Description" "24-bit delta-sigma ADC, Single Channel, 512 kSPS, SPI & Frame-Sync interface, PQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Texas Instruments high-speed 24bit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PQFP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ADS127L01IPBS_0_1")
		(symbol "ADS127L01IPBS_1_1"
			(pin input line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "AINP")
				(number "4")
			)
			(pin input line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "AINN")
				(number "3")
			)
			(pin input line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "REFP")
				(number "9")
			)
			(pin input line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "REFN")
				(number "10")
			)
			(pin input line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "REXT")
				(number "7")
			)
			(pin output line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "CAP1")
				(number "2")
			)
			(pin output line
				(at -20.32 0 0)
				(length 2.54)
				(name "CAP2")
				(number "11")
			)
			(pin output line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "CAP3")
				(number "25")
			)
			(pin input line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "CLK")
				(number "24")
			)
			(pin input line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "DAISYIN")
				(number "18")
			)
			(pin input line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "~{RESET}/~{PWDN}")
				(number "28")
			)
			(pin passive line
				(at -5.08 27.94 270)
				(length 2.54)
				(hide yes)
				(name "AVDD")
				(number "32")
			)
			(pin power_in line
				(at -5.08 27.94 270)
				(length 2.54)
				(name "AVDD")
				(number "6")
			)
			(pin passive line
				(at -2.54 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "31")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 2.54)
				(name "AGND")
				(number "5")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "DVDD")
				(number "27")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 2.54)
				(name "DGND")
				(number "26")
			)
			(pin power_in line
				(at 5.08 27.94 270)
				(length 2.54)
				(name "LVDD")
				(number "1")
			)
			(pin input line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "~{INTLDO}")
				(number "8")
			)
			(pin output line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "DOUT")
				(number "20")
			)
			(pin input line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "DIN")
				(number "21")
			)
			(pin input line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "SCLK")
				(number "22")
			)
			(pin input line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "~{CS}")
				(number "23")
			)
			(pin input line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "FILTER0")
				(number "13")
			)
			(pin input line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "FILTER1")
				(number "12")
			)
			(pin input line
				(at 20.32 0 180)
				(length 2.54)
				(name "FSMODE")
				(number "14")
			)
			(pin input line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "OSR0")
				(number "16")
			)
			(pin input line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "OSR1")
				(number "15")
			)
			(pin input line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "HR")
				(number "29")
			)
			(pin input line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "FORMAT")
				(number "30")
			)
			(pin input line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "START")
				(number "17")
			)
			(pin passive line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "~{DRDY}/FSYNC")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADS1298xPAG"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 41.91 0)
		)
		(property "Value" "ADS1298xPAG"
			(at 6.35 41.91 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_10x10mm_P0.5mm"
			(at 0 -53.34 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads1298.pdf"
			(at 0 -55.88 0)
		)
		(property "Description" "ADS1298 Low-Power, 8-Channel, 24-Bit Analog Front-End for Biopotential Measurements, TQFP-64"
			(at 0 -2.54 0)
		)
		(property "ki_keywords" "24bit ADC PGA SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ADS1298xPAG_0_1")
		(symbol "ADS1298xPAG_1_1"
			(pin input line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "IN1P")
				(number "16")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "IN1N")
				(number "15")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "IN2P")
				(number "14")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "IN2N")
				(number "13")
			)
			(pin input line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "IN3P")
				(number "12")
			)
			(pin input line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "IN3N")
				(number "11")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "IN4P")
				(number "10")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "IN4N")
				(number "9")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "IN5P")
				(number "8")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "IN5N")
				(number "7")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "IN6P")
				(number "6")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "IN6N")
				(number "5")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "IN7P")
				(number "4")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "IN7N")
				(number "3")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "IN8P")
				(number "2")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "IN8N")
				(number "1")
			)
			(pin passive line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "VCAP1")
				(number "28")
			)
			(pin passive line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "VCAP2")
				(number "30")
			)
			(pin passive line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "VCAP3")
				(number "55")
			)
			(pin passive line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "VCAP4")
				(number "26")
			)
			(pin passive line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "VREFP")
				(number "24")
			)
			(pin passive line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "VREFN")
				(number "25")
			)
			(pin power_in line
				(at -5.08 43.18 270)
				(length 2.54)
				(name "AVDD")
				(number "19")
			)
			(pin passive line
				(at -5.08 43.18 270)
				(length 2.54)
				(hide yes)
				(name "AVDD")
				(number "21")
			)
			(pin passive line
				(at -5.08 43.18 270)
				(length 2.54)
				(hide yes)
				(name "AVDD")
				(number "22")
			)
			(pin passive line
				(at -5.08 43.18 270)
				(length 2.54)
				(hide yes)
				(name "AVDD")
				(number "56")
			)
			(pin passive line
				(at -5.08 43.18 270)
				(length 2.54)
				(hide yes)
				(name "AVDD")
				(number "59")
			)
			(pin power_in line
				(at -5.08 -43.18 90)
				(length 2.54)
				(name "AVSS")
				(number "20")
			)
			(pin passive line
				(at -5.08 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "AVSS")
				(number "23")
			)
			(pin passive line
				(at -5.08 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "AVSS")
				(number "32")
			)
			(pin passive line
				(at -5.08 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "AVSS")
				(number "57")
			)
			(pin passive line
				(at -5.08 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "AVSS")
				(number "58")
			)
			(pin power_in line
				(at 0 43.18 270)
				(length 2.54)
				(name "AVDD1")
				(number "54")
			)
			(pin power_in line
				(at 0 -43.18 90)
				(length 2.54)
				(name "AVSS1")
				(number "53")
			)
			(pin power_in line
				(at 5.08 43.18 270)
				(length 2.54)
				(name "DVDD")
				(number "48")
			)
			(pin passive line
				(at 5.08 43.18 270)
				(length 2.54)
				(hide yes)
				(name "DVDD")
				(number "50")
			)
			(pin power_in line
				(at 5.08 -43.18 90)
				(length 2.54)
				(name "DGND")
				(number "33")
			)
			(pin passive line
				(at 5.08 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "DGND")
				(number "49")
			)
			(pin passive line
				(at 5.08 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "DGND")
				(number "51")
			)
			(pin no_connect line
				(at 15.24 -35.56 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "27")
			)
			(pin no_connect line
				(at 15.24 -38.1 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "29")
			)
			(pin output line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "WCT")
				(number "64")
			)
			(pin output line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "RLDOUT")
				(number "63")
			)
			(pin input line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "RLDIN")
				(number "62")
			)
			(pin input line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "RLDINV")
				(number "61")
			)
			(pin input line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "RLDREF")
				(number "60")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "TESTP_PACE_OUT1")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "TESTP_PACE_OUT2")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "GPIO1")
				(number "42")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "GPIO2")
				(number "44")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "GPIO3")
				(number "45")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "GPIO4")
				(number "46")
			)
			(pin input line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "DAISY_IN")
				(number "41")
			)
			(pin input line
				(at 17.78 0 180)
				(length 2.54)
				(name "SCLK")
				(number "40")
			)
			(pin input line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "DIN")
				(number "34")
			)
			(pin input line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "~{CS}")
				(number "39")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "DOUT")
				(number "43")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "CLK")
				(number "37")
			)
			(pin input line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "CLKSEL")
				(number "52")
			)
			(pin input line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "START")
				(number "38")
			)
			(pin output line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "~{DRDY}")
				(number "47")
			)
			(pin input line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "~{PWDN}")
				(number "35")
			)
			(pin input line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "~{RESET}")
				(number "36")
			)
			(pin input line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "RESV1")
				(number "31")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADS7040xDCU"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 -7.62 0)
		)
		(property "Value" "ADS7040xDCU"
			(at 2.54 -7.62 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_2.3x2mm_P0.5mm"
			(at 2.54 16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads7040.pdf"
			(at 0 0 0)
		)
		(property "Description" "Ultra-Low Power, Ultra-Small Size, 8-Bit, 1-MSPS, SAR ADC"
			(at 0 0 0)
		)
		(property "ki_keywords" "8 bit SAR ADC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*8*2.3x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ADS7040xDCU_0_1")
		(symbol "ADS7040xDCU_1_1"
			(pin input line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "AINP")
				(number "6")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "AINM")
				(number "5")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 3.81)
				(name "AVDD")
				(number "7")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 3.81)
				(name "DVDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 3.81)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 3.81)
				(name "SDO")
				(number "3")
			)
			(pin input clock
				(at 15.24 0 180)
				(length 3.81)
				(name "SCLK")
				(number "2")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 3.81)
				(name "~{CS}")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADS7828"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 15.24 0)
		)
		(property "Value" "ADS7828"
			(at 5.08 15.24 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 24.13 -17.78 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads7828.pdf"
			(at 0 0 0)
		)
		(property "Description" "12-Bits, 8-Channels, ADC, I2C, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C ADC 12Bits"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADS7828_0_1")
		(symbol "ADS7828_1_1"
			(pin input line
				(at -10.16 10.16 0)
				(length 3.81)
				(name "CH0")
				(number "1")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 3.81)
				(name "CH1")
				(number "2")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 3.81)
				(name "CH2")
				(number "3")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 3.81)
				(name "CH3")
				(number "4")
			)
			(pin input line
				(at -10.16 0 0)
				(length 3.81)
				(name "CH4")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 3.81)
				(name "CH5")
				(number "6")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 3.81)
				(name "CH6")
				(number "7")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 3.81)
				(name "CH7")
				(number "8")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 3.81)
				(name "COM")
				(number "11")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "GND")
				(number "9")
			)
			(pin bidirectional line
				(at 10.16 10.16 180)
				(length 3.81)
				(name "SDA")
				(number "15")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 3.81)
				(name "SCL")
				(number "14")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 3.81)
				(name "REF")
				(number "10")
			)
			(pin input line
				(at 10.16 -10.16 180)
				(length 3.81)
				(name "A0")
				(number "12")
			)
			(pin input line
				(at 10.16 -12.7 180)
				(length 3.81)
				(name "A1")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADS7866"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 6.35 0)
		)
		(property "Value" "ADS7866"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0 -1.27 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads7866.pdf"
			(at 1.27 6.35 0)
		)
		(property "Description" "Single Channel 12-bit ADC,  100-200ksps, SPI, micro-power, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOT?23?6*"
			(at 0 0 0)
		)
		(symbol "ADS7866_0_1")
		(symbol "ADS7866_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "AIN")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin tri_state line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDO")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCLK")
				(number "4")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{CS}")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADS8681RUM"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 13.97 0)
		)
		(property "Value" "ADS8681RUM"
			(at 6.35 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_4x4mm_P0.65mm_EP2.7x2.7mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads8681.pdf"
			(at 1.27 6.35 0)
		)
		(property "Description" "16-Bit, High-Speed, Single-Supply, SAR ADC Data Acquisition System with Programmable, Bipolar Input Ranges, 1MSPS, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC SPI analog digital"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.65mm*EP2.7x2.7mm*"
			(at 0 0 0)
		)
		(symbol "ADS8681RUM_0_1")
		(symbol "ADS8681RUM_1_1"
			(pin input line
				(at -17.78 2.54 0)
				(length 5.08)
				(name "AIN_P")
				(number "5")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 5.08)
				(name "AIN_GND")
				(number "6")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "AVDD")
				(number "16")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "AGND")
				(number "1")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "DVDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "DGND")
				(number "15")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "REFCAP")
				(number "4")
			)
			(pin passive line
				(at 5.08 12.7 270)
				(length 2.54)
				(name "REFIO")
				(number "2")
			)
			(pin power_in line
				(at 5.08 -12.7 90)
				(length 2.54)
				(name "REFGND")
				(number "3")
			)
			(pin power_in line
				(at 7.62 -12.7 90)
				(length 2.54)
				(name "PAD")
				(number "17")
			)
			(pin output line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "RVS")
				(number "13")
			)
			(pin input line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "~{RST}")
				(number "7")
			)
			(pin input line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "CONVST/~{CS}")
				(number "9")
			)
			(pin input line
				(at 20.32 0 180)
				(length 2.54)
				(name "SCLK")
				(number "10")
			)
			(pin input line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "SDI")
				(number "8")
			)
			(pin tri_state line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "SDO-0")
				(number "11")
			)
			(pin tri_state line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "SDO-1")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADS8684"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 31.75 0)
		)
		(property "Value" "ADS8684"
			(at 8.89 31.75 0)
		)
		(property "Footprint" "Package_SO:TSSOP-38_4.4x9.7mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads8688.pdf"
			(at 24.13 33.02 0)
		)
		(property "Description" "16-Bit, 500-kSPS, 4-Channels, Single-Supply, SAR ADC with Bipolar Input Range, TSSOP-38"
			(at 0 0 0)
		)
		(property "ki_keywords" "adc analog digital spi bipolar input"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ADS8684_0_1")
		(symbol "ADS8684_1_1"
			(pin input line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "AIN_0P")
				(number "16")
			)
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "AIN_0GND")
				(number "17")
			)
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "AIN_1P")
				(number "18")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "AIN_1GND")
				(number "19")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "AIN_2P")
				(number "21")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "AIN_2GND")
				(number "20")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "AIN_3P")
				(number "23")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "AIN_3GND")
				(number "22")
			)
			(pin input line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "AUX_IN")
				(number "10")
			)
			(pin input line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "AUX_GND")
				(number "11")
			)
			(pin no_connect line
				(at -10.16 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "25")
			)
			(pin no_connect line
				(at -10.16 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "24")
			)
			(pin no_connect line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "27")
			)
			(pin no_connect line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "26")
			)
			(pin no_connect line
				(at -10.16 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin no_connect line
				(at -10.16 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at -10.16 -12.7 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin no_connect line
				(at -10.16 -15.24 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin power_in line
				(at -2.54 33.02 270)
				(length 2.54)
				(name "AVDD")
				(number "9")
			)
			(pin passive line
				(at -2.54 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "28")
			)
			(pin passive line
				(at -2.54 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "29")
			)
			(pin passive line
				(at -2.54 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "31")
			)
			(pin passive line
				(at -2.54 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "32")
			)
			(pin power_in line
				(at -2.54 -33.02 90)
				(length 2.54)
				(name "AGND")
				(number "8")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "AVDD")
				(number "30")
			)
			(pin power_in line
				(at 2.54 33.02 270)
				(length 2.54)
				(name "DVDD")
				(number "34")
			)
			(pin power_in line
				(at 2.54 -33.02 90)
				(length 2.54)
				(name "DGND")
				(number "33")
			)
			(pin no_connect line
				(at 10.16 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "35")
			)
			(pin output line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "SDO")
				(number "36")
			)
			(pin input line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "SDI")
				(number "1")
			)
			(pin input line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "SCLK")
				(number "37")
			)
			(pin input line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "~{CS}")
				(number "38")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "DAISY")
				(number "3")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "~{RST/PD}")
				(number "2")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "~{REFSEL}")
				(number "4")
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "REFCAP")
				(number "7")
			)
			(pin passive line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "REFIO")
				(number "5")
			)
			(pin power_in line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "REFGND")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADS8688"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 31.75 0)
		)
		(property "Value" "ADS8688"
			(at 8.89 31.75 0)
		)
		(property "Footprint" "Package_SO:TSSOP-38_4.4x9.7mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads8688.pdf"
			(at 24.13 33.02 0)
		)
		(property "Description" "16-Bit, 500-kSPS, 8-Channels, Single-Supply, SAR ADC with Bipolar Input Range, TSSOP-38"
			(at 0 0 0)
		)
		(property "ki_keywords" "adc analog digital spi bipolar input"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ADS8688_0_1")
		(symbol "ADS8688_1_1"
			(pin input line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "AIN_0P")
				(number "16")
			)
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "AIN_0GND")
				(number "17")
			)
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "AIN_1P")
				(number "18")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "AIN_1GND")
				(number "19")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "AIN_2P")
				(number "21")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "AIN_2GND")
				(number "20")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "AIN_3P")
				(number "23")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "AIN_3GND")
				(number "22")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "AIN_4P")
				(number "25")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "AIN_4GND")
				(number "24")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "AIN_5P")
				(number "27")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "AIN_5GND")
				(number "26")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "AIN_6P")
				(number "12")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "AIN_6GND")
				(number "13")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "AIN_7P")
				(number "14")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "AIN_7GND")
				(number "15")
			)
			(pin input line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "AUX_IN")
				(number "10")
			)
			(pin input line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "AUX_GND")
				(number "11")
			)
			(pin power_in line
				(at -2.54 33.02 270)
				(length 2.54)
				(name "AVDD")
				(number "9")
			)
			(pin passive line
				(at -2.54 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "28")
			)
			(pin passive line
				(at -2.54 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "29")
			)
			(pin passive line
				(at -2.54 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "31")
			)
			(pin passive line
				(at -2.54 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "32")
			)
			(pin power_in line
				(at -2.54 -33.02 90)
				(length 2.54)
				(name "AGND")
				(number "8")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "AVDD")
				(number "30")
			)
			(pin power_in line
				(at 2.54 33.02 270)
				(length 2.54)
				(name "DVDD")
				(number "34")
			)
			(pin power_in line
				(at 2.54 -33.02 90)
				(length 2.54)
				(name "DGND")
				(number "33")
			)
			(pin no_connect line
				(at 10.16 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "35")
			)
			(pin output line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "SDO")
				(number "36")
			)
			(pin input line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "SDI")
				(number "1")
			)
			(pin input line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "SCLK")
				(number "37")
			)
			(pin input line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "~{CS}")
				(number "38")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "DAISY")
				(number "3")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "~{RST/PD}")
				(number "2")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "~{REFSEL}")
				(number "4")
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "REFCAP")
				(number "7")
			)
			(pin passive line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "REFIO")
				(number "5")
			)
			(pin power_in line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "REFGND")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AMC3336"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -1.27 22.86 0)
		)
		(property "Value" "AMC3336"
			(at 0 20.32 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 31.75 41.91 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/amc3336.pdf"
			(at 33.02 39.37 0)
		)
		(property "Description" "Reinforced Isolated Delta-Sigma Modulator With Integrated DC/DC Converter, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "isolated adc delta sigma integrated power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "AMC3336_0_1")
		(symbol "AMC3336_1_1"
			(pin power_out line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "DCDC_OUT")
				(number "1")
			)
			(pin power_out line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "DCDC_HGND")
				(number "2")
			)
			(pin power_in line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "HLDO_IN")
				(number "3")
			)
			(pin power_out line
				(at -17.78 0 0)
				(length 2.54)
				(name "HLDO_OUT")
				(number "5")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "INP")
				(number "6")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "INN")
				(number "7")
			)
			(pin no_connect line
				(at -7.62 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_in line
				(at -5.08 -17.78 90)
				(length 2.54)
				(name "HGND")
				(number "8")
			)
			(pin power_in line
				(at 5.08 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "12")
			)
			(pin power_in line
				(at 5.08 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin power_out line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "LDO_OUT")
				(number "13")
			)
			(pin power_in line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "DCDC_IN")
				(number "16")
			)
			(pin power_in line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "DCDC_GND")
				(number "15")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "DIAG")
				(number "14")
			)
			(pin input line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "CLKIN")
				(number "11")
			)
			(pin output line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "DOUT")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CA3300"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 17.78 0)
		)
		(property "Value" "CA3300"
			(at 5.08 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Convertisseur A->D 6 bits rapide"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC CAN"
			(at 0 0 0)
		)
		(symbol "CA3300_0_1")
		(symbol "CA3300_1_1"
			(pin input line
				(at -15.24 12.7 0)
				(length 3.81)
				(name "VIN")
				(number "11")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "-REF")
				(number "10")
			)
			(pin input line
				(at -15.24 0 0)
				(length 3.81)
				(name "+REF")
				(number "9")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 3.81)
				(name "CREF")
				(number "16")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 3.81)
				(name "ZEN")
				(number "4")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 3.81)
				(name "PHAS")
				(number "8")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "VCC")
				(number "12")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "GND")
				(number "3")
			)
			(pin tri_state line
				(at 15.24 12.7 180)
				(length 3.81)
				(name "OVF")
				(number "2")
			)
			(pin tri_state line
				(at 15.24 10.16 180)
				(length 3.81)
				(name "D0")
				(number "13")
			)
			(pin tri_state line
				(at 15.24 7.62 180)
				(length 3.81)
				(name "D1")
				(number "14")
			)
			(pin tri_state line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "D2")
				(number "15")
			)
			(pin tri_state line
				(at 15.24 2.54 180)
				(length 3.81)
				(name "D3")
				(number "17")
			)
			(pin tri_state line
				(at 15.24 0 180)
				(length 3.81)
				(name "D4")
				(number "18")
			)
			(pin tri_state line
				(at 15.24 -2.54 180)
				(length 3.81)
				(name "D5")
				(number "1")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 3.81)
				(name "CE2")
				(number "5")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 3.81)
				(name "CE1")
				(number "6")
			)
			(pin input clock
				(at 15.24 -12.7 180)
				(length 3.81)
				(name "CLK")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HX711"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 21.59 0)
		)
		(property "Value" "HX711"
			(at 7.62 19.05 0)
		)
		(property "Footprint" "Package_SO:SOP-16_3.9x9.9mm_P1.27mm"
			(at 3.81 1.27 0)
		)
		(property "Datasheet" "https://web.archive.org/web/20220615044707/https://akizukidenshi.com/download/ds/avia/hx711.pdf"
			(at 3.81 -1.27 0)
		)
		(property "Description" "24-Bit Analog-to-Digital Converter (ADC) for Weight Scales"
			(at 0 0 0)
		)
		(property "ki_keywords" "adc load cell 24-bits analog weight"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "HX711_0_1")
		(symbol "HX711_1_1"
			(pin passive line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "BASE")
				(number "2")
			)
			(pin power_in line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "AVDD")
				(number "3")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "VFB")
				(number "4")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "INA+")
				(number "8")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "INA-")
				(number "7")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "INB+")
				(number "10")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "INB-")
				(number "9")
			)
			(pin passive line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "VBG")
				(number "6")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 2.54)
				(name "VSUP")
				(number "1")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "AGND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "DVDD")
				(number "16")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "DOUT")
				(number "12")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PD_SCK")
				(number "11")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 2.54)
				(name "XO")
				(number "13")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "XI")
				(number "14")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "RATE")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ICL7106CPL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 31.75 0)
		)
		(property "Value" "ICL7106CPL"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 -31.75 0)
		)
		(property "Datasheet" "https://www.renesas.com/eu/en/www/doc/datasheet/icl7106-07-07s.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "3 1/2 Digit, LCD Display, A/D Converter, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "LCD ADC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24*"
			(at 0 0 0)
		)
		(symbol "ICL7106CPL_0_1")
		(symbol "ICL7106CPL_1_1"
			(pin output line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "A1")
				(number "5")
			)
			(pin output line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "B1")
				(number "4")
			)
			(pin output line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "C1")
				(number "3")
			)
			(pin output line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "D1")
				(number "2")
			)
			(pin output line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "E1")
				(number "8")
			)
			(pin output line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "F1")
				(number "6")
			)
			(pin output line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "G1")
				(number "7")
			)
			(pin output line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "A2")
				(number "12")
			)
			(pin output line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "B2")
				(number "11")
			)
			(pin output line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "C2")
				(number "10")
			)
			(pin output line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "D2")
				(number "9")
			)
			(pin output line
				(at -15.24 0 0)
				(length 2.54)
				(name "E2")
				(number "14")
			)
			(pin output line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "F2")
				(number "13")
			)
			(pin output line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "G2")
				(number "25")
			)
			(pin output line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "A3")
				(number "23")
			)
			(pin output line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "B3")
				(number "16")
			)
			(pin output line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "C3")
				(number "24")
			)
			(pin output line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "D3")
				(number "15")
			)
			(pin output line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "E3")
				(number "18")
			)
			(pin output line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "F3")
				(number "17")
			)
			(pin output line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "G3")
				(number "22")
			)
			(pin output line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "AB4")
				(number "19")
			)
			(pin output line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "POL")
				(number "20")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "V+")
				(number "1")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "V-")
				(number "26")
			)
			(pin passive line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "OSC1")
				(number "40")
			)
			(pin passive line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "OSC2")
				(number "39")
			)
			(pin passive line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "OSC3")
				(number "38")
			)
			(pin passive line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "TEST")
				(number "37")
			)
			(pin passive line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "REF_HI")
				(number "36")
			)
			(pin passive line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "REF_LO")
				(number "35")
			)
			(pin passive line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "CREF+")
				(number "34")
			)
			(pin passive line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "CREF-")
				(number "33")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "COMMON")
				(number "32")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "IN_HI")
				(number "31")
			)
			(pin input line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "IN_LO")
				(number "30")
			)
			(pin passive line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "A-Z")
				(number "29")
			)
			(pin output line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "BUFF")
				(number "28")
			)
			(pin passive line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "INT")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "BP/GND")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "INA234AxYBJ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "INA234AxYBJ"
			(at 6.35 8.89 0)
		)
		(property "Footprint" "Package_BGA:Texas_DSBGA-8_0.705x1.468mm_Layout2x4_P0.4mm"
			(at 20.32 -8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina234.pdf"
			(at 8.89 -2.54 0)
		)
		(property "Description" "Bidirectional Current/Voltage/Power Monitor (0-28V) With I2C Interface, DSBGA-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC I2C 12-Bit Current Voltage Power Shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DSBGA*0.705x1.468mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "INA234AxYBJ_0_1")
		(symbol "INA234AxYBJ_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN+")
				(number "A2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IN-")
				(number "B2")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VS")
				(number "D2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "C2")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SDA")
				(number "C1")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SCL")
				(number "D1")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{ALERT}")
				(number "A1")
				(alternate "ALERT" open_collector line)
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "A0")
				(number "B1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC1406CGN"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 20.32 0)
		)
		(property "Value" "LTC1406CGN"
			(at 7.62 20.32 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1406f.pdf"
			(at 0 0 0)
		)
		(property "Description" "ADC 8bit Low Power 20Msps, SSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Power ADC 8bit 20Msps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*"
			(at 0 0 0)
		)
		(symbol "LTC1406CGN_0_1")
		(symbol "LTC1406CGN_1_1"
			(pin input line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "AIN+")
				(number "7")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "AIN-")
				(number "8")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "VBIAS")
				(number "4")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 3.81)
				(name "VREF")
				(number "5")
			)
			(pin power_in line
				(at -7.62 -22.86 90)
				(length 3.81)
				(name "AGND")
				(number "6")
			)
			(pin power_in line
				(at -5.08 22.86 270)
				(length 3.81)
				(name "AVDD")
				(number "9")
			)
			(pin power_in line
				(at -5.08 -22.86 90)
				(length 3.81)
				(name "AGND")
				(number "10")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 3.81)
				(name "DVDD")
				(number "12")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 3.81)
				(name "DGND")
				(number "11")
			)
			(pin power_in line
				(at 5.08 22.86 270)
				(length 3.81)
				(name "OVDD")
				(number "2")
			)
			(pin power_in line
				(at 5.08 -22.86 90)
				(length 3.81)
				(name "OGND")
				(number "1")
			)
			(pin no_connect line
				(at 7.62 -19.05 90)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at 10.16 -19.05 90)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "D0")
				(number "15")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "D1")
				(number "16")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "D2")
				(number "17")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "D3")
				(number "18")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "D4")
				(number "19")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "D5")
				(number "20")
			)
			(pin output line
				(at 17.78 0 180)
				(length 3.81)
				(name "D6")
				(number "21")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "D7")
				(number "22")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "OF/UF")
				(number "23")
			)
			(pin input clock
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "CLK")
				(number "24")
			)
			(pin input line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "~{SHDN}")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC1594CS"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 17.78 0)
		)
		(property "Value" "LTC1594CS"
			(at 7.62 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/15948fb.pdf"
			(at 0 0 0)
		)
		(property "Description" "Micropower 12-bit 4 Channel ADC, Serial IO, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "12bit ADC 4 Channel"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*"
			(at 0 0 0)
		)
		(symbol "LTC1594CS_0_1")
		(symbol "LTC1594CS_1_1"
			(pin input line
				(at -15.24 12.7 0)
				(length 3.81)
				(name "CH0")
				(number "1")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 3.81)
				(name "CH1")
				(number "2")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "CH2")
				(number "3")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "CH3")
				(number "4")
			)
			(pin output line
				(at -15.24 0 0)
				(length 3.81)
				(name "MUXOUT")
				(number "15")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "ADCIN")
				(number "5")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 3.81)
				(name "VREF")
				(number "6")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 3.81)
				(name "COM")
				(number "7")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 3.81)
				(name "VCC")
				(number "11")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "GND")
				(number "8")
			)
			(pin input clock
				(at 15.24 12.7 180)
				(length 3.81)
				(name "CLK")
				(number "12")
			)
			(pin input line
				(at 15.24 10.16 180)
				(length 3.81)
				(name "DIN")
				(number "14")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 3.81)
				(name "DOUT")
				(number "10")
			)
			(pin input line
				(at 15.24 0 180)
				(length 3.81)
				(name "~{CSMUX}")
				(number "13")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 3.81)
				(name "~{CSADC}")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC1598CG"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 22.86 0)
		)
		(property "Value" "LTC1598CG"
			(at 2.54 22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/15948fb.pdf"
			(at 0 0 0)
		)
		(property "Description" "Micropower 12-bit 8 Channel ADC, Serial IO, SSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "12bit ADC 4 Channel"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*"
			(at 0 0 0)
		)
		(symbol "LTC1598CG_0_1")
		(symbol "LTC1598CG_1_1"
			(pin input line
				(at -15.24 17.78 0)
				(length 3.81)
				(name "CH0")
				(number "20")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 3.81)
				(name "CH1")
				(number "21")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 3.81)
				(name "CH2")
				(number "22")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 3.81)
				(name "CH3")
				(number "23")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "CH4")
				(number "24")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "CH5")
				(number "1")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "CH6")
				(number "2")
			)
			(pin input line
				(at -15.24 0 0)
				(length 3.81)
				(name "CH7")
				(number "3")
			)
			(pin output line
				(at -15.24 -5.08 0)
				(length 3.81)
				(name "MUXOUT")
				(number "18")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 3.81)
				(name "ADCIN")
				(number "17")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 3.81)
				(name "VREF")
				(number "16")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 3.81)
				(name "COM")
				(number "8")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 3.81)
				(name "VCC")
				(number "15")
			)
			(pin power_in line
				(at -2.54 -25.4 90)
				(length 3.81)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 3.81)
				(name "VCC")
				(number "19")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "GND")
				(number "9")
			)
			(pin no_connect line
				(at 2.54 -21.59 90)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin no_connect line
				(at 5.08 -21.59 90)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin input clock
				(at 15.24 17.78 180)
				(length 3.81)
				(name "CLK")
				(number "5")
			)
			(pin input clock
				(at 15.24 15.24 180)
				(length 3.81)
				(name "CLK")
				(number "14")
			)
			(pin input line
				(at 15.24 12.7 180)
				(length 3.81)
				(name "DIN")
				(number "7")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 3.81)
				(name "DOUT")
				(number "11")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 3.81)
				(name "~{CSMUX}")
				(number "6")
			)
			(pin input line
				(at 15.24 -12.7 180)
				(length 3.81)
				(name "~{CSADC}")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC1742"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 29.21 0)
		)
		(property "Value" "LTC1742"
			(at 10.16 29.21 0)
		)
		(property "Footprint" "Package_SO:TSSOP-48_6.1x12.5mm_P0.5mm"
			(at 0 -38.1 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1742f.pdf"
			(at -12.7 -7.62 0)
		)
		(property "Description" "14-Bit, 65Msps, Low Noise, ADC, TSSOP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC analog digital converter pipeline"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*6.1x12.5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC1742_0_1")
		(symbol "LTC1742_1_1"
			(pin input line
				(at -12.7 25.4 0)
				(length 2.54)
				(name "AIN+")
				(number "4")
			)
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "AIN-")
				(number "5")
			)
			(pin output line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "VCM")
				(number "2")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "SENSE")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "ENC")
				(number "23")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{ENC}")
				(number "24")
			)
			(pin passive line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "REFLB")
				(number "10")
			)
			(pin passive line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "REFHA")
				(number "11")
			)
			(pin passive line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "REFLA")
				(number "14")
			)
			(pin passive line
				(at -12.7 -25.4 0)
				(length 2.54)
				(name "REFHB")
				(number "15")
			)
			(pin passive line
				(at -2.54 30.48 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "17")
			)
			(pin passive line
				(at -2.54 30.48 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "18")
			)
			(pin passive line
				(at -2.54 30.48 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at -2.54 30.48 270)
				(length 2.54)
				(name "VDD")
				(number "7")
			)
			(pin passive line
				(at -2.54 30.48 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "8")
			)
			(pin passive line
				(at -2.54 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at -2.54 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at -2.54 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at -2.54 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "19")
			)
			(pin passive line
				(at -2.54 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at -2.54 -30.48 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at -2.54 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "36")
			)
			(pin passive line
				(at -2.54 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "37")
			)
			(pin passive line
				(at -2.54 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at -2.54 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 2.54)
				(name "OVDD")
				(number "32")
			)
			(pin passive line
				(at 0 30.48 270)
				(length 2.54)
				(hide yes)
				(name "OVDD")
				(number "43")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "OGND")
				(number "27")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "OGND")
				(number "38")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 2.54)
				(name "OGND")
				(number "47")
			)
			(pin output line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "D0")
				(number "28")
			)
			(pin output line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "D1")
				(number "29")
			)
			(pin output line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "D2")
				(number "30")
			)
			(pin output line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "D3")
				(number "31")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "D4")
				(number "33")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "D5")
				(number "34")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "D6")
				(number "35")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "D7")
				(number "39")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "D8")
				(number "40")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "D9")
				(number "41")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "D10")
				(number "42")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "D11")
				(number "44")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "D12")
				(number "45")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "D13")
				(number "46")
			)
			(pin output line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "OF")
				(number "48")
			)
			(pin output line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "CLKOUT")
				(number "26")
			)
			(pin input line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "~{MSBINV}")
				(number "22")
			)
			(pin input line
				(at 12.7 -25.4 180)
				(length 2.54)
				(name "~{OE}")
				(number "25")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC1864L"
		(pin_names
			(offset 1.27)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "LTC1864L"
			(at 11.43 7.62 0)
		)
		(property "Footprint" ""
			(at -2.54 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/18645lfs.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Single channel 16-bit SAR Analog to Digital Converter, 3V supply, differential input, 150ksps, SPI interface"
			(at 0 0 0)
		)
		(property "ki_keywords" "adc spi 1ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LTC1864L_0_1")
		(symbol "LTC1864L_1_1"
			(pin input line
				(at -20.32 2.54 0)
				(length 6.35)
				(name "IN^{+}")
				(number "2")
			)
			(pin input line
				(at -20.32 -2.54 0)
				(length 6.35)
				(name "IN^{-}")
				(number "3")
			)
			(pin input line
				(at -5.08 10.16 270)
				(length 3.81)
				(name "V_{REF}")
				(number "1")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 3.81)
				(name "V_{CC}")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 3.81)
				(name "GND")
				(number "4")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "SCK")
				(number "7")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 3.81)
				(name "SDO")
				(number "6")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 3.81)
				(name "CONV")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC1865L-MS"
		(pin_names
			(offset 1.27)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "LTC1865L-MS"
			(at 11.43 7.62 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/18645lfs.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual channel 16-bit SAR Analog to Digital Converter, 3V supply, 150ksps, SPI interface"
			(at 0 0 0)
		)
		(property "ki_keywords" "adc 2ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC1865L-MS_0_1")
		(symbol "LTC1865L-MS_1_1"
			(pin input line
				(at -20.32 2.54 0)
				(length 6.35)
				(name "CH0")
				(number "2")
			)
			(pin input line
				(at -20.32 -2.54 0)
				(length 6.35)
				(name "CH1")
				(number "3")
			)
			(pin input line
				(at -5.08 10.16 270)
				(length 3.81)
				(name "V_{REF}")
				(number "10")
			)
			(pin power_in line
				(at -5.08 -10.16 90)
				(length 3.81)
				(name "AGND")
				(number "4")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 3.81)
				(name "V_{CC}")
				(number "9")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 3.81)
				(name "DGND")
				(number "5")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "SCK")
				(number "8")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 3.81)
				(name "SDO")
				(number "7")
			)
			(pin input line
				(at 15.24 0 180)
				(length 3.81)
				(name "SDI")
				(number "6")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 3.81)
				(name "CONV")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC1865L-S8"
		(pin_names
			(offset 1.27)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "LTC1865L-S8"
			(at 11.43 7.62 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/18645lfs.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual channel 16-bit SAR Analog to Digital Converter, 3V supply, 150ksps, SPI interface"
			(at 0 0 0)
		)
		(property "ki_keywords" "adc 2ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LTC1865L-S8_0_1")
		(symbol "LTC1865L-S8_1_1"
			(pin input line
				(at -20.32 2.54 0)
				(length 6.35)
				(name "CH0")
				(number "2")
			)
			(pin input line
				(at -20.32 -2.54 0)
				(length 6.35)
				(name "CH1")
				(number "3")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 3.81)
				(name "V_{CC}")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 3.81)
				(name "GND")
				(number "4")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "SCK")
				(number "7")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 3.81)
				(name "SDO")
				(number "6")
			)
			(pin input line
				(at 15.24 0 180)
				(length 3.81)
				(name "SDI")
				(number "5")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 3.81)
				(name "CONV")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC2282xUP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "LTC2282xUP"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.15x7.15mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/2282fb.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual-Channel, 12-Bit Low Power ADC, 105Msps, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC2282xUP_0_1")
		(symbol "LTC2282xUP_1_1"
			(pin passive line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "VCMA")
				(number "61")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "SENSEA")
				(number "62")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "AINA+")
				(number "1")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "AINA-")
				(number "2")
			)
			(pin input line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "REFHA")
				(number "3")
			)
			(pin input line
				(at -17.78 22.86 0)
				(length 2.54)
				(hide yes)
				(name "REFHA")
				(number "4")
			)
			(pin input line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "REFLA")
				(number "5")
			)
			(pin input line
				(at -17.78 20.32 0)
				(length 2.54)
				(hide yes)
				(name "REFLA")
				(number "6")
			)
			(pin passive line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "VCMB")
				(number "20")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "SENSEB")
				(number "19")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "AINB+")
				(number "16")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "AINB-")
				(number "15")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "REFHB")
				(number "13")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 2.54)
				(hide yes)
				(name "REFHB")
				(number "14")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "REFLB")
				(number "11")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 2.54)
				(hide yes)
				(name "REFLB")
				(number "12")
			)
			(pin input line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "CLKA")
				(number "8")
			)
			(pin input line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "CLKB")
				(number "9")
			)
			(pin input line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "MUX")
				(number "21")
			)
			(pin input line
				(at -17.78 -40.64 0)
				(length 2.54)
				(name "MODE")
				(number "60")
			)
			(pin no_connect line
				(at -15.24 -20.32 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "24")
			)
			(pin no_connect line
				(at -15.24 -22.86 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "25")
			)
			(pin no_connect line
				(at -15.24 -25.4 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "41")
			)
			(pin no_connect line
				(at -15.24 -27.94 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "42")
			)
			(pin power_in line
				(at -7.62 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "10")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "18")
			)
			(pin power_in line
				(at -2.54 -48.26 90)
				(length 2.54)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at -2.54 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "64")
			)
			(pin passive line
				(at -2.54 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "65")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "63")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "OGND")
				(number "31")
			)
			(pin passive line
				(at 2.54 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "OGND")
				(number "50")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "OVDD")
				(number "32")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "OVDD")
				(number "49")
			)
			(pin output line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "DA0")
				(number "43")
			)
			(pin output line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "DA1")
				(number "44")
			)
			(pin output line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "DA2")
				(number "45")
			)
			(pin output line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "DA3")
				(number "46")
			)
			(pin output line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "DA4")
				(number "47")
			)
			(pin output line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "DA5")
				(number "48")
			)
			(pin output line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "DA6")
				(number "51")
			)
			(pin output line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "DA7")
				(number "52")
			)
			(pin output line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "DA8")
				(number "53")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "DA9")
				(number "54")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "DA10")
				(number "55")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "DA11")
				(number "56")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "OFA")
				(number "57")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "DB0")
				(number "26")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "DB1")
				(number "27")
			)
			(pin output line
				(at 17.78 0 180)
				(length 2.54)
				(name "DB2")
				(number "28")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "DB3")
				(number "29")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "DB4")
				(number "30")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "DB5")
				(number "33")
			)
			(pin output line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "DB6")
				(number "34")
			)
			(pin output line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "DB7")
				(number "35")
			)
			(pin output line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "DB8")
				(number "36")
			)
			(pin output line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "DB9")
				(number "37")
			)
			(pin output line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "DB10")
				(number "38")
			)
			(pin output line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "DB11")
				(number "39")
			)
			(pin output line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "OFB")
				(number "40")
			)
			(pin input line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "~{OEB}")
				(number "23")
			)
			(pin input line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "~{OEA}")
				(number "58")
			)
			(pin input line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "SHDNB")
				(number "22")
			)
			(pin input line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "SHDNA")
				(number "59")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC2309xF"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 13.97 0)
		)
		(property "Value" "LTC2309xF"
			(at 8.89 13.97 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 27.94 -16.51 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/2309fd.pdf"
			(at -6.35 13.97 0)
		)
		(property "Description" "8 Channels, 12-Bit SAR ADC, I2C interface, TSSOP-20 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "LT ADC 12bit I2C SAR TSSOP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LTC2309xF_0_1"
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "CH5")
				(number "16")
			)
		)
		(symbol "LTC2309xF_1_1"
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "CH0")
				(number "11")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "CH1")
				(number "12")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "CH2")
				(number "13")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "CH3")
				(number "14")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "CH4")
				(number "15")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "CH6")
				(number "17")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "CH7")
				(number "18")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "COM")
				(number "19")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "10")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin input line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "AD1")
				(number "5")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "AD0")
				(number "4")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "SDA")
				(number "7")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "VREF")
				(number "20")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "REFCOMP")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC2309xUF"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 13.97 0)
		)
		(property "Value" "LTC2309xUF"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 1.27 -16.51 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/2309fd.pdf"
			(at -8.89 13.97 0)
		)
		(property "Description" "8 Channels, 12-Bit SAR ADC, I2C interface, QFN-24 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "LT ADC 12bit I2C SAR QFN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC2309xUF_0_1"
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "CH5")
				(number "3")
			)
		)
		(symbol "LTC2309xUF_1_1"
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "CH0")
				(number "22")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "CH1")
				(number "23")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "CH2")
				(number "24")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "CH3")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "CH4")
				(number "2")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "CH6")
				(number "4")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "CH7")
				(number "5")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "COM")
				(number "6")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "12")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "13")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "21")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "19")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "20")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin input line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "AD1")
				(number "15")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "AD0")
				(number "14")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SCL")
				(number "16")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "SDA")
				(number "17")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "VREF")
				(number "7")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "REFCOMP")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC2311-16"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -14.605 13.97 0)
		)
		(property "Value" "LTC2311-16"
			(at 8.89 13.97 0)
		)
		(property "Footprint" "Package_SO:MSOP-16-1EP_3x4.039mm_P0.5mm_EP1.651x2.845mm"
			(at 34.29 21.59 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/231116fa.pdf"
			(at 48.26 19.05 0)
		)
		(property "Description" "16-Bit, 5Msps Differential Input ADC with Wide Input Common Mode Range, LVDS/CMOS interface, MSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "16-bit adc differential input 5 msps lvds cmos"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*1EP*3x4.039mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC2311-16_0_1")
		(symbol "LTC2311-16_1_1"
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "A_{IN+}")
				(number "6")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "A_{IN-}")
				(number "7")
			)
			(pin passive line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "REFIN")
				(number "2")
			)
			(pin passive line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "REFOUT")
				(number "3")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "V_{DD}")
				(number "4")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "OV_{DD}")
				(number "12")
			)
			(pin input line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "~{CNV}")
				(number "9")
			)
			(pin input line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "SCK^{+}")
				(number "16")
			)
			(pin input line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "SCK^{-}")
				(number "15")
			)
			(pin tri_state line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "SDO^{+}")
				(number "14")
			)
			(pin tri_state line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "SDO^{-}")
				(number "13")
			)
			(pin input line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "~{CMOS}/LVDS")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC2325-16"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 34.29 0)
		)
		(property "Value" "LTC2325-16"
			(at 8.89 34.29 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-52-1EP_7x8mm_P0.5mm_EP5.41x6.45mm_ThermalVias"
			(at -1.27 -55.88 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/232516fa.pdf"
			(at -6.35 60.96 0)
		)
		(property "Description" "Quad, 16-Bit, 5Msps/Ch Simultaneous Sampling ADC, LVDS/CMOS interface, QFN-52"
			(at 0 0 0)
		)
		(property "ki_keywords" "16-Bit 5msps 4 channel adc lvds cmos"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*P0.5mm*5.41x6.45mm*"
			(at 0 0 0)
		)
		(symbol "LTC2325-16_0_1")
		(symbol "LTC2325-16_1_1"
			(pin input line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "A_{IN1+}")
				(number "14")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "A_{IN1-}")
				(number "13")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "A_{IN2+}")
				(number "11")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "A_{IN2-}")
				(number "10")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "A_{IN3+}")
				(number "5")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "A_{IN3-}")
				(number "4")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "A_{IN4+}")
				(number "2")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "A_{IN4-}")
				(number "1")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "REFBUFEN")
				(number "43")
			)
			(pin passive line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "REF")
				(number "8")
			)
			(pin passive line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "REFOUT1")
				(number "22")
			)
			(pin passive line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "REFOUT2")
				(number "9")
			)
			(pin passive line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "REFOUT3")
				(number "6")
			)
			(pin passive line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "REFOUT4")
				(number "45")
			)
			(pin no_connect line
				(at -12.7 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin no_connect line
				(at -10.16 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin no_connect line
				(at -7.62 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "19")
			)
			(pin no_connect line
				(at -5.08 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "20")
			)
			(pin power_in line
				(at -2.54 35.56 270)
				(length 2.54)
				(name "V_{DD}")
				(number "15")
			)
			(pin passive line
				(at -2.54 35.56 270)
				(length 2.54)
				(hide yes)
				(name "V_{DD}")
				(number "21")
			)
			(pin passive line
				(at -2.54 35.56 270)
				(length 2.54)
				(hide yes)
				(name "V_{DD}")
				(number "44")
			)
			(pin passive line
				(at -2.54 35.56 270)
				(length 2.54)
				(hide yes)
				(name "V_{DD}")
				(number "52")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "26")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "32")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "38")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "46")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "49")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "53")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 2.54)
				(name "OV_{DD}")
				(number "31")
			)
			(pin passive line
				(at 2.54 35.56 270)
				(length 2.54)
				(hide yes)
				(name "OV_{DD}")
				(number "37")
			)
			(pin no_connect line
				(at 5.08 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "47")
			)
			(pin no_connect line
				(at 7.62 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "48")
			)
			(pin no_connect line
				(at 10.16 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "50")
			)
			(pin no_connect line
				(at 12.7 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "51")
			)
			(pin input line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "~{CNV}")
				(number "24")
			)
			(pin input line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "SCK^{+}")
				(number "41")
				(alternate "SCK" input line)
			)
			(pin input line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "SCK^{-}")
				(number "42")
				(alternate "DNC" no_connect line)
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "SDOA^{+}")
				(number "27")
				(alternate "SDOA" tri_state line)
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "SDOA^{-}")
				(number "28")
				(alternate "DNC" no_connect line)
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "SDOB^{+}")
				(number "29")
				(alternate "SDOB" tri_state line)
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "SDOB^{-}")
				(number "30")
				(alternate "DNC" no_connect line)
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "SDOC^{+}")
				(number "35")
				(alternate "SDOC" tri_state line)
			)
			(pin output line
				(at 17.78 0 180)
				(length 2.54)
				(name "SDOC^{-}")
				(number "36")
				(alternate "DNC" no_connect line)
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "SDOD^{+}")
				(number "39")
				(alternate "SDOD" tri_state line)
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "SDOD^{-}")
				(number "40")
				(alternate "DNC" no_connect line)
			)
			(pin output line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "CLKOUT^{+}")
				(number "33")
				(alternate "CLKOUT" tri_state line)
			)
			(pin output line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "CLKOUT^{-}")
				(number "34")
				(alternate "~{CLKOUTEN}" input line)
			)
			(pin input line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "~{CMOS}/LVDS")
				(number "25")
			)
			(pin input line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "~{SDR}/DDR")
				(number "23")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC2358-16"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "LTC2358-16"
			(at 6.35 36.83 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 0 -48.26 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/235816f.pdf"
			(at -6.35 19.05 0)
		)
		(property "Description" "LTC2358 Buffered Octal, 16 bit, 200ksps/Ch Differential ±10.24V Simultaneous Sampling ADC, 30Vpp common mode range, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "16bit Simultaneous Sampling ADC 8 Channels SPI buffered"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP?48*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC2358-16_0_1")
		(symbol "LTC2358-16_1_1"
			(pin input line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "IN0+")
				(number "14")
			)
			(pin input line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "IN0-")
				(number "13")
			)
			(pin input line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "IN1+")
				(number "12")
			)
			(pin input line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "IN1-")
				(number "11")
			)
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "IN2+")
				(number "10")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "IN2-")
				(number "9")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "IN3+")
				(number "8")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "IN3-")
				(number "7")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "IN4+")
				(number "6")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "IN4-")
				(number "5")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "IN5+")
				(number "4")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "IN5-")
				(number "3")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "IN6+")
				(number "2")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "IN6-")
				(number "1")
			)
			(pin input line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "IN7+")
				(number "48")
			)
			(pin input line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "IN7-")
				(number "47")
			)
			(pin passive line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "REFIN")
				(number "19")
			)
			(pin passive line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "REFBUF")
				(number "21")
			)
			(pin power_in line
				(at -5.08 38.1 270)
				(length 2.54)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at -2.54 -38.1 90)
				(length 2.54)
				(name "VEE")
				(number "17")
			)
			(pin passive line
				(at -2.54 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VEE")
				(number "45")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "OVDD")
				(number "31")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 2.54)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 2.54 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 2.54 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "20")
			)
			(pin passive line
				(at 2.54 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "30")
			)
			(pin passive line
				(at 2.54 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "41")
			)
			(pin passive line
				(at 2.54 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "44")
			)
			(pin passive line
				(at 2.54 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "46")
			)
			(pin passive line
				(at 5.08 38.1 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "42")
			)
			(pin power_in line
				(at 5.08 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "43")
			)
			(pin input line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "~{CS}")
				(number "39")
			)
			(pin output line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "BUSY")
				(number "38")
			)
			(pin input line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "SDI")
				(number "37")
			)
			(pin tri_state line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "SDO7")
				(number "36")
			)
			(pin tri_state line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "SDO-/SDO6")
				(number "35")
			)
			(pin tri_state line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "SDO+/SDO5")
				(number "34")
			)
			(pin tri_state line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "SCKO-/SDO4")
				(number "33")
			)
			(pin tri_state line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "SCKO+/SCKO")
				(number "32")
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "SCKI-/SCKI")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "SCKI+/SDO3")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "SDI-/SDO2")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "SDI+/SDO1")
				(number "26")
			)
			(pin tri_state line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "SDO0")
				(number "25")
			)
			(pin input line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "CNV")
				(number "24")
			)
			(pin input line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "LVDS/~{CMOS}")
				(number "23")
			)
			(pin input line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD")
				(number "22")
			)
			(pin passive line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "VDDLBYP")
				(number "40")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC2451xDDB"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "LTC2451xDDB"
			(at 11.43 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_2x3mm_P0.5mm_EP0.61x2.2mm"
			(at -15.24 12.7 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/2451fg.pdf"
			(at -17.78 12.7 0)
		)
		(property "Description" "Analog to Digital Converter, Single Channel, 16-Bit, 30/60 SPS, 2.7V to 5.5V, I2C interface, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "analog to digital converter adc i2c twi single channel delta sigma 16 bit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*2x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC2451xDDB_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN")
				(number "6")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "REF+")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "REF-")
				(number "2")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 2.54 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 2.54 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SCL")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SDA")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC2451xTS8"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "LTC2451xTS8"
			(at 11.43 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-8"
			(at -17.78 12.7 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/2451fg.pdf"
			(at -17.78 12.7 0)
		)
		(property "Description" "Analog to Digital Converter, Single Channel, 16-Bit, 30/60 SPS, 2.7V to 5.5V, I2C interface, TSOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "analog to digital converter adc i2c twi single channel delta sigma 16 bit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "LTC2451xTS8_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN")
				(number "6")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "REF+")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "REF-")
				(number "2")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 2.54 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SCL")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SDA")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC2508CDKD-32"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 19.05 0)
		)
		(property "Value" "LTC2508CDKD-32"
			(at 22.86 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-24-1EP_4x7mm_P0.5mm_EP2.64x6.44mm"
			(at -24.13 -24.13 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/250832fc.pdf"
			(at 5.08 -26.67 0)
		)
		(property "Description" "32-Bit Oversampling ADC with Configurable Digital Filter, 0°C to 70°C, DFN-24 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "LT ADC 32bit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*4x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC2508CDKD-32_0_1")
		(symbol "LTC2508CDKD-32_1_1"
			(pin input line
				(at -15.24 10.16 0)
				(length 5.08)
				(name "IN+")
				(number "5")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 5.08)
				(name "IN-")
				(number "6")
			)
			(pin input clock
				(at -15.24 2.54 0)
				(length 5.08)
				(name "MCLK")
				(number "13")
			)
			(pin input line
				(at -15.24 0 0)
				(length 5.08)
				(name "SYNC")
				(number "14")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 5.08)
				(name "SEL0")
				(number "11")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 5.08)
				(name "SEL1")
				(number "12")
			)
			(pin power_in line
				(at -5.08 22.86 270)
				(length 5.08)
				(name "V_{DD}")
				(number "3")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 5.08)
				(name "OV_{DD}")
				(number "22")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "23")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "24")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 5.08)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 5.08 22.86 270)
				(length 5.08)
				(hide yes)
				(name "REF")
				(number "10")
			)
			(pin passive line
				(at 5.08 22.86 270)
				(length 5.08)
				(name "REF")
				(number "8")
			)
			(pin passive line
				(at 5.08 22.86 270)
				(length 5.08)
				(hide yes)
				(name "REF")
				(number "9")
			)
			(pin input line
				(at 15.24 10.16 180)
				(length 5.08)
				(name "~{RDLA}")
				(number "1")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 5.08)
				(name "~{RDLB}")
				(number "2")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 5.08)
				(name "~{DRL}")
				(number "15")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "BUSY")
				(number "21")
			)
			(pin input clock
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "SCKA")
				(number "18")
			)
			(pin tri_state line
				(at 15.24 -5.08 180)
				(length 5.08)
				(name "SDOA")
				(number "17")
			)
			(pin input clock
				(at 15.24 -7.62 180)
				(length 5.08)
				(name "SCKB")
				(number "19")
			)
			(pin tri_state line
				(at 15.24 -10.16 180)
				(length 5.08)
				(name "SDOB")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX1112"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 10.16 -13.97 0)
		)
		(property "Value" "MAX1112"
			(at 10.16 16.51 0)
		)
		(property "Footprint" "Package_SO:SSOP-20_5.3x7.2mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX1112-MAX1113.pdf"
			(at 8.89 -13.97 0)
		)
		(property "Description" "8-Channel Single-Ended or 4-Channel Differential 8-Bit ADC, SSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "MAXIM ADC 5V 8-Bit SPI QSPI MICROWIRE"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x7.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MAX1112_0_1")
		(symbol "MAX1112_1_1"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "CH0")
				(number "1")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "CH1")
				(number "2")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "CH2")
				(number "3")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "CH3")
				(number "4")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "CH4")
				(number "5")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "CH5")
				(number "6")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "CH6")
				(number "7")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "CH7")
				(number "8")
			)
			(pin power_in line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "COM")
				(number "9")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "AGND")
				(number "13")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "DGND")
				(number "14")
			)
			(pin power_in line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "REFIN")
				(number "11")
			)
			(pin power_out line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "REFOUT")
				(number "12")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "~{CS}")
				(number "18")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "DOUT")
				(number "15")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "DIN")
				(number "17")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SCLK")
				(number "19")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "~{SHDN}")
				(number "10")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "SSTRB")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX11120xTI"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 19.05 0)
		)
		(property "Value" "MAX11120xTI"
			(at 10.16 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:TQFN-28-1EP_5x5mm_P0.5mm_EP3.25x3.25mm"
			(at 0 21.59 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX11120-MAX11128.pdf"
			(at 8.89 -16.51 0)
		)
		(property "Description" "4-Channel 8-Bit 1.5MHz Full-Linear Bandwidth External Reference High-Speed Low-Power ADC, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "MAXIM ADC 3.3V 8-Bit SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MAX11120xTI_0_1")
		(symbol "MAX11120xTI_1_1"
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "AIN0")
				(number "26")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "AIN1")
				(number "27")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "AIN2")
				(number "28")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "AIN3")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 2.54)
				(name "EP")
				(number "29")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin passive line
				(at 0 20.32 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "18")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "OVDD")
				(number "23")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "DGND")
				(number "22")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "~{CNVST}")
				(number "12")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "REF-")
				(number "13")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "REF+")
				(number "15")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "~{CS}")
				(number "20")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "DOUT")
				(number "24")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "DIN")
				(number "21")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "SCLK")
				(number "19")
			)
			(pin output line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "~{EOC}")
				(number "25")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX11123xTI"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 19.05 0)
		)
		(property "Value" "MAX11123xTI"
			(at 10.16 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:TQFN-28-1EP_5x5mm_P0.5mm_EP3.25x3.25mm"
			(at 0 21.59 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX11120-MAX11128.pdf"
			(at 8.89 -16.51 0)
		)
		(property "Description" "8-Channel 8-Bit 1.5MHz Full-Linear Bandwidth External Reference High-Speed Low-Power ADC, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "MAXIM ADC 3.3V 8-Bit SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MAX11123xTI_0_1")
		(symbol "MAX11123xTI_1_1"
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "AIN0")
				(number "26")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "AIN1")
				(number "27")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "AIN2")
				(number "28")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "AIN3")
				(number "1")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "AIN4")
				(number "2")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "AIN5")
				(number "3")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "AIN6")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "AIN7")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 2.54)
				(name "EP")
				(number "29")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin passive line
				(at 0 20.32 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "18")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "OVDD")
				(number "23")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "DGND")
				(number "22")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "~{CNVST}")
				(number "12")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "REF-")
				(number "13")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "REF+")
				(number "15")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "~{CS}")
				(number "20")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "DOUT")
				(number "24")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "DIN")
				(number "21")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "SCLK")
				(number "19")
			)
			(pin output line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "~{EOC}")
				(number "25")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX11126xTI"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 19.05 0)
		)
		(property "Value" "MAX11126xTI"
			(at 10.16 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:TQFN-28-1EP_5x5mm_P0.5mm_EP3.25x3.25mm"
			(at 0 21.59 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX11120-MAX11128.pdf"
			(at 8.89 -16.51 0)
		)
		(property "Description" "16-Channel 8-Bit 1.5MHz Full-Linear Bandwidth External Reference High-Speed Low-Power ADC, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "MAXIM ADC 3.3V 8-Bit SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MAX11126xTI_0_1")
		(symbol "MAX11126xTI_1_1"
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "AIN0")
				(number "26")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "AIN1")
				(number "27")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "AIN2")
				(number "28")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "AIN3")
				(number "1")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "AIN4")
				(number "2")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "AIN5")
				(number "3")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "AIN6")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "AIN7")
				(number "5")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "AIN8")
				(number "6")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "AIN9")
				(number "7")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "AIN10")
				(number "8")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "AIN11")
				(number "9")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "AIN12")
				(number "10")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 2.54)
				(name "EP")
				(number "29")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin passive line
				(at 0 20.32 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "18")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "16")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "OVDD")
				(number "23")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "DGND")
				(number "22")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "AIN13")
				(number "11")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "~{CNVST}/AIN14")
				(number "12")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "REF-/AIN15")
				(number "13")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "REF+")
				(number "15")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "~{CS}")
				(number "20")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "DOUT")
				(number "24")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "DIN")
				(number "21")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "SCLK")
				(number "19")
			)
			(pin output line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "~{EOC}")
				(number "25")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX1113"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 10.16 -13.97 0)
		)
		(property "Value" "MAX1113"
			(at 10.16 16.51 0)
		)
		(property "Footprint" "Package_SO:QSOP-16_3.9x4.9mm_P0.635mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX1112-MAX1113.pdf"
			(at 8.89 -13.97 0)
		)
		(property "Description" "4-Channel Single-Ended or 2-Channel Differential 8-Bit ADC, QSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "MAXIM ADC 5V 8-Bit SPI QSPI MICROWIRE"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "MAX1113_0_1")
		(symbol "MAX1113_1_1"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "CH0")
				(number "1")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "CH1")
				(number "2")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "CH2")
				(number "3")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "CH3")
				(number "4")
			)
			(pin power_in line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "COM")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "AGND")
				(number "9")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "DGND")
				(number "10")
			)
			(pin power_in line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "REFIN")
				(number "7")
			)
			(pin power_out line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "REFOUT")
				(number "8")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "~{CS}")
				(number "14")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "DOUT")
				(number "11")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "DIN")
				(number "13")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SCLK")
				(number "15")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "~{SHDN}")
				(number "6")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "SSTRB")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX11612"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 11.43 -3.81 0)
		)
		(property "Value" "MAX11612"
			(at 11.43 -6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 11.43 -8.89 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX11612-MAX11617.pdf"
			(at 2.54 12.7 0)
		)
		(property "Description" "4-channel single-ended or 2-channel, differential, 12-bit ADC, I2C, 4.096V internal reference, 8-MSOP package"
			(at 0 0 0)
		)
		(property "ki_keywords" "adc i2c 4ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MAX11612_0_1")
		(symbol "MAX11612_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "AIN0")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "AIN1")
				(number "2")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "AIN2")
				(number "3")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "AIN3/REF")
				(number "4")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "Vdd")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "SCL")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "SDA")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX11614"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 11.43 -11.43 0)
		)
		(property "Value" "MAX11614"
			(at 11.43 -13.97 0)
		)
		(property "Footprint" "Package_SO:QSOP-16_3.9x4.9mm_P0.635mm"
			(at 11.43 -16.51 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX11612-MAX11617.pdf"
			(at 2.54 20.32 0)
		)
		(property "Description" "8-channel single-ended or 4-channel, differential, 12-bit ADC, I2C, 4.096V internal reference, 16-QSOP package"
			(at 0 0 0)
		)
		(property "ki_keywords" "adc i2c 8ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "MAX11614_0_1")
		(symbol "MAX11614_1_1"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "AIN0")
				(number "5")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "AIN1")
				(number "6")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "AIN2")
				(number "7")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "AIN3")
				(number "8")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "AIN4")
				(number "9")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "AIN5")
				(number "10")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "AIN6")
				(number "11")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "AIN7")
				(number "12")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "REF")
				(number "1")
			)
			(pin no_connect line
				(at -10.16 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at -10.16 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at -10.16 -12.7 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "Vdd")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "15")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "SCL")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SDA")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX11616"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 11.43 -11.43 0)
		)
		(property "Value" "MAX11616"
			(at 11.43 -13.97 0)
		)
		(property "Footprint" "Package_SO:QSOP-16_3.9x4.9mm_P0.635mm"
			(at 11.43 -16.51 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX11612-MAX11617.pdf"
			(at 2.54 20.32 0)
		)
		(property "Description" "12-channel single-ended or 6-channel, differential, 12-bit ADC, I2C, 4.096V internal reference, 16-QSOP package"
			(at 0 0 0)
		)
		(property "ki_keywords" "adc i2c 12ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "MAX11616_0_1")
		(symbol "MAX11616_1_1"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "AIN0")
				(number "5")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "AIN1")
				(number "6")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "AIN2")
				(number "7")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "AIN3")
				(number "8")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "AIN4")
				(number "9")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "AIN5")
				(number "10")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "AIN6")
				(number "11")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "AIN7")
				(number "12")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "AIN8")
				(number "4")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "AIN9")
				(number "3")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "AIN10")
				(number "2")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "AIN11")
				(number "1")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "Vdd")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "15")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "SCL")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SDA")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX1248"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 19.05 0)
		)
		(property "Value" "MAX1248"
			(at 0 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX1248-MAX1249.pdf"
			(at 0 0 0)
		)
		(property "Description" "4-Channel 10-Bit ADC with Serial Interface, +2.7V to +5.25V, Internal 2.5V Reference, Low-Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "10-Bit ADC Internal Reference Serial 4-Channel Maxim"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* QSOP*"
			(at 0 0 0)
		)
		(symbol "MAX1248_0_1")
		(symbol "MAX1248_1_1"
			(pin input line
				(at -15.24 10.16 0)
				(length 5.08)
				(name "~{CS}")
				(number "15")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 5.08)
				(name "SCLK")
				(number "16")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 5.08)
				(name "DIN")
				(number "14")
			)
			(pin output line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "DOUT")
				(number "12")
			)
			(pin output line
				(at -15.24 -5.08 0)
				(length 5.08)
				(name "SSTRB")
				(number "13")
			)
			(pin tri_state line
				(at -15.24 -7.62 0)
				(length 5.08)
				(name "~{SHDN}")
				(number "7")
			)
			(pin power_in line
				(at -5.08 -22.86 90)
				(length 5.08)
				(name "DGND")
				(number "11")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 5.08)
				(name "AGND")
				(number "10")
			)
			(pin power_in line
				(at 5.08 -22.86 90)
				(length 5.08)
				(name "COM")
				(number "6")
			)
			(pin input line
				(at 15.24 10.16 180)
				(length 5.08)
				(name "CH0")
				(number "2")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 5.08)
				(name "CH1")
				(number "3")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 5.08)
				(name "CH2")
				(number "4")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "CH3")
				(number "5")
			)
			(pin power_in line
				(at 15.24 -5.08 180)
				(length 5.08)
				(name "VREF")
				(number "8")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 5.08)
				(name "REFADJ")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX1274"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 16.51 0)
		)
		(property "Value" "MAX1274"
			(at 1.27 13.97 0)
		)
		(property "Footprint" ""
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX1274-MAX1275.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "1.8Msps, Single-Supply, Low-Power, True-Differential, 12-Bit ADCs, bipolar input"
			(at 0 0 0)
		)
		(property "ki_keywords" "12bit ADC 1CH diff differential"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*4x4mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "MAX1274_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "AIN-")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "AIN+")
				(number "12")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "REF")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "RGND")
				(number "3")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "PAD")
				(number "13")
			)
			(pin no_connect line
				(at 7.62 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin no_connect line
				(at 7.62 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "VL")
				(number "7")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "CNVST")
				(number "9")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "DOUT")
				(number "8")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCLK")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP3002"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "MCP3002"
			(at 11.43 11.43 0)
		)
		(property "Footprint" ""
			(at 0 -2.54 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21294E.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Dual Channel 10-Bit A/D Converter with SPI Serial Interface"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Channel 10-Bit ADC SPI 2CH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm** SOIC*3.9x4.9mm*P1.27mm* TSSOP*3x3mm*P0.65mm* MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP3002_0_1")
		(symbol "MCP3002_1_1"
			(pin passive line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "CH0")
				(number "2")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "CH1")
				(number "3")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD/VREF")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin input line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "~{CS}/SHDN")
				(number "1")
			)
			(pin input line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "CLK")
				(number "7")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "DOUT")
				(number "6")
			)
			(pin input line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "DIN")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP3004"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 8.89 0)
		)
		(property "Value" "MCP3004"
			(at 10.16 8.89 0)
		)
		(property "Footprint" ""
			(at 22.86 -7.62 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21295C.pdf"
			(at 22.86 -7.62 0)
		)
		(property "Description" "4-Channel 10-Bit A/D Converters with SPI Interface"
			(at 0 0 0)
		)
		(property "ki_keywords" "10-Bit ADC SPI 4CH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x8.7mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP3004_0_0"
			(text "MUX"
				(at -6.35 -1.27 900)
			)
			(text "ADC"
				(at -0.635 -1.27 0)
			)
			(text "CNTRL"
				(at 5.969 -2.921 900)
			)
		)
		(symbol "MCP3004_0_1")
		(symbol "MCP3004_1_1"
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "CH0")
				(number "1")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "CH1")
				(number "2")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "CH2")
				(number "3")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "CH3")
				(number "4")
			)
			(pin no_connect line
				(at -12.7 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at -12.7 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "Vref")
				(number "13")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "AGND")
				(number "12")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "Vdd")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "DGND")
				(number "7")
			)
			(pin input clock
				(at 15.24 2.54 180)
				(length 2.54)
				(name "CLK")
				(number "11")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "Dout")
				(number "10")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "Din")
				(number "9")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "~{CS}/SHDN")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP3201"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 8.89 0)
		)
		(property "Value" "MCP3201"
			(at 3.81 6.35 0)
		)
		(property "Footprint" ""
			(at 19.05 -8.89 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21290D.pdf"
			(at 20.32 -2.54 0)
		)
		(property "Description" "2.7V 12-Bit A/D Converter with SPI™ Serial Interface, PDIP-8/SOIC-8/MSOP-8/TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "12-Bit Differential ADC SPI 1ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP3201_0_0")
		(symbol "MCP3201_1_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 3.81)
				(name "IN+")
				(number "2")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 3.81)
				(name "IN-")
				(number "3")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "Vref")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "Vss")
				(number "4")
			)
			(pin power_in line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "Vdd")
				(number "8")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CLK")
				(number "7")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "Dout")
				(number "6")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "~{CS}/SHDN")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP3204"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 10.795 0)
		)
		(property "Value" "MCP3204"
			(at -5.08 8.89 0)
		)
		(property "Footprint" ""
			(at 22.86 -7.62 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21298c.pdf"
			(at 22.86 -7.62 0)
		)
		(property "Description" "A/D Converter, 12-Bit, 4-Channel, SPI Interface, 2.7V-5.5V"
			(at 0 0 0)
		)
		(property "ki_keywords" "12bit ADC Reference Single Supply SPI 4ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* DIP*W7.62mm* TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP3204_0_0"
			(text "MUX"
				(at -6.35 -1.27 900)
			)
			(text "ADC"
				(at -0.635 -1.27 0)
			)
			(text "CNTRL"
				(at 5.969 -2.667 900)
			)
		)
		(symbol "MCP3204_0_1")
		(symbol "MCP3204_1_1"
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "CH0")
				(number "1")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "CH1")
				(number "2")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "CH2")
				(number "3")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "CH3")
				(number "4")
			)
			(pin no_connect line
				(at -10.16 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at -7.62 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "Vref")
				(number "13")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "AGND")
				(number "12")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "Vdd")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "DGND")
				(number "7")
			)
			(pin input clock
				(at 15.24 2.54 180)
				(length 2.54)
				(name "CLK")
				(number "11")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "Dout")
				(number "10")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "Din")
				(number "9")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "~{CS}/SHDN")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP3208"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 13.335 0)
		)
		(property "Value" "MCP3208"
			(at -5.08 11.43 0)
		)
		(property "Footprint" ""
			(at 2.54 2.54 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21298c.pdf"
			(at 2.54 2.54 0)
		)
		(property "Description" "A/D Converter, 12-Bit, 8-Channel, SPI Interface , 2.7V-5.5V"
			(at 0 0 0)
		)
		(property "ki_keywords" "12bit ADC Reference Single Supply SPI 8ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MCP3208_0_0"
			(text "MUX"
				(at -6.35 -1.27 900)
			)
			(text "ADC"
				(at -0.635 1.27 0)
			)
			(text "CNTRL"
				(at 5.969 -2.921 900)
			)
		)
		(symbol "MCP3208_0_1")
		(symbol "MCP3208_1_1"
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "CH0")
				(number "1")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "CH1")
				(number "2")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "CH2")
				(number "3")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "CH3")
				(number "4")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "CH4")
				(number "5")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "CH5")
				(number "6")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "CH6")
				(number "7")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "CH7")
				(number "8")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "Vref")
				(number "15")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "AGND")
				(number "14")
			)
			(pin power_in line
				(at 5.08 12.7 270)
				(length 2.54)
				(name "Vdd")
				(number "16")
			)
			(pin power_in line
				(at 5.08 -15.24 90)
				(length 2.54)
				(name "DGND")
				(number "9")
			)
			(pin input clock
				(at 15.24 2.54 180)
				(length 2.54)
				(name "CLK")
				(number "13")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "Dout")
				(number "12")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "Din")
				(number "11")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "~{CS}/SHDN")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP3221"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.112 7.874 0)
		)
		(property "Value" "MCP3221"
			(at 7.62 7.874 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0.508 -20.574 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/devicedoc/20001732e.pdf"
			(at 2.794 -23.114 0)
		)
		(property "Description" "Single channel 12bit SAR Analog to Digital Converter, I2C Interface, SOT-23-5"
			(at 2.032 -25.654 0)
		)
		(property "ki_keywords" "ADC 1ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MCP3221_0_1")
		(symbol "MCP3221_1_1"
			(pin input line
				(at -12.7 0 0)
				(length 3.81)
				(name "A_{IN}")
				(number "3")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 3.81)
				(name "V_{DD}")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 3.81)
				(name "V_{SS}")
				(number "2")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 3.81)
				(name "SCL")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 3.81)
				(name "SDA")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP3301"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 4.445 10.795 0)
		)
		(property "Value" "MCP3301"
			(at 4.445 8.89 0)
		)
		(property "Footprint" ""
			(at 20.32 -2.54 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21700D.pdf"
			(at 20.32 -2.54 0)
		)
		(property "Description" "13-Bit Differential Input, Low Power A/D Converter with SPI Interface"
			(at 0 0 0)
		)
		(property "ki_keywords" "13-Bit Differential ADC SPI  1ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MCP3301_0_0")
		(symbol "MCP3301_1_1"
			(pin input line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "IN+")
				(number "2")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "IN-")
				(number "3")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "Vref")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "Vss")
				(number "4")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "Vdd")
				(number "8")
			)
			(pin input clock
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CLK")
				(number "7")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "Dout")
				(number "6")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "~{CS}/SHDN")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP3422Axx-xSN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 8.89 0)
		)
		(property "Value" "MCP3422Axx-xSN"
			(at 20.32 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 21.59 -11.43 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22088c.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "2-Channel, 18-Bit, Delta-Sigma AD-Converter, I²C Interface, Reference, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "18-Bit ADC I2C Delta-Sigma-ADC Delta-Sigma-ADC Reference 2ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MCP3422Axx-xSN_0_0"
			(text "MUX&PGA"
				(at -4.826 -0.254 900)
			)
			(text "ADC"
				(at 0.889 -1.27 0)
			)
			(text "Vref"
				(at 5.969 -7.62 0)
			)
			(text "CNTRL"
				(at 6.731 -4.191 900)
			)
		)
		(symbol "MCP3422Axx-xSN_0_1")
		(symbol "MCP3422Axx-xSN_1_1"
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "CH1+")
				(number "1")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "CH1-")
				(number "2")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "CH2+")
				(number "7")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "CH2-")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V_{DD}")
				(number "3")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "V_{SS}")
				(number "6")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "SCL")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "SDA")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP3423x-xUN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 8.89 0)
		)
		(property "Value" "MCP3423x-xUN"
			(at 19.05 8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22088c.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "2-Channel, 18-Bit, Delta-Sigma AD-Converter, I²C Interface, Reference, MSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "18-Bit ADC I2C Delta-Sigma-ADC Delta-Sigma-ADC Reference 2ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MCP3423x-xUN_0_0"
			(text "MUX&PGA"
				(at -4.826 -0.254 900)
			)
			(text "ADC"
				(at 0.889 -1.27 0)
			)
			(text "Vref"
				(at 5.969 -7.62 0)
			)
			(text "CNTRL"
				(at 6.731 -4.191 900)
			)
		)
		(symbol "MCP3423x-xUN_0_1")
		(symbol "MCP3423x-xUN_1_1"
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "CH1+")
				(number "1")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "CH1-")
				(number "2")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "CH2+")
				(number "4")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "CH2-")
				(number "5")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V_{DD}")
				(number "6")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "V_{SS}")
				(number "3")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "SCL")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "SDA")
				(number "7")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "A0")
				(number "9")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "A1")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP3424x-xSL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 16.51 0)
		)
		(property "Value" "MCP3424x-xSL"
			(at 17.78 16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 21.59 -16.51 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22088c.pdf"
			(at 0 20.32 0)
		)
		(property "Description" "4-Channel, 18-Bit, Delta-Sigma AD-Converter, I²C Interface, Reference, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "18-Bit ADC I2C IIC I²C Delta-Sigma-ADC Reference 4ch quadruple"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MCP3424x-xSL_0_0"
			(text "MUX & PGA"
				(at -4.826 0 900)
			)
			(text "ADC"
				(at 0.889 1.27 0)
			)
			(text "Vref"
				(at 4.953 -6.35 0)
			)
			(text "CNTRL"
				(at 6.731 2.413 900)
			)
		)
		(symbol "MCP3424x-xSL_0_1")
		(symbol "MCP3424x-xSL_1_1"
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "CH1+")
				(number "1")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "CH1-")
				(number "2")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "CH2+")
				(number "3")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "CH2-")
				(number "4")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "CH3+")
				(number "11")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "CH3-")
				(number "12")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "CH4+")
				(number "13")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "CH4-")
				(number "14")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "V_{DD}")
				(number "6")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "V_{SS}")
				(number "5")
			)
			(pin input line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "SCL")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "SDA")
				(number "7")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "A0")
				(number "9")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "A1")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP3425Axx-xCH"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "MCP3425Axx-xCH"
			(at 2.54 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 16.51 -7.62 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22072b.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "Single Delta-Sigma 16bit Analog to Digital Converter, I2C Interface, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Sigma-Delta ADC Converter 16bit I2C  1ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MCP3425Axx-xCH_0_1")
		(symbol "MCP3425Axx-xCH_1_1"
			(pin passive line
				(at -12.7 2.54 0)
				(length 3.81)
				(name "Vin+")
				(number "1")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 3.81)
				(name "Vin-")
				(number "6")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 3.81)
				(name "V_{DD}")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 3.81)
				(name "V_{SS}")
				(number "2")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 3.81)
				(name "SCL")
				(number "3")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 3.81)
				(name "SDA")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP3426Axx-xMC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "MCP3426Axx-xMC"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.75x1.45mm"
			(at 31.75 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22226a.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "16-Bit, Multi-Channel ΔΣ Analog-to-Digital Converter with I2C Interface and On-Board Reference, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "adc 2ch 16bit i2c"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MCP3426Axx-xMC_0_1")
		(symbol "MCP3426Axx-xMC_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "CH1+")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "CH1-")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "CH2+")
				(number "7")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "CH2-")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V_{DD}")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "V_{SS}")
				(number "6")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "V_{SS}")
				(number "9")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SCL")
				(number "5")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP3426Axx-xMS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "MCP3426Axx-xMS"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 19.05 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22226a.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "16-Bit, Multi-Channel ΔΣ Analog-to-Digital Converter with I2C Interface and On-Board Reference, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "adc 2ch 16bit i2c"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP3426Axx-xMS_0_1")
		(symbol "MCP3426Axx-xMS_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "CH1+")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "CH1-")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "CH2+")
				(number "7")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "CH2-")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V_{DD}")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "V_{SS}")
				(number "6")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SCL")
				(number "5")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP3427x-xMF"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 8.89 0)
		)
		(property "Value" "MCP3427x-xMF"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.5mm_EP1.66x2.38mm"
			(at 33.02 -8.89 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22226a.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "16-Bit, Multi-Channel ΔΣ Analog-to-Digital Converter with I2C Interface and On-Board Reference, DFN-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "adc 2ch 16bit i2c"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MCP3427x-xMF_0_1")
		(symbol "MCP3427x-xMF_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "CH1+")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "CH1-")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "CH2+")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "CH2-")
				(number "5")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V_{DD}")
				(number "6")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "V_{SS}")
				(number "11")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "V_{SS}")
				(number "3")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SCL")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "7")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "Adr1")
				(number "10")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "Adr0")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP3427x-xUN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 8.89 0)
		)
		(property "Value" "MCP3427x-xUN"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 20.32 -8.89 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22226a.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "16-Bit, Multi-Channel ΔΣ Analog-to-Digital Converter with I2C Interface and On-Board Reference, MSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "adc 2ch 16bit i2c"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MCP3427x-xUN_0_1")
		(symbol "MCP3427x-xUN_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "CH1+")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "CH1-")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "CH2+")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "CH2-")
				(number "5")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V_{DD}")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "V_{SS}")
				(number "3")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SCL")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "7")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "Adr1")
				(number "10")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "Adr0")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP3428x-xSL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "MCP3428x-xSL"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 21.59 -13.97 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22226a.pdf"
			(at 0 15.24 0)
		)
		(property "Description" "16-Bit, Multi-Channel ΔΣ Analog-to-Digital Converter with I2C Interface and On-Board Reference, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "adc 4ch 16bit i2c"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MCP3428x-xSL_0_1")
		(symbol "MCP3428x-xSL_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "CH1+")
				(number "1")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "CH1-")
				(number "2")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "CH2+")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "CH2-")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "CH3+")
				(number "11")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "CH3-")
				(number "12")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "CH4+")
				(number "13")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "CH4-")
				(number "14")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V_{DD}")
				(number "6")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "V_{SS}")
				(number "5")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SCL")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "7")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "Adr1")
				(number "10")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "Adr0")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP3550-50-EMS"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 7.62 0)
		)
		(property "Value" "MCP3550-50-EMS"
			(at 5.08 7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/21950c.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Delta-Sigma 22bit Analog to Digital Converter, SPI Interface, 50Hz Rejection, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Sigma-Delta ADC Converter 22bit SPI 1ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*"
			(at 0 0 0)
		)
		(symbol "MCP3550-50-EMS_0_1")
		(symbol "MCP3550-50-EMS_1_1"
			(pin passive line
				(at -12.7 2.54 0)
				(length 3.81)
				(name "Vin+")
				(number "2")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 3.81)
				(name "Vin-")
				(number "3")
			)
			(pin input line
				(at -2.54 -10.16 90)
				(length 3.81)
				(name "Vref")
				(number "1")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 3.81)
				(name "Vdd")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 3.81)
				(name "Vss")
				(number "4")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 3.81)
				(name "SCK")
				(number "5")
			)
			(pin output line
				(at 12.7 0 180)
				(length 3.81)
				(name "SDO/~{RDY}")
				(number "6")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 3.81)
				(name "~{CS}")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP3550-60-ESN"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 7.62 0)
		)
		(property "Value" "MCP3550-60-ESN"
			(at 5.08 7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/21950c.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Delta-Sigma 22bit Analog to Digital Converter, SPI Interface, 60Hz Rejection, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Sigma-Delta ADC Converter 22bit SPI 1ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*"
			(at 0 0 0)
		)
		(symbol "MCP3550-60-ESN_0_1")
		(symbol "MCP3550-60-ESN_1_1"
			(pin passive line
				(at -12.7 2.54 0)
				(length 3.81)
				(name "Vin+")
				(number "2")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 3.81)
				(name "Vin-")
				(number "3")
			)
			(pin input line
				(at -2.54 -10.16 90)
				(length 3.81)
				(name "Vref")
				(number "1")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 3.81)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 3.81)
				(name "VSS")
				(number "4")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 3.81)
				(name "SCK")
				(number "5")
			)
			(pin output line
				(at 12.7 0 180)
				(length 3.81)
				(name "SDO/~{RDY}")
				(number "6")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 3.81)
				(name "~{CS}")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD6645"
		(extends "AD6644")
		(property "Reference" "U"
			(at -7.62 26.67 0)
		)
		(property "Value" "AD6645"
			(at 3.81 26.67 0)
		)
		(property "Footprint" "Package_QFP:TQFP-52-1EP_10x10mm_P0.65mm_EP6.5x6.5mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD6645.pdf"
			(at -2.54 -31.75 0)
		)
		(property "Description" "A/D Converter, 14-Bit, 80 MSPS/105 MSPS, TQFP-52"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC differential analog digital converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*1EP*10x10mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "AD7322"
		(extends "AD7321")
		(property "Reference" "U"
			(at 10.16 18.542 0)
		)
		(property "Value" "AD7322"
			(at 16.256 16.764 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at 17.084 -14.224 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD7322.pdf"
			(at 17.084 -18.796 0)
		)
		(property "Description" "2-Channel, software selectable input range ±10 V, ±5V, ±2.5V, 0 V to +10 V, true bipolar input, 12-Bit plus sign, 1 MSPS SAR ADC, TSSOP-14"
			(at 17.084 -16.51 0)
		)
		(property "ki_keywords" "Analog-Devices ADC bipolar 12-Bit SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "AD7324"
		(extends "AD7323")
		(property "Reference" "U"
			(at 10.16 18.542 0)
		)
		(property "Value" "AD7324"
			(at 16.256 16.764 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 17.084 -14.224 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD7324.pdf"
			(at 17.084 -18.796 0)
		)
		(property "Description" "4-Channel, software selectable input range ±10 V, ±5V, ±2.5V, 0 V to +10 V, true bipolar input, 12-Bit plus sign, 1 MSPS SAR ADC, TSSOP-16"
			(at 17.084 -16.51 0)
		)
		(property "ki_keywords" "Analog-Devices ADC bipolar 12-Bit SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "AD7328"
		(extends "AD7327")
		(property "Reference" "U"
			(at 10.16 21.082 0)
		)
		(property "Value" "AD7328"
			(at 16.256 19.304 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 17.084 -18.08 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD7328.pdf"
			(at 17.084 -15.51 0)
		)
		(property "Description" "8-Channel, software selectable input range ±10 V, ±5V, ±2.5V, 0 V to +10 V, true bipolar input, 12-Bit plus sign, 1 MSPS SAR ADC, TSSOP-20"
			(at 17.084 -13.716 0)
		)
		(property "ki_keywords" "Analog-Devices ADC bipolar 12-Bit SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "AD7689xCP"
		(extends "AD7949BCP")
		(property "Reference" "U"
			(at -10.16 16.51 0)
		)
		(property "Value" "AD7689xCP"
			(at 3.81 16.51 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-20-1EP_4x4mm_P0.5mm_EP2.5x2.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD7682_7689.pdf"
			(at 0 0 0)
		)
		(property "Description" "16-Bit, 8-Channel, 250 kSPS PulSAR ADC, LFSCP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC, SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "AD7699BCP"
		(extends "AD7949BCP")
		(property "Reference" "U"
			(at -10.16 16.51 0)
		)
		(property "Value" "AD7699BCP"
			(at 3.81 16.51 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-20-1EP_4x4mm_P0.5mm_EP2.5x2.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD7699.pdf"
			(at 0 0 0)
		)
		(property "Description" "16-Bit, 8-Channel, 500 kSPS PulSAR ADC, LFSCP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC, SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "AD7795"
		(extends "AD7794")
		(property "Reference" "U"
			(at -15.24 24.13 0)
		)
		(property "Value" "AD7795"
			(at 7.62 24.13 0)
		)
		(property "Footprint" "Package_SO:TSSOP-24_4.4x7.8mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD7794_7795.pdf"
			(at 2.54 -7.62 0)
		)
		(property "Description" "16-Bit, 6-Channel Sigma-Delta ADC, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "adc 6ch 16bit serial"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x7.8mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADC101C021CIMM"
		(extends "ADC081C021CIMM")
		(property "Reference" "U"
			(at 3.81 11.43 0)
		)
		(property "Value" "ADC101C021CIMM"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 20.32 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/adc101c021.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "I2C-Compatible, 10-Bit Analog-to-Digital Converter with Alert Function, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC I2C 10-bit Alert"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADC121C021CIMM"
		(extends "ADC081C021CIMM")
		(property "Reference" "U"
			(at 3.81 11.43 0)
		)
		(property "Value" "ADC121C021CIMM"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 20.32 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/adc121c021.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "I2C-Compatible, 12-Bit Analog-to-Digital Converter with Alert Function, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC I2C 12-bit Alert"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADS1113IDGS"
		(extends "ADS1013IDGS")
		(property "Reference" "U"
			(at 2.54 13.97 0)
		)
		(property "Value" "ADS1113IDGS"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_SO:TSSOP-10_3x3mm_P0.5mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads1113.pdf"
			(at 1.27 -17.78 0)
		)
		(property "Description" "Ultra-Small, Low-Power, I2C-Compatible, 860-SPS, 16-Bit ADCs With Internal Reference and Oscillator, VSSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "16 bit single channel I2C ADC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADS1114IDGS"
		(extends "ADS1014IDGS")
		(property "Reference" "U"
			(at 2.54 13.97 0)
		)
		(property "Value" "ADS1114IDGS"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_SO:TSSOP-10_3x3mm_P0.5mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads1113.pdf"
			(at -1.27 -22.86 0)
		)
		(property "Description" "Ultra-Small, Low-Power, I2C-Compatible, 860-SPS, 16-Bit ADCs With Internal Reference, Oscillator, and Programmable Comparator, VSSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "16 bit single channel I2C ADC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADS1115IDGS"
		(extends "ADS1015IDGS")
		(property "Reference" "U"
			(at 2.54 13.97 0)
		)
		(property "Value" "ADS1115IDGS"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_SO:TSSOP-10_3x3mm_P0.5mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads1113.pdf"
			(at -1.27 -22.86 0)
		)
		(property "Description" "Ultra-Small, Low-Power, I2C-Compatible, 860-SPS, 16-Bit ADCs With Internal Reference, Oscillator, and Programmable Comparator, VSSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "16 bit 4 channel I2C ADC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADS1118IDGS"
		(extends "ADS1018IDGS")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "ADS1118IDGS"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at -1.27 -1.27 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads1118.pdf"
			(at -22.86 10.16 0)
		)
		(property "Description" "Ultrasmall, Low-Power, SPI-Compatible, 16-Bit Analog-to-Digital Converter with Internal Reference and Temperature Sensor, VSSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "16 bit 4 channel SPI ADC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADS1220xPW"
		(extends "ADS1120-PW")
		(property "Reference" "U"
			(at -15.24 11.43 0)
		)
		(property "Value" "ADS1220xPW"
			(at 6.35 11.43 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 6.35 13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads1220.pdf"
			(at -12.7 10.16 0)
		)
		(property "Description" "Low-power, quad-input, 24-bit analog to digital converter, integrated temperature sensor, SPI interface, TSSOP-16 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "adc spi"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADS7029"
		(extends "ADS7040xDCU")
		(property "Reference" "U"
			(at -7.62 -7.62 0)
		)
		(property "Value" "ADS7029"
			(at 2.54 -7.62 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_2.3x2mm_P0.5mm"
			(at 2.54 16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads7029-q1.pdf"
			(at 0 0 0)
		)
		(property "Description" "Small-Size, Low-Power, 8-Bit, 2-MSPS, SAR ADC"
			(at 0 0 0)
		)
		(property "ki_keywords" "8 bit SAR ADC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*8*2.3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADS7039"
		(extends "ADS7040xDCU")
		(property "Reference" "U"
			(at -7.62 -7.62 0)
		)
		(property "Value" "ADS7039"
			(at 2.54 -7.62 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_2.3x2mm_P0.5mm"
			(at 2.54 16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads7039-q1.pdf"
			(at 0 0 0)
		)
		(property "Description" "Small-Size, Low-Power, 10-Bit, 2-MSPS, SAR ADC"
			(at 0 0 0)
		)
		(property "ki_keywords" "10 bit SAR ADC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*8*2.3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADS7041xDCU"
		(extends "ADS7040xDCU")
		(property "Reference" "U"
			(at -7.62 -7.62 0)
		)
		(property "Value" "ADS7041xDCU"
			(at 2.54 -7.62 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_2.3x2mm_P0.5mm"
			(at 2.54 16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads7041.pdf"
			(at 0 0 0)
		)
		(property "Description" "Ultra-Low Power, Ultra-Small Size, 10-Bit, 1-MSPS, SAR ADC"
			(at 0 0 0)
		)
		(property "ki_keywords" "10 bit SAR ADC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*8*2.3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADS7042xDCU"
		(extends "ADS7040xDCU")
		(property "Reference" "U"
			(at -7.62 -7.62 0)
		)
		(property "Value" "ADS7042xDCU"
			(at 2.54 -7.62 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_2.3x2mm_P0.5mm"
			(at 2.54 16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads7042.pdf"
			(at 0 0 0)
		)
		(property "Description" "Ultra-Low Power, Ultra-Small Size, 12-Bit, 1-MSPS, SAR ADC"
			(at 0 0 0)
		)
		(property "ki_keywords" "12 bit SAR ADC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*8*2.3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADS7043xDCU"
		(extends "ADS7040xDCU")
		(property "Reference" "U"
			(at -7.62 -7.62 0)
		)
		(property "Value" "ADS7043xDCU"
			(at 2.54 -7.62 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_2.3x2mm_P0.5mm"
			(at 2.54 16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads7043.pdf"
			(at 0 0 0)
		)
		(property "Description" "Ultra-Low Power, Ultra-Small Size, 12-Bit, 1-MSPS, SAR ADC"
			(at 0 0 0)
		)
		(property "ki_keywords" "12 bit SAR ADC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*8*2.3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADS7044xDCU"
		(extends "ADS7040xDCU")
		(property "Reference" "U"
			(at -7.62 -7.62 0)
		)
		(property "Value" "ADS7044xDCU"
			(at 2.54 -7.62 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_2.3x2mm_P0.5mm"
			(at 2.54 16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads7044.pdf"
			(at 0 0 0)
		)
		(property "Description" "Ultra-Low Power, Ultra-Small Size, 12-Bit, 1-MSPS, SAR ADC"
			(at 0 0 0)
		)
		(property "ki_keywords" "12 bit SAR ADC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*8*2.3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADS7049"
		(extends "ADS7040xDCU")
		(property "Reference" "U"
			(at -7.62 -7.62 0)
		)
		(property "Value" "ADS7049"
			(at 2.54 -7.62 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_2.3x2mm_P0.5mm"
			(at 2.54 16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads7049-q1.pdf"
			(at 0 0 0)
		)
		(property "Description" "Small-Size, Low-Power, 12-Bit, 2-MSPS, SAR ADC"
			(at 0 0 0)
		)
		(property "ki_keywords" "12 bit SAR ADC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*8*2.3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADS7867"
		(extends "ADS7866")
		(property "Reference" "U"
			(at 1.27 6.35 0)
		)
		(property "Value" "ADS7867"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0 -1.27 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads7866.pdf"
			(at 1.27 6.35 0)
		)
		(property "Description" "Single Channel 10-bit ADC,  100-200ksps, SPI, micro-power, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOT?23?6*"
			(at 0 0 0)
		)
	)
	(symbol "ADS7868"
		(extends "ADS7866")
		(property "Reference" "U"
			(at 1.27 6.35 0)
		)
		(property "Value" "ADS7868"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0 -1.27 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads7866.pdf"
			(at 1.27 6.35 0)
		)
		(property "Description" "Single Channel 8-bit ADC,  100-200ksps, SPI, micro-power, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOT?23?6*"
			(at 0 0 0)
		)
	)
	(symbol "ADS8685RUM"
		(extends "ADS8681RUM")
		(property "Reference" "U"
			(at 6.35 13.97 0)
		)
		(property "Value" "ADS8685RUM"
			(at 6.35 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_4x4mm_P0.65mm_EP2.7x2.7mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads8681.pdf"
			(at 1.27 6.35 0)
		)
		(property "Description" "16-Bit, High-Speed, Single-Supply, SAR ADC Data Acquisition System with Programmable, Bipolar Input Ranges 500KSPS, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC SPI analog digital"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.65mm*EP2.7x2.7mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADS8689RUM"
		(extends "ADS8681RUM")
		(property "Reference" "U"
			(at 6.35 13.97 0)
		)
		(property "Value" "ADS8689RUM"
			(at 6.35 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_4x4mm_P0.65mm_EP2.7x2.7mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads8681.pdf"
			(at 1.27 6.35 0)
		)
		(property "Description" "16-Bit, High-Speed, Single-Supply, SAR ADC Data Acquisition System with Programmable, Bipolar Input Ranges, 100KSPS, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC SPI analog digital"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.65mm*EP2.7x2.7mm*"
			(at 0 0 0)
		)
	)
	(symbol "ICL7107CPL"
		(extends "ICL7106CPL")
		(property "Reference" "U"
			(at -12.7 31.75 0)
		)
		(property "Value" "ICL7107CPL"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 -31.75 0)
		)
		(property "Datasheet" "https://www.renesas.com/eu/en/www/doc/datasheet/icl7106-07-07s.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "3 1/2 Digit, LED Display, A/D Converter, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED ADC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24*"
			(at 0 0 0)
		)
	)
	(symbol "LTC1406IGN"
		(extends "LTC1406CGN")
		(property "Reference" "U"
			(at -13.97 20.32 0)
		)
		(property "Value" "LTC1406IGN"
			(at 7.62 20.32 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1406f.pdf"
			(at 0 0 0)
		)
		(property "Description" "ADC 8bit Low Power 20Msps, SSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Power ADC 8bit 20Msps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*"
			(at 0 0 0)
		)
	)
	(symbol "LTC1594IS"
		(extends "LTC1594CS")
		(property "Reference" "U"
			(at -11.43 17.78 0)
		)
		(property "Value" "LTC1594IS"
			(at 7.62 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/15948fb.pdf"
			(at 0 0 0)
		)
		(property "Description" "Micropower 12-bit 4 Channel ADC, Serial IO, SO-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "12bit ADC 4 Channel"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*"
			(at 0 0 0)
		)
	)
	(symbol "LTC1598IG"
		(extends "LTC1598CG")
		(property "Reference" "U"
			(at -11.43 22.86 0)
		)
		(property "Value" "LTC1598IG"
			(at 2.54 22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/15948fb.pdf"
			(at 0 0 0)
		)
		(property "Description" "Micropower 12-bit 8 Channel ADC, Serial IO, SSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "12bit ADC 4 Channel"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*"
			(at 0 0 0)
		)
	)
	(symbol "LTC1744"
		(extends "LTC1742")
		(property "Reference" "U"
			(at -10.16 29.21 0)
		)
		(property "Value" "LTC1744"
			(at 10.16 29.21 0)
		)
		(property "Footprint" "Package_SO:TSSOP-48_6.1x12.5mm_P0.5mm"
			(at 0 -38.1 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1744f.pdf"
			(at -12.7 -7.62 0)
		)
		(property "Description" "14-Bit, 50Msps, ADC, TSSOP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC analog digital converter pipeline"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*6.1x12.5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC1746"
		(extends "LTC1742")
		(property "Reference" "U"
			(at -10.16 29.21 0)
		)
		(property "Value" "LTC1746"
			(at 10.16 29.21 0)
		)
		(property "Footprint" "Package_SO:TSSOP-48_6.1x12.5mm_P0.5mm"
			(at 0 -38.1 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1746f.pdf"
			(at -12.7 -7.62 0)
		)
		(property "Description" "Low Power, 14-Bit, 25Msps, ADC, TSSOP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC analog digital converter pipeline"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*6.1x12.5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC1748"
		(extends "LTC1742")
		(property "Reference" "U"
			(at -10.16 29.21 0)
		)
		(property "Value" "LTC1748"
			(at 10.16 29.21 0)
		)
		(property "Footprint" "Package_SO:TSSOP-48_6.1x12.5mm_P0.5mm"
			(at 0 -38.1 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1748fa.pdf"
			(at -12.7 -7.62 0)
		)
		(property "Description" "14-Bit, 80Msps, Low Noise, ADC, TSSOP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC analog digital converter pipeline"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*6.1x12.5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC1864"
		(extends "LTC1864L")
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "LTC1864"
			(at 11.43 7.62 0)
		)
		(property "Footprint" ""
			(at -2.54 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/18645fb.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Single channel 16-bit SAR Analog to Digital Converter, 5V supply, differential input, 150ksps, SPI interface"
			(at 0 0 0)
		)
		(property "ki_keywords" "adc spi 1ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC1865-MS"
		(extends "LTC1865L-MS")
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "LTC1865-MS"
			(at 11.43 7.62 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/18645fb.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual channel 16-bit SAR Analog to Digital Converter, 5V supply, 150ksps, SPI interface"
			(at 0 0 0)
		)
		(property "ki_keywords" "adc 2ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC1865-S8"
		(extends "LTC1865L-S8")
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "LTC1865-S8"
			(at 11.43 7.62 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/18645fb.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual channel 16-bit SAR Analog to Digital Converter, 5V supply, 150ksps, SPI interface"
			(at 0 0 0)
		)
		(property "ki_keywords" "adc 2ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC2284xUP"
		(extends "LTC2282xUP")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "LTC2284xUP"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.15x7.15mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/2284fa.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual-Channel, 14-Bit Low Power ADC, 105Msps, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC2290xUP"
		(extends "LTC2282xUP")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "LTC2290xUP"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.15x7.15mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/2290fa.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual-Channel, 12-Bit Low Power ADC, 10Msps, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC2291xUP"
		(extends "LTC2282xUP")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "LTC2291xUP"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.15x7.15mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/229321fa.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual-Channel, 12-Bit Low Power ADC, 25Msps, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC2292xUP"
		(extends "LTC2282xUP")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "LTC2292xUP"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.15x7.15mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/229321fa.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual-Channel, 12-Bit Low Power ADC, 40Msps, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC2293xUP"
		(extends "LTC2282xUP")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "LTC2293xUP"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.15x7.15mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/229321fa.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual-Channel, 12-Bit Low Power ADC, 65Msps, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC2294xUP"
		(extends "LTC2282xUP")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "LTC2294xUP"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.15x7.15mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/2294fa.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual-Channel, 12-Bit Low Power ADC, 80Msps, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC2295xUP"
		(extends "LTC2282xUP")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "LTC2295xUP"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.15x7.15mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/2295fa.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual-Channel, 14-Bit Low Power ADC, 10Msps, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC2296xUP"
		(extends "LTC2282xUP")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "LTC2296xUP"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.15x7.15mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/229876fa.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual-Channel, 14-Bit Low Power ADC, 25Msps, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC2297xUP"
		(extends "LTC2282xUP")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "LTC2297xUP"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.15x7.15mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/229876fa.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual-Channel, 14-Bit Low Power ADC, 40Msps, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC2298xUP"
		(extends "LTC2282xUP")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "LTC2298xUP"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.15x7.15mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/229876fa.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual-Channel, 14-Bit Low Power ADC, 65Msps, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC2299xUP"
		(extends "LTC2282xUP")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "LTC2299xUP"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.15x7.15mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/2299fa.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual-Channel, 14-Bit Low Power ADC, 80Msps, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC2358-18"
		(extends "LTC2358-16")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "LTC2358-18"
			(at 6.35 36.83 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 0 -48.26 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/235818f.pdf"
			(at -6.35 19.05 0)
		)
		(property "Description" "LTC2358 Buffered Octal, 18 bit, 200ksps/Ch Differential ±10.24V Simultaneous Sampling ADC, 30Vpp common mode range, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "18bit Simultaneous Sampling ADC 8 Channels SPI buffered"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP?48*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC2508IDKD-32"
		(extends "LTC2508CDKD-32")
		(property "Reference" "U"
			(at -10.16 19.05 0)
		)
		(property "Value" "LTC2508IDKD-32"
			(at 22.86 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-24-1EP_4x7mm_P0.5mm_EP2.64x6.44mm"
			(at -24.13 -24.13 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/250832fc.pdf"
			(at 5.08 -26.67 0)
		)
		(property "Description" "32-Bit Oversampling ADC with Configurable Digital Filter, -40°C to 85°C, DFN-24 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "LT ADC 32bit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*4x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX11121xTI"
		(extends "MAX11120xTI")
		(property "Reference" "U"
			(at -8.89 19.05 0)
		)
		(property "Value" "MAX11121xTI"
			(at 10.16 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:TQFN-28-1EP_5x5mm_P0.5mm_EP3.25x3.25mm"
			(at 0 21.59 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX11120-MAX11128.pdf"
			(at 8.89 -16.51 0)
		)
		(property "Description" "4-Channel 10-Bit 1.5MHz Full-Linear Bandwidth External Reference High-Speed Low-Power ADC, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "MAXIM ADC 3.3V 10-Bit SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX11122xTI"
		(extends "MAX11120xTI")
		(property "Reference" "U"
			(at -8.89 19.05 0)
		)
		(property "Value" "MAX11122xTI"
			(at 10.16 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:TQFN-28-1EP_5x5mm_P0.5mm_EP3.25x3.25mm"
			(at 0 21.59 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX11120-MAX11128.pdf"
			(at 8.89 -16.51 0)
		)
		(property "Description" "4-Channel 12-Bit 1.5MHz Full-Linear Bandwidth External Reference High-Speed Low-Power ADC, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "MAXIM ADC 3.3V 12-Bit SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX11124xTI"
		(extends "MAX11123xTI")
		(property "Reference" "U"
			(at -8.89 19.05 0)
		)
		(property "Value" "MAX11124xTI"
			(at 10.16 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:TQFN-28-1EP_5x5mm_P0.5mm_EP3.25x3.25mm"
			(at 0 21.59 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX11120-MAX11128.pdf"
			(at 8.89 -16.51 0)
		)
		(property "Description" "8-Channel 10-Bit 1.5MHz Full-Linear Bandwidth External Reference High-Speed Low-Power ADC, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "MAXIM ADC 3.3V 10-Bit SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX11125xTI"
		(extends "MAX11123xTI")
		(property "Reference" "U"
			(at -8.89 19.05 0)
		)
		(property "Value" "MAX11125xTI"
			(at 10.16 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:TQFN-28-1EP_5x5mm_P0.5mm_EP3.25x3.25mm"
			(at 0 21.59 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX11120-MAX11128.pdf"
			(at 8.89 -16.51 0)
		)
		(property "Description" "8-Channel 12-Bit 1.5MHz Full-Linear Bandwidth External Reference High-Speed Low-Power ADC, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "MAXIM ADC 3.3V 12-Bit SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX11127xTI"
		(extends "MAX11126xTI")
		(property "Reference" "U"
			(at -8.89 19.05 0)
		)
		(property "Value" "MAX11127xTI"
			(at 10.16 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:TQFN-28-1EP_5x5mm_P0.5mm_EP3.25x3.25mm"
			(at 0 21.59 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX11120-MAX11128.pdf"
			(at 8.89 -16.51 0)
		)
		(property "Description" "16-Channel 10-Bit 1.5MHz Full-Linear Bandwidth External Reference High-Speed Low-Power ADC, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "MAXIM ADC 3.3V 10-Bit SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX11128xTI"
		(extends "MAX11126xTI")
		(property "Reference" "U"
			(at -8.89 19.05 0)
		)
		(property "Value" "MAX11128xTI"
			(at 10.16 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:TQFN-28-1EP_5x5mm_P0.5mm_EP3.25x3.25mm"
			(at 0 21.59 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX11120-MAX11128.pdf"
			(at 8.89 -16.51 0)
		)
		(property "Description" "16-Channel 12-Bit 1.5MHz Full-Linear Bandwidth External Reference High-Speed Low-Power ADC, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "MAXIM ADC 3.3V 12-Bit SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX11613"
		(extends "MAX11612")
		(property "Reference" "U"
			(at 11.43 -3.81 0)
		)
		(property "Value" "MAX11613"
			(at 11.43 -6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 11.43 -8.89 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX11612-MAX11617.pdf"
			(at 2.54 12.7 0)
		)
		(property "Description" "4-channel single-ended or 2-channel, differential, 12-bit ADC, I2C, 2.048V internal reference, 8-MSOP package"
			(at 0 0 0)
		)
		(property "ki_keywords" "adc i2c 4ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX11615"
		(extends "MAX11614")
		(property "Reference" "U"
			(at 11.43 -11.43 0)
		)
		(property "Value" "MAX11615"
			(at 11.43 -13.97 0)
		)
		(property "Footprint" "Package_SO:QSOP-16_3.9x4.9mm_P0.635mm"
			(at 11.43 -16.51 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX11612-MAX11617.pdf"
			(at 2.54 20.32 0)
		)
		(property "Description" "8-channel single-ended or 4-channel, differential, 12-bit ADC, I2C, 2.048V internal reference, 16-QSOP package"
			(at 0 0 0)
		)
		(property "ki_keywords" "adc i2c 8ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX11617"
		(extends "MAX11616")
		(property "Reference" "U"
			(at 11.43 -11.43 0)
		)
		(property "Value" "MAX11617"
			(at 11.43 -13.97 0)
		)
		(property "Footprint" "Package_SO:QSOP-16_3.9x4.9mm_P0.635mm"
			(at 11.43 -16.51 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX11612-MAX11617.pdf"
			(at 2.54 20.32 0)
		)
		(property "Description" "12-channel single-ended or 6-channel, differential, 12-bit ADC, I2C, 2.048V internal reference, 16-QSOP package"
			(at 0 0 0)
		)
		(property "ki_keywords" "adc i2c 12ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX1249"
		(extends "MAX1248")
		(property "Reference" "U"
			(at -10.16 19.05 0)
		)
		(property "Value" "MAX1249"
			(at 0 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX1248-MAX1249.pdf"
			(at 0 0 0)
		)
		(property "Description" "4-Channel 10-Bit ADC with Serial Interface, +2.7V to +5.25V, Low-Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "10-Bit ADC Serial 4-Channel Maxim"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* QSOP*"
			(at 0 0 0)
		)
	)
	(symbol "MAX1275"
		(extends "MAX1274")
		(property "Reference" "U"
			(at 1.27 16.51 0)
		)
		(property "Value" "MAX1275"
			(at 1.27 13.97 0)
		)
		(property "Footprint" ""
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX1274-MAX1275.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "1.8Msps, Single-Supply, Low-Power, True-Differential, 12-Bit ADCs, unipolar input"
			(at 0 0 0)
		)
		(property "ki_keywords" "12bit ADC 1CH diff differential"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*4x4mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP3008"
		(extends "MCP3208")
		(property "Reference" "U"
			(at -5.08 13.335 0)
		)
		(property "Value" "MCP3008"
			(at -5.08 11.43 0)
		)
		(property "Footprint" ""
			(at 2.54 2.54 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21295d.pdf"
			(at 2.54 2.54 0)
		)
		(property "Description" "A/D Converter, 10-Bit, 8-Channel, SPI Interface , 2.7V-5.5V"
			(at 0 0 0)
		)
		(property "ki_keywords" "12bit ADC Reference Single Supply SPI 8CH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP3202"
		(extends "MCP3002")
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "MCP3202"
			(at 11.43 11.43 0)
		)
		(property "Footprint" ""
			(at 0 -2.54 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21034D.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "A/D Converter, 12-Bit, 2-Channel, SPI Interface, 2.7V-5.5V"
			(at 0 0 0)
		)
		(property "ki_keywords" "12bit ADC Reference Single Supply SPI 2ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm** SOIC*3.9x4.9mm*P1.27mm* TSSOP*3x3mm*P0.65mm* MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP3421A0T-ECH"
		(extends "MCP3425Axx-xCH")
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "MCP3421A0T-ECH"
			(at 2.54 7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22003e.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "Single Delta-Sigma 18bit Analog to Digital Converter, I2C Interface, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Sigma-Delta ADC Converter 18bit I2C 1ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP3422Axx-xMS"
		(extends "MCP3422Axx-xSN")
		(property "Reference" "U"
			(at -11.43 8.89 0)
		)
		(property "Value" "MCP3422Axx-xMS"
			(at 20.32 8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 20.32 -11.43 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22088c.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "2-Channel, 18-Bit, Delta-Sigma AD-Converter, I²C Interface, Reference, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "18-Bit ADC I2C Delta-Sigma-ADC Delta-Sigma-ADC Reference 2ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP3424x-xST"
		(extends "MCP3424x-xSL")
		(property "Reference" "U"
			(at -11.43 16.51 0)
		)
		(property "Value" "MCP3424x-xST"
			(at 17.78 16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at 21.59 -16.51 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22088c.pdf"
			(at 0 20.32 0)
		)
		(property "Description" "4-Channel, 18-Bit, Delta-Sigma AD-Converter, I²C Interface, Reference, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "18-Bit ADC I2C Delta-Sigma-ADC Reference 4ch quadruple"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP3426Axx-xSN"
		(extends "MCP3426Axx-xMS")
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "MCP3426Axx-xSN"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 20.32 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22226a.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "16-Bit, Multi-Channel ΔΣ Analog-to-Digital Converter with I2C Interface and On-Board Reference, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "adc 2ch 16bit i2c"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP3428x-xST"
		(extends "MCP3428x-xSL")
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "MCP3428x-xST"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at 21.59 -13.97 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22226a.pdf"
			(at 0 15.24 0)
		)
		(property "Description" "16-Bit, Multi-Channel ΔΣ Analog-to-Digital Converter with I2C Interface and On-Board Reference, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "adc 4ch 16bit i2c"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP3551-EMS"
		(extends "MCP3550-50-EMS")
		(property "Reference" "U"
			(at -11.43 7.62 0)
		)
		(property "Value" "MCP3551-EMS"
			(at 5.08 7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/21950c.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Delta-Sigma 22bit Analog to Digital Converter, SPI Interface, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Sigma-Delta ADC Converter 22bit SPI 1ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*"
			(at 0 0 0)
		)
	)
	(symbol "MCP3553-ESN"
		(extends "MCP3550-60-ESN")
		(property "Reference" "U"
			(at -5.08 7.62 0)
		)
		(property "Value" "MCP3553-ESN"
			(at 5.08 7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/21950c.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Delta-Sigma 22bit Analog to Digital Converter, SPI Interface, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Sigma-Delta ADC Converter 22bit SPI 1ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*"
			(at 0 0 0)
		)
	)
)
