(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "AD390JD"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 30.48 0)
		)
		(property "Value" "AD390JD"
			(at 8.89 30.48 0)
		)
		(property "Footprint" ""
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/AD390MIL.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Quad 12bit DAC, 4LSB Gain Error, DH-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "4ch DAC 12bit"
			(at 0 0 0)
		)
		(symbol "AD390JD_0_1")
		(symbol "AD390JD_1_1"
			(pin input line
				(at -17.78 25.4 0)
				(length 3.81)
				(name "D0")
				(number "1")
			)
			(pin input line
				(at -17.78 22.86 0)
				(length 3.81)
				(name "D1")
				(number "2")
			)
			(pin input line
				(at -17.78 20.32 0)
				(length 3.81)
				(name "D2")
				(number "3")
			)
			(pin input line
				(at -17.78 17.78 0)
				(length 3.81)
				(name "D3")
				(number "4")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "D4")
				(number "5")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "D5")
				(number "6")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "D6")
				(number "7")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "D7")
				(number "8")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "D8")
				(number "9")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "D9")
				(number "10")
			)
			(pin input line
				(at -17.78 0 0)
				(length 3.81)
				(name "D10")
				(number "11")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "D11")
				(number "12")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 3.81)
				(name "~{A0}")
				(number "24")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 3.81)
				(name "~{A1}")
				(number "23")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 3.81)
				(name "~{CS1}")
				(number "25")
			)
			(pin input line
				(at -17.78 -20.32 0)
				(length 3.81)
				(name "~{CS2}")
				(number "26")
			)
			(pin input line
				(at -17.78 -22.86 0)
				(length 3.81)
				(name "~{CS3}")
				(number "27")
			)
			(pin input line
				(at -17.78 -25.4 0)
				(length 3.81)
				(name "~{CS4}")
				(number "28")
			)
			(pin power_in line
				(at -5.08 33.02 270)
				(length 3.81)
				(name "+VS")
				(number "22")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 3.81)
				(name "GND")
				(number "13")
			)
			(pin power_in line
				(at 5.08 33.02 270)
				(length 3.81)
				(name "-VS")
				(number "14")
			)
			(pin passive line
				(at 17.78 20.32 180)
				(length 3.81)
				(name "VOUT1")
				(number "18")
			)
			(pin passive line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "VOUT2")
				(number "19")
			)
			(pin passive line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "VOUT3")
				(number "20")
			)
			(pin passive line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "VOUT4")
				(number "21")
			)
			(pin passive line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "REFIN")
				(number "17")
			)
			(pin passive line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "REFOUT")
				(number "16")
			)
			(pin passive line
				(at 17.78 -25.4 180)
				(length 3.81)
				(name "AGND")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD558JN"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 17.78 0)
		)
		(property "Value" "AD558JN"
			(at 2.54 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/AD558.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Single 8-bit DAC, Internal Reference, Output Amp, Single Supply, DIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "8bit DAC Reference Single Supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
		(symbol "AD558JN_0_1")
		(symbol "AD558JN_1_1"
			(pin input line
				(at -12.7 12.7 0)
				(length 3.81)
				(name "DB0")
				(number "1")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 3.81)
				(name "DB1")
				(number "2")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 3.81)
				(name "DB2")
				(number "3")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 3.81)
				(name "DB3")
				(number "4")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 3.81)
				(name "DB4")
				(number "5")
			)
			(pin input line
				(at -12.7 0 0)
				(length 3.81)
				(name "DB5")
				(number "6")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 3.81)
				(name "DB6")
				(number "7")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 3.81)
				(name "DB7")
				(number "8")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 3.81)
				(name "~{CE}")
				(number "9")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 3.81)
				(name "~{CS}")
				(number "10")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "V+")
				(number "11")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "DGND")
				(number "12")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 3.81)
				(name "VOUT")
				(number "16")
			)
			(pin input line
				(at 12.7 0 180)
				(length 3.81)
				(name "VSEN")
				(number "15")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 3.81)
				(name "VSEL")
				(number "14")
			)
			(pin power_in line
				(at 12.7 -12.7 180)
				(length 3.81)
				(name "AGND")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD558JP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 17.78 0)
		)
		(property "Value" "AD558JP"
			(at 2.54 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/AD558.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single 8-bit DAC, Internal Reference, Output Amp, Single Supply, PLCC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "8bit DAC Reference Single Supply"
			(at 0 0 0)
		)
		(symbol "AD558JP_0_1")
		(symbol "AD558JP_1_1"
			(pin input line
				(at -12.7 12.7 0)
				(length 3.81)
				(name "DB0")
				(number "2")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 3.81)
				(name "DB1")
				(number "3")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 3.81)
				(name "DB2")
				(number "4")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 3.81)
				(name "DB3")
				(number "5")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 3.81)
				(name "DB4")
				(number "7")
			)
			(pin input line
				(at -12.7 0 0)
				(length 3.81)
				(name "DB5")
				(number "8")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 3.81)
				(name "DB6")
				(number "9")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 3.81)
				(name "DB7")
				(number "10")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 3.81)
				(name "~{CE}")
				(number "12")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 3.81)
				(name "~{CS}")
				(number "13")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "V+")
				(number "14")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "DGND")
				(number "15")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 3.81)
				(name "VOUT")
				(number "20")
			)
			(pin input line
				(at 12.7 0 180)
				(length 3.81)
				(name "VSEN")
				(number "19")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 3.81)
				(name "VSEL")
				(number "18")
			)
			(pin power_in line
				(at 12.7 -12.7 180)
				(length 3.81)
				(name "AGND")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD5687BCPZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.89 11.43 0)
		)
		(property "Value" "AD5687BCPZ"
			(at 8.89 8.89 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-16-1EP_3x3mm_P0.5mm_EP1.854x1.854mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD5689_5687.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual, 12-Bit nanoDAC+ with SPI Interface, LFCSP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "dac 2nch 12bit spi"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AD5687BCPZ_0_1")
		(symbol "AD5687BCPZ_1_1"
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "SCLK")
				(number "10")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "SDIN")
				(number "12")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "~{SYNC}")
				(number "11")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{LDAC}")
				(number "7")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{RESET}")
				(number "13")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "GAIN")
				(number "8")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "RSTSEL")
				(number "14")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VLOGIC")
				(number "9")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin passive line
				(at 2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 5.08 15.24 270)
				(length 2.54)
				(name "VREF")
				(number "15")
			)
			(pin no_connect line
				(at 7.62 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin no_connect line
				(at 7.62 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VOUTA")
				(number "1")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUTB")
				(number "5")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SDO")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD5687BRUZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.89 11.43 0)
		)
		(property "Value" "AD5687BRUZ"
			(at 8.89 8.89 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD5689_5687.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual, 12-Bit nanoDAC+ with SPI Interface, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "dac 2nch 12bit spi"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AD5687BRUZ_0_1")
		(symbol "AD5687BRUZ_1_1"
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "SCLK")
				(number "12")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "SDIN")
				(number "14")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "~{SYNC}")
				(number "13")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{LDAC}")
				(number "9")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{RESET}")
				(number "15")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "GAIN")
				(number "10")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "RSTSEL")
				(number "16")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VLOGIC")
				(number "11")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 5.08 15.24 270)
				(length 2.54)
				(name "VREF")
				(number "1")
			)
			(pin no_connect line
				(at 7.62 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at 7.62 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VOUTA")
				(number "3")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUTB")
				(number "7")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SDO")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD5691RxRM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "AD5691RxRM"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 33.02 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD5693R_5692R_5691R_5693.pdf"
			(at 8.89 6.35 0)
		)
		(property "Description" "Tiny, 12-Bit, I2C, nanoDAC+, 2 ppm/°C Reference, MSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "serial DAC i2c digital analog converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AD5691RxRM_0_1")
		(symbol "AD5691RxRM_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SCL")
				(number "7")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SDA")
				(number "8")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{RESET}")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{LDAC}")
				(number "4")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A0")
				(number "6")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VLOGIC")
				(number "2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "VOUT")
				(number "10")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "VREF")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD5697RBCPZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.89 11.43 0)
		)
		(property "Value" "AD5697RBCPZ"
			(at 8.89 8.89 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-16-1EP_3x3mm_P0.5mm_EP1.854x1.854mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD5697R.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual, 12-Bit nanoDAC+ with 2 ppm/°C Reference, I2C Interface, LFCSP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "dac 2nch 12bit i2c"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AD5697RBCPZ_0_1")
		(symbol "AD5697RBCPZ_1_1"
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "SCL")
				(number "11")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "SDA")
				(number "6")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "~{LDAC}")
				(number "7")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{RESET}")
				(number "13")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A1")
				(number "12")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A0")
				(number "10")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "GAIN")
				(number "8")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "RSTSEL")
				(number "14")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VLOGIC")
				(number "9")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin passive line
				(at 2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 5.08 15.24 270)
				(length 2.54)
				(name "VREF")
				(number "15")
			)
			(pin no_connect line
				(at 7.62 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin no_connect line
				(at 7.62 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VOUTA")
				(number "1")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUTB")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD5697RBRUZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.89 11.43 0)
		)
		(property "Value" "AD5697RBRUZ"
			(at 8.89 8.89 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD5697R.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual, 12-Bit nanoDAC+ with 2 ppm/°C Reference, I2C Interface, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "dac 2nch 12bit i2c"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AD5697RBRUZ_0_1")
		(symbol "AD5697RBRUZ_1_1"
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "SCL")
				(number "13")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "SDA")
				(number "8")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "~{LDAC}")
				(number "9")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{RESET}")
				(number "15")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A1")
				(number "14")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A0")
				(number "12")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "GAIN")
				(number "10")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "RSTSEL")
				(number "16")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VLOGIC")
				(number "11")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 5.08 15.24 270)
				(length 2.54)
				(name "VREF")
				(number "1")
			)
			(pin no_connect line
				(at 7.62 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at 7.62 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VOUTA")
				(number "3")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUTB")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD5781xRUZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 17.78 0)
		)
		(property "Value" "AD5781xRUZ"
			(at 10.16 17.78 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -2.54 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ad5781.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "18Bit, ±0,5 LSB INL, Voltage Output DAC, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "1ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4?6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AD5781xRUZ_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "~{SYNC}")
				(number "14")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SCLK")
				(number "13")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SDIN")
				(number "12")
			)
			(pin output line
				(at -12.7 0 0)
				(length 2.54)
				(name "SDO")
				(number "11")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{LDAC}")
				(number "8")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "~{CLR}")
				(number "7")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "~{RESET}")
				(number "6")
			)
			(pin power_in line
				(at -7.62 17.78 270)
				(length 2.54)
				(name "V_{CC}")
				(number "9")
			)
			(pin power_in line
				(at -7.62 -20.32 90)
				(length 2.54)
				(name "DGND")
				(number "15")
			)
			(pin power_in line
				(at -5.08 17.78 270)
				(length 2.54)
				(name "IOV_{CC}")
				(number "10")
			)
			(pin power_in line
				(at -5.08 -20.32 90)
				(length 2.54)
				(name "AGND")
				(number "19")
			)
			(pin input line
				(at 0 17.78 270)
				(length 2.54)
				(name "V_{REFPF}")
				(number "4")
			)
			(pin input line
				(at 0 -20.32 90)
				(length 2.54)
				(name "V_{REFNF}")
				(number "16")
			)
			(pin output line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "V_{REFPS}")
				(number "3")
			)
			(pin output line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "V_{REFNS}")
				(number "17")
			)
			(pin power_in line
				(at 7.62 17.78 270)
				(length 2.54)
				(name "V_{DD}")
				(number "5")
			)
			(pin power_in line
				(at 7.62 -20.32 90)
				(length 2.54)
				(name "V_{SS}")
				(number "18")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "R_{FB}")
				(number "20")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "INV")
				(number "1")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "V_{OUT}")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD7224KN"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 22.86 0)
		)
		(property "Value" "AD7224KN"
			(at 6.35 22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/AD7224.pdf"
			(at 0 0 0)
		)
		(property "Description" "8bit DAC, Dual or Single Supply, DIP-18"
			(at 0 0 0)
		)
		(property "ki_keywords" "8bit DAC Dual Single Supply 1ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
		(symbol "AD7224KN_1_1"
			(pin input line
				(at -17.78 17.78 0)
				(length 3.81)
				(name "DB0(LSB)")
				(number "13")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "DB1")
				(number "12")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "DB2")
				(number "11")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "DB3")
				(number "10")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "DB4")
				(number "9")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "DB5")
				(number "8")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "DB6")
				(number "7")
			)
			(pin input line
				(at -17.78 0 0)
				(length 3.81)
				(name "DB7(MSB)")
				(number "6")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "~{CS}")
				(number "14")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "~{WR}")
				(number "15")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 3.81)
				(name "~{LDAC}")
				(number "16")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 3.81)
				(name "~{RST}")
				(number "17")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 3.81)
				(name "VDD")
				(number "18")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "DGND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 3.81)
				(name "VSS")
				(number "1")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "VOUT")
				(number "2")
			)
			(pin passive line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "VREF")
				(number "3")
			)
			(pin passive line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "AGND")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD7224KP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 22.86 0)
		)
		(property "Value" "AD7224KP"
			(at 5.08 22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/AD7224.pdf"
			(at 0 0 0)
		)
		(property "Description" "8bit DAC, Dual or Single Supply, PLCC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "8bit DAC Dual Single Supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PLCC*"
			(at 0 0 0)
		)
		(symbol "AD7224KP_1_1"
			(pin input line
				(at -17.78 17.78 0)
				(length 3.81)
				(name "DB0(LSB)")
				(number "15")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "DB1")
				(number "14")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "DB2")
				(number "13")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "DB3")
				(number "12")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "DB4")
				(number "10")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "DB5")
				(number "9")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "DB6")
				(number "8")
			)
			(pin input line
				(at -17.78 0 0)
				(length 3.81)
				(name "DB7(MSB)")
				(number "7")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "~{CS}")
				(number "16")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "~{WR}")
				(number "17")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 3.81)
				(name "~{LDAC}")
				(number "18")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 3.81)
				(name "~{RST}")
				(number "19")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 3.81)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "DGND")
				(number "6")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 3.81)
				(name "VSS")
				(number "2")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "VOUT")
				(number "3")
			)
			(pin passive line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "VREF")
				(number "4")
			)
			(pin passive line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "AGND")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD7224KR-1"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 22.86 0)
		)
		(property "Value" "AD7224KR-1"
			(at 5.08 22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/AD7224.pdf"
			(at 0 0 0)
		)
		(property "Description" "8bit DAC, Dual or Single Supply, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "8bit DAC Dual Single Supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*"
			(at 0 0 0)
		)
		(symbol "AD7224KR-1_1_1"
			(pin input line
				(at -17.78 17.78 0)
				(length 3.81)
				(name "DB0(LSB)")
				(number "15")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "DB1")
				(number "14")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "DB2")
				(number "13")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "DB3")
				(number "12")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "DB4")
				(number "9")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "DB5")
				(number "8")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "DB6")
				(number "7")
			)
			(pin input line
				(at -17.78 0 0)
				(length 3.81)
				(name "DB7(MSB)")
				(number "6")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "~{CS}")
				(number "16")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "~{WR}")
				(number "17")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 3.81)
				(name "~{LDAC}")
				(number "18")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 3.81)
				(name "~{RST}")
				(number "19")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 3.81)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "DGND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 3.81)
				(name "VSS")
				(number "1")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "VOUT")
				(number "2")
			)
			(pin passive line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "VREF")
				(number "3")
			)
			(pin passive line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "AGND")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD7224KR-18"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 22.86 0)
		)
		(property "Value" "AD7224KR-18"
			(at 5.08 22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/AD7224.pdf"
			(at 0 0 0)
		)
		(property "Description" "8bit DAC, Dual or Single Supply, SOIC-18"
			(at 0 0 0)
		)
		(property "ki_keywords" "8bit DAC Dual Single Supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*"
			(at 0 0 0)
		)
		(symbol "AD7224KR-18_1_1"
			(pin input line
				(at -17.78 17.78 0)
				(length 3.81)
				(name "DB0(LSB)")
				(number "13")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "DB1")
				(number "12")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "DB2")
				(number "11")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "DB3")
				(number "10")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "DB4")
				(number "9")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "DB5")
				(number "8")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "DB6")
				(number "7")
			)
			(pin input line
				(at -17.78 0 0)
				(length 3.81)
				(name "DB7(MSB)")
				(number "6")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "~{CS}")
				(number "14")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "~{WR}")
				(number "15")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 3.81)
				(name "~{LDAC}")
				(number "16")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 3.81)
				(name "~{RST}")
				(number "17")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 3.81)
				(name "VDD")
				(number "18")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "DGND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 3.81)
				(name "VSS")
				(number "1")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "VOUT")
				(number "2")
			)
			(pin passive line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "VREF")
				(number "3")
			)
			(pin passive line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "AGND")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD7225BRS"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 22.86 0)
		)
		(property "Value" "AD7225BRS"
			(at 7.62 22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/AD7225.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "Quad 8bit DAC, Separate Reference Voltage, SSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "8bit DAC 4CH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*"
			(at 0 0 0)
		)
		(symbol "AD7225BRS_0_1")
		(symbol "AD7225BRS_1_1"
			(pin input line
				(at -17.78 17.78 0)
				(length 3.81)
				(name "DB0")
				(number "16")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "DB1")
				(number "15")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "DB2")
				(number "14")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "DB3")
				(number "13")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "DB4")
				(number "12")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "DB5")
				(number "11")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "DB6")
				(number "10")
			)
			(pin input line
				(at -17.78 0 0)
				(length 3.81)
				(name "DB7")
				(number "9")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "~{WR}")
				(number "17")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "~{LDAC}")
				(number "8")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 3.81)
				(name "A0")
				(number "19")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 3.81)
				(name "A1")
				(number "18")
			)
			(pin power_in line
				(at -5.08 25.4 270)
				(length 3.81)
				(name "VDD")
				(number "22")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at 5.08 25.4 270)
				(length 3.81)
				(name "VSS")
				(number "3")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "VOUTA")
				(number "2")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "VOUTB")
				(number "1")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "VOUTC")
				(number "24")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "VOUTD")
				(number "23")
			)
			(pin input line
				(at 17.78 0 180)
				(length 3.81)
				(name "VREFA")
				(number "5")
			)
			(pin input line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "VREFB")
				(number "4")
			)
			(pin input line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "VREFC")
				(number "21")
			)
			(pin input line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "VREFD")
				(number "20")
			)
			(pin input line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "AGND")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD7225KN"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 22.86 0)
		)
		(property "Value" "AD7225KN"
			(at 7.62 22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/AD7225.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "Quad 8bit DAC, Separate Reference Voltage, PDIP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "8bit DAC 4CH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
		(symbol "AD7225KN_0_1")
		(symbol "AD7225KN_1_1"
			(pin input line
				(at -17.78 17.78 0)
				(length 3.81)
				(name "DB0")
				(number "16")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "DB1")
				(number "15")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "DB2")
				(number "14")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "DB3")
				(number "13")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "DB4")
				(number "12")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "DB5")
				(number "11")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "DB6")
				(number "10")
			)
			(pin input line
				(at -17.78 0 0)
				(length 3.81)
				(name "DB7")
				(number "9")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "~{WR}")
				(number "17")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "~{LDAC}")
				(number "8")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 3.81)
				(name "A0")
				(number "19")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 3.81)
				(name "A1")
				(number "18")
			)
			(pin power_in line
				(at -5.08 25.4 270)
				(length 3.81)
				(name "VDD")
				(number "22")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at 5.08 25.4 270)
				(length 3.81)
				(name "VSS")
				(number "3")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "VOUTA")
				(number "2")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "VOUTB")
				(number "1")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "VOUTC")
				(number "24")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "VOUTD")
				(number "23")
			)
			(pin input line
				(at 17.78 0 180)
				(length 3.81)
				(name "VREFA")
				(number "5")
			)
			(pin input line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "VREFB")
				(number "4")
			)
			(pin input line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "VREFC")
				(number "21")
			)
			(pin input line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "VREFD")
				(number "20")
			)
			(pin input line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "AGND")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD7225KP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 22.86 0)
		)
		(property "Value" "AD7225KP"
			(at 7.62 22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/AD7225.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "Quad 8bit DAC, Separate Reference Voltage, PLCC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "8bit DAC 4CH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PLCC*"
			(at 0 0 0)
		)
		(symbol "AD7225KP_0_1")
		(symbol "AD7225KP_1_1"
			(pin input line
				(at -17.78 17.78 0)
				(length 3.81)
				(name "DB0")
				(number "19")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "DB1")
				(number "18")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "DB2")
				(number "17")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "DB3")
				(number "16")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "DB4")
				(number "14")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "DB5")
				(number "13")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "DB6")
				(number "12")
			)
			(pin input line
				(at -17.78 0 0)
				(length 3.81)
				(name "DB7")
				(number "11")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "~{WR}")
				(number "20")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "~{LDAC}")
				(number "10")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 3.81)
				(name "A0")
				(number "21")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 3.81)
				(name "A1")
				(number "23")
			)
			(pin power_in line
				(at -5.08 25.4 270)
				(length 3.81)
				(name "VDD")
				(number "26")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at 5.08 25.4 270)
				(length 3.81)
				(name "VSS")
				(number "4")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "VOUTA")
				(number "3")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "VOUTB")
				(number "2")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "VOUTC")
				(number "28")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "VOUTD")
				(number "27")
			)
			(pin input line
				(at 17.78 0 180)
				(length 3.81)
				(name "VREFA")
				(number "6")
			)
			(pin input line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "VREFB")
				(number "5")
			)
			(pin input line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "VREFC")
				(number "25")
			)
			(pin input line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "VREFD")
				(number "24")
			)
			(pin input line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "AGND")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD7225KR"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 22.86 0)
		)
		(property "Value" "AD7225KR"
			(at 7.62 22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/AD7225.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "Quad 8bit DAC, Separate Reference Voltage, SOIC-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "8bit DAC 4CH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*"
			(at 0 0 0)
		)
		(symbol "AD7225KR_0_1")
		(symbol "AD7225KR_1_1"
			(pin input line
				(at -17.78 17.78 0)
				(length 3.81)
				(name "DB0")
				(number "16")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "DB1")
				(number "15")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "DB2")
				(number "14")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "DB3")
				(number "13")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "DB4")
				(number "12")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "DB5")
				(number "11")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "DB6")
				(number "10")
			)
			(pin input line
				(at -17.78 0 0)
				(length 3.81)
				(name "DB7")
				(number "9")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "~{WR}")
				(number "17")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "~{LDAC}")
				(number "8")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 3.81)
				(name "A0")
				(number "19")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 3.81)
				(name "A1")
				(number "18")
			)
			(pin power_in line
				(at -5.08 25.4 270)
				(length 3.81)
				(name "VDD")
				(number "22")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at 5.08 25.4 270)
				(length 3.81)
				(name "VSS")
				(number "3")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "VOUTA")
				(number "2")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "VOUTB")
				(number "1")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "VOUTC")
				(number "24")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "VOUTD")
				(number "23")
			)
			(pin input line
				(at 17.78 0 180)
				(length 3.81)
				(name "VREFA")
				(number "5")
			)
			(pin input line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "VREFB")
				(number "4")
			)
			(pin input line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "VREFC")
				(number "21")
			)
			(pin input line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "VREFD")
				(number "20")
			)
			(pin input line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "AGND")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD7226BRSZ"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 22.86 0)
		)
		(property "Value" "AD7226BRSZ"
			(at 7.62 22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/AD7226.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad 8bit DAC, 4 Channel, Single Reference Voltage, SSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "4CH DAC 8bit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*"
			(at 0 0 0)
		)
		(symbol "AD7226BRSZ_0_1")
		(symbol "AD7226BRSZ_1_1"
			(pin input line
				(at -17.78 17.78 0)
				(length 3.81)
				(name "DB0")
				(number "14")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "DB1")
				(number "13")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "DB2")
				(number "12")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "DB3")
				(number "11")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "DB4")
				(number "10")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "DB5")
				(number "9")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "DB6")
				(number "8")
			)
			(pin input line
				(at -17.78 0 0)
				(length 3.81)
				(name "DB7")
				(number "7")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "~{WR}")
				(number "15")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 3.81)
				(name "A0")
				(number "17")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 3.81)
				(name "A1")
				(number "16")
			)
			(pin power_in line
				(at -5.08 25.4 270)
				(length 3.81)
				(name "VDD")
				(number "18")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 5.08 25.4 270)
				(length 3.81)
				(name "VSS")
				(number "3")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "VOUTA")
				(number "2")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "VOUTB")
				(number "1")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "VOUTC")
				(number "20")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "VOUTD")
				(number "19")
			)
			(pin input line
				(at 17.78 0 180)
				(length 3.81)
				(name "VREF")
				(number "4")
			)
			(pin input line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "AGND")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD7226KN"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 22.86 0)
		)
		(property "Value" "AD7226KN"
			(at 7.62 22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/AD7226.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad 8bit DAC, 4 Channel, Single Reference Voltage, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "4CH DAC 8bit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
		(symbol "AD7226KN_0_1")
		(symbol "AD7226KN_1_1"
			(pin input line
				(at -17.78 17.78 0)
				(length 3.81)
				(name "DB0")
				(number "14")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "DB1")
				(number "13")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "DB2")
				(number "12")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "DB3")
				(number "11")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "DB4")
				(number "10")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "DB5")
				(number "9")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "DB6")
				(number "8")
			)
			(pin input line
				(at -17.78 0 0)
				(length 3.81)
				(name "DB7")
				(number "7")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "~{WR}")
				(number "15")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 3.81)
				(name "A0")
				(number "17")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 3.81)
				(name "A1")
				(number "16")
			)
			(pin power_in line
				(at -5.08 25.4 270)
				(length 3.81)
				(name "VDD")
				(number "18")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 5.08 25.4 270)
				(length 3.81)
				(name "VSS")
				(number "3")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "VOUTA")
				(number "2")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "VOUTB")
				(number "1")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "VOUTC")
				(number "20")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "VOUTD")
				(number "19")
			)
			(pin input line
				(at 17.78 0 180)
				(length 3.81)
				(name "VREF")
				(number "4")
			)
			(pin input line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "AGND")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD7226KP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 22.86 0)
		)
		(property "Value" "AD7226KP"
			(at 7.62 22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/AD7226.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad 8bit DAC, 4 Channel, Single Reference Voltage, PLCC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "4CH DAC 8bit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PLCC*"
			(at 0 0 0)
		)
		(symbol "AD7226KP_0_1")
		(symbol "AD7226KP_1_1"
			(pin input line
				(at -17.78 17.78 0)
				(length 3.81)
				(name "DB0")
				(number "14")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "DB1")
				(number "13")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "DB2")
				(number "12")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "DB3")
				(number "11")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "DB4")
				(number "10")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "DB5")
				(number "9")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "DB6")
				(number "8")
			)
			(pin input line
				(at -17.78 0 0)
				(length 3.81)
				(name "DB7")
				(number "7")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "~{WR}")
				(number "15")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 3.81)
				(name "A0")
				(number "17")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 3.81)
				(name "A1")
				(number "16")
			)
			(pin power_in line
				(at -5.08 25.4 270)
				(length 3.81)
				(name "VDD")
				(number "18")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 5.08 25.4 270)
				(length 3.81)
				(name "VSS")
				(number "3")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "VOUTA")
				(number "2")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "VOUTB")
				(number "1")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "VOUTC")
				(number "20")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "VOUTD")
				(number "19")
			)
			(pin input line
				(at 17.78 0 180)
				(length 3.81)
				(name "VREF")
				(number "4")
			)
			(pin input line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "AGND")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD7226KR"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 22.86 0)
		)
		(property "Value" "AD7226KR"
			(at 7.62 22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/AD7226.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad 8bit DAC, 4 Channel, Single Reference Voltage, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "4CH DAC 8bit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*"
			(at 0 0 0)
		)
		(symbol "AD7226KR_0_1")
		(symbol "AD7226KR_1_1"
			(pin input line
				(at -17.78 17.78 0)
				(length 3.81)
				(name "DB0")
				(number "14")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "DB1")
				(number "13")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "DB2")
				(number "12")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "DB3")
				(number "11")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "DB4")
				(number "10")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "DB5")
				(number "9")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "DB6")
				(number "8")
			)
			(pin input line
				(at -17.78 0 0)
				(length 3.81)
				(name "DB7")
				(number "7")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "~{WR}")
				(number "15")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 3.81)
				(name "A0")
				(number "17")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 3.81)
				(name "A1")
				(number "16")
			)
			(pin power_in line
				(at -5.08 25.4 270)
				(length 3.81)
				(name "VDD")
				(number "18")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 5.08 25.4 270)
				(length 3.81)
				(name "VSS")
				(number "3")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "VOUTA")
				(number "2")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "VOUTB")
				(number "1")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "VOUTC")
				(number "20")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "VOUTD")
				(number "19")
			)
			(pin input line
				(at 17.78 0 180)
				(length 3.81)
				(name "VREF")
				(number "4")
			)
			(pin input line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "AGND")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD7228ABN"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 22.86 0)
		)
		(property "Value" "AD7228ABN"
			(at 7.62 22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/AD7228.pdf"
			(at 0 0 0)
		)
		(property "Description" "8bit DAC 8 Channel, Single Reference, DIP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "8bit DAC 8CH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PDIP* DIP*"
			(at 0 0 0)
		)
		(symbol "AD7228ABN_0_1")
		(symbol "AD7228ABN_1_1"
			(pin input line
				(at -17.78 17.78 0)
				(length 3.81)
				(name "DB0")
				(number "20")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "DB1")
				(number "19")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "DB2")
				(number "18")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "DB3")
				(number "17")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "DB4")
				(number "16")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "DB5")
				(number "15")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "DB6")
				(number "14")
			)
			(pin input line
				(at -17.78 0 0)
				(length 3.81)
				(name "DB7")
				(number "13")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "~{WR}")
				(number "21")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 3.81)
				(name "A0")
				(number "24")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 3.81)
				(name "A1")
				(number "23")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 3.81)
				(name "A2")
				(number "22")
			)
			(pin power_in line
				(at -5.08 25.4 270)
				(length 3.81)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "GND")
				(number "12")
			)
			(pin power_in line
				(at 5.08 25.4 270)
				(length 3.81)
				(name "VSS")
				(number "10")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 3.81)
				(name "VOUT1")
				(number "9")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "VOUT2")
				(number "8")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "VOUT3")
				(number "7")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "VOUT4")
				(number "6")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "VOUT5")
				(number "5")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "VOUT6")
				(number "4")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "VOUT7")
				(number "3")
			)
			(pin output line
				(at 17.78 0 180)
				(length 3.81)
				(name "VOUT8")
				(number "2")
			)
			(pin passive line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "VREF")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD7228ABP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 22.86 0)
		)
		(property "Value" "AD7228ABP"
			(at 7.62 22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/AD7228.pdf"
			(at 0 0 0)
		)
		(property "Description" "8bit DAC 8 Channel, Single Reference, PLCC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "8bit DAC 8CH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PLCC*"
			(at 0 0 0)
		)
		(symbol "AD7228ABP_0_1")
		(symbol "AD7228ABP_1_1"
			(pin input line
				(at -17.78 17.78 0)
				(length 3.81)
				(name "DB0")
				(number "24")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "DB1")
				(number "23")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "DB2")
				(number "21")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "DB3")
				(number "20")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "DB4")
				(number "19")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "DB5")
				(number "18")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "DB6")
				(number "17")
			)
			(pin input line
				(at -17.78 0 0)
				(length 3.81)
				(name "DB7")
				(number "16")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "~{WR}")
				(number "25")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 3.81)
				(name "A0")
				(number "28")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 3.81)
				(name "A1")
				(number "27")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 3.81)
				(name "A2")
				(number "26")
			)
			(pin power_in line
				(at -5.08 25.4 270)
				(length 3.81)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "GND")
				(number "14")
			)
			(pin power_in line
				(at 5.08 25.4 270)
				(length 3.81)
				(name "VSS")
				(number "12")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 3.81)
				(name "VOUT1")
				(number "11")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "VOUT2")
				(number "10")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "VOUT3")
				(number "9")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "VOUT4")
				(number "7")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "VOUT5")
				(number "6")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "VOUT6")
				(number "5")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "VOUT7")
				(number "4")
			)
			(pin output line
				(at 17.78 0 180)
				(length 3.81)
				(name "VOUT8")
				(number "3")
			)
			(pin passive line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "VREF")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD7228ABR"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 22.86 0)
		)
		(property "Value" "AD7228ABR"
			(at 7.62 22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/AD7228.pdf"
			(at 0 0 0)
		)
		(property "Description" "8bit DAC 8 Channel, Single Reference, SOIC-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "8bit DAC 8CH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*"
			(at 0 0 0)
		)
		(symbol "AD7228ABR_0_1")
		(symbol "AD7228ABR_1_1"
			(pin input line
				(at -17.78 17.78 0)
				(length 3.81)
				(name "DB0")
				(number "20")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "DB1")
				(number "19")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "DB2")
				(number "18")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "DB3")
				(number "17")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "DB4")
				(number "16")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "DB5")
				(number "15")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "DB6")
				(number "14")
			)
			(pin input line
				(at -17.78 0 0)
				(length 3.81)
				(name "DB7")
				(number "13")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "~{WR}")
				(number "21")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 3.81)
				(name "A0")
				(number "24")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 3.81)
				(name "A1")
				(number "23")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 3.81)
				(name "A2")
				(number "22")
			)
			(pin power_in line
				(at -5.08 25.4 270)
				(length 3.81)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "GND")
				(number "12")
			)
			(pin power_in line
				(at 5.08 25.4 270)
				(length 3.81)
				(name "VSS")
				(number "10")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 3.81)
				(name "VOUT1")
				(number "9")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "VOUT2")
				(number "8")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "VOUT3")
				(number "7")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "VOUT4")
				(number "6")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "VOUT5")
				(number "5")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "VOUT6")
				(number "4")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "VOUT7")
				(number "3")
			)
			(pin output line
				(at 17.78 0 180)
				(length 3.81)
				(name "VOUT8")
				(number "2")
			)
			(pin passive line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "VREF")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD7304"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 13.97 0)
		)
		(property "Value" "AD7304"
			(at 2.54 13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD7304_7305.pdf"
			(at 0 0 0)
		)
		(property "Description" "3V/5V, Rail-to-Rail, Quad, 8-Bit DAC, SPI Interface, SOIC-16/TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "dac 4ch 8bit spi"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*W*7.5x10.3mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AD7304_0_1")
		(symbol "AD7304_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "CLK")
				(number "10")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SDI/SHDN")
				(number "11")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{CS}")
				(number "9")
			)
			(pin output line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{LDAC}")
				(number "7")
			)
			(pin output line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{CLR}")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "VSS")
				(number "3")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "VOUTA")
				(number "2")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "VOUTB")
				(number "1")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "VOUTC")
				(number "16")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "VOUTD")
				(number "15")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "VREFA")
				(number "4")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "VREFB")
				(number "5")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "VREFC")
				(number "12")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "VREFD")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD7305"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 16.51 0)
		)
		(property "Value" "AD7305"
			(at 3.81 16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD7304_7305.pdf"
			(at 0 0 0)
		)
		(property "Description" "3V/5V, Rail-to-Rail, Quad, 8-Bit DAC, Parallel Interface, SOIC-20/TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "dac 4ch 8bit parallel"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*W*7.5x12.8mm*P1.27mm* TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AD7305_0_1")
		(symbol "AD7305_1_1"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "DB7")
				(number "7")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "DB6")
				(number "8")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "DB5")
				(number "9")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "DB4")
				(number "10")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "DB3")
				(number "11")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "DB2")
				(number "12")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "DB1")
				(number "13")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "DB0")
				(number "14")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "~{LDAC}")
				(number "6")
			)
			(pin output line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "~{WR}")
				(number "15")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "18")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VSS")
				(number "3")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "VOUTA")
				(number "2")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "VOUTB")
				(number "1")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "VOUTC")
				(number "20")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "VOUTD")
				(number "19")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "VREF")
				(number "4")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "A0/SHDN")
				(number "17")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "A1")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD7390"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 10.795 0)
		)
		(property "Value" "AD7390"
			(at 1.27 8.89 0)
		)
		(property "Footprint" ""
			(at 22.86 -2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD7390_7391.pdf"
			(at 22.86 -2.54 0)
		)
		(property "Description" "Serial-Input Micropower 12-Bit DAC, DIP-8/SOIC-8/TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SPI 12 bit DAC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm* TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AD7390_0_0")
		(symbol "AD7390_1_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "~{LD}")
				(number "1")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "CLK")
				(number "2")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SDI")
				(number "3")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{CLR}")
				(number "4")
			)
			(pin input line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "Vref")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "Vdd")
				(number "7")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "Vss")
				(number "5")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "Vout")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD7533JN"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 17.78 0)
		)
		(property "Value" "AD7533JN"
			(at 3.81 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/AD7533.pdf"
			(at 0 0 0)
		)
		(property "Description" "10bit Multiplying DAC, 1 Channel, DIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "10bit DAC 1CH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
		(symbol "AD7533JN_0_1")
		(symbol "AD7533JN_1_1"
			(pin input line
				(at -15.24 12.7 0)
				(length 3.81)
				(name "D0(LSB)")
				(number "13")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 3.81)
				(name "D1")
				(number "12")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "D2")
				(number "11")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "D3")
				(number "10")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "D4")
				(number "9")
			)
			(pin input line
				(at -15.24 0 0)
				(length 3.81)
				(name "D5")
				(number "8")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "D6")
				(number "7")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 3.81)
				(name "D7")
				(number "6")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 3.81)
				(name "D8")
				(number "5")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 3.81)
				(name "D9(MSB)")
				(number "4")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 15.24 12.7 180)
				(length 3.81)
				(name "RFBACK")
				(number "16")
			)
			(pin passive line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "I_OUT1")
				(number "1")
			)
			(pin passive line
				(at 15.24 -2.54 180)
				(length 3.81)
				(name "I_OUT2")
				(number "2")
			)
			(pin passive line
				(at 15.24 -10.16 180)
				(length 3.81)
				(name "VREF")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD7533JP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 17.78 0)
		)
		(property "Value" "AD7533JP"
			(at 3.81 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/AD7533.pdf"
			(at 0 0 0)
		)
		(property "Description" "10bit Multiplying DAC, 1 Channel, PLCC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "10bit DAC 1CH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PLCC*"
			(at 0 0 0)
		)
		(symbol "AD7533JP_0_1")
		(symbol "AD7533JP_1_1"
			(pin input line
				(at -15.24 12.7 0)
				(length 3.81)
				(name "D0(LSB)")
				(number "17")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 3.81)
				(name "D1")
				(number "15")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "D2")
				(number "14")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "D3")
				(number "13")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "D4")
				(number "12")
			)
			(pin input line
				(at -15.24 0 0)
				(length 3.81)
				(name "D5")
				(number "10")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "D6")
				(number "9")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 3.81)
				(name "D7")
				(number "8")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 3.81)
				(name "D8")
				(number "7")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 3.81)
				(name "D9(MSB)")
				(number "5")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "VDD")
				(number "18")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 15.24 12.7 180)
				(length 3.81)
				(name "RFBACK")
				(number "20")
			)
			(pin passive line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "I_OUT1")
				(number "2")
			)
			(pin passive line
				(at 15.24 -2.54 180)
				(length 3.81)
				(name "I_OUT2")
				(number "3")
			)
			(pin passive line
				(at 15.24 -12.7 180)
				(length 3.81)
				(name "VREF")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD7533KR"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 17.78 0)
		)
		(property "Value" "AD7533KR"
			(at 3.81 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/AD7533.pdf"
			(at 0 0 0)
		)
		(property "Description" "10bit Multiplying DAC, 1 Channel, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "10bit DAC 1CH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
		(symbol "AD7533KR_0_1")
		(symbol "AD7533KR_1_1"
			(pin input line
				(at -15.24 12.7 0)
				(length 3.81)
				(name "D0(LSB)")
				(number "13")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 3.81)
				(name "D1")
				(number "12")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "D2")
				(number "11")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "D3")
				(number "10")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "D4")
				(number "9")
			)
			(pin input line
				(at -15.24 0 0)
				(length 3.81)
				(name "D5")
				(number "8")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "D6")
				(number "7")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 3.81)
				(name "D7")
				(number "6")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 3.81)
				(name "D8")
				(number "5")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 3.81)
				(name "D9(MSB)")
				(number "4")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 15.24 12.7 180)
				(length 3.81)
				(name "RFBACK")
				(number "16")
			)
			(pin passive line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "I_OUT1")
				(number "1")
			)
			(pin passive line
				(at 15.24 -2.54 180)
				(length 3.81)
				(name "I_OUT2")
				(number "2")
			)
			(pin passive line
				(at 15.24 -10.16 180)
				(length 3.81)
				(name "VREF")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD775"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 17.78 0)
		)
		(property "Value" "AD775"
			(at 8.89 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD775.pdf"
			(at 0 0 0)
		)
		(property "Description" "DA Converter 8 bits - 20MHz, PDIP/SOIC-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "DAC CNA"
			(at 0 0 0)
		)
		(symbol "AD775_0_1")
		(symbol "AD775_1_1"
			(pin input line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "VIN")
				(number "19")
			)
			(pin input line
				(at -17.78 0 0)
				(length 3.81)
				(name "VRTS")
				(number "16")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "VRT")
				(number "17")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 3.81)
				(name "VRB")
				(number "23")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 3.81)
				(name "VRBS")
				(number "22")
			)
			(pin power_in line
				(at -7.62 20.32 270)
				(length 3.81)
				(name "AVDD")
				(number "14")
			)
			(pin power_in line
				(at -5.08 20.32 270)
				(length 3.81)
				(name "AVDD")
				(number "15")
			)
			(pin power_in line
				(at -5.08 -20.32 90)
				(length 3.81)
				(name "AGND")
				(number "20")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 3.81)
				(name "AVDD")
				(number "18")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 3.81)
				(name "AGND")
				(number "21")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 3.81)
				(name "DVDD")
				(number "11")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 3.81)
				(name "DGND")
				(number "2")
			)
			(pin power_in line
				(at 5.08 20.32 270)
				(length 3.81)
				(name "DVDD")
				(number "13")
			)
			(pin power_in line
				(at 5.08 -20.32 90)
				(length 3.81)
				(name "DGND")
				(number "24")
			)
			(pin tri_state line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "D0")
				(number "3")
			)
			(pin tri_state line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "D1")
				(number "4")
			)
			(pin tri_state line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "D2")
				(number "5")
			)
			(pin tri_state line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "D3")
				(number "6")
			)
			(pin tri_state line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "D4")
				(number "7")
			)
			(pin tri_state line
				(at 17.78 0 180)
				(length 3.81)
				(name "D5")
				(number "8")
			)
			(pin tri_state line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "D6")
				(number "9")
			)
			(pin tri_state line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "D7")
				(number "10")
			)
			(pin input line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "~{OE}")
				(number "1")
			)
			(pin input clock
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "CLK")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD9106BCP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 29.21 0)
		)
		(property "Value" "AD9106BCP"
			(at 11.43 29.21 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-32-1EP_5x5mm_P0.5mm_EP3.6x3.6mm"
			(at 0 3.81 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ad9106.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "Analog Devices Quad, Low Power, 12-Bit, 180 MSPS, Digital-to-Analog Converter and Waveform Generator"
			(at 0 0 0)
		)
		(property "ki_keywords" "analog devices DAC DDS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*LFCSP*1EP*5x5mm*P0.5mm*EP3.6x3.6mm*"
			(at 0 0 0)
		)
		(symbol "AD9106BCP_0_0"
			(text "DAC"
				(at 1.778 16.51 0)
			)
			(text "DAC"
				(at 1.778 8.89 0)
			)
			(text "DAC"
				(at 1.778 1.27 0)
			)
			(text "DAC"
				(at 1.778 -6.35 0)
			)
		)
		(symbol "AD9106BCP_0_1")
		(symbol "AD9106BCP_1_1"
			(pin input line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "~{RESET}")
				(number "9")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "~{CS}")
				(number "8")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "SCLK")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "SDIO")
				(number "2")
			)
			(pin output line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "SDO")
				(number "7")
				(alternate "DOUT" output line)
				(alternate "SDI2" input line)
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "~{TRIGGER}")
				(number "32")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "CLKP")
				(number "21")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "CLKN")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "CLDO")
				(number "22")
			)
			(pin power_out line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "DLDO1")
				(number "6")
			)
			(pin power_out line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "DLDO2")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "REFIO")
				(number "18")
			)
			(pin power_in line
				(at -5.08 30.48 270)
				(length 2.54)
				(name "DVDD")
				(number "5")
			)
			(pin power_in line
				(at -5.08 -30.48 90)
				(length 2.54)
				(name "DGND")
				(number "3")
			)
			(pin passive line
				(at -5.08 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "DGND")
				(number "33")
			)
			(pin power_in line
				(at -2.54 30.48 270)
				(length 2.54)
				(name "CLKVDD")
				(number "23")
			)
			(pin power_in line
				(at -2.54 -30.48 90)
				(length 2.54)
				(name "CLKGND")
				(number "19")
			)
			(pin power_in line
				(at 2.54 30.48 270)
				(length 2.54)
				(name "AVDD1")
				(number "29")
			)
			(pin power_in line
				(at 5.08 30.48 270)
				(length 2.54)
				(name "AVDD2")
				(number "12")
			)
			(pin power_in line
				(at 5.08 -30.48 90)
				(length 2.54)
				(name "AGND")
				(number "15")
			)
			(pin passive line
				(at 5.08 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "26")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "IOUTP1")
				(number "27")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "IOUTN1")
				(number "28")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "IOUTP2")
				(number "31")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "IOUTN2")
				(number "30")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "IOUTP3")
				(number "14")
			)
			(pin output line
				(at 17.78 0 180)
				(length 2.54)
				(name "IOUTN3")
				(number "13")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "IOUTP4")
				(number "10")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "IOUTN4")
				(number "11")
			)
			(pin output line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "FSADJ1")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "FSADJ2/CAL_SENSE")
				(number "24")
			)
			(pin output line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "FSADJ3")
				(number "16")
			)
			(pin output line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "FSADJ4")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD9142"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" "AD9142"
			(at -10.16 -59.69 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-72-1EP_10x10mm_P0.5mm_EP6.15x6.15mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD9142.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.6GSPS 16bit dual-channel DAC, LFCSP-72"
			(at 0 0 0)
		)
		(property "ki_keywords" "16bit DAC 2CH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*10x10mm*P0.5mm*EP6.15x6.15mm*"
			(at 0 0 0)
		)
		(symbol "AD9142_0_0"
			(text "IFC"
				(at -6.35 2.54 900)
			)
			(text "PLL"
				(at 1.27 -46.99 0)
			)
			(text "DAC"
				(at 2.54 34.29 0)
			)
			(text "DAC"
				(at 2.54 19.05 0)
			)
			(text "CTRL"
				(at 6.35 -20.32 900)
			)
		)
		(symbol "AD9142_0_1")
		(symbol "AD9142_1_1"
			(pin input line
				(at -17.78 53.34 0)
				(length 2.54)
				(name "FRAMEP")
				(number "8")
			)
			(pin input line
				(at -17.78 50.8 0)
				(length 2.54)
				(name "FRAMEN")
				(number "9")
			)
			(pin input line
				(at -17.78 45.72 0)
				(length 2.54)
				(name "D0P")
				(number "46")
			)
			(pin input line
				(at -17.78 43.18 0)
				(length 2.54)
				(name "D0N")
				(number "47")
			)
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "D1P")
				(number "44")
			)
			(pin input line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "D1N")
				(number "45")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "D2P")
				(number "41")
			)
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "D2N")
				(number "42")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "D3P")
				(number "39")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "D3N")
				(number "40")
			)
			(pin input line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "D4P")
				(number "37")
			)
			(pin input line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "D4N")
				(number "38")
			)
			(pin input line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "D5P")
				(number "34")
			)
			(pin input line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "D5N")
				(number "35")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "D6P")
				(number "32")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "D6N")
				(number "33")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "D7P")
				(number "30")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "D7N")
				(number "31")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "D8P")
				(number "26")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "D8N")
				(number "27")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "D9P")
				(number "24")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "D9N")
				(number "25")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "D10P")
				(number "22")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "D10N")
				(number "23")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "D11P")
				(number "20")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "D11N")
				(number "21")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "D12P")
				(number "17")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "D12N")
				(number "18")
			)
			(pin input line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "D13P")
				(number "15")
			)
			(pin input line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "D13N")
				(number "16")
			)
			(pin input line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "D14P")
				(number "13")
			)
			(pin input line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "D14N")
				(number "14")
			)
			(pin input line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "D15P")
				(number "10")
			)
			(pin input line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "D15N")
				(number "11")
			)
			(pin input line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "DCIP")
				(number "28")
			)
			(pin input line
				(at -17.78 -40.64 0)
				(length 2.54)
				(name "DCIN")
				(number "29")
			)
			(pin input line
				(at -17.78 -45.72 0)
				(length 2.54)
				(name "REFP/SYNCP")
				(number "2")
			)
			(pin input line
				(at -17.78 -48.26 0)
				(length 2.54)
				(name "REFN/SYNCN")
				(number "3")
			)
			(pin input line
				(at -17.78 -50.8 0)
				(length 2.54)
				(name "DACCLKP")
				(number "62")
			)
			(pin input line
				(at -17.78 -53.34 0)
				(length 2.54)
				(name "DACCLKN")
				(number "61")
			)
			(pin passive line
				(at -2.54 60.96 270)
				(length 2.54)
				(hide yes)
				(name "DVDD18")
				(number "12")
			)
			(pin passive line
				(at -2.54 60.96 270)
				(length 2.54)
				(hide yes)
				(name "DVDD18")
				(number "19")
			)
			(pin passive line
				(at -2.54 60.96 270)
				(length 2.54)
				(hide yes)
				(name "DVDD18")
				(number "36")
			)
			(pin passive line
				(at -2.54 60.96 270)
				(length 2.54)
				(hide yes)
				(name "DVDD18")
				(number "43")
			)
			(pin passive line
				(at -2.54 60.96 270)
				(length 2.54)
				(hide yes)
				(name "DVDD18")
				(number "48")
			)
			(pin passive line
				(at -2.54 60.96 270)
				(length 2.54)
				(hide yes)
				(name "DVDD18")
				(number "49")
			)
			(pin power_in line
				(at -2.54 60.96 270)
				(length 2.54)
				(name "DVDD18")
				(number "7")
			)
			(pin power_in line
				(at 0 60.96 270)
				(length 2.54)
				(name "CVDD18")
				(number "1")
			)
			(pin passive line
				(at 0 60.96 270)
				(length 2.54)
				(hide yes)
				(name "CVDD18")
				(number "4")
			)
			(pin passive line
				(at 0 60.96 270)
				(length 2.54)
				(hide yes)
				(name "CVDD18")
				(number "59")
			)
			(pin passive line
				(at 0 60.96 270)
				(length 2.54)
				(hide yes)
				(name "CVDD18")
				(number "60")
			)
			(pin passive line
				(at 0 60.96 270)
				(length 2.54)
				(hide yes)
				(name "CVDD18")
				(number "63")
			)
			(pin passive line
				(at 0 60.96 270)
				(length 2.54)
				(hide yes)
				(name "CVDD18")
				(number "64")
			)
			(pin passive line
				(at 0 60.96 270)
				(length 2.54)
				(hide yes)
				(name "CVDD18")
				(number "71")
			)
			(pin passive line
				(at 0 60.96 270)
				(length 2.54)
				(hide yes)
				(name "CVDD18")
				(number "72")
			)
			(pin power_in line
				(at 0 -60.96 90)
				(length 2.54)
				(name "AVSS")
				(number "73")
			)
			(pin power_in line
				(at 2.54 60.96 270)
				(length 2.54)
				(name "AVDD33")
				(number "55")
			)
			(pin passive line
				(at 2.54 60.96 270)
				(length 2.54)
				(hide yes)
				(name "AVDD33")
				(number "58")
			)
			(pin passive line
				(at 2.54 60.96 270)
				(length 2.54)
				(hide yes)
				(name "AVDD33")
				(number "65")
			)
			(pin passive line
				(at 2.54 60.96 270)
				(length 2.54)
				(hide yes)
				(name "AVDD33")
				(number "68")
			)
			(pin output line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "IOUT1P")
				(number "67")
			)
			(pin output line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "IOUT1N")
				(number "66")
			)
			(pin output line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "IOUT2P")
				(number "56")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "IOUT2N")
				(number "57")
			)
			(pin input line
				(at 17.78 0 180)
				(length 2.54)
				(name "FSADJ")
				(number "69")
			)
			(pin input line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "REFIO")
				(number "70")
			)
			(pin input line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "~{IRQ1}")
				(number "51")
			)
			(pin input line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "~{IRQ2}")
				(number "50")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "SDIO")
				(number "52")
			)
			(pin input line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "SCLK")
				(number "53")
			)
			(pin input line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "~{CS}")
				(number "54")
			)
			(pin input line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "~{RESET}")
				(number "5")
			)
			(pin input line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "TXEN")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD9744"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 -24.13 0)
		)
		(property "Value" "AD9744"
			(at 7.62 24.13 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at 15.24 5.08 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD9744.pdf"
			(at 15.24 5.08 0)
		)
		(property "Description" "210MSPS 14bit DAC, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "14bit DAC 1CH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AD9744_0_1")
		(symbol "AD9744_1_1"
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "D0")
				(number "14")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "D1")
				(number "13")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "D2")
				(number "12")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "D3")
				(number "11")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "D4")
				(number "10")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "D5")
				(number "9")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "D6")
				(number "8")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "D7")
				(number "7")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "D8")
				(number "6")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "D9")
				(number "5")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "D10")
				(number "4")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "D11")
				(number "3")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "D12")
				(number "2")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "D13")
				(number "1")
			)
			(pin input line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "CLK")
				(number "28")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "DVDD")
				(number "27")
			)
			(pin power_in line
				(at -2.54 -25.4 90)
				(length 2.54)
				(name "AGND")
				(number "20")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "AVDD")
				(number "24")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "DGND")
				(number "26")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "IOUTA")
				(number "22")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "IOUTB")
				(number "21")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "SLEEP")
				(number "15")
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "MODE")
				(number "25")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "FS_ADJ")
				(number "18")
			)
			(pin input line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "REFIO")
				(number "17")
			)
			(pin input line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "REFLO")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADS7830"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 13.716 0)
		)
		(property "Value" "ADS7830"
			(at 1.778 13.716 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 2.54 -17.78 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads7830.pdf"
			(at 5.08 -11.43 0)
		)
		(property "Description" "Single-supply, 8bit, 8 ch, SAR, 70kHz SR, 2.7 - 5 VDD, I2C, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "8bit DAC 8CH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADS7830_0_1")
		(symbol "ADS7830_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "CH0")
				(number "1")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "CH1")
				(number "2")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "CH2")
				(number "3")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "CH3")
				(number "4")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "CH4")
				(number "5")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "CH5")
				(number "6")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "CH6")
				(number "7")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "CH7")
				(number "8")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "COM")
				(number "11")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "SDA")
				(number "15")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "SCL")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "REFin/REFout")
				(number "10")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "A1")
				(number "13")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "A0")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CS434x-xZZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "CS434x-xZZ"
			(at 6.35 -8.89 0)
		)
		(property "Footprint" "Package_SO:TSSOP-10_3x3mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://statics.cirrus.com/pubs/proDatasheet/CS4344-45-48_F2.pdf"
			(at 0 0 0)
		)
		(property "Description" "24-Bit, 192-kHz Stereo D/A Converter, TSSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "24-bit PCM DAC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "CS434x-xZZ_0_1")
		(symbol "CS434x-xZZ_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SDIN")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "~{DEM}/SCLK")
				(number "2")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "LRCK")
				(number "3")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "MCLK")
				(number "4")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VA")
				(number "9")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "AGND")
				(number "8")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "AOUTL")
				(number "7")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "AOUTR")
				(number "10")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "FILT+")
				(number "6")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "VQ")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DAC08"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 17.78 0)
		)
		(property "Value" "DAC08"
			(at 5.08 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/DAC08.pdf"
			(at 0 0 0)
		)
		(property "Description" "DA Converter 8 bits"
			(at 0 0 0)
		)
		(property "ki_keywords" "DAC CNA"
			(at 0 0 0)
		)
		(symbol "DAC08_0_1")
		(symbol "DAC08_1_1"
			(pin input line
				(at -15.24 12.7 0)
				(length 3.81)
				(name "B0")
				(number "5")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 3.81)
				(name "B1")
				(number "6")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "B2")
				(number "7")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "B3")
				(number "8")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "B4")
				(number "9")
			)
			(pin input line
				(at -15.24 0 0)
				(length 3.81)
				(name "B5")
				(number "10")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "B6")
				(number "11")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 3.81)
				(name "B7")
				(number "12")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 3.81)
				(name "CMP")
				(number "16")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "V+")
				(number "13")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "V-")
				(number "3")
			)
			(pin input line
				(at 15.24 12.7 180)
				(length 3.81)
				(name "VLC")
				(number "1")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "I+")
				(number "2")
			)
			(pin output line
				(at 15.24 0 180)
				(length 3.81)
				(name "I-")
				(number "4")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 3.81)
				(name "R+")
				(number "14")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 3.81)
				(name "R-")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DAC081C081CIMK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 8.89 0)
		)
		(property "Value" "DAC081C081CIMK"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 16.51 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/dac081c081.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit Micropower DAC with I2C-Compatible Interface, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C DAC 8-bit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "DAC081C081CIMK_0_1")
		(symbol "DAC081C081CIMK_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SCL")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "SDA")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "ADR0")
				(number "6")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VA")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "VOUT")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DAC1007LCN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -24.765 26.67 0)
		)
		(property "Value" "DAC1007LCN"
			(at 19.685 26.67 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at 5.08 -2.54 0)
		)
		(property "Datasheet" "https://pdf.datasheetcatalog.com/datasheets/400/195351_DS.pdf"
			(at 35.56 -2.54 0)
		)
		(property "Description" "Double-Buffered D to A Converters, DIP-20"
			(at 7.62 -2.54 0)
		)
		(property "ki_keywords" "DAC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "DAC1007LCN_1_1"
			(text "1st"
				(at -8.255 -10.16 0)
			)
			(text "BYTE\nSTROBE"
				(at -6.35 -13.335 0)
			)
			(text "2st"
				(at -4.445 -10.16 0)
			)
			(text "XFER\nSTROBE"
				(at 2.54 -11.43 0)
			)
			(text_box "10\nBIT\n\nINP\nUT\n\nLAT\nCH"
				(at -10.16 20.32 0)
				(size 6.35 -27.94)
				(margins 1.016 1.016 1.016 1.016)
				(fill
					(type none)
				)
			)
			(text_box "\n\n\nCONTROL LOGIC"
				(at -10.16 -8.89 0)
				(size 26.67 -10.16)
				(margins 1.016 1.016 1.016 1.016)
				(fill
					(type none)
				)
			)
			(text_box "DAC\n\nREG\nIST\nER"
				(at 0 20.32 0)
				(size 5.08 -27.94)
				(margins 1.016 1.016 1.016 1.016)
				(fill
					(type none)
				)
			)
			(text_box "10\nBIT\n\nMUL\nTIP\nLYI\nNG\n\nD/A\nCON\nVER\nTER"
				(at 8.89 20.32 0)
				(size 7.62 -27.94)
				(margins 1.016 1.016 1.016 1.016)
				(fill
					(type none)
				)
			)
			(pin input line
				(at -27.94 17.78 0)
				(length 2.54)
				(name "DI0(LSB)")
				(number "15")
			)
			(pin input line
				(at -27.94 15.24 0)
				(length 2.54)
				(name "DI1")
				(number "16")
			)
			(pin input line
				(at -27.94 12.7 0)
				(length 2.54)
				(name "DI2")
				(number "17")
			)
			(pin input line
				(at -27.94 10.16 0)
				(length 2.54)
				(name "DI3")
				(number "18")
			)
			(pin input line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "DI4")
				(number "19")
			)
			(pin input line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "DI5")
				(number "5")
			)
			(pin input line
				(at -27.94 2.54 0)
				(length 2.54)
				(name "DI6")
				(number "6")
			)
			(pin input line
				(at -27.94 0 0)
				(length 2.54)
				(name "DI7")
				(number "7")
			)
			(pin input line
				(at -27.94 -2.54 0)
				(length 2.54)
				(name "DI8")
				(number "8")
			)
			(pin input line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "DI9(MSB)")
				(number "9")
			)
			(pin input line
				(at -27.94 -10.16 0)
				(length 2.54)
				(name "~{CS}")
				(number "1")
			)
			(pin input line
				(at -27.94 -12.7 0)
				(length 2.54)
				(name "~{WR}")
				(number "2")
			)
			(pin input line
				(at -27.94 -15.24 0)
				(length 2.54)
				(name "Byte1/~{Byte2}")
				(number "3")
			)
			(pin input line
				(at -27.94 -17.78 0)
				(length 2.54)
				(name "~{XFER}")
				(number "4")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin input line
				(at 27.94 15.24 180)
				(length 2.54)
				(name "V_{REF}")
				(number "13")
			)
			(pin output line
				(at 27.94 10.16 180)
				(length 2.54)
				(name "I_{OUT}2")
				(number "11")
			)
			(pin output line
				(at 27.94 7.62 180)
				(length 2.54)
				(name "I_{OUT}1")
				(number "12")
			)
			(pin input line
				(at 27.94 2.54 180)
				(length 2.54)
				(name "R_{FB}")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DAC1220E"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 11.43 0)
		)
		(property "Value" "DAC1220E"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_SO:SSOP-16_3.9x4.9mm_P0.635mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/dac1220.pdf"
			(at -1.27 1.27 0)
		)
		(property "Description" "20-Bit , Low-Power Digital-to-Analog Converter, SSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "DAC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "DAC1220E_0_1")
		(symbol "DAC1220E_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "VREF")
				(number "12")
			)
			(pin passive line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "C1")
				(number "9")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{CS}")
				(number "14")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "SDIO")
				(number "15")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "SCLK")
				(number "16")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "DVDD")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "DGND")
				(number "4")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "AVDD")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "AGND")
				(number "13")
			)
			(pin no_connect line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "6")
			)
			(pin no_connect line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "7")
			)
			(pin no_connect line
				(at 10.16 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "8")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "VOUT")
				(number "11")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "C2")
				(number "10")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "XOUT")
				(number "2")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "XIN")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DAC5311xDCK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "DAC5311xDCK"
			(at 7.62 -11.43 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/dac5311.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-Bit, Single-Channel, Voltage Output, Serial Interface Digital-to-Analog Converters, SC-70"
			(at 0 0 0)
		)
		(property "ki_keywords" "DAC SPI 1-channel"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
		(symbol "DAC5311xDCK_0_1")
		(symbol "DAC5311xDCK_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "DIN")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "SCLK")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{SYNC}")
				(number "1")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "AVDD/AVREF")
				(number "4")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "VOUT")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DAC5578xPW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "DAC5578xPW"
			(at 7.62 13.97 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/dac5578.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-Bit, Octal-Channel, Ultra-Low Glitch, Voltage Output, Two-Wire Interface Digital-to-Analog Converters, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "DAC I2C TWI 8-channel"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "DAC5578xPW_0_1")
		(symbol "DAC5578xPW_1_1"
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "~{LDAC}")
				(number "1")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "~{CLR}")
				(number "9")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "VREFIN")
				(number "8")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "ADDR0")
				(number "2")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "SCL")
				(number "16")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "SDA")
				(number "15")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "AVDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "14")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "VOUTA")
				(number "4")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VOUTB")
				(number "13")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUTC")
				(number "5")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "VOUTD")
				(number "12")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "VOUTE")
				(number "6")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "VOUTF")
				(number "11")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "VOUTG")
				(number "7")
			)
			(pin output line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "VOUTH")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DAC5578xRGE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "DAC5578xRGE"
			(at 7.62 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.7x2.7mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/dac5578.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-Bit, Octal-Channel, Ultra-Low Glitch, Voltage Output, Two-Wire Interface Digital-to-Analog Converters, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "DAC I2C TWI 8-channel"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "DAC5578xRGE_0_1")
		(symbol "DAC5578xRGE_1_1"
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "~{LDAC}")
				(number "22")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "~{CLR}")
				(number "12")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "RSTSEL")
				(number "9")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "TWOC")
				(number "21")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "VREFIN")
				(number "8")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "ADDR0")
				(number "11")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "ADDR1")
				(number "10")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "SCL")
				(number "20")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "SDA")
				(number "19")
			)
			(pin passive line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "EP")
				(number "25")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "AVDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "17")
			)
			(pin no_connect line
				(at 2.54 10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "24")
			)
			(pin no_connect line
				(at 5.08 12.7 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "23")
			)
			(pin no_connect line
				(at 5.08 10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at 7.62 12.7 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "18")
			)
			(pin no_connect line
				(at 7.62 10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "VOUTA")
				(number "3")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VOUTB")
				(number "16")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUTC")
				(number "4")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "VOUTD")
				(number "15")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "VOUTE")
				(number "5")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "VOUTF")
				(number "14")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "VOUTG")
				(number "6")
			)
			(pin output line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "VOUTH")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DAC7513_DCN"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 12.065 0)
		)
		(property "Value" "DAC7513_DCN"
			(at -2.54 10.16 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-8"
			(at 1.27 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com.cn/cn/lit/ds/symlink/dac7513.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Power, Rail-to-Rail Output, 12-Bit Serial Input DAC"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI DAC 12 bit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "DAC7513_DCN_0_1")
		(symbol "DAC7513_DCN_1_1"
			(pin input line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "DIN")
				(number "6")
			)
			(pin input clock
				(at -15.24 0 0)
				(length 3.81)
				(name "SCLK")
				(number "7")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 3.81)
				(name "~{SYNC}")
				(number "8")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 3.81)
				(name "VCC")
				(number "4")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 3.81)
				(name "GND")
				(number "5")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "VOUT")
				(number "1")
			)
			(pin input line
				(at 15.24 0 180)
				(length 3.81)
				(name "VFB")
				(number "2")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 3.81)
				(name "VREF")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DAC80502"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "DAC80502"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_SON:Texas_DRX_WSON-10_2.5x2.5mm_P0.5mm"
			(at 5.08 -17.78 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/dac80502.pdf"
			(at 5.08 -20.32 0)
		)
		(property "Description" "16-bit dual-channel voltage output DAC, 2.5V 5ppm/°C internal reference, WSON-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "texas digital-analog converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*2.5x2.5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "DAC80502_0_0"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SPI2C")
				(number "5")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RSTSEL")
				(number "3")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SDIN/SDA")
				(number "8")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "~{SYNC}/A0")
				(number "7")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "AGND")
				(number "4")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "VREFIO")
				(number "10")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "VOUTA")
				(number "2")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "VOUTB")
				(number "9")
			)
		)
		(symbol "DAC80502_1_0"
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "SCLK/SCL")
				(number "6")
			)
		)
		(symbol "DAC80502_1_1")
		(embedded_fonts no)
	)
	(symbol "DAC80504"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.192 16.51 0)
		)
		(property "Value" "DAC80504"
			(at 10.922 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RTE0016D_WQFN-16-1EP_3x3mm_P0.5mm_EP0.8x0.8mm_ThermalVias"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/dac80504.pdf"
			(at 0 0 0)
		)
		(property "Description" "16-bit quad-channel voltage output DAC, 2.5V 2ppm/°C internal reference, WQFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "texas quad digital-analog converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RTE0016D*WQFN*16*EP0.8x0.8mm*"
			(at 0 0 0)
		)
		(symbol "DAC80504_0_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "GAIN")
				(number "8")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "RSTSEL")
				(number "9")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "REFDIV")
				(number "10")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{LDAC}")
				(number "11")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "SDI")
				(number "14")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "~{CS}")
				(number "12")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "SCLK")
				(number "13")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 2.54)
				(name "VIO")
				(number "16")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "OUT0")
				(number "2")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "OUT1")
				(number "3")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OUT2")
				(number "4")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "OUT3")
				(number "5")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "SDO/~{ALARM}")
				(number "15")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "REF")
				(number "1")
			)
		)
		(symbol "DAC80504_1_0"
			(pin passive line
				(at -2.54 -17.78 90)
				(length 2.54)
				(name "EP")
				(number "17")
			)
		)
		(symbol "DAC80504_1_1")
		(embedded_fonts no)
	)
	(symbol "DAC8165"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 21.59 0)
		)
		(property "Value" "DAC8165"
			(at 10.16 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at -22.86 -17.78 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/dac8165.pdf"
			(at -25.4 -17.78 0)
		)
		(property "Description" "14-bit quad-channel voltage output DAC with 2.5V internal reference"
			(at 0 0 0)
		)
		(property "ki_keywords" "14-bit quad DAC voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "DAC8165_0_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "LDAC")
				(number "16")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "~{SYNC}")
				(number "9")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "SCLK")
				(number "10")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "DIN")
				(number "11")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "VREFH/VREFOUT")
				(number "3")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "VREFL")
				(number "5")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "~{RST}")
				(number "13")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "RSTSEL")
				(number "14")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "~{ENABLE}")
				(number "15")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 2.54)
				(name "AVDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "IOVDD")
				(number "12")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "VOUTA")
				(number "1")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "VOUTB")
				(number "2")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "VOUTC")
				(number "7")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "VOUTD")
				(number "8")
			)
		)
		(symbol "DAC8165_0_1")
		(embedded_fonts no)
	)
	(symbol "DAC8501E"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 8.89 0)
		)
		(property "Value" "DAC8501E"
			(at 8.89 -8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 2.54 -12.7 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/dac8501.pdf"
			(at 2.54 -15.24 0)
		)
		(property "Description" "16-bit DAC, Voltage Output, Rail-to-Rail Output, SPI interface, MSOP-8 3x3mm package"
			(at 0 0 0)
		)
		(property "ki_keywords" "DAC 16-Bit  Voltage Output Rail-to-Rail SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm?P0.65mm*"
			(at 0 0 0)
		)
		(symbol "DAC8501E_0_0"
			(text "DAC"
				(at 0.635 -0.635 0)
			)
		)
		(symbol "DAC8501E_0_1")
		(symbol "DAC8501E_1_1"
			(text "CTRL"
				(at -5.715 -5.08 0)
			)
			(text "-"
				(at 6.985 0.635 0)
			)
			(text "+"
				(at 6.985 -0.635 0)
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "SCLK")
				(number "6")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "D_{IN}")
				(number "7")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "~{SYNC}")
				(number "5")
			)
			(pin input line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "V_{REF}")
				(number "2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "V_{DD}")
				(number "1")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "V_{FB}")
				(number "3")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "V_{OUT}")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DAC8552"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.112 10.922 0)
		)
		(property "Value" "DAC8552"
			(at 7.112 8.89 0)
		)
		(property "Footprint" "Package_SO:Texas_S-PDSO-G8_3x3mm_P0.65mm"
			(at 27.686 -12.192 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/dac8552.pdf"
			(at 27.178 -14.732 0)
		)
		(property "Description" "Digital to analog converter, 16 Bit, 2 ch, ultra-low glitch, 2.7 - 5.5 VDD, MSOP-8"
			(at 44.704 -9.652 0)
		)
		(property "ki_keywords" "Texas dual DAC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*S?PDSO?G8*3x3mm*P0.65*"
			(at 0 0 0)
		)
		(symbol "DAC8552_0_1")
		(symbol "DAC8552_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "D_{IN}")
				(number "7")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SCLK")
				(number "6")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{SYNC}")
				(number "5")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V_{DD}")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin power_in line
				(at 5.08 10.16 270)
				(length 2.54)
				(name "V_{REF}")
				(number "2")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "V_{OUT}A")
				(number "4")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "V_{OUT}B")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DAC8560IxDGK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 8.255 0)
		)
		(property "Value" "DAC8560IxDGK"
			(at 6.35 -8.89 0)
		)
		(property "Footprint" "Package_SON:VSON-8-1EP_3x3mm_P0.65mm_EP1.65x2.4mm"
			(at 0 -12.065 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/dac8560.pdf"
			(at 0 -14.605 0)
		)
		(property "Description" "16-bit DAC, Voltage Output, Ultra-Low Glitch, Rail-to-Rail Output, 2.5V 2-ppm/°C Internal Reference, SPI interface, VSON-8 3x3mm package"
			(at 0 0 0)
		)
		(property "ki_keywords" "DAC 16-Bit Voltage Output Rail-to-Rail Internal Reference SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSON*3x3mm?P0.65mm*"
			(at 0 0 0)
		)
		(symbol "DAC8560IxDGK_0_0"
			(text "DAC"
				(at 0.635 -0.635 0)
			)
		)
		(symbol "DAC8560IxDGK_0_1")
		(symbol "DAC8560IxDGK_1_1"
			(text "2.5V"
				(at -7.62 5.08 0)
			)
			(text "CTRL"
				(at -5.715 -5.08 0)
			)
			(text "-"
				(at 6.985 0.635 0)
			)
			(text "+"
				(at 6.985 -0.635 0)
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "SCLK")
				(number "6")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "D_{IN}")
				(number "7")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "~{SYNC}")
				(number "5")
			)
			(pin bidirectional line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "V_{REF}")
				(number "2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "V_{DD}")
				(number "1")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "V_{FB}")
				(number "3")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "V_{OUT}")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DAC8571IDGK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "DAC8571IDGK"
			(at 10.16 -8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 2.54 -12.7 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/dac8571.pdf"
			(at 2.54 -15.24 0)
		)
		(property "Description" "DAC, 16-Bit, Low Power, Voltage Output, Rail-to-Rail Output, I2C Interface, MSOP-8 3x3mm package"
			(at 0 0 0)
		)
		(property "ki_keywords" "DAC 16-Bit Voltage Output Rail-to-Rail I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm?P0.65mm*"
			(at 0 0 0)
		)
		(symbol "DAC8571IDGK_0_0"
			(text "DAC"
				(at 0.635 -0.635 0)
			)
		)
		(symbol "DAC8571IDGK_0_1")
		(symbol "DAC8571IDGK_1_1"
			(text "CTRL"
				(at -5.715 -5.08 0)
			)
			(text "-"
				(at 6.985 0.635 0)
			)
			(text "+"
				(at 6.985 -0.635 0)
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "SDA")
				(number "7")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "A0")
				(number "5")
			)
			(pin input line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "V_{REF}")
				(number "2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "V_{DD}")
				(number "1")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "V_{SENSE}")
				(number "3")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "V_{OUT}")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DAC8750xRHA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 19.05 0)
		)
		(property "Value" "DAC8750xRHA"
			(at 3.81 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHA_VQFN-40-1EP_6x6mm_P0.5mm_EP4.6x4.6mm_ThermalVias"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/dac7750.pdf"
			(at 0 -17.78 0)
		)
		(property "Description" "Single-Channel, 16bit Programmable Current Output DAC for 4-mA to 20-mA Current Loop Applications, VQFN-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "DAC Current Loop 20mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RHA*EP4.6x4.6mm*"
			(at 0 0 0)
		)
		(symbol "DAC8750xRHA_1_1"
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "DIN")
				(number "8")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "SCLK")
				(number "7")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "CLR")
				(number "5")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "LATCH")
				(number "6")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "DVDD-EN")
				(number "23")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "HART-IN")
				(number "24")
			)
			(pin output line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "SDO")
				(number "9")
			)
			(pin no_connect line
				(at -10.16 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "21")
			)
			(pin no_connect line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -10.16 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "40")
			)
			(pin no_connect line
				(at -10.16 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "38")
			)
			(pin no_connect line
				(at -10.16 -12.7 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at -5.08 17.78 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin no_connect line
				(at -5.08 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "30")
			)
			(pin no_connect line
				(at -2.54 17.78 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "22")
			)
			(pin no_connect line
				(at -2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "31")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "DVDD")
				(number "39")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "37")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "41")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "AVDD")
				(number "36")
			)
			(pin no_connect line
				(at 2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "32")
			)
			(pin no_connect line
				(at 5.08 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "33")
			)
			(pin no_connect line
				(at 10.16 10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "20")
			)
			(pin no_connect line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "35")
			)
			(pin no_connect line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "34")
			)
			(pin no_connect line
				(at 10.16 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "19")
			)
			(pin passive line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "CAP1")
				(number "28")
			)
			(pin passive line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "CAP2")
				(number "29")
			)
			(pin open_collector line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "~{ALARM}")
				(number "2")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "R3-SENSE")
				(number "25")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "BOOST")
				(number "27")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "IOUT")
				(number "26")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "REFOUT")
				(number "17")
			)
			(pin input line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "REFIN")
				(number "18")
			)
			(pin passive line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "ISET-R")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC1257"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 10.16 0)
		)
		(property "Value" "LTC1257"
			(at 3.81 10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1257fc.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Supply 12-bit DAC with Internal Reference Voltage, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "DAC 12-bit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*"
			(at 0 0 0)
		)
		(symbol "LTC1257_0_1")
		(symbol "LTC1257_1_1"
			(pin input line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "DIN")
				(number "2")
			)
			(pin output line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "DOUT")
				(number "4")
			)
			(pin input clock
				(at -15.24 0 0)
				(length 3.81)
				(name "CKL")
				(number "1")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 3.81)
				(name "~{LOAD}")
				(number "3")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 3.81)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 3.81)
				(name "GND")
				(number "5")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "VOUT")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 3.81)
				(name "VREF")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC1446"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 10.795 0)
		)
		(property "Value" "LTC1446"
			(at -2.54 8.89 0)
		)
		(property "Footprint" ""
			(at 20.32 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1446fa.pdf"
			(at 20.32 -7.62 0)
		)
		(property "Description" "2-Channel 12-Bit Rail-To-Rail D/A Converters with SPI Interface and Internal Reference (4.096V)"
			(at 0 0 0)
		)
		(property "ki_keywords" "12-Bit DAC SPI Reference 2ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LTC1446_0_0"
			(text "CNTRL"
				(at -2.54 -2.54 900)
			)
			(text "DAC"
				(at 3.81 1.27 0)
			)
			(text "DAC"
				(at 3.81 -3.81 0)
			)
		)
		(symbol "LTC1446_0_1")
		(symbol "LTC1446_1_1"
			(pin input clock
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SCK")
				(number "1")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "SDI")
				(number "2")
			)
			(pin output line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SDO")
				(number "4")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{CS}/LD")
				(number "3")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "7")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "VA")
				(number "5")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "VB")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC1664CGN"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 12.7 0)
		)
		(property "Value" "LTC1664CGN"
			(at 2.54 12.7 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1664fa.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad Micropower 10-bit DAC, Standard, SSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Quad DAC Micropower 10bit 4ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SSOP*"
			(at 0 0 0)
		)
		(symbol "LTC1664CGN_0_1")
		(symbol "LTC1664CGN_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 3.81)
				(name "DIN")
				(number "9")
			)
			(pin output line
				(at -12.7 5.08 0)
				(length 3.81)
				(name "DOUT")
				(number "10")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 3.81)
				(name "SCK")
				(number "8")
			)
			(pin input line
				(at -12.7 0 0)
				(length 3.81)
				(name "~{CS}/LD")
				(number "7")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 3.81)
				(name "~{CLR}")
				(number "11")
			)
			(pin no_connect line
				(at -5.08 -11.43 90)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin no_connect line
				(at -2.54 -11.43 90)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 3.81)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin no_connect line
				(at 2.54 -11.43 90)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin no_connect line
				(at 5.08 -11.43 90)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 3.81)
				(name "OUTA")
				(number "2")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 3.81)
				(name "OUTB")
				(number "3")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 3.81)
				(name "OUTC")
				(number "4")
			)
			(pin output line
				(at 12.7 0 180)
				(length 3.81)
				(name "OUTD")
				(number "5")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 3.81)
				(name "REF")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX5139"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.89 17.145 0)
		)
		(property "Value" "MAX5139"
			(at 8.89 15.24 0)
		)
		(property "Footprint" "Package_DFN_QFN:TQFN-16-1EP_3x3mm_P0.5mm_EP1.23x1.23mm"
			(at 8.89 12.7 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX5138-MAX5139.pdf"
			(at 8.89 10.16 0)
		)
		(property "Description" "Low-Power, Single, 12-Bit, Buffered Voltage-Output DAC"
			(at 0 0 0)
		)
		(property "ki_keywords" "12-bit DAC 1CH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MAX5139_0_1")
		(symbol "MAX5139_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "M/~{Z}")
				(number "2")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "~{LDAC}")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "SCLK")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "DIN")
				(number "7")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{CS}")
				(number "6")
			)
			(pin output line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "~{READY}")
				(number "10")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 2.54)
				(name "DVDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 2.54)
				(name "AGND")
				(number "16")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "AVDD")
				(number "13")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "AGND")
				(number "8")
			)
			(pin no_connect line
				(at 7.62 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at 7.62 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at 7.62 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "OUT")
				(number "12")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "REFO")
				(number "15")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "REFI")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX5215"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "MAX5215"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 33.02 -8.89 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX5215-MAX5217.pdf"
			(at 8.89 6.35 0)
		)
		(property "Description" "Digital to analog, 14 Bit, 1 ch, 2.7 - 5.5 VDD, I2C, uMAX-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "DA 14 Bit 1 ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MAX5215_0_1")
		(symbol "MAX5215_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SCL")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SDA")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{AUX}")
				(number "5")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "ADDR")
				(number "2")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "REF")
				(number "1")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX5717xSD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "MAX5717xSD"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX5717-MAX5719.pdf"
			(at 0 0 0)
		)
		(property "Description" "16-bit Voltage Digital-to-Analog converter, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "DAC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MAX5717xSD_0_1")
		(symbol "MAX5717xSD_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "REFF")
				(number "6")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "REFS")
				(number "5")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{CS}")
				(number "7")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "DIN")
				(number "10")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "SCLK")
				(number "8")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "~{LDAC}")
				(number "11")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "DGND")
				(number "12")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "AGNDF")
				(number "3")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "AGNDS")
				(number "4")
			)
			(pin no_connect line
				(at 10.16 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "RFB")
				(number "1")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "OUT")
				(number "2")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "INV")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX5741"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "MAX5741"
			(at 6.096 8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX5741.pdf"
			(at 19.05 16.51 0)
		)
		(property "Description" "Digital to analog, 10 Bit, 4 ch, 2.7 - 5.5 VDD, SPI, uMAX-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "DA 8 Bit 4 ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm?P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MAX5741_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "~{CS}")
				(number "1")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "SCLK")
				(number "2")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "DIN")
				(number "5")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "REF")
				(number "6")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "OUTA")
				(number "7")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OUTB")
				(number "8")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "OUTC")
				(number "9")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "OUTD")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX5813"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 11.43 0)
		)
		(property "Value" "MAX5813"
			(at 8.89 11.43 0)
		)
		(property "Footprint" ""
			(at 11.43 1.27 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX5813-MAX5815.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "Digital to analog, 8 Bit, 4 ch, 2.7 - 5.5 VDD, I2C, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "DA 8 Bit 4 ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TSSOP*14*4.4*"
			(at 0 0 0)
		)
		(symbol "MAX5813_0_1")
		(symbol "MAX5813_1_1"
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "SDA")
				(number "11")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SCL")
				(number "10")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{LDAC}")
				(number "14")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{CLR}")
				(number "12")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "ADDR0")
				(number "9")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "ADDR1")
				(number "8")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDDIO")
				(number "13")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "REF")
				(number "1")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OUTA")
				(number "2")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "OUTB")
				(number "3")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "OUTC")
				(number "5")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "OUTD")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX5813WLP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "MAX5813WLP"
			(at 8.89 8.89 0)
		)
		(property "Footprint" ""
			(at 11.43 -1.27 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX5813-MAX5815.pdf"
			(at 1.27 -2.54 0)
		)
		(property "Description" "Digital to analog, 8 Bit, 4 ch, 2.7 - 5.5 VDD, I2C, TSSOP-14, Maxim_WLP-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "DA 8 Bit 4 ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Maxim*WLP*12*"
			(at 0 0 0)
		)
		(symbol "MAX5813WLP_0_1")
		(symbol "MAX5813WLP_1_1"
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SDA")
				(number "C2")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SCL")
				(number "C3")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{CLR}")
				(number "C1")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "ADDR0")
				(number "C4")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "B4")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDDIO")
				(number "B3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "B2")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "REF")
				(number "B1")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OUTA")
				(number "A1")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "OUTB")
				(number "A2")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "OUTC")
				(number "A3")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "OUTD")
				(number "A4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC1408_DIP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 16.51 0)
		)
		(property "Value" "MC1408_DIP"
			(at 2.54 13.97 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.pinballpcb.com/datasheets/OnMC1408-dac.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit multiplying DAC"
			(at 0 0 0)
		)
		(property "ki_keywords" "8 bit multiplying DAC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MC1408_DIP_0_0")
		(symbol "MC1408_DIP_1_1"
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "A8")
				(number "5")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "A7")
				(number "6")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "A6")
				(number "7")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A5")
				(number "8")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A4")
				(number "9")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A3")
				(number "10")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A2")
				(number "11")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A1")
				(number "12")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "13")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "VEE")
				(number "3")
			)
			(pin no_connect line
				(at 7.62 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin output line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "VREF+")
				(number "14")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "VREF-")
				(number "15")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "I0")
				(number "4")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "COMPEN")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC1408_SOIC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 16.51 0)
		)
		(property "Value" "MC1408_SOIC"
			(at 2.54 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.pinballpcb.com/datasheets/OnMC1408-dac.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit multiplying DAC"
			(at 0 0 0)
		)
		(property "ki_keywords" "8 bit multiplying DAC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MC1408_SOIC_0_0")
		(symbol "MC1408_SOIC_1_1"
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "A8")
				(number "16")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "A7")
				(number "15")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "A6")
				(number "14")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A5")
				(number "13")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A4")
				(number "12")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A3")
				(number "11")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A2")
				(number "10")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A1")
				(number "9")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "VEE")
				(number "7")
			)
			(pin no_connect line
				(at 7.62 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin output line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "VREF+")
				(number "2")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "VREF-")
				(number "3")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "I0")
				(number "8")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "COMPEN")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP4725xxx-xCH"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MCP4725xxx-xCH"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22039d.pdf"
			(at 0 0 0)
		)
		(property "Description" "12-bit Digital-to-Analog Converter, integrated EEPROM, I2C interface, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "dac twi"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MCP4725xxx-xCH_0_1")
		(symbol "MCP4725xxx-xCH_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SCL")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "SDA")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A0")
				(number "6")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "VSS")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "VOUT")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP4728"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 6.35 0)
		)
		(property "Value" "MCP4728"
			(at 12.7 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22187E.pdf"
			(at 0 6.35 0)
		)
		(property "Description" "12-bit digital to analog converter, quad output, 2.048V internal reference, integrated EEPROM, I2C interface"
			(at 0 0 0)
		)
		(property "ki_keywords" "dac i2c"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MCP4728_0_1")
		(symbol "MCP4728_1_1"
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "SCL")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "SDA")
				(number "3")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "~{LDAC}")
				(number "4")
			)
			(pin output line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "RDY/~{BSY}")
				(number "5")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "10")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "VOUTA")
				(number "6")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "VOUTB")
				(number "7")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "VOUTC")
				(number "8")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "VOUTD")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP4801"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 10.795 0)
		)
		(property "Value" "MCP4801"
			(at 1.27 8.89 0)
		)
		(property "Footprint" ""
			(at 22.86 -2.54 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22244B.pdf"
			(at 22.86 -2.54 0)
		)
		(property "Description" "8-Bit D/A Converters with SPI Interface, internal Reference (2.048V)"
			(at 0 0 0)
		)
		(property "ki_keywords" "8-Bit DAC SPI Reference 1ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* MSOP*3x3mm*P0.65mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MCP4801_0_0")
		(symbol "MCP4801_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "6")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "~{LDAC}")
				(number "5")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{CS}")
				(number "2")
			)
			(pin input clock
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SCK")
				(number "3")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "SDI")
				(number "4")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "Vdd")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "Vss")
				(number "7")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "Vout")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP4801-EMC"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 10.795 0)
		)
		(property "Value" "MCP4801-EMC"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.75x1.45mm"
			(at 0 -11.938 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22244B.pdf"
			(at 22.86 -2.54 0)
		)
		(property "Description" "8-Bit D/A Converters with SPI Interface, internal Reference (2.048V)"
			(at 0 0 0)
		)
		(property "ki_keywords" "8-Bit DAC SPI Reference 1ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MCP4801-EMC_0_0")
		(symbol "MCP4801-EMC_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "6")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "~{LDAC}")
				(number "5")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{CS}")
				(number "2")
			)
			(pin input clock
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SCK")
				(number "3")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "SDI")
				(number "4")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "Vdd")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "Vss")
				(number "7")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "PAD/Vss")
				(number "9")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "Vout")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP4802"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 10.795 0)
		)
		(property "Value" "MCP4802"
			(at -2.54 8.89 0)
		)
		(property "Footprint" ""
			(at 20.32 -7.62 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002249B.pdf"
			(at 20.32 -7.62 0)
		)
		(property "Description" "2-Channel 8-Bit D/A Converters with SPI Interface and Internal Reference (2.048V)"
			(at 0 0 0)
		)
		(property "ki_keywords" "8-Bit DAC SPI Reference 2ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm* MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP4802_0_0"
			(text "CNTRL"
				(at -2.032 -4.191 900)
			)
			(text "DAC"
				(at 3.81 1.27 0)
			)
			(text "DAC"
				(at 3.81 -3.81 0)
			)
		)
		(symbol "MCP4802_0_1")
		(symbol "MCP4802_1_1"
			(pin input clock
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SCK")
				(number "3")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{LDAC}")
				(number "5")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SDI")
				(number "4")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{CS}")
				(number "2")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "Vdd")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "Vss")
				(number "7")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "VA")
				(number "8")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "VB")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP4901"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 10.795 0)
		)
		(property "Value" "MCP4901"
			(at 6.35 8.89 0)
		)
		(property "Footprint" ""
			(at 25.4 -2.54 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22248a.pdf"
			(at 25.4 -2.54 0)
		)
		(property "Description" "8-Bit D/A Converters with SPI Interface"
			(at 0 0 0)
		)
		(property "ki_keywords" "8-Bit DAC SPI  1ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* MSOP*3x3mm*P0.65mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MCP4901_0_0")
		(symbol "MCP4901_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{LDAC}")
				(number "5")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{CS}")
				(number "2")
			)
			(pin input clock
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SCK")
				(number "3")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SDI")
				(number "4")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "Vdd")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "Vss")
				(number "7")
			)
			(pin power_in line
				(at 5.08 10.16 270)
				(length 2.54)
				(name "Vref")
				(number "6")
			)
			(pin output line
				(at 17.78 0 180)
				(length 2.54)
				(name "Vout")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP4901-EMC"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 10.795 0)
		)
		(property "Value" "MCP4901-EMC"
			(at 6.35 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.75x1.45mm"
			(at 0 -12.192 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22248a.pdf"
			(at 25.4 -2.54 0)
		)
		(property "Description" "8-Bit D/A Converters with SPI Interface"
			(at 0 0 0)
		)
		(property "ki_keywords" "8-Bit DAC SPI  1ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MCP4901-EMC_0_0")
		(symbol "MCP4901-EMC_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{LDAC}")
				(number "5")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{CS}")
				(number "2")
			)
			(pin input clock
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SCK")
				(number "3")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SDI")
				(number "4")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "Vdd")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "Vss")
				(number "7")
			)
			(pin power_in line
				(at 5.08 10.16 270)
				(length 2.54)
				(name "Vref")
				(number "6")
			)
			(pin power_in line
				(at 5.08 -10.16 90)
				(length 2.54)
				(name "PAD/Vss")
				(number "9")
			)
			(pin output line
				(at 17.78 0 180)
				(length 2.54)
				(name "Vout")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP4902"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -1.905 10.795 0)
		)
		(property "Value" "MCP4902"
			(at -1.905 8.89 0)
		)
		(property "Footprint" ""
			(at 20.32 -7.62 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22250A.pdf"
			(at 20.32 -7.62 0)
		)
		(property "Description" "2-Channel 8-Bit D/A Converters with SPI Interface"
			(at 0 0 0)
		)
		(property "ki_keywords" "8-Bit DAC SPI  2ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x8.7mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP4902_0_0"
			(text "CNTRL"
				(at -2.032 -6.731 900)
			)
			(text "DAC"
				(at 3.81 1.27 0)
			)
			(text "DAC"
				(at 3.81 -3.81 0)
			)
		)
		(symbol "MCP4902_0_1")
		(symbol "MCP4902_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "9")
			)
			(pin input clock
				(at -12.7 0 0)
				(length 2.54)
				(name "SCK")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{LDAC}")
				(number "8")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "SDI")
				(number "5")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "~{CS}")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -2.54 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "Vdd")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "Vss")
				(number "12")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "VrefA")
				(number "13")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "VA")
				(number "14")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "VB")
				(number "10")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "VrefB")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP4921-EMS"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 7.62 0)
		)
		(property "Value" "MCP4921-EMS"
			(at 0 7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/21897a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single 12-bit Digital to Analog Converter, SPI Interface, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single DAC 1ch 12bit SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP* SOIC* DIP* PDIP*"
			(at 0 0 0)
		)
		(symbol "MCP4921-EMS_0_1")
		(symbol "MCP4921-EMS_1_1"
			(pin input line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "SDI")
				(number "4")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "SCK")
				(number "3")
			)
			(pin input line
				(at -15.24 0 0)
				(length 3.81)
				(name "~{CS}")
				(number "2")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "~{LDAC}")
				(number "5")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 3.81)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 3.81)
				(name "AVSS")
				(number "7")
			)
			(pin passive line
				(at 2.54 -10.16 90)
				(length 3.81)
				(name "VrefA")
				(number "6")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(name "VoutA")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP4922-EP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 10.16 0)
		)
		(property "Value" "MCP4922-EP"
			(at 3.81 10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/21897a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual 12-bit Digital to Analog Converter, SPI Interface, PDIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual DAC 1ch 12bit SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SO* SOIC* TSSOP*"
			(at 0 0 0)
		)
		(symbol "MCP4922-EP_0_1")
		(symbol "MCP4922-EP_1_1"
			(pin input line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "SDI")
				(number "5")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "SCK")
				(number "4")
			)
			(pin input line
				(at -15.24 0 0)
				(length 3.81)
				(name "~{CS}")
				(number "3")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "~{LDAC}")
				(number "8")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 3.81)
				(name "~{SHDN}")
				(number "9")
			)
			(pin no_connect line
				(at -10.16 -8.89 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at -7.62 -8.89 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -5.08 -8.89 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 3.81)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 3.81)
				(name "AVSS")
				(number "12")
			)
			(pin passive line
				(at 2.54 12.7 270)
				(length 3.81)
				(name "VrefA")
				(number "13")
			)
			(pin passive line
				(at 2.54 -12.7 90)
				(length 3.81)
				(name "VrefB")
				(number "11")
			)
			(pin passive line
				(at 15.24 5.08 180)
				(length 5.08)
				(name "VoutA")
				(number "14")
			)
			(pin passive line
				(at 15.24 -5.08 180)
				(length 5.08)
				(name "VoutB")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "THS5641AxDW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 22.86 0)
		)
		(property "Value" "THS5641AxDW"
			(at 10.16 22.86 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at -10.16 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ths5641a.pdf"
			(at -13.97 -16.51 0)
		)
		(property "Description" "8-Bit, 100 MSPS, CommsDAC, Parallel Current DAC, SOIC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "DAC IDAC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "THS5641AxDW_0_1")
		(symbol "THS5641AxDW_1_1"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "MODE")
				(number "25")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "CLK")
				(number "28")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "D0")
				(number "8")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "D1")
				(number "7")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "D2")
				(number "6")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "D3")
				(number "5")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "D4")
				(number "4")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "D5")
				(number "3")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "D6")
				(number "2")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "D7")
				(number "1")
			)
			(pin no_connect line
				(at -10.16 -15.24 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at -10.16 -17.78 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 2.54)
				(name "DVDD")
				(number "27")
			)
			(pin power_in line
				(at -2.54 -22.86 90)
				(length 2.54)
				(name "DGND")
				(number "26")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "AVDD")
				(number "24")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "AGND")
				(number "20")
			)
			(pin no_connect line
				(at 10.16 17.78 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin no_connect line
				(at 10.16 12.7 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at 10.16 -15.24 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin no_connect line
				(at 10.16 -17.78 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin input line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "COMP1")
				(number "19")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "IOUT1")
				(number "22")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "~{IOUT2}")
				(number "21")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "EXTLO")
				(number "16")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "EXTIO")
				(number "17")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "COMP2")
				(number "23")
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "BIASJ")
				(number "18")
			)
			(pin input line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "SLEEP")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "THS5641AxPW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 22.86 0)
		)
		(property "Value" "THS5641AxPW"
			(at 10.16 22.86 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at -10.16 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ths5641a.pdf"
			(at -13.97 -16.51 0)
		)
		(property "Description" "8-Bit, 100 MSPS, CommsDAC, Parallel Current DAC, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "DAC IDAC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "THS5641AxPW_0_1")
		(symbol "THS5641AxPW_1_1"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "MODE")
				(number "25")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "CLK")
				(number "28")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "D0")
				(number "8")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "D1")
				(number "7")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "D2")
				(number "6")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "D3")
				(number "5")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "D4")
				(number "4")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "D5")
				(number "3")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "D6")
				(number "2")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "D7")
				(number "1")
			)
			(pin no_connect line
				(at -10.16 -15.24 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at -10.16 -17.78 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 2.54)
				(name "DVDD")
				(number "27")
			)
			(pin power_in line
				(at -2.54 -22.86 90)
				(length 2.54)
				(name "DGND")
				(number "26")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "AVDD")
				(number "24")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "AGND")
				(number "20")
			)
			(pin no_connect line
				(at 10.16 17.78 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin no_connect line
				(at 10.16 12.7 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at 10.16 -15.24 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin no_connect line
				(at 10.16 -17.78 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin input line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "COMP1")
				(number "19")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "IOUT1")
				(number "22")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "~{IOUT2}")
				(number "21")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "EXTLO")
				(number "16")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "EXTIO")
				(number "17")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "COMP2")
				(number "23")
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "BIASJ")
				(number "18")
			)
			(pin input line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "SLEEP")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLV5627CD"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 12.7 0)
		)
		(property "Value" "TLV5627CD"
			(at 6.35 12.7 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv5627.pdf"
			(at 0 0 0)
		)
		(property "Description" "4-Channel DAC, 8bit, w/ Power Down, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "DAC 4CH 8bit"
			(at 0 0 0)
		)
		(symbol "TLV5627CD_0_1")
		(symbol "TLV5627CD_1_1"
			(pin input line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "DIN")
				(number "4")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "SCLK")
				(number "5")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "FS")
				(number "7")
			)
			(pin input line
				(at -17.78 0 0)
				(length 3.81)
				(name "~{CS}")
				(number "6")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "~{LDAC}")
				(number "3")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "~{PD}")
				(number "2")
			)
			(pin power_in line
				(at -5.08 15.24 270)
				(length 3.81)
				(name "DVDD")
				(number "1")
			)
			(pin power_in line
				(at -5.08 -15.24 90)
				(length 3.81)
				(name "DGND")
				(number "8")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 3.81)
				(name "AVDD")
				(number "16")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 3.81)
				(name "AGND")
				(number "9")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "OUTA")
				(number "14")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "OUTB")
				(number "13")
			)
			(pin input line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "REFINAB")
				(number "15")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "OUTC")
				(number "12")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "OUTD")
				(number "11")
			)
			(pin input line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "REFINCD")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD390KD"
		(extends "AD390JD")
		(property "Reference" "U"
			(at -13.97 30.48 0)
		)
		(property "Value" "AD390KD"
			(at 8.89 30.48 0)
		)
		(property "Footprint" ""
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/AD390MIL.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Quad 12bit DAC, 2LSB Gain Error, DH-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "4ch DAC 12bit"
			(at 0 0 0)
		)
	)
	(symbol "AD558KN"
		(extends "AD558JN")
		(property "Reference" "U"
			(at -8.89 17.78 0)
		)
		(property "Value" "AD558KN"
			(at 2.54 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/AD558.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Single 8-bit DAC, Internal Reference, Output Amp, Single Supply, DIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "8bit DAC Reference Single Supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
	)
	(symbol "AD558KP"
		(extends "AD558JP")
		(property "Reference" "U"
			(at -8.89 17.78 0)
		)
		(property "Value" "AD558KP"
			(at 2.54 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/AD558.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single 8-bit DAC, Internal Reference, Output Amp, Single Supply, PLCC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "8bit DAC Reference Single Supply"
			(at 0 0 0)
		)
	)
	(symbol "AD5687RBCPZ"
		(extends "AD5687BCPZ")
		(property "Reference" "U"
			(at 8.89 11.43 0)
		)
		(property "Value" "AD5687RBCPZ"
			(at 8.89 8.89 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-16-1EP_3x3mm_P0.5mm_EP1.854x1.854mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD5689R_5687R.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual, 12-Bit nanoDAC+ with 2 ppm/°C Reference, SPI Interface, LFCSP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "dac 2nch 12bit spi"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "AD5687RBRUZ"
		(extends "AD5687BRUZ")
		(property "Reference" "U"
			(at 8.89 11.43 0)
		)
		(property "Value" "AD5687RBRUZ"
			(at 8.89 8.89 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD5689R_5687R.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual, 12-Bit nanoDAC+ with 2 ppm/°C Reference, SPI Interface, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "dac 2nch 12bit spi"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "AD5689BCPZ"
		(extends "AD5687BCPZ")
		(property "Reference" "U"
			(at 8.89 11.43 0)
		)
		(property "Value" "AD5689BCPZ"
			(at 8.89 8.89 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-16-1EP_3x3mm_P0.5mm_EP1.854x1.854mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD5689_5687.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual, 16-Bit nanoDAC+ with SPI Interface, LFCSP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "dac 2nch 16bit spi"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "AD5689BRUZ"
		(extends "AD5687BRUZ")
		(property "Reference" "U"
			(at 8.89 11.43 0)
		)
		(property "Value" "AD5689BRUZ"
			(at 8.89 8.89 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD5689_5687.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual, 16-Bit nanoDAC+ with SPI Interface, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "dac 2nch 16bit spi"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "AD5689RxCPZ"
		(extends "AD5687BCPZ")
		(property "Reference" "U"
			(at 8.89 11.43 0)
		)
		(property "Value" "AD5689RxCPZ"
			(at 8.89 8.89 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-16-1EP_3x3mm_P0.5mm_EP1.854x1.854mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD5689R_5687R.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual, 16-Bit nanoDAC+ with 2 ppm/°C Reference, SPI Interface, LFCSP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "dac 2nch 16bit spi"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "AD5689RxRUZ"
		(extends "AD5687BRUZ")
		(property "Reference" "U"
			(at 8.89 11.43 0)
		)
		(property "Value" "AD5689RxRUZ"
			(at 8.89 8.89 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD5689R_5687R.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual, 16-Bit nanoDAC+ with 2 ppm/°C Reference, SPI Interface, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "dac 2nch 16bit spi"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "AD5692RxRM"
		(extends "AD5691RxRM")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "AD5692RxRM"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 33.02 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD5693R_5692R_5691R_5693.pdf"
			(at 8.89 6.35 0)
		)
		(property "Description" "Tiny, 14-Bit, I2C, nanoDAC+, 2 ppm/°C Reference, MSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "serial DAC i2c digital analog converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "AD5693RxRM"
		(extends "AD5691RxRM")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "AD5693RxRM"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 33.02 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD5693R_5692R_5691R_5693.pdf"
			(at 8.89 6.35 0)
		)
		(property "Description" "Tiny, 16-Bit, I2C, nanoDAC+, 2 ppm/°C Reference, MSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "serial DAC i2c digital analog converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "AD5791xRUZ"
		(extends "AD5781xRUZ")
		(property "Reference" "U"
			(at -10.16 15.875 0)
		)
		(property "Value" "AD5791xRUZ"
			(at -10.16 13.97 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 11.43 -13.97 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ad5791.pdf"
			(at 0 -25.4 0)
		)
		(property "Description" "1 ppm, 20-Bit, ±1 LSB INL, Voltage Output DAC, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "1ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4?6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "AD7224LN"
		(extends "AD7224KN")
		(property "Reference" "U"
			(at -13.97 22.86 0)
		)
		(property "Value" "AD7224LN"
			(at 6.35 22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/AD7224.pdf"
			(at 0 0 0)
		)
		(property "Description" "8bit DAC, Dual or Single Supply, DIP-18"
			(at 0 0 0)
		)
		(property "ki_keywords" "8bit DAC Dual Single Supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
	)
	(symbol "AD7224LP"
		(extends "AD7224KP")
		(property "Reference" "U"
			(at -13.97 22.86 0)
		)
		(property "Value" "AD7224LP"
			(at 5.08 22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/AD7224.pdf"
			(at 0 0 0)
		)
		(property "Description" "8bit DAC, Dual or Single Supply, PLCC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "8bit DAC Dual Single Supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PLCC*"
			(at 0 0 0)
		)
	)
	(symbol "AD7224LR-1"
		(extends "AD7224KR-1")
		(property "Reference" "U"
			(at -13.97 22.86 0)
		)
		(property "Value" "AD7224LR-1"
			(at 5.08 22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/AD7224.pdf"
			(at 0 0 0)
		)
		(property "Description" "8bit DAC, Dual or Single Supply, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "8bit DAC Dual Single Supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*"
			(at 0 0 0)
		)
	)
	(symbol "AD7224LR-18"
		(extends "AD7224KR-18")
		(property "Reference" "U"
			(at -13.97 22.86 0)
		)
		(property "Value" "AD7224LR-18"
			(at 5.08 22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/AD7224.pdf"
			(at 0 0 0)
		)
		(property "Description" "8bit DAC, Dual or Single Supply, SOIC-18"
			(at 0 0 0)
		)
		(property "ki_keywords" "8bit DAC Dual Single Supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*"
			(at 0 0 0)
		)
	)
	(symbol "AD7225CRS"
		(extends "AD7225BRS")
		(property "Reference" "U"
			(at -13.97 22.86 0)
		)
		(property "Value" "AD7225CRS"
			(at 7.62 22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/AD7225.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "Quad 8bit DAC, Separate Reference Voltage, SSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "8bit DAC 4CH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*"
			(at 0 0 0)
		)
	)
	(symbol "AD7225LN"
		(extends "AD7225KN")
		(property "Reference" "U"
			(at -13.97 22.86 0)
		)
		(property "Value" "AD7225LN"
			(at 7.62 22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/AD7225.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "Quad 8bit DAC, Separate Reference Voltage, PDIP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "8bit DAC 4CH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
	)
	(symbol "AD7225LP"
		(extends "AD7225KP")
		(property "Reference" "U"
			(at -13.97 22.86 0)
		)
		(property "Value" "AD7225LP"
			(at 7.62 22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/AD7225.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "Quad 8bit DAC, Separate Reference Voltage, PLCC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "8bit DAC 4CH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PLCC*"
			(at 0 0 0)
		)
	)
	(symbol "AD7225LR"
		(extends "AD7225KR")
		(property "Reference" "U"
			(at -13.97 22.86 0)
		)
		(property "Value" "AD7225LR"
			(at 7.62 22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/AD7225.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "Quad 8bit DAC, Separate Reference Voltage, SO-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "8bit DAC 4CH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*"
			(at 0 0 0)
		)
	)
	(symbol "AD7228ACN"
		(extends "AD7228ABN")
		(property "Reference" "U"
			(at -13.97 22.86 0)
		)
		(property "Value" "AD7228ACN"
			(at 7.62 22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/AD7228.pdf"
			(at 0 0 0)
		)
		(property "Description" "8bit DAC 8 Channel, Single Reference, DIP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "8bit DAC 8CH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PDIP* DIP*"
			(at 0 0 0)
		)
	)
	(symbol "AD7228ACP"
		(extends "AD7228ABP")
		(property "Reference" "U"
			(at -13.97 22.86 0)
		)
		(property "Value" "AD7228ACP"
			(at 7.62 22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/AD7228.pdf"
			(at 0 0 0)
		)
		(property "Description" "8bit DAC 8 Channel, Single Reference, PLCC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "8bit DAC 8CH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PLCC*"
			(at 0 0 0)
		)
	)
	(symbol "AD7228ACR"
		(extends "AD7228ABR")
		(property "Reference" "U"
			(at -13.97 22.86 0)
		)
		(property "Value" "AD7228ACR"
			(at 7.62 22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/AD7228.pdf"
			(at 0 0 0)
		)
		(property "Description" "8bit DAC 8 Channel, Single Reference, SOIC-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "8bit DAC 8CH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*"
			(at 0 0 0)
		)
	)
	(symbol "AD7391"
		(extends "AD7390")
		(property "Reference" "U"
			(at 1.27 10.795 0)
		)
		(property "Value" "AD7391"
			(at 1.27 8.89 0)
		)
		(property "Footprint" ""
			(at 22.86 -2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD7390_7391.pdf"
			(at 22.86 -2.54 0)
		)
		(property "Description" "Serial-Input Micropower 10-Bit DAC, DIP-8/SOIC-8/TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SPI 10 bit DAC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm* TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "AD7533KN"
		(extends "AD7533JN")
		(property "Reference" "U"
			(at -11.43 17.78 0)
		)
		(property "Value" "AD7533KN"
			(at 3.81 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/AD7533.pdf"
			(at 0 0 0)
		)
		(property "Description" "10bit Multiplying DAC, 1 Channel, DIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "10bit DAC 1CH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
	)
	(symbol "AD7533KP"
		(extends "AD7533JP")
		(property "Reference" "U"
			(at -11.43 17.78 0)
		)
		(property "Value" "AD7533KP"
			(at 3.81 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/AD7533.pdf"
			(at 0 0 0)
		)
		(property "Description" "10bit Multiplying DAC, 1 Channel, PLCC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "10bit DAC 1CH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PLCC*"
			(at 0 0 0)
		)
	)
	(symbol "AD7533LN"
		(extends "AD7533JN")
		(property "Reference" "U"
			(at -11.43 17.78 0)
		)
		(property "Value" "AD7533LN"
			(at 3.81 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/AD7533.pdf"
			(at 0 0 0)
		)
		(property "Description" "10bit Multiplying DAC, 1 Channel, DIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "10bit DAC 1CH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
	)
	(symbol "DAC0808_DIP"
		(extends "MC1408_DIP")
		(property "Reference" "U"
			(at 2.54 16.51 0)
		)
		(property "Value" "DAC0808_DIP"
			(at 2.54 13.97 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/dac0808.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit multiplying DAC"
			(at 0 0 0)
		)
		(property "ki_keywords" "8 bit multiplying DAC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "DAC0808_SOIC"
		(extends "MC1408_SOIC")
		(property "Reference" "U"
			(at 2.54 16.51 0)
		)
		(property "Value" "DAC0808_SOIC"
			(at 2.54 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/dac0808.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit multiplying DAC"
			(at 0 0 0)
		)
		(property "ki_keywords" "8 bit multiplying DAC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "DAC1006LCN"
		(extends "DAC1007LCN")
		(property "Reference" "U"
			(at -24.765 26.67 0)
		)
		(property "Value" "DAC1006LCN"
			(at 19.685 26.67 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at 5.08 -2.54 0)
		)
		(property "Datasheet" "https://pdf.datasheetcatalog.com/datasheets/400/195351_DS.pdf"
			(at 35.56 -2.54 0)
		)
		(property "Description" "Double-Buffered D to A Converters, DIP-20"
			(at 7.62 -2.54 0)
		)
		(property "ki_keywords" "DAC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "DAC1006LCWM"
		(extends "DAC1007LCN")
		(property "Reference" "U"
			(at -24.765 26.67 0)
		)
		(property "Value" "DAC1006LCWM"
			(at 19.685 26.67 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 5.08 -2.54 0)
		)
		(property "Datasheet" "https://pdf.datasheetcatalog.com/datasheets/400/195351_DS.pdf"
			(at 35.56 -2.54 0)
		)
		(property "Description" "Double-Buffered D to A Converters, DIP-20"
			(at 7.62 -2.54 0)
		)
		(property "ki_keywords" "DAC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*W_7.5x12.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "DAC1008LCN"
		(extends "DAC1007LCN")
		(property "Reference" "U"
			(at -24.765 26.67 0)
		)
		(property "Value" "DAC1008LCN"
			(at 19.685 26.67 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at 5.08 -2.54 0)
		)
		(property "Datasheet" "https://pdf.datasheetcatalog.com/datasheets/400/195351_DS.pdf"
			(at 35.56 -2.54 0)
		)
		(property "Description" "Double-Buffered D to A Converters, DIP-20"
			(at 7.62 -2.54 0)
		)
		(property "ki_keywords" "DAC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "DAC101C081CIMK"
		(extends "DAC081C081CIMK")
		(property "Reference" "U"
			(at 2.54 8.89 0)
		)
		(property "Value" "DAC101C081CIMK"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 16.51 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/dac101c081.pdf"
			(at 0 0 0)
		)
		(property "Description" "10-bit Micropower DAC with I2C-Compatible Interface, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C DAC 10-bit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "DAC121C081CIMK"
		(extends "DAC081C081CIMK")
		(property "Reference" "U"
			(at 2.54 8.89 0)
		)
		(property "Value" "DAC121C081CIMK"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 16.51 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/dac121c081.pdf"
			(at 0 0 0)
		)
		(property "Description" "12-bit Micropower DAC with I2C-Compatible Interface, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C DAC 12-bit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "DAC60502"
		(extends "DAC80502")
		(property "Reference" "U"
			(at -10.16 16.51 0)
		)
		(property "Value" "DAC60502"
			(at 7.62 16.51 0)
		)
		(property "Footprint" "Package_SON:Texas_DRX_WSON-10_2.5x2.5mm_P0.5mm"
			(at 5.08 -27.94 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/dac80502.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "12-bit dual-channel voltage output DAC, 2.5V 5ppm/°C internal reference, WSON-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "texas digital-analog converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*2.5x2.5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "DAC60504"
		(extends "DAC80504")
		(property "Reference" "U"
			(at -12.192 16.51 0)
		)
		(property "Value" "DAC60504"
			(at 10.922 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RTE0016D_WQFN-16-1EP_3x3mm_P0.5mm_EP0.8x0.8mm_ThermalVias"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/dac60504"
			(at 0 0 0)
		)
		(property "Description" "12-bit quad-channel voltage output DAC, 2.5V 2ppm/°C internal reference, WQFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "texas quad digital-analog converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RTE0016D*WQFN*16*EP0.8x0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "DAC6311xDCK"
		(extends "DAC5311xDCK")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "DAC6311xDCK"
			(at 7.62 -11.43 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/dac5311.pdf"
			(at 0 0 0)
		)
		(property "Description" "10-Bit, Single-Channel, Voltage Output, Serial Interface Digital-to-Analog Converters, SC-70"
			(at 0 0 0)
		)
		(property "ki_keywords" "DAC SPI 1-channel"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "DAC6578xPW"
		(extends "DAC5578xPW")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "DAC6578xPW"
			(at 7.62 13.97 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/dac5578.pdf"
			(at 0 0 0)
		)
		(property "Description" "10-Bit, Octal-Channel, Ultra-Low Glitch, Voltage Output, Two-Wire Interface Digital-to-Analog Converters, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "DAC I2C TWI 8-channel"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "DAC6578xRGE"
		(extends "DAC5578xRGE")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "DAC6578xRGE"
			(at 7.62 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.7x2.7mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/dac5578.pdf"
			(at 0 0 0)
		)
		(property "Description" "10-Bit, Octal-Channel, Ultra-Low Glitch, Voltage Output, Two-Wire Interface Digital-to-Analog Converters, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "DAC I2C TWI 8-channel"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "DAC70502"
		(extends "DAC80502")
		(property "Reference" "U"
			(at -10.16 16.51 0)
		)
		(property "Value" "DAC70502"
			(at 7.62 16.51 0)
		)
		(property "Footprint" "Package_SON:Texas_DRX_WSON-10_2.5x2.5mm_P0.5mm"
			(at 5.08 -27.94 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/dac80502.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "14-bit dual-channel voltage output DAC, 2.5V 5ppm/°C internal reference, WSON-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "texas digital-analog converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*2.5x2.5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "DAC70504"
		(extends "DAC80504")
		(property "Reference" "U"
			(at -12.192 16.51 0)
		)
		(property "Value" "DAC70504"
			(at 10.922 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RTE0016D_WQFN-16-1EP_3x3mm_P0.5mm_EP0.8x0.8mm_ThermalVias"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/dac70504"
			(at 0 0 0)
		)
		(property "Description" "14-bit quad-channel voltage output DAC, 2.5V 2ppm/°C internal reference, WQFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "texas quad digital-analog converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RTE0016D*WQFN*16*EP0.8x0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "DAC7311xDCK"
		(extends "DAC5311xDCK")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "DAC7311xDCK"
			(at 7.62 -11.43 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/dac5311.pdf"
			(at 0 0 0)
		)
		(property "Description" "12-Bit, Single-Channel, Voltage Output, Serial Interface Digital-to-Analog Converters, SC-70"
			(at 0 0 0)
		)
		(property "ki_keywords" "DAC SPI 1-channel"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "DAC7565"
		(extends "DAC8165")
		(property "Reference" "U"
			(at -8.89 21.59 0)
		)
		(property "Value" "DAC7565"
			(at 10.16 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at -22.86 -17.78 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/dac7565.pdf"
			(at -25.4 -17.78 0)
		)
		(property "Description" "12-bit quad-channel voltage output DAC with 2.5V internal reference"
			(at 0 0 0)
		)
		(property "ki_keywords" "12-bit quad DAC voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "DAC7578xPW"
		(extends "DAC5578xPW")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "DAC7578xPW"
			(at 7.62 13.97 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/dac5578.pdf"
			(at 0 0 0)
		)
		(property "Description" "12-Bit, Octal-Channel, Ultra-Low Glitch, Voltage Output, Two-Wire Interface Digital-to-Analog Converters, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "DAC I2C TWI 8-channel"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "DAC7578xRGE"
		(extends "DAC5578xRGE")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "DAC7578xRGE"
			(at 7.62 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.7x2.7mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/dac5578.pdf"
			(at 0 0 0)
		)
		(property "Description" "12-Bit, Octal-Channel, Ultra-Low Glitch, Voltage Output, Two-Wire Interface Digital-to-Analog Converters, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "DAC I2C TWI 8-channel"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "DAC7750xRHA"
		(extends "DAC8750xRHA")
		(property "Reference" "U"
			(at -8.89 19.05 0)
		)
		(property "Value" "DAC7750xRHA"
			(at 3.81 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHA_VQFN-40-1EP_6x6mm_P0.5mm_EP4.6x4.6mm_ThermalVias"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/dac7750.pdf"
			(at 0 -17.78 0)
		)
		(property "Description" "Single-Channel, 12bit Programmable Current Output DAC for 4-mA to 20-mA Current Loop Applications, VQFN-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "DAC Current Loop 20mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RHA*EP4.6x4.6mm*"
			(at 0 0 0)
		)
	)
	(symbol "DAC8531E"
		(extends "DAC8501E")
		(property "Reference" "U"
			(at 6.35 8.89 0)
		)
		(property "Value" "DAC8531E"
			(at 8.89 -8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 2.54 -12.7 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/dac8531.pdf"
			(at 2.54 -15.24 0)
		)
		(property "Description" "16-bit DAC, Voltage Output, Rail-to-Rail Output, SPI interface, MSOP-8 3x3mm package"
			(at 0 0 0)
		)
		(property "ki_keywords" "DAC 16-Bit  Voltage Output Rail-to-Rail SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm?P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "DAC8531IDRB"
		(extends "DAC8501E")
		(property "Reference" "U"
			(at 6.35 8.89 0)
		)
		(property "Value" "DAC8531IDRB"
			(at 8.89 -8.89 0)
		)
		(property "Footprint" "Package_SON:VSON-8-1EP_3x3mm_P0.65mm_EP1.65x2.4mm"
			(at 2.54 -12.7 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/dac8531.pdf"
			(at 2.54 -15.24 0)
		)
		(property "Description" "16-bit DAC, Voltage Output, Rail-to-Rail Output, SPI interface, VSON-8 3x3mm package"
			(at 0 0 0)
		)
		(property "ki_keywords" "DAC 16-Bit  Voltage Output Rail-to-Rail SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSON*3x3mm?P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "DAC8550IxDGK"
		(extends "DAC8501E")
		(property "Reference" "U"
			(at 6.35 8.89 0)
		)
		(property "Value" "DAC8550IxDGK"
			(at 8.89 -8.89 0)
		)
		(property "Footprint" "Package_SON:VSON-8-1EP_3x3mm_P0.65mm_EP1.65x2.4mm"
			(at 2.54 -12.7 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/dac8550.pdf"
			(at 2.54 -15.24 0)
		)
		(property "Description" "16-bit DAC, Voltage Output, Ultra-Low Glitch, Rail-to-Rail Output, SPI interface, VSON-8 3x3mm package"
			(at 0 0 0)
		)
		(property "ki_keywords" "DAC 16-Bit  Voltage Output Rail-to-Rail SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSON*3x3mm?P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "DAC8551IxDGK"
		(extends "DAC8501E")
		(property "Reference" "U"
			(at 6.35 8.89 0)
		)
		(property "Value" "DAC8551IxDGK"
			(at 8.89 -8.89 0)
		)
		(property "Footprint" "Package_SON:VSON-8-1EP_3x3mm_P0.65mm_EP1.65x2.4mm"
			(at 2.54 -12.7 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/dac8551.pdf"
			(at 2.54 -15.24 0)
		)
		(property "Description" "16-bit DAC, Voltage Output, Ultralow-Glitch, Rail-to-Rail Output, SPI interface, VSON-8 3x3mm package"
			(at 0 0 0)
		)
		(property "ki_keywords" "DAC 16-Bit  Voltage Output Rail-to-Rail SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSON*3x3mm?P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "DAC8565"
		(extends "DAC8165")
		(property "Reference" "U"
			(at -8.89 21.59 0)
		)
		(property "Value" "DAC8565"
			(at 10.16 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at -22.86 -17.78 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/dac8565.pdf"
			(at -25.4 -17.78 0)
		)
		(property "Description" "16-bit quad-channel voltage output DAC with 2.5V internal reference"
			(at 0 0 0)
		)
		(property "ki_keywords" "16-bit quad DAC voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC1446L"
		(extends "LTC1446")
		(property "Reference" "U"
			(at -2.54 10.795 0)
		)
		(property "Value" "LTC1446L"
			(at -2.54 8.89 0)
		)
		(property "Footprint" ""
			(at 20.32 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1446fa.pdf"
			(at 20.32 -7.62 0)
		)
		(property "Description" "2-Channel 12-Bit Rail-To-Rail D/A Converters with SPI Interface and Internal Reference (2.500V)"
			(at 0 0 0)
		)
		(property "ki_keywords" "12-Bit DAC SPI 2ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC1664CN"
		(extends "LTC1664CGN")
		(property "Reference" "U"
			(at -8.89 12.7 0)
		)
		(property "Value" "LTC1664CN"
			(at 2.54 12.7 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1664fa.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad Micropower 10-bit DAC, Standard, DIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Quad DAC Micropower 10bit 4ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SSOP*"
			(at 0 0 0)
		)
	)
	(symbol "LTC1664IGN"
		(extends "LTC1664CGN")
		(property "Reference" "U"
			(at -8.89 12.7 0)
		)
		(property "Value" "LTC1664IGN"
			(at 2.54 12.7 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1664fa.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad Micropower 10-bit DAC, Industrial, SSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Quad DAC Micropower 10bit 4ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SSOP*"
			(at 0 0 0)
		)
	)
	(symbol "LTC1664IN"
		(extends "LTC1664CGN")
		(property "Reference" "U"
			(at -8.89 12.7 0)
		)
		(property "Value" "LTC1664IN"
			(at 2.54 12.7 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1664fa.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad Micropower 10-bit DAC, Industrial, DIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Quad DAC Micropower 10bit 4ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SSOP*"
			(at 0 0 0)
		)
	)
	(symbol "MAX5138"
		(extends "MAX5139")
		(property "Reference" "U"
			(at 8.89 17.145 0)
		)
		(property "Value" "MAX5138"
			(at 8.89 15.24 0)
		)
		(property "Footprint" "Package_DFN_QFN:TQFN-16-1EP_3x3mm_P0.5mm_EP1.23x1.23mm"
			(at 8.89 12.7 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX5138-MAX5139.pdf"
			(at 8.89 10.16 0)
		)
		(property "Description" "Low-Power, Single, 16-Bit, Buffered Voltage-Output DAC"
			(at 0 0 0)
		)
		(property "ki_keywords" "16-bit DAC 1CH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX5217"
		(extends "MAX5215")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "MAX5217"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 33.02 -8.89 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX5215-MAX5217.pdf"
			(at 8.89 6.35 0)
		)
		(property "Description" "Digital to analog, 16 Bit, 1 ch, 2.7 - 5.5 VDD, I2C, uMAX-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "DA 16 Bit 1 ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX5719xSD"
		(extends "MAX5717xSD")
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "MAX5719xSD"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX5717-MAX5719.pdf"
			(at 0 0 0)
		)
		(property "Description" "20-bit Voltage Digital-to-Analog converter, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "DAC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX5814"
		(extends "MAX5813")
		(property "Reference" "U"
			(at -8.89 11.43 0)
		)
		(property "Value" "MAX5814"
			(at 8.89 11.43 0)
		)
		(property "Footprint" ""
			(at 11.43 1.27 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX5813-MAX5815.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "Digital to analog, 10 Bit, 4 ch, 2.7 - 5.5 VDD, I2C, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "DA 10 Bit 4 ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TSSOP*14*4.4*"
			(at 0 0 0)
		)
	)
	(symbol "MAX5814WLP"
		(extends "MAX5813WLP")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "MAX5814WLP"
			(at 8.89 8.89 0)
		)
		(property "Footprint" ""
			(at 11.43 -1.27 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX5813-MAX5815.pdf"
			(at 1.27 -2.54 0)
		)
		(property "Description" "Digital to analog, 10 Bit, 4 ch, 2.7 - 5.5 VDD, I2C, TSSOP-14, Maxim_WLP-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "DA 10 Bit 4 ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Maxim*WLP*12*"
			(at 0 0 0)
		)
	)
	(symbol "MAX5815"
		(extends "MAX5813")
		(property "Reference" "U"
			(at -8.89 11.43 0)
		)
		(property "Value" "MAX5815"
			(at 8.89 11.43 0)
		)
		(property "Footprint" ""
			(at 11.43 1.27 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX5813-MAX5815.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "Digital to analog, 12 Bit, 4 ch, 2.7 - 5.5 VDD, I2C, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "DA 12 Bit 4 ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TSSOP*14*4.4*"
			(at 0 0 0)
		)
	)
	(symbol "MAX5815WLP"
		(extends "MAX5813WLP")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "MAX5815WLP"
			(at 8.89 8.89 0)
		)
		(property "Footprint" ""
			(at 11.43 -1.27 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX5813-MAX5815.pdf"
			(at 1.27 -2.54 0)
		)
		(property "Description" "Digital to analog, 12 Bit, 4 ch, 2.7 - 5.5 VDD, I2C, TSSOP-14, Maxim_WLP-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "DA 12 Bit 4 ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Maxim*WLP*12*"
			(at 0 0 0)
		)
	)
	(symbol "MCP4811"
		(extends "MCP4801")
		(property "Reference" "U"
			(at 1.27 10.795 0)
		)
		(property "Value" "MCP4811"
			(at 1.27 8.89 0)
		)
		(property "Footprint" ""
			(at 22.86 -2.54 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22244B.pdf"
			(at 22.86 -2.54 0)
		)
		(property "Description" "10-Bit D/A Converters with SPI Interface, internal Reference (2.048V)"
			(at 0 0 0)
		)
		(property "ki_keywords" "10-Bit DAC SPI Reference 1ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* MSOP*3x3mm*P0.65mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP4811-EMC"
		(extends "MCP4801-EMC")
		(property "Reference" "U"
			(at 1.27 10.795 0)
		)
		(property "Value" "MCP4811-EMC"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.75x1.45mm"
			(at 0 -11.938 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22244B.pdf"
			(at 22.86 -2.54 0)
		)
		(property "Description" "10-Bit D/A Converters with SPI Interface, internal Reference (2.048V)"
			(at 0 0 0)
		)
		(property "ki_keywords" "10-Bit DAC SPI Reference 1ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP4812"
		(extends "MCP4802")
		(property "Reference" "U"
			(at -2.54 10.795 0)
		)
		(property "Value" "MCP4812"
			(at -2.54 8.89 0)
		)
		(property "Footprint" ""
			(at 20.32 -7.62 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002249B.pdf"
			(at 20.32 -7.62 0)
		)
		(property "Description" "2-Channel 10-Bit D/A Converters with SPI Interface and Internal Reference (2.048V)"
			(at 0 0 0)
		)
		(property "ki_keywords" "10-Bit DAC SPI Reference 2ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm* MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP4821"
		(extends "MCP4801")
		(property "Reference" "U"
			(at 1.27 10.795 0)
		)
		(property "Value" "MCP4821"
			(at 1.27 8.89 0)
		)
		(property "Footprint" ""
			(at 22.86 -2.54 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22244B.pdf"
			(at 22.86 -2.54 0)
		)
		(property "Description" "12-Bit D/A Converters with SPI Interface, internal Reference (2.048V)"
			(at 0 0 0)
		)
		(property "ki_keywords" "12-Bit DAC SPI Reference 1ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* MSOP*3x3mm*P0.65mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP4821-EMC"
		(extends "MCP4801-EMC")
		(property "Reference" "U"
			(at 1.27 10.795 0)
		)
		(property "Value" "MCP4821-EMC"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.75x1.45mm"
			(at 0 -11.938 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22244B.pdf"
			(at 22.86 -2.54 0)
		)
		(property "Description" "12-Bit D/A Converters with SPI Interface, internal Reference (2.048V)"
			(at 0 0 0)
		)
		(property "ki_keywords" "12-Bit DAC SPI Reference 1ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP4822"
		(extends "MCP4802")
		(property "Reference" "U"
			(at -2.54 10.795 0)
		)
		(property "Value" "MCP4822"
			(at -2.54 8.89 0)
		)
		(property "Footprint" ""
			(at 20.32 -7.62 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002249B.pdf"
			(at 20.32 -7.62 0)
		)
		(property "Description" "2-Channel 12-Bit D/A Converters with SPI Interface and Internal Reference (2.048V)"
			(at 0 0 0)
		)
		(property "ki_keywords" "12-Bit DAC SPI Reference 2ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm* MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP4911"
		(extends "MCP4901")
		(property "Reference" "U"
			(at 6.35 10.795 0)
		)
		(property "Value" "MCP4911"
			(at 6.35 8.89 0)
		)
		(property "Footprint" ""
			(at 25.4 -2.54 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22248a.pdf"
			(at 25.4 -2.54 0)
		)
		(property "Description" "10-Bit D/A Converters with SPI Interface"
			(at 0 0 0)
		)
		(property "ki_keywords" "10-Bit DAC SPI 1ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* MSOP*3x3mm*P0.65mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP4911-EMC"
		(extends "MCP4901-EMC")
		(property "Reference" "U"
			(at 6.35 10.795 0)
		)
		(property "Value" "MCP4911-EMC"
			(at 6.35 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.75x1.45mm"
			(at 0 -12.192 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22248a.pdf"
			(at 25.4 -2.54 0)
		)
		(property "Description" "10-Bit D/A Converters with SPI Interface"
			(at 0 0 0)
		)
		(property "ki_keywords" "10-Bit DAC SPI  1ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP4912"
		(extends "MCP4902")
		(property "Reference" "U"
			(at -1.905 10.795 0)
		)
		(property "Value" "MCP4912"
			(at -1.905 8.89 0)
		)
		(property "Footprint" ""
			(at 20.32 -7.62 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22250A.pdf"
			(at 20.32 -7.62 0)
		)
		(property "Description" "2-Channel 10-Bit D/A Converters with SPI Interface"
			(at 0 0 0)
		)
		(property "ki_keywords" "10-Bit DAC SPI 2ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x8.7mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP4921"
		(extends "MCP4901")
		(property "Reference" "U"
			(at 6.35 10.795 0)
		)
		(property "Value" "MCP4921"
			(at 6.35 8.89 0)
		)
		(property "Footprint" ""
			(at 25.4 -2.54 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22248a.pdf"
			(at 25.4 -2.54 0)
		)
		(property "Description" "12-Bit D/A Converters with SPI Interface"
			(at 0 0 0)
		)
		(property "ki_keywords" "12-Bit DAC SPI 1ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* MSOP*3x3mm*P0.65mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP4921-EMC"
		(extends "MCP4901-EMC")
		(property "Reference" "U"
			(at 6.35 10.795 0)
		)
		(property "Value" "MCP4921-EMC"
			(at 6.35 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.75x1.45mm"
			(at 0 -12.192 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22248a.pdf"
			(at 25.4 -2.54 0)
		)
		(property "Description" "12-Bit D/A Converters with SPI Interface"
			(at 0 0 0)
		)
		(property "ki_keywords" "12-Bit DAC SPI  1ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP4921-EP"
		(extends "MCP4921-EMS")
		(property "Reference" "U"
			(at -11.43 7.62 0)
		)
		(property "Value" "MCP4921-EP"
			(at 0 7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/21897a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single 12-bit Digital to Analog Converter, SPI Interface, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single DAC 1ch 12bit SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP* SOIC* DIP* PDIP*"
			(at 0 0 0)
		)
	)
	(symbol "MCP4921-ESN"
		(extends "MCP4921-EMS")
		(property "Reference" "U"
			(at -11.43 7.62 0)
		)
		(property "Value" "MCP4921-ESN"
			(at 0 7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/21897a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single 12-bit Digital to Analog Converter, SPI Interface, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single DAC 1ch 12bit SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP* SOIC* DIP* PDIP*"
			(at 0 0 0)
		)
	)
	(symbol "MCP4922"
		(extends "MCP4902")
		(property "Reference" "U"
			(at -1.905 10.795 0)
		)
		(property "Value" "MCP4922"
			(at -1.905 8.89 0)
		)
		(property "Footprint" ""
			(at 20.32 -7.62 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22250A.pdf"
			(at 20.32 -7.62 0)
		)
		(property "Description" "2-Channel 12-Bit D/A Converters with SPI Interface"
			(at 0 0 0)
		)
		(property "ki_keywords" "12-Bit DAC SPI 2CH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x8.7mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP4922-ESL"
		(extends "MCP4922-EP")
		(property "Reference" "U"
			(at -10.16 10.16 0)
		)
		(property "Value" "MCP4922-ESL"
			(at 3.81 10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/21897a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual 12-bit Digital to Analog Converter, SPI Interface, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual DAC 1ch 12bit SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SO* SOIC* TSSOP*"
			(at 0 0 0)
		)
	)
	(symbol "MCP4922-EST"
		(extends "MCP4922-EP")
		(property "Reference" "U"
			(at -10.16 10.16 0)
		)
		(property "Value" "MCP4922-EST"
			(at 3.81 10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/21897a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual 12-bit Digital to Analog Converter, SPI Interface, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual DAC 1ch 12bit SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SO* SOIC* TSSOP*"
			(at 0 0 0)
		)
	)
	(symbol "TLV5627CPW"
		(extends "TLV5627CD")
		(property "Reference" "U"
			(at -13.97 12.7 0)
		)
		(property "Value" "TLV5627CPW"
			(at 6.35 12.7 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv5627.pdf"
			(at 0 0 0)
		)
		(property "Description" "4-Channel DAC, 8bit, w/ Power Down, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "DAC 4CH 8bit"
			(at 0 0 0)
		)
	)
)
