(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "ADG1408YRUZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 23.495 0)
		)
		(property "Value" "ADG1408YRUZ"
			(at -7.62 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at -19.05 -24.13 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADG1408_1409.pdf"
			(at 0.254 0 0)
		)
		(property "Description" "8-channel iCMOS analog multiplexer, 4.7 Ohm Ron, 60 MHz, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "analog switch  multiplexer SP8T"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADG1408YRUZ_0_0"
			(pin power_in line
				(at 5.08 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "14")
			)
		)
		(symbol "ADG1408YRUZ_0_1")
		(symbol "ADG1408YRUZ_1_1"
			(pin input line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "A0")
				(number "1")
			)
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "A1")
				(number "16")
			)
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "A2")
				(number "15")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "EN")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "S1")
				(number "4")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "S2")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "S3")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "S4")
				(number "7")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "S5")
				(number "12")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "S6")
				(number "11")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "S7")
				(number "10")
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "S8")
				(number "9")
			)
			(pin power_in line
				(at 5.08 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "13")
			)
			(pin power_in line
				(at 7.62 -20.32 90)
				(length 2.54)
				(name "VSS")
				(number "3")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "D")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADG1414BRU"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 21.59 0)
		)
		(property "Value" "ADG1414BRU"
			(at 11.43 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-24_4.4x7.8mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADG1414.pdf"
			(at 0 0 0)
		)
		(property "Description" "±15V, +12V, ±5V, 9.5 Ohm on resistance, iCMOS Serially-Controlled Octal SPST Switches, TSSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "SPI SPST Analog Switches"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x7.8mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADG1414BRU_1_0"
			(text "SHIFT REGISTER"
				(at 0 -6.35 0)
			)
		)
		(symbol "ADG1414BRU_1_1"
			(pin passive line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "S1")
				(number "5")
			)
			(pin passive line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "S2")
				(number "7")
			)
			(pin passive line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "S3")
				(number "9")
			)
			(pin passive line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "S4")
				(number "11")
			)
			(pin passive line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "S5")
				(number "14")
			)
			(pin passive line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "S6")
				(number "16")
			)
			(pin passive line
				(at -20.32 0 0)
				(length 2.54)
				(name "S7")
				(number "18")
			)
			(pin passive line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "S8")
				(number "20")
			)
			(pin input line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "DIN")
				(number "3")
			)
			(pin input line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "~{SYNC}")
				(number "24")
			)
			(pin input line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "SCLK")
				(number "1")
			)
			(pin open_collector line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "SDO")
				(number "22")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 2.54)
				(name "VL")
				(number "23")
			)
			(pin power_in line
				(at -2.54 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "21")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 2.54 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "D1")
				(number "6")
			)
			(pin passive line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "D2")
				(number "8")
			)
			(pin passive line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "D3")
				(number "10")
			)
			(pin passive line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "D4")
				(number "12")
			)
			(pin passive line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "D5")
				(number "13")
			)
			(pin passive line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "D6")
				(number "15")
			)
			(pin passive line
				(at 20.32 0 180)
				(length 2.54)
				(name "D7")
				(number "17")
			)
			(pin passive line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "D8")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADG1607xCP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 34.29 0)
		)
		(property "Value" "ADG1607xCP"
			(at -3.81 31.75 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 5.08 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADG1606_1607.pdf"
			(at 5.08 -5.08 0)
		)
		(property "Description" "Differential 8-channel ±5V, +12V, +5V, and +3.3V iCMOS analog multiplexer, 4.5 Ohm Ron, 37 MHz, LFCSP-32 5x5mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "analog switch multiplexer DP8T"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ADG1607xCP_0_0"
			(pin power_in line
				(at 5.08 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
		)
		(symbol "ADG1607xCP_0_1")
		(symbol "ADG1607xCP_1_1"
			(pin input line
				(at -10.16 27.94 0)
				(length 2.54)
				(name "A0")
				(number "15")
			)
			(pin input line
				(at -10.16 25.4 0)
				(length 2.54)
				(name "A1")
				(number "14")
			)
			(pin input line
				(at -10.16 22.86 0)
				(length 2.54)
				(name "A2")
				(number "10")
			)
			(pin input line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "EN")
				(number "16")
			)
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "S1A")
				(number "17")
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "S2A")
				(number "18")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "S3A")
				(number "19")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "S4A")
				(number "20")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "S5A")
				(number "21")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "S6A")
				(number "22")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "S7A")
				(number "23")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "S8A")
				(number "24")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "S1B")
				(number "8")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "S2B")
				(number "7")
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "S3B")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "S4B")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 -20.32 0)
				(length 2.54)
				(name "S5B")
				(number "4")
			)
			(pin bidirectional line
				(at -10.16 -22.86 0)
				(length 2.54)
				(name "S6B")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 -25.4 0)
				(length 2.54)
				(name "S7B")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 -27.94 0)
				(length 2.54)
				(name "S8B")
				(number "1")
			)
			(pin power_in line
				(at 5.08 33.02 270)
				(length 2.54)
				(name "V_{DD}")
				(number "29")
			)
			(pin power_in line
				(at 7.62 -33.02 90)
				(length 2.54)
				(name "V_{SS}")
				(number "25")
			)
			(pin passive line
				(at 7.62 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "V_{SS}")
				(number "33")
			)
			(pin no_connect line
				(at 10.16 20.32 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin no_connect line
				(at 10.16 17.78 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin no_connect line
				(at 10.16 15.24 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at 10.16 12.7 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "26")
			)
			(pin no_connect line
				(at 10.16 10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "28")
			)
			(pin no_connect line
				(at 10.16 7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "30")
			)
			(pin no_connect line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "32")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "DA")
				(number "27")
			)
			(pin bidirectional line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "DB")
				(number "31")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADG419BRM"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 7.239 0)
		)
		(property "Value" "ADG419BRM"
			(at -3.175 5.461 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 3.81 -14.605 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADG419.pdf"
			(at 3.81 -12.065 0)
		)
		(property "Description" "Single SPDT Monolithic LC²MOS Analog Switch, 25Ohm Ron, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADG419BRM_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(symbol "ADG419BRM_2_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VL")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "7")
			)
		)
		(symbol "ADG419BRM_2_1")
		(embedded_fonts no)
	)
	(symbol "ADG633YCP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 7.874 0)
		)
		(property "Value" "ADG633YCP"
			(at -3.175 6.096 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-16-1EP_4x4mm_P0.65mm_EP2.1x2.1mm"
			(at 6.35 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/adg633.pdf"
			(at 6.35 -6.35 0)
		)
		(property "Description" "Triple SPDT CMOS Analog Switch, 52Ohm Ron, LFCSP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*4x4mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADG633YCP_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "11")
			)
		)
		(symbol "ADG633YCP_2_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "13")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "16")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "15")
			)
		)
		(symbol "ADG633YCP_3_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "ADG633YCP_4_0"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "~{EN}")
				(number "4")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 5.08 -12.7 90)
				(length 2.54)
				(name "EP")
				(number "17")
			)
		)
		(symbol "ADG633YCP_4_1")
		(embedded_fonts no)
	)
	(symbol "ADG633YRU"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 7.874 0)
		)
		(property "Value" "ADG633YRU"
			(at -3.175 6.096 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 5.08 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADG633.pdf"
			(at 5.08 -7.62 0)
		)
		(property "Description" "Triple SPDT CMOS Analog Switch, 52Ohm Ron, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADG633YRU_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "14")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "13")
			)
		)
		(symbol "ADG633YRU_2_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "15")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "ADG633YRU_3_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(symbol "ADG633YRU_4_0"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "~{EN}")
				(number "6")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
		)
		(symbol "ADG633YRU_4_1")
		(embedded_fonts no)
	)
	(symbol "ADG658YCP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 23.495 0)
		)
		(property "Value" "ADG658YCP"
			(at -7.62 21.59 0)
		)
		(property "Footprint" "Package_CSP:Analog_LFCSP-16-1EP_4x4mm_P0.65mm_EP2.1x2.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADG658_659.pdf"
			(at 0.254 0 0)
		)
		(property "Description" "8-channel iCMOS analog multiplexer, 45 Ohm Ron, 210 MHz, LFCSP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "analog switch multiplexer SP8T"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*LFCSP*1EP*4x4mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADG658YCP_0_0"
			(pin power_in line
				(at 5.08 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
		)
		(symbol "ADG658YCP_0_1")
		(symbol "ADG658YCP_1_1"
			(pin input line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "A0")
				(number "9")
			)
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "A1")
				(number "8")
			)
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "A2")
				(number "7")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "~{EN}")
				(number "4")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "S1")
				(number "11")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "S2")
				(number "12")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "S3")
				(number "13")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "S4")
				(number "10")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "S5")
				(number "15")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "S6")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "S7")
				(number "16")
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "S8")
				(number "2")
			)
			(pin no_connect line
				(at 2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "EPAD")
				(number "17")
			)
			(pin power_in line
				(at 5.08 22.86 270)
				(length 2.54)
				(name "V_{DD}")
				(number "14")
			)
			(pin power_in line
				(at 7.62 -20.32 90)
				(length 2.54)
				(name "V_{SS}")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "D")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADG707BRU"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 34.29 0)
		)
		(property "Value" "ADG707BRU"
			(at -7.62 31.75 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at -22.86 7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADG706_707.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Differential 8-to-1 Multiplexer, 2.5 Ohm Ron, 36Mhz, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "analog switch selector differencial multiplexer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADG707BRU_0_1")
		(symbol "ADG707BRU_1_1"
			(pin input line
				(at -10.16 27.94 0)
				(length 2.54)
				(name "A0")
				(number "17")
			)
			(pin input line
				(at -10.16 25.4 0)
				(length 2.54)
				(name "A1")
				(number "16")
			)
			(pin input line
				(at -10.16 22.86 0)
				(length 2.54)
				(name "A2")
				(number "15")
			)
			(pin input line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "EN")
				(number "18")
			)
			(pin passive line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "S1A")
				(number "19")
			)
			(pin passive line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "S2A")
				(number "20")
			)
			(pin passive line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "S3A")
				(number "21")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "S4A")
				(number "22")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "S5A")
				(number "23")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "S6A")
				(number "24")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "S7A")
				(number "25")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "S8A")
				(number "26")
			)
			(pin passive line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "S1B")
				(number "11")
			)
			(pin passive line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "S2B")
				(number "10")
			)
			(pin passive line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "S3B")
				(number "9")
			)
			(pin passive line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "S4B")
				(number "8")
			)
			(pin passive line
				(at -10.16 -20.32 0)
				(length 2.54)
				(name "S5B")
				(number "7")
			)
			(pin passive line
				(at -10.16 -22.86 0)
				(length 2.54)
				(name "S6B")
				(number "6")
			)
			(pin passive line
				(at -10.16 -25.4 0)
				(length 2.54)
				(name "S7B")
				(number "5")
			)
			(pin passive line
				(at -10.16 -27.94 0)
				(length 2.54)
				(name "S8B")
				(number "4")
			)
			(pin power_in line
				(at 5.08 33.02 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 5.08 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "12")
			)
			(pin power_in line
				(at 7.62 -33.02 90)
				(length 2.54)
				(name "VSS")
				(number "27")
			)
			(pin no_connect line
				(at 10.16 27.94 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at 10.16 25.4 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at 10.16 22.86 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 2.54)
				(name "DA")
				(number "28")
			)
			(pin passive line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "DB")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADG715"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 24.13 0)
		)
		(property "Value" "ADG715"
			(at 10.16 24.13 0)
		)
		(property "Footprint" "Package_SO:TSSOP-24_4.4x7.8mm_P0.65mm"
			(at 25.4 -19.05 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADG714_715.pdf"
			(at 0 -30.48 0)
		)
		(property "Description" "CMOS, Low Voltage, Serially Controlled, Octal SPST Switch, I2C interface, TSSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS, Switch, I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x7.8mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADG715_0_0"
			(text "INTERFACE LOGIC"
				(at 0 -3.81 0)
			)
		)
		(symbol "ADG715_0_1")
		(symbol "ADG715_1_1"
			(pin passive line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "S1")
				(number "5")
			)
			(pin passive line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "S2")
				(number "7")
			)
			(pin passive line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "S3")
				(number "9")
			)
			(pin passive line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "S4")
				(number "11")
			)
			(pin passive line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "S5")
				(number "14")
			)
			(pin passive line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "S6")
				(number "16")
			)
			(pin passive line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "S7")
				(number "18")
			)
			(pin passive line
				(at -20.32 0 0)
				(length 2.54)
				(name "S8")
				(number "20")
			)
			(pin input line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "~{RESET}")
				(number "23")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "SDA")
				(number "3")
			)
			(pin input line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "SCL")
				(number "1")
			)
			(pin input line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "A0")
				(number "24")
			)
			(pin input line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "A1")
				(number "22")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 2.54)
				(name "VSS")
				(number "21")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "D1")
				(number "6")
			)
			(pin passive line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "D2")
				(number "8")
			)
			(pin passive line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "D3")
				(number "10")
			)
			(pin passive line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "D4")
				(number "12")
			)
			(pin passive line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "D5")
				(number "13")
			)
			(pin passive line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "D6")
				(number "15")
			)
			(pin passive line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "D7")
				(number "17")
			)
			(pin passive line
				(at 20.32 0 180)
				(length 2.54)
				(name "D8")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADG728"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 23.495 0)
		)
		(property "Value" "ADG728"
			(at -7.62 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 6.35 -21.59 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADG728_729.pdf"
			(at 0.254 0 0)
		)
		(property "Description" "Single 8-to-1 CMOS Low Voltage 2-Wire Serially Controlled, Matrix Switches"
			(at 0 0 0)
		)
		(property "ki_keywords" "analog switch selector multiplexer TWI I2C IIC 8-to-1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADG728_0_1")
		(symbol "ADG728_1_1"
			(pin input line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "SCL")
				(number "1")
			)
			(pin bidirectional line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "SDA")
				(number "3")
			)
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "A0")
				(number "16")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "A1")
				(number "15")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "~{RESET}")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "S1")
				(number "4")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "S2")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "S3")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "S4")
				(number "7")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "S5")
				(number "12")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "S6")
				(number "11")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "S7")
				(number "10")
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "S8")
				(number "9")
			)
			(pin power_in line
				(at 5.08 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "13")
			)
			(pin power_in line
				(at 5.08 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "14")
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "D")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADG729"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 20.955 0)
		)
		(property "Value" "ADG729"
			(at -7.62 19.05 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 6.35 -21.59 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADG728_729.pdf"
			(at 0.254 0 0)
		)
		(property "Description" "Dual 4-to-1 CMOS Low Voltage 2-Wire Serially Controlled, Matrix Switches"
			(at 0 0 0)
		)
		(property "ki_keywords" "analog switch selector multiplexer TWI I2C IIC 4-to-1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADG729_0_1")
		(symbol "ADG729_1_1"
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "SCL")
				(number "1")
			)
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "SDA")
				(number "3")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "A0")
				(number "16")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "S1A")
				(number "4")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "S2A")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "S3A")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "S4A")
				(number "7")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "S1B")
				(number "13")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "S2B")
				(number "12")
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "S3B")
				(number "11")
			)
			(pin bidirectional line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "S4B")
				(number "10")
			)
			(pin power_in line
				(at 5.08 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 5.08 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "15")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "DA")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "DB")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADG733BRQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 7.874 0)
		)
		(property "Value" "ADG733BRQ"
			(at -3.175 6.096 0)
		)
		(property "Footprint" "Package_SO:QSOP-16_3.9x4.9mm_P0.635mm"
			(at 2.54 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADG733_734.pdf"
			(at 2.54 -8.89 0)
		)
		(property "Description" "Triple SPDT CMOS Analog Switch, 2.5Ohm Ron, QSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "ADG733BRQ_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "14")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "13")
			)
		)
		(symbol "ADG733BRQ_2_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "15")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "ADG733BRQ_3_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(symbol "ADG733BRQ_4_0"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "6")
				(number "~{EN}")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
		)
		(symbol "ADG733BRQ_4_1")
		(embedded_fonts no)
	)
	(symbol "ADG734"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 7.874 0)
		)
		(property "Value" "ADG734"
			(at -3.175 6.096 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 3.175 -11.43 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADG733_734.pdf"
			(at 3.175 -13.97 0)
		)
		(property "Description" "Quad SPDT CMOS Analog Switch, 2.5Ohm Ron, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADG734_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(symbol "ADG734_2_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "9")
			)
		)
		(symbol "ADG734_3_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "13")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "12")
			)
		)
		(symbol "ADG734_4_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "18")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "20")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "17")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "19")
			)
		)
		(symbol "ADG734_5_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin no_connect line
				(at 2.54 10.16 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
		)
		(symbol "ADG734_5_1")
		(embedded_fonts no)
	)
	(symbol "ADG758CPZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 23.495 0)
		)
		(property "Value" "ADG758CPZ"
			(at -7.62 21.59 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-20-1EP_4x4mm_P0.5mm_EP2.1x2.1mm"
			(at 0 -1.27 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADG758_759.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "8-channel CMOS analog multiplexer, 3 Ohm Ron, 55 MHz, LFCSP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "analog switch multiplexer SP8T"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*LFCSP*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ADG758CPZ_0_1")
		(symbol "ADG758CPZ_1_0"
			(pin power_in line
				(at 5.08 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "15")
			)
		)
		(symbol "ADG758CPZ_1_1"
			(pin input line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "A0")
				(number "19")
			)
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "A1")
				(number "18")
			)
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "A2")
				(number "17")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "S1")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "S2")
				(number "4")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "S3")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "S4")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "S5")
				(number "13")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "S6")
				(number "12")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "S7")
				(number "11")
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "S8")
				(number "10")
			)
			(pin power_in line
				(at 5.08 22.86 270)
				(length 2.54)
				(name "V_{DD}")
				(number "14")
			)
			(pin power_in line
				(at 7.62 -20.32 90)
				(length 2.54)
				(name "V_{SS}")
				(number "2")
			)
			(pin passive line
				(at 7.62 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "V_{SS}")
				(number "21")
			)
			(pin no_connect line
				(at 10.16 15.24 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at 10.16 12.7 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at 10.16 10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin no_connect line
				(at 10.16 7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "20")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "D")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADG824BCP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "ADG824BCP"
			(at 0.635 16.51 0)
		)
		(property "Footprint" "Package_CSP:Analog_LFCSP-UQ-10_1.3x1.6mm_P0.4mm"
			(at 1.27 -17.145 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADG884.pdf"
			(at 1.27 -19.05 0)
		)
		(property "Description" "0.5Ω CMOS 1.65V to 3.6V Dual SPDT/2:1 MUX, Mini LFCSP-10 Package 1.3x1.6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "analog switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Analog_LFCSP*1.3x1.6mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "ADG824BCP_0_1")
		(symbol "ADG824BCP_1_1"
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "S1A")
				(number "1")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "S1B")
				(number "3")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN1")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IN2")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "S2A")
				(number "9")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "S2B")
				(number "7")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "D1")
				(number "2")
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "D2")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADG884xCP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "ADG884xCP"
			(at 0.635 16.51 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-WD-10-1EP_3x3mm_P0.5mm_EP1.64x2.38mm"
			(at 1.905 -16.51 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADG884.pdf"
			(at 1.905 -18.415 0)
		)
		(property "Description" "0.5Ω CMOS, Dual 2:1 MUX/SPDT Audio Switch, LFCSP-WD-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "analog switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ADG884xCP_0_1")
		(symbol "ADG884xCP_1_1"
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "S1A")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "S1B")
				(number "5")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN1")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IN2")
				(number "8")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "S2A")
				(number "10")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "S2B")
				(number "7")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "D1")
				(number "3")
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "D2")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADG884xRM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "ADG884xRM"
			(at 0.635 16.51 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 1.27 -18.415 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADG884.pdf"
			(at 1.27 -16.51 0)
		)
		(property "Description" "0.5Ω CMOS, Dual 2:1 MUX/SPDT Audio Switch, MSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "analog switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ADG884xRM_0_1")
		(symbol "ADG884xRM_1_1"
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "S1A")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "S1B")
				(number "5")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN1")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IN2")
				(number "8")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "S2A")
				(number "10")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "S2B")
				(number "7")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "D1")
				(number "3")
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "D2")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CBTL02043A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "CBTL02043A"
			(at 6.35 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:WQFN-20-1EP_2.5x4.5mm_P0.5mm_EP1x2.9mm"
			(at 1.905 -22.86 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/CBTL02043A_CBTL02043B.pdf"
			(at 3.175 -8.89 0)
		)
		(property "Description" "3.3 V, 2 differential channel, 2:1 MUX/deMUX switch, 10 Gbps, WQFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Multiplexer Demultiplexer Switch Hi-Speed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WQFN*1EP*2.5x4.5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "CBTL02043A_0_1")
		(symbol "CBTL02043A_1_1"
			(pin passive line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "A0_P")
				(number "3")
			)
			(pin passive line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "A0_N")
				(number "4")
			)
			(pin passive line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "A1_P")
				(number "7")
			)
			(pin passive line
				(at -15.24 0 0)
				(length 2.54)
				(name "A1_N")
				(number "8")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "SEL")
				(number "9")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "XSD")
				(number "2")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin passive line
				(at 0 22.86 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "10")
			)
			(pin passive line
				(at 0 22.86 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "6")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "20")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "B0_P")
				(number "19")
			)
			(pin passive line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "B0_N")
				(number "18")
			)
			(pin passive line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "B1_P")
				(number "17")
			)
			(pin passive line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "B1_N")
				(number "16")
			)
			(pin passive line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "C0_P")
				(number "15")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 2.54)
				(name "C0_N")
				(number "14")
			)
			(pin passive line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "C1_P")
				(number "13")
			)
			(pin passive line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "C1_N")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CBTL02043B"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "CBTL02043B"
			(at 6.35 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:WQFN-20-1EP_2.5x4.5mm_P0.5mm_EP1x2.9mm"
			(at 1.905 -22.86 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/CBTL02043A_CBTL02043B.pdf"
			(at 3.175 -8.89 0)
		)
		(property "Description" "3.3 V, 2 differential channel, 2:1 MUX/deMUX switch, 10 Gbps, WQFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Multiplexer Demultiplexer Switch Hi-Speed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WQFN*1EP*2.5x4.5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "CBTL02043B_0_1")
		(symbol "CBTL02043B_1_1"
			(pin passive line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "A0_P")
				(number "2")
			)
			(pin passive line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "A0_N")
				(number "3")
			)
			(pin passive line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "A1_P")
				(number "6")
			)
			(pin passive line
				(at -15.24 0 0)
				(length 2.54)
				(name "A1_N")
				(number "7")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "SEL")
				(number "12")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "XSD")
				(number "19")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "11")
			)
			(pin passive line
				(at 0 22.86 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "16")
			)
			(pin passive line
				(at 0 22.86 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin passive line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "B0_P")
				(number "18")
			)
			(pin passive line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "B0_N")
				(number "17")
			)
			(pin passive line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "B1_P")
				(number "14")
			)
			(pin passive line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "B1_N")
				(number "13")
			)
			(pin passive line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "C0_P")
				(number "4")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 2.54)
				(name "C0_N")
				(number "5")
			)
			(pin passive line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "C1_P")
				(number "8")
			)
			(pin passive line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "C1_N")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CD4051B"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 16.51 0)
		)
		(property "Value" "CD4051B"
			(at 3.81 16.51 0)
		)
		(property "Footprint" ""
			(at 3.81 -19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/cd4052b.pdf"
			(at -0.508 2.54 0)
		)
		(property "Description" "CMOS single 8-channel analog multiplexer demultiplexer, TSSOP-16/DIP-16/SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "analog switch selector multiplexer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm* DIP*W7.62* SOIC*3.9x9.9mm*P1.27mm* SO*5.3x10.2mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "CD4051B_0_1")
		(symbol "CD4051B_1_1"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "A")
				(number "11")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "B")
				(number "10")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "C")
				(number "9")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "X")
				(number "3")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "INH")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 2.54)
				(name "VEE")
				(number "7")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "X0")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "X1")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "X2")
				(number "15")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "X3")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "X4")
				(number "1")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "X5")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "X6")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "X7")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CD4052B"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 16.51 0)
		)
		(property "Value" "CD4052B"
			(at 3.81 16.51 0)
		)
		(property "Footprint" ""
			(at 3.81 -19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/cd4052b.pdf"
			(at -0.508 5.08 0)
		)
		(property "Description" "CMOS double 4-channel analog multiplexer/demultiplexer, TSSOP-16/DIP-16/SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "analog switch selector multiplexer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm* DIP*W7.62* SOIC*3.9x9.9mm*P1.27mm* SO*5.3x10.2mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "CD4052B_0_1")
		(symbol "CD4052B_1_1"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "A")
				(number "10")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "B")
				(number "9")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "X")
				(number "13")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "Y")
				(number "3")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "INH")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 2.54)
				(name "VEE")
				(number "7")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "X0")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "X1")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "X2")
				(number "15")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "X3")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "Y0")
				(number "1")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "Y1")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "Y2")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "Y3")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CD4053B"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 16.51 0)
		)
		(property "Value" "CD4053B"
			(at 3.81 16.51 0)
		)
		(property "Footprint" ""
			(at 3.81 -19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/cd4052b.pdf"
			(at -0.508 5.08 0)
		)
		(property "Description" "CMOS triple 2-channel analog multiplexer/demultiplexer, TSSOP-16/DIP-16/SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "analog switch selector multiplexer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm* DIP*W7.62* SOIC*3.9x9.9mm*P1.27mm* SO*5.3x10.2mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "CD4053B_0_1")
		(symbol "CD4053B_1_1"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "S1")
				(number "11")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "S2")
				(number "10")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "S3")
				(number "9")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "A")
				(number "14")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "B")
				(number "15")
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "C")
				(number "4")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "INH")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 2.54)
				(name "VEE")
				(number "7")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "A0")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "A1")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "B0")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "B1")
				(number "1")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "C0")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "C1")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CD4066BE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 3.81 0)
		)
		(property "Value" "CD4066BE"
			(at 7.62 3.81 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/cd4066b.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad 20V analog SPST 1:1 switch, DIP-14"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "analog switch selector multiplexer spst mux amux"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62*"
			(at 0 0 0)
		)
		(symbol "CD4066BE_1_1"
			(pin bidirectional line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "13")
			)
			(pin bidirectional line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(symbol "CD4066BE_2_1"
			(pin bidirectional line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin bidirectional line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(symbol "CD4066BE_3_1"
			(pin bidirectional line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin bidirectional line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "9")
			)
		)
		(symbol "CD4066BE_4_1"
			(pin bidirectional line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin bidirectional line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "10")
			)
		)
		(symbol "CD4066BE_5_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V_{DD}")
				(number "14")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "V_{SS}")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CD4097B"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 29.21 0)
		)
		(property "Value" "CD4097B"
			(at 3.81 29.21 0)
		)
		(property "Footprint" ""
			(at 3.81 -2.54 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/cd4097b.pdf"
			(at -0.508 12.446 0)
		)
		(property "Description" "CMOS double 8-channel analog multiplexer/demultiplexer, TSSOP-24/DIP-24/SOIC-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "analog switch selector multiplexer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x7.8mm*P0.65mm* SOIC*7.5*15.4*1.27mm* SO*5.3x15.0mm*P1.27mm* DIP*15.24mm*"
			(at 0 0 0)
		)
		(symbol "CD4097B_0_1")
		(symbol "CD4097B_1_1"
			(pin input line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "A")
				(number "10")
			)
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "B")
				(number "11")
			)
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "C")
				(number "14")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "X")
				(number "1")
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "Y")
				(number "17")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "INH")
				(number "13")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 2.54)
				(name "VSS")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "X0")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "X1")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "X2")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "X3")
				(number "6")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "X4")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "X5")
				(number "4")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "X6")
				(number "3")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "X7")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "Y0")
				(number "23")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "Y1")
				(number "22")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "Y2")
				(number "21")
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "Y3")
				(number "20")
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "Y4")
				(number "19")
			)
			(pin bidirectional line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "Y5")
				(number "18")
			)
			(pin bidirectional line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "Y6")
				(number "16")
			)
			(pin bidirectional line
				(at 12.7 -25.4 180)
				(length 2.54)
				(name "Y7")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DG308AxJ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "DG308AxJ"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheets/70/494502_DS.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad SPST Analog Switches, normally OFF, 60Ohm Ron, DIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "DG308AxJ_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(symbol "DG308AxJ_2_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "DG308AxJ_3_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "11")
			)
		)
		(symbol "DG308AxJ_4_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "15")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "16")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(symbol "DG308AxJ_5_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "13")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin no_connect line
				(at 2.54 10.16 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "4")
			)
		)
		(symbol "DG308AxJ_5_1")
		(embedded_fonts no)
	)
	(symbol "DG308AxY"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "DG308AxY"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheets/70/494502_DS.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad SPST Analog Switches, normally OFF, 60Ohm Ron, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "DG308AxY_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(symbol "DG308AxY_2_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "DG308AxY_3_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "11")
			)
		)
		(symbol "DG308AxY_4_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "15")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "16")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(symbol "DG308AxY_5_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "13")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin no_connect line
				(at 2.54 10.16 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "4")
			)
		)
		(symbol "DG308AxY_5_1")
		(embedded_fonts no)
	)
	(symbol "DG309xJ"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "DG309xJ"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheets/70/494502_DS.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad SPST Analog Switches, normally ON, 60Ohm Ron, DIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "DG309xJ_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(symbol "DG309xJ_2_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "DG309xJ_3_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "11")
			)
		)
		(symbol "DG309xJ_4_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "15")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "16")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(symbol "DG309xJ_5_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "13")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin no_connect line
				(at 2.54 10.16 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "4")
			)
		)
		(symbol "DG309xJ_5_1")
		(embedded_fonts no)
	)
	(symbol "DG309xY"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "DG309xY"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheets/70/494502_DS.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad SPST Analog Switches, normally ON, 60Ohm Ron, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "DG309xY_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(symbol "DG309xY_2_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "DG309xY_3_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "11")
			)
		)
		(symbol "DG309xY_4_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "15")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "16")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(symbol "DG309xY_5_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "13")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin no_connect line
				(at 2.54 10.16 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "4")
			)
		)
		(symbol "DG309xY_5_1")
		(embedded_fonts no)
	)
	(symbol "DG411xJ"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "DG411xJ"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DG411-DG413.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad SPST Monolithic CMOS Analog Switches, normally ON, 17Ohm Ron, DIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "DG411xJ_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(symbol "DG411xJ_2_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "DG411xJ_3_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "11")
			)
		)
		(symbol "DG411xJ_4_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "15")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "16")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(symbol "DG411xJ_5_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "13")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VL")
				(number "12")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "4")
			)
		)
		(symbol "DG411xJ_5_1")
		(embedded_fonts no)
	)
	(symbol "DG411xUE"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "DG411xUE"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DG411-DG413.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad SPST Monolithic CMOS Analog Switches, normally ON, 17Ohm Ron, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "DG411xUE_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(symbol "DG411xUE_2_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "DG411xUE_3_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "11")
			)
		)
		(symbol "DG411xUE_4_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "15")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "16")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(symbol "DG411xUE_5_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "13")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VL")
				(number "12")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "4")
			)
		)
		(symbol "DG411xUE_5_1")
		(embedded_fonts no)
	)
	(symbol "DG411xY"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "DG411xY"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DG411-DG413.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad SPST Monolithic CMOS Analog Switches, normally ON, 17Ohm Ron, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "DG411xY_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(symbol "DG411xY_2_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "DG411xY_3_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "11")
			)
		)
		(symbol "DG411xY_4_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "15")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "16")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(symbol "DG411xY_5_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "13")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VL")
				(number "12")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "4")
			)
		)
		(symbol "DG411xY_5_1")
		(embedded_fonts no)
	)
	(symbol "DG412xJ"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "DG412xJ"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DG411-DG413.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad SPST Monolithic CMOS Analog Switches, normally OFF, 17Ohm Ron, DIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "DG412xJ_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(symbol "DG412xJ_2_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "DG412xJ_3_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "11")
			)
		)
		(symbol "DG412xJ_4_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "15")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "16")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(symbol "DG412xJ_5_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "13")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VL")
				(number "12")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "4")
			)
		)
		(symbol "DG412xJ_5_1")
		(embedded_fonts no)
	)
	(symbol "DG412xUE"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "DG412xUE"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DG411-DG413.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad SPST Monolithic CMOS Analog Switches, normally OFF, 17Ohm Ron, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "DG412xUE_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(symbol "DG412xUE_2_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "DG412xUE_3_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "11")
			)
		)
		(symbol "DG412xUE_4_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "15")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "16")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(symbol "DG412xUE_5_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "13")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VL")
				(number "12")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "4")
			)
		)
		(symbol "DG412xUE_5_1")
		(embedded_fonts no)
	)
	(symbol "DG412xY"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "DG412xY"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DG411-DG413.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad SPST Monolithic CMOS Analog Switches, normally OFF, 17Ohm Ron, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "DG412xY_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(symbol "DG412xY_2_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "DG412xY_3_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "11")
			)
		)
		(symbol "DG412xY_4_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "15")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "16")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(symbol "DG412xY_5_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "13")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VL")
				(number "12")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "4")
			)
		)
		(symbol "DG412xY_5_1")
		(embedded_fonts no)
	)
	(symbol "DG413xJ"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "DG413xJ"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DG411-DG413.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad SPST Monolithic CMOS Analog Switches, normally 2xON + 2xOFF, 17Ohm Ron, DIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "DG413xJ_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(symbol "DG413xJ_2_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "DG413xJ_3_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "11")
			)
		)
		(symbol "DG413xJ_4_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "15")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "16")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(symbol "DG413xJ_5_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "13")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VL")
				(number "12")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "4")
			)
		)
		(symbol "DG413xJ_5_1")
		(embedded_fonts no)
	)
	(symbol "DG413xUE"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "DG413xUE"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DG411-DG413.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad SPST Monolithic CMOS Analog Switches, normally 2xON + 2xOFF, 17Ohm Ron, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "DG413xUE_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(symbol "DG413xUE_2_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "DG413xUE_3_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "11")
			)
		)
		(symbol "DG413xUE_4_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "15")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "16")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(symbol "DG413xUE_5_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "13")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VL")
				(number "12")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "4")
			)
		)
		(symbol "DG413xUE_5_1")
		(embedded_fonts no)
	)
	(symbol "DG413xY"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "DG413xY"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DG411-DG413.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad SPST Monolithic CMOS Analog Switches, normally 2xON + 2xOFF, 17Ohm Ron, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "DG413xY_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(symbol "DG413xY_2_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "DG413xY_3_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "11")
			)
		)
		(symbol "DG413xY_4_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "15")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "16")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(symbol "DG413xY_5_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "13")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VL")
				(number "12")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "4")
			)
		)
		(symbol "DG413xY_5_1")
		(embedded_fonts no)
	)
	(symbol "DG417LDJ"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "DG417LDJ"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DG417L-DG419L.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single SPST 3V Logic Compatible CMOS Analog Switch, normally ON, 35Ohm Ron, with Vlogic, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "DG417LDJ_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(symbol "DG417LDJ_2_0"
			(pin no_connect line
				(at -2.54 10.16 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VL")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "7")
			)
		)
		(symbol "DG417LDJ_2_1")
		(embedded_fonts no)
	)
	(symbol "DG417LDJ_Maxim"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "DG417LDJ_Maxim"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DG417L-DG419L.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single SPST 3V Logic Compatible CMOS Analog Switch, normally ON, 35Ohm Ron, Maxim-variant without Vlogic, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "DG417LDJ_Maxim_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(symbol "DG417LDJ_Maxim_2_0"
			(pin no_connect line
				(at -2.54 10.16 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin no_connect line
				(at 2.54 10.16 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "7")
			)
		)
		(symbol "DG417LDJ_Maxim_2_1")
		(embedded_fonts no)
	)
	(symbol "DG417LDY"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "DG417LDY"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DG417-DG419.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single SPST 3V Logic Compatible CMOS Analog Switch, normally ON, 20Ohm Ron, with Vlogic, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "DG417LDY_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(symbol "DG417LDY_2_0"
			(pin no_connect line
				(at -2.54 10.16 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VL")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "7")
			)
		)
		(symbol "DG417LDY_2_1")
		(embedded_fonts no)
	)
	(symbol "DG417LDY_Maxim"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "DG417LDY_Maxim"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DG417-DG419.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single SPST 3V Logic Compatible CMOS Analog Switch, normally ON, 20Ohm Ron, Maxim-variant without Vlogic, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "DG417LDY_Maxim_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(symbol "DG417LDY_Maxim_2_0"
			(pin no_connect line
				(at -2.54 10.16 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin no_connect line
				(at 2.54 10.16 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "7")
			)
		)
		(symbol "DG417LDY_Maxim_2_1")
		(embedded_fonts no)
	)
	(symbol "DG417LEUA"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "DG417LEUA"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DG417-DG419.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single SPST 3V Logic Compatible CMOS Analog Switch, normally ON, 20Ohm Ron, with Vlogic, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "DG417LEUA_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(symbol "DG417LEUA_2_0"
			(pin no_connect line
				(at -2.54 10.16 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VL")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "7")
			)
		)
		(symbol "DG417LEUA_2_1")
		(embedded_fonts no)
	)
	(symbol "DG417LEUA_Maxim"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "DG417LEUA_Maxim"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DG417-DG419.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single SPST 3V Logic Compatible CMOS Analog Switch, normally ON, 20Ohm Ron, Maxim-variant without Vlogic, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "DG417LEUA_Maxim_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(symbol "DG417LEUA_Maxim_2_0"
			(pin no_connect line
				(at -2.54 10.16 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin no_connect line
				(at 2.54 10.16 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "7")
			)
		)
		(symbol "DG417LEUA_Maxim_2_1")
		(embedded_fonts no)
	)
	(symbol "DG417xJ"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "DG417xJ"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DG417-DG419.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single SPST Monolithic CMOS Analog Switch, normally ON, 20Ohm Ron, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "DG417xJ_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(symbol "DG417xJ_2_0"
			(pin no_connect line
				(at -2.54 10.16 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VL")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "7")
			)
		)
		(symbol "DG417xJ_2_1")
		(embedded_fonts no)
	)
	(symbol "DG417xY"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "DG417xY"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DG417-DG419.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single SPST Monolithic CMOS Analog Switch, normally ON, 20Ohm Ron, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "DG417xY_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(symbol "DG417xY_2_0"
			(pin no_connect line
				(at -2.54 10.16 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VL")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "7")
			)
		)
		(symbol "DG417xY_2_1")
		(embedded_fonts no)
	)
	(symbol "DG418LDJ"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "DG418LDJ"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DG417-DG419.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single SPST 3V Logic Compatible CMOS Analog Switch, normally OFF, 35Ohm Ron, with Vlogic, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "DG418LDJ_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(symbol "DG418LDJ_2_0"
			(pin no_connect line
				(at -2.54 10.16 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VL")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "7")
			)
		)
		(symbol "DG418LDJ_2_1")
		(embedded_fonts no)
	)
	(symbol "DG418LDJ_Maxim"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "DG418LDJ_Maxim"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DG417-DG419.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single SPST 3V Logic Compatible CMOS Analog Switch, normally OFF, 35Ohm Ron, Maxim-variant without Vlogic, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "DG418LDJ_Maxim_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(symbol "DG418LDJ_Maxim_2_0"
			(pin no_connect line
				(at -2.54 10.16 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin no_connect line
				(at 2.54 10.16 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "7")
			)
		)
		(symbol "DG418LDJ_Maxim_2_1")
		(embedded_fonts no)
	)
	(symbol "DG418LDY"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "DG418LDY"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DG417-DG419.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single SPST 3V Logic Compatible CMOS Analog Switch, normally OFF, 35Ohm Ron, with Vlogic, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "DG418LDY_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(symbol "DG418LDY_2_0"
			(pin no_connect line
				(at -2.54 10.16 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VL")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "7")
			)
		)
		(symbol "DG418LDY_2_1")
		(embedded_fonts no)
	)
	(symbol "DG418LDY_Maxim"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "DG418LDY_Maxim"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DG417-DG419.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single SPST 3V Logic Compatible CMOS Analog Switch, normally OFF, 35Ohm Ron, Maxim-variant without Vlogic, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "DG418LDY_Maxim_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(symbol "DG418LDY_Maxim_2_0"
			(pin no_connect line
				(at -2.54 10.16 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin no_connect line
				(at 2.54 10.16 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "7")
			)
		)
		(symbol "DG418LDY_Maxim_2_1")
		(embedded_fonts no)
	)
	(symbol "DG418LEUA"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "DG418LEUA"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DG417-DG419.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single SPST 3V Logic Compatible CMOS Analog Switch, normally OFF, 35Ohm Ron, with Vlogic, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "DG418LEUA_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(symbol "DG418LEUA_2_0"
			(pin no_connect line
				(at -2.54 10.16 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VL")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "7")
			)
		)
		(symbol "DG418LEUA_2_1")
		(embedded_fonts no)
	)
	(symbol "DG418LEUA_Maxim"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "DG418LEUA_Maxim"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DG417-DG419.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single SPST 3V Logic Compatible CMOS Analog Switch, normally OFF, 35Ohm Ron, Maxim-variant without Vlogic, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "DG418LEUA_Maxim_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(symbol "DG418LEUA_Maxim_2_0"
			(pin no_connect line
				(at -2.54 10.16 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin no_connect line
				(at 2.54 10.16 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "7")
			)
		)
		(symbol "DG418LEUA_Maxim_2_1")
		(embedded_fonts no)
	)
	(symbol "DG418xJ"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "DG418xJ"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DG417-DG419.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single SPST Monolithic CMOS Analog Switch, normally OFF, 20Ohm Ron, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "DG418xJ_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(symbol "DG418xJ_2_0"
			(pin no_connect line
				(at -2.54 10.16 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VL")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "7")
			)
		)
		(symbol "DG418xJ_2_1")
		(embedded_fonts no)
	)
	(symbol "DG418xY"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "DG418xY"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DG417-DG419.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single SPST Monolithic CMOS Analog Switch, normally OFF, 20Ohm Ron, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "DG418xY_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(symbol "DG418xY_2_0"
			(pin no_connect line
				(at -2.54 10.16 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VL")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "7")
			)
		)
		(symbol "DG418xY_2_1")
		(embedded_fonts no)
	)
	(symbol "DG419LDJ"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 7.239 0)
		)
		(property "Value" "DG419LDJ"
			(at -3.175 5.461 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 3.81 -13.97 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DG417-DG419.pdf"
			(at 3.81 -11.43 0)
		)
		(property "Description" "Single SPDT 3V Logic Compatible CMOS Analog Switch, 35Ohm Ron, with Vlogic, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "DG419LDJ_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(symbol "DG419LDJ_2_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VL")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "7")
			)
		)
		(symbol "DG419LDJ_2_1")
		(embedded_fonts no)
	)
	(symbol "DG419LDJ_Maxim"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 7.239 0)
		)
		(property "Value" "DG419LDJ_Maxim"
			(at -3.175 5.461 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 3.175 -13.97 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DG417-DG419.pdf"
			(at 3.175 -11.43 0)
		)
		(property "Description" "Single SPDT 3V Logic Compatible CMOS Analog Switch, 35Ohm Ron, Maxim-variant without Vlogic, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "DG419LDJ_Maxim_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(symbol "DG419LDJ_Maxim_2_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin no_connect line
				(at 2.54 10.16 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "7")
			)
		)
		(symbol "DG419LDJ_Maxim_2_1")
		(embedded_fonts no)
	)
	(symbol "DG419LDY"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 7.239 0)
		)
		(property "Value" "DG419LDY"
			(at -3.175 5.461 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 3.81 -14.605 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DG417-DG419.pdf"
			(at 3.81 -12.065 0)
		)
		(property "Description" "Single SPDT 3V Logic Compatible CMOS Analog Switch, 35Ohm Ron, with Vlogic, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "DG419LDY_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(symbol "DG419LDY_2_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VL")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "7")
			)
		)
		(symbol "DG419LDY_2_1")
		(embedded_fonts no)
	)
	(symbol "DG419LDY_Maxim"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 7.239 0)
		)
		(property "Value" "DG419LDY_Maxim"
			(at -3.175 5.461 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 3.81 -13.97 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DG417-DG419.pdf"
			(at 3.81 -11.43 0)
		)
		(property "Description" "Single SPDT 3V Logic Compatible CMOS Analog Switch, 35Ohm Ron, Maxim-variant without Vlogic, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "DG419LDY_Maxim_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(symbol "DG419LDY_Maxim_2_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin no_connect line
				(at 2.54 10.16 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "7")
			)
		)
		(symbol "DG419LDY_Maxim_2_1")
		(embedded_fonts no)
	)
	(symbol "DG419LEUA"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 7.239 0)
		)
		(property "Value" "DG419LEUA"
			(at -3.175 5.461 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 3.175 -13.97 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DG417-DG419.pdf"
			(at 3.175 -12.065 0)
		)
		(property "Description" "Single SPDT 3V Logic Compatible CMOS Analog Switch, 35Ohm Ron, with Vlogic, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "DG419LEUA_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(symbol "DG419LEUA_2_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VL")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "7")
			)
		)
		(symbol "DG419LEUA_2_1")
		(embedded_fonts no)
	)
	(symbol "DG419LEUA_Maxim"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 7.62 0)
		)
		(property "Value" "DG419LEUA_Maxim"
			(at -3.175 5.715 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DG417-DG419.pdf"
			(at 1.27 -9.525 0)
		)
		(property "Description" "Single SPDT 3V Logic Compatible CMOS Analog Switch, 35Ohm Ron, Maxim-variant without Vlogic, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "DG419LEUA_Maxim_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(symbol "DG419LEUA_Maxim_2_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin no_connect line
				(at 2.54 10.16 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "7")
			)
		)
		(symbol "DG419LEUA_Maxim_2_1")
		(embedded_fonts no)
	)
	(symbol "DG419xJ"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 7.62 0)
		)
		(property "Value" "DG419xJ"
			(at -3.175 5.461 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 3.175 -13.97 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DG417-DG419.pdf"
			(at 3.175 -12.065 0)
		)
		(property "Description" "Single SPDT Monolithic CMOS Analog Switch, 20Ohm Ron, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "DG419xJ_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(symbol "DG419xJ_2_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VL")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "7")
			)
		)
		(symbol "DG419xJ_2_1")
		(embedded_fonts no)
	)
	(symbol "DG419xY"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 7.62 0)
		)
		(property "Value" "DG419xY"
			(at -3.175 5.461 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 3.81 -13.335 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DG417-DG419.pdf"
			(at 3.81 -11.43 0)
		)
		(property "Description" "Single SPDT Monolithic CMOS Analog Switch, 20Ohm Ron, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "DG419xY_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(symbol "DG419xY_2_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VL")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "7")
			)
		)
		(symbol "DG419xY_2_1")
		(embedded_fonts no)
	)
	(symbol "DG884DN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 34.29 0)
		)
		(property "Value" "DG884DN"
			(at 11.43 34.29 0)
		)
		(property "Footprint" "Package_LCC:PLCC-44"
			(at 3.81 -26.67 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/70071/dg884.pdf"
			(at 0 0 0)
		)
		(property "Description" "8 x 4 Wideband Video Crosspoint Array, 45Ohm Ron, PLCC-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch Video Crosspoint"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PLCC?44*"
			(at 0 0 0)
		)
		(symbol "DG884DN_0_1")
		(symbol "DG884DN_1_1"
			(pin input line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "IN1")
				(number "5")
			)
			(pin input line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "IN2")
				(number "7")
			)
			(pin input line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "IN3")
				(number "9")
			)
			(pin input line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "IN4")
				(number "11")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "IN5")
				(number "13")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "IN6")
				(number "15")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "IN7")
				(number "17")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "IN8")
				(number "19")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "B0")
				(number "27")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "B1")
				(number "28")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "~{I}/O")
				(number "29")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "~{CS}")
				(number "30")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "A0")
				(number "31")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "A1")
				(number "32")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "A2")
				(number "33")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "A3")
				(number "34")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "~{WR}")
				(number "35")
			)
			(pin input line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "~{SALVO}")
				(number "36")
			)
			(pin input line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "~{RS}")
				(number "37")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 2.54)
				(name "GNDA")
				(number "1")
			)
			(pin passive line
				(at -2.54 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GNDA")
				(number "10")
			)
			(pin passive line
				(at -2.54 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GNDA")
				(number "12")
			)
			(pin passive line
				(at -2.54 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GNDA")
				(number "14")
			)
			(pin passive line
				(at -2.54 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GNDA")
				(number "16")
			)
			(pin passive line
				(at -2.54 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GNDA")
				(number "18")
			)
			(pin passive line
				(at -2.54 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GNDA")
				(number "20")
			)
			(pin passive line
				(at -2.54 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GNDA")
				(number "3")
			)
			(pin passive line
				(at -2.54 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GNDA")
				(number "4")
			)
			(pin passive line
				(at -2.54 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GNDA")
				(number "41")
			)
			(pin passive line
				(at -2.54 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GNDA")
				(number "43")
			)
			(pin passive line
				(at -2.54 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GNDA")
				(number "6")
			)
			(pin passive line
				(at -2.54 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GNDA")
				(number "8")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 2.54)
				(name "V+")
				(number "26")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "39")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 2.54)
				(name "VCC")
				(number "38")
			)
			(pin passive line
				(at 2.54 -27.94 90)
				(length 2.54)
				(name "V-")
				(number "21")
			)
			(pin output line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "OUT1")
				(number "2")
			)
			(pin output line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "OUT2")
				(number "44")
			)
			(pin output line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "OUT3")
				(number "42")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "OUT4")
				(number "40")
			)
			(pin open_collector line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "~{DIS1}")
				(number "22")
			)
			(pin open_collector line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "~{DIS2}")
				(number "23")
			)
			(pin open_collector line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "~{DIS3}")
				(number "24")
			)
			(pin open_collector line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "~{DIS4}")
				(number "25")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DG9421DV"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.683 5.334 0)
		)
		(property "Value" "DG9421DV"
			(at -3.683 3.556 0)
		)
		(property "Footprint" "Package_SO:TSOP-6_1.65x3.05mm_P0.95mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/70679/dg9421.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single SPST Precision Low-Voltage, Low-Glitch CMOS Analog Switch, normally ON, 2Ohm Ron, TSOP-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOP*1.65x3.05mm*P0.95mm*"
			(at 0 0 0)
		)
		(symbol "DG9421DV_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(symbol "DG9421DV_2_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "3")
			)
		)
		(symbol "DG9421DV_2_1")
		(embedded_fonts no)
	)
	(symbol "DG9422DV"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.683 5.334 0)
		)
		(property "Value" "DG9422DV"
			(at -3.683 3.556 0)
		)
		(property "Footprint" "Package_SO:TSOP-6_1.65x3.05mm_P0.95mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/70679/dg9421.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single SPST Precision Low-Voltage, Low-Glitch CMOS Analog Switch, normally OFF, 2Ohm Ron, TSOP-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOP*1.65x3.05mm*P0.95mm*"
			(at 0 0 0)
		)
		(symbol "DG9422DV_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(symbol "DG9422DV_2_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "3")
			)
		)
		(symbol "DG9422DV_2_1")
		(embedded_fonts no)
	)
	(symbol "HEF4066BT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -4.572 9.144 0)
		)
		(property "Value" "HEF4066BT"
			(at 7.62 9.144 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0.508 -17.78 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/HEF4066B.pdf"
			(at 0 -15.24 0)
		)
		(property "Description" "Quad single-pole single-throw analog switch, 3.0...15.0V supply, VI = 0...VDD, f(-3dB) = 90MHz, RON(peak) = 350 / 80 / 60 ohms (for VI from 0V to VDD, with VDD 5 / 10 / 15V respectively), SOIC-14"
			(at 0 -12.7 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "ESD CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SO*3.9*8.*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "HEF4066BT_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "1Y")
				(number "1")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "1E")
				(number "13")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "1Z")
				(number "2")
			)
		)
		(symbol "HEF4066BT_2_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "2Y")
				(number "4")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "2E")
				(number "5")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "2Z")
				(number "3")
			)
		)
		(symbol "HEF4066BT_3_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "3Y")
				(number "8")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "3E")
				(number "6")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "3Z")
				(number "9")
			)
		)
		(symbol "HEF4066BT_4_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "4Y")
				(number "11")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "4E")
				(number "12")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "4Z")
				(number "10")
			)
		)
		(symbol "HEF4066BT_5_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HI524"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "HI524"
			(at 1.905 16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-18_W7.62mm"
			(at 3.175 -16.51 0)
		)
		(property "Datasheet" "https://www.intersil.com/content/dam/Intersil/documents/hi-5/hi-524.pdf"
			(at 0 0 0)
		)
		(property "Description" "4-Channel Wideband and Video Multiplexer, DIP-18"
			(at 0 0 0)
		)
		(property "ki_keywords" "Video Multiplexer analog switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "HI524_0_1")
		(symbol "HI524_1_1"
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "A0")
				(number "10")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "A1")
				(number "9")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "EN")
				(number "11")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "FBI")
				(number "18")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IN1")
				(number "12")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "IN2")
				(number "14")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "IN3")
				(number "7")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "IN4")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "V+")
				(number "1")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "V-")
				(number "17")
			)
			(pin passive line
				(at 2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "SIGGND")
				(number "13")
			)
			(pin passive line
				(at 2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "SIGGND")
				(number "15")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "SIGGND")
				(number "3")
			)
			(pin passive line
				(at 2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "SIGGND")
				(number "4")
			)
			(pin passive line
				(at 2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "SIGGND")
				(number "6")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "FBO")
				(number "16")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "OUT")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX14662"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 26.67 0)
		)
		(property "Value" "MAX14662"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_4x4mm_P0.4mm_EP2.6x2.6mm"
			(at 0 -45.72 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX14662.pdf"
			(at 0 -48.26 0)
		)
		(property "Description" "Analog Switch, beyond-the-Rails 8xSPST, I²C/SPI interface, 1.6..5.5V supply, 0.425Ohm Ron, TQFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "analog switch octal SPST i2c spi"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "MAX14662_0_0"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "~{CS}/AD0")
				(number "23")
			)
		)
		(symbol "MAX14662_0_1")
		(symbol "MAX14662_1_0"
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "DIN/SDA")
				(number "27")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "DOUT/AD1")
				(number "28")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "V_{CC}")
				(number "26")
			)
			(pin no_connect line
				(at 7.62 22.86 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at 7.62 20.32 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin no_connect line
				(at 7.62 17.78 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
		)
		(symbol "MAX14662_1_1"
			(pin input line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "~{SD}")
				(number "22")
			)
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "SPI/~{I²C}")
				(number "1")
			)
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "SCLK/SCL")
				(number "24")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A3")
				(number "4")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "A4")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "A5")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "A6")
				(number "7")
			)
			(pin bidirectional line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "A7")
				(number "8")
			)
			(pin bidirectional line
				(at -10.16 -20.32 0)
				(length 2.54)
				(name "A8")
				(number "9")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B1")
				(number "21")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "B2")
				(number "20")
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "B3")
				(number "19")
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "B4")
				(number "18")
			)
			(pin bidirectional line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "B5")
				(number "17")
			)
			(pin bidirectional line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "B6")
				(number "16")
			)
			(pin bidirectional line
				(at 10.16 -17.78 180)
				(length 2.54)
				(name "B7")
				(number "15")
			)
			(pin bidirectional line
				(at 10.16 -20.32 180)
				(length 2.54)
				(name "B8")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX14759"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "MAX14759"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.65mm_EP1.55x2.4mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX14759-MAX14763.pdf"
			(at -1.27 0 90)
		)
		(property "Description" "Above- and Below-the-Rails Low On-Resistance Analog Switches, max 2 Ohms On-Resistance, TDFN-8"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "analog switch low resistance above below rails"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MAX14759_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "A")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "8")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "B")
				(number "4")
			)
		)
		(symbol "MAX14759_2_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "VP")
				(number "6")
			)
			(pin no_connect line
				(at -2.54 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "VN")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "VN")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX14761"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "MAX14761"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-10-1EP_3x3mm_P0.5mm_EP1.55x2.48mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX14759-MAX14763.pdf"
			(at 12.7 -2.54 90)
		)
		(property "Description" "Above- and Below-the-Rails Low On-Resistance Analog Switches, max 2 Ohm On resistor, TDFN-10"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "analog switch low resistance above below rails"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MAX14761_1_1"
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "A1")
				(number "8")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN1")
				(number "10")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "B1")
				(number "3")
			)
		)
		(symbol "MAX14761_2_1"
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "A2")
				(number "6")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN2")
				(number "9")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "B2")
				(number "5")
			)
		)
		(symbol "MAX14761_3_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "VP")
				(number "7")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "VN")
				(number "11")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "VN")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX14778"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "MAX14778"
			(at 8.89 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:TQFN-20-1EP_5x5mm_P0.65mm_EP3.1x3.1mm"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX14778.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual ±25V Above- and Below-the-Rails 4:1 Analog Multiplexer, TQFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Analog Differential Multiplexer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFN*1EP*5x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MAX14778_0_1")
		(symbol "MAX14778_1_1"
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "ENA")
				(number "10")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "SA0")
				(number "11")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SA1")
				(number "12")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "ACOM")
				(number "5")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "BCOM")
				(number "1")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "ENB")
				(number "16")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "SB0")
				(number "15")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "SB1")
				(number "14")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "13")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "VP")
				(number "2")
			)
			(pin passive line
				(at 2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "VN")
				(number "21")
			)
			(pin passive line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "VN")
				(number "4")
			)
			(pin passive line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "A0")
				(number "6")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "A1")
				(number "7")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "A2")
				(number "8")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "A3")
				(number "9")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B0")
				(number "20")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "B1")
				(number "19")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "B2")
				(number "18")
			)
			(pin passive line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "B3")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX323CPA"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "MAX323CPA"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX323-MAX325.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual SPST CMOS Analog Switches, normally OFF, 60Ohm Ron, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MAX323CPA_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(symbol "MAX323CPA_2_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(symbol "MAX323CPA_3_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "4")
			)
		)
		(symbol "MAX323CPA_3_1")
		(embedded_fonts no)
	)
	(symbol "MAX323CSA"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "MAX323CSA"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX323-MAX325.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual SPST CMOS Analog Switches, normally OFF, 60Ohm Ron, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MAX323CSA_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(symbol "MAX323CSA_2_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(symbol "MAX323CSA_3_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "4")
			)
		)
		(symbol "MAX323CSA_3_1")
		(embedded_fonts no)
	)
	(symbol "MAX323CUA"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "MAX323CUA"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX323-MAX325.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual SPST CMOS Analog Switches, normally OFF, 60Ohm Ron, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MAX323CUA_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(symbol "MAX323CUA_2_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(symbol "MAX323CUA_3_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "4")
			)
		)
		(symbol "MAX323CUA_3_1")
		(embedded_fonts no)
	)
	(symbol "MAX324CPA"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "MAX324CPA"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX323-MAX325.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual SPST CMOS Analog Switches, normally ON, 60Ohm Ron, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MAX324CPA_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(symbol "MAX324CPA_2_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(symbol "MAX324CPA_3_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "4")
			)
		)
		(symbol "MAX324CPA_3_1")
		(embedded_fonts no)
	)
	(symbol "MAX324CSA"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "MAX324CSA"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX323-MAX325.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual SPST CMOS Analog Switches, normally ON, 60Ohm Ron, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MAX324CSA_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(symbol "MAX324CSA_2_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(symbol "MAX324CSA_3_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "4")
			)
		)
		(symbol "MAX324CSA_3_1")
		(embedded_fonts no)
	)
	(symbol "MAX324CUA"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "MAX324CUA"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX323-MAX325.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual SPST CMOS Analog Switches, normally ON, 60Ohm Ron, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MAX324CUA_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(symbol "MAX324CUA_2_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(symbol "MAX324CUA_3_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "4")
			)
		)
		(symbol "MAX324CUA_3_1")
		(embedded_fonts no)
	)
	(symbol "MAX325CPA"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "MAX325CPA"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX323-MAX325.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual SPST CMOS Analog Switches, normally 1xOFF and 1xON, 60Ohm Ron, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MAX325CPA_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(symbol "MAX325CPA_2_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(symbol "MAX325CPA_3_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "4")
			)
		)
		(symbol "MAX325CPA_3_1")
		(embedded_fonts no)
	)
	(symbol "MAX325CSA"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "MAX325CSA"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX323-MAX325.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual SPST CMOS Analog Switches, normally 1xOFF and 1xON, 60Ohm Ron, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MAX325CSA_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(symbol "MAX325CSA_2_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(symbol "MAX325CSA_3_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "4")
			)
		)
		(symbol "MAX325CSA_3_1")
		(embedded_fonts no)
	)
	(symbol "MAX325CUA"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "MAX325CUA"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX323-MAX325.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual SPST CMOS Analog Switches, normally 1xOFF and 1xON, 60Ohm Ron, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MAX325CUA_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(symbol "MAX325CUA_2_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(symbol "MAX325CUA_3_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "4")
			)
		)
		(symbol "MAX325CUA_3_1")
		(embedded_fonts no)
	)
	(symbol "MAX333"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 7.874 0)
		)
		(property "Value" "MAX333"
			(at -3.175 6.096 0)
		)
		(property "Footprint" ""
			(at 0 5.08 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX333.pdf"
			(at 3.048 -11.43 0)
		)
		(property "Description" "Quad SPDT CMOS Analog Switch, DIP-20/SOIC-20/SSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x7.2mm*P0.65mm* SOIC*7.5x10.3mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MAX333_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(symbol "MAX333_2_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "9")
			)
		)
		(symbol "MAX333_3_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "13")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "12")
			)
		)
		(symbol "MAX333_4_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "18")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "20")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "17")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "19")
			)
		)
		(symbol "MAX333_5_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "16")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "5")
			)
			(pin no_connect line
				(at 2.54 10.16 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
		)
		(symbol "MAX333_5_1")
		(embedded_fonts no)
	)
	(symbol "MAX333A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 7.874 0)
		)
		(property "Value" "MAX333A"
			(at -3.175 6.096 0)
		)
		(property "Footprint" ""
			(at 0 5.08 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX333A.pdf"
			(at 3.048 -11.43 0)
		)
		(property "Description" "Quad SPDT CMOS Analog Switch, 17Ohm Ron, DIP-20/SOIC-20/SSOP-20/TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm* SSOP*5.3x7.2mm*P0.65mm* SOIC*7.5x10.3mm*P1.27mm* DIP*W7.62mm* SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MAX333A_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(symbol "MAX333A_2_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "9")
			)
		)
		(symbol "MAX333A_3_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "13")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "12")
			)
		)
		(symbol "MAX333A_4_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "18")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "20")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "17")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "19")
			)
		)
		(symbol "MAX333A_5_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "16")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "V-")
				(number "5")
			)
			(pin no_connect line
				(at 2.54 10.16 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
		)
		(symbol "MAX333A_5_1")
		(embedded_fonts no)
	)
	(symbol "MAX40200ANS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MAX40200ANS"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_BGA:WLP-4_0.728x0.728mm_Layout2x2_P0.35mm"
			(at 0 10.16 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX40200.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Ideal Diode, Ultra-Low Voltage Drop, 1.5-5.5V, 1A, WLP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "current switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLP*0.728x0.728mm*Layout2x2*P0.35mm*"
			(at 0 0 0)
		)
		(symbol "MAX40200ANS_0_1")
		(symbol "MAX40200ANS_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VDD")
				(number "A1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "B1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "B2")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "A2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX40200AUK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MAX40200AUK"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX40200.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "Ideal Diode, Ultra-Low Voltage Drop, 1.5-5.5V, 1A, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "current switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MAX40200AUK_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NC7SB3157L6X"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 7.493 0)
		)
		(property "Value" "NC7SB3157L6X"
			(at -3.175 5.715 0)
		)
		(property "Footprint" "Package_SON:Fairchild_MicroPak-6_1.0x1.45mm_P0.5mm"
			(at 2.54 -12.065 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NC7SB3157-D.PDF"
			(at 3.175 -9.525 0)
		)
		(property "Description" "Single SPDT Low-Voltage Analog Switch or 2:1 Multiplexer/De-Multiplexer Bus Switch, 10Ohm Ron, MicroPak-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Fairchild*MicroPak*1.0x1.45mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "NC7SB3157L6X_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "NC7SB3157L6X_2_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "5")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
		)
		(symbol "NC7SB3157L6X_2_1")
		(embedded_fonts no)
	)
	(symbol "NC7SB3157P6X"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 7.239 0)
		)
		(property "Value" "NC7SB3157P6X"
			(at -3.175 5.461 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 1.27 -14.605 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NC7SB3157-D.PDF"
			(at 1.27 -12.065 0)
		)
		(property "Description" "Single SPDT Low-Voltage Analog Switch or 2:1 Multiplexer/De-Multiplexer Bus Switch, 10Ohm Ron, SC-70-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
		(symbol "NC7SB3157P6X_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "NC7SB3157P6X_2_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "5")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
		)
		(symbol "NC7SB3157P6X_2_1")
		(embedded_fonts no)
	)
	(symbol "NX3L4051HR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 23.495 0)
		)
		(property "Value" "NX3L4051HR"
			(at -7.62 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:HXQFN-16-1EP_3x3mm_P0.5mm_EP1.85x1.85mm"
			(at 0.254 36.576 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/NX3L4051.pdf"
			(at 0.508 34.798 0)
		)
		(property "Description" "Single 8-channel analog switch, break before switch, low-ohmic 0.5 Ohm, 1.4V-4.3V , HXQFN-16"
			(at -1.016 38.354 0)
		)
		(property "ki_keywords" "multiplexer SP8T"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HXQFN*16*3x3mm*P0.5mm*EP1.85x1.85mm*"
			(at 0 0 0)
		)
		(symbol "NX3L4051HR_0_1")
		(symbol "NX3L4051HR_1_0"
			(pin no_connect line
				(at 2.54 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at 5.08 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 7.62 -22.86 90)
				(length 2.54)
				(name "EP")
				(number "17")
			)
		)
		(symbol "NX3L4051HR_1_1"
			(pin input line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "S1")
				(number "9")
			)
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "S2")
				(number "8")
			)
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "S3")
				(number "7")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "~{E}")
				(number "4")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "Y0")
				(number "11")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "Y1")
				(number "12")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "Y2")
				(number "13")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "Y3")
				(number "10")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "Y4")
				(number "15")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "Y5")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "Y6")
				(number "16")
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "Y7")
				(number "2")
			)
			(pin power_in line
				(at 5.08 22.86 270)
				(length 2.54)
				(name "V_{CC}")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "Z")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NX3L4051PW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 23.495 0)
		)
		(property "Value" "NX3L4051PW"
			(at -7.62 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 0.254 36.576 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/NX3L4051.pdf"
			(at 0.254 0 0)
		)
		(property "Description" "Single 8-channel analog switch, break before switch, low-ohmic 0.5 Ohm, 1.4V-4.3V , TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "multiplexer SP8T"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*16*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "NX3L4051PW_0_1")
		(symbol "NX3L4051PW_1_0"
			(pin power_in line
				(at 5.08 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin no_connect line
				(at 8.89 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
		)
		(symbol "NX3L4051PW_1_1"
			(pin input line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "S1")
				(number "11")
			)
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "S2")
				(number "10")
			)
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "S3")
				(number "9")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "~{E}")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "Y0")
				(number "13")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "Y1")
				(number "14")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "Y2")
				(number "15")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "Y3")
				(number "12")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "Y4")
				(number "1")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "Y5")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "Y6")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "Y7")
				(number "4")
			)
			(pin power_in line
				(at 5.08 22.86 270)
				(length 2.54)
				(name "V_{CC}")
				(number "16")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "Z")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SN74CBT3253"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "SN74CBT3253"
			(at -11.43 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74cbt3253"
			(at 0 0 0)
		)
		(property "Description" "Dual 1 to 4 Analog Multiplexer"
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL Analog Multiplexer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm* SSOP*5.3x6.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "SN74CBT3253_0_1")
		(symbol "SN74CBT3253_1_1"
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "1A")
				(number "7")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "2A")
				(number "9")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "S0")
				(number "14")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "S1")
				(number "2")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "1~{OE}")
				(number "1")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "2~{OE}")
				(number "15")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "1B1")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "1B2")
				(number "5")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "1B3")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "1B4")
				(number "3")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "2B1")
				(number "10")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "2B2")
				(number "11")
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "2B3")
				(number "12")
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "2B4")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMUX1101DBV"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "TMUX1101DBV"
			(at -12.7 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tmux1101.pdf"
			(at 0 -11.43 0)
		)
		(property "Description" "SPST Analog Switch, 1.08V to 5.5V Supply, 3pA Leakage Current, Normally OFF, 1.8Ohm Ron, SC-70"
			(at 0 0 0)
		)
		(property "ki_keywords" "Analog Switch SPST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
		(symbol "TMUX1101DBV_0_1")
		(symbol "TMUX1101DBV_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "4")
			)
			(pin power_in line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "V_{DD}")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMUX1102DBV"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "TMUX1102DBV"
			(at -6.35 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tmux1102.pdf"
			(at 0 -11.43 0)
		)
		(property "Description" "SPST Analog Switch, 1.08V to 5.5V Supply, 3pA Leakage Current, Normally ON, 1.8Ohm Ron, SC-70"
			(at 0 0 0)
		)
		(property "ki_keywords" "Analog Switch SPST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
		(symbol "TMUX1102DBV_0_1")
		(symbol "TMUX1102DBV_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "~")
				(number "4")
			)
			(pin power_in line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "V_{DD}")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMUX154EDGS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 16.51 0)
		)
		(property "Value" "TMUX154EDGS"
			(at 8.89 16.51 0)
		)
		(property "Footprint" "Package_SO:VSSOP-10_3x3mm_P0.5mm"
			(at 20.32 -16.51 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tmux154e.pdf"
			(at 25.4 -19.05 0)
		)
		(property "Description" "ESD-Protected, Low Capacitance, 2-Channel, 2:1 Switch, With Powered-off Protection, VSSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "mux multiplexer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TMUX154EDGS_1_1"
			(pin passive line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "A")
				(number "4")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "B")
				(number "6")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "SEL")
				(number "1")
			)
			(pin passive line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "~{EN}")
				(number "9")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VCC")
				(number "10")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "A0")
				(number "2")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "A1")
				(number "3")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 2.54)
				(name "B0")
				(number "8")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "B1")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMUX154ERSW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 16.51 0)
		)
		(property "Value" "TMUX154ERSW"
			(at 8.89 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:UQFN-10_1.4x1.8mm_P0.4mm"
			(at 25.4 -16.51 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tmux154e.pdf"
			(at 25.4 -19.05 0)
		)
		(property "Description" "ESD-Protected, Low Capacitance, 2-Channel, 2:1 Switch, With Powered-off Protection, UQFN-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "mux multiplexer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UQFN*1.4x1.8mm?P0.4mm*"
			(at 0 0 0)
		)
		(symbol "TMUX154ERSW_1_1"
			(pin passive line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "A")
				(number "3")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "B")
				(number "5")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "SEL")
				(number "10")
			)
			(pin passive line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "~{EN}")
				(number "8")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VCC")
				(number "9")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "A0")
				(number "1")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 2.54)
				(name "B0")
				(number "7")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "B1")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TS3A24159DGS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 7.62 0)
		)
		(property "Value" "TS3A24159DGS"
			(at -3.81 5.715 0)
		)
		(property "Footprint" "Package_SO:TSSOP-10_3x3mm_P0.5mm"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ts3a24159.pdf"
			(at 1.27 -13.335 0)
		)
		(property "Description" "Dual SPDT 0.3Ω Bidirectional Analog Switch, TSSOP-10"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "switch analog SPDT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TS3A24159DGS_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(symbol "TS3A24159DGS_2_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "10")
			)
		)
		(symbol "TS3A24159DGS_3_1"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TS3A24159DRC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 7.62 0)
		)
		(property "Value" "TS3A24159DRC"
			(at -3.81 5.715 0)
		)
		(property "Footprint" "Package_SON:Texas_S-PVSON-N10"
			(at 3.81 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ts3a24159.pdf"
			(at 3.81 -13.335 0)
		)
		(property "Description" "Dual SPDT 0.3Ω Bidirectional Analog Switch, VSON-10"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "switch analog SPDT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*S?PVSON?N10*"
			(at 0 0 0)
		)
		(symbol "TS3A24159DRC_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(symbol "TS3A24159DRC_2_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "10")
			)
		)
		(symbol "TS3A24159DRC_3_1"
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin passive line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "PAD")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TS3A24159YZP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 7.62 0)
		)
		(property "Value" "TS3A24159YZP"
			(at -3.81 5.715 0)
		)
		(property "Footprint" "Package_BGA:Texas_DSBGA-10_1.36x1.86mm_Layout3x4_P0.5mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ts3a24159.pdf"
			(at 1.27 -13.97 0)
		)
		(property "Description" "Dual SPDT 0.3Ω Bidirectional Analog Switch, DSBGA-10"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "switch analog SPDT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DSBGA*1.36x1.86mm*Layout3x4*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TS3A24159YZP_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "C1")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "B1")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "D1")
			)
		)
		(symbol "TS3A24159YZP_2_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "C3")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "B3")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "A3")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "D3")
			)
		)
		(symbol "TS3A24159YZP_3_1"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "D2")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "A2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TS3A27518EPW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 19.05 0)
		)
		(property "Value" "TS3A27518EPW"
			(at 8.89 19.05 0)
		)
		(property "Footprint" "Package_SO:TSSOP-24_4.4x7.8mm_P0.65mm"
			(at 0 25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ts3a27518e.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "6-channel analog mux, TSSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "SPI qSPI multiplexer demux"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x7.8mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TS3A27518EPW_0_1")
		(symbol "TS3A27518EPW_1_1"
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "COM1")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "COM2")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "COM3")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "COM4")
				(number "9")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "COM5")
				(number "10")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "COM6")
				(number "12")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "~{EN}")
				(number "20")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "IN1")
				(number "24")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "IN2")
				(number "14")
			)
			(pin no_connect line
				(at -15.24 -15.24 0)
				(length 2.54)
				(hide yes)
				(name "N.C.")
				(number "3")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "NC1")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "NC2")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "NC3")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "NC4")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "NC5")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "NC6")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "NO1")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "NO2")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "NO3")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "NO4")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "NO5")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "NO6")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TS3A27518ERTW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 19.05 0)
		)
		(property "Value" "TS3A27518ERTW"
			(at 8.89 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:WQFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ts3a27518e.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "6-channel analog mux, WQFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "SPI qSPI multiplexer demux"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WQFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TS3A27518ERTW_0_1")
		(symbol "TS3A27518ERTW_1_1"
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "COM1")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "COM2")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "COM3")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "COM4")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "COM5")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "COM6")
				(number "9")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "~{EN}")
				(number "17")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "IN1")
				(number "21")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "IN2")
				(number "11")
			)
			(pin no_connect line
				(at -15.24 -15.24 0)
				(length 2.54)
				(hide yes)
				(name "N.C.")
				(number "24")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "NC1")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "NC2")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "NC3")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "NC4")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "NC5")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "NC6")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "NO1")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "NO2")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "NO3")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "NO4")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "NO5")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "NO6")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TS3A5017RGY"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 13.97 0)
		)
		(property "Value" "TS3A5017RGY"
			(at 7.62 -13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGY_R-PVQFN-N16_EP2.05x2.55mm"
			(at 0 26.67 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ts3a5017.pdf"
			(at 0 -26.67 0)
		)
		(property "Description" "Dual SP4T Analog Switch Mux Demux, VQFN"
			(at 0 0 0)
		)
		(property "ki_keywords" "Analog switch SP4T"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGY*R*PVQFN*N*"
			(at 0 0 0)
		)
		(symbol "TS3A5017RGY_0_1")
		(symbol "TS3A5017RGY_1_1"
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "1D")
				(number "7")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "2D")
				(number "9")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN2")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IN1")
				(number "14")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "1~{EN}")
				(number "1")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "2~{EN}")
				(number "15")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "V+")
				(number "16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "1S1")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "1S2")
				(number "5")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "1S3")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "1S4")
				(number "3")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "2S1")
				(number "10")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "2S2")
				(number "11")
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "2S3")
				(number "12")
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "2S4")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TS3A5017RSV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 13.97 0)
		)
		(property "Value" "TS3A5017RSV"
			(at 7.62 -13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:UQFN-16_1.8x2.6mm_P0.4mm"
			(at 0 -25.4 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ts3a5017.pdf"
			(at 0 25.4 0)
		)
		(property "Description" "Dual SP4T Analog Switch Mux Demux, UQFN-16"
			(at 0 27.94 0)
		)
		(property "ki_keywords" "Analog switch SP4T"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UQFN*1.8x2.6mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "TS3A5017RSV_0_1")
		(symbol "TS3A5017RSV_1_1"
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "1D")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "2D")
				(number "7")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "1~{EN}")
				(number "15")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IN1")
				(number "12")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "2~{EN}")
				(number "13")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "IN2")
				(number "16")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "V+")
				(number "14")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "1S1")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "1S2")
				(number "3")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "1S3")
				(number "2")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "1S4")
				(number "1")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "2S1")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "2S2")
				(number "9")
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "2S3")
				(number "10")
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "2S4")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TS3DS10224RUK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" "TS3DS10224RUK"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:WQFN-20-1EP_3x3mm_P0.4mm_EP1.7x1.7mm_ThermalVias"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ts3ds10224.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "High-Speed Differential Crosspoint, WQFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "multiplexer demultiplexer 1:4 differential"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WQFN*1EP*3x3mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "TS3DS10224RUK_0_1")
		(symbol "TS3DS10224RUK_1_1"
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "INA+")
				(number "1")
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "INA-")
				(number "2")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "INB+")
				(number "3")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "INB-")
				(number "4")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "SAI")
				(number "14")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "SAO")
				(number "15")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "SBI")
				(number "12")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "SBO")
				(number "11")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "13")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "OUTB0+")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "OUTB0-")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "OUTB1+")
				(number "6")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "OUTB1-")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OUTA0+")
				(number "18")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "OUTA0-")
				(number "17")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "OUTA1+")
				(number "20")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "OUTA1-")
				(number "19")
			)
			(pin input line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "ENA")
				(number "16")
			)
			(pin input line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "ENB")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TS3L501ERUA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 -10.16 0)
		)
		(property "Value" "TS3L501ERUA"
			(at 7.62 -10.16 0)
		)
		(property "Footprint" "Package_DFN_QFN:WQFN-42-1EP_3.5x9mm_P0.5mm_EP2.05x7.55mm"
			(at 27.94 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ts3l501e.pdf"
			(at -5.715 -12.065 0)
		)
		(property "Description" "8-Channel SPDT/16-Bit to 8-Bit Multiplexer and Demultiplexer, Ethernet LAN Switch With Power-Down Mode, WQFN-42"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "gbit base-t lvds lvpecl video"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WQFN*1EP*3.5x9mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TS3L501ERUA_1_1"
			(pin bidirectional line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "A0")
				(number "2")
			)
			(pin bidirectional line
				(at -7.62 0 0)
				(length 2.54)
				(name "A1")
				(number "3")
			)
			(pin bidirectional line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "B0")
				(number "38")
			)
			(pin bidirectional line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "B1")
				(number "37")
			)
			(pin bidirectional line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "C0")
				(number "36")
			)
			(pin bidirectional line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "C1")
				(number "35")
			)
		)
		(symbol "TS3L501ERUA_2_1"
			(pin bidirectional line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "A2")
				(number "6")
			)
			(pin bidirectional line
				(at -7.62 0 0)
				(length 2.54)
				(name "A3")
				(number "7")
			)
			(pin bidirectional line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "B2")
				(number "34")
			)
			(pin bidirectional line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "B3")
				(number "33")
			)
			(pin bidirectional line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "C2")
				(number "32")
			)
			(pin bidirectional line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "C3")
				(number "31")
			)
		)
		(symbol "TS3L501ERUA_3_1"
			(pin bidirectional line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "A4")
				(number "9")
			)
			(pin bidirectional line
				(at -7.62 0 0)
				(length 2.54)
				(name "A5")
				(number "10")
			)
			(pin bidirectional line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "B4")
				(number "29")
			)
			(pin bidirectional line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "B5")
				(number "28")
			)
			(pin bidirectional line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "C4")
				(number "27")
			)
			(pin bidirectional line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "C5")
				(number "26")
			)
		)
		(symbol "TS3L501ERUA_4_1"
			(pin bidirectional line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "A6")
				(number "11")
			)
			(pin bidirectional line
				(at -7.62 0 0)
				(length 2.54)
				(name "A7")
				(number "12")
			)
			(pin bidirectional line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "B6")
				(number "25")
			)
			(pin bidirectional line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "B7")
				(number "24")
			)
			(pin bidirectional line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "C6")
				(number "23")
			)
			(pin bidirectional line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "C7")
				(number "22")
			)
		)
		(symbol "TS3L501ERUA_5_1"
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "LED_A0")
				(number "15")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "LED_A1")
				(number "16")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "LED_A2")
				(number "42")
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "LED_B0")
				(number "17")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "LED_B1")
				(number "18")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "LED_B2")
				(number "41")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "LED_C0")
				(number "19")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "LED_C1")
				(number "20")
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "LED_C2")
				(number "40")
			)
		)
		(symbol "TS3L501ERUA_6_0")
		(symbol "TS3L501ERUA_6_1"
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "PD")
				(number "5")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SEL")
				(number "13")
			)
			(pin power_in line
				(at -7.62 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "43")
			)
			(pin power_in line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "21")
			)
			(pin power_in line
				(at 5.08 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "30")
			)
			(pin power_in line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "39")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TS5A23159DGS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "TS5A23159DGS"
			(at -5.08 6.985 0)
		)
		(property "Footprint" "Package_SO:VSSOP-10_3x3mm_P0.5mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ts5a23159.pdf"
			(at 1.27 -13.97 0)
		)
		(property "Description" "Dual SPDT 1ohm Bidirectional Analog Switch with Off protection, VSSOP-10"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "switch analog SPDT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TS5A23159DGS_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(symbol "TS5A23159DGS_2_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(symbol "TS5A23159DGS_3_1"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TS5A23159RSE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "TS5A23159RSE"
			(at -5.08 6.985 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_R-PUQFN-N10"
			(at 1.27 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ts5a23159.pdf"
			(at 1.27 -12.065 0)
		)
		(property "Description" "Dual SPDT 1ohm Bidirectional Analog Switch with Off protection, UQFN-10"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "switch analog SPDT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas?R*PUQFN*"
			(at 0 0 0)
		)
		(symbol "TS5A23159RSE_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(symbol "TS5A23159RSE_2_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(symbol "TS5A23159RSE_3_1"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TS5A3159AYZPR"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 7.239 0)
		)
		(property "Value" "TS5A3159AYZPR"
			(at -3.175 5.461 0)
		)
		(property "Footprint" "Package_BGA:Texas_DSBGA-6_0.9x1.4mm_Layout2x3_P0.5mm"
			(at 1.27 -14.605 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ts5a3159a.pdf"
			(at 1.27 -12.065 0)
		)
		(property "Description" "Single SPDT Analog Switch, 1.65-V to 5.5-V Single-Supply Operation, 1Ohm Ron, DSBGA-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DSBGA*0.9x1.4mm*2x3*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TS5A3159AYZPR_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "C2")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "A2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "C1")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "A1")
			)
		)
		(symbol "TS5A3159AYZPR_2_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "B2")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "B1")
			)
		)
		(symbol "TS5A3159AYZPR_2_1")
		(embedded_fonts no)
	)
	(symbol "TS5A3159DBV"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 7.239 0)
		)
		(property "Value" "TS5A3159DBV"
			(at -3.175 5.461 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -14.605 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ts5a3159.pdf"
			(at 1.27 -12.065 0)
		)
		(property "Description" "Single SPDT Analog Switch, 1.65-V to 5.5-V Single-Supply Operation, 1Ohm Ron, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TS5A3159DBV_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "TS5A3159DBV_2_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "5")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
		)
		(symbol "TS5A3159DBV_2_1")
		(embedded_fonts no)
	)
	(symbol "TS5A3166DBVR"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "TS5A3166DBVR"
			(at 3.81 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -1.27 -3.81 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ts5a3166.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Single SPST Analog Switch, 5-V/3.3-V, normally OFF, 0.9Ohm Ron, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Analog Switch SPST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TS5A3166DBVR_0_1")
		(symbol "TS5A3166DBVR_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin power_in line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "V+")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TS5A3166DCKR"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "TS5A3166DCKR"
			(at 3.81 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at -1.27 -3.81 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ts5a3166.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Single SPST Analog Switch, 5-V/3.3-V, normally OFF, 0.9Ohm Ron, SC-70"
			(at 0 0 0)
		)
		(property "ki_keywords" "Analog Switch SPST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70?5*"
			(at 0 0 0)
		)
		(symbol "TS5A3166DCKR_0_1")
		(symbol "TS5A3166DCKR_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin power_in line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "V+")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADG1207BCPZ"
		(extends "ADG1607xCP")
		(property "Reference" "U"
			(at -15.24 34.29 0)
		)
		(property "Value" "ADG1207BCPZ"
			(at 10.16 34.29 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADG1206_1207.pdf"
			(at 0 0 0)
		)
		(property "Description" "Differential 8-channel ±5V, +12V, +5V, and +3.3V iCMOS analog multiplexer, 4.5 Ohm Ron, 37 MHz, LFCSP-32 5x5mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "analog switch multiplexer DP8T"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP?32*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADG417BN"
		(extends "DG418xJ")
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "ADG417BN"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADG417.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single SPST Monolithic LC²MOS Analog Switch, normally OFF, 25Ohm Ron, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADG417BR"
		(extends "DG418xY")
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "ADG417BR"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADG417.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single SPST Monolithic LC²MOS Analog Switch, normally OFF, 25Ohm Ron, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADG419BN"
		(extends "DG419xJ")
		(property "Reference" "U"
			(at -3.175 7.493 0)
		)
		(property "Value" "ADG419BN"
			(at -3.175 5.715 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 3.81 -14.605 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADG419.pdf"
			(at 3.81 -12.065 0)
		)
		(property "Description" "Single SPDT Monolithic LC²MOS Analog Switch, 25Ohm Ron, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADG419BR"
		(extends "DG419xY")
		(property "Reference" "U"
			(at -3.175 4.699 0)
		)
		(property "Value" "ADG419BR"
			(at -3.175 2.921 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 3.175 -13.335 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADG419.pdf"
			(at 3.175 -11.43 0)
		)
		(property "Description" "Single SPDT Monolithic LC²MOS Analog Switch, 25Ohm Ron, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADG733BRU"
		(extends "ADG633YRU")
		(property "Reference" "U"
			(at -3.048 7.874 0)
		)
		(property "Value" "ADG733BRU"
			(at -3.048 6.096 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 3.81 -13.97 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADG733_734.pdf"
			(at 3.81 -11.43 0)
		)
		(property "Description" "Triple SPDT CMOS Analog Switch, 2.5Ohm Ron, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "CD4066BM"
		(extends "CD4066BE")
		(property "Reference" "U"
			(at -5.08 3.81 0)
		)
		(property "Value" "CD4066BM"
			(at 7.62 3.81 0)
		)
		(property "Footprint" "Package_SO:SO-14_3.9x8.65mm_P1.27mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/cd4066b.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad 20V analog SPST 1:1 switch, SO-14 (3.9x8.65mm)"
			(at 0 0 0)
		)
		(property "ki_keywords" "analog switch selector multiplexer spst mux amux"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*3.9x8.65mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "CD4066BNS"
		(extends "CD4066BE")
		(property "Reference" "U"
			(at -5.08 3.81 0)
		)
		(property "Value" "CD4066BNS"
			(at 7.62 3.81 0)
		)
		(property "Footprint" "Package_SO:SO-14_5.3x10.2mm_P1.27mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/cd4066b.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad 20V analog SPST 1:1 switch, SO-14 (5.3x10.2mm)"
			(at 0 0 0)
		)
		(property "ki_keywords" "analog switch selector multiplexer spst mux amux"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*5.3x10.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "CD4066BPW"
		(extends "CD4066BE")
		(property "Reference" "U"
			(at -5.08 3.81 0)
		)
		(property "Value" "CD4066BPW"
			(at 7.62 3.81 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/cd4066b.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad 20V analog SPST 1:1 switch, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "analog switch selector multiplexer spst mux amux"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "DG441xJ"
		(extends "DG309xJ")
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "DG441xJ"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DG441-DG442.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad SPST Analog Switches, normally ON, 60Ohm Ron, DIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "DG441xY"
		(extends "DG309xY")
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "DG441xY"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DG441-DG442.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad SPST Analog Switches, normally ON, 60Ohm Ron, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "DG442xJ"
		(extends "DG308AxJ")
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "DG442xJ"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DG441-DG442.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad SPST Analog Switches, normally OFF, 60Ohm Ron, DIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "DG442xY"
		(extends "DG308AxY")
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "DG442xY"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DG441-DG442.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad SPST Analog Switches, normally OFF, 60Ohm Ron, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "FSA3157L6X"
		(extends "NC7SB3157L6X")
		(property "Reference" "U"
			(at -3.175 7.493 0)
		)
		(property "Value" "FSA3157L6X"
			(at -3.175 5.715 0)
		)
		(property "Footprint" "Package_SON:Fairchild_MicroPak-6_1.0x1.45mm_P0.5mm"
			(at 0.635 -13.335 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NC7SB3157-D.PDF"
			(at 0.635 -11.43 0)
		)
		(property "Description" "Single SPDT Low-Voltage Analog Switch or 2:1 Multiplexer/De-Multiplexer Bus Switch, 10Ohm Ron, MicroPak-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Fairchild*MicroPak*1.0x1.45mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "FSA3157P6X"
		(extends "NC7SB3157P6X")
		(property "Reference" "U"
			(at -3.175 7.493 0)
		)
		(property "Value" "FSA3157P6X"
			(at -3.175 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0.635 -13.335 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NC7SB3157-D.PDF"
			(at 0.635 -11.43 0)
		)
		(property "Description" "Single SPDT Low-Voltage Analog Switch or 2:1 Multiplexer/De-Multiplexer Bus Switch, 10Ohm Ron, SC-70-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "MAX312CPE"
		(extends "DG411xJ")
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "MAX312CPE"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX312-MAX314.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad SPST CMOS Analog Switches, normally ON, 6.5Ohm Ron, DIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX312CSE"
		(extends "DG411xY")
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "MAX312CSE"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX312-MAX314.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad SPST CMOS Analog Switches, normally ON, 6.5Ohm Ron, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX312CUE"
		(extends "DG411xUE")
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "MAX312CUE"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX312-MAX314.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad SPST CMOS Analog Switches, normally ON, 6.5Ohm Ron, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX313CPE"
		(extends "DG412xJ")
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "MAX313CPE"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX312-MAX314.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad SPST CMOS Analog Switches, normally OFF, 6.5Ohm Ron, DIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX313CSE"
		(extends "DG412xY")
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "MAX313CSE"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX312-MAX314.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad SPST CMOS Analog Switches, normally OFF, 6.5Ohm Ron, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX313CUE"
		(extends "DG412xUE")
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "MAX313CUE"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX312-MAX314.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad SPST CMOS Analog Switches, normally OFF, 6.5Ohm Ron, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX314CPE"
		(extends "DG413xJ")
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "MAX314CPE"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX312-MAX314.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad SPST CMOS Analog Switches, normally 2xON + 2xOFF, 6.5Ohm Ron, DIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX314CSE"
		(extends "DG413xY")
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "MAX314CSE"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX312-MAX314.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad SPST CMOS Analog Switches, normally 2xON + 2xOFF, 6.5Ohm Ron, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX314CUE"
		(extends "DG413xUE")
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "MAX314CUE"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX312-MAX314.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad SPST CMOS Analog Switches, normally 2xON + 2xOFF, 6.5Ohm Ron, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX317xPA"
		(extends "DG417xJ")
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "MAX317xPA"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX317-MAX319.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single SPST Monolithic CMOS Analog Switch, normally ON, 20Ohm Ron, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX317xSA"
		(extends "DG417xY")
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "MAX317xSA"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX317-MAX319.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single SPST Monolithic CMOS Analog Switch, normally ON, 20Ohm Ron, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX318xPA"
		(extends "DG418xJ")
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "MAX318xPA"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX317-MAX319.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single SPST Monolithic CMOS Analog Switch, normally OFF, 20Ohm Ron, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX318xSA"
		(extends "DG418xY")
		(property "Reference" "U"
			(at -3.175 5.334 0)
		)
		(property "Value" "MAX318xSA"
			(at -3.175 3.556 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX317-MAX319.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single SPST Monolithic CMOS Analog Switch, normally OFF, 20Ohm Ron, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX319xPA"
		(extends "DG419xJ")
		(property "Reference" "U"
			(at -3.175 7.493 0)
		)
		(property "Value" "MAX319xPA"
			(at -3.175 5.715 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0.635 -8.255 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX317-MAX319.pdf"
			(at 0.635 -5.715 0)
		)
		(property "Description" "Single SPDT Monolithic CMOS Analog Switch, 20Ohm Ron, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX319xSA"
		(extends "DG419xY")
		(property "Reference" "U"
			(at -3.175 4.699 0)
		)
		(property "Value" "MAX319xSA"
			(at -3.175 2.921 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 3.175 -13.335 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX317-MAX319.pdf"
			(at 3.175 -11.43 0)
		)
		(property "Description" "Single SPDT Monolithic CMOS Analog Switch, 20Ohm Ron, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX394"
		(extends "MAX333A")
		(property "Reference" "U"
			(at -3.175 7.493 0)
		)
		(property "Value" "MAX394"
			(at -3.175 5.715 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX394.pdf"
			(at 3.175 -12.065 0)
		)
		(property "Description" "Quad SPDT CMOS Analog Switch, 35Ohm Ron, DIP-20/SOIC-20/SSOP-20/TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm* SSOP*5.3x7.2mm*P0.65mm* SOIC*7.5x10.3mm*P1.27mm* DIP*W7.62mm* SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TMUX1101DCK"
		(extends "TMUX1101DBV")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "TMUX1101DCK"
			(at -12.7 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tmux1101.pdf"
			(at 0 -11.43 0)
		)
		(property "Description" "SPST Analog Switch, 1.08V to 5.5V Supply, 3pA Leakage Current, Normally OFF, 1.8Ohm Ron, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Analog Switch SPST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TMUX1102DCK"
		(extends "TMUX1102DBV")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "TMUX1102DCK"
			(at -6.35 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tmux1102.pdf"
			(at 0 -11.43 0)
		)
		(property "Description" "SPST Analog Switch, 1.08V to 5.5V Supply, 3pA Leakage Current, Normally ON, 1.8Ohm Ron, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Analog Switch SPST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TMUX1108PW"
		(extends "ADG1408YRUZ")
		(property "Reference" "U"
			(at -10.16 16.51 0)
		)
		(property "Value" "TMUX1108PW"
			(at 3.81 16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tmux1108.pdf"
			(at 0 0 0)
		)
		(property "Description" "5V / ±2.5V, Low-Leakage-Current, 8:1 Precision Multiplexer, 2.5 Ohm Ron, 90Mhz, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "analog switch selector multiplexer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TS3A5223RSW"
		(extends "TS3A24159DGS")
		(property "Reference" "U"
			(at -3.81 7.62 0)
		)
		(property "Value" "TS3A5223RSW"
			(at -3.81 5.715 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RSW0010A_UQFN-10_1.4x1.8mm_P0.4mm"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ts3a5223.pdf"
			(at 1.27 -13.335 0)
		)
		(property "Description" "Dual SPDT 0.45..0.85mΩ Bidirectional Analog switch, 1.65..3.6V supply, UQFN-10"
			(at 1.27 -15.494 0)
		)
		(property "ki_keywords" "MUX DEMUX Texas"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*UQFN*1.4*1.8*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "TS5A3159ADBVR"
		(extends "TS5A3159DBV")
		(property "Reference" "U"
			(at -3.175 4.699 0)
		)
		(property "Value" "TS5A3159ADBVR"
			(at -3.175 2.921 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0.635 -13.335 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ts5a3159a.pdf"
			(at 0.635 -11.43 0)
		)
		(property "Description" "Single SPDT Analog Switch, 1.65-V to 5.5-V Single-Supply Operation, 1Ohm Ron, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TS5A3159ADCK"
		(extends "NC7SB3157P6X")
		(property "Reference" "U"
			(at -3.175 4.699 0)
		)
		(property "Value" "TS5A3159ADCK"
			(at -3.175 2.921 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0.635 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ts5a3159a.pdf"
			(at 0.635 -11.43 0)
		)
		(property "Description" "Single SPDT Analog Switch, 1.65-V to 5.5-V Single-Supply Operation, 1Ohm Ron, SC-70-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "TS5A3159DCK"
		(extends "NC7SB3157P6X")
		(property "Reference" "U"
			(at -3.175 7.493 0)
		)
		(property "Value" "TS5A3159DCK"
			(at -3.175 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0.635 -13.335 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ts5a3159.pdf"
			(at 0.635 -11.43 0)
		)
		(property "Description" "Single SPDT Analog Switch, 1.65-V to 5.5-V Single-Supply Operation, 1Ohm Ron, SC-70-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Analog Switch SPDT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "TS5A3160DBV"
		(extends "TS5A3159DBV")
		(property "Reference" "U"
			(at -3.175 4.699 0)
		)
		(property "Value" "TS5A3160DBV"
			(at -3.175 2.921 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0.635 -13.335 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ts5a3160.pdf"
			(at 0.635 -11.43 0)
		)
		(property "Description" "Single SPDT Analog Switch, 1.65-V to 5.5-V Single-Supply Operation, 1Ohm Ron, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TS5A3160DCK"
		(extends "NC7SB3157P6X")
		(property "Reference" "U"
			(at -3.175 7.493 0)
		)
		(property "Value" "TS5A3160DCK"
			(at -3.175 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0.635 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ts5a3160.pdf"
			(at 0.635 -12.065 0)
		)
		(property "Description" "Single SPDT Analog Switch, 1.65-V to 5.5-V Single-Supply Operation, 1Ohm Ron, SC-70-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "TS5A63157DBV"
		(extends "TS5A3159DBV")
		(property "Reference" "U"
			(at -3.175 4.699 0)
		)
		(property "Value" "TS5A63157DBV"
			(at -3.175 2.921 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -13.335 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ts5a63157.pdf"
			(at 1.27 -11.43 0)
		)
		(property "Description" "Single SPDT Analog Switch, 5V/3.3V Single-Supply Operation, 12Ohm Ron, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Analog Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
)
