(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "AD1853"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 11.43 24.13 0)
		)
		(property "Value" "AD1853"
			(at 11.43 21.59 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at 11.43 -25.4 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD1853.pdf"
			(at 0 0 0)
		)
		(property "Description" "Stereo, 24-Bit, 192 kHz, Multibit Sigma-Delta DAC, SSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio dac 2ch 24bit 192kHz"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x10.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AD1853_0_1")
		(symbol "AD1853_1_1"
			(pin input line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "MCLK")
				(number "2")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "BCLK")
				(number "26")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "L/~{R}CLK")
				(number "25")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "SDATA")
				(number "27")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "INT4X")
				(number "6")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "INT2X")
				(number "7")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "IDPM0")
				(number "21")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "IDPM1")
				(number "20")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "CCLK")
				(number "4")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "CDATA")
				(number "5")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "CLATCH")
				(number "3")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "~{RST}")
				(number "24")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "MUTE")
				(number "23")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "DEEMP")
				(number "9")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 2.54)
				(name "DVDD")
				(number "28")
			)
			(pin power_in line
				(at -2.54 -22.86 90)
				(length 2.54)
				(name "DGND")
				(number "1")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "AVDD")
				(number "18")
			)
			(pin power_in line
				(at 2.54 -22.86 90)
				(length 2.54)
				(name "AGND")
				(number "11")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "OUTL+")
				(number "12")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "OUTL-")
				(number "13")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "ZEROL")
				(number "22")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "OUTR+")
				(number "17")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "OUTR-")
				(number "16")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "ZEROR")
				(number "8")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "FILTR")
				(number "14")
			)
			(pin passive line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "IREF")
				(number "10")
			)
			(pin output line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "FILTB")
				(number "19")
			)
			(pin output line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "FCR")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD1855"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 11.43 24.13 0)
		)
		(property "Value" "AD1855"
			(at 11.43 21.59 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at 5.08 -25.4 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD1855.pdf"
			(at 0 0 0)
		)
		(property "Description" "Stereo, 96 kHz, Multibit Sigma-Delta DAC, SSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio dac 2ch 24bit 96kHz"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x10.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AD1855_0_1")
		(symbol "AD1855_1_1"
			(pin input line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "MCLK")
				(number "2")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "BCLK")
				(number "26")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "L/~{R}CLK")
				(number "25")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "SDATA")
				(number "27")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "384/~{256}")
				(number "6")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "96/~{48}")
				(number "10")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "X2MCLK")
				(number "7")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "IDPM0")
				(number "21")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "IDPM1")
				(number "20")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "CCLK")
				(number "4")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "CDATA")
				(number "5")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "CLATCH")
				(number "3")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "~{PD/RST}")
				(number "24")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "MUTE")
				(number "23")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "DEEMP")
				(number "9")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 2.54)
				(name "DVDD")
				(number "28")
			)
			(pin power_in line
				(at -2.54 -22.86 90)
				(length 2.54)
				(name "DGND")
				(number "1")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "AVDD")
				(number "18")
			)
			(pin power_in line
				(at 2.54 -22.86 90)
				(length 2.54)
				(name "AGND")
				(number "11")
			)
			(pin passive line
				(at 2.54 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "15")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "OUTL+")
				(number "17")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "OUTL-")
				(number "16")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "ZEROL")
				(number "22")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "OUTR+")
				(number "12")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "OUTR-")
				(number "13")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "ZEROR")
				(number "8")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "FILTR")
				(number "14")
			)
			(pin output line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "FILTB")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD1955"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 11.43 26.67 0)
		)
		(property "Value" "AD1955"
			(at 11.43 24.13 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD1955.pdf"
			(at 0 0 0)
		)
		(property "Description" "High Performance Multibit Sigma-Delta DAC with SACD Playback, SSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio dac 2ch 24bit 192kHz"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x10.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AD1955_0_1")
		(symbol "AD1955_1_1"
			(pin input line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "MCLK")
				(number "27")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "BCLK/EF_BCLK")
				(number "3")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "LRCLK/EF_WCLK")
				(number "2")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "SDATA/EF_LDATA")
				(number "4")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "EF_RDATA")
				(number "5")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "DSD_SCLK")
				(number "6")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "DSD_LDATA")
				(number "7")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "DSD_RDATA")
				(number "8")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "DSD_PHASE")
				(number "9")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "CCLK")
				(number "26")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "CDATA")
				(number "24")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "~{CLATCH}")
				(number "25")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "~{PD/RST}")
				(number "23")
			)
			(pin input line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "MUTE")
				(number "22")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "DVDD")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -25.4 90)
				(length 2.54)
				(name "DGND")
				(number "28")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "AVDD")
				(number "15")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "AGND")
				(number "10")
			)
			(pin passive line
				(at 2.54 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "19")
			)
			(pin output line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "OUTL+")
				(number "18")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "OUTL-")
				(number "17")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "ZEROL")
				(number "21")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "OUTR+")
				(number "11")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "OUTR-")
				(number "12")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "ZEROR")
				(number "20")
			)
			(pin output line
				(at 17.78 0 180)
				(length 2.54)
				(name "FILTR")
				(number "13")
			)
			(pin passive line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "IREF")
				(number "14")
			)
			(pin output line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "FILTB")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADAU1978xBCP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 12.7 25.4 0)
		)
		(property "Value" "ADAU1978xBCP"
			(at 12.7 22.86 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-40-1EP_6x6mm_P0.5mm_EP3.9x3.9mm"
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADAU1978.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "Quad Analog-to-Digital Converter, 2Vrms differential inputs, LFCSP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Audio ADC I2S TDM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*6x6mm*P0.5mm*EP3.9x3.9mm*"
			(at 0 0 0)
		)
		(symbol "ADAU1978xBCP_0_1")
		(symbol "ADAU1978xBCP_1_1"
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "AIN1P")
				(number "33")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "AIN1N")
				(number "32")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "AIN2P")
				(number "35")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "AIN2N")
				(number "34")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "AIN3P")
				(number "37")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "AIN3N")
				(number "36")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "AIN4P")
				(number "39")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "AIN4N")
				(number "38")
			)
			(pin output line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "VREF")
				(number "2")
			)
			(pin output line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PLL_FILT")
				(number "3")
			)
			(pin no_connect line
				(at -10.16 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "23")
			)
			(pin no_connect line
				(at -7.62 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "24")
			)
			(pin no_connect line
				(at -5.08 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "25")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 2.54)
				(hide yes)
				(name "AVDD")
				(number "31")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 2.54)
				(name "AVDD")
				(number "4")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 2.54)
				(hide yes)
				(name "AVDD")
				(number "40")
			)
			(pin power_in line
				(at -2.54 -22.86 90)
				(length 2.54)
				(name "AGND")
				(number "1")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "21")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "22")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "28")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "29")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "5")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "EP")
				(number "41")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "IOVDD")
				(number "12")
			)
			(pin power_in line
				(at 2.54 -22.86 90)
				(length 2.54)
				(name "DGND")
				(number "11")
			)
			(pin no_connect line
				(at 5.08 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "26")
			)
			(pin no_connect line
				(at 7.62 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "27")
			)
			(pin no_connect line
				(at 10.16 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "30")
			)
			(pin no_connect line
				(at 12.7 17.78 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin input line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "MCLKIN")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "LRCLK")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "BCLK")
				(number "16")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "SDATAOUT1")
				(number "13")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "SDATAOUT2")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "SDA")
				(number "17")
				(alternate "COUT" output line)
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "SCL")
				(number "18")
				(alternate "CCLK" input line)
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "ADDR0")
				(number "19")
				(alternate "~{CLATCH}" input line)
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "ADDR1")
				(number "20")
				(alternate "CIN" input line)
			)
			(pin input line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "SA_MODE")
				(number "9")
			)
			(pin input line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "~{PD}/~{RST}")
				(number "6")
			)
			(pin power_out line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "DVDD")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AK5392VS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 10.16 29.21 0)
		)
		(property "Value" "AK5392VS"
			(at 10.16 26.67 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x18.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://media.digikey.com/pdf/Data%20Sheets/AKM%20Semiconductor%20Inc.%20PDFs/AK5392.pdf"
			(at 19.05 -7.62 0)
		)
		(property "Description" "Enhanced Dual Bit Sigma-Delta 24Bit ADC, SOIC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio adc 2ch 24bit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x18.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "AK5392VS_0_1")
		(symbol "AK5392VS_1_1"
			(pin output line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "VREFL")
				(number "1")
			)
			(pin power_in line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "GNDL")
				(number "2")
			)
			(pin output line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "VCOML")
				(number "3")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "AINL-")
				(number "5")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "AINL+")
				(number "4")
			)
			(pin output line
				(at -17.78 0 0)
				(length 2.54)
				(name "VREFR")
				(number "28")
			)
			(pin output line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "GNDR")
				(number "27")
			)
			(pin output line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "VCOMR")
				(number "26")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "AINR-")
				(number "24")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "AINR+")
				(number "25")
			)
			(pin input line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "ZCAL")
				(number "6")
			)
			(pin power_in line
				(at -5.08 -27.94 90)
				(length 2.54)
				(name "AGND")
				(number "22")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VA")
				(number "23")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "BGND")
				(number "21")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VD")
				(number "7")
			)
			(pin power_in line
				(at 5.08 -27.94 90)
				(length 2.54)
				(name "DGND")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "SCLK")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "LRCK")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "FSYNC")
				(number "16")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "SDATA")
				(number "15")
			)
			(pin input line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "SMODE1")
				(number "12")
			)
			(pin input line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "SMODE2")
				(number "11")
			)
			(pin input line
				(at 17.78 0 180)
				(length 2.54)
				(name "CLK")
				(number "17")
			)
			(pin input line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "CMODE")
				(number "18")
			)
			(pin input line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "TEST")
				(number "20")
			)
			(pin input line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "HPFE")
				(number "19")
			)
			(pin input line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "~{RST}")
				(number "10")
			)
			(pin output line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "CAL")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AK5393VS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 10.16 29.21 0)
		)
		(property "Value" "AK5393VS"
			(at 10.16 26.67 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x18.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.akm.com/akm/en/file/datasheet/AK5393VS.pdf"
			(at 21.59 -10.16 0)
		)
		(property "Description" "Enhanced Dual Bit Sigma-Delta 96kHz 24-Bit ADC, SOIC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio adc 2ch 24bit 96kHz"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x18.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "AK5393VS_0_1")
		(symbol "AK5393VS_1_1"
			(pin output line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "VREFL")
				(number "1")
			)
			(pin power_in line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "GNDL")
				(number "2")
			)
			(pin output line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "VCOML")
				(number "3")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "AINL-")
				(number "5")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "AINL+")
				(number "4")
			)
			(pin output line
				(at -17.78 0 0)
				(length 2.54)
				(name "VREFR")
				(number "28")
			)
			(pin output line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "GNDR")
				(number "27")
			)
			(pin output line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "VCOMR")
				(number "26")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "AINR-")
				(number "24")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "AINR+")
				(number "25")
			)
			(pin input line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "ZCAL")
				(number "6")
			)
			(pin power_in line
				(at -5.08 -27.94 90)
				(length 2.54)
				(name "AGND")
				(number "22")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VA")
				(number "23")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "BGND")
				(number "21")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VD")
				(number "7")
			)
			(pin power_in line
				(at 5.08 -27.94 90)
				(length 2.54)
				(name "DGND")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "SCLK")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "LRCK")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "FSYNC")
				(number "16")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "SDATA")
				(number "15")
			)
			(pin input line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "SMODE1")
				(number "12")
			)
			(pin input line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "SMODE2")
				(number "11")
			)
			(pin input line
				(at 17.78 0 180)
				(length 2.54)
				(name "MCLK")
				(number "17")
			)
			(pin input line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "DFS")
				(number "18")
			)
			(pin input line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "TEST")
				(number "20")
			)
			(pin input line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "HPFE")
				(number "19")
			)
			(pin input line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "~{RST}")
				(number "10")
			)
			(pin output line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "CAL")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AK5394AVS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 10.16 29.21 0)
		)
		(property "Value" "AK5394AVS"
			(at 10.16 26.67 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x18.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.akm.com/akm/en/file/datasheet/AK5394AVS.pdf"
			(at 21.59 -10.16 0)
		)
		(property "Description" "Super High Performance 192kHz 24-Bit Sigma-Delta ADC, SOIC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio adc 2ch 24bit 192kHz"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x18.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "AK5394AVS_0_1")
		(symbol "AK5394AVS_1_1"
			(pin output line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "VREFL+")
				(number "1")
			)
			(pin output line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "VREFL-")
				(number "2")
			)
			(pin output line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "VCOML")
				(number "3")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "AINL-")
				(number "5")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "AINL+")
				(number "4")
			)
			(pin output line
				(at -17.78 0 0)
				(length 2.54)
				(name "VREFR+")
				(number "28")
			)
			(pin output line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "VREFR-")
				(number "27")
			)
			(pin output line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "VCOMR")
				(number "26")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "AINR-")
				(number "24")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "AINR+")
				(number "25")
			)
			(pin input line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "ZCAL")
				(number "6")
			)
			(pin power_in line
				(at -5.08 -27.94 90)
				(length 2.54)
				(name "AGND")
				(number "22")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VA")
				(number "23")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "BGND")
				(number "21")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VD")
				(number "7")
			)
			(pin power_in line
				(at 5.08 -27.94 90)
				(length 2.54)
				(name "DGND")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "SCLK")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "LRCK")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "FSYNC")
				(number "16")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "SDATA")
				(number "15")
			)
			(pin input line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "SMODE1")
				(number "12")
			)
			(pin input line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "SMODE2")
				(number "11")
			)
			(pin input line
				(at 17.78 0 180)
				(length 2.54)
				(name "MCLK")
				(number "17")
			)
			(pin input line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "DFS0")
				(number "18")
			)
			(pin input line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "DFS1")
				(number "20")
			)
			(pin input line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "HPFE")
				(number "19")
			)
			(pin input line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "~{RST}")
				(number "10")
			)
			(pin output line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "CAL")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AK5720VT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 16.51 0)
		)
		(property "Value" "AK5720VT"
			(at 8.89 16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.akm.com/akm/en/file/datasheet/AK5720VT.pdf"
			(at 17.78 -3.81 0)
		)
		(property "Description" "Stereo, 96kHz, 24-Bit, Delta-Sigma ADC, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio adc 2ch 24bit 96kHz I2S MSB TDM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AK5720VT_0_1")
		(symbol "AK5720VT_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "RIN")
				(number "2")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "LIN")
				(number "3")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "VCOM")
				(number "1")
			)
			(pin passive line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "REGO")
				(number "8")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 2.54)
				(name "VA")
				(number "5")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "VD")
				(number "6")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "MCLK")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "BICK")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "LRCLK")
				(number "10")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "SDTO")
				(number "9")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "~{PDN}")
				(number "13")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "GSEL")
				(number "7")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "FSEL")
				(number "15")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "DIF/TDMI")
				(number "14")
			)
			(pin input line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "CKS")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AK7742EQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 36.83 0)
		)
		(property "Value" "AK7742EQ"
			(at 13.97 36.83 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.akm.com/akm/en/file/datasheet/AK7742EQ.pdf"
			(at -21.59 0 0)
		)
		(property "Description" "24bit 2ch ADC + 24bit 4ch DAC with Audio DSP, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio adc 2ch dac 4ch dsp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AK7742EQ_0_1")
		(symbol "AK7742EQ_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "AIN1LP")
				(number "47")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "AIN1LN")
				(number "46")
			)
			(pin input line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "AIN1RP")
				(number "45")
			)
			(pin input line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "AIN1RN")
				(number "44")
			)
			(pin input line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "AIN2L")
				(number "3")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "AIN2R")
				(number "2")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "AIN3L")
				(number "1")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "AIN3R")
				(number "48")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "XTI")
				(number "11")
			)
			(pin output line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "XTO")
				(number "12")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "~{IRESET}")
				(number "18")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "SDA")
				(number "26")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "SCL")
				(number "27")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "I2CSEL")
				(number "19")
			)
			(pin input line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "CAD0")
				(number "28")
			)
			(pin input line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "CAD1")
				(number "29")
			)
			(pin input line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "CKM0")
				(number "17")
			)
			(pin input line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "CKM1")
				(number "16")
			)
			(pin input line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "CKM2")
				(number "8")
			)
			(pin power_in line
				(at -5.08 38.1 270)
				(length 2.54)
				(name "DVDD")
				(number "9")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "DVDD")
				(number "20")
			)
			(pin power_in line
				(at -2.54 -38.1 90)
				(length 2.54)
				(name "VSS2")
				(number "10")
			)
			(pin passive line
				(at -2.54 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS2")
				(number "21")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "AVDD")
				(number "4")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(name "TEST1")
				(number "7")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "AVDD")
				(number "32")
			)
			(pin passive line
				(at 2.54 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS1")
				(number "30")
			)
			(pin passive line
				(at 2.54 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS1")
				(number "41")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 2.54)
				(name "VSS1")
				(number "5")
			)
			(pin power_in line
				(at 5.08 38.1 270)
				(length 2.54)
				(name "AVDD")
				(number "43")
			)
			(pin output line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "AOUT1LP")
				(number "40")
			)
			(pin output line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "AOUT1LN")
				(number "39")
			)
			(pin output line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "AOUT1RP")
				(number "38")
			)
			(pin output line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "AOUT1RN")
				(number "37")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "AOUT2LP")
				(number "36")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "AOUT2LN")
				(number "35")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "AOUT2RP")
				(number "34")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "AOUT2RN")
				(number "33")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "BICK")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "LRCK")
				(number "22")
			)
			(pin input line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "SDIN1/JX1")
				(number "14")
			)
			(pin input line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "SDIN2/JX2")
				(number "15")
			)
			(pin output line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "SDOUT1")
				(number "13")
			)
			(pin output line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "SO/RDY/GPO/SDOUT2")
				(number "25")
			)
			(pin output line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "CLKO/SDOUT3")
				(number "24")
			)
			(pin passive line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "LFLT")
				(number "6")
			)
			(pin passive line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "AVDRV")
				(number "31")
			)
			(pin passive line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "VCOM")
				(number "42")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AS3310"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 17.78 0)
		)
		(property "Value" "AS3310"
			(at 5.08 17.78 0)
		)
		(property "Footprint" ""
			(at 15.24 -7.62 0)
		)
		(property "Datasheet" "http://www.alfarzpp.lv/eng/sc/AS3310.pdf"
			(at 16.51 -12.7 0)
		)
		(property "Description" "ADSR Voltage Controlled Envelope Generator, DIP-16/SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "VCEG CEM3310 ALFA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "AS3310_0_1")
		(symbol "AS3310_1_1"
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "VP")
				(number "3")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "GATE")
				(number "4")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "TRIG")
				(number "5")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VCA")
				(number "15")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VCD")
				(number "12")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "VCS")
				(number "9")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "VCR")
				(number "13")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "IIN")
				(number "10")
			)
			(pin passive line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "CCOMP")
				(number "8")
			)
			(pin passive line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "CAP")
				(number "1")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VCC")
				(number "11")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VEE")
				(number "6")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "PGND")
				(number "7")
			)
			(pin power_in line
				(at 5.08 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "14")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "ENVOUT")
				(number "2")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "ATKOUT")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AS3320"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 17.78 0)
		)
		(property "Value" "AS3320"
			(at 5.08 17.78 0)
		)
		(property "Footprint" "Package_DIP:DIP-18_W7.62mm"
			(at 15.24 -7.62 0)
		)
		(property "Datasheet" "http://www.alfarzpp.lv/eng/sc/AS3320.pdf"
			(at 25.4 -10.16 0)
		)
		(property "Description" "Voltage Controlled Filter (VCF), DIP-18"
			(at 0 0 0)
		)
		(property "ki_keywords" "VCF CEM3320 ALFA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "AS3320_0_1")
		(symbol "AS3320_1_1"
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "IN1")
				(number "1")
			)
			(pin passive line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "CAP1")
				(number "5")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "IN2")
				(number "2")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "CAP2")
				(number "4")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN3")
				(number "17")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "CAP3")
				(number "16")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IN4")
				(number "18")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "CAP4")
				(number "11")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "VRES")
				(number "8")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "IRES")
				(number "9")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "VCFI")
				(number "12")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VEE")
				(number "13")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "OUT1")
				(number "7")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OUT2")
				(number "6")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT3")
				(number "15")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "OUT4")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AS3320F"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 17.78 0)
		)
		(property "Value" "AS3320F"
			(at 5.08 17.78 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.7x2.7mm"
			(at 35.56 -15.24 0)
		)
		(property "Datasheet" "http://www.alfarzpp.lv/eng/sc/AS3320.pdf"
			(at 45.72 -15.24 0)
		)
		(property "Description" "Voltage Controlled Filter (VCF), QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "VCF CEM3320 ALFA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AS3320F_0_1")
		(symbol "AS3320F_1_1"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "IN1")
				(number "4")
			)
			(pin passive line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "CAP1")
				(number "9")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "IN2")
				(number "5")
			)
			(pin passive line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "CAP2")
				(number "8")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "IN3")
				(number "2")
			)
			(pin passive line
				(at -12.7 0 0)
				(length 2.54)
				(name "CAP3")
				(number "24")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "IN4")
				(number "3")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "CAP4")
				(number "17")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "VRES")
				(number "14")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "IRES")
				(number "15")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "VCFI")
				(number "19")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VCC")
				(number "22")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VEE")
				(number "20")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin no_connect line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at 10.16 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 10.16 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at 10.16 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at 10.16 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "18")
			)
			(pin no_connect line
				(at 10.16 -12.7 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "21")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "OUT1")
				(number "12")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "OUT2")
				(number "11")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "OUT3")
				(number "23")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "OUT4")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AS3330"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 12.7 0)
		)
		(property "Value" "AS3330"
			(at 5.08 12.7 0)
		)
		(property "Footprint" "Package_DIP:DIP-18_W7.62mm"
			(at 17.78 -2.54 0)
		)
		(property "Datasheet" "http://www.alfarzpp.lv/eng/sc/AS3330.pdf"
			(at 16.51 -1.27 0)
		)
		(property "Description" "Dual Voltage Controlled Amplifier (VCA), DIP-18"
			(at 0 0 0)
		)
		(property "ki_keywords" "VCA CEM3330 ALFA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "AS3330_0_1"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "10")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "VEE")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "18")
			)
		)
		(symbol "AS3330_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "IN1")
				(number "4")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VG1")
				(number "2")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "VCE1")
				(number "6")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "VCL1")
				(number "7")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "DTRIM1")
				(number "3")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "CCOMP1")
				(number "9")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "IDLE")
				(number "8")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "OUT1")
				(number "1")
			)
		)
		(symbol "AS3330_2_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "IN2")
				(number "13")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VG2")
				(number "15")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "VCE2")
				(number "14")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "VCL2")
				(number "12")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "DTRIM2")
				(number "17")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "CCOMP2")
				(number "11")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "OUT2")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AS3330F"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 12.7 0)
		)
		(property "Value" "AS3330F"
			(at 5.08 12.7 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.7x2.7mm"
			(at 38.1 -10.16 0)
		)
		(property "Datasheet" "http://www.alfarzpp.lv/eng/sc/AS3330.pdf"
			(at 16.51 -6.35 0)
		)
		(property "Description" "Dual Voltage Controlled Amplifier (VCA), QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "VCA CEM3330 ALFA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AS3330F_0_1"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "VEE")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
		)
		(symbol "AS3330F_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "IN1")
				(number "8")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VG1")
				(number "5")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "VCE1")
				(number "11")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "VCL1")
				(number "12")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "DTRIM1")
				(number "7")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "CCOMP1")
				(number "15")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "IDLE")
				(number "14")
			)
			(pin no_connect line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at 10.16 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at 10.16 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "18")
			)
			(pin no_connect line
				(at 10.16 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "21")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "OUT1")
				(number "4")
			)
		)
		(symbol "AS3330F_2_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "IN2")
				(number "20")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VG2")
				(number "23")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "VCE2")
				(number "22")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "VCL2")
				(number "19")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "DTRIM2")
				(number "2")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "CCOMP2")
				(number "17")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "OUT2")
				(number "24")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AS3340"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 17.78 0)
		)
		(property "Value" "AS3340"
			(at 5.08 17.78 0)
		)
		(property "Footprint" ""
			(at 12.7 -7.62 0)
		)
		(property "Datasheet" "http://www.alfarzpp.lv/eng/sc/AS3340.pdf"
			(at 15.24 -11.43 0)
		)
		(property "Description" "Voltage Controlled Oscillator (VCO), DIP-16/SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "VCO CEM340 ALFA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "AS3340_0_1")
		(symbol "AS3340_1_1"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "SCALE1")
				(number "1")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "SCALE2")
				(number "2")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "VPWM")
				(number "5")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VHSI")
				(number "6")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "VHFT")
				(number "7")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "VSSI")
				(number "9")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "VLFI")
				(number "13")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "VFCI")
				(number "15")
			)
			(pin passive line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "CAP")
				(number "11")
			)
			(pin passive line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "VS")
				(number "14")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VEE")
				(number "3")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "12")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "VP")
				(number "4")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "VSO")
				(number "8")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "VTO")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AS3345"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 17.78 0)
		)
		(property "Value" "AS3345"
			(at 5.08 17.78 0)
		)
		(property "Footprint" "Package_DIP:DIP-18_W7.62mm"
			(at 17.78 -10.16 0)
		)
		(property "Datasheet" "http://www.alfarzpp.lv/eng/sc/AS3340.pdf"
			(at 15.24 -13.97 0)
		)
		(property "Description" "Voltage Controlled Oscillator (VCO), DIP-18"
			(at 0 0 0)
		)
		(property "ki_keywords" "VCO CEM345 ALFA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "AS3345_0_1")
		(symbol "AS3345_1_1"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "SCALE1")
				(number "1")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "SCALE2")
				(number "2")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "VPWM")
				(number "5")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VHSI")
				(number "6")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "VHFT")
				(number "8")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "VSSI")
				(number "10")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "VLFI")
				(number "15")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "VFCI")
				(number "17")
			)
			(pin passive line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "CAP")
				(number "12")
			)
			(pin passive line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "VS")
				(number "16")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VCC")
				(number "18")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VEE")
				(number "3")
			)
			(pin passive line
				(at 2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "14")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "VP")
				(number "4")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "VMO")
				(number "7")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "VSO")
				(number "9")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "VTO")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AS3345F"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 17.78 0)
		)
		(property "Value" "AS3345F"
			(at 5.08 17.78 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.7x2.7mm"
			(at 35.56 -15.24 0)
		)
		(property "Datasheet" "http://www.alfarzpp.lv/eng/sc/AS3340.pdf"
			(at 15.24 -13.97 0)
		)
		(property "Description" "Voltage Controlled Oscillator (VCO), QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "VCO CEM345 ALFA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AS3345F_0_1")
		(symbol "AS3345F_1_1"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "SCALE1")
				(number "4")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "SCALE2")
				(number "5")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "VPWM")
				(number "9")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VHSI")
				(number "11")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "VHFT")
				(number "14")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "VSSI")
				(number "16")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "VLFI")
				(number "23")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "VFCI")
				(number "2")
			)
			(pin passive line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "CAP")
				(number "19")
			)
			(pin passive line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "VS")
				(number "24")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VEE")
				(number "7")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "20")
			)
			(pin passive line
				(at 2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "22")
			)
			(pin no_connect line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at 10.16 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 10.16 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at 10.16 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at 10.16 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "18")
			)
			(pin no_connect line
				(at 10.16 -12.7 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "21")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "VP")
				(number "8")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "VMO")
				(number "12")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "VSO")
				(number "15")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "VTO")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AS3360"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 10.16 0)
		)
		(property "Value" "AS3360"
			(at 5.08 10.16 0)
		)
		(property "Footprint" ""
			(at 17.78 -17.78 0)
		)
		(property "Datasheet" "http://www.alfarzpp.lv/eng/sc/AS3360.pdf"
			(at 16.51 -16.51 0)
		)
		(property "Description" "Dual Voltage Controlled Amplifier (VCA), DIP-14/SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "VCA CEM3360 ALFA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "AS3360_0_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VEE")
				(number "7")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
		)
		(symbol "AS3360_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VE1")
				(number "3")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VC1")
				(number "5")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "II1")
				(number "6")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "VREF")
				(number "8")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VO1")
				(number "4")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "IO1")
				(number "2")
			)
		)
		(symbol "AS3360_2_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VE2")
				(number "12")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VC2")
				(number "10")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "II2")
				(number "9")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VO2")
				(number "11")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "IO2")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CS4245"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 16.51 36.83 0)
		)
		(property "Value" "CS4245"
			(at 16.51 34.29 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://d3uzseaevmutz1.cloudfront.net/pubs/proDatasheet/CS4245_F3.pdf"
			(at 0 0 0)
		)
		(property "Description" "104 dB, 24-Bit, 192 kHz Stereo Audio CODEC, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio codec 2ch 24bit 192kHz"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "CS4245_0_1")
		(symbol "CS4245_1_1"
			(pin input line
				(at -22.86 30.48 0)
				(length 2.54)
				(name "AIN1A")
				(number "11")
			)
			(pin input line
				(at -22.86 27.94 0)
				(length 2.54)
				(name "AIN1B")
				(number "12")
			)
			(pin input line
				(at -22.86 25.4 0)
				(length 2.54)
				(name "AIN2A")
				(number "9")
			)
			(pin input line
				(at -22.86 22.86 0)
				(length 2.54)
				(name "AIN2B")
				(number "10")
			)
			(pin input line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "AIN3A")
				(number "7")
			)
			(pin input line
				(at -22.86 17.78 0)
				(length 2.54)
				(name "AIN3B")
				(number "8")
			)
			(pin input line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "AIN4A/MICIN1")
				(number "21")
			)
			(pin input line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "AIN4B/MICIN2")
				(number "22")
			)
			(pin input line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "AIN5A")
				(number "23")
			)
			(pin input line
				(at -22.86 7.62 0)
				(length 2.54)
				(name "AIN5B")
				(number "24")
			)
			(pin input line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "AIN6A")
				(number "26")
			)
			(pin input line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "AIN6B")
				(number "27")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "SDA/CDOUT")
				(number "1")
			)
			(pin input line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "SCL/CCLK")
				(number "2")
			)
			(pin input line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "AD0/~{CS}")
				(number "3")
			)
			(pin input line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "AD1/CDIN")
				(number "4")
			)
			(pin input line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "MCLK1")
				(number "44")
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 2.54)
				(name "LRCK1")
				(number "43")
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 2.54)
				(name "SCLK1")
				(number "42")
			)
			(pin output line
				(at -22.86 -22.86 0)
				(length 2.54)
				(name "SDOUT")
				(number "41")
			)
			(pin input line
				(at -22.86 -27.94 0)
				(length 2.54)
				(name "~{RESET}")
				(number "6")
			)
			(pin input line
				(at -10.16 35.56 270)
				(length 2.54)
				(name "VLC")
				(number "5")
			)
			(pin power_in line
				(at -5.08 35.56 270)
				(length 2.54)
				(name "VLS")
				(number "36")
			)
			(pin power_in line
				(at -2.54 -33.02 90)
				(length 2.54)
				(name "DGND")
				(number "45")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VD")
				(number "46")
			)
			(pin power_in line
				(at 2.54 -33.02 90)
				(length 2.54)
				(name "AGND")
				(number "13")
			)
			(pin passive line
				(at 2.54 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "31")
			)
			(pin passive line
				(at 2.54 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "32")
			)
			(pin power_in line
				(at 5.08 35.56 270)
				(length 2.54)
				(name "VA")
				(number "14")
			)
			(pin power_in line
				(at 7.62 35.56 270)
				(length 2.54)
				(name "VA")
				(number "30")
			)
			(pin input line
				(at 22.86 30.48 180)
				(length 2.54)
				(name "MCLK2")
				(number "40")
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "LRCK2")
				(number "39")
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "SCLK2")
				(number "38")
			)
			(pin input line
				(at 22.86 22.86 180)
				(length 2.54)
				(name "SDIN")
				(number "37")
			)
			(pin output line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "AOUTA")
				(number "33")
			)
			(pin output line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "AOUTB")
				(number "34")
			)
			(pin output line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "AUXOUTA")
				(number "28")
			)
			(pin output line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "AUXOUTB")
				(number "29")
			)
			(pin output line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "~{MUTEC}")
				(number "35")
			)
			(pin output line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "INT")
				(number "47")
			)
			(pin output line
				(at 22.86 0 180)
				(length 2.54)
				(name "OVFL")
				(number "48")
			)
			(pin output line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "MICBIAS")
				(number "25")
			)
			(pin output line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "VQ1")
				(number "17")
			)
			(pin output line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "VQ2")
				(number "18")
			)
			(pin output line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "FILT1+")
				(number "19")
			)
			(pin output line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "FILT2+")
				(number "20")
			)
			(pin output line
				(at 22.86 -25.4 180)
				(length 2.54)
				(name "AFILTA")
				(number "15")
			)
			(pin output line
				(at 22.86 -27.94 180)
				(length 2.54)
				(name "AFILTB")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CS4265"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 26.67 0)
		)
		(property "Value" "CS4265"
			(at 11.43 -26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.6x3.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://statics.cirrus.com/pubs/proDatasheet/CS4265_F5.pdf"
			(at 0 0 0)
		)
		(property "Description" "104 dB, 24-Bit, 192 kHz Stereo Audio CODEC, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Audio codec 24bit 192khz stereo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*0.5mm*"
			(at 0 0 0)
		)
		(symbol "CS4265_0_1")
		(symbol "CS4265_1_1"
			(pin input line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "AINA")
				(number "7")
			)
			(pin input line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "AINB")
				(number "8")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "VLS")
				(number "22")
			)
			(pin output line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "SDOUT")
				(number "26")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "SDIN1")
				(number "25")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "SDIN2")
				(number "24")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "TXSDIN")
				(number "23")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "MCLK")
				(number "29")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "SCLK")
				(number "27")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "LRCK")
				(number "28")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "~{RESET}")
				(number "4")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "SCL")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "SDA")
				(number "1")
			)
			(pin input line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "VLC")
				(number "3")
			)
			(pin power_in line
				(at -5.08 -27.94 90)
				(length 2.54)
				(name "SGND")
				(number "9")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VD")
				(number "31")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 2.54)
				(name "DGND")
				(number "30")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VA")
				(number "5")
			)
			(pin passive line
				(at 2.54 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "18")
			)
			(pin passive line
				(at 2.54 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "33")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 2.54)
				(name "AGND")
				(number "6")
			)
			(pin power_in line
				(at 5.08 27.94 270)
				(length 2.54)
				(name "VA")
				(number "17")
			)
			(pin output line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "~{MUTEC}")
				(number "21")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "AOUTA")
				(number "19")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "AOUTB")
				(number "20")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "AFILTA")
				(number "10")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "AFILTB")
				(number "11")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "VQ")
				(number "12")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "TXOUT")
				(number "32")
			)
			(pin input line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "MICIN1")
				(number "14")
			)
			(pin input line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "MICIN2")
				(number "15")
			)
			(pin output line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "MICBIAS")
				(number "16")
			)
			(pin output line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "FILT+")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CS4270"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 21.59 0)
		)
		(property "Value" "CS4270"
			(at 8.89 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-24_4.4x7.8mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://statics.cirrus.com/pubs/proDatasheet/CS4270_F1.pdf"
			(at 0 25.4 90)
		)
		(property "Description" "24-Bit, 192-kHz Stereo Audio CODEC, TSSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Audio Codec"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x7.8mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "CS4270_0_1")
		(symbol "CS4270_1_0"
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "SDIN")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "LRCLK")
				(number "2")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "MCLK")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "SCLK")
				(number "4")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "AINA")
				(number "15")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "AINB")
				(number "16")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "SDA/CDOUT/M1")
				(number "9")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "SCL/CCLK/M0")
				(number "10")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "AD0/~{CS}/I2S/~{LJ}")
				(number "11")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "AD1/CDIN/MDIV1")
				(number "12")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "AD2/MDIV2")
				(number "13")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "~{RST}")
				(number "14")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 2.54)
				(name "VD")
				(number "5")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VA")
				(number "19")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "DGND")
				(number "6")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "VLC")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -22.86 90)
				(length 2.54)
				(name "AGND")
				(number "20")
			)
			(pin output line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "SDOUT")
				(number "7")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "OUTA")
				(number "22")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "OUTB")
				(number "23")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "~{MUTEA}")
				(number "21")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "~{MUTEB}")
				(number "24")
			)
			(pin passive line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "FIL+")
				(number "18")
			)
			(pin passive line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "VQ")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CS4272"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 24.13 0)
		)
		(property "Value" "CS4272"
			(at 5.08 -24.13 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://statics.cirrus.com/pubs/proDatasheet/CS4272_F1.pdf"
			(at 0 0 0)
		)
		(property "Description" "24-Bit, 192 kHz Stereo Audio CODEC, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "stereo 2ch audio codec i2s 24bit 192kHz"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "CS4272_0_1")
		(symbol "CS4272_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "~{RST}")
				(number "14")
			)
			(pin output line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "XT0")
				(number "1")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "XTI")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "MCLK")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "LRCK")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "SCLK")
				(number "5")
			)
			(pin output line
				(at -15.24 0 0)
				(length 2.54)
				(name "SDOUT(M/~{S})")
				(number "6")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "SDIN")
				(number "7")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "SCL/CCLK(M0)")
				(number "11")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "SDA/CDIN(M1)")
				(number "12")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "AD0/~{CS}(I2S/~{LJ})")
				(number "13")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "VL")
				(number "10")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VD")
				(number "9")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "DGND")
				(number "8")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VA")
				(number "20")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "AGND")
				(number "21")
			)
			(pin output line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "VCOM")
				(number "15")
			)
			(pin output line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "FILT+")
				(number "22")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "~{AMUTEC}")
				(number "23")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "~{BMUTEC}")
				(number "28")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "AOUTA+")
				(number "25")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "AOUTA-")
				(number "24")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "AOUTB+")
				(number "26")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "AOUTB-")
				(number "27")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "AINA+")
				(number "17")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "AINA-")
				(number "16")
			)
			(pin input line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "AINB+")
				(number "18")
			)
			(pin input line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "AINB-")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CS4334"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "CS4334"
			(at 6.35 -8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://statics.cirrus.com/pubs/proDatasheet/CS4334-5-8-9_F7.pdf"
			(at 0 0 0)
		)
		(property "Description" "24-Bit, 96kHz Stereo D/A Converter, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "stereo 2ch audio codec i2s 24bit 96kHz"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "CS4334_0_1")
		(symbol "CS4334_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SDATA")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "~{DEM}/SCLK")
				(number "2")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "LRCK")
				(number "3")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "MCLK")
				(number "4")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VA")
				(number "7")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "AGND")
				(number "6")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "AOUTR")
				(number "5")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "AOUTL")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CS4344"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "CS4344"
			(at 6.35 11.43 0)
		)
		(property "Footprint" "Package_SO:TSSOP-10_3x3mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://statics.cirrus.com/pubs/proDatasheet/CS4344-45-48_F2.pdf"
			(at 0 0 0)
		)
		(property "Description" "16 to 24-Bit, 192 kHz Stereo D/A Converter, I2S Audio Format, TSSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "stereo 2ch audio codec"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "CS4344_0_1")
		(symbol "CS4344_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "SDIN")
				(number "1")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "~{DEM}/SCLK")
				(number "2")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "LRCK")
				(number "3")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "MCLK")
				(number "4")
			)
			(pin output line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "VQ")
				(number "5")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VA")
				(number "9")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "AOUTR")
				(number "10")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "AOUTL")
				(number "7")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "FILT+")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CS43L21"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 12.7 24.13 0)
		)
		(property "Value" "CS43L21"
			(at 12.7 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://d3uzseaevmutz1.cloudfront.net/pubs/proDatasheet/CS43L21_F1.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Power, Stereo Digital-to-Analog Converter, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio dac 2ch 24bit 96kHz"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "CS43L21_0_1")
		(symbol "CS43L21_1_1"
			(pin input line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "FLYP")
				(number "6")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "FLYN")
				(number "8")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "MCLK")
				(number "30")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "SCLK")
				(number "31")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "LRCK")
				(number "1")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "SDIN")
				(number "32")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "TESTO/M/~{S}")
				(number "29")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "~{RESET}")
				(number "25")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "SCL/CCLK/I2S/~{LJ}")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "SDA/MCLKDIV2")
				(number "2")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "AD0/~{CS}/DEM")
				(number "4")
			)
			(pin no_connect line
				(at -12.7 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "NIC")
				(number "16")
			)
			(pin no_connect line
				(at -10.16 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "TSTO")
				(number "17")
			)
			(pin input line
				(at -7.62 22.86 270)
				(length 2.54)
				(name "VL")
				(number "26")
			)
			(pin no_connect line
				(at -7.62 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "TSTO")
				(number "18")
			)
			(pin no_connect line
				(at -5.08 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "TSTO")
				(number "19")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 2.54)
				(name "VD")
				(number "27")
			)
			(pin no_connect line
				(at -2.54 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "TSTO")
				(number "20")
			)
			(pin no_connect line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "TSTO")
				(number "21")
			)
			(pin input line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "VA")
				(number "12")
			)
			(pin no_connect line
				(at 2.54 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "TSTO")
				(number "22")
			)
			(pin power_in line
				(at 5.08 -22.86 90)
				(length 2.54)
				(name "DGND")
				(number "28")
			)
			(pin input line
				(at 7.62 22.86 270)
				(length 2.54)
				(name "VA_HP")
				(number "5")
			)
			(pin no_connect line
				(at 7.62 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "TSTO")
				(number "23")
			)
			(pin power_in line
				(at 10.16 -22.86 90)
				(length 2.54)
				(name "AGND")
				(number "13")
			)
			(pin passive line
				(at 10.16 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "33")
			)
			(pin no_connect line
				(at 12.7 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "TSTO")
				(number "24")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "AOUTA")
				(number "11")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "AOUTB")
				(number "10")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "VSS_HP")
				(number "9")
			)
			(pin input line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "GND_HP")
				(number "7")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "FILT+")
				(number "14")
			)
			(pin output line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "VQ")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CS5343"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "CS5343"
			(at 6.35 11.43 0)
		)
		(property "Footprint" "Package_SO:TSSOP-10_3x3mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://statics.cirrus.com/pubs/proDatasheet/CS5343-44_F5.pdf"
			(at 0 0 0)
		)
		(property "Description" "98 dB, 96 kHz, 24bit Stereo Audio A/D Converter, I2S Audio Format, TSSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "stereo 2ch audio codec"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "CS5343_0_1")
		(symbol "CS5343_1_1"
			(pin output line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "SDOUT")
				(number "1")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SCLK")
				(number "2")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "LRCK")
				(number "3")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "MCLK")
				(number "4")
			)
			(pin output line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "VQ")
				(number "7")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VA")
				(number "10")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "AINR")
				(number "8")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "AINL")
				(number "6")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "FILT+")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CS5361"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 24.13 0)
		)
		(property "Value" "CS5361"
			(at -6.35 21.59 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://d3uzseaevmutz1.cloudfront.net/pubs/proDatasheet/CS5361_F2.pdf"
			(at 0 0 0)
		)
		(property "Description" "114 dB, 192 kHz, Multi-Bit Audio A/D Converter, SOIC-24/TSSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio adc 2ch 24bit 192kHz"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x15.4mm*P1.27mm* TSSOP*4.4x7.8mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "CS5361_0_1")
		(symbol "CS5361_1_1"
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "AINL+")
				(number "16")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "AINL-")
				(number "17")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "AINR+")
				(number "21")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "AINR-")
				(number "20")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{RST}")
				(number "1")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{OVFL}")
				(number "15")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "I2S/~{LJ}")
				(number "12")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "M/~{S}")
				(number "2")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "~{HPF}")
				(number "11")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "M0")
				(number "13")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "M1")
				(number "14")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "MDIV")
				(number "10")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VA")
				(number "19")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at 5.08 22.86 270)
				(length 2.54)
				(name "VD")
				(number "6")
			)
			(pin power_in line
				(at 5.08 -22.86 90)
				(length 2.54)
				(name "REFGND")
				(number "23")
			)
			(pin power_in line
				(at 7.62 22.86 270)
				(length 2.54)
				(name "VL")
				(number "8")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "MCLK")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "LRCK")
				(number "3")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "SCLK")
				(number "4")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "SDOUT")
				(number "9")
			)
			(pin power_out line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "FILT+")
				(number "24")
			)
			(pin power_out line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "VQ")
				(number "22")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CS8406"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 11.43 26.67 0)
		)
		(property "Value" "CS8406"
			(at 11.43 24.13 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://d3uzseaevmutz1.cloudfront.net/pubs/proDatasheet/CS8406_F6.pdf"
			(at 0 0 0)
		)
		(property "Description" "192 kHz Digital Audio Interface Transmitter, SOIC-28/TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio digital interface transmitter 192kHz"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x17.9mm*P1.27mm* TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "CS8406_0_0")
		(symbol "CS8406_1_0"
			(pin input line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "~{RST}")
				(number "9")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "VD")
				(number "6")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "22")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VL")
				(number "23")
			)
			(pin input line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "H/~{S}")
				(number "24")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "TXP")
				(number "26")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "TXN")
				(number "25")
			)
			(pin input line
				(at 17.78 0 180)
				(length 2.54)
				(name "OMCK")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "ILRCK")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "ISCLK")
				(number "13")
			)
			(pin input line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "SDIN")
				(number "14")
			)
		)
		(symbol "CS8406_1_1"
			(pin input line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "TEST/U")
				(number "17")
			)
			(pin input line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "TEST/V")
				(number "18")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "U/HWCK0")
				(number "20")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "AD1/CDIN/HWCK1")
				(number "27")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "RXP/SFMT0")
				(number "4")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "TSTN/SFMT1")
				(number "5")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "TEST/APMS")
				(number "10")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "TEST/TCBLD")
				(number "11")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "TEST/CEN")
				(number "16")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "AD0/~{CS}/TEST")
				(number "2")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "AD2/~{EMPH}")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "INT/~{AUDIO}")
				(number "19")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "SCL/CCLK/ORIG")
				(number "28")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "SDA/CDOUT/COPY/C")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "TCBL")
				(number "15")
			)
			(pin input line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "TEST")
				(number "7")
			)
			(pin input line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "TEST")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CS8414"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 11.43 26.67 0)
		)
		(property "Value" "CS8414"
			(at 11.43 24.13 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://lampizator.eu/LAMPIZATOR/TRANSPORT/CS8414_receiver.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "96 kHz Digital Audio Receiver, SOIC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio digital interface receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "CS8414_0_1")
		(symbol "CS8414_1_1"
			(pin input line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "RXP")
				(number "9")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "RXN")
				(number "10")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "CS12/FCK")
				(number "13")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "SEL")
				(number "16")
			)
			(pin output line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "ERF")
				(number "25")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "M0")
				(number "23")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "M1")
				(number "24")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "M2")
				(number "18")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "M3")
				(number "17")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "FILT")
				(number "20")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "VD")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -25.4 90)
				(length 2.54)
				(name "AGND")
				(number "21")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VA")
				(number "22")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "DGND")
				(number "8")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "MCK")
				(number "19")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "VERF")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "SCK")
				(number "12")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "SDATA")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "FSYNC")
				(number "11")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "C0/E0")
				(number "6")
			)
			(pin output line
				(at 17.78 0 180)
				(length 2.54)
				(name "CA/E1")
				(number "5")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "CB/E2")
				(number "4")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "CC/F0")
				(number "3")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "CD/F1")
				(number "2")
			)
			(pin output line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "CE/F2")
				(number "27")
			)
			(pin output line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "C")
				(number "1")
			)
			(pin output line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "U")
				(number "14")
			)
			(pin output line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "CBL")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CS8416-xNZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 12.7 26.67 0)
		)
		(property "Value" "CS8416-xNZ"
			(at 12.7 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_5x5mm_P0.5mm_EP3.35x3.35mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://d3uzseaevmutz1.cloudfront.net/pubs/proDatasheet/CS8416_F3.pdf"
			(at 0 0 0)
		)
		(property "Description" "192 kHz Digital Audio Interface Receiver, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio digital interface receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "CS8416-xNZ_0_1")
		(symbol "CS8416-xNZ_1_1"
			(pin input line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "RXN")
				(number "2")
			)
			(pin input line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "RXP0")
				(number "1")
			)
			(pin input line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "RXP1")
				(number "28")
			)
			(pin input line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "RXP2")
				(number "27")
			)
			(pin input line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "RXP3")
				(number "26")
			)
			(pin input line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "RXP4/RXSEL1")
				(number "7")
			)
			(pin input line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "RXP5/RXSEL0")
				(number "8")
			)
			(pin input line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "RXP6/TXSEL1")
				(number "9")
			)
			(pin input line
				(at -20.32 0 0)
				(length 2.54)
				(name "RXP7/TXSEL0")
				(number "10")
			)
			(pin input line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "~{RESET}")
				(number "6")
			)
			(pin input line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "AD0/~{CS}/NV/RERR")
				(number "11")
			)
			(pin input line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "AD1/CDIN/~{AUDIO}")
				(number "12")
			)
			(pin input line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "SCL/CCLK/96KHZ")
				(number "13")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "SDA/CDOUT/RCBL")
				(number "14")
			)
			(pin passive line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "FILT")
				(number "5")
			)
			(pin power_in line
				(at -5.08 25.4 270)
				(length 2.54)
				(name "VA")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -25.4 90)
				(length 2.54)
				(name "AGND")
				(number "4")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VD")
				(number "20")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "TP")
				(number "29")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "DGND")
				(number "19")
			)
			(pin power_in line
				(at 5.08 25.4 270)
				(length 2.54)
				(name "VL")
				(number "18")
			)
			(pin output line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "SDOUT")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "OLRCK")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "OSCLK")
				(number "24")
			)
			(pin output line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "RMCK")
				(number "21")
			)
			(pin input line
				(at 20.32 0 180)
				(length 2.54)
				(name "OMCK")
				(number "22")
			)
			(pin output line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "TX/GPO0")
				(number "17")
			)
			(pin output line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "C/GPO1")
				(number "16")
			)
			(pin output line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "U/AD2/GPO2")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CS8416-xSZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 12.7 26.67 0)
		)
		(property "Value" "CS8416-xSZ"
			(at 12.7 24.13 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://d3uzseaevmutz1.cloudfront.net/pubs/proDatasheet/CS8416_F3.pdf"
			(at 0 0 0)
		)
		(property "Description" "192 kHz Digital Audio Interface Receiver, SOIC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio digital interface receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x17.9mm*P1.27mm* TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "CS8416-xSZ_0_1")
		(symbol "CS8416-xSZ_1_1"
			(pin input line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "RXN")
				(number "5")
			)
			(pin input line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "RXP0")
				(number "4")
			)
			(pin input line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "RXP1")
				(number "3")
			)
			(pin input line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "RXP2")
				(number "2")
			)
			(pin input line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "RXP3")
				(number "1")
			)
			(pin input line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "RXP4/RXSEL1")
				(number "10")
			)
			(pin input line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "RXP5/RXSEL0")
				(number "11")
			)
			(pin input line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "RXP6/TXSEL1")
				(number "12")
			)
			(pin input line
				(at -20.32 0 0)
				(length 2.54)
				(name "RXP7/TXSEL0")
				(number "13")
			)
			(pin input line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "~{RESET}")
				(number "9")
			)
			(pin input line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "AD0/~{CS}/NV/RERR")
				(number "14")
			)
			(pin input line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "AD1/CDIN/~{AUDIO}")
				(number "15")
			)
			(pin input line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "SCL/CCLK/96KHZ")
				(number "16")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "SDA/CDOUT/RCBL")
				(number "17")
			)
			(pin passive line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "FILT")
				(number "8")
			)
			(pin power_in line
				(at -5.08 25.4 270)
				(length 2.54)
				(name "VA")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -25.4 90)
				(length 2.54)
				(name "AGND")
				(number "7")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VD")
				(number "23")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "DGND")
				(number "22")
			)
			(pin power_in line
				(at 5.08 25.4 270)
				(length 2.54)
				(name "VL")
				(number "21")
			)
			(pin output line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "SDOUT")
				(number "26")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "OLRCK")
				(number "28")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "OSCLK")
				(number "27")
			)
			(pin output line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "RMCK")
				(number "24")
			)
			(pin input line
				(at 20.32 0 180)
				(length 2.54)
				(name "OMCK")
				(number "25")
			)
			(pin output line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "TX/GPO0")
				(number "20")
			)
			(pin output line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "C/GPO1")
				(number "19")
			)
			(pin output line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "U/AD2/GPO2")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CS8420"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 12.7 31.75 0)
		)
		(property "Value" "CS8420"
			(at 12.7 29.21 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://d3uzseaevmutz1.cloudfront.net/pubs/proDatasheet/CS8420_F4.pdf"
			(at 0 0 0)
		)
		(property "Description" "Digital Audio Sample Rate Converter, SOIC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio sample rate converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "CS8420_0_1")
		(symbol "CS8420_1_1"
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "ILRCK/TCBLD/RCBL")
				(number "12")
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "ISCLK/PRO/C")
				(number "13")
			)
			(pin input line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "SDIN/MUTE/CHS")
				(number "14")
			)
			(pin input line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "RXP/SMFT0")
				(number "4")
			)
			(pin input line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "RXN/SMFT1")
				(number "5")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "SDA/CDOUT/COPY/C")
				(number "1")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "SCL/CCLK/ORIG/U")
				(number "28")
			)
			(pin input line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "AD0/~{CS}/DFC0")
				(number "2")
			)
			(pin input line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "AD1/CDIN/DFC1")
				(number "27")
			)
			(pin input line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "H/~{S}")
				(number "24")
			)
			(pin input line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "~{RST}")
				(number "9")
			)
			(pin passive line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "FILT")
				(number "8")
			)
			(pin power_in line
				(at -2.54 30.48 270)
				(length 2.54)
				(name "VA+")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -30.48 90)
				(length 2.54)
				(name "AGND")
				(number "7")
			)
			(pin power_in line
				(at 2.54 30.48 270)
				(length 2.54)
				(name "VD+")
				(number "23")
			)
			(pin power_in line
				(at 2.54 -30.48 90)
				(length 2.54)
				(name "DGND")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "OLRCK/V")
				(number "17")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "OSCLK/CEN")
				(number "16")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "SDOUT/U")
				(number "18")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "RMCK/APMS")
				(number "10")
			)
			(pin input line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "OMCK/APMS")
				(number "21")
			)
			(pin output line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "TXP/C")
				(number "26")
			)
			(pin output line
				(at 20.32 0 180)
				(length 2.54)
				(name "TXN/U")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "TCBL/NVERR")
				(number "15")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "U/S/~{AES}/PRO/C")
				(number "20")
			)
			(pin output line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "RERR/~{LOCK}/TBCLD")
				(number "11")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "~{EMPH}/U/V")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "INT/~{AUDIO}/V/CUVEN")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DSD1794A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 11.43 21.59 0)
		)
		(property "Value" "DSD1794A"
			(at 11.43 19.05 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/dsd1794a.pdf"
			(at 0 0 0)
		)
		(property "Description" "24-Bit, 192-kHz Sampling, Advanced Segment, Audio Stereo Digital-to-Analog Converter, SW Control, SSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio dac 2ch 24bit 192kHz"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x10.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "DSD1794A_0_1")
		(symbol "DSD1794A_1_1"
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "DBCK")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "DSDL")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "DSDR")
				(number "2")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "SCK")
				(number "7")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PBK")
				(number "6")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PLRCK")
				(number "4")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "PDATA")
				(number "5")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "SCL")
				(number "12")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "SDA")
				(number "13")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "ADR0")
				(number "10")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "ADR1")
				(number "11")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "~{RST}")
				(number "14")
			)
			(pin power_in line
				(at -5.08 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "9")
			)
			(pin power_in line
				(at -5.08 -20.32 90)
				(length 2.54)
				(name "DGND")
				(number "8")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VCC1")
				(number "23")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "AGND1")
				(number "19")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "VCC2L")
				(number "28")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "AGND2")
				(number "24")
			)
			(pin power_in line
				(at 5.08 20.32 270)
				(length 2.54)
				(name "VCC2R")
				(number "15")
			)
			(pin power_in line
				(at 5.08 -20.32 90)
				(length 2.54)
				(name "AGND3L")
				(number "27")
			)
			(pin power_in line
				(at 7.62 -20.32 90)
				(length 2.54)
				(name "AGND3R")
				(number "16")
			)
			(pin passive line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "VCOML")
				(number "22")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "VCOMR")
				(number "21")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "IOUTL+")
				(number "25")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "IOUTL-")
				(number "26")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "IOUTR+")
				(number "17")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "IOUTR-")
				(number "18")
			)
			(pin passive line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "IREF")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISD2560E"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.192 24.13 0)
		)
		(property "Value" "ISD2560E"
			(at 9.144 24.13 0)
		)
		(property "Footprint" "Package_SO:TSOP-I-28_11.8x8mm_P0.55mm"
			(at 1.27 -5.08 0)
		)
		(property "Datasheet" "https://datasheetspdf.com/pdf-file/700027/Winbond/ISD2560/1"
			(at 16.51 -6.35 0)
		)
		(property "Description" "Single-Chip Voice Record/Playback Device 60-Second Duration, TSOP-I-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "isd2560"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOP*11.8x8mm*P0.55mm*"
			(at 0 0 0)
		)
		(symbol "ISD2560E_0_1")
		(symbol "ISD2560E_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "A0/M0")
				(number "1")
			)
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "A1/M1")
				(number "2")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "A2/M2")
				(number "3")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "A3/M3")
				(number "4")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "A4/M4")
				(number "5")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "A5/M5")
				(number "6")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "A6/M6")
				(number "7")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "A7")
				(number "8")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "A8")
				(number "9")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "A9")
				(number "10")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "~{CE}")
				(number "23")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PD")
				(number "24")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "P/~{R}")
				(number "27")
			)
			(pin output line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "~{EOM}")
				(number "25")
			)
			(pin output line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "~{OVF}")
				(number "22")
			)
			(pin input line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "XCLK")
				(number "26")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VCCA")
				(number "16")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSSA")
				(number "13")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VCCD")
				(number "28")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "VSSD")
				(number "12")
			)
			(pin output line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "SP+")
				(number "14")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "SP-")
				(number "15")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "AUX_IN")
				(number "11")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "ANA_IN")
				(number "20")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "ANA_OUT")
				(number "21")
			)
			(pin passive line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "MIC_REF")
				(number "18")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "MIC")
				(number "17")
			)
			(pin passive line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "AGC")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISD2560P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.192 24.13 0)
		)
		(property "Value" "ISD2560P"
			(at 9.144 24.13 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W15.24mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://datasheetspdf.com/pdf-file/700027/Winbond/ISD2560/1"
			(at 16.51 -6.35 0)
		)
		(property "Description" "Single-Chip Voice Record/Playback Device 60-Second Duration, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "isd2560"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "ISD2560P_0_1")
		(symbol "ISD2560P_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "A0/M0")
				(number "1")
			)
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "A1/M1")
				(number "2")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "A2/M2")
				(number "3")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "A3/M3")
				(number "4")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "A4/M4")
				(number "5")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "A5/M5")
				(number "6")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "A6/M6")
				(number "7")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "A7")
				(number "8")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "A8")
				(number "9")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "A9")
				(number "10")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "~{CE}")
				(number "23")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PD")
				(number "24")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "P/~{R}")
				(number "27")
			)
			(pin output line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "~{EOM}")
				(number "25")
			)
			(pin output line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "~{OVF}")
				(number "22")
			)
			(pin input line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "XCLK")
				(number "26")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VCCA")
				(number "16")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSSA")
				(number "13")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VCCD")
				(number "28")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "VSSD")
				(number "12")
			)
			(pin output line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "SP+")
				(number "14")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "SP-")
				(number "15")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "AUX_IN")
				(number "11")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "ANA_IN")
				(number "20")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "ANA_OUT")
				(number "21")
			)
			(pin passive line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "MIC_REF")
				(number "18")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "MIC")
				(number "17")
			)
			(pin passive line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "AGC")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISD2560S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.192 24.13 0)
		)
		(property "Value" "ISD2560S"
			(at 9.144 24.13 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 1.27 -5.08 0)
		)
		(property "Datasheet" "https://datasheetspdf.com/pdf-file/700027/Winbond/ISD2560/1"
			(at 16.51 -6.35 0)
		)
		(property "Description" "Single-Chip Voice Record/Playback Device 60-Second Duration, SOIC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "isd2560"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ISD2560S_0_1")
		(symbol "ISD2560S_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "A0/M0")
				(number "1")
			)
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "A1/M1")
				(number "2")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "A2/M2")
				(number "3")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "A3/M3")
				(number "4")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "A4/M4")
				(number "5")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "A5/M5")
				(number "6")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "A6/M6")
				(number "7")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "A7")
				(number "8")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "A8")
				(number "9")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "A9")
				(number "10")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "~{CE}")
				(number "23")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PD")
				(number "24")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "P/~{R}")
				(number "27")
			)
			(pin output line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "~{EOM}")
				(number "25")
			)
			(pin output line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "~{OVF}")
				(number "22")
			)
			(pin input line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "XCLK")
				(number "26")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VCCA")
				(number "16")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSSA")
				(number "13")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VCCD")
				(number "28")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "VSSD")
				(number "12")
			)
			(pin output line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "SP+")
				(number "14")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "SP-")
				(number "15")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "AUX_IN")
				(number "11")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "ANA_IN")
				(number "20")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "ANA_OUT")
				(number "21")
			)
			(pin passive line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "MIC_REF")
				(number "18")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "MIC")
				(number "17")
			)
			(pin passive line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "AGC")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX98357A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 11.43 0)
		)
		(property "Value" "MAX98357A"
			(at 10.16 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:TQFN-16-1EP_3x3mm_P0.5mm_EP1.23x1.23mm"
			(at -1.27 -2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX98357A-MAX98357B.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "Mono DAC with amplifier, I2S, PCM, TDM, 32-bit, 96khz, 3.2W, TQFP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "pcm tdm i2s left-justified amplifier audio dac"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFN*3x3mm*P0.5mm*EP1.23x1.23mm*"
			(at 0 0 0)
		)
		(symbol "MAX98357A_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "DIN")
				(number "1")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "BCLK")
				(number "16")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "LRCLK")
				(number "14")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{SD_MODE}")
				(number "4")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "GAIN_SLOT")
				(number "2")
			)
			(pin passive line
				(at -2.54 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at -2.54 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "7")
			)
			(pin passive line
				(at 0 12.7 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "8")
			)
			(pin unspecified line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "PAD")
				(number "17")
			)
			(pin no_connect line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 10.16 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin no_connect line
				(at 10.16 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "OUTP")
				(number "9")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "OUTN")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MN3005"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 12.7 0)
		)
		(property "Value" "MN3005"
			(at 10.16 -12.7 0)
		)
		(property "Footprint" ""
			(at -10.16 7.62 0)
		)
		(property "Datasheet" "http://www.experimentalistsanonymous.com/diy/Datasheets/MN3005.pdf"
			(at -7.62 10.16 0)
		)
		(property "Description" "4096-STAGE LONG DELAY BBD (bucket brigade device), delay time 20.48ms to 204.8ms, S/N 75dB, clock frequency range 10KHz to 100KHz"
			(at 0 0 0)
		)
		(property "ki_keywords" "Matsushita Panasonic BBD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP-8*"
			(at 0 0 0)
		)
		(symbol "MN3005_0_1")
		(symbol "MN3005_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "CP1")
				(number "6")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "CP2")
				(number "2")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "IN")
				(number "7")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VGG")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "5")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OUT1")
				(number "3")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "OUT2")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MN3007"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 12.7 0)
		)
		(property "Value" "MN3007"
			(at 10.16 -12.7 0)
		)
		(property "Footprint" ""
			(at -10.16 7.62 0)
		)
		(property "Datasheet" "http://www.experimentalistsanonymous.com/diy/Datasheets/MN3007.pdf"
			(at -7.62 10.16 0)
		)
		(property "Description" "1024-STAGE LOW NOISE BBD (bucket brigade device), delay time 5.12ms to 51.2ms, S/N 80dB, clock frequency range 10KHz to 100KHz"
			(at 0 0 0)
		)
		(property "ki_keywords" "Matsushita Panasonic BBD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP-8*"
			(at 0 0 0)
		)
		(symbol "MN3007_0_1")
		(symbol "MN3007_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "CP1")
				(number "2")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "CP2")
				(number "6")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "IN")
				(number "3")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VGG")
				(number "4")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "5")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OUT1")
				(number "7")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "OUT2")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MN3207"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 12.7 0)
		)
		(property "Value" "MN3207"
			(at 10.16 -12.7 0)
		)
		(property "Footprint" ""
			(at -10.16 7.62 0)
		)
		(property "Datasheet" "http://www.experimentalistsanonymous.com/diy/Datasheets/MN3207.pdf"
			(at -7.62 10.16 0)
		)
		(property "Description" "1024-STAGE LOW VOLTAGE OPERATION LOW NOISE BBD (bucket brigade device), delay time 2.56ms to 51.2ms, S/N 73dB, clock frequency range 10KHz to 200KHz"
			(at 0 0 0)
		)
		(property "ki_keywords" "Matsushita Panasonic BBD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP-8*"
			(at 0 0 0)
		)
		(symbol "MN3207_0_1")
		(symbol "MN3207_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "CP1")
				(number "2")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "CP2")
				(number "6")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "IN")
				(number "3")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VGG")
				(number "4")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "5")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OUT1")
				(number "7")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "OUT2")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSGEQ7"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 13.97 0)
		)
		(property "Value" "MSGEQ7"
			(at -2.54 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://mix-sig.com/images/datasheets/MSGEQ7.pdf"
			(at 0 0 0)
		)
		(property "Description" "Seven Band Graphic Equalizer, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "equalizer filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MSGEQ7_0_0"
			(text "FLT"
				(at -5.588 0 0)
			)
			(text "BP"
				(at -0.635 -3.429 0)
			)
			(text "MUX"
				(at 2.286 -1.016 900)
			)
		)
		(symbol "MSGEQ7_0_1")
		(symbol "MSGEQ7_1_1"
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "IN")
				(number "5")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "CKIN")
				(number "8")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "2")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "STROBE")
				(number "4")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "RESET")
				(number "7")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
			(pin power_out line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "GND")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCM1754DBQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 -17.78 0)
		)
		(property "Value" "PCM1754DBQ"
			(at 11.43 16.51 0)
		)
		(property "Footprint" "Package_SO:SSOP-16_3.9x4.9mm_P0.635mm"
			(at -2.54 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/pcm1754.pdf"
			(at -2.54 2.54 0)
		)
		(property "Description" "24-bit, 192-kHz sampling, Stereo Audio DAC, SSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio dac 24-bit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "PCM1754DBQ_0_1")
		(symbol "PCM1754DBQ_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "BCK")
				(number "1")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "SCK")
				(number "16")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "LRCLK")
				(number "3")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "DATA")
				(number "2")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "TEST")
				(number "12")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "DEMP")
				(number "13")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "MUTE")
				(number "14")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "FMT")
				(number "15")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 2.54)
				(name "DGND")
				(number "4")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "V_{CC}")
				(number "6")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "AGND")
				(number "9")
			)
			(pin no_connect line
				(at 10.16 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "V_{COM}")
				(number "10")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "V_{OUT}L")
				(number "7")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "V_{OUT}R")
				(number "8")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "ZEROA")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCM1780"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -9.652 16.764 0)
		)
		(property "Value" "PCM1780"
			(at 12.192 16.764 0)
		)
		(property "Footprint" "Package_SO:SSOP-16_3.9x4.9mm_P0.635mm"
			(at -0.254 -31.242 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/pcm1780.pdf"
			(at 0.508 -28.448 0)
		)
		(property "Description" "24-bit, 192-kHz sampling, Stereo Audio DAC, SSOP-16"
			(at 0.254 -34.29 0)
		)
		(property "ki_keywords" "audio dac 24-bit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "PCM1780_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "BCK")
				(number "7")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "SCK")
				(number "5")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "LRCK")
				(number "8")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "DATA")
				(number "6")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "MC")
				(number "3")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "MD")
				(number "4")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "~{MS}")
				(number "2")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "Vcc")
				(number "11")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "AGND")
				(number "12")
			)
			(pin no_connect line
				(at 10.16 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at 10.16 -12.7 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "V_{COM}")
				(number "13")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "V_{OUT}L")
				(number "15")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "V_{OUT}R")
				(number "14")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "ZEROL")
				(number "1")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "ZEROR")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCM1792A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 11.43 21.59 0)
		)
		(property "Value" "PCM1792A"
			(at 11.43 19.05 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/pcm1792a.pdf"
			(at 0 0 0)
		)
		(property "Description" "24-Bit, 192-kHz Sampling, Advanced Segment, Audio Stereo Digital-to-Analog Converter, SW Control, SSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio dac 2ch 24bit 192kHz"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x10.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PCM1792A_0_1")
		(symbol "PCM1792A_1_1"
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "SCK")
				(number "7")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "BCK")
				(number "6")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "LRCK")
				(number "4")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "DATA")
				(number "5")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "MC")
				(number "12")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "MDI")
				(number "11")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "MDO")
				(number "13")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "~{MS}")
				(number "10")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "MSEL")
				(number "3")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "~{RST}")
				(number "14")
			)
			(pin power_in line
				(at -5.08 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "9")
			)
			(pin power_in line
				(at -5.08 -20.32 90)
				(length 2.54)
				(name "DGND")
				(number "8")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VCC1")
				(number "23")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "AGND1")
				(number "19")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "VCC2L")
				(number "28")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "AGND2")
				(number "24")
			)
			(pin power_in line
				(at 5.08 20.32 270)
				(length 2.54)
				(name "VCC2R")
				(number "15")
			)
			(pin power_in line
				(at 5.08 -20.32 90)
				(length 2.54)
				(name "AGND3L")
				(number "27")
			)
			(pin power_in line
				(at 7.62 -20.32 90)
				(length 2.54)
				(name "AGND3R")
				(number "16")
			)
			(pin passive line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "VCOML")
				(number "22")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "VCOMR")
				(number "21")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "IOUTL+")
				(number "25")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "IOUTL-")
				(number "26")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "ZEROL")
				(number "1")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "IOUTR+")
				(number "17")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "IOUTR-")
				(number "18")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "ZEROR")
				(number "2")
			)
			(pin passive line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "IREF")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCM1794A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 11.43 21.59 0)
		)
		(property "Value" "PCM1794A"
			(at 11.43 19.05 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/pcm1794a.pdf"
			(at 0 0 0)
		)
		(property "Description" "24-Bit, 192-kHz Sampling, Advanced Segment, Audio Stereo Digital-to-Analog Converter, HW Control, SSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio dac 2ch 24bit 192kHz"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x10.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PCM1794A_0_1")
		(symbol "PCM1794A_1_1"
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "SCK")
				(number "7")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "BCK")
				(number "6")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "LRCK")
				(number "4")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "DATA")
				(number "5")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "MONO")
				(number "1")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "CHSL")
				(number "2")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "DEM")
				(number "3")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "MUTE")
				(number "10")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "FMT0")
				(number "11")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "FMT1")
				(number "12")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "~{RST}")
				(number "14")
			)
			(pin power_in line
				(at -5.08 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "9")
			)
			(pin power_in line
				(at -5.08 -20.32 90)
				(length 2.54)
				(name "DGND")
				(number "8")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VCC1")
				(number "23")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "AGND1")
				(number "19")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "VCC2L")
				(number "28")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "AGND2")
				(number "24")
			)
			(pin power_in line
				(at 5.08 20.32 270)
				(length 2.54)
				(name "VCC2R")
				(number "15")
			)
			(pin power_in line
				(at 5.08 -20.32 90)
				(length 2.54)
				(name "AGND3L")
				(number "27")
			)
			(pin power_in line
				(at 7.62 -20.32 90)
				(length 2.54)
				(name "AGND3R")
				(number "16")
			)
			(pin passive line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "VCOML")
				(number "22")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "VCOMR")
				(number "21")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "IOUTL+")
				(number "25")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "IOUTL-")
				(number "26")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "IOUTR+")
				(number "17")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "IOUTR-")
				(number "18")
			)
			(pin open_collector line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "ZERO")
				(number "13")
			)
			(pin passive line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "IREF")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCM2902"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -14.732 21.59 0)
		)
		(property "Value" "PCM2902"
			(at 10.922 21.59 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/pcm2902c.pdf"
			(at 9.398 24.638 0)
		)
		(property "Description" "Stereo Audio Codec with USB interface, Analog Input/Output, and S/PDIF, SSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "pcm2902 usb audio"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x10.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PCM2902_0_1")
		(symbol "PCM2902_1_1"
			(pin input line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "VINL")
				(number "12")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "VINR")
				(number "13")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "DIN")
				(number "24")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "SEL0")
				(number "8")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "SEL1")
				(number "9")
			)
			(pin output line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "~{SSPND}")
				(number "28")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "HID0")
				(number "5")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "HID1")
				(number "6")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "HID2")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "D+")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "D-")
				(number "2")
			)
			(pin power_in line
				(at -5.08 -22.86 90)
				(length 2.54)
				(name "DGNDU")
				(number "4")
			)
			(pin power_out line
				(at -2.54 22.86 270)
				(length 2.54)
				(name "VDDI")
				(number "27")
			)
			(pin power_in line
				(at -2.54 -22.86 90)
				(length 2.54)
				(name "DGND")
				(number "26")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VBUS")
				(number "3")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "AGNDC")
				(number "11")
			)
			(pin power_in line
				(at 2.54 -22.86 90)
				(length 2.54)
				(name "AGNDP")
				(number "18")
			)
			(pin power_in line
				(at 5.08 -22.86 90)
				(length 2.54)
				(name "AGNDX")
				(number "22")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "VOUTL")
				(number "16")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "VOUTR")
				(number "15")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "DOUT")
				(number "25")
			)
			(pin input line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "XTI")
				(number "21")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "XTO")
				(number "20")
			)
			(pin passive line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "VCCCI")
				(number "10")
			)
			(pin passive line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "VCOM")
				(number "14")
			)
			(pin passive line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "VCCP1I")
				(number "17")
			)
			(pin passive line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "VCCP2I")
				(number "19")
			)
			(pin passive line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "VCCXI")
				(number "23")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCM3060"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -9.398 26.67 0)
		)
		(property "Value" "PCM3060"
			(at 8.89 26.67 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at 0 -42.418 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/pcm3060"
			(at 0 -39.624 0)
		)
		(property "Description" "24-bit Asynchronous Stereo Audio Codec with 96/192kHz sampling rate, TSSOP-28"
			(at -1.016 -44.958 0)
		)
		(property "ki_keywords" "audio codec 2ch 24bit 192kHz"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PCM3060_0_1")
		(symbol "PCM3060_1_1"
			(text "ADC"
				(at -1.016 0 0)
			)
			(text "DAC"
				(at -1.016 -13.97 0)
			)
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "MC/SCL/FMT")
				(number "1")
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "MD/SDA/DEMP")
				(number "2")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "~{MS}/AD/IFMD")
				(number "27")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "~{RST}")
				(number "15")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "MODE")
				(number "28")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "V_{IN}L")
				(number "25")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "V_{IN}R")
				(number "26")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "LRCK1")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "BCK1")
				(number "5")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "SCKI1")
				(number "6")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "DIN")
				(number "12")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "LRCK2")
				(number "11")
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "BCK2")
				(number "10")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "SCKI2")
				(number "9")
			)
			(pin power_in line
				(at -5.08 -27.94 90)
				(length 2.54)
				(name "DGND")
				(number "8")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "V_{DD}")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 2.54)
				(name "SGND")
				(number "16")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "V_{CC}")
				(number "24")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 2.54)
				(name "AGND1")
				(number "23")
			)
			(pin power_in line
				(at 5.08 -27.94 90)
				(length 2.54)
				(name "AGND2")
				(number "22")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "V_{OUT}L+")
				(number "20")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "V_{OUT}L-")
				(number "19")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "V_{OUT}R+")
				(number "18")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "V_{OUT}R-")
				(number "17")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "ZEROL")
				(number "14")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "ZEROR")
				(number "13")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "DOUT")
				(number "3")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "V_{COM}")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCM5100"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 13.97 0)
		)
		(property "Value" "PCM5100"
			(at 3.81 13.97 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -1.27 19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/pcm5100.pdf"
			(at -1.27 19.05 0)
		)
		(property "Description" "2VRMS DirectPath, 100dB Audio Stereo DAC with 32-bit, 384kHz PCM Interface, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio dac 2ch 32bit 384kHz"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PCM5100_0_1")
		(symbol "PCM5100_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "LRCK")
				(number "15")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "DIN")
				(number "14")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "BCK")
				(number "13")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SCK")
				(number "12")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "FLT")
				(number "11")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "DEMP")
				(number "10")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "XSMT")
				(number "17")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "FMT")
				(number "16")
			)
			(pin passive line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "CPVDD")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 2.54)
				(name "CPGND")
				(number "3")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "DVDD")
				(number "20")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "DGND")
				(number "19")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "AVDD")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "AGND")
				(number "9")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "OUTL")
				(number "6")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "OUTR")
				(number "7")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CAPP")
				(number "2")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "CAPM")
				(number "4")
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "LDOO")
				(number "18")
			)
			(pin passive line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "VNEG")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCM5122PW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 21.59 0)
		)
		(property "Value" "PCM5122PW"
			(at 10.16 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/pcm5122.pdf"
			(at 0 26.67 0)
		)
		(property "Description" "2VRMS DirectPath, 112dB Audio Stereo DAC with 32-bit, 384kHz PCM Interface, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio dac 2ch 32bit 384kHz"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PCM5122PW_0_1")
		(symbol "PCM5122PW_1_1"
			(pin input line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "SCK")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "BCK")
				(number "21")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "LRCK")
				(number "23")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "DIN")
				(number "22")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "SCL/MC/ATT1")
				(number "12")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "SDA/MOSI/ATT2")
				(number "11")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "ADR1/MISO/FMT")
				(number "24")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "ADR2/GPIO2/DOUT")
				(number "16")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "MODE1")
				(number "17")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "MODE2/MS")
				(number "18")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "XSMT")
				(number "25")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 2.54)
				(name "CPVDD")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -22.86 90)
				(length 2.54)
				(name "CPGND")
				(number "3")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "DVDD")
				(number "28")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "DGND")
				(number "27")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "AVDD")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -22.86 90)
				(length 2.54)
				(name "AGND")
				(number "9")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "OUTL")
				(number "6")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "OUTR")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "GPIO3/AGNS")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "GPIO4/MAST")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "GPIO5/ATT0")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "GPIO6/FLT")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "VCOM/DEMP")
				(number "10")
			)
			(pin passive line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "CAPP")
				(number "2")
			)
			(pin passive line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "CAPM")
				(number "4")
			)
			(pin passive line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "LDOO")
				(number "26")
			)
			(pin passive line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "VNEG")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PGA2310UA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 12.7 0 0)
		)
		(property "Value" "PGA2310UA"
			(at 17.78 -2.54 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -38.1 0)
		)
		(property "Datasheet" "https://www.ti.com.cn/cn/lit/gpn/pga2310"
			(at 0 -40.64 0)
		)
		(property "Description" "2-Channel Audio Volume Control, SPI Interface, +31.5dB to -95.5dB, SOL-16"
			(at 0 -35.56 0)
		)
		(property "ki_keywords" "audio volume control 2ch spi"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*16W*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "PGA2310UA_0_0"
			(text "G"
				(at -0.889 14.986 0)
			)
			(text "G"
				(at -0.889 -15.494 0)
			)
			(text "SERIAL CONTROL PORT"
				(at 0 0 900)
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "~{MUTE}")
				(number "8")
			)
		)
		(symbol "PGA2310UA_0_1")
		(symbol "PGA2310UA_1_1"
			(pin power_in line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "AGNDL")
				(number "15")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "V_{IN}L")
				(number "16")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "ZCEN")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SCLK")
				(number "6")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "SDI")
				(number "3")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{CS}")
				(number "2")
			)
			(pin output line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "SDO")
				(number "7")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "V_{IN}R")
				(number "9")
			)
			(pin power_in line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "AGNDR")
				(number "10")
			)
			(pin power_in line
				(at -5.08 27.94 270)
				(length 2.54)
				(name "V_{D}+")
				(number "4")
			)
			(pin power_in line
				(at -5.08 -27.94 90)
				(length 2.54)
				(name "DGND")
				(number "5")
			)
			(pin power_in line
				(at 5.08 27.94 270)
				(length 2.54)
				(name "V_{A}+")
				(number "12")
			)
			(pin power_in line
				(at 5.08 -27.94 90)
				(length 2.54)
				(name "V_{A}-")
				(number "13")
			)
			(pin output line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "V_{OUT}L")
				(number "14")
			)
			(pin output line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "V_{OUT}R")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PGA2500"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -9.398 26.416 0)
		)
		(property "Value" "PGA2500"
			(at 5.842 26.924 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at 0.254 -39.116 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/pga2500.pdf"
			(at 0 -33.782 0)
		)
		(property "Description" "Digitally Controlled Microphone Preamplifier"
			(at 0 -36.576 0)
		)
		(property "ki_keywords" "Digitally Controlled Microphone Preamplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3*10.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PGA2500_0_1")
		(symbol "PGA2500_1_1"
			(pin input line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "V_{IN}+")
				(number "27")
			)
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "V_{IN}-")
				(number "26")
			)
			(pin power_in line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "VIN_{COM}")
				(number "25")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "~{DCEN}")
				(number "7")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "0dB")
				(number "8")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "ZCEN")
				(number "9")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SDI")
				(number "10")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{CS}")
				(number "11")
			)
			(pin input clock
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "SCLK")
				(number "12")
			)
			(pin output line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "SDO")
				(number "13")
			)
			(pin power_in line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "VA+")
				(number "18")
			)
			(pin power_in line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "VA+")
				(number "19")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 2.54)
				(name "DGND")
				(number "6")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 2.54)
				(name "AGND")
				(number "28")
			)
			(pin output line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "V_{OUT}+")
				(number "17")
			)
			(pin output line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "V_{OUT}-")
				(number "16")
			)
			(pin output line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "GPO1")
				(number "1")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "GPO2")
				(number "2")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "GPO3")
				(number "3")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "GPO4")
				(number "4")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OVR")
				(number "5")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "C_{S11}")
				(number "24")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "C_{S12}")
				(number "23")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "C_{S21}")
				(number "22")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "C_{S22}")
				(number "21")
			)
			(pin power_in line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "VA-")
				(number "15")
			)
			(pin power_in line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "VA-")
				(number "20")
			)
			(pin power_in line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "VD-")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PGA4311"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 29.21 0)
		)
		(property "Value" "PGA4311"
			(at 3.81 29.21 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/pga4311.pdf"
			(at 0 0 0)
		)
		(property "Description" "4-Channel Audio Volume Control, SPI Interface, +31.5dB to -95.5dB, SOIC-28W"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio volume control 4ch spi"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "PGA4311_0_0"
			(text "G"
				(at -0.889 20.066 0)
			)
			(text "G"
				(at -0.889 12.446 0)
			)
			(text "G"
				(at -0.889 -12.954 0)
			)
			(text "G"
				(at -0.889 -20.574 0)
			)
			(text "SERIAL CONTROL PORT"
				(at 0 0 900)
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{MUTE}")
				(number "1")
			)
		)
		(symbol "PGA4311_0_1")
		(symbol "PGA4311_1_1"
			(pin input line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "Ain-1")
				(number "3")
			)
			(pin power_in line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "AGND_1")
				(number "2")
			)
			(pin passive line
				(at -12.7 17.78 0)
				(length 2.54)
				(hide yes)
				(name "AGND_1")
				(number "4")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "Ain-2")
				(number "26")
			)
			(pin power_in line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "AGND_2")
				(number "25")
			)
			(pin passive line
				(at -12.7 10.16 0)
				(length 2.54)
				(hide yes)
				(name "AGND_2")
				(number "27")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SCLK")
				(number "15")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SDI")
				(number "13")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{CS}")
				(number "14")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "ZCEN")
				(number "28")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "Ain-3")
				(number "10")
			)
			(pin passive line
				(at -12.7 -15.24 0)
				(length 2.54)
				(hide yes)
				(name "AGND_3")
				(number "11")
			)
			(pin power_in line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "AGND_3")
				(number "9")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "Ain-4")
				(number "19")
			)
			(pin power_in line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "AGND_4")
				(number "18")
			)
			(pin passive line
				(at -12.7 -22.86 0)
				(length 2.54)
				(hide yes)
				(name "AGND_4")
				(number "20")
			)
			(pin passive line
				(at -2.54 30.48 270)
				(length 2.54)
				(hide yes)
				(name "VA+")
				(number "22")
			)
			(pin power_in line
				(at -2.54 30.48 270)
				(length 2.54)
				(name "VA+")
				(number "7")
			)
			(pin passive line
				(at -2.54 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "VA-")
				(number "23")
			)
			(pin power_in line
				(at -2.54 -30.48 90)
				(length 2.54)
				(name "VA-")
				(number "6")
			)
			(pin power_in line
				(at 2.54 30.48 270)
				(length 2.54)
				(name "VD+")
				(number "12")
			)
			(pin power_in line
				(at 2.54 -30.48 90)
				(length 2.54)
				(name "DGND")
				(number "17")
			)
			(pin output line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "Aout_1")
				(number "5")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "Aout_2")
				(number "24")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "SDO")
				(number "16")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "Aout_3")
				(number "8")
			)
			(pin output line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "Aout_4")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PT2258"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 16.51 0)
		)
		(property "Value" "PT2258"
			(at 6.35 16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at 0 -24.13 0)
		)
		(property "Datasheet" "http://www.princeton.com.tw/Portals/0/Product/PT2258-s.pdf"
			(at 0 -27.94 0)
		)
		(property "Description" "6-Channel Electronic Volume Controller, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Volume"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PT2258_0_1")
		(symbol "PT2258_1_1"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "IN1")
				(number "1")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "IN2")
				(number "2")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "IN3")
				(number "3")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "IN4")
				(number "8")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "IN5")
				(number "9")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "IN6")
				(number "10")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "CODE1")
				(number "17")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "CODE2")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "SDA")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "14")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "DGND")
				(number "5")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "OUT1")
				(number "20")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "OUT2")
				(number "19")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "OUT3")
				(number "18")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "OUT4")
				(number "13")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OUT5")
				(number "12")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "OUT6")
				(number "11")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "REF")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PT2399"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 17.78 0)
		)
		(property "Value" "PT2399"
			(at 0 -17.78 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.princeton.com.tw/Portals/0/Product/PT2399_1.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "Echo Processor IC, DIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS ADC DAC 44K Digital processing VCO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PT2399_0_1")
		(symbol "PT2399_1_1"
			(pin power_in line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin passive line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "REF")
				(number "2")
			)
			(pin power_in line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "AGND")
				(number "3")
			)
			(pin power_in line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "DGND")
				(number "4")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "CLK_O")
				(number "5")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "VCO")
				(number "6")
			)
			(pin passive line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "CC1")
				(number "7")
			)
			(pin passive line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "CC0")
				(number "8")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "LPF1-IN")
				(number "16")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "LPF1-OUT")
				(number "15")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "LPF2-OUT")
				(number "14")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "LPF2-IN")
				(number "13")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "OP2-OUT")
				(number "12")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "OP2-IN")
				(number "11")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "OP1-IN")
				(number "10")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "OP1-OUT")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RD5106A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 12.7 0)
		)
		(property "Value" "RD5106A"
			(at 10.16 -12.7 0)
		)
		(property "Footprint" ""
			(at -10.16 7.62 0)
		)
		(property "Datasheet" "http://pdf.datasheetarchive.com/indexerfiles/Scans-091/DSAHI00048836.pdf"
			(at -7.62 10.16 0)
		)
		(property "Description" "Analog Delay Line 256 sample bucket brigade device, 512usec to more than 1second, input signal frequency range 0 to 170KHz, clock frequency range 500Hz to 1MHz"
			(at 0 0 0)
		)
		(property "ki_keywords" "EG&G RETICON BBD N-channel silicon-gate"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP-8*"
			(at 0 0 0)
		)
		(symbol "RD5106A_0_1")
		(symbol "RD5106A_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "Clock")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "Sync")
				(number "7")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "Input")
				(number "6")
			)
			(pin no_connect line
				(at -10.16 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VBB")
				(number "5")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "2")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "Output")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RE46C317"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "RE46C317"
			(at 6.35 8.89 0)
		)
		(property "Footprint" ""
			(at 5.08 -6.35 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/22301B.pdf"
			(at 3.81 -17.78 0)
		)
		(property "Description" "Piezoelectric Horn Driver with Boost Converter, 3.3V supply, Tri-State Horn Enable, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Microchip step-up"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*8*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "RE46C317_0_0")
		(symbol "RE46C317_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "LX")
				(number "3")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "V_{O}")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "HRNEN")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V_{DD}")
				(number "2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "V_{SS}")
				(number "4")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "FEED")
				(number "1")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "HORNS")
				(number "7")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "HORNB")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SAD1024"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 11.43 0)
		)
		(property "Value" "SAD1024"
			(at 7.62 11.43 0)
		)
		(property "Footprint" ""
			(at -10.16 7.62 0)
		)
		(property "Datasheet" "http://thmq.mysteria.cz/em1022/SAD1024.pdf"
			(at -7.62 10.16 0)
		)
		(property "Description" "SAD-1024 DUAL ANALOG DELAY LINE, bucket brigade device, 2 independent 512 stages, signal frequency range 0 to 200KHz, clock frequency range 1.5KHz to 1.5MHz"
			(at 0 0 0)
		)
		(property "ki_keywords" "EG&G RETICON BBD N-channel silicon-gate"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP-16*"
			(at 0 0 0)
		)
		(symbol "SAD1024_0_1"
			(pin no_connect line
				(at -7.62 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at -5.08 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "Vbb")
				(number "9")
			)
			(pin no_connect line
				(at -2.54 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "Vdd")
				(number "7")
			)
		)
		(symbol "SAD1024_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "01A")
				(number "8")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "02A")
				(number "3")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "IN_A")
				(number "2")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OUT_A")
				(number "5")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "OUT_A'")
				(number "6")
			)
		)
		(symbol "SAD1024_2_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "01B")
				(number "10")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "02B")
				(number "14")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "IN_B")
				(number "15")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OUT_B")
				(number "12")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "OUT_B'")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SGTL5000XNAA3"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" "SGTL5000XNAA3"
			(at -7.62 -31.75 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.6x3.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/SGTL5000.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low Power Stereo Codec with Headphone Amp, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Codec"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "SGTL5000XNAA3_0_1")
		(symbol "SGTL5000XNAA3_1_1"
			(pin passive line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "VAG")
				(number "10")
			)
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "LINEIN_R")
				(number "13")
			)
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "LINEIN_L")
				(number "14")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "MIC")
				(number "15")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "MIC_BIAS")
				(number "16")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "CPFILT")
				(number "18")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "SYS_MCLK")
				(number "21")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "I2S_LRCLK")
				(number "23")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "I2S_SCLK")
				(number "24")
			)
			(pin output line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "I2S_DOUT")
				(number "25")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "I2S_DIN")
				(number "26")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "CTRL_DATA")
				(number "27")
			)
			(pin input line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "CTRL_CLK")
				(number "29")
			)
			(pin input line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "CTRL_ADR0_CS")
				(number "31")
			)
			(pin input line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "CTRL_MODE")
				(number "32")
			)
			(pin power_in line
				(at -5.08 33.02 270)
				(length 2.54)
				(name "VDDIO")
				(number "20")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "VDDD")
				(number "30")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin power_in line
				(at 7.62 33.02 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin power_in line
				(at 7.62 -33.02 90)
				(length 2.54)
				(name "AGND")
				(number "7")
			)
			(pin no_connect line
				(at 10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "19")
			)
			(pin no_connect line
				(at 10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "22")
			)
			(pin no_connect line
				(at 10.16 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "28")
			)
			(pin no_connect line
				(at 10.16 -15.24 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at 10.16 -17.78 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at 10.16 -20.32 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin output line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "LINEOUT_R")
				(number "11")
			)
			(pin output line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "LINEOUT_L")
				(number "12")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "HP_R")
				(number "2")
			)
			(pin power_out line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "HP_VGND")
				(number "4")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "HP_L")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SGTL5000XNLA3"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" "SGTL5000XNLA3"
			(at -5.08 -27.94 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_3x3mm_P0.4mm_EP1.65x1.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/SGTL5000.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low Power Stereo Codec with Headphone Amp, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Codec"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*3x3mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "SGTL5000XNLA3_0_1")
		(symbol "SGTL5000XNLA3_1_1"
			(pin passive line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "VAG")
				(number "5")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "LINEIN_R")
				(number "8")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "LINEIN_L")
				(number "9")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "MIC")
				(number "10")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "MIC_BIAS")
				(number "11")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "SYS_MCLK")
				(number "13")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "I2S_LRCLK")
				(number "14")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "I2S_SCLK")
				(number "15")
			)
			(pin output line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "I2S_DOUT")
				(number "16")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "I2S_DIN")
				(number "17")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "CTRL_DATA")
				(number "18")
			)
			(pin input line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "CTRL_CLK")
				(number "19")
			)
			(pin power_in line
				(at -5.08 27.94 270)
				(length 2.54)
				(name "VDDIO")
				(number "12")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDDD")
				(number "20")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 5.08 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "3")
			)
			(pin output line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "LINEOUT_R")
				(number "6")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "LINEOUT_L")
				(number "7")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "HP_R")
				(number "1")
			)
			(pin power_out line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "HP_VGND")
				(number "2")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "HP_L")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SPN1001"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 19.05 0)
		)
		(property "Value" "SPN1001"
			(at 7.62 19.05 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 0 -30.48 0)
		)
		(property "Datasheet" "http://www.spinsemi.com/Products/datasheets/spn1001/FV-1.pdf"
			(at 1.27 -34.29 0)
		)
		(property "Description" "Spin Semiconductor FV-1 Reverb IC, SOIC-28W"
			(at 0 0 0)
		)
		(property "ki_keywords" "SpinSemi FV-1 SPN1001"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*"
			(at 0 0 0)
		)
		(symbol "SPN1001_0_1")
		(symbol "SPN1001_1_1"
			(pin power_out line
				(at -15.24 15.24 0)
				(length 5.08)
				(name "CLIP")
				(number "5")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 5.08)
				(name "LIN")
				(number "1")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 5.08)
				(name "RIN")
				(number "2")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "POT0")
				(number "20")
			)
			(pin input line
				(at -15.24 0 0)
				(length 5.08)
				(name "POT1")
				(number "21")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "POT2")
				(number "22")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 5.08)
				(name "S0")
				(number "16")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 5.08)
				(name "S1")
				(number "17")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 5.08)
				(name "S2")
				(number "18")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 5.08)
				(name "AVDD")
				(number "6")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "19")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "24")
			)
			(pin power_in line
				(at -2.54 -22.86 90)
				(length 5.08)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 22.86 270)
				(length 5.08)
				(hide yes)
				(name "DVDD")
				(number "23")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 5.08)
				(name "DVDD")
				(number "8")
			)
			(pin input line
				(at 2.54 22.86 270)
				(length 5.08)
				(name "REFP")
				(number "26")
			)
			(pin input line
				(at 2.54 -22.86 90)
				(length 5.08)
				(name "REFN")
				(number "25")
			)
			(pin output line
				(at 15.24 15.24 180)
				(length 5.08)
				(name "LOUT")
				(number "28")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 5.08)
				(name "ROUT")
				(number "27")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 5.08)
				(name "X1")
				(number "10")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 5.08)
				(name "X2")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 5.08)
				(name "SDA")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "SCK")
				(number "14")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 5.08)
				(name "T0")
				(number "13")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 5.08)
				(name "T1")
				(number "12")
			)
			(pin power_out line
				(at 15.24 -15.24 180)
				(length 5.08)
				(name "MID")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SRC4392xPFB"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 31.75 0)
		)
		(property "Value" "SRC4392xPFB"
			(at 15.24 31.75 0)
		)
		(property "Footprint" "Package_QFP:TQFP-48_7x7mm_P0.5mm"
			(at 1.27 -29.21 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/src4392.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Two-Channel, Asynchronous Sample Rate Converter with Integrated Digital Audio Interface Receiver and Transmitter, TQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio sample rate converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "SRC4392xPFB_0_1")
		(symbol "SRC4392xPFB_1_1"
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BCKA")
				(number "37")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "LRCKA")
				(number "38")
			)
			(pin input line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "SDINA")
				(number "39")
			)
			(pin output line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "SDOUTA")
				(number "40")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "BCKB")
				(number "48")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "LRCKB")
				(number "47")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "SDINB")
				(number "46")
			)
			(pin output line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "SDOUTB")
				(number "45")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "RX1+")
				(number "1")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "RX1-")
				(number "2")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "RX2+")
				(number "3")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "RX2-")
				(number "4")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "RX3+")
				(number "5")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "RX3-")
				(number "6")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "RX4+")
				(number "7")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "RX4-")
				(number "8")
			)
			(pin input line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "MCLK")
				(number "25")
			)
			(pin input line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "RXCKI")
				(number "13")
			)
			(pin output line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "RXCKO")
				(number "12")
			)
			(pin power_in line
				(at -5.08 33.02 270)
				(length 2.54)
				(name "VIO")
				(number "42")
			)
			(pin power_in line
				(at -5.08 -30.48 90)
				(length 2.54)
				(name "DGND1")
				(number "16")
			)
			(pin power_in line
				(at -2.54 33.02 270)
				(length 2.54)
				(name "VDD33")
				(number "33")
			)
			(pin power_in line
				(at -2.54 -30.48 90)
				(length 2.54)
				(name "DGND2")
				(number "30")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "VCC")
				(number "9")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 2.54)
				(name "DGND3")
				(number "43")
			)
			(pin power_in line
				(at 2.54 -30.48 90)
				(length 2.54)
				(name "AGND")
				(number "10")
			)
			(pin power_in line
				(at 5.08 33.02 270)
				(length 2.54)
				(name "VDD18")
				(number "17")
			)
			(pin power_in line
				(at 5.08 -30.48 90)
				(length 2.54)
				(name "BGND")
				(number "44")
			)
			(pin no_connect line
				(at 10.16 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "41")
			)
			(pin output line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "SYNC")
				(number "36")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "BLS")
				(number "35")
			)
			(pin output line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "AESOUT")
				(number "34")
			)
			(pin output line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "TX+")
				(number "32")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "TX-")
				(number "31")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "GPO1")
				(number "26")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "GPO2")
				(number "27")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "GPO3")
				(number "28")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "GPO4")
				(number "29")
			)
			(pin input line
				(at 17.78 0 180)
				(length 2.54)
				(name "~{RST}")
				(number "24")
			)
			(pin open_collector line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "~{INT}")
				(number "23")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "~{RDY}")
				(number "15")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "~{LOCK}")
				(number "11")
			)
			(pin input line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "MUTE")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "CDOUT/SDA")
				(number "22")
			)
			(pin input line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "CCLK/SCL")
				(number "20")
			)
			(pin input line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "~{CS}/A0")
				(number "19")
			)
			(pin input line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "CDIN/A1")
				(number "21")
			)
			(pin input line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "CPM")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SSI2144"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "SSI2144"
			(at 6.35 26.67 0)
		)
		(property "Footprint" "Package_SO:SSOP-16_3.9x4.9mm_P0.635mm"
			(at 22.86 -2.54 0)
		)
		(property "Datasheet" "http://www.soundsemiconductor.com/downloads/ssi2144datasheet.pdf"
			(at 17.78 -6.35 0)
		)
		(property "Description" "Four-pole VCF, SSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Sound Semiconductor VCF SSM2044"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "SSI2144_0_1")
		(symbol "SSI2144_1_1"
			(pin input line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "SIG_IN+")
				(number "1")
			)
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "SIG_IN-")
				(number "2")
			)
			(pin passive line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "C1A")
				(number "13")
			)
			(pin passive line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "C1B")
				(number "12")
			)
			(pin passive line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "C2A")
				(number "11")
			)
			(pin passive line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "C2B")
				(number "10")
			)
			(pin passive line
				(at -15.24 0 0)
				(length 2.54)
				(name "C3A")
				(number "6")
			)
			(pin passive line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "C3B")
				(number "7")
			)
			(pin passive line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "C4A")
				(number "4")
			)
			(pin passive line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "C4B")
				(number "5")
			)
			(pin passive line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "FREQ_CTRL")
				(number "15")
			)
			(pin passive line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "Q_CTRL")
				(number "14")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "V+")
				(number "16")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "V-")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SSI2164"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 19.05 0)
		)
		(property "Value" "SSI2164"
			(at 5.08 19.05 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 20.32 -2.54 0)
		)
		(property "Datasheet" "http://www.soundsemiconductor.com/downloads/ssi2164datasheet.pdf"
			(at 15.24 -11.43 0)
		)
		(property "Description" "Quad VCA, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Sound Semiconductor VCA SSM2164"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "SSI2164_0_1")
		(symbol "SSI2164_1_1"
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "I_IN1")
				(number "2")
			)
			(pin passive line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "VC1")
				(number "3")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "I_IN2")
				(number "7")
			)
			(pin passive line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VC2")
				(number "6")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "I_IN3")
				(number "10")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "VC3")
				(number "11")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "I_IN4")
				(number "15")
			)
			(pin passive line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "VC4")
				(number "14")
			)
			(pin passive line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "MODE")
				(number "1")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "V+")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "V-")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "I_OUT1")
				(number "4")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "I_OUT2")
				(number "5")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "I_OUT3")
				(number "12")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "I_OUT4")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TDA1022"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 12.7 0)
		)
		(property "Value" "TDA1022"
			(at 8.89 12.7 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://thmq.mysteria.cz/em1022/TDA1022.pdf"
			(at -7.62 10.16 0)
		)
		(property "Description" "BUCKET BRIGADE DELAY LINE FOR ANALOGUE SIGNALS, 512 stages, delay time 0.512ms to 51.2ms, signal frequency range 0 to 45KHz, clock frequency range 5KHz to 500KHz, DIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "PHILIPS BBD MOS monolithic delay analogue"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "TDA1022_0_1")
		(symbol "TDA1022_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "CL1")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "CL2")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "Input")
				(number "5")
			)
			(pin no_connect line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -10.16 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at -5.08 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "V13-16")
				(number "13")
			)
			(pin no_connect line
				(at -2.54 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "16")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "9")
			)
			(pin no_connect line
				(at 2.54 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at 5.08 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin no_connect line
				(at 10.16 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin no_connect line
				(at 10.16 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "Output513")
				(number "8")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "Output512")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "THAT1580"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 7.62 0)
		)
		(property "Value" "THAT1580"
			(at 5.08 5.08 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_4x4mm_P0.65mm_EP2.1x2.1mm_ThermalVias"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.thatcorp.com/datashts/THAT_1580_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, Differential Audio Preamplifier IC, 0.005% THD+N, -134.8dBu EIN, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "diff amp mic preamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "THAT1580_0_1")
		(symbol "THAT1580_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IN1")
				(number "7")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "Rg1")
				(number "6")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "Rg2")
				(number "15")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "IN2")
				(number "10")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 5.08)
				(name "V+")
				(number "13")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 5.08)
				(name "V-")
				(number "12")
			)
			(pin passive line
				(at -2.54 -10.16 90)
				(length 5.08)
				(hide yes)
				(name "V-")
				(number "17")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 5.08)
				(name "1")
				(number "3")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 5.08)
				(name "2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "THAT5171"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 13.97 0)
		)
		(property "Value" "THAT5171"
			(at 5.08 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_7x7mm_P0.65mm_EP5.4x5.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.thatcorp.com/datashts/THAT_5171_Datasheet.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "High-Performance Digital Preamplifier Controller IC, QFN-32"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "mic preamp gain controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "THAT5171_0_1")
		(symbol "THAT5171_1_1"
			(pin passive line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "SCAP2")
				(number "30")
			)
			(pin output line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SOUT2")
				(number "32")
			)
			(pin output line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SOUT1")
				(number "31")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SCAP1")
				(number "29")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "Rg2")
				(number "6")
			)
			(pin passive line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "Rg1")
				(number "3")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "9")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "VEE")
				(number "11")
			)
			(pin passive line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "PAD")
				(number "33")
			)
			(pin power_in line
				(at 5.08 -15.24 90)
				(length 2.54)
				(name "AGND")
				(number "10")
			)
			(pin passive line
				(at 5.08 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "28")
			)
			(pin no_connect line
				(at 7.62 10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at 7.62 7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at 7.62 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at 7.62 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "27")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "IN2")
				(number "5")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "IN1")
				(number "4")
			)
		)
		(symbol "THAT5171_2_1"
			(pin passive line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "TRC")
				(number "14")
			)
			(pin output line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "BSY")
				(number "22")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{RST}")
				(number "15")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{CS}")
				(number "16")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SCLK")
				(number "17")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "DIN")
				(number "18")
			)
			(pin tri_state line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "DOUT")
				(number "19")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "13")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "21")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "DGND")
				(number "12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "DGND")
				(number "20")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "GPO0")
				(number "23")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "GPO1")
				(number "24")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "GPO2")
				(number "25")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "GPO3")
				(number "26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "THAT5173"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 13.97 0)
		)
		(property "Value" "THAT5173"
			(at 5.08 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_5x5mm_P0.65mm_EP3.4x3.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.thatcorp.com/datashts/THAT_5173_Datasheet.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "Audio Preamplifier Digital Controller IC, QFN-24"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "mic preamp gain controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "THAT5173_0_1")
		(symbol "THAT5173_1_1"
			(pin passive line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "SCAP2")
				(number "1")
			)
			(pin output line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SOUT2")
				(number "23")
			)
			(pin output line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SOUT1")
				(number "22")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SCAP1")
				(number "24")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "Rg2")
				(number "5")
			)
			(pin passive line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "Rg1")
				(number "2")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "VEE")
				(number "19")
			)
			(pin passive line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "PAD")
				(number "25")
			)
			(pin power_in line
				(at 5.08 -15.24 90)
				(length 2.54)
				(name "AGND")
				(number "21")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "IN2")
				(number "4")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "IN1")
				(number "3")
			)
		)
		(symbol "THAT5173_2_1"
			(pin passive line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "TRC")
				(number "10")
			)
			(pin output line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "BSY")
				(number "14")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{RST}")
				(number "6")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{CS}")
				(number "7")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SCLK")
				(number "8")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "DIN")
				(number "9")
			)
			(pin tri_state line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "DOUT")
				(number "13")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "DGND")
				(number "12")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "GPO0")
				(number "15")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "GPO1")
				(number "16")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "GPO2")
				(number "17")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "GPO3")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "THAT5263"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 13.97 0)
		)
		(property "Value" "THAT5263"
			(at 5.08 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_5x5mm_P0.65mm_EP3.4x3.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.thatcorp.com/datashts/THAT_5263_Datasheet.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "2-Channel Digital Preamplifier Controller IC, QFN-24"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "dual mic preamp gain controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "THAT5263_0_1")
		(symbol "THAT5263_1_1"
			(pin passive line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "RB_CH1")
				(number "9")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "RG2_CH1")
				(number "8")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "RG1_CH1")
				(number "7")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "RA_CH1")
				(number "6")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "V-")
				(number "3")
			)
			(pin passive line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "PAD")
				(number "25")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "IN2_CH1")
				(number "10")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "IN1_CH1")
				(number "5")
			)
		)
		(symbol "THAT5263_2_1"
			(pin output line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "BSY_CH1")
				(number "17")
			)
			(pin output line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "BSY_CH2")
				(number "18")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{CS}")
				(number "11")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SCLK")
				(number "12")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "DIN")
				(number "13")
			)
			(pin tri_state line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "DOUT")
				(number "14")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "15")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "DGND")
				(number "16")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "GPO_CH1")
				(number "19")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "GPO_CH2")
				(number "20")
			)
		)
		(symbol "THAT5263_3_1"
			(pin passive line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "RB_CH2")
				(number "1")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "RG2_CH2")
				(number "24")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "RG1_CH2")
				(number "23")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "RA_CH2")
				(number "22")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "IN2_CH2")
				(number "2")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "IN1_CH2")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "THAT6261"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 8.89 0)
		)
		(property "Value" "THAT6261"
			(at 15.24 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.45x5.45mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.thatcorp.com/datashts/THAT_626x_Datasheet.pdf"
			(at -2.54 -2.54 0)
		)
		(property "Description" "2-Channel Low-Noise Programmable-Gain Preamplifier - ADC Driver IC, 1dB Step, QFN-48"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "dual mic preamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "THAT6261_1_0"
			(text "PREAMP"
				(at -6.35 0 0)
			)
			(text "ADC DRIVER"
				(at 7.62 0 0)
			)
		)
		(symbol "THAT6261_1_1"
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "IN+_CH1")
				(number "14")
			)
			(pin passive line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "CG1_CH1")
				(number "12")
			)
			(pin passive line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "CG2_CH1")
				(number "11")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "IN-_CH1")
				(number "13")
			)
			(pin passive line
				(at -10.16 10.16 270)
				(length 2.54)
				(hide yes)
				(name "VA+")
				(number "10")
			)
			(pin power_in line
				(at -10.16 10.16 270)
				(length 2.54)
				(name "VA+")
				(number "4")
			)
			(pin passive line
				(at -10.16 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "VA-")
				(number "15")
			)
			(pin passive line
				(at -10.16 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "VA-")
				(number "20")
			)
			(pin power_in line
				(at -10.16 -10.16 90)
				(length 2.54)
				(name "VA-")
				(number "9")
			)
			(pin power_in line
				(at -7.62 10.16 270)
				(length 2.54)
				(name "VCM")
				(number "44")
			)
			(pin passive line
				(at -7.62 -10.16 90)
				(length 2.54)
				(name "PAD")
				(number "49")
			)
			(pin power_in line
				(at -5.08 10.16 270)
				(length 2.54)
				(name "VAD")
				(number "45")
			)
			(pin power_in line
				(at -5.08 -10.16 90)
				(length 2.54)
				(name "AGND")
				(number "43")
			)
			(pin output line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "PO+_CH1")
				(number "7")
			)
			(pin output line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "PO-_CH1")
				(number "8")
			)
			(pin input line
				(at 0 10.16 270)
				(length 2.54)
				(name "DI+_CH1")
				(number "5")
			)
			(pin input line
				(at 0 -10.16 90)
				(length 2.54)
				(name "DI-_CH1")
				(number "6")
			)
			(pin passive line
				(at 7.62 10.16 270)
				(length 2.54)
				(name "RFB+_CH1")
				(number "1")
			)
			(pin passive line
				(at 7.62 -10.16 90)
				(length 2.54)
				(name "RFB-_CH1")
				(number "48")
			)
			(pin passive line
				(at 10.16 10.16 270)
				(length 2.54)
				(name "CFB+_CH1")
				(number "3")
			)
			(pin passive line
				(at 10.16 -10.16 90)
				(length 2.54)
				(name "CFB-_CH1")
				(number "2")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "OUT+_CH1")
				(number "47")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "OUT-_CH1")
				(number "46")
			)
		)
		(symbol "THAT6261_2_1"
			(pin output line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "BSY_CH1")
				(number "27")
			)
			(pin output line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "BSY_CH2")
				(number "34")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{CS}")
				(number "30")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SCLK")
				(number "31")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "DIN")
				(number "32")
			)
			(pin tri_state line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "DOUT")
				(number "33")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VD")
				(number "29")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "DGND")
				(number "28")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "GPO0_CH1")
				(number "25")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "GPO1_CH1")
				(number "26")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "GPO_CH2")
				(number "35")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "GP1_CH2")
				(number "36")
			)
		)
		(symbol "THAT6261_3_0"
			(text "PREAMP"
				(at -6.35 0 0)
			)
			(text "ADC DRIVER"
				(at 6.985 0 0)
			)
		)
		(symbol "THAT6261_3_1"
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "IN+_CH2")
				(number "19")
			)
			(pin passive line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "CG1_CH2")
				(number "17")
			)
			(pin passive line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "CG2_CH2")
				(number "16")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "IN-_CH2")
				(number "18")
			)
			(pin output line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "PO+_CH2")
				(number "21")
			)
			(pin output line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "PO-_CH2")
				(number "22")
			)
			(pin input line
				(at 0 10.16 270)
				(length 2.54)
				(name "DI+_CH2")
				(number "23")
			)
			(pin input line
				(at 0 -10.16 90)
				(length 2.54)
				(name "DI-_CH2")
				(number "24")
			)
			(pin passive line
				(at 7.62 10.16 270)
				(length 2.54)
				(name "RFB+_CH2")
				(number "39")
			)
			(pin passive line
				(at 7.62 -10.16 90)
				(length 2.54)
				(name "RFB-_CH2")
				(number "40")
			)
			(pin passive line
				(at 10.16 10.16 270)
				(length 2.54)
				(name "CFB+_CH2")
				(number "37")
			)
			(pin passive line
				(at 10.16 -10.16 90)
				(length 2.54)
				(name "CFB-_CH2")
				(number "38")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "OUT+_CH2")
				(number "41")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "OUT-_CH2")
				(number "42")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLV320AIC23BPW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 16.51 26.67 0)
		)
		(property "Value" "TLV320AIC23BPW"
			(at 16.51 24.13 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv320aic23b.pdf"
			(at 0 0 0)
		)
		(property "Description" "Stero Audio CODEC, 8- to 96-kHz, With Integrated Headphone Amplifier, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio codec 2ch 96kHz headphone amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TLV320AIC23BPW_0_1")
		(symbol "TLV320AIC23BPW_1_1"
			(pin input line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "SDIN")
				(number "23")
			)
			(pin input line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "SCLK")
				(number "24")
			)
			(pin input line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "MODE")
				(number "22")
			)
			(pin input line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "~{CS}")
				(number "21")
			)
			(pin input line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "DIN")
				(number "4")
			)
			(pin input line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "LRCIN")
				(number "5")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "BCLK")
				(number "3")
			)
			(pin output line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "DOUT")
				(number "6")
			)
			(pin output line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "LRCOUT")
				(number "7")
			)
			(pin passive line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "XTI/MCK")
				(number "25")
			)
			(pin passive line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "XTO")
				(number "26")
			)
			(pin output line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "CLKOUT")
				(number "2")
			)
			(pin power_in line
				(at -7.62 25.4 270)
				(length 2.54)
				(name "BVDD")
				(number "1")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "DVDD")
				(number "27")
			)
			(pin power_in line
				(at -2.54 -25.4 90)
				(length 2.54)
				(name "DGND")
				(number "28")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "AVDD")
				(number "14")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "AGND")
				(number "15")
			)
			(pin power_in line
				(at 7.62 25.4 270)
				(length 2.54)
				(name "HPVDD")
				(number "8")
			)
			(pin power_in line
				(at 7.62 -25.4 90)
				(length 2.54)
				(name "HPGND")
				(number "11")
			)
			(pin passive line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "LOUT")
				(number "12")
			)
			(pin passive line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "ROUT")
				(number "13")
			)
			(pin passive line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "LHPOUT")
				(number "9")
			)
			(pin passive line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "RHPOUT")
				(number "10")
			)
			(pin passive line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "LLINEIN")
				(number "20")
			)
			(pin passive line
				(at 20.32 0 180)
				(length 2.54)
				(name "RLINEIN")
				(number "19")
			)
			(pin passive line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "MICBIAS")
				(number "17")
			)
			(pin passive line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "MICIN")
				(number "18")
			)
			(pin passive line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "VMID")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLV320AIC23BRHD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 15.24 26.67 0)
		)
		(property "Value" "TLV320AIC23BRHD"
			(at 16.51 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_5x5mm_P0.5mm_EP3.35x3.35mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv320aic23b.pdf"
			(at 0 0 0)
		)
		(property "Description" "Stero Audio CODEC, 8- to 96-kHz, With Integrated Headphone Amplifier, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio codec 2ch 96kHz headphone amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TLV320AIC23BRHD_0_1")
		(symbol "TLV320AIC23BRHD_1_1"
			(pin input line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "SDIN")
				(number "20")
			)
			(pin input line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "SCLK")
				(number "21")
			)
			(pin input line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "MODE")
				(number "19")
			)
			(pin input line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "~{CS}")
				(number "18")
			)
			(pin input line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "DIN")
				(number "1")
			)
			(pin input line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "LRCIN")
				(number "2")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "BCLK")
				(number "28")
			)
			(pin output line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "DOUT")
				(number "3")
			)
			(pin output line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "LRCOUT")
				(number "4")
			)
			(pin passive line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "XTI/MCK")
				(number "22")
			)
			(pin passive line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "XTO")
				(number "23")
			)
			(pin output line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "CLKOUT")
				(number "27")
			)
			(pin power_in line
				(at -7.62 25.4 270)
				(length 2.54)
				(name "BVDD")
				(number "26")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "DVDD")
				(number "24")
			)
			(pin power_in line
				(at -2.54 -25.4 90)
				(length 2.54)
				(name "DGND")
				(number "25")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "AVDD")
				(number "11")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "AGND")
				(number "12")
			)
			(pin passive line
				(at 2.54 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "29")
			)
			(pin power_in line
				(at 7.62 25.4 270)
				(length 2.54)
				(name "HPVDD")
				(number "5")
			)
			(pin power_in line
				(at 7.62 -25.4 90)
				(length 2.54)
				(name "HPGND")
				(number "8")
			)
			(pin passive line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "LOUT")
				(number "9")
			)
			(pin passive line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "ROUT")
				(number "10")
			)
			(pin passive line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "LHPOUT")
				(number "6")
			)
			(pin passive line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "RHPOUT")
				(number "7")
			)
			(pin passive line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "LLINEIN")
				(number "17")
			)
			(pin passive line
				(at 20.32 0 180)
				(length 2.54)
				(name "RLINEIN")
				(number "16")
			)
			(pin passive line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "MICBIAS")
				(number "14")
			)
			(pin passive line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "MICIN")
				(number "15")
			)
			(pin passive line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "VMID")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLV320AIC23BxQE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 16.51 26.67 0)
		)
		(property "Value" "TLV320AIC23BxQE"
			(at 16.51 24.13 0)
		)
		(property "Footprint" "Package_BGA:Texas_MicroStar_Junior_BGA-80_5.0x5.0mm_Layout9x9_P0.5mm"
			(at 13.97 -36.83 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv320aic23b.pdf"
			(at 0 0 0)
		)
		(property "Description" "Stero Audio CODEC, 8- to 96-kHz, With Integrated Headphone Amplifier, BGA-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio codec 2ch 96kHz headphone amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*MicroStar*Junior*BGA*5*x5*mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TLV320AIC23BxQE_0_1")
		(symbol "TLV320AIC23BxQE_1_1"
			(pin input line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "SDIN")
				(number "J6")
			)
			(pin input line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "SCLK")
				(number "J7")
			)
			(pin input line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "MODE")
				(number "J5")
			)
			(pin input line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "~{CS}")
				(number "J4")
			)
			(pin input line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "DIN")
				(number "B9")
			)
			(pin input line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "LRCIN")
				(number "A8")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "BCLK")
				(number "C9")
			)
			(pin output line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "DOUT")
				(number "A7")
			)
			(pin output line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "LRCOUT")
				(number "A6")
			)
			(pin passive line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "XTI/MCK")
				(number "J8")
			)
			(pin passive line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "XTO")
				(number "H9")
			)
			(pin output line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "CLKOUT")
				(number "D9")
			)
			(pin no_connect line
				(at -12.7 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "A1")
			)
			(pin no_connect line
				(at -10.16 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "J1")
			)
			(pin power_in line
				(at -7.62 25.4 270)
				(length 2.54)
				(name "BVDD")
				(number "E9")
			)
			(pin no_connect line
				(at -7.62 12.7 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "H2")
			)
			(pin no_connect line
				(at -7.62 7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "G2")
			)
			(pin no_connect line
				(at -7.62 2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "F2")
			)
			(pin no_connect line
				(at -7.62 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "E2")
			)
			(pin no_connect line
				(at -7.62 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "D2")
			)
			(pin no_connect line
				(at -7.62 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "C2")
			)
			(pin no_connect line
				(at -7.62 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "B2")
			)
			(pin no_connect line
				(at -7.62 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "J9")
			)
			(pin no_connect line
				(at -5.08 12.7 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "H3")
			)
			(pin no_connect line
				(at -5.08 7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "G3")
			)
			(pin no_connect line
				(at -5.08 2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "F3")
			)
			(pin no_connect line
				(at -5.08 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "E3")
			)
			(pin no_connect line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "D3")
			)
			(pin no_connect line
				(at -5.08 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "B3")
			)
			(pin no_connect line
				(at -5.08 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "A9")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "DVDD")
				(number "G9")
			)
			(pin no_connect line
				(at -2.54 12.7 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "H4")
			)
			(pin no_connect line
				(at -2.54 7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "G4")
			)
			(pin no_connect line
				(at -2.54 2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "F4")
			)
			(pin no_connect line
				(at -2.54 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "E4")
			)
			(pin no_connect line
				(at -2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "D4")
			)
			(pin no_connect line
				(at -2.54 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "C4")
			)
			(pin no_connect line
				(at -2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "B4")
			)
			(pin power_in line
				(at -2.54 -25.4 90)
				(length 2.54)
				(name "DGND")
				(number "F9")
			)
			(pin no_connect line
				(at 0 12.7 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "H5")
			)
			(pin no_connect line
				(at 0 7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "G5")
			)
			(pin no_connect line
				(at 0 2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "F5")
			)
			(pin no_connect line
				(at 0 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "E5")
			)
			(pin no_connect line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "D5")
			)
			(pin no_connect line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "C5")
			)
			(pin no_connect line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "B5")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "AVDD")
				(number "D1")
			)
			(pin no_connect line
				(at 2.54 12.7 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "H6")
			)
			(pin no_connect line
				(at 2.54 7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "G6")
			)
			(pin no_connect line
				(at 2.54 2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "F6")
			)
			(pin no_connect line
				(at 2.54 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "E6")
			)
			(pin no_connect line
				(at 2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "D6")
			)
			(pin no_connect line
				(at 2.54 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "C6")
			)
			(pin no_connect line
				(at 2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "B6")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "AGND")
				(number "E1")
			)
			(pin no_connect line
				(at 5.08 12.7 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "H7")
			)
			(pin no_connect line
				(at 5.08 7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "G7")
			)
			(pin no_connect line
				(at 5.08 2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "F7")
			)
			(pin no_connect line
				(at 5.08 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "E7")
			)
			(pin no_connect line
				(at 5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "D7")
			)
			(pin no_connect line
				(at 5.08 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "C7")
			)
			(pin no_connect line
				(at 5.08 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "B7")
			)
			(pin power_in line
				(at 7.62 25.4 270)
				(length 2.54)
				(name "HPVDD")
				(number "A5")
			)
			(pin no_connect line
				(at 7.62 12.7 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "H8")
			)
			(pin no_connect line
				(at 7.62 7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "G8")
			)
			(pin no_connect line
				(at 7.62 2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "F8")
			)
			(pin no_connect line
				(at 7.62 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "E8")
			)
			(pin no_connect line
				(at 7.62 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "D8")
			)
			(pin no_connect line
				(at 7.62 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "C8")
			)
			(pin no_connect line
				(at 7.62 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "B8")
			)
			(pin power_in line
				(at 7.62 -25.4 90)
				(length 2.54)
				(name "HPGND")
				(number "A2")
			)
			(pin passive line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "LOUT")
				(number "B1")
			)
			(pin passive line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "ROUT")
				(number "C1")
			)
			(pin passive line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "LHPOUT")
				(number "A4")
			)
			(pin passive line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "RHPOUT")
				(number "A3")
			)
			(pin passive line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "LLINEIN")
				(number "J3")
			)
			(pin passive line
				(at 20.32 0 180)
				(length 2.54)
				(name "RLINEIN")
				(number "J2")
			)
			(pin passive line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "MICBIAS")
				(number "G1")
			)
			(pin passive line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "MICIN")
				(number "H1")
			)
			(pin passive line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "VMID")
				(number "F1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLV320AIC3100"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 20.32 0)
		)
		(property "Value" "TLV320AIC3100"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-32-1EP_5x5mm_P0.5mm_EP3.5x3.5mm"
			(at 0 -30.48 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv320aic3100.pdf"
			(at -30.48 -38.1 0)
		)
		(property "Description" "Low Power Audio Codec with Audio Processing and Mono Class‑D Amplifier, VQFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio codec 2ch 192kHz class-d amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TLV320AIC3100_0_1")
		(symbol "TLV320AIC3100_1_1"
			(pin input line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "~{RESET}")
				(number "31")
			)
			(pin input line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "SCL")
				(number "10")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "SDA")
				(number "9")
			)
			(pin input line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "DIN")
				(number "5")
			)
			(pin output line
				(at -20.32 0 0)
				(length 2.54)
				(name "DOUT")
				(number "4")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "BCLK")
				(number "7")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "WCLK")
				(number "6")
			)
			(pin input line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "MCLK")
				(number "8")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "GPIO1")
				(number "32")
			)
			(pin power_in line
				(at -7.62 20.32 270)
				(length 2.54)
				(name "AVDD")
				(number "17")
			)
			(pin power_in line
				(at -7.62 -20.32 90)
				(length 2.54)
				(name "AVSS")
				(number "16")
			)
			(pin power_in line
				(at -5.08 20.32 270)
				(length 2.54)
				(name "DVDD")
				(number "3")
			)
			(pin power_in line
				(at -5.08 -20.32 90)
				(length 2.54)
				(name "DVSS")
				(number "18")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 2.54)
				(name "HPVDD")
				(number "28")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 2.54)
				(name "HPVSS")
				(number "29")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "IOVDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "IOVSS")
				(number "1")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "SPKVDD")
				(number "21")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "SPKVSS")
				(number "20")
			)
			(pin passive line
				(at 2.54 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "SPKVSS")
				(number "25")
			)
			(pin power_in line
				(at 5.08 20.32 270)
				(length 2.54)
				(name "SPKVDD")
				(number "24")
			)
			(pin power_in line
				(at 5.08 -20.32 90)
				(length 2.54)
				(name "EP")
				(number "33")
			)
			(pin output line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "SPKP")
				(number "22")
			)
			(pin passive line
				(at 20.32 15.24 180)
				(length 2.54)
				(hide yes)
				(name "SPKP")
				(number "26")
			)
			(pin output line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "SPKM")
				(number "19")
			)
			(pin passive line
				(at 20.32 10.16 180)
				(length 2.54)
				(hide yes)
				(name "SPKM")
				(number "23")
			)
			(pin output line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "HPL")
				(number "27")
			)
			(pin output line
				(at 20.32 0 180)
				(length 2.54)
				(name "HPR")
				(number "30")
			)
			(pin input line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "VOL/MICDET")
				(number "11")
			)
			(pin input line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "MIC1LM")
				(number "15")
			)
			(pin power_out line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "MICBIAS")
				(number "12")
			)
			(pin input line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "MIC1LP")
				(number "13")
			)
			(pin input line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "MIC1RP")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPA5050"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 16.51 0)
		)
		(property "Value" "TPA5050"
			(at 7.62 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_S-PVQFN-N16_EP2.7x2.7mm_ThermalVias"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tpa5050.pdf"
			(at 0 0 0)
		)
		(property "Description" "Stereo Digital Audio Lip-Sync Delay Processor With I2C Control, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio delay"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas?S?PVQFN?N*"
			(at 0 0 0)
		)
		(symbol "TPA5050_0_1")
		(symbol "TPA5050_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "BCLK")
				(number "16")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "LRCLK")
				(number "1")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "DATA")
				(number "2")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "SCL")
				(number "3")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SDA")
				(number "4")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "ADD0")
				(number "10")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "ADD1")
				(number "11")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "ADD2")
				(number "12")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "DATA_OUT")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "UDA1334ATS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 16.51 0)
		)
		(property "Value" "UDA1334ATS"
			(at 3.81 16.51 0)
		)
		(property "Footprint" "Package_SO:SSOP-16_4.4x5.2mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/UDA1334ATS.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low Power Audio DAC with PLL, SSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio dac 2ch 24bit 96kHz"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*4.4x5.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "UDA1334ATS_0_1")
		(symbol "UDA1334ATS_1_1"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "BCK")
				(number "1")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "WS")
				(number "2")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "DATAI")
				(number "3")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PLL0")
				(number "10")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "SYSCLK/PLL1")
				(number "6")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "DEEM/CLKOUT")
				(number "9")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "MUTE")
				(number "8")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "SFOR0")
				(number "11")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "SFOR1")
				(number "7")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VSSD")
				(number "5")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "VSSA")
				(number "15")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "VOUTL")
				(number "14")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "VOUTR")
				(number "16")
			)
			(pin passive line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "Vref(DAC)")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "WM8731CLSEFL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 21.59 0)
		)
		(property "Value" "WM8731CLSEFL"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_5x5mm_P0.5mm_EP3.35x3.35mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://statics.cirrus.com/pubs/proDatasheet/WM8731_v4.9.pdf"
			(at 0 0 0)
		)
		(property "Description" "Portable Internet Audio CODEC with Headphone Driver and Programmable Sample Rates, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "wolfson stereo audio codec adc dac headphone"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "WM8731CLSEFL_0_1")
		(symbol "WM8731CLSEFL_1_1"
			(pin input line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "DACDAT")
				(number "8")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "DACLRC")
				(number "9")
			)
			(pin output line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "ADCDAT")
				(number "10")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "ADCLRC")
				(number "11")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "BCLK")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "SDIN")
				(number "27")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "SCLK")
				(number "28")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "~{CSB}")
				(number "26")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "MODE")
				(number "25")
			)
			(pin output line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "CLKOUT")
				(number "6")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "XTI/MCLK")
				(number "1")
			)
			(pin output line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "XTO")
				(number "2")
			)
			(pin power_in line
				(at -5.08 22.86 270)
				(length 2.54)
				(name "DCVDD")
				(number "3")
			)
			(pin power_in line
				(at -5.08 -22.86 90)
				(length 2.54)
				(name "DGND")
				(number "4")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 2.54)
				(name "DBVDD")
				(number "5")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "AVDD")
				(number "18")
			)
			(pin power_in line
				(at 2.54 -22.86 90)
				(length 2.54)
				(name "AGND")
				(number "19")
			)
			(pin passive line
				(at 2.54 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "29")
			)
			(pin power_in line
				(at 5.08 22.86 270)
				(length 2.54)
				(name "HPVDD")
				(number "12")
			)
			(pin power_in line
				(at 5.08 -22.86 90)
				(length 2.54)
				(name "HPGND")
				(number "15")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "LHPOUT")
				(number "13")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "RHPOUT")
				(number "14")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "LOUT")
				(number "16")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "ROUT")
				(number "17")
			)
			(pin input line
				(at 17.78 0 180)
				(length 2.54)
				(name "LLINEIN")
				(number "24")
			)
			(pin input line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "RLINEIN")
				(number "23")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "MICBIAS")
				(number "21")
			)
			(pin input line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "MICIN")
				(number "22")
			)
			(pin passive line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "VMID")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "WM8731SEDS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 21.59 0)
		)
		(property "Value" "WM8731SEDS"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://statics.cirrus.com/pubs/proDatasheet/WM8731_v4.9.pdf"
			(at 0 0 0)
		)
		(property "Description" "Portable Internet Audio CODEC with Headphone Driver and Programmable Sample Rates, SSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "wolfson stereo audio codec adc dac headphone"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x10.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "WM8731SEDS_0_1")
		(symbol "WM8731SEDS_1_1"
			(pin input line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "DACDAT")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "DACLRC")
				(number "5")
			)
			(pin output line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "ADCDAT")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "ADCLRC")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "BCLK")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "SDIN")
				(number "23")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "SCLK")
				(number "24")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "~{CSB}")
				(number "22")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "MODE")
				(number "21")
			)
			(pin output line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "CLKOUT")
				(number "2")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "XTI/MCLK")
				(number "25")
			)
			(pin output line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "XTO")
				(number "26")
			)
			(pin power_in line
				(at -5.08 22.86 270)
				(length 2.54)
				(name "DCVDD")
				(number "27")
			)
			(pin power_in line
				(at -5.08 -22.86 90)
				(length 2.54)
				(name "DGND")
				(number "28")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 2.54)
				(name "DBVDD")
				(number "1")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "AVDD")
				(number "14")
			)
			(pin power_in line
				(at 2.54 -22.86 90)
				(length 2.54)
				(name "AGND")
				(number "15")
			)
			(pin power_in line
				(at 5.08 22.86 270)
				(length 2.54)
				(name "HPVDD")
				(number "8")
			)
			(pin power_in line
				(at 5.08 -22.86 90)
				(length 2.54)
				(name "HPGND")
				(number "11")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "LHPOUT")
				(number "9")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "RHPOUT")
				(number "10")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "LOUT")
				(number "12")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "ROUT")
				(number "13")
			)
			(pin input line
				(at 17.78 0 180)
				(length 2.54)
				(name "LLINEIN")
				(number "20")
			)
			(pin input line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "RLINEIN")
				(number "19")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "MICBIAS")
				(number "17")
			)
			(pin input line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "MICIN")
				(number "18")
			)
			(pin passive line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "VMID")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "YM2149"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 29.21 0)
		)
		(property "Value" "YM2149"
			(at 3.81 29.21 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 16.51 -35.56 0)
		)
		(property "Datasheet" "http://www.ym2149.com/ym2149.pdf"
			(at 0 0 0)
		)
		(property "Description" "Software-Controlled Sound Generator, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio ssg 3ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "YM2149_0_1")
		(symbol "YM2149_1_1"
			(pin bidirectional line
				(at -12.7 25.4 0)
				(length 2.54)
				(name "DA0")
				(number "37")
			)
			(pin bidirectional line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "DA1")
				(number "36")
			)
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "DA2")
				(number "35")
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "DA3")
				(number "34")
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "DA4")
				(number "33")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "DA5")
				(number "32")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "DA6")
				(number "31")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "DA7")
				(number "30")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "A8")
				(number "25")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{A9}")
				(number "24")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "BDIR")
				(number "27")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "BC1")
				(number "29")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "BC2")
				(number "28")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "CLOCK")
				(number "22")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "~{SEL}")
				(number "26")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "~{RESET}")
				(number "23")
			)
			(pin passive line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "TEST1")
				(number "39")
			)
			(pin no_connect line
				(at -10.16 -17.78 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -10.16 -20.32 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 2.54)
				(name "VCC")
				(number "40")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 2.54)
				(name "VSS")
				(number "1")
			)
			(pin output line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "A")
				(number "3")
			)
			(pin output line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "B")
				(number "4")
			)
			(pin output line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "C")
				(number "38")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "IOA0")
				(number "21")
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "IOA1")
				(number "20")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "IOA2")
				(number "19")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "IOA3")
				(number "18")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "IOA4")
				(number "17")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "IOA5")
				(number "16")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "IOA6")
				(number "15")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "IOA7")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "IOB0")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "IOB1")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "IOB2")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "IOB3")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "IOB4")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "IOB5")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "IOB6")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -25.4 180)
				(length 2.54)
				(name "IOB7")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADAU1979xBCP"
		(extends "ADAU1978xBCP")
		(property "Reference" "U"
			(at 12.7 25.4 0)
		)
		(property "Value" "ADAU1979xBCP"
			(at 12.7 22.86 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-40-1EP_6x6mm_P0.5mm_EP3.9x3.9mm"
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADAU1979.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "Quad Analog-to-Digital Converter, 4.5Vrms differential inputs, LFCSP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Audio ADC I2S TDM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*6x6mm*P0.5mm*EP3.9x3.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "CS4345"
		(extends "CS4344")
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "CS4345"
			(at 6.35 11.43 0)
		)
		(property "Footprint" "Package_SO:TSSOP-10_3x3mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://statics.cirrus.com/pubs/proDatasheet/CS4344-45-48_F2.pdf"
			(at 0 0 0)
		)
		(property "Description" "16 to 24-Bit, 192 kHz Stereo D/A Converter, Left-Justified Audio Format, TSSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "stereo 2ch audio codec"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "CS4348"
		(extends "CS4344")
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "CS4348"
			(at 6.35 11.43 0)
		)
		(property "Footprint" "Package_SO:TSSOP-10_3x3mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://statics.cirrus.com/pubs/proDatasheet/CS4344-45-48_F2.pdf"
			(at 0 0 0)
		)
		(property "Description" "16-Bit, 192 kHz Stereo D/A Converter, Right-Justified Audio Format, TSSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "stereo 2ch audio codec"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "CS5344"
		(extends "CS5343")
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "CS5344"
			(at 6.35 11.43 0)
		)
		(property "Footprint" "Package_SO:TSSOP-10_3x3mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://statics.cirrus.com/pubs/proDatasheet/CS5343-44_F5.pdf"
			(at 0 0 0)
		)
		(property "Description" "98 dB, 96 kHz, 24bit Stereo Audio A/D Converter, Left-Justified Audio Format, TSSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "stereo 2ch audio codec"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "CS8416-xZZ"
		(extends "CS8416-xSZ")
		(property "Reference" "U"
			(at 12.7 26.67 0)
		)
		(property "Value" "CS8416-xZZ"
			(at 12.7 24.13 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://d3uzseaevmutz1.cloudfront.net/pubs/proDatasheet/CS8416_F3.pdf"
			(at 0 0 0)
		)
		(property "Description" "192 kHz Digital Audio Interface Receiver, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio digital interface receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x17.9mm*P1.27mm* TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ISD25120P"
		(extends "ISD2560P")
		(property "Reference" "U"
			(at -12.192 24.13 0)
		)
		(property "Value" "ISD25120P"
			(at 9.144 24.13 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W15.24mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://datasheetspdf.com/pdf-file/700027/Winbond/ISD2560/1"
			(at 16.51 -6.35 0)
		)
		(property "Description" "Single-Chip Voice Record/Playback Device 120-Second Duration, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "isd25120"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "ISD25120S"
		(extends "ISD2560S")
		(property "Reference" "U"
			(at -12.192 24.13 0)
		)
		(property "Value" "ISD25120S"
			(at 9.144 24.13 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 1.27 -5.08 0)
		)
		(property "Datasheet" "https://datasheetspdf.com/pdf-file/700027/Winbond/ISD2560/1"
			(at 16.51 -6.35 0)
		)
		(property "Description" "Single-Chip Voice Record/Playback Device 120-Second Duration, SOIC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "isd25120"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ISD2575E"
		(extends "ISD2560E")
		(property "Reference" "U"
			(at -12.192 24.13 0)
		)
		(property "Value" "ISD2575E"
			(at 9.144 24.13 0)
		)
		(property "Footprint" "Package_SO:TSOP-I-28_11.8x8mm_P0.55mm"
			(at 1.27 -5.08 0)
		)
		(property "Datasheet" "https://datasheetspdf.com/pdf-file/700027/Winbond/ISD2560/1"
			(at 16.51 -6.35 0)
		)
		(property "Description" "Single-Chip Voice Record/Playback Device 75-Second Duration, TSOP-I-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "isd2575"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOP*11.8x8mm*P0.55mm*"
			(at 0 0 0)
		)
	)
	(symbol "ISD2575P"
		(extends "ISD2560P")
		(property "Reference" "U"
			(at -12.192 24.13 0)
		)
		(property "Value" "ISD2575P"
			(at 9.144 24.13 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W15.24mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://datasheetspdf.com/pdf-file/700027/Winbond/ISD2560/1"
			(at 16.51 -6.35 0)
		)
		(property "Description" "Single-Chip Voice Record/Playback Device 75-Second Duration, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "isd2575"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "ISD2575S"
		(extends "ISD2560S")
		(property "Reference" "U"
			(at -12.192 24.13 0)
		)
		(property "Value" "ISD2575S"
			(at 9.144 24.13 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 1.27 -5.08 0)
		)
		(property "Datasheet" "https://datasheetspdf.com/pdf-file/700027/Winbond/ISD2560/1"
			(at 16.51 -6.35 0)
		)
		(property "Description" "Single-Chip Voice Record/Playback Device 75-Second Duration, SOIC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "isd2575"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ISD2590E"
		(extends "ISD2560E")
		(property "Reference" "U"
			(at -12.192 24.13 0)
		)
		(property "Value" "ISD2590E"
			(at 9.144 24.13 0)
		)
		(property "Footprint" "Package_SO:TSOP-I-28_11.8x8mm_P0.55mm"
			(at 1.27 -5.08 0)
		)
		(property "Datasheet" "https://datasheetspdf.com/pdf-file/700027/Winbond/ISD2560/1"
			(at 16.51 -6.35 0)
		)
		(property "Description" "Single-Chip Voice Record/Playback Device 90-Second Duration, TSOP-I-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "isd2590"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOP*11.8x8mm*P0.55mm*"
			(at 0 0 0)
		)
	)
	(symbol "ISD2590P"
		(extends "ISD2560P")
		(property "Reference" "U"
			(at -12.192 24.13 0)
		)
		(property "Value" "ISD2590P"
			(at 9.144 24.13 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W15.24mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://datasheetspdf.com/pdf-file/700027/Winbond/ISD2560/1"
			(at 16.51 -6.35 0)
		)
		(property "Description" "Single-Chip Voice Record/Playback Device 90-Second Duration, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "isd2590"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "ISD2590S"
		(extends "ISD2560S")
		(property "Reference" "U"
			(at -12.192 24.13 0)
		)
		(property "Value" "ISD2590S"
			(at 9.144 24.13 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 1.27 -5.08 0)
		)
		(property "Datasheet" "https://datasheetspdf.com/pdf-file/700027/Winbond/ISD2560/1"
			(at 16.51 -6.35 0)
		)
		(property "Description" "Single-Chip Voice Record/Playback Device 90-Second Duration, SOIC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "isd2590"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX98357B"
		(extends "MAX98357A")
		(property "Reference" "U"
			(at -8.89 11.43 0)
		)
		(property "Value" "MAX98357B"
			(at 10.16 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:TQFN-16-1EP_3x3mm_P0.5mm_EP1.23x1.23mm"
			(at -1.27 -2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX98357A-MAX98357B.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "Mono DAC with amplifier, I2S, left-justified, TDM, 32-bit, 96khz, 3.2W, TQFP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "tdm i2s left-justified amplifier audio dac"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFN*3x3mm*P0.5mm*EP1.23x1.23mm*"
			(at 0 0 0)
		)
	)
	(symbol "PCM5100A"
		(extends "PCM5100")
		(property "Reference" "U"
			(at -10.16 13.97 0)
		)
		(property "Value" "PCM5100A"
			(at 3.81 13.97 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 25.4 -16.51 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/pcm5100a.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.1 VRMS, 100dB Audio Stereo DAC with PLL and 32-bit, 384kHz PCM Interface, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio dac 2ch 32bit 384kHz"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PCM5101"
		(extends "PCM5100")
		(property "Reference" "U"
			(at -10.16 13.97 0)
		)
		(property "Value" "PCM5101"
			(at 3.81 13.97 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -1.27 19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/pcm5101.pdf"
			(at -1.27 19.05 0)
		)
		(property "Description" "2VRMS DirectPath, 106dB Audio Stereo DAC with 32-bit, 384kHz PCM Interface, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio dac 2ch 32bit 384kHz"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PCM5101A"
		(extends "PCM5100")
		(property "Reference" "U"
			(at -10.16 13.97 0)
		)
		(property "Value" "PCM5101A"
			(at 3.81 13.97 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 25.4 -16.51 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/pcm5101a.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.1 VRMS, 106dB Audio Stereo DAC with PLL and 32-bit, 384kHz PCM Interface, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio dac 2ch 32bit 384kHz"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PCM5102"
		(extends "PCM5100")
		(property "Reference" "U"
			(at -10.16 13.97 0)
		)
		(property "Value" "PCM5102"
			(at 3.81 13.97 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -1.27 19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/pcm5102.pdf"
			(at -1.27 19.05 0)
		)
		(property "Description" "2VRMS DirectPath, 112dB Audio Stereo DAC with 32-bit, 384kHz PCM Interface, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio dac 2ch 32bit 384kHz"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PCM5102A"
		(extends "PCM5100")
		(property "Reference" "U"
			(at -10.16 13.97 0)
		)
		(property "Value" "PCM5102A"
			(at 3.81 13.97 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 25.4 -16.51 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/pcm5102a.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.1 VRMS, 112dB Audio Stereo DAC with PLL and 32-bit, 384kHz PCM Interface, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio dac 2ch 32bit 384kHz"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PCM5121PW"
		(extends "PCM5122PW")
		(property "Reference" "U"
			(at -13.97 21.59 0)
		)
		(property "Value" "PCM5121PW"
			(at 10.16 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/pcm5121.pdf"
			(at 0 26.67 0)
		)
		(property "Description" "2VRMS DirectPath, 106dB Audio Stereo DAC with 32-bit, 384kHz PCM Interface, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio dac 2ch 32bit 384kHz"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PGA2310PA"
		(extends "PGA2310UA")
		(property "Reference" "U"
			(at 12.7 0 0)
		)
		(property "Value" "PGA2310PA"
			(at 17.78 -2.54 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 0 -38.1 0)
		)
		(property "Datasheet" "https://www.ti.com.cn/cn/lit/gpn/pga2310"
			(at 0 -40.64 0)
		)
		(property "Description" "2-Channel Audio Volume Control, SPI Interface, +31.5dB to -95.5dB, PDIP-16"
			(at 0 -35.56 0)
		)
		(property "ki_keywords" "audio volume control 2ch spi"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*16*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "PT2258-S"
		(extends "PT2258")
		(property "Reference" "U"
			(at -8.89 16.51 0)
		)
		(property "Value" "PT2258-S"
			(at 6.35 16.51 0)
		)
		(property "Footprint" "Package_SO:SO-20_12.8x7.5mm_P1.27mm"
			(at 0 -24.13 0)
		)
		(property "Datasheet" "http://www.princeton.com.tw/Portals/0/Product/PT2258-s.pdf"
			(at 0 -27.94 0)
		)
		(property "Description" "6-Channel Electronic Volume Controller, SOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Volume"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*12.8x7.5mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "RD5107A"
		(extends "RD5106A")
		(property "Reference" "U"
			(at -10.16 12.7 0)
		)
		(property "Value" "RD5107A"
			(at 10.16 -12.7 0)
		)
		(property "Footprint" ""
			(at -10.16 7.62 0)
		)
		(property "Datasheet" "http://pdf.datasheetarchive.com/indexerfiles/Scans-091/DSAHI00048836.pdf"
			(at -7.62 10.16 0)
		)
		(property "Description" "Analog Delay Line 512 sample bucket brigade device, 1msec to more than 2seconds, input signal frequency range 0 to 170KHz, clock frequency range 500Hz to 1MHz"
			(at 0 0 0)
		)
		(property "ki_keywords" "EG&G RETICON BBD N-channel silicon-gate"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP-8*"
			(at 0 0 0)
		)
	)
	(symbol "RE46C318"
		(extends "RE46C317")
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "RE46C318"
			(at 12.7 8.89 0)
		)
		(property "Footprint" ""
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22301B.pdf"
			(at 3.81 -15.24 0)
		)
		(property "Description" "Piezoelectric Horn Driver with Boost Converter, 3.3V supply, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Horn driver Piezo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*8*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "SAD512"
		(extends "SAD1024")
		(property "Reference" "U"
			(at -8.89 11.43 0)
		)
		(property "Value" "SAD512"
			(at 7.62 11.43 0)
		)
		(property "Footprint" ""
			(at -10.16 7.62 0)
		)
		(property "Datasheet" "http://thmq.mysteria.cz/em1022/SAD1024.pdf"
			(at -7.62 10.16 0)
		)
		(property "Description" "SAD-512 ANALOG DELAY LINE, bucket brigade device, 512 stages, signal frequency range 0 to 200KHz, clock frequency range 1.5KHz to 1.5MHz"
			(at 0 0 0)
		)
		(property "ki_keywords" "EG&G RETICON BBD N-channel silicon-gate"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP-16*"
			(at 0 0 0)
		)
	)
	(symbol "THAT1583"
		(extends "THAT1580")
		(property "Reference" "U"
			(at 3.81 7.62 0)
		)
		(property "Value" "THAT1583"
			(at 5.08 5.08 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_4x4mm_P0.65mm_EP2.1x2.1mm_ThermalVias"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.thatcorp.com/datashts/THAT_1583_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, Differential Audio Preamplifier IC, 0.006% THD+N, -128.9dBu EIN, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "diff amp mic preamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "THAT6262"
		(extends "THAT6261")
		(property "Reference" "U"
			(at -13.97 8.89 0)
		)
		(property "Value" "THAT6262"
			(at 15.24 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.45x5.45mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.thatcorp.com/datashts/THAT_626x_Datasheet.pdf"
			(at -2.54 -2.54 0)
		)
		(property "Description" "2-Channel Low-Noise Programmable-Gain Preamplifier - ADC Driver IC, 2dB Step, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual mic preamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "THAT6263"
		(extends "THAT6261")
		(property "Reference" "U"
			(at -13.97 8.89 0)
		)
		(property "Value" "THAT6263"
			(at 15.24 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.45x5.45mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.thatcorp.com/datashts/THAT_626x_Datasheet.pdf"
			(at -2.54 -2.54 0)
		)
		(property "Description" "2-Channel Low-Noise Programmable-Gain Preamplifier - ADC Driver IC, 3dB Step, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual mic preamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "WM8731CSEFL"
		(extends "WM8731CLSEFL")
		(property "Reference" "U"
			(at -13.97 21.59 0)
		)
		(property "Value" "WM8731CSEFL"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_5x5mm_P0.5mm_EP3.35x3.35mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://statics.cirrus.com/pubs/proDatasheet/WM8731_v4.9.pdf"
			(at 0 0 0)
		)
		(property "Description" "Portable Internet Audio CODEC with Headphone Driver and Programmable Sample Rates, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "wolfson stereo audio codec adc dac headphone"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
)
