(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "ADP5063"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 -16.51 0)
		)
		(property "Value" "ADP5063"
			(at 2.54 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.5x2.5mm"
			(at 6.35 -22.86 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP5063.pdf"
			(at -55.88 36.83 0)
		)
		(property "Description" "Linear LiFePO4 Battery Charger with Power Path and USB Compatibility, LFCSP"
			(at 0 0 0)
		)
		(property "ki_keywords" "LiFePo4 Battery USB PMIC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ADP5063_1_1"
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(hide yes)
				(name "VINx")
				(number "6")
			)
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "VINx")
				(number "7")
			)
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(hide yes)
				(name "VINx")
				(number "8")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "D_IO1")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "D_IO2")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "D_IO3")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SCL")
				(number "1")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SDA")
				(number "17")
			)
			(pin passive line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "CBP")
				(number "19")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "20")
			)
			(pin passive line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "EP")
				(number "21")
			)
			(pin power_out line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "ISO_Sx")
				(number "10")
			)
			(pin passive line
				(at 10.16 12.7 180)
				(length 2.54)
				(hide yes)
				(name "ISO_Sx")
				(number "11")
			)
			(pin passive line
				(at 10.16 12.7 180)
				(length 2.54)
				(hide yes)
				(name "ISO_Sx")
				(number "9")
			)
			(pin open_collector line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "ILED")
				(number "15")
			)
			(pin open_collector line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SYS_EN")
				(number "16")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "ISO_Bx")
				(number "12")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "ISO_Bx")
				(number "13")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "ISO_Bx")
				(number "14")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "BAT_SNS")
				(number "4")
			)
			(pin passive line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "THR")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADP5090ACP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 13.97 0)
		)
		(property "Value" "ADP5090ACP"
			(at 7.62 13.97 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-16-1EP_3x3mm_P0.5mm_EP1.7x1.7mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP5090.pdf"
			(at 7.62 -7.62 0)
		)
		(property "Description" "Ultralow Power Boost Regulator with MPPT and Charge Management, LFCSP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "boost regulator MPPT charge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ADP5090ACP_0_1")
		(symbol "ADP5090ACP_1_1"
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "SW")
				(number "9")
			)
			(pin power_in line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "VIN")
				(number "7")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "MPPT")
				(number "5")
			)
			(pin passive line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "BACKUP")
				(number "12")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "DIS_SW")
				(number "14")
			)
			(pin passive line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "CBP")
				(number "6")
			)
			(pin passive line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "MINOP")
				(number "4")
			)
			(pin passive line
				(at -2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "17")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "AGND")
				(number "3")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "PGND")
				(number "8")
			)
			(pin power_out line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "SYS")
				(number "11")
			)
			(pin power_out line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "BAT")
				(number "10")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PGOOD")
				(number "13")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "REF")
				(number "15")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "SETSD")
				(number "1")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "SETPG")
				(number "16")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "TERM")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADP5091"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "ADP5091"
			(at 7.62 26.67 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-24-1EP_4x4mm_P0.5mm_EP2.3x2.3mm"
			(at 30.48 -26.67 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP5091-5092.pdf"
			(at 0 0 0)
		)
		(property "Description" "Ultralow Power Energy Harvester PMUs with MPPT and Charge Management, LFCSP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "energy harvester"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ADP5091_0_1")
		(symbol "ADP5091_1_1"
			(pin power_in line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "SW")
				(number "13")
			)
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "MPPT")
				(number "9")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "REG_D1")
				(number "23")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "REG_D0")
				(number "24")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "VID")
				(number "20")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "DIS_SW")
				(number "22")
			)
			(pin passive line
				(at -15.24 0 0)
				(length 2.54)
				(name "MINOP")
				(number "21")
			)
			(pin passive line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "CBP")
				(number "8")
			)
			(pin passive line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "REF")
				(number "1")
			)
			(pin passive line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "SETSD")
				(number "2")
			)
			(pin passive line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "SETBK")
				(number "3")
			)
			(pin passive line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "TERM")
				(number "4")
			)
			(pin passive line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "SETPG")
				(number "5")
			)
			(pin passive line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "SETHYST")
				(number "6")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VIN")
				(number "10")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 2.54)
				(name "PGND")
				(number "12")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "25")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "AGND")
				(number "7")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "BACK_UP")
				(number "18")
			)
			(pin power_out line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "BAT")
				(number "17")
			)
			(pin power_out line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "REG_FB")
				(number "15")
			)
			(pin power_out line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "REG_OUT")
				(number "14")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "LLD")
				(number "11")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PGOOD")
				(number "19")
			)
			(pin power_out line
				(at 15.24 0 180)
				(length 2.54)
				(name "SYS")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADP5092"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "ADP5092"
			(at 7.62 26.67 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-24-1EP_4x4mm_P0.5mm_EP2.3x2.3mm"
			(at 30.48 -26.67 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP5091-5092.pdf"
			(at 0 0 0)
		)
		(property "Description" "Ultralow Power Energy Harvester PMUs with MPPT and Charge Management, LFCSP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "energy harvester"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ADP5092_0_1")
		(symbol "ADP5092_1_1"
			(pin power_in line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "SW")
				(number "13")
			)
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "MPPT")
				(number "9")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "REG_D1")
				(number "23")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "REG_D0")
				(number "24")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "VID")
				(number "20")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "DIS_SW")
				(number "22")
			)
			(pin passive line
				(at -15.24 0 0)
				(length 2.54)
				(name "MINOP")
				(number "21")
			)
			(pin passive line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "CBP")
				(number "8")
			)
			(pin passive line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "REF")
				(number "1")
			)
			(pin passive line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "SETSD")
				(number "2")
			)
			(pin passive line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "SETBK")
				(number "3")
			)
			(pin passive line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "TERM")
				(number "4")
			)
			(pin passive line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "SETPG")
				(number "5")
			)
			(pin passive line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "SETHYST")
				(number "6")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VIN")
				(number "10")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 2.54)
				(name "PGND")
				(number "12")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "25")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "AGND")
				(number "7")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "BACK_UP")
				(number "18")
			)
			(pin power_out line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "BAT")
				(number "17")
			)
			(pin power_out line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "REG_FB")
				(number "15")
			)
			(pin power_out line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "REG_OUT")
				(number "14")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "REG_GOOD")
				(number "11")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PGOOD")
				(number "19")
			)
			(pin power_out line
				(at 15.24 0 180)
				(length 2.54)
				(name "SYS")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AP9101CK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AP9101CK"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -1.27 0 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP9101C.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "Li+ Battery Protection IC for Single Cell Pack, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery protection li-ion li-po"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "AP9101CK_0_1")
		(symbol "AP9101CK_1_1"
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "VM")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "VSS")
				(number "3")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "CO")
				(number "5")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "DO")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AP9101CK6"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AP9101CK6"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP9101C.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "Li+ Battery Protection IC for Single Cell Pack, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery protection li-ion li-po"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "AP9101CK6_0_1")
		(symbol "AP9101CK6_1_1"
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "VM")
				(number "2")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "VSS")
				(number "6")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "CO")
				(number "3")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "DO")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "APW7261"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.604 16.256 0)
		)
		(property "Value" "APW7261"
			(at 3.302 16.256 0)
		)
		(property "Footprint" "Package_CSP:Anpec_WLCSP-20_1.76x2.03mm_Layout4x5_P0.4mm"
			(at 0 -29.972 0)
		)
		(property "Datasheet" "https://www.lcsc.com/datasheet/lcsc_datasheet_2007032014_Anpec-Elec-APW7261HAI-TRG_C691404.pdf"
			(at 0.254 -35.052 0)
		)
		(property "Description" "USB-OTG switch-mode lithium battery charger, WLCSP-20"
			(at 0 -32.512 0)
		)
		(property "ki_keywords" "lipo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Anpec*WLCSP*1.76x2.03mm*Layout4x5*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "APW7261_1_1"
			(pin power_in line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "VBUS")
				(number "A1")
			)
			(pin passive line
				(at -10.16 12.7 0)
				(length 2.54)
				(hide yes)
				(name "VBUS")
				(number "A2")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "PMID")
				(number "B1")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(hide yes)
				(name "PMID")
				(number "B2")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(hide yes)
				(name "PMID")
				(number "B3")
			)
			(pin power_out line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "REGN")
				(number "E3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "OTG")
				(number "D4")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "CD")
				(number "E2")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "PGND")
				(number "D1")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "D2")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "D3")
			)
			(pin power_out line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "SW")
				(number "C1")
			)
			(pin passive line
				(at 10.16 12.7 180)
				(length 2.54)
				(hide yes)
				(name "SW")
				(number "C2")
			)
			(pin passive line
				(at 10.16 12.7 180)
				(length 2.54)
				(hide yes)
				(name "SW")
				(number "C3")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "BOOT")
				(number "A3")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "CSIN")
				(number "E1")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "CSOUT")
				(number "E4")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "SCL")
				(number "A4")
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "SDA")
				(number "B4")
			)
			(pin open_collector line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "STAT")
				(number "C4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AS8506C"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 21.59 0)
		)
		(property "Value" "AS8506C"
			(at 11.43 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-40-1EP_6x6mm_P0.5mm_EP4.6x4.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ams.com/eng/content/download/476603/1402377/252935"
			(at -24.13 5.08 0)
		)
		(property "Description" "Stackable cell monitor, cell balancer, 3-7 Cells, SPI Interface"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery balance lithium charge afe"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*6x6mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AS8506C_0_1")
		(symbol "AS8506C_1_1"
			(pin input line
				(at -22.86 17.78 0)
				(length 2.54)
				(name "VREF_H")
				(number "40")
			)
			(pin input line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "VREF_IN")
				(number "12")
			)
			(pin input line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "VC7")
				(number "3")
			)
			(pin input line
				(at -22.86 7.62 0)
				(length 2.54)
				(name "VC6")
				(number "4")
			)
			(pin input line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "VS5")
				(number "5")
			)
			(pin input line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "VC4")
				(number "6")
			)
			(pin input line
				(at -22.86 0 0)
				(length 2.54)
				(name "VC3")
				(number "7")
			)
			(pin input line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "VC2")
				(number "8")
			)
			(pin input line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "VC1")
				(number "9")
			)
			(pin input line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "CGND")
				(number "10")
			)
			(pin input line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "TSECH")
				(number "1")
			)
			(pin input line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "TSECL")
				(number "2")
			)
			(pin no_connect line
				(at -10.16 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin power_in line
				(at -7.62 22.86 270)
				(length 2.54)
				(name "VSUP")
				(number "38")
			)
			(pin no_connect line
				(at -7.62 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "NC_T")
				(number "20")
			)
			(pin input line
				(at -5.08 22.86 270)
				(length 2.54)
				(name "TRIG_OUT")
				(number "37")
			)
			(pin power_in line
				(at -5.08 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin input line
				(at -2.54 22.86 270)
				(length 2.54)
				(name "CLK_OUT")
				(number "36")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 2.54)
				(name "PAD")
				(number "41")
			)
			(pin input line
				(at 0 22.86 270)
				(length 2.54)
				(name "CVT_NOK_IN")
				(number "35")
			)
			(pin input line
				(at 0 -20.32 90)
				(length 2.54)
				(name "MS_SL")
				(number "39")
			)
			(pin input line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "BD_IN")
				(number "34")
			)
			(pin input line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "FD_OUT")
				(number "18")
			)
			(pin input line
				(at 5.08 22.86 270)
				(length 2.54)
				(name "FD_IN")
				(number "33")
			)
			(pin input line
				(at 5.08 -20.32 90)
				(length 2.54)
				(name "BD_OUT")
				(number "17")
			)
			(pin input line
				(at 7.62 22.86 270)
				(length 2.54)
				(name "WAKE_OUT")
				(number "32")
			)
			(pin input line
				(at 10.16 22.86 270)
				(length 2.54)
				(name "V5V_IN")
				(number "31")
			)
			(pin input line
				(at 10.16 -20.32 90)
				(length 2.54)
				(name "CVT_NOK_OUT")
				(number "16")
			)
			(pin input line
				(at 12.7 -20.32 90)
				(length 2.54)
				(name "WAKE_IN")
				(number "19")
			)
			(pin input line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "V5V")
				(number "30")
			)
			(pin input line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "REF_T")
				(number "29")
			)
			(pin input line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "CELL_THU")
				(number "25")
			)
			(pin input line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "CELL_THL")
				(number "26")
			)
			(pin input line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "TEMP_IN2")
				(number "27")
			)
			(pin input line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "TEMP_IN1")
				(number "28")
			)
			(pin input line
				(at 22.86 0 180)
				(length 2.54)
				(name "TRIG_IN")
				(number "14")
			)
			(pin input line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "CLK_IN")
				(number "15")
			)
			(pin output line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "SDO")
				(number "21")
			)
			(pin input line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "SDI")
				(number "22")
			)
			(pin input line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "SCKL")
				(number "23")
			)
			(pin input line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "~{CS}")
				(number "24")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BQ2003"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 26.67 0)
		)
		(property "Value" "BQ2003"
			(at 5.08 -26.67 0)
		)
		(property "Footprint" ""
			(at 3.048 24.13 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/bq2003.pdf"
			(at 0 30.48 0)
		)
		(property "Description" "Standalone switchmode NiCd/NiMH battery charger, 2-4 cells, negative dV and dT/dt termination"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery nickel cadmium metal hydride"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "BQ2003_0_1")
		(symbol "BQ2003_1_1"
			(pin input line
				(at -10.16 20.32 0)
				(length 2.54)
				(name "CCMD")
				(number "1")
			)
			(pin input line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "DCMD")
				(number "2")
			)
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "DVEN")
				(number "3")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "TM_{1}")
				(number "4")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "TM_{2}")
				(number "5")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "TS")
				(number "6")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "BAT")
				(number "7")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "SNS")
				(number "9")
			)
			(pin input line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "TCO")
				(number "10")
			)
			(pin input line
				(at -10.16 -20.32 0)
				(length 2.54)
				(name "MCV")
				(number "11")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "V_{CC}")
				(number "16")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "V_{SS}")
				(number "8")
			)
			(pin output line
				(at 10.16 20.32 180)
				(length 2.54)
				(name "TEMP")
				(number "12")
			)
			(pin output line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "CHG")
				(number "13")
			)
			(pin output line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "MOD")
				(number "14")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "DIS")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BQ21040DBV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "BQ21040DBV"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/bq21040.pdf"
			(at 0 -18.288 0)
		)
		(property "Description" "Single cell, 0.8A Li-Ion/Li-Po linear charge management controller, up to 30V input, 4.2V charge voltage, Open-Drain Status Output, Temperature sense input, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "1-cell battery charger lithium"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "BQ21040DBV_0_1")
		(symbol "BQ21040DBV_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "6")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "ISET")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "2")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "TS")
				(number "1")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{CHG}")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BQ24004"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 16.51 0)
		)
		(property "Value" "BQ24004"
			(at 5.08 16.51 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3.4x6.5mm_Mask2.4x3.7mm"
			(at 0 29.21 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/bq24006.pdf"
			(at 0 45.72 0)
		)
		(property "Description" "2-Cell Li-Ion Charge Management IC, HTSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "2-Cell Li-Ion Charge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*1EP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "BQ24004_0_1")
		(symbol "BQ24004_1_1"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "3")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "ISNS")
				(number "5")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "EN")
				(number "8")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "APG/THERM")
				(number "7")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "VSEL")
				(number "9")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "CR")
				(number "12")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "TMR_SEL")
				(number "13")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 5.08 -17.78 90)
				(length 2.54)
				(name "AGND")
				(number "16")
			)
			(pin no_connect line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "N/C")
				(number "15")
			)
			(pin no_connect line
				(at 10.16 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "N/C")
				(number "1")
			)
			(pin no_connect line
				(at 10.16 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "N/C")
				(number "6")
			)
			(pin no_connect line
				(at 10.16 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "N/C")
				(number "11")
			)
			(pin no_connect line
				(at 10.16 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "N/C")
				(number "20")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "OUT")
				(number "18")
			)
			(pin passive line
				(at 12.7 12.7 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "19")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "VSENSE")
				(number "17")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "STAT1")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BQ24005"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 16.51 0)
		)
		(property "Value" "BQ24005"
			(at 5.08 16.51 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3.4x6.5mm_Mask2.4x3.7mm"
			(at 0 29.21 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/bq24006.pdf"
			(at 0 45.72 0)
		)
		(property "Description" "2-Cell Li-Ion Charge Management IC, HTSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "2-Cell Li-Ion Charge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*1EP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "BQ24005_0_1")
		(symbol "BQ24005_1_1"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "3")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "ISNS")
				(number "5")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "EN")
				(number "8")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "APG/THERM")
				(number "7")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "VSEL")
				(number "9")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "CR")
				(number "12")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "TMR_SEL")
				(number "13")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 5.08 -17.78 90)
				(length 2.54)
				(name "AGND")
				(number "16")
			)
			(pin no_connect line
				(at 10.16 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "N/C")
				(number "1")
			)
			(pin no_connect line
				(at 10.16 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "N/C")
				(number "6")
			)
			(pin no_connect line
				(at 10.16 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "N/C")
				(number "11")
			)
			(pin no_connect line
				(at 10.16 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "N/C")
				(number "20")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "OUT")
				(number "18")
			)
			(pin passive line
				(at 12.7 12.7 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "19")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "VSENSE")
				(number "17")
			)
			(pin open_collector line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "STAT1")
				(number "14")
			)
			(pin open_collector line
				(at 12.7 0 180)
				(length 2.54)
				(name "STAT2")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BQ24006"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 16.51 0)
		)
		(property "Value" "BQ24006"
			(at 5.08 16.51 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3.4x6.5mm_Mask2.4x3.7mm"
			(at 0 45.72 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/bq24006.pdf"
			(at 0 45.72 0)
		)
		(property "Description" "2-Cell Li-Ion Charge Management IC, HTSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "2-Cell Li-Ion Charge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*1EP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "BQ24006_0_1")
		(symbol "BQ24006_1_1"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "3")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "ISNS")
				(number "5")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "EN")
				(number "8")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "APG/THERM")
				(number "7")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "VSEL")
				(number "9")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "CR")
				(number "12")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "TMR_SEL")
				(number "13")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 5.08 -17.78 90)
				(length 2.54)
				(name "AGND")
				(number "16")
			)
			(pin no_connect line
				(at 10.16 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "N/C")
				(number "1")
			)
			(pin no_connect line
				(at 10.16 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "N/C")
				(number "6")
			)
			(pin no_connect line
				(at 10.16 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "N/C")
				(number "11")
			)
			(pin no_connect line
				(at 10.16 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "N/C")
				(number "20")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "OUT")
				(number "18")
			)
			(pin passive line
				(at 12.7 12.7 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "19")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "VSENSE")
				(number "17")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "STAT1")
				(number "14")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "STAT2")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BQ24012"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 15.24 0)
		)
		(property "Value" "BQ24012"
			(at -12.7 17.78 0)
		)
		(property "Footprint" "Package_SON:VSON-10-1EP_3x3mm_P0.5mm_EP1.65x2.4mm_ThermalVias"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/bq24012.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Chip Li-Ion Charge Management IC, DFN-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "Battery Charger Li-Ion"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSON*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "BQ24012_0_1")
		(symbol "BQ24012_1_1"
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{CE}")
				(number "8")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "2")
			)
			(pin passive line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "1EP")
				(number "11")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "BAT")
				(number "9")
			)
			(pin power_out line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "OUT")
				(number "10")
			)
			(pin open_collector line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "STAT1")
				(number "3")
			)
			(pin open_collector line
				(at 12.7 0 180)
				(length 2.54)
				(name "STAT2")
				(number "4")
			)
			(pin open_collector line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "~{PG}")
				(number "7")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "ISET")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BQ24013"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 12.7 0)
		)
		(property "Value" "BQ24013"
			(at 7.62 12.7 0)
		)
		(property "Footprint" "Package_SON:Texas_DRC0010J_ThermalVias"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/bq24012.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "Single-Chip Li-Ion Charge Management IC, VSON-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "Batter Charger Li-Ion"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DRC0010J*"
			(at 0 0 0)
		)
		(symbol "BQ24013_0_1")
		(symbol "BQ24013_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{CE}")
				(number "7")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{TTE}")
				(number "8")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "2")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "11")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin power_out line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "OUT")
				(number "10")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "BAT")
				(number "9")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "STAT1")
				(number "3")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "STAT2")
				(number "4")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "ISET")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BQ24072RGT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 13.97 0)
		)
		(property "Value" "BQ24072RGT"
			(at 16.51 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.6x1.6mm"
			(at 7.62 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/bq24072.pdf"
			(at 7.62 5.08 0)
		)
		(property "Description" "USB-Friendly Li-Ion Battery Charger and Power-Path Management, VQFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB Charger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "BQ24072RGT_0_1")
		(symbol "BQ24072RGT_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "TD")
				(number "15")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "~{CE}")
				(number "4")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "TMR")
				(number "14")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "EN1")
				(number "6")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "EN2")
				(number "5")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "ILIM")
				(number "12")
			)
			(pin passive line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "ISET")
				(number "16")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "IN")
				(number "13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "17")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "VSS")
				(number "8")
			)
			(pin power_out line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "OUT")
				(number "10")
			)
			(pin passive line
				(at 12.7 10.16 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "11")
			)
			(pin power_out line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "BAT")
				(number "2")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(hide yes)
				(name "BAT")
				(number "3")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "TS")
				(number "1")
			)
			(pin open_collector line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "~{PGOOD}")
				(number "7")
			)
			(pin open_collector line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "~{CHG}")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BQ24074RGT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 13.97 0)
		)
		(property "Value" "BQ24074RGT"
			(at 16.51 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.6x1.6mm"
			(at 7.62 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/bq24074.pdf"
			(at 7.62 5.08 0)
		)
		(property "Description" "USB-Friendly Li-Ion Battery Charger and Power-Path Management, VQFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB Charger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "BQ24074RGT_0_1")
		(symbol "BQ24074RGT_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "ITERM")
				(number "15")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "~{CE}")
				(number "4")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "TMR")
				(number "14")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "EN1")
				(number "6")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "EN2")
				(number "5")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "ILIM")
				(number "12")
			)
			(pin passive line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "ISET")
				(number "16")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "IN")
				(number "13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "17")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "VSS")
				(number "8")
			)
			(pin power_out line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "OUT")
				(number "10")
			)
			(pin passive line
				(at 12.7 10.16 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "11")
			)
			(pin power_out line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "BAT")
				(number "2")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(hide yes)
				(name "BAT")
				(number "3")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "TS")
				(number "1")
			)
			(pin open_collector line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "~{PGOOD}")
				(number "7")
			)
			(pin open_collector line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "~{CHG}")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BQ24075RGT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 13.97 0)
		)
		(property "Value" "BQ24075RGT"
			(at 16.51 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.6x1.6mm"
			(at 7.62 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/bq24075.pdf"
			(at 7.62 5.08 0)
		)
		(property "Description" "USB-Friendly Li-Ion Battery Charger and Power-Path Management, VQFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB Charger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "BQ24075RGT_0_1")
		(symbol "BQ24075RGT_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "SYSOFF")
				(number "15")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "~{CE}")
				(number "4")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "TMR")
				(number "14")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "EN1")
				(number "6")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "EN2")
				(number "5")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "ILIM")
				(number "12")
			)
			(pin passive line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "ISET")
				(number "16")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "IN")
				(number "13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "17")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "VSS")
				(number "8")
			)
			(pin power_out line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "OUT")
				(number "10")
			)
			(pin passive line
				(at 12.7 10.16 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "11")
			)
			(pin power_out line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "BAT")
				(number "2")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(hide yes)
				(name "BAT")
				(number "3")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "TS")
				(number "1")
			)
			(pin open_collector line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "~{PGOOD}")
				(number "7")
			)
			(pin open_collector line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "~{CHG}")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BQ24090DGQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -9.398 13.462 0)
		)
		(property "Value" "BQ24090DGQ"
			(at -3.81 11.43 0)
		)
		(property "Footprint" "Package_SO:HVSSOP-10-1EP_3x3mm_P0.5mm_EP1.57x1.88mm_ThermalVias"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/bq24090.pdf"
			(at -7.62 19.05 0)
		)
		(property "Description" "1A, Single-Input, SingleCell Li-Ion and Li-Pol BatteryCharger, HVSSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery charger singlecell li-ion li-poly"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HVSSOP*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "BQ24090DGQ_0_1")
		(symbol "BQ24090DGQ_1_1"
			(pin power_in line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin passive line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "ISET")
				(number "2")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "ISET2")
				(number "7")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PRETERM")
				(number "4")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "11")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "3")
			)
			(pin no_connect line
				(at 5.08 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin power_out line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "OUT")
				(number "10")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "TS")
				(number "9")
			)
			(pin open_collector line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "~{CHG}")
				(number "8")
			)
			(pin open_collector line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "~{PG}")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BQ24133RGY"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 19.05 0)
		)
		(property "Value" "BQ24133RGY"
			(at 7.62 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGY_R-PVQFN-N24_EP2.05x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/bq24133.pdf"
			(at 0 0 0)
		)
		(property "Description" "Synchronous switched mode Li-Ion and Li-Polymer battery charger, integrated MOSFETs and power path selector, Texas R-PVQFN-N24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Battery Charger Li-Ion Li-Poly"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGY*R*PVQFN*N*"
			(at 0 0 0)
		)
		(symbol "BQ24133RGY_0_1")
		(symbol "BQ24133RGY_1_1"
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "ACN")
				(number "5")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "ACP")
				(number "6")
			)
			(pin output line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "CMSRC")
				(number "7")
			)
			(pin output line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "ACDRV")
				(number "8")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "OVPSET")
				(number "18")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "TS")
				(number "10")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "TTC")
				(number "11")
			)
			(pin open_collector line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "STAT")
				(number "9")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 2.54)
				(name "AVCC")
				(number "4")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 2.54)
				(name "AGND")
				(number "25")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "PVCC")
				(number "2")
			)
			(pin passive line
				(at 2.54 20.32 270)
				(length 2.54)
				(hide yes)
				(name "PVCC")
				(number "3")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "PGND")
				(number "22")
			)
			(pin passive line
				(at 2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "23")
			)
			(pin passive line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "CELL")
				(number "14")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "~{BATDRV}")
				(number "19")
			)
			(pin power_out line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "SW")
				(number "1")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 2.54)
				(hide yes)
				(name "SW")
				(number "24")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "BTST")
				(number "21")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "SRP")
				(number "16")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "SRN")
				(number "15")
			)
			(pin power_out line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "VREF")
				(number "12")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "ISET")
				(number "13")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "ACSET")
				(number "17")
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "REGN")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BQ24166RGE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 24.13 0)
		)
		(property "Value" "BQ24166RGE"
			(at 2.54 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGE0024H_VQFN-24-1EP_4x4mm_P0.5mm_EP2.7x2.7mm"
			(at 3.81 -24.13 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/bq24166.pdf"
			(at 22.86 -34.29 0)
		)
		(property "Description" "High efficiency switched mode Li-Ion and Li-Polymer battery charger, integrated MOSFETs, power path selector and standard temperature sensing, Texas R-RGE0024H"
			(at 0 0 0)
		)
		(property "ki_keywords" "Battery Charger Li-Ion Li-Poly"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGE0024H*"
			(at 0 0 0)
		)
		(symbol "BQ24166RGE_0_1")
		(symbol "BQ24166RGE_1_1"
			(pin input line
				(at -10.16 20.32 0)
				(length 2.54)
				(name "IN")
				(number "21")
			)
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "VDPM")
				(number "1")
			)
			(pin passive line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "PMIDI")
				(number "20")
			)
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "USB")
				(number "22")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "PMIDU")
				(number "23")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "IUSB1")
				(number "4")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "IUSB2")
				(number "3")
			)
			(pin passive line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "IUSB3")
				(number "2")
			)
			(pin input line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "~{CE}")
				(number "24")
			)
			(pin passive line
				(at -10.16 -20.32 0)
				(length 2.54)
				(name "ILIM")
				(number "15")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "PGND")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "17")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "25")
			)
			(pin passive line
				(at 10.16 20.32 180)
				(length 2.54)
				(name "SW")
				(number "18")
			)
			(pin passive line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "BOOT")
				(number "19")
			)
			(pin power_out line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "SYS")
				(number "13")
			)
			(pin passive line
				(at 10.16 10.16 180)
				(length 2.54)
				(hide yes)
				(name "SYS")
				(number "14")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "BGATE")
				(number "10")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "BAT")
				(number "11")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "BAT")
				(number "12")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "DRV")
				(number "6")
			)
			(pin passive line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "TS")
				(number "9")
			)
			(pin open_collector line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "~{PG}")
				(number "7")
			)
			(pin open_collector line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "~{CHG}")
				(number "8")
			)
			(pin passive line
				(at 10.16 -20.32 180)
				(length 2.54)
				(name "ISET")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BQ24610"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "BQ24610"
			(at 7.62 -26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-24-1EP_4x4mm_P0.5mm_EP2.45x2.45mm"
			(at 0 -40.64 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/bq24610.pdf"
			(at 0 -38.1 0)
		)
		(property "Description" "10A, 28V max voltage, Li-Ion Charger w/600kHz NMOS-NMOS Synchronous Buck Converter, VQFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Li-ion buck"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "BQ24610_1_1"
			(pin input line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "ACN")
				(number "1")
			)
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "ACP")
				(number "2")
			)
			(pin output line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "~{ACDRV}")
				(number "3")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "CE")
				(number "4")
			)
			(pin power_out line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VREF")
				(number "10")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "ISET1")
				(number "11")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "ISET2")
				(number "15")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "ACSET")
				(number "16")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "TTC")
				(number "7")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VCC")
				(number "24")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin output line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "~{BATDRV}")
				(number "23")
			)
			(pin output line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "HIDRV")
				(number "21")
			)
			(pin power_in line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PH")
				(number "20")
			)
			(pin power_in line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "BTST")
				(number "22")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "REGN")
				(number "18")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "LODRV")
				(number "19")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "SRP")
				(number "14")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "SRN")
				(number "13")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "VFB")
				(number "12")
			)
			(pin open_collector line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "STAT1")
				(number "5")
			)
			(pin open_collector line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "STAT2")
				(number "9")
			)
			(pin open_collector line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "~{PG}")
				(number "8")
			)
			(pin input line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "TS")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BQ24650"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 21.59 0)
		)
		(property "Value" "BQ24650"
			(at 7.62 -21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RVA_VQFN-16-1EP_3.5x3.5mm_P0.5mm_EP2.14x2.14mm_ThermalVias"
			(at 0 -45.72 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/bq24650.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "10A, 28V max voltage, Battery Charger w/600kHz NMOS-NMOS Synchronous Buck Converter for Solar, VQFN-16"
			(at 0 -5.08 0)
		)
		(property "ki_keywords" "li-ion lion lipo lithium polymer iron phosphate lead acid buck solar power point battery charger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RVA*1EP*3.5x3.5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "BQ24650_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "VREF")
				(number "6")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "TERM_EN")
				(number "7")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "MPPSET")
				(number "2")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin output line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "HIDRV")
				(number "15")
			)
			(pin input line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PH")
				(number "14")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "BTST")
				(number "16")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "REGN")
				(number "12")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "LODRV")
				(number "13")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "SRP")
				(number "10")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SRN")
				(number "9")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "VFB")
				(number "8")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "TS")
				(number "4")
			)
			(pin open_collector line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "STAT1")
				(number "3")
			)
			(pin open_collector line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "STAT2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BQ2501x"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 16.51 0)
		)
		(property "Value" "BQ2501x"
			(at 6.35 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_VQFN-RHL-20_ThermalVias"
			(at 27.94 -17.78 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/bq25010.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "500mA Li-Ion Charger w/Integrated 150mA Synchronous Buck Converter, QFN-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Li-ion buck"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas?VQFN?RHL*"
			(at 0 0 0)
		)
		(symbol "BQ2501x_1_1"
			(pin power_in line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "AC")
				(number "5")
			)
			(pin power_in line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "USB")
				(number "6")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "~{CE}")
				(number "15")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "FPWM")
				(number "20")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "ISET1")
				(number "12")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "ISET2")
				(number "13")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin no_connect line
				(at 10.16 7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin power_out line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "SW")
				(number "19")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "FB")
				(number "2")
			)
			(pin power_out line
				(at 12.7 0 180)
				(length 2.54)
				(name "BAT/OUT")
				(number "16")
			)
			(pin power_in line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "BAT/OUT")
				(number "17")
			)
			(pin open_collector line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "STAT1")
				(number "7")
			)
			(pin open_collector line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "STAT2")
				(number "8")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "~{PG}")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BQ25040"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "BQ25040"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_SON:WSON-10-1EP_2x3mm_P0.5mm_EP0.84x2.4mm_ThermalVias"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/bq25040.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.1A, single cell Li-ion battery charger with 50mA LDO, up to 30V input, WSON-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "lithium"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*10*1EP*2x3mm*P0.5mm*EP0.84x2.4mm*"
			(at 0 0 0)
		)
		(symbol "BQ25040_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IFULL")
				(number "5")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN/SET")
				(number "6")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "ISET")
				(number "2")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "11")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "3")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "7")
			)
			(pin power_out line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "BAT")
				(number "10")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "LDO")
				(number "4")
			)
			(pin open_collector line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "~{PG}")
				(number "9")
			)
			(pin open_collector line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "~{CHG}")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BQ25173DSG"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "BQ25173DSG"
			(at 6.35 8.89 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm"
			(at 29.21 -8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/bq25173.pdf"
			(at 0 0 0)
		)
		(property "Description" "800-mA Linear Charger for 1- to 4-Cell Supercapacitor, input 3 to 18v, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear charger supercapacitor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "BQ25173DSG_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{CE}")
				(number "3")
			)
			(pin open_collector line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "STAT")
				(number "5")
			)
			(pin open_collector line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{PG}")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin power_out line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OUT")
				(number "8")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~{FB}")
				(number "7")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "ISET")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BQ25504"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 20.32 0)
		)
		(property "Value" "BQ25504"
			(at -7.62 22.86 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.68x1.68mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/bq25504.pdf"
			(at -7.62 20.32 0)
		)
		(property "Description" "Energy Harvesting Boost Converter with Battery Management, VQFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "energy harvesting li-ion battery solar TEG"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "BQ25504_0_1")
		(symbol "BQ25504_1_1"
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "VOC_SAMP")
				(number "3")
			)
			(pin output line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "VRDIV")
				(number "7")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "VBAT_OV")
				(number "6")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "VBAT_UV")
				(number "8")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "OK_HYST")
				(number "9")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "OK_PROG")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "VREF_SAMP")
				(number "4")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "OT_PROG")
				(number "5")
			)
			(pin power_in line
				(at -10.16 20.32 270)
				(length 2.54)
				(name "VIN_DC")
				(number "2")
			)
			(pin power_in line
				(at -5.08 -20.32 90)
				(length 2.54)
				(name "VSS")
				(number "1")
			)
			(pin passive line
				(at -5.08 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "13")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(name "PAD")
				(number "17")
			)
			(pin bidirectional line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "LBST")
				(number "16")
			)
			(pin power_in line
				(at 5.08 -20.32 90)
				(length 2.54)
				(name "AVSS")
				(number "12")
			)
			(pin power_out line
				(at 10.16 20.32 270)
				(length 2.54)
				(name "VBAT")
				(number "14")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "VBAT_OK")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "VSTOR")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BQ25570"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 16.51 0)
		)
		(property "Value" "BQ25570"
			(at 10.16 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_3.5x3.5mm_P0.5mm_EP2x2mm"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/bq25570.pdf"
			(at 10.16 30.48 0)
		)
		(property "Description" "Nano Power Boost Charger and Buck Converter for Energy Harvester Powered Applications, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "harvester solar TEG charger li-on buck"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*3.5x3.5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "BQ25570_0_1")
		(symbol "BQ25570_1_1"
			(pin passive line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "LBOOST")
				(number "20")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "VOC_SAMP")
				(number "3")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "~{EN}")
				(number "5")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "VOUT_EN")
				(number "6")
			)
			(pin passive line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "VREF_SAMP")
				(number "4")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 2.54)
				(name "VIN_DC")
				(number "2")
			)
			(pin power_out line
				(at 0 17.78 270)
				(length 2.54)
				(name "VSTOR")
				(number "19")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VSS")
				(number "1")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "15")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "17")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "21")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "9")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "VBAT")
				(number "18")
			)
			(pin passive line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "LBUCK")
				(number "16")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "VOUT")
				(number "14")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "VBAT_OK")
				(number "13")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "VRDIV")
				(number "8")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "OK_HYST")
				(number "10")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "OK_PROG")
				(number "11")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "VBAT_OV")
				(number "7")
			)
			(pin input line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "VOUT_SET")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BQ25601"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 26.67 0)
		)
		(property "Value" "BQ25601"
			(at 6.35 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RTW_WQFN-24-1EP_4x4mm_P0.5mm_EP2.7x2.7mm_ThermalVias"
			(at 0 29.21 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/bq25601.pdf"
			(at 0 35.56 0)
		)
		(property "Description" "I2C Controlled 3A Single-Cell Battery Charger for High Input Voltage and Narrow Voltage DC Power Path Management, WQFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "LiPO charger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RTW*EP2.7x2.7mm*"
			(at 0 0 0)
		)
		(symbol "BQ25601_0_1")
		(symbol "BQ25601_1_1"
			(pin input line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "VAC")
				(number "1")
			)
			(pin power_in line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "VBUS")
				(number "24")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SDA")
				(number "6")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "SCL")
				(number "5")
			)
			(pin open_collector line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{INT}")
				(number "7")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{CE}")
				(number "9")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "PSEL")
				(number "2")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "~{QON}")
				(number "12")
			)
			(pin passive line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "PMID")
				(number "23")
			)
			(pin no_connect line
				(at -10.16 15.24 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at -10.16 12.7 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin passive line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "SW")
				(number "19")
			)
			(pin passive line
				(at 12.7 22.86 180)
				(length 2.54)
				(hide yes)
				(name "SW")
				(number "20")
			)
			(pin input line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "BTST")
				(number "21")
			)
			(pin passive line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "SYS")
				(number "15")
			)
			(pin passive line
				(at 12.7 10.16 180)
				(length 2.54)
				(hide yes)
				(name "SYS")
				(number "16")
			)
			(pin open_collector line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "STAT")
				(number "4")
			)
			(pin open_collector line
				(at 12.7 0 180)
				(length 2.54)
				(name "~{PG}")
				(number "3")
			)
			(pin power_in line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "BAT")
				(number "13")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "BAT")
				(number "14")
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "REGN")
				(number "22")
			)
			(pin passive line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "TS")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BQ25886RGE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.604 21.844 0)
		)
		(property "Value" "BQ25886RGE"
			(at 3.556 21.844 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGE0024H_VQFN-24-1EP_4x4mm_P0.5mm_EP2.7x2.7mm"
			(at 0 -29.464 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/bq25886.pdf"
			(at 0 -27.432 0)
		)
		(property "Description" "Standalone 2-Cell (Li-Ion / Li-Polymer), 2A Boost-Mode Battery Charger With PowerPath, USB BC1.2 Detection, USB On-The-Go Boost (OTG), 4.3..6.2V VBUS, 8.2/8.4/8.7/8.8V charge voltage, 9.2V BATOVP, 1.5MHz, VQFN-24"
			(at 0 -25.4 0)
		)
		(property "ki_keywords" "Power-Path-Management"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*VQFN*4x4mm*P0.5mm*EP2.7x2.7*"
			(at 0 0 0)
		)
		(symbol "BQ25886RGE_0_1")
		(symbol "BQ25886RGE_1_1"
			(pin power_in line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "VBUS")
				(number "23")
			)
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "D+")
				(number "24")
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "D-")
				(number "1")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "OTG")
				(number "5")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{CE}")
				(number "3")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "ILIM")
				(number "8")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "VSET")
				(number "6")
			)
			(pin passive line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "ICHGSET")
				(number "10")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "19")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "20")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin open_collector line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "STAT")
				(number "2")
			)
			(pin open_collector line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "~{PG}")
				(number "9")
			)
			(pin power_out line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "PMID")
				(number "21")
			)
			(pin passive line
				(at 10.16 10.16 180)
				(length 2.54)
				(hide yes)
				(name "PMID")
				(number "22")
			)
			(pin power_in line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SW")
				(number "17")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "SW")
				(number "18")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "BTST")
				(number "12")
			)
			(pin power_out line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "SYS")
				(number "15")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "SYS")
				(number "16")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "BAT")
				(number "13")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "BAT")
				(number "14")
			)
			(pin power_out line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "REGN")
				(number "11")
			)
			(pin input line
				(at 10.16 -17.78 180)
				(length 2.54)
				(name "TS")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BQ25887"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.985 16.51 0)
		)
		(property "Value" "BQ25887"
			(at -3.175 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-24-1EP_4x4mm_P0.5mm_EP2.5x2.5mm"
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/bq25887.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "I2C Controller 2-Cell 2A Boost mode LiIon Charger with cell balancing"
			(at 0 0 0)
		)
		(property "ki_keywords" "LiIon Charger Boost"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*4x4mm*"
			(at 0 0 0)
		)
		(symbol "BQ25887_1_1"
			(pin power_in line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "VBUS")
				(number "23")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "SDA")
				(number "4")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SCL")
				(number "5")
			)
			(pin open_collector line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{INT}")
				(number "6")
			)
			(pin open_collector line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{PG}")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "CD")
				(number "3")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "PSEL")
				(number "24")
			)
			(pin open_collector line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "STAT")
				(number "2")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "ILIM")
				(number "8")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "19")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "20")
			)
			(pin power_out line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "PMID")
				(number "21")
			)
			(pin passive line
				(at 10.16 12.7 180)
				(length 2.54)
				(hide yes)
				(name "PMID")
				(number "22")
			)
			(pin power_out line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "SW")
				(number "17")
			)
			(pin passive line
				(at 10.16 10.16 180)
				(length 2.54)
				(hide yes)
				(name "SW")
				(number "18")
			)
			(pin power_out line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "BTST")
				(number "12")
			)
			(pin power_out line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "BAT")
				(number "13")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "BAT")
				(number "14")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "MID")
				(number "9")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "CBSET")
				(number "10")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "SNS")
				(number "15")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "SNS")
				(number "16")
			)
			(pin power_out line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "REGN")
				(number "11")
			)
			(pin input line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "TS")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BQ25895RTW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 22.86 0)
		)
		(property "Value" "BQ25895RTW"
			(at 5.08 22.86 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RTW_WQFN-24-1EP_4x4mm_P0.5mm_EP2.7x2.7mm_ThermalVias"
			(at -2.54 25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/bq25895.pdf"
			(at -5.08 20.32 0)
		)
		(property "Description" "Controlled Single Cell 5A Fast Charger with MaxCharge, WQFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Battery Charger and Power Path Management"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RTW*EP2.7x2.7mm*"
			(at 0 0 0)
		)
		(symbol "BQ25895RTW_0_1")
		(symbol "BQ25895RTW_1_1"
			(pin power_in line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "VBUS")
				(number "1")
			)
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "D+")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "D-")
				(number "3")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "ILIM")
				(number "10")
			)
			(pin open_collector line
				(at -10.16 0 0)
				(length 2.54)
				(name "STAT")
				(number "4")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SDA")
				(number "6")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "SCL")
				(number "5")
			)
			(pin open_collector line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "INT")
				(number "7")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "OTG")
				(number "8")
			)
			(pin input line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "~{CE}")
				(number "9")
			)
			(pin input line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "~{QON}")
				(number "12")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "PGND")
				(number "17")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "18")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "25")
			)
			(pin power_out line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "PMID")
				(number "23")
			)
			(pin power_out line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "SW")
				(number "19")
			)
			(pin passive line
				(at 10.16 12.7 180)
				(length 2.54)
				(hide yes)
				(name "SW")
				(number "20")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "BTST")
				(number "21")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SYS")
				(number "15")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "SYS")
				(number "16")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "BAT")
				(number "13")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "BAT")
				(number "14")
			)
			(pin open_collector line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "DSEL")
				(number "24")
			)
			(pin passive line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "REGN")
				(number "22")
			)
			(pin passive line
				(at 10.16 -17.78 180)
				(length 2.54)
				(name "TS")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BQ27441-G1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 15.875 0)
		)
		(property "Value" "BQ27441-G1"
			(at -5.08 13.97 0)
		)
		(property "Footprint" "Package_SON:Texas_S-PDSO-N12"
			(at 6.35 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/bq27441-g1.pdf"
			(at 5.08 5.08 0)
		)
		(property "Description" "System Side Li Ion/Polymer Fuel Gauge, PDSON-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "Fuel Gauge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PDSO*N12*"
			(at 0 0 0)
		)
		(symbol "BQ27441-G1_0_1")
		(symbol "BQ27441-G1_1_1"
			(pin power_in line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "BAT")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "SDA")
				(number "1")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "SCL")
				(number "2")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "SRN")
				(number "7")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "SRP")
				(number "8")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "BIN")
				(number "10")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "PAD")
				(number "13")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "V_{SS}")
				(number "3")
			)
			(pin no_connect line
				(at 10.16 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin no_connect line
				(at 10.16 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at 10.16 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_out line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "V_{DD}")
				(number "5")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "GPOUT")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BQ27750"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 13.335 0)
		)
		(property "Value" "BQ27750"
			(at -5.08 11.43 0)
		)
		(property "Footprint" "Package_SON:Texas_S-PDSO-N12"
			(at 2.54 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/bq27750.pdf"
			(at 5.08 2.54 0)
		)
		(property "Description" "System Side Li Ion/Polymer Fuel Gauge, VSON-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "Fuel Gauge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*PDSO*N12*"
			(at 0 0 0)
		)
		(symbol "BQ27750_0_1")
		(symbol "BQ27750_1_1"
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "SDA")
				(number "6")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SCL")
				(number "5")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "SRN")
				(number "2")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SRP")
				(number "3")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PBI")
				(number "10")
			)
			(pin input line
				(at 0 12.7 270)
				(length 2.54)
				(name "PACK")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "1")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "13")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "DSG")
				(number "7")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "CHG")
				(number "9")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "BAT")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "VCELL/INT")
				(number "12")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "TS1")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BQ297xy"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "BQ297xy"
			(at 5.08 -6.35 0)
		)
		(property "Footprint" "Package_SON:WSON-6_1.5x1.5mm_P0.5mm"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/bq2970.pdf"
			(at -6.35 5.08 0)
		)
		(property "Description" "Voltage and Current Protection for Single-Cell Li-Ion and Li-Polymer Batteries"
			(at 0 0 0)
		)
		(property "ki_keywords" "protection Li-Ion Li-Pol"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1.5x1.5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "BQ297xy_0_1")
		(symbol "BQ297xy_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "BAT")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "V-")
				(number "6")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "Cout")
				(number "2")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "Dout")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BQ51050BRHL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 21.59 0)
		)
		(property "Value" "BQ51050BRHL"
			(at 7.62 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_VQFN-RHL-20"
			(at 20.32 -21.59 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/bq51050b.pdf"
			(at 0 0 0)
		)
		(property "Description" "Qi v1.2, Wireless Power Receiver and Battery Charger, Vout 4.2V, VQFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Qi Wireless Power Receiver Battery Charger 4.2V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas?VQFN?RHL*"
			(at 0 0 0)
		)
		(symbol "BQ51050BRHL_0_1")
		(symbol "BQ51050BRHL_1_1"
			(pin output line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "~{AD-EN}")
				(number "8")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "AD")
				(number "9")
			)
			(pin open_collector line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "CLAMP1")
				(number "5")
			)
			(pin open_collector line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "COMM1")
				(number "6")
			)
			(pin passive line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "BOOT1")
				(number "3")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "AC1")
				(number "2")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "AC2")
				(number "19")
			)
			(pin passive line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "BOOT2")
				(number "17")
			)
			(pin open_collector line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "COMM2")
				(number "15")
			)
			(pin open_collector line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "CLAMP2")
				(number "16")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "PGND")
				(number "1")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "20")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "21")
			)
			(pin power_out line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "BAT")
				(number "4")
			)
			(pin open_collector line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "~{CHG}")
				(number "7")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "TS/CTRL")
				(number "13")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "EN2")
				(number "11")
			)
			(pin passive line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "ILIM")
				(number "12")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "FOD")
				(number "14")
			)
			(pin passive line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "RECT")
				(number "18")
			)
			(pin input line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "TERM")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BQ51050BYFP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 21.59 0)
		)
		(property "Value" "BQ51050BYFP"
			(at 7.62 21.59 0)
		)
		(property "Footprint" "Package_BGA:Texas_DSBGA-28_1.9x3mm_Layout4x7_P0.4mm"
			(at 30.48 -21.59 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/bq51050b.pdf"
			(at 0 0 0)
		)
		(property "Description" "Qi v1.2, Wireless Power Receiver and Battery Charger, Vout 4.2V, DSBGA-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Qi Wireless Power Receiver Battery Charger 4.2V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DSBGA*1.9x3mm*Layout4x7*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "BQ51050BYFP_0_1")
		(symbol "BQ51050BYFP_1_1"
			(pin output line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "~{AD-EN}")
				(number "F3")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "AD")
				(number "G4")
			)
			(pin open_collector line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "CLAMP1")
				(number "E3")
			)
			(pin open_collector line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "COMM1")
				(number "E4")
			)
			(pin passive line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "BOOT1")
				(number "C4")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "AC1")
				(number "B3")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(hide yes)
				(name "AC1")
				(number "B4")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "AC2")
				(number "B1")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "AC2")
				(number "B2")
			)
			(pin passive line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "BOOT2")
				(number "C1")
			)
			(pin open_collector line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "COMM2")
				(number "E1")
			)
			(pin open_collector line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "CLAMP2")
				(number "E2")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "PGND")
				(number "A1")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "A2")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "A3")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "A4")
			)
			(pin power_out line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "BAT")
				(number "D1")
			)
			(pin passive line
				(at 12.7 17.78 180)
				(length 2.54)
				(hide yes)
				(name "BAT")
				(number "D2")
			)
			(pin passive line
				(at 12.7 17.78 180)
				(length 2.54)
				(hide yes)
				(name "BAT")
				(number "D3")
			)
			(pin passive line
				(at 12.7 17.78 180)
				(length 2.54)
				(hide yes)
				(name "BAT")
				(number "D4")
			)
			(pin open_collector line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "~{CHG}")
				(number "F4")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "TS/CTRL")
				(number "F1")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "EN2")
				(number "G2")
			)
			(pin passive line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "ILIM")
				(number "G1")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "FOD")
				(number "F2")
			)
			(pin passive line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "RECT")
				(number "C2")
			)
			(pin passive line
				(at 12.7 -12.7 180)
				(length 2.54)
				(hide yes)
				(name "RECT")
				(number "C3")
			)
			(pin input line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "TERM")
				(number "G3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BQ76200PW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 13.97 0)
		)
		(property "Value" "BQ76200PW"
			(at 7.62 13.97 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 21.59 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/bq76200.pdf"
			(at 0 0 0)
		)
		(property "Description" "High Voltage Battery Pack Front-End Charge/Discharge High-Side NFET Driver, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Battery Pack Charge/Discharge High-Side"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "BQ76200PW_0_1")
		(symbol "BQ76200PW_1_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "CHG_EN")
				(number "4")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "CP_EN")
				(number "5")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "DSG_EN")
				(number "6")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PCHG_EN")
				(number "8")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PMON_EN")
				(number "7")
			)
			(pin no_connect line
				(at -10.16 10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at -10.16 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "BAT")
				(number "2")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "PACK")
				(number "11")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "VSS")
				(number "9")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "VDDCP")
				(number "1")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PCHG")
				(number "14")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CHG")
				(number "16")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "DSG")
				(number "12")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PACKDIV")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BQ76920PW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 19.05 0)
		)
		(property "Value" "BQ76920PW"
			(at 12.7 19.05 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 22.86 -19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/bq76920.pdf"
			(at 17.78 13.97 0)
		)
		(property "Description" "Lithium battery monitor, 3-5 cells, integrated balancing, I2C interface, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "lithium battery balance charge afe"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "BQ76920PW_0_1")
		(symbol "BQ76920PW_1_0"
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "ALERT")
				(number "20")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "TS1")
				(number "6")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "CAP1")
				(number "7")
			)
			(pin no_connect line
				(at -2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "REGSRC")
				(number "9")
			)
			(pin power_out line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "REGOUT")
				(number "8")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "BAT")
				(number "10")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "VC5")
				(number "12")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "VC4")
				(number "13")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "VC3")
				(number "14")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "VC2")
				(number "15")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "VC1")
				(number "16")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "VC0")
				(number "17")
			)
			(pin input line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "SRP")
				(number "18")
			)
			(pin input line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "SRN")
				(number "19")
			)
		)
		(symbol "BQ76920PW_1_1"
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "SDA")
				(number "4")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "SCL")
				(number "5")
			)
			(pin output line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "DSG")
				(number "1")
			)
			(pin output line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "CHG")
				(number "2")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "VSS")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BQ76930DBT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 26.67 0)
		)
		(property "Value" "BQ76930DBT"
			(at 13.97 26.67 0)
		)
		(property "Footprint" "Package_SO:TSSOP-30_4.4x7.8mm_P0.5mm"
			(at 22.86 -26.67 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/bq76930.pdf"
			(at 17.78 21.59 0)
		)
		(property "Description" "Lithium battery monitor, 6-10 cells, integrated balancing, I2C interface, TSSOP-30"
			(at 0 0 0)
		)
		(property "ki_keywords" "lithium battery balance charge afe"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x7.8mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "BQ76930DBT_0_1")
		(symbol "BQ76930DBT_1_0"
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "ALERT")
				(number "30")
			)
			(pin passive line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "TS2")
				(number "13")
			)
			(pin passive line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VC5X")
				(number "10")
			)
			(pin passive line
				(at -12.7 0 0)
				(length 2.54)
				(name "CAP2")
				(number "14")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "NC(CAP2)")
				(number "11")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "NC(CAP2)")
				(number "12")
			)
			(pin passive line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "TS1")
				(number "6")
			)
			(pin passive line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "CAP1")
				(number "7")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "REGSRC")
				(number "9")
			)
			(pin power_out line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "REGOUT")
				(number "8")
			)
			(pin input line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "BAT")
				(number "15")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "VC10")
				(number "16")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "VC9")
				(number "17")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "VC8")
				(number "18")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "VC7")
				(number "19")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "VC6")
				(number "20")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "VC5B")
				(number "21")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "VC5")
				(number "22")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "VC4")
				(number "23")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "VC3")
				(number "24")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "VC2")
				(number "25")
			)
			(pin input line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "VC1")
				(number "26")
			)
			(pin input line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "VC0")
				(number "27")
			)
			(pin input line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "SRP")
				(number "28")
			)
			(pin input line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "SRN")
				(number "29")
			)
		)
		(symbol "BQ76930DBT_1_1"
			(pin bidirectional line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "SDA")
				(number "4")
			)
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "SCL")
				(number "5")
			)
			(pin output line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "DSG")
				(number "1")
			)
			(pin output line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "CHG")
				(number "2")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "VSS")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BQ76940DBT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 34.29 0)
		)
		(property "Value" "BQ76940DBT"
			(at 12.7 34.29 0)
		)
		(property "Footprint" "Package_SO:TSSOP-44_4.4x11.2mm_P0.5mm"
			(at 22.86 -34.29 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/bq76940.pdf"
			(at 17.78 29.21 0)
		)
		(property "Description" "Lithium battery monitor, 9-15 cells, integrated balancing, I2C interface, TSSOP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "lithium battery balance charge afe"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x11.2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "BQ76940DBT_0_1")
		(symbol "BQ76940DBT_1_0"
			(pin bidirectional line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "ALERT")
				(number "44")
			)
			(pin passive line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "TS3")
				(number "18")
			)
			(pin passive line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "VC10X")
				(number "15")
			)
			(pin passive line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "CAP3")
				(number "19")
			)
			(pin passive line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "NC(CAP3)")
				(number "16")
			)
			(pin passive line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "NC(CAP3)")
				(number "17")
			)
			(pin passive line
				(at -12.7 0 0)
				(length 2.54)
				(name "TS2")
				(number "13")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "VC5X")
				(number "10")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "CAP2")
				(number "14")
			)
			(pin passive line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "NC(CAP2)")
				(number "11")
			)
			(pin passive line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "NC(CAP2)")
				(number "12")
			)
			(pin passive line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "TS1")
				(number "6")
			)
			(pin passive line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "CAP1")
				(number "7")
			)
			(pin no_connect line
				(at -5.08 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "21")
			)
			(pin no_connect line
				(at -2.54 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "22")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "REGSRC")
				(number "9")
			)
			(pin no_connect line
				(at 2.54 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "23")
			)
			(pin power_out line
				(at 12.7 30.48 180)
				(length 2.54)
				(name "REGOUT")
				(number "8")
			)
			(pin input line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "BAT")
				(number "20")
			)
			(pin input line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "VC15")
				(number "24")
			)
			(pin input line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "VC14")
				(number "25")
			)
			(pin input line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "VC13")
				(number "26")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "VC12")
				(number "27")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "VC11")
				(number "28")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "VC10B")
				(number "29")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "VC10")
				(number "30")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "VC9")
				(number "31")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "VC8")
				(number "32")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "VC7")
				(number "33")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "VC6")
				(number "34")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "VC5B")
				(number "35")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "VC5")
				(number "36")
			)
			(pin input line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "VC4")
				(number "37")
			)
			(pin input line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "VC3")
				(number "38")
			)
			(pin input line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "VC2")
				(number "39")
			)
			(pin input line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "VC1")
				(number "40")
			)
			(pin input line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "VC0")
				(number "41")
			)
			(pin input line
				(at 12.7 -27.94 180)
				(length 2.54)
				(name "SRP")
				(number "42")
			)
			(pin input line
				(at 12.7 -30.48 180)
				(length 2.54)
				(name "SRN")
				(number "43")
			)
		)
		(symbol "BQ76940DBT_1_1"
			(pin bidirectional line
				(at -12.7 30.48 0)
				(length 2.54)
				(name "SDA")
				(number "4")
			)
			(pin input line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "SCL")
				(number "5")
			)
			(pin output line
				(at -12.7 -27.94 0)
				(length 2.54)
				(name "DSG")
				(number "1")
			)
			(pin output line
				(at -12.7 -30.48 0)
				(length 2.54)
				(name "CHG")
				(number "2")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "VSS")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BQ78350DBT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "BQ78350DBT"
			(at 13.97 26.67 0)
		)
		(property "Footprint" "Package_SO:TSSOP-30_4.4x7.8mm_P0.5mm"
			(at 21.59 -26.67 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/bq78350.pdf"
			(at -17.78 29.21 0)
		)
		(property "Description" "Lithium battery fuel gauge, battery management controller for BQ769x0, TSSOP-30"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery management Li-Ion Gauge controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x7.8mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "BQ78350DBT_0_1")
		(symbol "BQ78350DBT_1_1"
			(pin input line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "~{MRST}")
				(number "24")
			)
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "BAT")
				(number "7")
			)
			(pin open_collector line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "VEN")
				(number "12")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "VAUX")
				(number "6")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SDA")
				(number "3")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SCL")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "ALERT")
				(number "2")
			)
			(pin output line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{PRECHG}")
				(number "5")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "~{PRES}")
				(number "8")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "~{KEYIN}")
				(number "9")
			)
			(pin output line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "SAFE")
				(number "10")
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "GPIO_A")
				(number "21")
			)
			(pin bidirectional line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "GPIO_B")
				(number "28")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VCC")
				(number "26")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "22")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "25")
			)
			(pin output line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "LED1")
				(number "16")
			)
			(pin output line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "LED2")
				(number "17")
			)
			(pin output line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "LED3")
				(number "18")
			)
			(pin output line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "LED4")
				(number "19")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "LED5")
				(number "20")
			)
			(pin open_collector line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "COM")
				(number "1")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "~{DISP}")
				(number "14")
			)
			(pin open_collector line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PWRM")
				(number "15")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "SMBD")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SMBC")
				(number "13")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "ADREN")
				(number "29")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "SMBA")
				(number "30")
			)
			(pin passive line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "RBI")
				(number "27")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DS2745U"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.096 6.604 0)
		)
		(property "Value" "DS2745U"
			(at 1.27 6.604 0)
		)
		(property "Footprint" "Package_SO:TSSOP-8_3x3mm_P0.65mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DS2745.pdf"
			(at 2.54 -10.16 0)
		)
		(property "Description" "Current-flow, voltage and temperature measurement to support battery capacity monitoring, 2.5V to 4.5V VDD, -40 to +85 degree Celsius, TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery capacity monitor I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "DS2745U_0_1")
		(symbol "DS2745U_1_1"
			(pin open_collector line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "PIO")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SCL")
				(number "1")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SDA")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V_{DD}")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "V_{SS}")
				(number "5")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VIN")
				(number "7")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SNS")
				(number "4")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "CTG")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DW01A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.604 6.35 0)
		)
		(property "Value" "DW01A"
			(at 4.318 6.604 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
		)
		(property "Datasheet" "https://hmsemi.com/downfile/DW01A.PDF"
			(at 0 0 0)
		)
		(property "Description" "Overcharge, overcurrent and overdischarge protection IC for single cell lithium-ion/polymer battery"
			(at 0.254 1.524 0)
		)
		(property "ki_keywords" "battery protection li-ion lipo overcurrent overdischarge overcharge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "DW01A_0_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin output line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "OD")
				(number "1")
			)
			(pin output line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "OC")
				(number "3")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "CS")
				(number "2")
			)
		)
		(symbol "DW01A_1_1"
			(pin no_connect line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "TD")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LC709203FQH-01TWG"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "LC709203FQH-01TWG"
			(at 11.43 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:WDFN-8-1EP_4x3mm_P0.65mm_EP2.4x1.8mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.onsemi.com/download/data-sheet/pdf/lc709203f-d.pdf"
			(at -1.27 -2.54 0)
		)
		(property "Description" "Single LiPo battery fuel gauge, I2C, type 01, WDFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Battery gauge I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WDFN*1EP*4x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LC709203FQH-01TWG_0_1")
		(symbol "LC709203FQH-01TWG_1_1"
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SDA")
				(number "7")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "SCL")
				(number "8")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "TEST")
				(number "1")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V_{DD}")
				(number "3")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "V_{SS}")
				(number "2")
			)
			(pin passive line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "EP")
				(number "9")
			)
			(pin open_collector line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~{ALARMB}")
				(number "4")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "T_{SW}")
				(number "5")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "T_{SENSE}")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LGS5500EP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.684 11.176 0)
		)
		(property "Value" "LGS5500EP"
			(at 8.382 11.176 0)
		)
		(property "Footprint" "Package_SO:SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.41x3.3mm"
			(at -0.254 -29.972 0)
		)
		(property "Datasheet" "https://www.lcsc.com/datasheet/lcsc_datasheet_2304071430_Legend-Si-LGS5500EP_C5280699.pdf"
			(at 0.254 -25.654 0)
		)
		(property "Description" "LiPo charger and 5V boost converter, 4.5-5.5V input, 4.2-4.4V battery, 400-1000mA charge current, 800mA boost output, SOIC-8-1EP"
			(at 0 -27.94 0)
		)
		(property "ki_keywords" "lipo lithium battery charger boost"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*1EP*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LGS5500EP_1_1"
			(pin power_in line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "NTC")
				(number "8")
			)
			(pin passive line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "ISET")
				(number "1")
			)
			(pin no_connect line
				(at -12.7 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin power_out line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "VH")
				(number "5")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "LX")
				(number "4")
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "VL")
				(number "3")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "VSET/LED")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LP3947"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 17.78 0)
		)
		(property "Value" "LP3947"
			(at -12.7 15.24 0)
		)
		(property "Footprint" "Package_SON:WSON-14-1EP_4.0x4.0mm_P0.5mm_EP2.6x2.6mm"
			(at 30.48 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp3947.pdf"
			(at -2.54 5.08 0)
		)
		(property "Description" "Single Cell Li-Ion LDO Battery Charger IC, Up to 1A, Support USB charging scheme"
			(at 0 0 0)
		)
		(property "ki_keywords" "li-ion battery charger usb"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*4.0x4.0mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LP3947_0_1")
		(symbol "LP3947_1_1"
			(pin input line
				(at -15.24 12.7 0)
				(length 3.81)
				(name "EN")
				(number "1")
			)
			(pin open_collector output_low
				(at -15.24 7.62 0)
				(length 3.81)
				(name "EOC")
				(number "10")
			)
			(pin open_collector output_low
				(at -15.24 5.08 0)
				(length 3.81)
				(name "CHG")
				(number "12")
			)
			(pin input line
				(at -15.24 0 0)
				(length 3.81)
				(name "MODE")
				(number "7")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "ISEL")
				(number "13")
			)
			(pin input clock
				(at -15.24 -7.62 0)
				(length 3.81)
				(name "SCL")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 3.81)
				(name "SDA")
				(number "3")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 3.81)
				(name "CHG_IN")
				(number "14")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 3.81)
				(name "GND")
				(number "11")
			)
			(pin power_out line
				(at 2.54 17.78 270)
				(length 3.81)
				(name "BATT")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 3.81)
				(name "EP")
				(number "15")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 3.81)
				(name "VB_{SENSE}")
				(number "6")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "Ts")
				(number "9")
			)
			(pin power_out line
				(at 15.24 2.54 180)
				(length 3.81)
				(name "V_{T}")
				(number "5")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 3.81)
				(name "DIFF_AMP")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT3652EDD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.382 11.43 0)
		)
		(property "Value" "LT3652EDD"
			(at 1.778 11.684 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-12-1EP_3x3mm_P0.45mm_EP1.65x2.38mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3652fe.pdf"
			(at 15.24 -20.32 0)
		)
		(property "Description" "Step-down battery charger for solar power, Lithium Phosphate (LiFePO4), Lead (Pb), Lithium+ (Li+) , 4.95V to 32V VDD, 2A, -40 to +125 degree Celsius, DFN-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery charger solar"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P0.45mm*"
			(at 0 0 0)
		)
		(symbol "LT3652EDD_0_1")
		(symbol "LT3652EDD_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "3")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "V_{IN_REG}")
				(number "2")
			)
			(pin open_collector line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{CHRG}")
				(number "4")
			)
			(pin open_collector line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{FAULT}")
				(number "5")
			)
			(pin output line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "TIMER")
				(number "6")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V_{IN}")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "SW")
				(number "12")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "BOOST")
				(number "11")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "SENSE")
				(number "10")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "BAT")
				(number "9")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "NTC")
				(number "8")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "V_{FB}")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT3652EMSE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.382 11.43 0)
		)
		(property "Value" "LT3652EMSE"
			(at 1.778 11.684 0)
		)
		(property "Footprint" "Package_SO:MSOP-12-1EP_3x4.039mm_P0.65mm_EP1.651x2.845mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3652fe.pdf"
			(at 15.24 -20.32 0)
		)
		(property "Description" "Step-down battery charger for solar power, Lithium Phosphate (LiFePO4), Lead (Pb), Lithium+ (Li+) , 4.95V to 32V VDD, 2A, -40 to +125 degree Celsius, MSOP-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery charger solar"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*1EP*3x4.039mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LT3652EMSE_0_1")
		(symbol "LT3652EMSE_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "3")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "V_{IN_REG}")
				(number "2")
			)
			(pin open_collector line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{CHRG}")
				(number "4")
			)
			(pin open_collector line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{FAULT}")
				(number "5")
			)
			(pin output line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "TIMER")
				(number "6")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V_{IN}")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "SW")
				(number "12")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "BOOST")
				(number "11")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "SENSE")
				(number "10")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "BAT")
				(number "9")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "NTC")
				(number "8")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "V_{FB}")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC2942"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LTC2942"
			(at 10.16 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6-1EP_3x2mm_P0.5mm_EP1.65x1.35mm"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/2942fa.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Battery Gas Gauge with Temperature, Voltage Measurement, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Fuel gauge coulomb counter I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC2942_0_1")
		(symbol "LTC2942_1_1"
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "~{AL}/CC")
				(number "5")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "SCL")
				(number "3")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SDA")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "SENSE+")
				(number "1")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SENSE-")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC2959"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.414 11.938 0)
		)
		(property "Value" "LTC2959"
			(at 10.16 11.938 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-10-1EP_2x3mm_P0.5mm_EP0.64x2.4mm"
			(at 0 15.24 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ltc2959.pdf"
			(at 0 -17.78 0)
		)
		(property "Description" "Ultra-Low Power Battery Gas Gauge with Temperature, Voltage Measurement, DFN-10"
			(at 0 -15.24 0)
		)
		(property "ki_keywords" "Ultra-low power fuel gauge coulomb counter I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*2x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC2959_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SDA")
				(number "7")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "GPIO")
				(number "8")
			)
			(pin no_connect line
				(at -10.16 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "EP")
				(number "11")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V_{DD}")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "SENSEP")
				(number "2")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "CFP")
				(number "3")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 2.54)
				(name "CFN")
				(number "4")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SENSEN")
				(number "5")
			)
			(pin power_out line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "V_{REG}")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC3553"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 15.24 -21.59 0)
		)
		(property "Value" "LTC3553"
			(at 15.24 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_3x3mm_P0.4mm_EP1.65x1.65mm"
			(at 0 -1.27 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3553fc.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Micropower USB Power Manager With Li-Ion Charger, LDO and Buck Regulator, 4.2V float, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB PMIC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*3x3mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "LTC3553_0_1")
		(symbol "LTC3553_1_1"
			(pin input line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "HPWR")
				(number "1")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "SUSP")
				(number "19")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "LDO_ON")
				(number "5")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "BUCK_ON")
				(number "7")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "STBY")
				(number "6")
			)
			(pin open_collector line
				(at -17.78 0 0)
				(length 2.54)
				(name "~{CHRG}")
				(number "14")
			)
			(pin output line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PBSTAT")
				(number "3")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "~{ON}")
				(number "4")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "SEQ")
				(number "2")
			)
			(pin passive line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PROG")
				(number "16")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VBUS")
				(number "20")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "21")
			)
			(pin power_out line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "VOUT")
				(number "18")
			)
			(pin power_out line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "BAT")
				(number "17")
			)
			(pin passive line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "NTC")
				(number "15")
			)
			(pin power_in line
				(at 17.78 0 180)
				(length 2.54)
				(name "VINLDO")
				(number "11")
			)
			(pin power_out line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "LDO")
				(number "10")
			)
			(pin input line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "LDO_FB")
				(number "9")
			)
			(pin power_in line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "BVIN")
				(number "12")
			)
			(pin power_out line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "SW")
				(number "13")
			)
			(pin input line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "BUCK_FB")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC3555"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 15.24 -29.21 0)
		)
		(property "Value" "LTC3555"
			(at 15.24 29.21 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_4x5mm_P0.5mm_EP2.65x3.65mm"
			(at 0 -1.27 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3555fe.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "High Efficiency USB Power Manager + Triple Step-Down DC/DC, 4.2V float, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB PMIC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC3555_0_1")
		(symbol "LTC3555_1_1"
			(pin power_in line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "DV_{CC}")
				(number "8")
			)
			(pin input line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "SCL")
				(number "9")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "SDA")
				(number "10")
			)
			(pin open_collector line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "~{CHRG}")
				(number "21")
			)
			(pin open_collector line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "~{RST3}")
				(number "15")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "EN1")
				(number "16")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "EN2")
				(number "7")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "EN3")
				(number "13")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "I_{LIM0}")
				(number "27")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "I_{LIM1}")
				(number "28")
			)
			(pin passive line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "CLPROG")
				(number "2")
			)
			(pin passive line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PROG")
				(number "20")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 2.54)
				(name "VBUS")
				(number "25")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 2.54)
				(name "GND")
				(number "29")
			)
			(pin power_out line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "LDO3V3")
				(number "1")
			)
			(pin power_out line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "V_{OUT}")
				(number "24")
			)
			(pin power_out line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "SW")
				(number "26")
			)
			(pin power_out line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "BAT")
				(number "23")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "GATE")
				(number "22")
			)
			(pin passive line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "NTC")
				(number "3")
			)
			(pin power_in line
				(at 17.78 0 180)
				(length 2.54)
				(name "V_{IN1}")
				(number "18")
			)
			(pin power_out line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "SW1")
				(number "17")
			)
			(pin input line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "FB1")
				(number "19")
			)
			(pin power_in line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "V_{IN2}")
				(number "5")
			)
			(pin power_out line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "SW2")
				(number "6")
			)
			(pin input line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "FB2")
				(number "4")
			)
			(pin power_in line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "V_{IN3}")
				(number "11")
			)
			(pin power_out line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "SW3")
				(number "12")
			)
			(pin input line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "FB3")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC4001"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 16.51 0)
		)
		(property "Value" "LTC4001"
			(at 6.35 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_4x4mm_P0.65mm_EP2.15x2.15mm"
			(at 1.27 -19.05 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/4001f.pdf"
			(at -8.89 16.51 0)
		)
		(property "Description" "Single cell (4.2V) programmable synchronous buck Li-Ion charger, 2A, 5.5V input, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Li-Ion charger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LTC4001_0_1")
		(symbol "LTC4001_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "~{EN}")
				(number "6")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "NTC")
				(number "11")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "TIMER")
				(number "15")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "IDET")
				(number "13")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PROG")
				(number "12")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "SS")
				(number "14")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 2.54)
				(name "P_{VIN}")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 2.54)
				(name "PGND")
				(number "3")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "V_{INSENSE}")
				(number "9")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GNDSENS")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "PAD")
				(number "17")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "SW")
				(number "5")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "SENSE")
				(number "2")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "BATSENS")
				(number "16")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "BAT")
				(number "1")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "FAULT")
				(number "10")
			)
			(pin open_collector line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "~{CHRG}")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC4002EDD-4.2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "LTC4002EDD-4.2"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-10-1EP_3x3mm_P0.5mm_EP1.55x2.48mm"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/4002f.pdf"
			(at -10.16 8.89 0)
		)
		(property "Description" "Standalone Li-Ion Switch Mode Battery Charger, 4.7-22V input, single cell, DFN-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "lithium li-ion battery charger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*10*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC4002EDD-4.2_0_1")
		(symbol "LTC4002EDD-4.2_1_1"
			(pin open_collector line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "~{CHRG}")
				(number "6")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "COMP")
				(number "1")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "NTC")
				(number "9")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "PGND")
				(number "4")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V_{CC}")
				(number "2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "SGND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin no_connect line
				(at 5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "GATE")
				(number "3")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "SENSE")
				(number "8")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "BAT")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC4002ES8-4.2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "LTC4002ES8-4.2"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/4002f.pdf"
			(at -10.16 8.89 0)
		)
		(property "Description" "Standalone Li-Ion Switch Mode Battery Charger, 4.7-22V input, single cell, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "lithium li-ion battery charger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*8*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LTC4002ES8-4.2_0_1")
		(symbol "LTC4002ES8-4.2_1_1"
			(pin open_collector line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "~{CHRG}")
				(number "5")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "COMP")
				(number "1")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "NTC")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V_{CC}")
				(number "2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "GATE")
				(number "3")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "SENSE")
				(number "7")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "BAT")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC4007"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 24.13 0)
		)
		(property "Value" "LTC4007"
			(at 10.16 24.13 0)
		)
		(property "Footprint" "Package_SO:SSOP-24_3.9x8.7mm_P0.635mm"
			(at 0 -25.4 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/4007fc.pdf"
			(at 0 0 0)
		)
		(property "Description" "4A high efficiency standalone Li-ion battery charger, SSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "lithium ion polymer li-po battery"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*3.9x8.7mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "LTC4007_0_1")
		(symbol "LTC4007_1_1"
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "DCIN")
				(number "1")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "3C4C")
				(number "7")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "CHEM")
				(number "16")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "SHDN")
				(number "24")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "NTC")
				(number "9")
			)
			(pin output line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{LOBAT}")
				(number "8")
			)
			(pin output line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{ICL}")
				(number "13")
			)
			(pin open_collector line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "ACP")
				(number "3")
			)
			(pin open_collector line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "~{FAULT}")
				(number "5")
			)
			(pin output line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "~{CHG}")
				(number "2")
			)
			(pin open_collector line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "~{FLAG}")
				(number "17")
			)
			(pin passive line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "R_{T}")
				(number "4")
			)
			(pin no_connect line
				(at -2.54 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 2.54 -22.86 90)
				(length 2.54)
				(name "PGND")
				(number "21")
			)
			(pin output line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "INFET")
				(number "23")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "CLP")
				(number "18")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "CLN")
				(number "19")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "TGATE")
				(number "20")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "BGATE")
				(number "22")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "CSP")
				(number "14")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "BAT")
				(number "15")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PROG")
				(number "11")
			)
			(pin passive line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "ITH")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC4011CFE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 21.59 0)
		)
		(property "Value" "LTC4011CFE"
			(at 12.7 -21.59 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP2.74x3.86mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/4011fb.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "High efficiency standalone NiMH battery charger, HTSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "NiMH nickel battery charger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*1EP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LTC4011CFE_0_1")
		(symbol "LTC4011CFE_1_1"
			(pin output line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "INFET")
				(number "20")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "DCIN")
				(number "1")
			)
			(pin open_collector line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "~{FAULT}")
				(number "2")
			)
			(pin open_collector line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "~{CHRG}")
				(number "3")
			)
			(pin open_collector line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "~{TOC}")
				(number "13")
			)
			(pin open_collector line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{READY}")
				(number "19")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "TIMER")
				(number "10")
			)
			(pin passive line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "CHEM")
				(number "4")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at -2.54 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "V_{CC}")
				(number "18")
			)
			(pin power_in line
				(at 2.54 -22.86 90)
				(length 2.54)
				(name "PGND")
				(number "16")
			)
			(pin power_out line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "INTVDD")
				(number "14")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "TGATE")
				(number "17")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "BGATE")
				(number "15")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "SENSE")
				(number "11")
			)
			(pin power_out line
				(at 12.7 0 180)
				(length 2.54)
				(name "BAT")
				(number "12")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "V_{CDIV}")
				(number "9")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "V_{CELL}")
				(number "8")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "V_{TEMP}")
				(number "7")
			)
			(pin output line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "V_{RT}")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC4054ES5-4.2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.842 6.604 0)
		)
		(property "Value" "LTC4054ES5-4.2"
			(at 1.524 6.604 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/405442xf.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "Constant-current/constant-voltage linear charger for single cell lithium-ion batteries with 2.9V Trickle Charge, 4.5V to 6.5V VDD, -40 to +85 degree Celsius, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Constant-current constant-voltage linear charger single cell lithium-ion battery"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "LTC4054ES5-4.2_0_1")
		(symbol "LTC4054ES5-4.2_1_1"
			(pin open_collector line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{CHRG}")
				(number "1")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "PROG")
				(number "5")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V_{CC}")
				(number "4")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "BAT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC4055"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 13.97 0)
		)
		(property "Value" "LTC4055"
			(at 3.81 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_4x4mm_P0.65mm_EP2.15x2.15mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/4055fb.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "USB Power Controller and Li-Ion Charger (4.2V Float Voltage)"
			(at 0 0 0)
		)
		(property "ki_keywords" "charger PMIC Liion USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LTC4055_0_1")
		(symbol "LTC4055_1_1"
			(pin passive line
				(at -10.16 10.16 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "1")
			)
			(pin power_in line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "IN")
				(number "4")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "WALL")
				(number "5")
			)
			(pin open_collector line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{ACPR}")
				(number "13")
			)
			(pin open_collector line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{CHRG}")
				(number "14")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "CLPROG")
				(number "9")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "PROG")
				(number "11")
			)
			(pin passive line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "TIMER")
				(number "12")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "BAT")
				(number "2")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VNTC")
				(number "15")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "NTC")
				(number "16")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "SHDN")
				(number "6")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "SUSP")
				(number "7")
			)
			(pin input line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "HPWR")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC4060EDHC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.382 13.97 0)
		)
		(property "Value" "LTC4060EDHC"
			(at 2.54 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-16-1EP_3x5mm_P0.5mm_EP1.66x4.4mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/405442xf.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "Complete fast charging system for 2, 3 or 4 series NiMH or NiCd batteries, 0.4 to 2A, 4.5 to 10V VDD, -40 to +85 degree Celcisus, DFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery charger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC4060EDHC_0_1")
		(symbol "LTC4060EDHC_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "5")
			)
			(pin open_collector line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "~{CHRG}")
				(number "15")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "NTC")
				(number "11")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "ARCT")
				(number "8")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PROG")
				(number "7")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PAUSE")
				(number "6")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "SEL1")
				(number "10")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "SEL0")
				(number "9")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "V_{CC}")
				(number "14")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "16")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "GNDPAD")
				(number "17")
			)
			(pin open_collector line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "~{ACP}")
				(number "13")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "SENSE")
				(number "3")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "DRIVE")
				(number "1")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "BAT")
				(number "2")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "TIMER")
				(number "4")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "CHEM")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC4060EFE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.382 13.97 0)
		)
		(property "Value" "LTC4060EFE"
			(at 1.524 13.97 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16-1EP_4.4x5mm_P0.65mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/405442xf.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "Complete fast charging system for 2, 3 or 4 series NiMH or NiCd batteries, 0.4 to 2A, 4.5 to 10V VDD, -40 to +85 degree Celcisus, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery charger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*EP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LTC4060EFE_0_1")
		(symbol "LTC4060EFE_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "5")
			)
			(pin open_collector line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "~{CHRG}")
				(number "15")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "NTC")
				(number "11")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "ARCT")
				(number "8")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PROG")
				(number "7")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PAUSE")
				(number "6")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "SEL1")
				(number "10")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "SEL0")
				(number "9")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "V_{CC}")
				(number "14")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "16")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "GNDPAD")
				(number "17")
			)
			(pin open_collector line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "~{ACP}")
				(number "13")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "SENSE")
				(number "3")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "DRIVE")
				(number "1")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "BAT")
				(number "2")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "TIMER")
				(number "4")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "CHEM")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC4067EDE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 19.05 0)
		)
		(property "Value" "LTC4067EDE"
			(at 5.08 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-12-1EP_3x4mm_P0.5mm_EP1.7x3.3mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/4067f.pdf"
			(at 0 22.86 0)
		)
		(property "Description" "Li-Ion Battery Manager and Charger, Power Switcher, 1.25A max charge current, DFN-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "Polymer NTC constant-current"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x4mm*"
			(at 0 0 0)
		)
		(symbol "LTC4067EDE_0_1")
		(symbol "LTC4067EDE_1_1"
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "OVI")
				(number "6")
			)
			(pin output line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "OVP")
				(number "7")
			)
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IN")
				(number "12")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "NTC")
				(number "3")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "ILIM0")
				(number "4")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "ILIM1")
				(number "5")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "CLPROG")
				(number "1")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin power_out line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "OUT")
				(number "11")
			)
			(pin output line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "GATE")
				(number "9")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "BAT")
				(number "10")
			)
			(pin open_collector line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "~{CHRG}")
				(number "2")
			)
			(pin input line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "PROG")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC4156"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 24.13 0)
		)
		(property "Value" "LTC4156"
			(at 6.35 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_4x5mm_P0.5mm_EP2.65x3.65mm"
			(at 0 -27.94 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/4156fa.pdf"
			(at 0 -30.48 0)
		)
		(property "Description" "Dual-Input Power Manager / 3.5A LiFePO4 Battery Charger with I2C Control and USB OTG, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "lifepo charger PMIC USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC4156_0_1")
		(symbol "LTC4156_1_1"
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "WALLSNS")
				(number "7")
			)
			(pin output line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "WALLGT")
				(number "11")
			)
			(pin passive line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "V_{BUS}")
				(number "23")
			)
			(pin passive line
				(at -12.7 12.7 0)
				(length 2.54)
				(hide yes)
				(name "V_{BUS}")
				(number "24")
			)
			(pin passive line
				(at -12.7 12.7 0)
				(length 2.54)
				(hide yes)
				(name "V_{BUS}")
				(number "25")
			)
			(pin output line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "USBGT")
				(number "9")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "USBSNS")
				(number "8")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "ID")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "SDA")
				(number "1")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "SCL")
				(number "28")
			)
			(pin open_collector line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "~{IRQ}")
				(number "3")
			)
			(pin passive line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "CLPROG1")
				(number "5")
			)
			(pin passive line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "CLPROG2")
				(number "6")
			)
			(pin passive line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "PROG")
				(number "18")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "DVCC")
				(number "2")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "29")
			)
			(pin passive line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "SW")
				(number "26")
			)
			(pin passive line
				(at 12.7 20.32 180)
				(length 2.54)
				(hide yes)
				(name "SW")
				(number "27")
			)
			(pin input line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "V_{OUTSNS}")
				(number "13")
			)
			(pin passive line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "V_{OUT}")
				(number "21")
			)
			(pin passive line
				(at 12.7 15.24 180)
				(length 2.54)
				(hide yes)
				(name "V_{OUT}")
				(number "22")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "CHGSNS")
				(number "19")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 2.54)
				(hide yes)
				(name "CHGSNS")
				(number "20")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "BATGATE")
				(number "17")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "BATSNS")
				(number "16")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "NTCBIAS")
				(number "14")
			)
			(pin input line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "NTC")
				(number "15")
			)
			(pin passive line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "OVGCAP")
				(number "10")
			)
			(pin passive line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "V_{C}")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC6803-2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 34.29 0)
		)
		(property "Value" "LTC6803-2"
			(at -10.16 -34.29 0)
		)
		(property "Footprint" "Package_SO:SSOP-44_5.3x12.8mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/680324fa.pdf"
			(at 13.97 34.29 0)
		)
		(property "Description" "Multicell Battery Stack Monitor, 12-cell max, multi-chemistry, integrated balancing, stackable, serial interface"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery balance afe"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x12.8mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC6803-2_0_1")
		(symbol "LTC6803-2_1_1"
			(pin input line
				(at -12.7 30.48 0)
				(length 2.54)
				(name "V_{REF}")
				(number "30")
			)
			(pin input line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "V_{REG}")
				(number "31")
			)
			(pin input line
				(at -12.7 25.4 0)
				(length 2.54)
				(name "TOS")
				(number "32")
			)
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "A0")
				(number "37")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "A1")
				(number "38")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "A2")
				(number "39")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "A3")
				(number "40")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "GPIO1")
				(number "35")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "GPIO2")
				(number "36")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "SCKI")
				(number "41")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "SDI")
				(number "42")
			)
			(pin open_collector line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "SDO")
				(number "43")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "~{CSBI}")
				(number "44")
			)
			(pin input line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "V_{TEMP1}")
				(number "28")
			)
			(pin input line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "V_{TEMP2}")
				(number "29")
			)
			(pin open_collector line
				(at -12.7 -30.48 0)
				(length 2.54)
				(name "~{WDTB}")
				(number "34")
			)
			(pin no_connect line
				(at -2.54 33.02 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "33")
			)
			(pin no_connect line
				(at 0 33.02 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "27")
			)
			(pin input line
				(at 2.54 35.56 270)
				(length 2.54)
				(name "V^{+}")
				(number "1")
			)
			(pin input line
				(at 5.08 -35.56 90)
				(length 2.54)
				(name "V^{-}")
				(number "26")
			)
			(pin input line
				(at 12.7 30.48 180)
				(length 2.54)
				(name "C12")
				(number "2")
			)
			(pin input line
				(at 12.7 27.94 180)
				(length 2.54)
				(name "S12")
				(number "3")
			)
			(pin input line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "C11")
				(number "4")
			)
			(pin input line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "S11")
				(number "5")
			)
			(pin input line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "C10")
				(number "6")
			)
			(pin input line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "S10")
				(number "7")
			)
			(pin input line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "C9")
				(number "8")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "S9")
				(number "9")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "C8")
				(number "10")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "S8")
				(number "11")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "C7")
				(number "12")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "S7")
				(number "13")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "C6")
				(number "14")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "S6")
				(number "15")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "C5")
				(number "16")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "S5")
				(number "17")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "C4")
				(number "18")
			)
			(pin input line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "S4")
				(number "19")
			)
			(pin input line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "C3")
				(number "20")
			)
			(pin input line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "S3")
				(number "21")
			)
			(pin input line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "C2")
				(number "22")
			)
			(pin input line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "S2")
				(number "23")
			)
			(pin input line
				(at 12.7 -25.4 180)
				(length 2.54)
				(name "C1")
				(number "24")
			)
			(pin input line
				(at 12.7 -27.94 180)
				(length 2.54)
				(name "S1")
				(number "25")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC6803-4"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 34.29 0)
		)
		(property "Value" "LTC6803-4"
			(at -10.16 -34.29 0)
		)
		(property "Footprint" "Package_SO:SSOP-44_5.3x12.8mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/680324fa.pdf"
			(at 13.97 34.29 0)
		)
		(property "Description" "Multicell Battery Stack Monitor, 12-cell max, multi-chemistry, integrated balancing, stackable, serial interface"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery balance afe"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x12.8mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC6803-4_0_1")
		(symbol "LTC6803-4_1_1"
			(pin input line
				(at -12.7 30.48 0)
				(length 2.54)
				(name "V_{REF}")
				(number "31")
			)
			(pin input line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "V_{REG}")
				(number "32")
			)
			(pin input line
				(at -12.7 25.4 0)
				(length 2.54)
				(name "TOS")
				(number "33")
			)
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "A0")
				(number "37")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "A1")
				(number "38")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "A2")
				(number "39")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "A3")
				(number "40")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "GPIO1")
				(number "35")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "GPIO2")
				(number "36")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "SCKI")
				(number "41")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "SDI")
				(number "42")
			)
			(pin open_collector line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "SDO")
				(number "43")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "~{CSBI}")
				(number "44")
			)
			(pin input line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "V_{TEMP1}")
				(number "29")
			)
			(pin input line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "V_{TEMP2}")
				(number "30")
			)
			(pin open_collector line
				(at -12.7 -30.48 0)
				(length 2.54)
				(name "~{WDTB}")
				(number "34")
			)
			(pin no_connect line
				(at 0 33.02 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "28")
			)
			(pin input line
				(at 2.54 35.56 270)
				(length 2.54)
				(name "V^{+}")
				(number "1")
			)
			(pin input line
				(at 5.08 -35.56 90)
				(length 2.54)
				(name "V^{-}")
				(number "27")
			)
			(pin input line
				(at 12.7 30.48 180)
				(length 2.54)
				(name "C12")
				(number "2")
			)
			(pin input line
				(at 12.7 27.94 180)
				(length 2.54)
				(name "S12")
				(number "3")
			)
			(pin input line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "C11")
				(number "4")
			)
			(pin input line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "S11")
				(number "5")
			)
			(pin input line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "C10")
				(number "6")
			)
			(pin input line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "S10")
				(number "7")
			)
			(pin input line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "C9")
				(number "8")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "S9")
				(number "9")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "C8")
				(number "10")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "S8")
				(number "11")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "C7")
				(number "12")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "S7")
				(number "13")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "C6")
				(number "14")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "S6")
				(number "15")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "C5")
				(number "16")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "S5")
				(number "17")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "C4")
				(number "18")
			)
			(pin input line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "S4")
				(number "19")
			)
			(pin input line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "C3")
				(number "20")
			)
			(pin input line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "S3")
				(number "21")
			)
			(pin input line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "C2")
				(number "22")
			)
			(pin input line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "S2")
				(number "23")
			)
			(pin input line
				(at 12.7 -25.4 180)
				(length 2.54)
				(name "C1")
				(number "24")
			)
			(pin input line
				(at 12.7 -27.94 180)
				(length 2.54)
				(name "S1")
				(number "25")
			)
			(pin input line
				(at 12.7 -30.48 180)
				(length 2.54)
				(name "C0")
				(number "26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC6804-1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 34.29 0)
		)
		(property "Value" "LTC6804-1"
			(at -16.51 -34.29 0)
		)
		(property "Footprint" "Package_SO:SSOP-48_5.3x12.8mm_P0.5mm"
			(at -1.27 2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/680412fc.pdf"
			(at 13.97 34.29 0)
		)
		(property "Description" "Multicell Battery Stack Monitor, 12-cell max, multi-chemistry, integrated balancing, stackable, serial interface, SSOP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery balance afe"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x12.8mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC6804-1_0_1")
		(symbol "LTC6804-1_1_1"
			(pin output line
				(at -12.7 30.48 0)
				(length 2.54)
				(name "DRIVE")
				(number "38")
			)
			(pin input line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "VREG")
				(number "37")
			)
			(pin input line
				(at -12.7 25.4 0)
				(length 2.54)
				(name "ISOMD")
				(number "40")
			)
			(pin input line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "SWTEN")
				(number "36")
			)
			(pin output line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "VREF1")
				(number "35")
			)
			(pin output line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "VREF2")
				(number "34")
			)
			(pin passive line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "ICMP")
				(number "46")
			)
			(pin passive line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "IBIAS")
				(number "45")
			)
			(pin output line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "WDT")
				(number "39")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "IMB")
				(number "47")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "IPB")
				(number "48")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "CSB(IMA)")
				(number "41")
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "SCK(IPA)")
				(number "42")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "SDI(NC)")
				(number "43")
			)
			(pin open_collector line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "SDO(NC)")
				(number "44")
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "GPIO1")
				(number "27")
			)
			(pin bidirectional line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "GPIO2")
				(number "28")
			)
			(pin bidirectional line
				(at -12.7 -25.4 0)
				(length 2.54)
				(name "GPIO3")
				(number "29")
			)
			(pin bidirectional line
				(at -12.7 -27.94 0)
				(length 2.54)
				(name "GPIO4")
				(number "32")
			)
			(pin bidirectional line
				(at -12.7 -30.48 0)
				(length 2.54)
				(name "GPIO5")
				(number "33")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "V+")
				(number "1")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "V-")
				(number "30")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(name "V-")
				(number "31")
			)
			(pin input line
				(at 12.7 30.48 180)
				(length 2.54)
				(name "C12")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 27.94 180)
				(length 2.54)
				(name "S12")
				(number "3")
			)
			(pin input line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "C11")
				(number "4")
			)
			(pin bidirectional line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "S11")
				(number "5")
			)
			(pin input line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "C10")
				(number "6")
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "S10")
				(number "7")
			)
			(pin input line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "C9")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "S9")
				(number "9")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "C8")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "S8")
				(number "11")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "C7")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "S7")
				(number "13")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "C6")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "S6")
				(number "15")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "C5")
				(number "16")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "S5")
				(number "17")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "C4")
				(number "18")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "S4")
				(number "19")
			)
			(pin input line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "C3")
				(number "20")
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "S3")
				(number "21")
			)
			(pin input line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "C2")
				(number "22")
			)
			(pin bidirectional line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "S2")
				(number "23")
			)
			(pin input line
				(at 12.7 -25.4 180)
				(length 2.54)
				(name "C1")
				(number "24")
			)
			(pin bidirectional line
				(at 12.7 -27.94 180)
				(length 2.54)
				(name "S1")
				(number "25")
			)
			(pin input line
				(at 12.7 -30.48 180)
				(length 2.54)
				(name "C0")
				(number "26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX1647"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "MAX1647"
			(at 12.7 21.59 0)
		)
		(property "Footprint" "Package_SO:SSOP-20_5.3x7.2mm_P0.65mm"
			(at 0 25.4 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX1647-MAX1648.pdf"
			(at -12.7 21.59 0)
		)
		(property "Description" "Smart Battery Charger, 18V battery, 28V input, SMBus serial interface"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery charger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x7.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MAX1647_0_1")
		(symbol "MAX1647_1_1"
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "SCLK")
				(number "13")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "SDA")
				(number "14")
			)
			(pin open_collector line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "~{INT}")
				(number "11")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "REF")
				(number "9")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "SEL")
				(number "6")
			)
			(pin passive line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "CCI")
				(number "5")
			)
			(pin passive line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "CCV")
				(number "4")
			)
			(pin output line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "DACV")
				(number "15")
			)
			(pin power_in line
				(at -2.54 -22.86 90)
				(length 2.54)
				(name "AGND")
				(number "10")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "DCIN")
				(number "2")
			)
			(pin power_in line
				(at 2.54 -22.86 90)
				(length 2.54)
				(name "PGND")
				(number "16")
			)
			(pin output line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "IOUT")
				(number "1")
			)
			(pin input line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "BATT")
				(number "8")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "CS")
				(number "7")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "THM")
				(number "12")
			)
			(pin power_out line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "VL")
				(number "3")
			)
			(pin power_in line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "BST")
				(number "20")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "DHI")
				(number "18")
			)
			(pin input line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "LX")
				(number "19")
			)
			(pin output line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "DLO")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX1648"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 19.05 0)
		)
		(property "Value" "MAX1648"
			(at 12.7 19.05 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 22.86 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX1647-MAX1648.pdf"
			(at -12.7 19.05 0)
		)
		(property "Description" "Smart Battery Charger, 18V battery, 28V input, standalone"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery charger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MAX1648_0_1")
		(symbol "MAX1648_1_1"
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "SETI")
				(number "10")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "SETV")
				(number "11")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "REF")
				(number "7")
			)
			(pin passive line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "CCI")
				(number "4")
			)
			(pin passive line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "CCV")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 2.54)
				(name "AGND")
				(number "8")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "DCIN")
				(number "1")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "PGND")
				(number "12")
			)
			(pin input line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "BATT")
				(number "6")
			)
			(pin input line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "CS")
				(number "5")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "THM")
				(number "9")
			)
			(pin power_out line
				(at 15.24 0 180)
				(length 2.54)
				(name "VL")
				(number "2")
			)
			(pin power_in line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "BST")
				(number "16")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "DHI")
				(number "14")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "LX")
				(number "15")
			)
			(pin output line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "DLO")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX17261xxTD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.985 11.43 0)
		)
		(property "Value" "MAX17261xxTD"
			(at 8.255 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:TDFN-14-1EP_3x3mm_P0.4mm_EP1.78x2.35mm"
			(at 0 -30.48 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX17261.pdf"
			(at 15.24 2.54 0)
		)
		(property "Description" "5.1μA Multi-Cell Fuel Gauge with ModelGauge m5 EZ, TDFN-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Charge pump battery"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDFN*1EP*3x3mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "MAX17261xxTD_0_1")
		(symbol "MAX17261xxTD_1_1"
			(pin output line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "SW")
				(number "3")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "CELLX")
				(number "10")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "TH")
				(number "1")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "CSN")
				(number "7")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "CSPL")
				(number "9")
			)
			(pin no_connect line
				(at -2.54 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "BATT")
				(number "6")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin no_connect line
				(at 2.54 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at 5.08 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "SCL")
				(number "14")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SDA")
				(number "13")
			)
			(pin open_collector line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "ALRT")
				(number "12")
			)
			(pin power_out line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "REG")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX17261xxWL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.985 11.43 0)
		)
		(property "Value" "MAX17261xxWL"
			(at 8.255 11.43 0)
		)
		(property "Footprint" "Package_BGA:Maxim_WLP-9_1.595x1.415_Layout3x3_P0.4mm_Ball0.27mm_Pad0.25mm_NSMD"
			(at 27.94 -20.32 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX17261.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "5.1μA Multi-Cell Fuel Gauge with ModelGauge m5 EZ, WLP-9"
			(at 0 0 0)
		)
		(property "ki_keywords" "Charge pump battery"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Maxim*WLP*1.595x1.415*Layout3x3*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "MAX17261xxWL_0_1")
		(symbol "MAX17261xxWL_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "CELLX")
				(number "C2")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "TH")
				(number "A1")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "CSN")
				(number "A3")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "BATT")
				(number "B1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND/CSPL")
				(number "C3")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "SCL")
				(number "A2")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SDA")
				(number "C1")
			)
			(pin open_collector line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "ALRT")
				(number "B2")
			)
			(pin power_out line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "REG")
				(number "B3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX17263xxTE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 17.78 0)
		)
		(property "Value" "MAX17263xxTE"
			(at 2.54 15.24 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-14-1EP_3x3mm_P0.4mm_EP1.78x2.35mm"
			(at 0 5.08 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX17263.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Single/Multi-Cell Fuel Gauge, ModelGauge m5 EZ, Integrated LED Control, TDFN-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "fuel-gauge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "MAX17263xxTE_0_1")
		(symbol "MAX17263xxTE_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "CELLX/CSPH")
				(number "10")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "CSN")
				(number "7")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "CSPL")
				(number "9")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "TH")
				(number "1")
			)
			(pin passive line
				(at -5.08 -15.24 90)
				(length 2.54)
				(name "EP")
				(number "15")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "BATT")
				(number "6")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin open_collector line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "ALRT")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "SDA")
				(number "13")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "SCL")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "L1")
				(number "2")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "L2")
				(number "3")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "L3")
				(number "4")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "L4")
				(number "5")
			)
			(pin power_out line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "REG")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX1811"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MAX1811"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 6.35 -8.89 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX1811.pdf"
			(at 0 -17.78 0)
		)
		(property "Description" "USB Powered Li+ Charger, 4.1V/4.2V battery, 5V input, 0.1/0.5A charging current"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB Battery Charger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*"
			(at 0 0 0)
		)
		(symbol "MAX1811_0_1")
		(symbol "MAX1811_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IN")
				(number "4")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "EN")
				(number "7")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SELV")
				(number "1")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SELI")
				(number "2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin power_out line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "BATT")
				(number "5")
			)
			(pin open_collector line
				(at 12.7 0 180)
				(length 2.54)
				(name "~{CHG}")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX1873REEE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.096 13.97 0)
		)
		(property "Value" "MAX1873REEE"
			(at 2.286 13.97 0)
		)
		(property "Footprint" "Package_SO:QSOP-16_3.9x4.9mm_P0.635mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX1873.pdf"
			(at 5.08 0 0)
		)
		(property "Description" "Charger for 2 lithium-ion (Li+), 5/6 NickelCadium (NiCD) cells or 5/6 NickelMetalHydride (NiMH), 9 to 28V VDD, -40 to +85 degree Celsius, QSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "li-ion battery charger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "MAX1873REEE_0_1")
		(symbol "MAX1873REEE_1_1"
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "VH")
				(number "13")
			)
			(pin output line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IOUT")
				(number "7")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "ICHG/EN")
				(number "6")
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "REF")
				(number "9")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "VADJ")
				(number "8")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "VL")
				(number "16")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "DCIN")
				(number "15")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "12")
			)
			(pin input line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "CSSP")
				(number "2")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "CSSN")
				(number "1")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "EXT")
				(number "14")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "CSB")
				(number "11")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "BATT")
				(number "10")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "CCI")
				(number "5")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "CCS")
				(number "3")
			)
			(pin input line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "CCV")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX712CPE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.382 13.97 0)
		)
		(property "Value" "MAX712CPE"
			(at 2.54 13.97 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 15.24 -13.97 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX712-MAX713.pdf"
			(at -17.78 5.08 0)
		)
		(property "Description" "Fast-charge Nickel Metal Hydride (NiMH) from a DC source, 0 to +70 Degree Celsius, PDIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery charger controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MAX712CPE_0_1")
		(symbol "MAX712CPE_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "THI")
				(number "5")
			)
			(pin power_in line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "REF")
				(number "16")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VLIMIT")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "TEMP")
				(number "7")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PGM0")
				(number "3")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PGM1")
				(number "4")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PGM2")
				(number "9")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "PGM3")
				(number "10")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "V+")
				(number "15")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "DRV")
				(number "14")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "BATT+")
				(number "2")
			)
			(pin open_collector line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "~{FASTCHG}")
				(number "8")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "BATT-")
				(number "12")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "CC")
				(number "11")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "TLO")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX712CSE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.382 13.97 0)
		)
		(property "Value" "MAX712CSE"
			(at 2.54 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX712-MAX713.pdf"
			(at -17.78 5.08 0)
		)
		(property "Description" "Fast-charge Nickel Metal Hydride (NiMH) from a DC source, 0 to +70 Degree Celsius, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery charger controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MAX712CSE_0_1")
		(symbol "MAX712CSE_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "THI")
				(number "5")
			)
			(pin power_in line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "REF")
				(number "16")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VLIMIT")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "TEMP")
				(number "7")
			)
			(pin power_out line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PGM0")
				(number "3")
			)
			(pin power_out line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PGM1")
				(number "4")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PGM2")
				(number "9")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "PGM3")
				(number "10")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "V+")
				(number "15")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "DRV")
				(number "14")
			)
			(pin power_out line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "BATT+")
				(number "2")
			)
			(pin open_collector line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "~{FASTCHG}")
				(number "8")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "BATT-")
				(number "12")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "CC")
				(number "11")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "TLO")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC34673"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 10.795 0)
		)
		(property "Value" "MC34673"
			(at 10.16 10.795 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.75x1.45mm"
			(at 1.27 -10.795 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/MC34673.pdf"
			(at 2.54 -15.24 0)
		)
		(property "Description" "High Input Voltage 1.2A Charger for Single-cell Li-Ion Batteries, UDFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lithium-Ion Battery Charger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MC34673_0_1")
		(symbol "MC34673_1_1"
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{EN}")
				(number "4")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "EPAD")
				(number "9")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_out line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "BAT")
				(number "8")
			)
			(pin open_collector line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "~{PPR}")
				(number "2")
			)
			(pin open_collector line
				(at 12.7 0 180)
				(length 2.54)
				(name "~{CHG}")
				(number "3")
			)
			(pin open_collector line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "~{FAST}")
				(number "6")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "ISET")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP73812T-420I-OT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MCP73812T-420I-OT"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22036b.pdf"
			(at -6.35 6.35 0)
		)
		(property "Description" "Simple, Miniature Single-Cell, Fully Integrated Li-Ion / Li-Polymer Charge Management Controllers, 50mA-500mA, 4.2V, SOT23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lithium-Ion Battery Charger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MCP73812T-420I-OT_0_1")
		(symbol "MCP73812T-420I-OT_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "CE")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "PROG")
				(number "5")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V_{DD}")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "V_{SS}")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "V_{BAT}")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP73831-2-MC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MCP73831-2-MC"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.7x1.4mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001984g.pdf"
			(at -3.81 -1.27 0)
		)
		(property "Description" "Single cell, Li-Ion/Li-Po charge management controller, 4.20V, Tri-State Status Output, in DFN-8 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery charger lithium"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x2mm*P0.5mm*EP1.7x1.4mm*"
			(at 0 0 0)
		)
		(symbol "MCP73831-2-MC_0_1")
		(symbol "MCP73831-2-MC_1_1"
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "PROG")
				(number "8")
			)
			(pin no_connect line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(hide yes)
				(name "V_{DD}")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V_{DD}")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "V_{SS}")
				(number "6")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "V_{BAT}")
				(number "3")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "V_{BAT}")
				(number "4")
			)
			(pin tri_state line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "STAT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP73831-2-OT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MCP73831-2-OT"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001984g.pdf"
			(at 0 -18.288 0)
		)
		(property "Description" "Single cell, Li-Ion/Li-Po charge management controller, 4.20V, Tri-State Status Output, in SOT23-5 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery charger lithium"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MCP73831-2-OT_0_1")
		(symbol "MCP73831-2-OT_1_1"
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "PROG")
				(number "5")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V_{DD}")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "V_{SS}")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "V_{BAT}")
				(number "3")
			)
			(pin tri_state line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "STAT")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP73832-2-MC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MCP73832-2-MC"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.7x1.4mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001984g.pdf"
			(at 0 -18.288 0)
		)
		(property "Description" "Single cell, Li-Ion/Li-Po charge management controller, 4.20V, Open-Drain Status Output, in DFN-8 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery charger lithium"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x2mm*P0.5mm*EP1.7x1.4mm*"
			(at 0 0 0)
		)
		(symbol "MCP73832-2-MC_0_1")
		(symbol "MCP73832-2-MC_1_1"
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "PROG")
				(number "8")
			)
			(pin no_connect line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(hide yes)
				(name "V_{DD}")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V_{DD}")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "V_{SS}")
				(number "6")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "V_{BAT}")
				(number "3")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "V_{BAT}")
				(number "4")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "STAT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP73832-2-OT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MCP73832-2-OT"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001984g.pdf"
			(at 0 -18.796 0)
		)
		(property "Description" "Single cell, Li-Ion/Li-Po charge management controller, 4.20V, Open-Drain Status Output, in SOT23-5 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery charger lithium"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MCP73832-2-OT_0_1")
		(symbol "MCP73832-2-OT_1_1"
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "PROG")
				(number "5")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V_{DD}")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "V_{SS}")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "V_{BAT}")
				(number "3")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "STAT")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP73833-xxx-MF"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "MCP73833-xxx-MF"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-10-1EP_3x3mm_P0.5mm_EP1.58x2.35mm"
			(at 33.02 -8.89 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/OTH/ProductDocuments/DataSheets/22005b.pdf"
			(at 0 0 0)
		)
		(property "Description" "Stand-Alone Linear Li-Ion / Li-Polymer Charge Management Controller, DFN-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "lithium-ion battery charger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P0.5mm*EP1.58x2.35mm*"
			(at 0 0 0)
		)
		(symbol "MCP73833-xxx-MF_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "V_{DD}")
				(number "1")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "V_{DD}")
				(number "2")
			)
			(pin open_collector line
				(at -10.16 0 0)
				(length 2.54)
				(name "STAT1")
				(number "3")
			)
			(pin open_collector line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "STAT2")
				(number "4")
			)
			(pin open_collector line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{PG}")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "EP")
				(number "11")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "V_{SS}")
				(number "5")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "V_{BAT}")
				(number "10")
			)
			(pin power_out line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "V_{BAT}")
				(number "9")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "THERM")
				(number "8")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "PROG")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP73833-xxx-UN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "MCP73833-xxx-UN"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 20.32 -8.89 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/OTH/ProductDocuments/DataSheets/22005b.pdf"
			(at 0 0 0)
		)
		(property "Description" "Stand-Alone Linear Li-Ion / Li-Polymer Charge Management Controller, MSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "lithium-ion battery charger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MCP73833-xxx-UN_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "V_{DD}")
				(number "1")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "V_{DD}")
				(number "2")
			)
			(pin open_collector line
				(at -10.16 0 0)
				(length 2.54)
				(name "STAT1")
				(number "3")
			)
			(pin open_collector line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "STAT2")
				(number "4")
			)
			(pin open_collector line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{PG}")
				(number "7")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "V_{SS}")
				(number "5")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "V_{BAT}")
				(number "10")
			)
			(pin power_out line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "V_{BAT}")
				(number "9")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "THERM")
				(number "8")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "PROG")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP73871"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 24.13 0)
		)
		(property "Value" "MCP73871"
			(at -15.24 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.5x2.5mm"
			(at 5.08 -22.86 0)
		)
		(property "Datasheet" "http://www.mouser.com/ds/2/268/22090a-52174.pdf"
			(at -3.81 13.97 0)
		)
		(property "Description" "Single cell, Li-Ion/Li-Po charge management controller"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery charger lithium"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MCP73871_0_1")
		(symbol "MCP73871_1_1"
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "VPCC")
				(number "2")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "SEL")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PROG1")
				(number "13")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PROG2")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PROG3")
				(number "12")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "THERM")
				(number "5")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "~{TE}")
				(number "9")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "CE")
				(number "17")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "IN")
				(number "18")
			)
			(pin passive line
				(at 0 22.86 270)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "19")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "V_{SS}")
				(number "10")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "V_{SS}")
				(number "11")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "V_{SS}")
				(number "21")
			)
			(pin power_out line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin passive line
				(at 17.78 15.24 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "20")
			)
			(pin power_out line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "V_{BAT}")
				(number "14")
			)
			(pin passive line
				(at 17.78 7.62 180)
				(length 2.54)
				(hide yes)
				(name "V_{BAT}")
				(number "15")
			)
			(pin input line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "V_{BAT_SENSE}")
				(number "16")
			)
			(pin open_collector line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "~{PG}")
				(number "6")
			)
			(pin open_collector line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "STAT1/~{LBO}")
				(number "8")
			)
			(pin open_collector line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "STAT2")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SLM6800"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.112 16.51 0)
		)
		(property "Value" "SLM6800"
			(at 4.826 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_4x4mm_P0.65mm_EP2.15x2.15mm"
			(at 20.066 -21.336 0)
		)
		(property "Datasheet" "https://datasheet.lcsc.com/lcsc/1912111437_SOLA-IC-SLM6800_C388594.pdf"
			(at 20.066 -23.876 0)
		)
		(property "Description" "1.5A, 2-Cell 8.4V, standalone switch-mode Li-Ion Charger, 5Vin, 750kHz, QFN-16"
			(at 20.066 -26.416 0)
		)
		(property "ki_keywords" "battery charger dual-cell two-cell li-ion li-poly"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "SLM6800_0_0"
			(pin open_collector line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "~{CHRG}")
				(number "13")
			)
			(pin open_collector line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "~{STBY}")
				(number "14")
			)
		)
		(symbol "SLM6800_1_0"
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "EN")
				(number "16")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "ILIM")
				(number "10")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "ISET")
				(number "11")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "TM")
				(number "12")
			)
			(pin passive line
				(at -2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "17")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 2.54)
				(name "PGND")
				(number "4")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "SGND")
				(number "15")
			)
			(pin output line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "LX")
				(number "5")
			)
			(pin passive line
				(at 10.16 12.7 180)
				(length 2.54)
				(hide yes)
				(name "LX")
				(number "6")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "BST")
				(number "3")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "NTC")
				(number "1")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "BAT")
				(number "9")
			)
			(pin output line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "VSYS")
				(number "7")
			)
			(pin passive line
				(at 10.16 -12.7 180)
				(length 2.54)
				(hide yes)
				(name "VSYS")
				(number "8")
			)
		)
		(symbol "SLM6800_1_1")
		(embedded_fonts no)
	)
	(symbol "TP4056-42-ESOP8"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.604 11.684 0)
		)
		(property "Value" "TP4056-42-ESOP8"
			(at 10.16 11.684 0)
		)
		(property "Footprint" "Package_SO:SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.41x3.3mm_ThermalVias"
			(at 0.508 -22.86 0)
		)
		(property "Datasheet" "https://www.lcsc.com/datasheet/lcsc_datasheet_2410121619_TOPPOWER-Nanjing-Extension-Microelectronics-TP4056-42-ESOP8_C16581.pdf"
			(at 0 -25.4 0)
		)
		(property "Description" "1A Standalone Linear Li-ion/LiPo single-cell battery charger, 4.2V ±1% charge voltage, VCC = 4.0..8.0V, SOIC-8 (SOP-8)"
			(at 0.508 -20.32 0)
		)
		(property "ki_keywords" "lithium-ion lithium-polymer Li-Poly"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SO*3.9x4.*P1.27mm*EP2.4*x3.3*mm*"
			(at 0 0 0)
		)
		(symbol "TP4056-42-ESOP8_1_0"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "CE")
				(number "8")
			)
			(pin open_collector line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{CHRG}")
				(number "7")
			)
			(pin open_collector line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{STDBY}")
				(number "6")
			)
			(pin passive line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "EPAD")
				(number "9")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V_{CC}")
				(number "4")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_out line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "BAT")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "TEMP")
				(number "1")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "PROG")
				(number "2")
			)
		)
		(symbol "TP4056-42-ESOP8_1_1")
		(embedded_fonts no)
	)
	(symbol "TP4057"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.604 0)
		)
		(property "Value" "TP4057"
			(at 1.524 6.604 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://toppwr.com/uploadfile/file/20230304/640302a47b738.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "Constant-current/constant-voltage linear charger for single cell lithium-ion batteries with 2.9V Trickle Charge, 4.5V to 6.5V VDD, -40 to +85 degree Celsius, TSOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Constant-current constant-voltage linear charger single-cell lithium-ion battery"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "TP4057_0_1")
		(symbol "TP4057_1_1"
			(pin open_collector line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{CHRG}")
				(number "1")
			)
			(pin open_collector line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "STDBY")
				(number "5")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V_{CC}")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "BAT")
				(number "3")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "PROG")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BQ24073RGT"
		(extends "BQ24072RGT")
		(property "Reference" "U"
			(at -8.89 13.97 0)
		)
		(property "Value" "BQ24073RGT"
			(at 16.51 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.6x1.6mm"
			(at 7.62 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/bq24073.pdf"
			(at 7.62 5.08 0)
		)
		(property "Description" "USB-Friendly Li-Ion Battery Charger and Power-Path Management, VQFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB Charger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "BQ24079RGT"
		(extends "BQ24075RGT")
		(property "Reference" "U"
			(at -8.89 13.97 0)
		)
		(property "Value" "BQ24079RGT"
			(at 16.51 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.6x1.6mm"
			(at 7.62 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/bq24079.pdf"
			(at 7.62 5.08 0)
		)
		(property "Description" "USB-Friendly Li-Ion Battery Charger and Power-Path Management, VQFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB Charger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "BQ24167RGE"
		(extends "BQ24166RGE")
		(property "Reference" "U"
			(at -6.35 24.13 0)
		)
		(property "Value" "BQ24167RGE"
			(at 2.54 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGE0024H_VQFN-24-1EP_4x4mm_P0.5mm_EP2.7x2.7mm"
			(at 3.81 -24.13 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/bq24166.pdf"
			(at 22.86 -34.29 0)
		)
		(property "Description" "High efficiency switched mode Li-Ion and Li-Polymer battery charger, integrated MOSFETs, power path selector and JEITA compatible temperature sensing, Texas R-RGE0024H"
			(at 0 0 0)
		)
		(property "ki_keywords" "Battery Charger Li-Ion Li-Poly"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGE0024H*"
			(at 0 0 0)
		)
	)
	(symbol "BQ24617"
		(extends "BQ24610")
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "BQ24617"
			(at 7.62 -26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-24-1EP_4x4mm_P0.5mm_EP2.45x2.45mm"
			(at 0 -40.64 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/bq24610.pdf"
			(at 0 -38.1 0)
		)
		(property "Description" "10A, 24V max voltage, Li-Ion Charger w/600kHz NMOS-NMOS Synchronous Buck Converter, VQFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Li-ion buck"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "BQ27441DRZR-G1A"
		(extends "BQ27441-G1")
		(property "Reference" "U"
			(at -5.08 15.875 0)
		)
		(property "Value" "BQ27441DRZR-G1A"
			(at -5.08 13.97 0)
		)
		(property "Footprint" "Package_SON:Texas_S-PDSO-N12"
			(at 6.35 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/bq27441-g1.pdf"
			(at 5.08 5.08 0)
		)
		(property "Description" "System Side Li Ion/Polymer Fuel Gauge, 4.2V, PDSON-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "Fuel Gauge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PDSO*N12*"
			(at 0 0 0)
		)
	)
	(symbol "BQ27441DRZR-G1B"
		(extends "BQ27441-G1")
		(property "Reference" "U"
			(at -5.08 15.875 0)
		)
		(property "Value" "BQ27441DRZR-G1B"
			(at -5.08 13.97 0)
		)
		(property "Footprint" "Package_SON:Texas_S-PDSO-N12"
			(at 6.35 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/bq27441-g1.pdf"
			(at 5.08 5.08 0)
		)
		(property "Description" "System Side Li Ion/Polymer Fuel Gauge, 4.30-4.35V, PDSON-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "Fuel Gauge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PDSO*N12*"
			(at 0 0 0)
		)
	)
	(symbol "BQ27441DRZT-G1A"
		(extends "BQ27441-G1")
		(property "Reference" "U"
			(at -5.08 15.875 0)
		)
		(property "Value" "BQ27441DRZT-G1A"
			(at -5.08 13.97 0)
		)
		(property "Footprint" "Package_SON:Texas_S-PDSO-N12"
			(at 6.35 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/bq27441-g1.pdf"
			(at 5.08 5.08 0)
		)
		(property "Description" "System Side Li Ion/Polymer Fuel Gauge, 4.2V, PDSON-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "Fuel Gauge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PDSO*N12*"
			(at 0 0 0)
		)
	)
	(symbol "BQ27441DRZT-G1B"
		(extends "BQ27441-G1")
		(property "Reference" "U"
			(at -5.08 15.875 0)
		)
		(property "Value" "BQ27441DRZT-G1B"
			(at -5.08 13.97 0)
		)
		(property "Footprint" "Package_SON:Texas_S-PDSO-N12"
			(at 6.35 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/bq27441-g1.pdf"
			(at 5.08 5.08 0)
		)
		(property "Description" "System Side Li Ion/Polymer Fuel Gauge, 4.30-4.35V, PDSON-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "Fuel Gauge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PDSO*N12*"
			(at 0 0 0)
		)
	)
	(symbol "BQ51051BRHL"
		(extends "BQ51050BRHL")
		(property "Reference" "U"
			(at -8.89 21.59 0)
		)
		(property "Value" "BQ51051BRHL"
			(at 7.62 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_VQFN-RHL-20"
			(at 20.32 -21.59 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/bq51051b.pdf"
			(at 0 0 0)
		)
		(property "Description" "Qi v1.2, Wireless Power Receiver and Battery Charger, Vout 4.35V, VQFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Qi Wireless Power Receiver Battery Charger 4.35V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas?VQFN?RHL*"
			(at 0 0 0)
		)
	)
	(symbol "BQ51051BYFP"
		(extends "BQ51050BYFP")
		(property "Reference" "U"
			(at -8.89 21.59 0)
		)
		(property "Value" "BQ51051BYFP"
			(at 7.62 21.59 0)
		)
		(property "Footprint" "Package_BGA:Texas_DSBGA-28_1.9x3mm_Layout4x7_P0.4mm"
			(at 30.48 -21.59 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/bq51051b.pdf"
			(at 0 0 0)
		)
		(property "Description" "Qi v1.2, Wireless Power Receiver and Battery Charger, Vout 4.35V, DSBGA-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Qi Wireless Power Receiver Battery Charger 4.35V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DSBGA*1.9x3mm*Layout4x7*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "BQ51052BYFP"
		(extends "BQ51050BYFP")
		(property "Reference" "U"
			(at -8.89 21.59 0)
		)
		(property "Value" "BQ51052BYFP"
			(at 7.62 21.59 0)
		)
		(property "Footprint" "Package_BGA:Texas_DSBGA-28_1.9x3mm_Layout4x7_P0.4mm"
			(at 30.48 -21.59 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/bq51052b.pdf"
			(at 0 0 0)
		)
		(property "Description" "Qi v1.2, Wireless Power Receiver and Battery Charger, Vout 4.40V, DSBGA-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Qi Wireless Power Receiver Battery Charger 4.40V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DSBGA*1.9x3mm*Layout4x7*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "BQ78350DBT-R1"
		(extends "BQ78350DBT")
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "BQ78350DBT-R1"
			(at 13.97 26.67 0)
		)
		(property "Footprint" "Package_SO:TSSOP-30_4.4x7.8mm_P0.5mm"
			(at 21.59 -26.67 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/bq78350-r1.pdf"
			(at -17.78 29.21 0)
		)
		(property "Description" "Lithium battery fuel gauge, battery management controller for BQ769x0, TSSOP-30"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery management Li-Ion gauge controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x7.8mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LC709203FQH-02TWG"
		(extends "LC709203FQH-01TWG")
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "LC709203FQH-02TWG"
			(at 11.43 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:WDFN-8-1EP_4x3mm_P0.65mm_EP2.4x1.8mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.onsemi.com/download/data-sheet/pdf/lc709203f-d.pdf"
			(at -1.27 -2.54 0)
		)
		(property "Description" "Single LiPo battery fuel gauge, I2C, type 02, WDFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Battery gauge I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WDFN*1EP*4x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LC709203FQH-03TWG"
		(extends "LC709203FQH-01TWG")
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "LC709203FQH-03TWG"
			(at 11.43 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:WDFN-8-1EP_4x3mm_P0.65mm_EP2.4x1.8mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.onsemi.com/download/data-sheet/pdf/lc709203f-d.pdf"
			(at -1.27 -2.54 0)
		)
		(property "Description" "Single LiPo battery fuel gauge, I2C, type 03, WDFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Battery gauge I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WDFN*1EP*4x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LC709203FQH-04TWG"
		(extends "LC709203FQH-01TWG")
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "LC709203FQH-04TWG"
			(at 11.43 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:WDFN-8-1EP_4x3mm_P0.65mm_EP2.4x1.8mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.onsemi.com/download/data-sheet/pdf/lc709203f-d.pdf"
			(at -1.27 -2.54 0)
		)
		(property "Description" "Single LiPo battery fuel gauge, I2C, type 04, WDFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Battery gauge I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WDFN*1EP*4x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT3652IDD"
		(extends "LT3652EDD")
		(property "Reference" "U"
			(at -8.382 11.43 0)
		)
		(property "Value" "LT3652IDD"
			(at 1.778 11.684 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-12-1EP_3x3mm_P0.45mm_EP1.65x2.38mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3652fe.pdf"
			(at 15.24 -20.32 0)
		)
		(property "Description" "Step-down battery charger for solar power, Lithium Phosphate (LiFePO4), Lead (Pb), Lithium+ (Li+) , 4.95V to 32V VDD, 2A, -40 to +125 degree Celsius, DFN-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery charger solar"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P0.45mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT3652IMSE"
		(extends "LT3652EMSE")
		(property "Reference" "U"
			(at -8.382 11.43 0)
		)
		(property "Value" "LT3652IMSE"
			(at 1.778 11.684 0)
		)
		(property "Footprint" "Package_SO:MSOP-12-1EP_3x4.039mm_P0.65mm_EP1.651x2.845mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3652fe.pdf"
			(at 15.24 -20.32 0)
		)
		(property "Description" "Step-down battery charger for solar power, Lithium Phosphate (LiFePO4), Lead (Pb), Lithium+ (Li+) , 4.95V to 32V VDD, 2A, -40 to +125 degree Celsius, MSOP-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery charger solar"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*1EP*3x4.039mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC2942-1"
		(extends "LTC2942")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LTC2942-1"
			(at 10.16 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6-1EP_3x2mm_P0.5mm_EP1.65x1.35mm"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/29421f.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "1A Battery Gas Gauge with Internal Sense Resistor and Temperature/Voltage Measurement, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Fuel gauge coulomb counter I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC3555-1"
		(extends "LTC3555")
		(property "Reference" "U"
			(at 15.24 -29.21 0)
		)
		(property "Value" "LTC3555-1"
			(at 15.24 29.21 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_4x5mm_P0.5mm_EP2.65x3.65mm"
			(at 0 -1.27 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3555fe.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "High Efficiency USB Power Manager + Triple Step-Down DC/DC, instant-on power, 4.2V float, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB PMIC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC3555-3"
		(extends "LTC3555")
		(property "Reference" "U"
			(at 15.24 -29.21 0)
		)
		(property "Value" "LTC3555-3"
			(at 15.24 29.21 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_4x5mm_P0.5mm_EP2.65x3.65mm"
			(at 0 -1.27 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3555fe.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "High Efficiency USB Power Manager + Triple Step-Down DC/DC, instant-on power, 4.1V float, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB PMIC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC4001-1"
		(extends "LTC4001")
		(property "Reference" "U"
			(at -8.89 16.51 0)
		)
		(property "Value" "LTC4001-1"
			(at 6.35 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_4x4mm_P0.65mm_EP2.15x2.15mm"
			(at 1.27 -19.05 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/40011fa.pdf"
			(at -8.89 16.51 0)
		)
		(property "Description" "Single cell (4.1V) programmable synchronous buck Li-Ion charger, 2A, 5.5V input, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Li-Ion Charger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC4002EDD-8.4"
		(extends "LTC4002EDD-4.2")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "LTC4002EDD-8.4"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-10-1EP_3x3mm_P0.5mm_EP1.55x2.48mm"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/4002f.pdf"
			(at -10.16 8.89 0)
		)
		(property "Description" "Standalone Li-Ion Switch Mode Battery Charger, 8.9-22V input, double cell, DFN-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "lithium li-ion battery charger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*10*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC4002ES8-8.4"
		(extends "LTC4002ES8-4.2")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "LTC4002ES8-8.4"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/4002f.pdf"
			(at -10.16 8.89 0)
		)
		(property "Description" "Standalone Li-Ion Switch Mode Battery Charger, 8.9-22V input, double cell, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "lithium li-ion battery charger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*8*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC4054XES5-4.2"
		(extends "LTC4054ES5-4.2")
		(property "Reference" "U"
			(at -5.842 6.604 0)
		)
		(property "Value" "LTC4054XES5-4.2"
			(at 1.524 6.604 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/405442xf.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "Constant-current/constant-voltage linear charger for single cell lithium-ion batteries no Trickle Charge, 4.5V to 6.5V VDD, -40 to +85 degree Celsius, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Constant-current constant-voltage linear charger single cell lithium-ion battery"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LTC4055-1"
		(extends "LTC4055")
		(property "Reference" "U"
			(at -6.35 13.97 0)
		)
		(property "Value" "LTC4055-1"
			(at 3.81 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_4x4mm_P0.65mm_EP2.15x2.15mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/4055fb.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "USB Power Controller and Li-Ion Charger (4.1V Float Voltage)"
			(at 0 0 0)
		)
		(property "ki_keywords" "charger PMIC Liion USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX1873SEEE"
		(extends "MAX1873REEE")
		(property "Reference" "U"
			(at -6.096 13.97 0)
		)
		(property "Value" "MAX1873SEEE"
			(at 2.286 13.97 0)
		)
		(property "Footprint" "Package_SO:QSOP-16_3.9x4.9mm_P0.635mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX1873.pdf"
			(at 5.08 0 0)
		)
		(property "Description" "Charger for 3 lithium-ion (Li+), 7/9 NickelCadium (NiCD) cells or 7/9 NickelMetalHydride (NiMH), 9 to 28V VDD, -40 to +85 degree Celsius, QSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "li-ion battery charger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX1873TEEE"
		(extends "MAX1873REEE")
		(property "Reference" "U"
			(at -6.096 13.97 0)
		)
		(property "Value" "MAX1873TEEE"
			(at 2.286 13.97 0)
		)
		(property "Footprint" "Package_SO:QSOP-16_3.9x4.9mm_P0.635mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX1873.pdf"
			(at 5.08 0 0)
		)
		(property "Description" "Charger for 4 lithium-ion (Li+), 10 NickelCadium (NiCD) cells or 10 NickelMetalHydride (NiMH), 9 to 28V VDD, -40 to +85 degree Celsius, QSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "li-ion battery charger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX712EPE"
		(extends "MAX712CPE")
		(property "Reference" "U"
			(at -8.382 13.97 0)
		)
		(property "Value" "MAX712EPE"
			(at 2.54 13.97 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 15.24 -13.97 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX712-MAX713.pdf"
			(at -17.78 5.08 0)
		)
		(property "Description" "Fast-charge Nickel Metal Hydride (NiMH) from a DC source, -40 to +85 Degree Celsius, PDIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery charger controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX712ESE"
		(extends "MAX712CSE")
		(property "Reference" "U"
			(at -8.382 13.97 0)
		)
		(property "Value" "MAX712ESE"
			(at 2.54 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX712-MAX713.pdf"
			(at -17.78 5.08 0)
		)
		(property "Description" "Fast-charge Nickel Metal Hydride (NiMH) from a DC source, -40 to +85 Degree Celsius, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery charger controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX712MJE"
		(extends "MAX712CPE")
		(property "Reference" "U"
			(at -8.382 13.97 0)
		)
		(property "Value" "MAX712MJE"
			(at 2.54 13.97 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 15.24 -13.97 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX712-MAX713.pdf"
			(at -17.78 5.08 0)
		)
		(property "Description" "Fast-charge Nickel Metal Hydride (NiMH) from a DC source, ceramic, -55 to +125 Degree Celsius, PDIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery charger controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX713CPE"
		(extends "MAX712CPE")
		(property "Reference" "U"
			(at -8.382 13.97 0)
		)
		(property "Value" "MAX713CPE"
			(at 2.54 13.97 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 15.24 -13.97 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX712-MAX713.pdf"
			(at -17.78 5.08 0)
		)
		(property "Description" "Fast-charge Nickel Cadmium (NiCd) from a DC source, 0 to +70 Degree Celsius, PDIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery charger controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX713CSE"
		(extends "MAX712CSE")
		(property "Reference" "U"
			(at -8.382 13.97 0)
		)
		(property "Value" "MAX713CSE"
			(at 2.54 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX712-MAX713.pdf"
			(at -17.78 5.08 0)
		)
		(property "Description" "Fast-charge Nickel Cadmium (NiCd) from a DC source, 0 to +70 Degree Celsius, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery charger controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX713EPE"
		(extends "MAX712CPE")
		(property "Reference" "U"
			(at -8.382 13.97 0)
		)
		(property "Value" "MAX713EPE"
			(at 2.54 13.97 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 15.24 -13.97 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX712-MAX713.pdf"
			(at -17.78 5.08 0)
		)
		(property "Description" "Fast-charge Nickel Cadmium (NiCd) from a DC source, -40 to +85 Degree Celsius, PDIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery charger controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX713ESE"
		(extends "MAX712CSE")
		(property "Reference" "U"
			(at -8.382 13.97 0)
		)
		(property "Value" "MAX713ESE"
			(at 2.54 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX712-MAX713.pdf"
			(at -17.78 5.08 0)
		)
		(property "Description" "Fast-charge Nickel Cadmium (NiCd) from a DC source, -40 to +85 Degree Celsius, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery charger controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX713MJE"
		(extends "MAX712CPE")
		(property "Reference" "U"
			(at -8.382 13.97 0)
		)
		(property "Value" "MAX713MJE"
			(at 2.54 13.97 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 15.24 -13.97 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX712-MAX713.pdf"
			(at -17.78 5.08 0)
		)
		(property "Description" "Fast-charge Nickel Cadmium (NiCd) from a DC source, ceramic, -55 to +125 Degree Celsius, PDIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery charger controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP73811T-420I-OT"
		(extends "MCP73812T-420I-OT")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MCP73811T-420I-OT"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22036b.pdf"
			(at -6.35 6.35 0)
		)
		(property "Description" "Simple, Miniature Single-Cell, Fully Integrated Li-Ion / Li-Polymer Charge Management Controllers, 85mA/450mA, 4.2V, SOT23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lithium-Ion Battery Charger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP73811T-435I-OT"
		(extends "MCP73812T-420I-OT")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MCP73811T-435I-OT"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22036b.pdf"
			(at -6.35 6.35 0)
		)
		(property "Description" "Simple, Miniature Single-Cell, Fully Integrated Li-Ion / Li-Polymer Charge Management Controllers, 85mA/450mA, 4.35V, SOT23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lithium-Ion Battery Charger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP73812T-435I-OT"
		(extends "MCP73812T-420I-OT")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MCP73812T-435I-OT"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22036b.pdf"
			(at -6.35 6.35 0)
		)
		(property "Description" "Simple, Miniature Single-Cell, Fully Integrated Li-Ion / Li-Polymer Charge Management Controllers, 50mA-500mA, 4.35V, SOT23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lithium-Ion Battery Charger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP73831-3-MC"
		(extends "MCP73831-2-MC")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MCP73831-3-MC"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.7x1.4mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001984g.pdf"
			(at -3.81 -1.27 0)
		)
		(property "Description" "Single cell, Li-Ion/Li-Po charge management controller, 4.35V, Tri-State Status Output, in DFN-8 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery charger lithium"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x2mm*P0.5mm*EP1.7x1.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP73831-3-OT"
		(extends "MCP73831-2-OT")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MCP73831-3-OT"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001984g.pdf"
			(at -3.81 -1.27 0)
		)
		(property "Description" "Single cell, Li-Ion/Li-Po charge management controller, 4.35V, Tri-State Status Output, in SOT23-5 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery charger lithium"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP73831-4-MC"
		(extends "MCP73831-2-MC")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MCP73831-4-MC"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.7x1.4mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001984g.pdf"
			(at -3.81 -1.27 0)
		)
		(property "Description" "Single cell, Li-Ion/Li-Po charge management controller, 4.40V, Tri-State Status Output, in DFN-8 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery charger lithium"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x2mm*P0.5mm*EP1.7x1.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP73831-4-OT"
		(extends "MCP73831-2-OT")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MCP73831-4-OT"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001984g.pdf"
			(at -3.81 -1.27 0)
		)
		(property "Description" "Single cell, Li-Ion/Li-Po charge management controller, 4.40V, Tri-State Status Output, in SOT23-5 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery charger lithium"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP73831-5-MC"
		(extends "MCP73831-2-MC")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MCP73831-5-MC"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.7x1.4mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001984g.pdf"
			(at -3.81 -1.27 0)
		)
		(property "Description" "Single cell, Li-Ion/Li-Po charge management controller, 4.50V, Tri-State Status Output, in DFN-8 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery charger lithium"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x2mm*P0.5mm*EP1.7x1.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP73831-5-OT"
		(extends "MCP73831-2-OT")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MCP73831-5-OT"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001984g.pdf"
			(at -3.81 -1.27 0)
		)
		(property "Description" "Single cell, Li-Ion/Li-Po charge management controller, 4.50V, Tri-State Status Output, in SOT23-5 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery charger lithium"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP73832-3-MC"
		(extends "MCP73832-2-MC")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MCP73832-3-MC"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.7x1.4mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001984g.pdf"
			(at -3.81 -1.27 0)
		)
		(property "Description" "Single cell, Li-Ion/Li-Po charge management controller, 4.35V, Open-Drain Status Output, in DFN-8 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery charger lithium"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x2mm*P0.5mm*EP1.7x1.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP73832-3-OT"
		(extends "MCP73832-2-OT")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MCP73832-3-OT"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001984g.pdf"
			(at -3.81 -1.27 0)
		)
		(property "Description" "Single cell, Li-Ion/Li-Po charge management controller, 4.35V, Open-Drain Status Output, in SOT23-5 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery charger lithium"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP73832-4-MC"
		(extends "MCP73832-2-MC")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MCP73832-4-MC"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.7x1.4mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001984g.pdf"
			(at -3.81 -1.27 0)
		)
		(property "Description" "Single cell, Li-Ion/Li-Po charge management controller, 4.40V, Open-Drain Status Output, in DFN-8 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery charger lithium"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x2mm*P0.5mm*EP1.7x1.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP73832-4-OT"
		(extends "MCP73832-2-OT")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MCP73832-4-OT"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001984g.pdf"
			(at -3.81 -1.27 0)
		)
		(property "Description" "Single cell, Li-Ion/Li-Po charge management controller, 4.40V, Open-Drain Status Output, in SOT23-5 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery charger lithium"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP73832-5-MC"
		(extends "MCP73832-2-MC")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MCP73832-5-MC"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.7x1.4mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001984g.pdf"
			(at -3.81 -1.27 0)
		)
		(property "Description" "Single cell, Li-Ion/Li-Po charge management controller, 4.50V, Open-Drain Status Output, in DFN-8 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery charger lithium"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x2mm*P0.5mm*EP1.7x1.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP73832-5-OT"
		(extends "MCP73832-2-OT")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MCP73832-5-OT"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001984g.pdf"
			(at -3.81 -1.27 0)
		)
		(property "Description" "Single cell, Li-Ion/Li-Po charge management controller, 4.50V, Open-Drain Status Output, in SOT23-5 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery charger lithium"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP73871-1AA"
		(extends "MCP73871")
		(property "Reference" "U"
			(at -7.62 24.13 0)
		)
		(property "Value" "MCP73871-1AA"
			(at -15.24 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.5x2.5mm"
			(at 5.08 -22.86 0)
		)
		(property "Datasheet" "http://www.mouser.com/ds/2/268/22090a-52174.pdf"
			(at -3.81 13.97 0)
		)
		(property "Description" "Single cell, Li-Ion/Li-Po charge management controller, 4.10V"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery charger lithium"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP73871-1CA"
		(extends "MCP73871")
		(property "Reference" "U"
			(at -7.62 24.13 0)
		)
		(property "Value" "MCP73871-1CA"
			(at -15.24 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.5x2.5mm"
			(at 5.08 -22.86 0)
		)
		(property "Datasheet" "http://www.mouser.com/ds/2/268/22090a-52174.pdf"
			(at -3.81 13.97 0)
		)
		(property "Description" "Single cell, Li-Ion/Li-Po charge management controller, 4.10V, 6h safety timer"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery charger lithium"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP73871-1CC"
		(extends "MCP73871")
		(property "Reference" "U"
			(at -7.62 24.13 0)
		)
		(property "Value" "MCP73871-1CC"
			(at -15.24 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.5x2.5mm"
			(at 5.08 -22.86 0)
		)
		(property "Datasheet" "http://www.mouser.com/ds/2/268/22090a-52174.pdf"
			(at -3.81 13.97 0)
		)
		(property "Description" "Single cell, Li-Ion/Li-Po charge management controller, 4.10V, 6h safety timer, 3.1V LBO threshold"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery charger lithium"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP73871-2AA"
		(extends "MCP73871")
		(property "Reference" "U"
			(at -7.62 24.13 0)
		)
		(property "Value" "MCP73871-2AA"
			(at -15.24 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.5x2.5mm"
			(at 5.08 -22.86 0)
		)
		(property "Datasheet" "http://www.mouser.com/ds/2/268/22090a-52174.pdf"
			(at -3.81 13.97 0)
		)
		(property "Description" "Single cell, Li-Ion/Li-Po charge management controller, 4.20V"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery charger lithium"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP73871-2CA"
		(extends "MCP73871")
		(property "Reference" "U"
			(at -7.62 24.13 0)
		)
		(property "Value" "MCP73871-2CA"
			(at -15.24 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.5x2.5mm"
			(at 5.08 -22.86 0)
		)
		(property "Datasheet" "http://www.mouser.com/ds/2/268/22090a-52174.pdf"
			(at -3.81 13.97 0)
		)
		(property "Description" "Single cell, Li-Ion/Li-Po charge management controller, 4.20V, 6h safety timer"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery charger lithium"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP73871-2CC"
		(extends "MCP73871")
		(property "Reference" "U"
			(at -7.62 24.13 0)
		)
		(property "Value" "MCP73871-2CC"
			(at -15.24 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.5x2.5mm"
			(at 5.08 -22.86 0)
		)
		(property "Datasheet" "http://www.mouser.com/ds/2/268/22090a-52174.pdf"
			(at -3.81 13.97 0)
		)
		(property "Description" "Single cell, Li-Ion/Li-Po charge management controller, 4.20V, 6h safety timer, 3.1V LBO threshold"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery charger lithium"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP73871-3CA"
		(extends "MCP73871")
		(property "Reference" "U"
			(at -7.62 24.13 0)
		)
		(property "Value" "MCP73871-3CA"
			(at -15.24 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.5x2.5mm"
			(at 5.08 -22.86 0)
		)
		(property "Datasheet" "http://www.mouser.com/ds/2/268/22090a-52174.pdf"
			(at -3.81 13.97 0)
		)
		(property "Description" "Single cell, Li-Ion/Li-Po charge management controller, 4.35V, 6h safety timer"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery charger lithium"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP73871-3CC"
		(extends "MCP73871")
		(property "Reference" "U"
			(at -7.62 24.13 0)
		)
		(property "Value" "MCP73871-3CC"
			(at -15.24 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.5x2.5mm"
			(at 5.08 -22.86 0)
		)
		(property "Datasheet" "http://www.mouser.com/ds/2/268/22090a-52174.pdf"
			(at -3.81 13.97 0)
		)
		(property "Description" "Single cell, Li-Ion/Li-Po charge management controller, 4.35V, 6h safety timer, 3.1V LBO threshold"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery charger lithium"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP73871-4CA"
		(extends "MCP73871")
		(property "Reference" "U"
			(at -7.62 24.13 0)
		)
		(property "Value" "MCP73871-4CA"
			(at -15.24 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.5x2.5mm"
			(at 5.08 -22.86 0)
		)
		(property "Datasheet" "http://www.mouser.com/ds/2/268/22090a-52174.pdf"
			(at -3.81 13.97 0)
		)
		(property "Description" "Single cell, Li-Ion/Li-Po charge management controller, 4.40V, 6h safety timer"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery charger lithium"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP73871-4CC"
		(extends "MCP73871")
		(property "Reference" "U"
			(at -7.62 24.13 0)
		)
		(property "Value" "MCP73871-4CC"
			(at -15.24 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.5x2.5mm"
			(at 5.08 -22.86 0)
		)
		(property "Datasheet" "http://www.mouser.com/ds/2/268/22090a-52174.pdf"
			(at -3.81 13.97 0)
		)
		(property "Description" "Single cell, Li-Ion/Li-Po charge management controller, 4.40V, 6h safety timer, 3.1V LBO threshold"
			(at 0 0 0)
		)
		(property "ki_keywords" "battery charger lithium"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
)
