(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "CDCV304"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "CDCV304"
			(at 6.35 8.89 0)
		)
		(property "Footprint" "Package_SO:TSSOP-8_4.4x3mm_P0.65mm"
			(at 5.08 -12.7 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/cdcv304.pdf"
			(at 5.08 -15.24 0)
		)
		(property "Description" "0-200 MHz 1:4 Clock Buffer, PCI-X Compliant, TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "texas quadruple"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "CDCV304_0_1")
		(symbol "CDCV304_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "OE")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "CLKIN")
				(number "1")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V_{DD}")
				(number "6")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "1Y0")
				(number "3")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "1Y1")
				(number "5")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "1Y2")
				(number "7")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "1Y3")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PI6C5946002ZH"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.89 11.43 0)
		)
		(property "Value" "PI6C5946002ZH"
			(at -8.89 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:TQFN-16-1EP_3x3mm_P0.5mm_EP1.6x1.6mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/PI6C5946002.pdf"
			(at 0 -17.78 0)
		)
		(property "Description" "6 GHz / 12 Gbps Clock / Data 1:2 Fanout Buffer with Internal Termination, TQFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "buffer clock data"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "PI6C5946002ZH_0_1")
		(symbol "PI6C5946002ZH_1_1"
			(pin output line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "VREF-AC")
				(number "10")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "REF_IN+")
				(number "12")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "VTH")
				(number "11")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "REF_IN-")
				(number "9")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "EN")
				(number "8")
			)
			(pin no_connect line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "5")
			)
			(pin no_connect line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "6")
			)
			(pin passive line
				(at 0 12.7 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin no_connect line
				(at 10.16 7.62 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "16")
			)
			(pin no_connect line
				(at 10.16 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "15")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "Q0+")
				(number "1")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "Q0-")
				(number "2")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "Q1+")
				(number "3")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "Q1-")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
)
