(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "EP1210"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 34.925 0)
		)
		(property "Value" "EP1210"
			(at -5.08 33.02 0)
		)
		(property "Footprint" ""
			(at 1.27 -33.02 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "EPLD"
			(at 0 0 0)
		)
		(property "ki_keywords" "EPLD"
			(at 0 0 0)
		)
		(symbol "EP1210_0_1")
		(symbol "EP1210_1_1"
			(pin input clock
				(at -20.32 27.94 0)
				(length 3.81)
				(name "CLK1")
				(number "1")
			)
			(pin input line
				(at -20.32 22.86 0)
				(length 3.81)
				(name "I0")
				(number "2")
			)
			(pin input line
				(at -20.32 20.32 0)
				(length 3.81)
				(name "I1")
				(number "3")
			)
			(pin input line
				(at -20.32 17.78 0)
				(length 3.81)
				(name "I2")
				(number "4")
			)
			(pin input line
				(at -20.32 15.24 0)
				(length 3.81)
				(name "I3")
				(number "5")
			)
			(pin input line
				(at -20.32 12.7 0)
				(length 3.81)
				(name "I4")
				(number "6")
			)
			(pin input line
				(at -20.32 10.16 0)
				(length 3.81)
				(name "I5")
				(number "7")
			)
			(pin input line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "B10")
				(number "8")
			)
			(pin input line
				(at -20.32 2.54 0)
				(length 3.81)
				(name "B11")
				(number "9")
			)
			(pin input line
				(at -20.32 0 0)
				(length 3.81)
				(name "B12")
				(number "10")
			)
			(pin input line
				(at -20.32 -2.54 0)
				(length 3.81)
				(name "B13")
				(number "11")
			)
			(pin input line
				(at -20.32 -7.62 0)
				(length 3.81)
				(name "B20")
				(number "12")
			)
			(pin input line
				(at -20.32 -10.16 0)
				(length 3.81)
				(name "B21")
				(number "13")
			)
			(pin input line
				(at -20.32 -12.7 0)
				(length 3.81)
				(name "B22")
				(number "14")
			)
			(pin input line
				(at -20.32 -15.24 0)
				(length 3.81)
				(name "B23")
				(number "15")
			)
			(pin input line
				(at -20.32 -20.32 0)
				(length 3.81)
				(name "B30")
				(number "16")
			)
			(pin input line
				(at -20.32 -22.86 0)
				(length 3.81)
				(name "B31")
				(number "17")
			)
			(pin input line
				(at -20.32 -25.4 0)
				(length 3.81)
				(name "B32")
				(number "18")
			)
			(pin input line
				(at -20.32 -27.94 0)
				(length 3.81)
				(name "B33")
				(number "19")
			)
			(pin power_in line
				(at -2.54 35.56 270)
				(length 3.81)
				(name "VCC")
				(number "40")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 3.81)
				(name "GND")
				(number "20")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 3.81)
				(name "VCC")
				(number "39")
			)
			(pin input line
				(at 20.32 22.86 180)
				(length 3.81)
				(name "I6")
				(number "38")
			)
			(pin input line
				(at 20.32 20.32 180)
				(length 3.81)
				(name "I7")
				(number "37")
			)
			(pin input line
				(at 20.32 17.78 180)
				(length 3.81)
				(name "I8")
				(number "36")
			)
			(pin input line
				(at 20.32 15.24 180)
				(length 3.81)
				(name "I9")
				(number "35")
			)
			(pin input line
				(at 20.32 12.7 180)
				(length 3.81)
				(name "I10")
				(number "34")
			)
			(pin input line
				(at 20.32 10.16 180)
				(length 3.81)
				(name "I11")
				(number "33")
			)
			(pin input line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "A10")
				(number "32")
			)
			(pin input line
				(at 20.32 2.54 180)
				(length 3.81)
				(name "A11")
				(number "31")
			)
			(pin input line
				(at 20.32 0 180)
				(length 3.81)
				(name "A12")
				(number "30")
			)
			(pin input line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "A13")
				(number "29")
			)
			(pin input line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "A20")
				(number "28")
			)
			(pin input line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "A21")
				(number "27")
			)
			(pin input line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "A22")
				(number "26")
			)
			(pin input line
				(at 20.32 -15.24 180)
				(length 3.81)
				(name "A23")
				(number "25")
			)
			(pin input line
				(at 20.32 -20.32 180)
				(length 3.81)
				(name "A30")
				(number "24")
			)
			(pin input line
				(at 20.32 -22.86 180)
				(length 3.81)
				(name "A31")
				(number "23")
			)
			(pin input line
				(at 20.32 -25.4 180)
				(length 3.81)
				(name "A32")
				(number "22")
			)
			(pin input line
				(at 20.32 -27.94 180)
				(length 3.81)
				(name "A33")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EP1810"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 47.625 0)
		)
		(property "Value" "EP1810"
			(at -5.08 45.72 0)
		)
		(property "Footprint" ""
			(at 3.81 -43.18 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "EPLD"
			(at 0 0 0)
		)
		(property "ki_keywords" "EPLD"
			(at 0 0 0)
		)
		(symbol "EP1810_0_1")
		(symbol "EP1810_1_1"
			(pin input line
				(at -25.4 43.18 0)
				(length 3.81)
				(name "I/O_1A")
				(number "2")
			)
			(pin input line
				(at -25.4 40.64 0)
				(length 3.81)
				(name "I/O_2A")
				(number "3")
			)
			(pin input line
				(at -25.4 38.1 0)
				(length 3.81)
				(name "I/O_3A")
				(number "4")
			)
			(pin input line
				(at -25.4 35.56 0)
				(length 3.81)
				(name "I/O_4A")
				(number "5")
			)
			(pin input line
				(at -25.4 33.02 0)
				(length 3.81)
				(name "I/O_5A")
				(number "6")
			)
			(pin input line
				(at -25.4 30.48 0)
				(length 3.81)
				(name "I/O_6A")
				(number "7")
			)
			(pin input line
				(at -25.4 27.94 0)
				(length 3.81)
				(name "I/O_7A")
				(number "8")
			)
			(pin input line
				(at -25.4 25.4 0)
				(length 3.81)
				(name "I/O_8A")
				(number "9")
			)
			(pin input line
				(at -25.4 22.86 0)
				(length 3.81)
				(name "I/O_9A")
				(number "10")
			)
			(pin input line
				(at -25.4 20.32 0)
				(length 3.81)
				(name "I/O_10A")
				(number "11")
			)
			(pin input line
				(at -25.4 17.78 0)
				(length 3.81)
				(name "I/O_11A")
				(number "12")
			)
			(pin input line
				(at -25.4 15.24 0)
				(length 3.81)
				(name "I/O_12A")
				(number "13")
			)
			(pin input line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "INP1")
				(number "14")
			)
			(pin input line
				(at -25.4 7.62 0)
				(length 3.81)
				(name "INP2")
				(number "15")
			)
			(pin input line
				(at -25.4 5.08 0)
				(length 3.81)
				(name "INP3")
				(number "16")
			)
			(pin input line
				(at -25.4 2.54 0)
				(length 3.81)
				(name "INP4/CLK1")
				(number "17")
			)
			(pin input line
				(at -25.4 0 0)
				(length 3.81)
				(name "INP5/CLK2")
				(number "19")
			)
			(pin input line
				(at -25.4 -2.54 0)
				(length 3.81)
				(name "INP6")
				(number "20")
			)
			(pin input line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "INP7")
				(number "21")
			)
			(pin input line
				(at -25.4 -7.62 0)
				(length 3.81)
				(name "INP8")
				(number "22")
			)
			(pin input line
				(at -25.4 -12.7 0)
				(length 3.81)
				(name "I/O_13B")
				(number "23")
			)
			(pin input line
				(at -25.4 -15.24 0)
				(length 3.81)
				(name "I/O_14B")
				(number "24")
			)
			(pin input line
				(at -25.4 -17.78 0)
				(length 3.81)
				(name "I/O_15B")
				(number "25")
			)
			(pin input line
				(at -25.4 -20.32 0)
				(length 3.81)
				(name "I/O_16B")
				(number "26")
			)
			(pin input line
				(at -25.4 -22.86 0)
				(length 3.81)
				(name "I/O_17B")
				(number "27")
			)
			(pin input line
				(at -25.4 -25.4 0)
				(length 3.81)
				(name "I/O_18B")
				(number "28")
			)
			(pin input line
				(at -25.4 -27.94 0)
				(length 3.81)
				(name "I/O_19B")
				(number "29")
			)
			(pin input line
				(at -25.4 -30.48 0)
				(length 3.81)
				(name "I/O_20B")
				(number "30")
			)
			(pin input line
				(at -25.4 -33.02 0)
				(length 3.81)
				(name "I/O_21B")
				(number "31")
			)
			(pin input line
				(at -25.4 -35.56 0)
				(length 3.81)
				(name "I/O_22B")
				(number "32")
			)
			(pin input line
				(at -25.4 -38.1 0)
				(length 3.81)
				(name "I/O_23B")
				(number "33")
			)
			(pin input line
				(at -25.4 -40.64 0)
				(length 3.81)
				(name "I/O_24B")
				(number "34")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 3.81)
				(name "VCC")
				(number "18")
			)
			(pin power_in line
				(at -2.54 -45.72 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 3.81)
				(name "VCC")
				(number "52")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 3.81)
				(name "GND")
				(number "35")
			)
			(pin input line
				(at 25.4 43.18 180)
				(length 3.81)
				(name "I/O_48D")
				(number "68")
			)
			(pin input line
				(at 25.4 40.64 180)
				(length 3.81)
				(name "I/O_47D")
				(number "67")
			)
			(pin input line
				(at 25.4 38.1 180)
				(length 3.81)
				(name "I/O_46D")
				(number "66")
			)
			(pin input line
				(at 25.4 35.56 180)
				(length 3.81)
				(name "I/O_45D")
				(number "65")
			)
			(pin input line
				(at 25.4 33.02 180)
				(length 3.81)
				(name "I/O_44D")
				(number "64")
			)
			(pin input line
				(at 25.4 30.48 180)
				(length 3.81)
				(name "I/O_43D")
				(number "63")
			)
			(pin input line
				(at 25.4 27.94 180)
				(length 3.81)
				(name "I/O_42D")
				(number "62")
			)
			(pin input line
				(at 25.4 25.4 180)
				(length 3.81)
				(name "I/O_41D")
				(number "61")
			)
			(pin input line
				(at 25.4 22.86 180)
				(length 3.81)
				(name "I/O_40D")
				(number "60")
			)
			(pin input line
				(at 25.4 20.32 180)
				(length 3.81)
				(name "I/O_39D")
				(number "59")
			)
			(pin input line
				(at 25.4 17.78 180)
				(length 3.81)
				(name "I/O_38D")
				(number "58")
			)
			(pin input line
				(at 25.4 15.24 180)
				(length 3.81)
				(name "I/O_37D")
				(number "57")
			)
			(pin input line
				(at 25.4 10.16 180)
				(length 3.81)
				(name "INP16")
				(number "56")
			)
			(pin input line
				(at 25.4 7.62 180)
				(length 3.81)
				(name "INP15")
				(number "55")
			)
			(pin input line
				(at 25.4 5.08 180)
				(length 3.81)
				(name "INP14")
				(number "54")
			)
			(pin input line
				(at 25.4 2.54 180)
				(length 3.81)
				(name "CLK4/INP13")
				(number "53")
			)
			(pin input line
				(at 25.4 0 180)
				(length 3.81)
				(name "CLK3/INP12")
				(number "51")
			)
			(pin input line
				(at 25.4 -2.54 180)
				(length 3.81)
				(name "INP11")
				(number "50")
			)
			(pin input line
				(at 25.4 -5.08 180)
				(length 3.81)
				(name "INP10")
				(number "49")
			)
			(pin input line
				(at 25.4 -7.62 180)
				(length 3.81)
				(name "INP9")
				(number "48")
			)
			(pin input line
				(at 25.4 -12.7 180)
				(length 3.81)
				(name "I/O_36C")
				(number "47")
			)
			(pin input line
				(at 25.4 -15.24 180)
				(length 3.81)
				(name "I/O_35C")
				(number "46")
			)
			(pin input line
				(at 25.4 -17.78 180)
				(length 3.81)
				(name "I/O_34C")
				(number "45")
			)
			(pin input line
				(at 25.4 -20.32 180)
				(length 3.81)
				(name "I/O_33C")
				(number "44")
			)
			(pin input line
				(at 25.4 -22.86 180)
				(length 3.81)
				(name "I/O_32C")
				(number "43")
			)
			(pin input line
				(at 25.4 -25.4 180)
				(length 3.81)
				(name "I/O_31C")
				(number "42")
			)
			(pin input line
				(at 25.4 -27.94 180)
				(length 3.81)
				(name "I/O_30C")
				(number "41")
			)
			(pin input line
				(at 25.4 -30.48 180)
				(length 3.81)
				(name "I/O_29C")
				(number "40")
			)
			(pin input line
				(at 25.4 -33.02 180)
				(length 3.81)
				(name "I/O_28C")
				(number "39")
			)
			(pin input line
				(at 25.4 -35.56 180)
				(length 3.81)
				(name "I/O_27C")
				(number "38")
			)
			(pin input line
				(at 25.4 -38.1 180)
				(length 3.81)
				(name "I/O_26C")
				(number "37")
			)
			(pin input line
				(at 25.4 -40.64 180)
				(length 3.81)
				(name "I/O_25C")
				(number "36")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EP300"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 17.145 0)
		)
		(property "Value" "EP300"
			(at -2.54 15.24 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at 1.27 -15.24 0)
		)
		(property "Datasheet" "~"
			(at 0 -1.27 0)
		)
		(property "Description" "EPLD, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "EPLD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "EP300_0_1")
		(symbol "EP300_1_1"
			(pin input line
				(at -12.7 12.7 0)
				(length 3.81)
				(name "CLK")
				(number "1")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 3.81)
				(name "IN1")
				(number "2")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 3.81)
				(name "IN2")
				(number "3")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 3.81)
				(name "IN3")
				(number "4")
			)
			(pin input line
				(at -12.7 0 0)
				(length 3.81)
				(name "IN4")
				(number "5")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 3.81)
				(name "IN5")
				(number "6")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 3.81)
				(name "IN6")
				(number "7")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 3.81)
				(name "IN7")
				(number "8")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 3.81)
				(name "IN9")
				(number "9")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 3.81)
				(name "IN10")
				(number "11")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 3.81)
				(name "GND")
				(number "10")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 3.81)
				(name "IO8")
				(number "19")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 3.81)
				(name "IO7")
				(number "18")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 3.81)
				(name "IO6")
				(number "17")
			)
			(pin input line
				(at 12.7 0 180)
				(length 3.81)
				(name "IO5")
				(number "16")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 3.81)
				(name "IO4")
				(number "15")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 3.81)
				(name "IO3")
				(number "14")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 3.81)
				(name "IO2")
				(number "13")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 3.81)
				(name "IO1")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EP320"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 17.145 0)
		)
		(property "Value" "EP320"
			(at -2.54 15.24 0)
		)
		(property "Footprint" ""
			(at 1.27 -15.24 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "EPLD"
			(at 0 0 0)
		)
		(property "ki_keywords" "EPLD"
			(at 0 0 0)
		)
		(symbol "EP320_0_1")
		(symbol "EP320_1_1"
			(pin input line
				(at -15.24 10.16 0)
				(length 3.81)
				(name "CK/IN")
				(number "1")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "IN2")
				(number "2")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "IN3")
				(number "3")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "IN4")
				(number "4")
			)
			(pin input line
				(at -15.24 0 0)
				(length 3.81)
				(name "IN5")
				(number "5")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "IN6")
				(number "6")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 3.81)
				(name "IN7")
				(number "7")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 3.81)
				(name "IN8")
				(number "8")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 3.81)
				(name "IN9")
				(number "9")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 3.81)
				(name "GND")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 3.81)
				(name "I/O11")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 3.81)
				(name "I/O12")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "I/O13")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 3.81)
				(name "I/O14")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 3.81)
				(name "I/O15")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 3.81)
				(name "I/O16")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 3.81)
				(name "I/O17")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 3.81)
				(name "I/O18")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 3.81)
				(name "I/O19")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EP600"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 24.765 0)
		)
		(property "Value" "EP600"
			(at -2.54 22.86 0)
		)
		(property "Footprint" ""
			(at 1.27 -20.32 0)
		)
		(property "Datasheet" "~"
			(at 0 1.27 0)
		)
		(property "Description" "EPLD"
			(at 0 0 0)
		)
		(property "ki_keywords" "EPLD"
			(at 0 0 0)
		)
		(symbol "EP600_0_1")
		(symbol "EP600_1_1"
			(pin input clock
				(at -15.24 17.78 0)
				(length 3.81)
				(name "CLK1")
				(number "1")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 3.81)
				(name "IN2")
				(number "2")
			)
			(pin passive line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "I/O3")
				(number "3")
			)
			(pin passive line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "I/O4")
				(number "4")
			)
			(pin passive line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "I/O5")
				(number "5")
			)
			(pin passive line
				(at -15.24 0 0)
				(length 3.81)
				(name "I/O6")
				(number "6")
			)
			(pin passive line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "I/O7")
				(number "7")
			)
			(pin passive line
				(at -15.24 -5.08 0)
				(length 3.81)
				(name "I/O8")
				(number "8")
			)
			(pin passive line
				(at -15.24 -7.62 0)
				(length 3.81)
				(name "I/O9")
				(number "9")
			)
			(pin passive line
				(at -15.24 -10.16 0)
				(length 3.81)
				(name "I/O10")
				(number "10")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 3.81)
				(name "IN11")
				(number "11")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 3.81)
				(name "VCC")
				(number "24")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 3.81)
				(name "GND")
				(number "12")
			)
			(pin input line
				(at 15.24 17.78 180)
				(length 3.81)
				(name "IN23")
				(number "23")
			)
			(pin passive line
				(at 15.24 12.7 180)
				(length 3.81)
				(name "I/O22")
				(number "22")
			)
			(pin passive line
				(at 15.24 10.16 180)
				(length 3.81)
				(name "I/O21")
				(number "21")
			)
			(pin passive line
				(at 15.24 7.62 180)
				(length 3.81)
				(name "I/O20")
				(number "20")
			)
			(pin passive line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "I/O19")
				(number "19")
			)
			(pin passive line
				(at 15.24 2.54 180)
				(length 3.81)
				(name "I/O18")
				(number "18")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(name "I/O17")
				(number "17")
			)
			(pin passive line
				(at 15.24 -2.54 180)
				(length 3.81)
				(name "I/O16")
				(number "16")
			)
			(pin passive line
				(at 15.24 -5.08 180)
				(length 3.81)
				(name "I/O15")
				(number "15")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 3.81)
				(name "IN14")
				(number "14")
			)
			(pin input clock
				(at 15.24 -15.24 180)
				(length 3.81)
				(name "CLK2")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EP910"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 32.385 0)
		)
		(property "Value" "EP910"
			(at -2.54 30.48 0)
		)
		(property "Footprint" ""
			(at 1.27 -33.02 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "EPLD"
			(at 0 0 0)
		)
		(property "ki_keywords" "EPLD"
			(at 0 0 0)
		)
		(symbol "EP910_0_1")
		(symbol "EP910_1_1"
			(pin input clock
				(at -20.32 27.94 0)
				(length 3.81)
				(name "CLK1")
				(number "1")
			)
			(pin input line
				(at -20.32 22.86 0)
				(length 3.81)
				(name "I0")
				(number "2")
			)
			(pin input line
				(at -20.32 20.32 0)
				(length 3.81)
				(name "I1")
				(number "3")
			)
			(pin input line
				(at -20.32 17.78 0)
				(length 3.81)
				(name "I2")
				(number "4")
			)
			(pin input line
				(at -20.32 12.7 0)
				(length 3.81)
				(name "IO0")
				(number "5")
			)
			(pin input line
				(at -20.32 10.16 0)
				(length 3.81)
				(name "IO1")
				(number "6")
			)
			(pin input line
				(at -20.32 7.62 0)
				(length 3.81)
				(name "IO2")
				(number "7")
			)
			(pin input line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "IO3")
				(number "8")
			)
			(pin input line
				(at -20.32 2.54 0)
				(length 3.81)
				(name "IO4")
				(number "9")
			)
			(pin input line
				(at -20.32 0 0)
				(length 3.81)
				(name "IO5")
				(number "10")
			)
			(pin input line
				(at -20.32 -2.54 0)
				(length 3.81)
				(name "IO6")
				(number "11")
			)
			(pin input line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "IO7")
				(number "12")
			)
			(pin input line
				(at -20.32 -7.62 0)
				(length 3.81)
				(name "IO8")
				(number "13")
			)
			(pin input line
				(at -20.32 -10.16 0)
				(length 3.81)
				(name "IO9")
				(number "14")
			)
			(pin input line
				(at -20.32 -12.7 0)
				(length 3.81)
				(name "IO10")
				(number "15")
			)
			(pin input line
				(at -20.32 -15.24 0)
				(length 3.81)
				(name "IO11")
				(number "16")
			)
			(pin input line
				(at -20.32 -20.32 0)
				(length 3.81)
				(name "I3")
				(number "17")
			)
			(pin input line
				(at -20.32 -22.86 0)
				(length 3.81)
				(name "I4")
				(number "18")
			)
			(pin input line
				(at -20.32 -25.4 0)
				(length 3.81)
				(name "I5")
				(number "19")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 3.81)
				(name "VCC")
				(number "40")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 3.81)
				(name "GND")
				(number "20")
			)
			(pin input line
				(at 20.32 22.86 180)
				(length 3.81)
				(name "I6")
				(number "39")
			)
			(pin input line
				(at 20.32 20.32 180)
				(length 3.81)
				(name "I7")
				(number "38")
			)
			(pin input line
				(at 20.32 17.78 180)
				(length 3.81)
				(name "I8")
				(number "37")
			)
			(pin input line
				(at 20.32 12.7 180)
				(length 3.81)
				(name "IO12")
				(number "36")
			)
			(pin input line
				(at 20.32 10.16 180)
				(length 3.81)
				(name "IO13")
				(number "35")
			)
			(pin input line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "IO14")
				(number "34")
			)
			(pin input line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "IO15")
				(number "33")
			)
			(pin input line
				(at 20.32 2.54 180)
				(length 3.81)
				(name "IO16")
				(number "32")
			)
			(pin input line
				(at 20.32 0 180)
				(length 3.81)
				(name "IO17")
				(number "31")
			)
			(pin input line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "IO18")
				(number "30")
			)
			(pin input line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "IO19")
				(number "29")
			)
			(pin input line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "IO20")
				(number "28")
			)
			(pin input line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "IO21")
				(number "27")
			)
			(pin input line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "IO22")
				(number "26")
			)
			(pin input line
				(at 20.32 -15.24 180)
				(length 3.81)
				(name "IO23")
				(number "25")
			)
			(pin input line
				(at 20.32 -20.32 180)
				(length 3.81)
				(name "I9")
				(number "24")
			)
			(pin input line
				(at 20.32 -22.86 180)
				(length 3.81)
				(name "I10")
				(number "23")
			)
			(pin input line
				(at 20.32 -25.4 180)
				(length 3.81)
				(name "I11")
				(number "22")
			)
			(pin input line
				(at 20.32 -30.48 180)
				(length 3.81)
				(name "CLK2")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EPM1270F256"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 15.24 72.39 0)
		)
		(property "Value" "EPM1270F256"
			(at 12.7 -72.39 0)
		)
		(property "Footprint" "Package_BGA:BGA-256_17.0x17.0mm_Layout16x16_P1.0mm_Ball0.5mm_Pad0.4mm_NSMD"
			(at 12.7 -74.93 0)
		)
		(property "Datasheet" "https://www.altera.com/content/dam/altera-www/global/en_US/pdfs/literature/hb/max2/max2_mii5v1.pdf"
			(at 0 0 0)
		)
		(property "Description" "Altera MAX2 CPLD with 1270 LE"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "MAX2 FBGA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*BGA*P1.0mm*"
			(at 0 0 0)
		)
		(symbol "EPM1270F256_1_1"
			(pin bidirectional line
				(at -30.48 68.58 0)
				(length 5.08)
				(name "IO1_C2")
				(number "C2")
			)
			(pin bidirectional line
				(at -30.48 66.04 0)
				(length 5.08)
				(name "IO1_C3")
				(number "C3")
			)
			(pin bidirectional line
				(at -30.48 63.5 0)
				(length 5.08)
				(name "IO1_D1")
				(number "D1")
			)
			(pin bidirectional line
				(at -30.48 60.96 0)
				(length 5.08)
				(name "IO1_D2")
				(number "D2")
			)
			(pin bidirectional line
				(at -30.48 58.42 0)
				(length 5.08)
				(name "IO1_D3")
				(number "D3")
			)
			(pin bidirectional line
				(at -30.48 55.88 0)
				(length 5.08)
				(name "IO1_E1")
				(number "E1")
			)
			(pin bidirectional line
				(at -30.48 53.34 0)
				(length 5.08)
				(name "IO1_E2")
				(number "E2")
			)
			(pin bidirectional line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "IO1_E3")
				(number "E3")
			)
			(pin bidirectional line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "IO1_E4")
				(number "E4")
			)
			(pin bidirectional line
				(at -30.48 45.72 0)
				(length 5.08)
				(name "IO1_E5")
				(number "E5")
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "IO1_F1")
				(number "F1")
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "IO1_F2")
				(number "F2")
			)
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "IO1_F3")
				(number "F3")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "IO1_F4")
				(number "F4")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "IO1_F5")
				(number "F5")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "IO1_F6")
				(number "F6")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "IO1_G1")
				(number "G1")
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "IO1_G2")
				(number "G2")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "IO1_G3")
				(number "G3")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "IO1_G4")
				(number "G4")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "IO1_G5")
				(number "G5")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "IO1_G6")
				(number "G6")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "IO1_H1")
				(number "H1")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "IO1_H2")
				(number "H2")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "IO1_H3")
				(number "H3")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "IO1_H4")
				(number "H4")
			)
			(pin bidirectional clock
				(at -30.48 2.54 0)
				(length 5.08)
				(name "IO1_H5/GCLK0")
				(number "H5")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "IO1_J1")
				(number "J1")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "IO1_J2")
				(number "J2")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "IO1_J3")
				(number "J3")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "IO1_J4")
				(number "J4")
			)
			(pin bidirectional clock
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "IO1_J5/GCLK1")
				(number "J5")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "IO1_K1")
				(number "K1")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "IO1_K2")
				(number "K2")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "IO1_K3")
				(number "K3")
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "IO1_K4")
				(number "K4")
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "IO1_K5")
				(number "K5")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "IO1_K6")
				(number "K6")
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 5.08)
				(name "IO1_L1")
				(number "L1")
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "IO1_L2")
				(number "L2")
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "IO1_L3")
				(number "L3")
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "IO1_L4")
				(number "L4")
			)
			(pin bidirectional line
				(at -30.48 -38.1 0)
				(length 5.08)
				(name "IO1_L5")
				(number "L5")
			)
			(pin bidirectional line
				(at -30.48 -40.64 0)
				(length 5.08)
				(name "IO1_M1")
				(number "M1")
			)
			(pin bidirectional line
				(at -30.48 -43.18 0)
				(length 5.08)
				(name "IO1_M2")
				(number "M2")
			)
			(pin bidirectional line
				(at -30.48 -45.72 0)
				(length 5.08)
				(name "IO1_M3")
				(number "M3")
			)
			(pin bidirectional line
				(at -30.48 -48.26 0)
				(length 5.08)
				(name "IO1_M4")
				(number "M4")
			)
			(pin bidirectional line
				(at -30.48 -50.8 0)
				(length 5.08)
				(name "IO1_N1")
				(number "N1")
			)
			(pin bidirectional line
				(at -30.48 -53.34 0)
				(length 5.08)
				(name "IO1_N2")
				(number "N2")
			)
			(pin bidirectional line
				(at -30.48 -55.88 0)
				(length 5.08)
				(name "IO1_N3")
				(number "N3")
			)
			(pin bidirectional line
				(at -30.48 -58.42 0)
				(length 5.08)
				(name "IO1_P2")
				(number "P2")
			)
			(pin input line
				(at -30.48 -60.96 0)
				(length 5.08)
				(name "TMS")
				(number "N4")
			)
			(pin input line
				(at -30.48 -63.5 0)
				(length 5.08)
				(name "TDI")
				(number "L6")
			)
			(pin input clock
				(at -30.48 -66.04 0)
				(length 5.08)
				(name "TCK")
				(number "P3")
			)
			(pin output line
				(at -30.48 -68.58 0)
				(length 5.08)
				(name "TDO")
				(number "M5")
			)
			(pin power_in line
				(at -15.24 76.2 270)
				(length 5.08)
				(name "VCCINT")
				(number "H8")
			)
			(pin power_in line
				(at -12.7 76.2 270)
				(length 5.08)
				(name "VCCINT")
				(number "H10")
			)
			(pin power_in line
				(at -12.7 -76.2 90)
				(length 5.08)
				(name "GNDINT")
				(number "H7")
			)
			(pin power_in line
				(at -10.16 76.2 270)
				(length 5.08)
				(name "VCCINT")
				(number "J7")
			)
			(pin power_in line
				(at -10.16 -76.2 90)
				(length 5.08)
				(name "GNDINT")
				(number "H9")
			)
			(pin power_in line
				(at -7.62 76.2 270)
				(length 5.08)
				(name "VCCINT")
				(number "J9")
			)
			(pin power_in line
				(at -7.62 -76.2 90)
				(length 5.08)
				(name "GNDINT")
				(number "J8")
			)
			(pin power_in line
				(at -5.08 76.2 270)
				(length 5.08)
				(name "VCCIO1")
				(number "C1")
			)
			(pin power_in line
				(at -5.08 -76.2 90)
				(length 5.08)
				(name "GNDINT")
				(number "J10")
			)
			(pin power_in line
				(at -2.54 76.2 270)
				(length 5.08)
				(name "VCCIO1")
				(number "H6")
			)
			(pin power_in line
				(at -2.54 -76.2 90)
				(length 5.08)
				(name "GNDIO")
				(number "A1")
			)
			(pin power_in line
				(at 0 76.2 270)
				(length 5.08)
				(name "VCCIO1")
				(number "J6")
			)
			(pin power_in line
				(at 0 -76.2 90)
				(length 5.08)
				(name "GNDIO")
				(number "A16")
			)
			(pin power_in line
				(at 2.54 76.2 270)
				(length 5.08)
				(name "VCCIO1")
				(number "P1")
			)
			(pin power_in line
				(at 2.54 -76.2 90)
				(length 5.08)
				(name "GNDIO")
				(number "B2")
			)
			(pin power_in line
				(at 5.08 76.2 270)
				(length 5.08)
				(name "VCCIO2")
				(number "A3")
			)
			(pin power_in line
				(at 5.08 -76.2 90)
				(length 5.08)
				(name "GNDIO")
				(number "B15")
			)
			(pin power_in line
				(at 7.62 76.2 270)
				(length 5.08)
				(name "VCCIO2")
				(number "A14")
			)
			(pin power_in line
				(at 7.62 -76.2 90)
				(length 5.08)
				(name "GNDIO")
				(number "G7")
			)
			(pin power_in line
				(at 10.16 76.2 270)
				(length 5.08)
				(name "VCCIO2")
				(number "F8")
			)
			(pin power_in line
				(at 10.16 -76.2 90)
				(length 5.08)
				(name "GNDIO")
				(number "G8")
			)
			(pin power_in line
				(at 12.7 76.2 270)
				(length 5.08)
				(name "VCCIO2")
				(number "F9")
			)
			(pin bidirectional line
				(at 30.48 68.58 180)
				(length 5.08)
				(name "IO2_A2")
				(number "A2")
			)
			(pin bidirectional line
				(at 30.48 66.04 180)
				(length 5.08)
				(name "IO2_A4")
				(number "A4")
			)
			(pin bidirectional line
				(at 30.48 63.5 180)
				(length 5.08)
				(name "IO2_A5")
				(number "A5")
			)
			(pin bidirectional line
				(at 30.48 60.96 180)
				(length 5.08)
				(name "IO2_A6")
				(number "A6")
			)
			(pin bidirectional line
				(at 30.48 58.42 180)
				(length 5.08)
				(name "IO2_A7")
				(number "A7")
			)
			(pin bidirectional line
				(at 30.48 55.88 180)
				(length 5.08)
				(name "IO2_A8")
				(number "A8")
			)
			(pin bidirectional line
				(at 30.48 53.34 180)
				(length 5.08)
				(name "IO2_A9")
				(number "A9")
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 5.08)
				(name "IO2_A10")
				(number "A10")
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "IO2_A11")
				(number "A11")
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "IO2_A12")
				(number "A12")
			)
			(pin bidirectional line
				(at 30.48 43.18 180)
				(length 5.08)
				(name "IO2_A13")
				(number "A13")
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "IO2_A15")
				(number "A15")
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "IO2_B1")
				(number "B1")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "IO2_B3")
				(number "B3")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "IO2_B4")
				(number "B4")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "IO2_B5")
				(number "B5")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "IO2_B6")
				(number "B6")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "IO2_B7")
				(number "B7")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "IO2_B8")
				(number "B8")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "IO2_B9")
				(number "B9")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "IO2_B10")
				(number "B10")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "IO2_B11")
				(number "B11")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "IO2_B12")
				(number "B12")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "IO2_B13")
				(number "B13")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "IO2_B14")
				(number "B14")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "IO2_B16")
				(number "B16")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "IO2_C4")
				(number "C4")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "IO2_C5")
				(number "C5")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "IO2_C6")
				(number "C6")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "IO2_C7")
				(number "C7")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "IO2_C8")
				(number "C8")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "IO2_C9")
				(number "C9")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "IO2_C10")
				(number "C10")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "IO2_C11")
				(number "C11")
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "IO2_C12")
				(number "C12")
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 5.08)
				(name "IO2_C13")
				(number "C13")
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "IO2_D4")
				(number "D4")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "IO2_D5")
				(number "D5")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "IO2_D6")
				(number "D6")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "IO2_D7")
				(number "D7")
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "IO2_D8")
				(number "D8")
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "IO2_D9")
				(number "D9")
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "IO2_D10")
				(number "D10")
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "IO2_D11")
				(number "D11")
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 5.08)
				(name "IO2_D12")
				(number "D12")
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "IO2_E6")
				(number "E6")
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "IO2_E7")
				(number "E7")
			)
			(pin bidirectional line
				(at 30.48 -50.8 180)
				(length 5.08)
				(name "IO2_E8")
				(number "E8")
			)
			(pin bidirectional line
				(at 30.48 -53.34 180)
				(length 5.08)
				(name "IO2_E9")
				(number "E9")
			)
			(pin bidirectional line
				(at 30.48 -55.88 180)
				(length 5.08)
				(name "IO2_E10")
				(number "E10")
			)
			(pin bidirectional line
				(at 30.48 -58.42 180)
				(length 5.08)
				(name "IO2_E11")
				(number "E11")
			)
			(pin bidirectional line
				(at 30.48 -60.96 180)
				(length 5.08)
				(name "IO2_F7")
				(number "F7")
			)
			(pin bidirectional line
				(at 30.48 -63.5 180)
				(length 5.08)
				(name "IO2_F10")
				(number "F10")
			)
		)
		(symbol "EPM1270F256_2_1"
			(pin bidirectional line
				(at -30.48 68.58 0)
				(length 5.08)
				(name "IO3_C14")
				(number "C14")
			)
			(pin bidirectional line
				(at -30.48 66.04 0)
				(length 5.08)
				(name "IO3_C15")
				(number "C15")
			)
			(pin bidirectional line
				(at -30.48 63.5 0)
				(length 5.08)
				(name "IO3_D13")
				(number "D13")
			)
			(pin bidirectional line
				(at -30.48 60.96 0)
				(length 5.08)
				(name "IO3_D14")
				(number "D14")
			)
			(pin bidirectional line
				(at -30.48 58.42 0)
				(length 5.08)
				(name "IO3_D15")
				(number "D15")
			)
			(pin bidirectional line
				(at -30.48 55.88 0)
				(length 5.08)
				(name "IO3_D16")
				(number "D16")
			)
			(pin bidirectional line
				(at -30.48 53.34 0)
				(length 5.08)
				(name "IO3_E12")
				(number "E12")
			)
			(pin bidirectional line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "IO3_E13")
				(number "E13")
			)
			(pin bidirectional line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "IO3_E14")
				(number "E14")
			)
			(pin bidirectional line
				(at -30.48 45.72 0)
				(length 5.08)
				(name "IO3_E15")
				(number "E15")
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "IO3_E16")
				(number "E16")
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "IO3_F11")
				(number "F11")
			)
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "IO3_F12")
				(number "F12")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "IO3_F13")
				(number "F13")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "IO3_F14")
				(number "F14")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "IO3_F15")
				(number "F15")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "IO3_F16")
				(number "F16")
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "IO3_G11")
				(number "G11")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "IO3_G12")
				(number "G12")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "IO3_G13")
				(number "G13")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "IO3_G14")
				(number "G14")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "IO3_G15")
				(number "G15")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "IO3_G16")
				(number "G16")
			)
			(pin bidirectional clock
				(at -30.48 10.16 0)
				(length 5.08)
				(name "IO3_H12/GCLK3")
				(number "H12")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "IO3_H13")
				(number "H13")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "IO3_H14")
				(number "H14")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "IO3_H15")
				(number "H15")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "IO3_H16")
				(number "H16")
			)
			(pin bidirectional clock
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "IO3_J12/GCLK2")
				(number "J12")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "IO3_J13")
				(number "J13")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "IO3_J14")
				(number "J14")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "IO3_J15")
				(number "J15")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "IO3_J16")
				(number "J16")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "IO3_K11")
				(number "K11")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "IO3_K12")
				(number "K12")
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "IO3_K13")
				(number "K13")
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "IO3_K14")
				(number "K14")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "IO3_K15")
				(number "K15")
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 5.08)
				(name "IO3_K16")
				(number "K16")
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "IO3_L11")
				(number "L11")
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "IO3_L12")
				(number "L12")
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "IO3_L13")
				(number "L13")
			)
			(pin bidirectional line
				(at -30.48 -38.1 0)
				(length 5.08)
				(name "IO3_L14")
				(number "L14")
			)
			(pin bidirectional line
				(at -30.48 -40.64 0)
				(length 5.08)
				(name "IO3_L15")
				(number "L15")
			)
			(pin bidirectional line
				(at -30.48 -43.18 0)
				(length 5.08)
				(name "IO3_L16")
				(number "L16")
			)
			(pin bidirectional line
				(at -30.48 -45.72 0)
				(length 5.08)
				(name "IO3_M13")
				(number "M13")
			)
			(pin bidirectional line
				(at -30.48 -48.26 0)
				(length 5.08)
				(name "IO3_M14")
				(number "M14")
			)
			(pin bidirectional line
				(at -30.48 -50.8 0)
				(length 5.08)
				(name "IO3_M15")
				(number "M15")
			)
			(pin bidirectional line
				(at -30.48 -53.34 0)
				(length 5.08)
				(name "IO3_M16")
				(number "M16")
			)
			(pin bidirectional line
				(at -30.48 -55.88 0)
				(length 5.08)
				(name "IO3_N13")
				(number "N13")
			)
			(pin bidirectional line
				(at -30.48 -58.42 0)
				(length 5.08)
				(name "IO3_N14")
				(number "N14")
			)
			(pin bidirectional line
				(at -30.48 -60.96 0)
				(length 5.08)
				(name "IO3_N15")
				(number "N15")
			)
			(pin bidirectional line
				(at -30.48 -63.5 0)
				(length 5.08)
				(name "IO3_N16")
				(number "N16")
			)
			(pin bidirectional line
				(at -30.48 -66.04 0)
				(length 5.08)
				(name "IO3_P14")
				(number "P14")
			)
			(pin bidirectional line
				(at -30.48 -68.58 0)
				(length 5.08)
				(name "IO3_P15")
				(number "P15")
			)
			(pin power_in line
				(at -12.7 -76.2 90)
				(length 5.08)
				(name "GNDIO")
				(number "G9")
			)
			(pin power_in line
				(at -10.16 76.2 270)
				(length 5.08)
				(name "VCCIO3")
				(number "C16")
			)
			(pin power_in line
				(at -10.16 -76.2 90)
				(length 5.08)
				(name "GNDIO")
				(number "G10")
			)
			(pin power_in line
				(at -7.62 76.2 270)
				(length 5.08)
				(name "VCCIO3")
				(number "H11")
			)
			(pin power_in line
				(at -7.62 -76.2 90)
				(length 5.08)
				(name "GNDIO")
				(number "K7")
			)
			(pin power_in line
				(at -5.08 76.2 270)
				(length 5.08)
				(name "VCCIO3")
				(number "J11")
			)
			(pin power_in line
				(at -5.08 -76.2 90)
				(length 5.08)
				(name "GNDIO")
				(number "K8")
			)
			(pin power_in line
				(at -2.54 76.2 270)
				(length 5.08)
				(name "VCCIO3")
				(number "P16")
			)
			(pin power_in line
				(at -2.54 -76.2 90)
				(length 5.08)
				(name "GNDIO")
				(number "K9")
			)
			(pin power_in line
				(at 0 76.2 270)
				(length 5.08)
				(name "VCCIO4")
				(number "L8")
			)
			(pin power_in line
				(at 0 -76.2 90)
				(length 5.08)
				(name "GNDIO")
				(number "K10")
			)
			(pin power_in line
				(at 2.54 76.2 270)
				(length 5.08)
				(name "VCCIO4")
				(number "L9")
			)
			(pin power_in line
				(at 2.54 -76.2 90)
				(length 5.08)
				(name "GNDIO")
				(number "R2")
			)
			(pin power_in line
				(at 5.08 76.2 270)
				(length 5.08)
				(name "VCCIO4")
				(number "T3")
			)
			(pin power_in line
				(at 5.08 -76.2 90)
				(length 5.08)
				(name "GNDIO")
				(number "R15")
			)
			(pin power_in line
				(at 7.62 76.2 270)
				(length 5.08)
				(name "VCCIO4")
				(number "T14")
			)
			(pin power_in line
				(at 7.62 -76.2 90)
				(length 5.08)
				(name "GNDIO")
				(number "T1")
			)
			(pin power_in line
				(at 10.16 -76.2 90)
				(length 5.08)
				(name "GNDIO")
				(number "T16")
			)
			(pin bidirectional line
				(at 30.48 68.58 180)
				(length 5.08)
				(name "IO4_L7")
				(number "L7")
			)
			(pin bidirectional line
				(at 30.48 66.04 180)
				(length 5.08)
				(name "IO4_L10")
				(number "L10")
			)
			(pin bidirectional line
				(at 30.48 63.5 180)
				(length 5.08)
				(name "IO4_M6")
				(number "M6")
			)
			(pin bidirectional line
				(at 30.48 60.96 180)
				(length 5.08)
				(name "IO4_M7")
				(number "M7")
			)
			(pin bidirectional line
				(at 30.48 58.42 180)
				(length 5.08)
				(name "IO4_M8/DEV_OE")
				(number "M8")
			)
			(pin bidirectional line
				(at 30.48 55.88 180)
				(length 5.08)
				(name "IO4_M9/DEV_CLRn")
				(number "M9")
			)
			(pin bidirectional line
				(at 30.48 53.34 180)
				(length 5.08)
				(name "IO4_M10")
				(number "M10")
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 5.08)
				(name "IO4_M11")
				(number "M11")
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "IO4_M12")
				(number "M12")
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "IO4_N5")
				(number "N5")
			)
			(pin bidirectional line
				(at 30.48 43.18 180)
				(length 5.08)
				(name "IO4_N6")
				(number "N6")
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "IO4_N7")
				(number "N7")
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "IO4_N8")
				(number "N8")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "IO4_N9")
				(number "N9")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "IO4_N10")
				(number "N10")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "IO4_N11")
				(number "N11")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "IO4_N12")
				(number "N12")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "IO4_P4")
				(number "P4")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "IO4_P5")
				(number "P5")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "IO4_P6")
				(number "P6")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "IO4_P7")
				(number "P7")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "IO4_P8")
				(number "P8")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "IO4_P9")
				(number "P9")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "IO4_P10")
				(number "P10")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "IO4_P11")
				(number "P11")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "IO4_P12")
				(number "P12")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "IO4_P13")
				(number "P13")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "IO4_R1")
				(number "R1")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "IO4_R3")
				(number "R3")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "IO4_R4")
				(number "R4")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "IO4_R5")
				(number "R5")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "IO4_R6")
				(number "R6")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "IO4_R7")
				(number "R7")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "IO4_R8")
				(number "R8")
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "IO4_R9")
				(number "R9")
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 5.08)
				(name "IO4_R10")
				(number "R10")
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "IO4_R11")
				(number "R11")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "IO4_R12")
				(number "R12")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "IO4_R13")
				(number "R13")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "IO4_R14")
				(number "R14")
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "IO4_R16")
				(number "R16")
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "IO4_T2")
				(number "T2")
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "IO4_T4")
				(number "T4")
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "IO4_T5")
				(number "T5")
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 5.08)
				(name "IO4_T6")
				(number "T6")
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "IO4_T7")
				(number "T7")
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "IO4_T8")
				(number "T8")
			)
			(pin bidirectional line
				(at 30.48 -50.8 180)
				(length 5.08)
				(name "IO4_T9")
				(number "T9")
			)
			(pin bidirectional line
				(at 30.48 -53.34 180)
				(length 5.08)
				(name "IO4_T10")
				(number "T10")
			)
			(pin bidirectional line
				(at 30.48 -55.88 180)
				(length 5.08)
				(name "IO4_T11")
				(number "T11")
			)
			(pin bidirectional line
				(at 30.48 -58.42 180)
				(length 5.08)
				(name "IO4_T12")
				(number "T12")
			)
			(pin bidirectional line
				(at 30.48 -60.96 180)
				(length 5.08)
				(name "IO4_T13")
				(number "T13")
			)
			(pin bidirectional line
				(at 30.48 -63.5 180)
				(length 5.08)
				(name "IO4_T15")
				(number "T15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EPM1270M256"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 15.24 72.39 0)
		)
		(property "Value" "EPM1270M256"
			(at 12.7 -72.39 0)
		)
		(property "Footprint" "Package_BGA:BGA-256_11.0x11.0mm_Layout20x20_P0.5mm_Ball0.3mm_Pad0.25mm_NSMD"
			(at 12.7 -74.93 0)
		)
		(property "Datasheet" "https://www.altera.com/content/dam/altera-www/global/en_US/pdfs/literature/hb/max2/max2_mii5v1.pdf"
			(at 0 0 0)
		)
		(property "Description" "Altera MAX2 CPLD with 1270 LE"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "MAX2 MBGA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*BGA*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "EPM1270M256_1_1"
			(pin bidirectional line
				(at -30.48 68.58 0)
				(length 5.08)
				(name "IO1_B1")
				(number "B1")
			)
			(pin bidirectional line
				(at -30.48 66.04 0)
				(length 5.08)
				(name "IO1_C1")
				(number "C1")
			)
			(pin bidirectional line
				(at -30.48 63.5 0)
				(length 5.08)
				(name "IO1_C2")
				(number "C2")
			)
			(pin bidirectional line
				(at -30.48 60.96 0)
				(length 5.08)
				(name "IO1_C3")
				(number "C3")
			)
			(pin bidirectional line
				(at -30.48 58.42 0)
				(length 5.08)
				(name "IO1_C4")
				(number "C4")
			)
			(pin bidirectional line
				(at -30.48 55.88 0)
				(length 5.08)
				(name "IO1_D1")
				(number "D1")
			)
			(pin bidirectional line
				(at -30.48 53.34 0)
				(length 5.08)
				(name "IO1_D2")
				(number "D2")
			)
			(pin bidirectional line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "IO1_D3")
				(number "D3")
			)
			(pin bidirectional line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "IO1_D4")
				(number "D4")
			)
			(pin bidirectional line
				(at -30.48 45.72 0)
				(length 5.08)
				(name "IO1_E1")
				(number "E1")
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "IO1_E2")
				(number "E2")
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "IO1_E3")
				(number "E3")
			)
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "IO1_E4")
				(number "E4")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "IO1_F1")
				(number "F1")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "IO1_F2")
				(number "F2")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "IO1_F3")
				(number "F3")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "IO1_F4")
				(number "F4")
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "IO1_G1")
				(number "G1")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "IO1_G2")
				(number "G2")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "IO1_G3")
				(number "G3")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "IO1_G4")
				(number "G4")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "IO1_H1")
				(number "H1")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "IO1_H2")
				(number "H2")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "IO1_H4")
				(number "H4")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "IO1_J1")
				(number "J1")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "IO1_J2")
				(number "J2")
			)
			(pin bidirectional clock
				(at -30.48 2.54 0)
				(length 5.08)
				(name "IO1_K1/GCLK0")
				(number "K1")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "IO1_K2")
				(number "K2")
			)
			(pin bidirectional clock
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "IO1_L1/GCLK1")
				(number "L1")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "IO1_L2")
				(number "L2")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "IO1_M1")
				(number "M1")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "IO1_M2")
				(number "M2")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "IO1_N1")
				(number "N1")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "IO1_N2")
				(number "N2")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "IO1_N4")
				(number "N4")
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "IO1_P1")
				(number "P1")
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "IO1_P2")
				(number "P2")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "IO1_P3")
				(number "P3")
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 5.08)
				(name "IO1_P4")
				(number "P4")
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "IO1_R1")
				(number "R1")
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "IO1_R2")
				(number "R2")
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "IO1_R3")
				(number "R3")
			)
			(pin bidirectional line
				(at -30.48 -38.1 0)
				(length 5.08)
				(name "IO1_R4")
				(number "R4")
			)
			(pin bidirectional line
				(at -30.48 -40.64 0)
				(length 5.08)
				(name "IO1_T1")
				(number "T1")
			)
			(pin bidirectional line
				(at -30.48 -43.18 0)
				(length 5.08)
				(name "IO1_T2")
				(number "T2")
			)
			(pin bidirectional line
				(at -30.48 -45.72 0)
				(length 5.08)
				(name "IO1_T4")
				(number "T4")
			)
			(pin bidirectional line
				(at -30.48 -48.26 0)
				(length 5.08)
				(name "IO1_U1")
				(number "U1")
			)
			(pin bidirectional line
				(at -30.48 -50.8 0)
				(length 5.08)
				(name "IO1_U3")
				(number "U3")
			)
			(pin bidirectional line
				(at -30.48 -53.34 0)
				(length 5.08)
				(name "IO1_V1")
				(number "V1")
			)
			(pin bidirectional line
				(at -30.48 -55.88 0)
				(length 5.08)
				(name "IO1_V3")
				(number "V3")
			)
			(pin bidirectional line
				(at -30.48 -58.42 0)
				(length 5.08)
				(name "IO1_W1")
				(number "W1")
			)
			(pin input line
				(at -30.48 -60.96 0)
				(length 5.08)
				(name "TMS")
				(number "T3")
			)
			(pin input line
				(at -30.48 -63.5 0)
				(length 5.08)
				(name "TDI")
				(number "U2")
			)
			(pin input clock
				(at -30.48 -66.04 0)
				(length 5.08)
				(name "TCK")
				(number "W2")
			)
			(pin output line
				(at -30.48 -68.58 0)
				(length 5.08)
				(name "TDO")
				(number "V2")
			)
			(pin power_in line
				(at -15.24 76.2 270)
				(length 5.08)
				(name "VCCINT")
				(number "K4")
			)
			(pin power_in line
				(at -12.7 76.2 270)
				(length 5.08)
				(name "VCCINT")
				(number "U11")
			)
			(pin power_in line
				(at -12.7 -76.2 90)
				(length 5.08)
				(name "GNDINT")
				(number "J4")
			)
			(pin power_in line
				(at -10.16 76.2 270)
				(length 5.08)
				(name "VCCINT")
				(number "L17")
			)
			(pin power_in line
				(at -10.16 -76.2 90)
				(length 5.08)
				(name "GNDINT")
				(number "U12")
			)
			(pin power_in line
				(at -7.62 76.2 270)
				(length 5.08)
				(name "VCCINT")
				(number "D11")
			)
			(pin power_in line
				(at -7.62 -76.2 90)
				(length 5.08)
				(name "GNDINT")
				(number "M17")
			)
			(pin power_in line
				(at -5.08 76.2 270)
				(length 5.08)
				(name "VCCIO1")
				(number "K3")
			)
			(pin power_in line
				(at -5.08 -76.2 90)
				(length 5.08)
				(name "GNDINT")
				(number "D12")
			)
			(pin power_in line
				(at -2.54 76.2 270)
				(length 5.08)
				(name "VCCIO1")
				(number "L3")
			)
			(pin power_in line
				(at -2.54 -76.2 90)
				(length 5.08)
				(name "GNDIO")
				(number "H3")
			)
			(pin power_in line
				(at 0 76.2 270)
				(length 5.08)
				(name "VCCIO1")
				(number "L4")
			)
			(pin power_in line
				(at 0 -76.2 90)
				(length 5.08)
				(name "GNDIO")
				(number "J3")
			)
			(pin power_in line
				(at 2.54 76.2 270)
				(length 5.08)
				(name "VCCIO1")
				(number "M3")
			)
			(pin power_in line
				(at 2.54 -76.2 90)
				(length 5.08)
				(name "GNDIO")
				(number "M4")
			)
			(pin power_in line
				(at 5.08 76.2 270)
				(length 5.08)
				(name "VCCIO2")
				(number "C9")
			)
			(pin power_in line
				(at 5.08 -76.2 90)
				(length 5.08)
				(name "GNDIO")
				(number "N3")
			)
			(pin power_in line
				(at 7.62 76.2 270)
				(length 5.08)
				(name "VCCIO2")
				(number "C10")
			)
			(pin power_in line
				(at 7.62 -76.2 90)
				(length 5.08)
				(name "GNDIO")
				(number "U9")
			)
			(pin power_in line
				(at 10.16 76.2 270)
				(length 5.08)
				(name "VCCIO2")
				(number "D10")
			)
			(pin power_in line
				(at 10.16 -76.2 90)
				(length 5.08)
				(name "GNDIO")
				(number "V8")
			)
			(pin power_in line
				(at 12.7 76.2 270)
				(length 5.08)
				(name "VCCIO2")
				(number "C11")
			)
			(pin bidirectional line
				(at 30.48 68.58 180)
				(length 5.08)
				(name "IO2_A1")
				(number "A1")
			)
			(pin bidirectional line
				(at 30.48 66.04 180)
				(length 5.08)
				(name "IO2_A2")
				(number "A2")
			)
			(pin bidirectional line
				(at 30.48 63.5 180)
				(length 5.08)
				(name "IO2_A3")
				(number "A3")
			)
			(pin bidirectional line
				(at 30.48 60.96 180)
				(length 5.08)
				(name "IO2_A4")
				(number "A4")
			)
			(pin bidirectional line
				(at 30.48 58.42 180)
				(length 5.08)
				(name "IO2_A5")
				(number "A5")
			)
			(pin bidirectional line
				(at 30.48 55.88 180)
				(length 5.08)
				(name "IO2_A6")
				(number "A6")
			)
			(pin bidirectional line
				(at 30.48 53.34 180)
				(length 5.08)
				(name "IO2_A7")
				(number "A7")
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 5.08)
				(name "IO2_A8")
				(number "A8")
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "IO2_A9")
				(number "A9")
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "IO2_A10")
				(number "A10")
			)
			(pin bidirectional line
				(at 30.48 43.18 180)
				(length 5.08)
				(name "IO2_A11")
				(number "A11")
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "IO2_A12")
				(number "A12")
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "IO2_A13")
				(number "A13")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "IO2_A14")
				(number "A14")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "IO2_A15")
				(number "A15")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "IO2_A16")
				(number "A16")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "IO2_A17")
				(number "A17")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "IO2_A18")
				(number "A18")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "IO2_A19")
				(number "A19")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "IO2_A20")
				(number "A20")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "IO2_B2")
				(number "B2")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "IO2_B3")
				(number "B3")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "IO2_B4")
				(number "B4")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "IO2_B5")
				(number "B5")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "IO2_B6")
				(number "B6")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "IO2_B7")
				(number "B7")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "IO2_B8")
				(number "B8")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "IO2_B9")
				(number "B9")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "IO2_B10")
				(number "B10")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "IO2_B11")
				(number "B11")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "IO2_B12")
				(number "B12")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "IO2_B13")
				(number "B13")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "IO2_B14")
				(number "B14")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "IO2_B15")
				(number "B15")
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "IO2_B16")
				(number "B16")
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 5.08)
				(name "IO2_B17")
				(number "B17")
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "IO2_B18")
				(number "B18")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "IO2_B19")
				(number "B19")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "IO2_C5")
				(number "C5")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "IO2_C6")
				(number "C6")
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "IO2_C7")
				(number "C7")
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "IO2_C14")
				(number "C14")
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "IO2_C15")
				(number "C15")
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "IO2_C16")
				(number "C16")
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 5.08)
				(name "IO2_C17")
				(number "C17")
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "IO2_D5")
				(number "D5")
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "IO2_D6")
				(number "D6")
			)
			(pin bidirectional line
				(at 30.48 -50.8 180)
				(length 5.08)
				(name "IO2_D7")
				(number "D7")
			)
			(pin bidirectional line
				(at 30.48 -53.34 180)
				(length 5.08)
				(name "IO2_D8")
				(number "D8")
			)
			(pin bidirectional line
				(at 30.48 -55.88 180)
				(length 5.08)
				(name "IO2_D13")
				(number "D13")
			)
			(pin bidirectional line
				(at 30.48 -58.42 180)
				(length 5.08)
				(name "IO2_D14")
				(number "D14")
			)
			(pin bidirectional line
				(at 30.48 -60.96 180)
				(length 5.08)
				(name "IO2_D15")
				(number "D15")
			)
			(pin bidirectional line
				(at 30.48 -63.5 180)
				(length 5.08)
				(name "IO2_D16")
				(number "D16")
			)
		)
		(symbol "EPM1270M256_2_1"
			(pin bidirectional line
				(at -30.48 68.58 0)
				(length 5.08)
				(name "IO3_B20")
				(number "B20")
			)
			(pin bidirectional line
				(at -30.48 66.04 0)
				(length 5.08)
				(name "IO3_C18")
				(number "C18")
			)
			(pin bidirectional line
				(at -30.48 63.5 0)
				(length 5.08)
				(name "IO3_C19")
				(number "C19")
			)
			(pin bidirectional line
				(at -30.48 60.96 0)
				(length 5.08)
				(name "IO3_C20")
				(number "C20")
			)
			(pin bidirectional line
				(at -30.48 58.42 0)
				(length 5.08)
				(name "IO3_D17")
				(number "D17")
			)
			(pin bidirectional line
				(at -30.48 55.88 0)
				(length 5.08)
				(name "IO3_D18")
				(number "D18")
			)
			(pin bidirectional line
				(at -30.48 53.34 0)
				(length 5.08)
				(name "IO3_D19")
				(number "D19")
			)
			(pin bidirectional line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "IO3_D20")
				(number "D20")
			)
			(pin bidirectional line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "IO3_E17")
				(number "E17")
			)
			(pin bidirectional line
				(at -30.48 45.72 0)
				(length 5.08)
				(name "IO3_E18")
				(number "E18")
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "IO3_E19")
				(number "E19")
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "IO3_E20")
				(number "E20")
			)
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "IO3_F17")
				(number "F17")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "IO3_F18")
				(number "F18")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "IO3_F19")
				(number "F19")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "IO3_F20")
				(number "F20")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "IO3_G17")
				(number "G17")
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "IO3_G18")
				(number "G18")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "IO3_G19")
				(number "G19")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "IO3_G20")
				(number "G20")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "IO3_H17")
				(number "H17")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "IO3_H19")
				(number "H19")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "IO3_H20")
				(number "H20")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "IO3_J19")
				(number "J19")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "IO3_J20")
				(number "J20")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "IO3_K19")
				(number "K19")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "IO3_K20")
				(number "K20")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "IO3_L19")
				(number "L19")
			)
			(pin bidirectional clock
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "IO3_L20/GCLK3")
				(number "L20")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "IO3_M19")
				(number "M19")
			)
			(pin bidirectional clock
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "IO3_M20/GCLK2")
				(number "M20")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "IO3_N17")
				(number "N17")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "IO3_N19")
				(number "N19")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "IO3_N20")
				(number "N20")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "IO3_P17")
				(number "P17")
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "IO3_P18")
				(number "P18")
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "IO3_P19")
				(number "P19")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "IO3_P20")
				(number "P20")
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 5.08)
				(name "IO3_R17")
				(number "R17")
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "IO3_R18")
				(number "R18")
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "IO3_R19")
				(number "R19")
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "IO3_R20")
				(number "R20")
			)
			(pin bidirectional line
				(at -30.48 -38.1 0)
				(length 5.08)
				(name "IO3_T17")
				(number "T17")
			)
			(pin bidirectional line
				(at -30.48 -40.64 0)
				(length 5.08)
				(name "IO3_T18")
				(number "T18")
			)
			(pin bidirectional line
				(at -30.48 -43.18 0)
				(length 5.08)
				(name "IO3_T19")
				(number "T19")
			)
			(pin bidirectional line
				(at -30.48 -45.72 0)
				(length 5.08)
				(name "IO3_T20")
				(number "T20")
			)
			(pin bidirectional line
				(at -30.48 -48.26 0)
				(length 5.08)
				(name "IO3_U17")
				(number "U17")
			)
			(pin bidirectional line
				(at -30.48 -50.8 0)
				(length 5.08)
				(name "IO3_U18")
				(number "U18")
			)
			(pin bidirectional line
				(at -30.48 -53.34 0)
				(length 5.08)
				(name "IO3_U19")
				(number "U19")
			)
			(pin bidirectional line
				(at -30.48 -55.88 0)
				(length 5.08)
				(name "IO3_U20")
				(number "U20")
			)
			(pin bidirectional line
				(at -30.48 -58.42 0)
				(length 5.08)
				(name "IO3_V19")
				(number "V19")
			)
			(pin bidirectional line
				(at -30.48 -60.96 0)
				(length 5.08)
				(name "IO3_V20")
				(number "V20")
			)
			(pin bidirectional line
				(at -30.48 -63.5 0)
				(length 5.08)
				(name "IO3_W19")
				(number "W19")
			)
			(pin bidirectional line
				(at -30.48 -66.04 0)
				(length 5.08)
				(name "IO3_W20")
				(number "W20")
			)
			(pin bidirectional line
				(at -30.48 -68.58 0)
				(length 5.08)
				(name "IO3_Y20")
				(number "Y20")
			)
			(pin power_in line
				(at -12.7 -76.2 90)
				(length 5.08)
				(name "GNDIO")
				(number "V9")
			)
			(pin power_in line
				(at -10.16 76.2 270)
				(length 5.08)
				(name "VCCIO3")
				(number "J18")
			)
			(pin power_in line
				(at -10.16 -76.2 90)
				(length 5.08)
				(name "GNDIO")
				(number "V13")
			)
			(pin power_in line
				(at -7.62 76.2 270)
				(length 5.08)
				(name "VCCIO3")
				(number "K17")
			)
			(pin power_in line
				(at -7.62 -76.2 90)
				(length 5.08)
				(name "GNDIO")
				(number "H18")
			)
			(pin power_in line
				(at -5.08 76.2 270)
				(length 5.08)
				(name "VCCIO3")
				(number "K18")
			)
			(pin power_in line
				(at -5.08 -76.2 90)
				(length 5.08)
				(name "GNDIO")
				(number "J17")
			)
			(pin power_in line
				(at -2.54 76.2 270)
				(length 5.08)
				(name "VCCIO3")
				(number "L18")
			)
			(pin power_in line
				(at -2.54 -76.2 90)
				(length 5.08)
				(name "GNDIO")
				(number "N18")
			)
			(pin power_in line
				(at 0 76.2 270)
				(length 5.08)
				(name "VCCIO4")
				(number "U10")
			)
			(pin power_in line
				(at 0 -76.2 90)
				(length 5.08)
				(name "GNDIO")
				(number "C8")
			)
			(pin power_in line
				(at 2.54 76.2 270)
				(length 5.08)
				(name "VCCIO4")
				(number "V10")
			)
			(pin power_in line
				(at 2.54 -76.2 90)
				(length 5.08)
				(name "GNDIO")
				(number "D9")
			)
			(pin power_in line
				(at 5.08 76.2 270)
				(length 5.08)
				(name "VCCIO4")
				(number "V11")
			)
			(pin power_in line
				(at 5.08 -76.2 90)
				(length 5.08)
				(name "GNDIO")
				(number "C12")
			)
			(pin power_in line
				(at 7.62 76.2 270)
				(length 5.08)
				(name "VCCIO4")
				(number "V12")
			)
			(pin power_in line
				(at 7.62 -76.2 90)
				(length 5.08)
				(name "GNDIO")
				(number "C13")
			)
			(pin power_in line
				(at 10.16 -76.2 90)
				(length 5.08)
				(name "GNDIO")
				(number "M18")
			)
			(pin bidirectional line
				(at 30.48 68.58 180)
				(length 5.08)
				(name "IO4_U4")
				(number "U4")
			)
			(pin bidirectional line
				(at 30.48 66.04 180)
				(length 5.08)
				(name "IO4_U5")
				(number "U5")
			)
			(pin bidirectional line
				(at 30.48 63.5 180)
				(length 5.08)
				(name "IO4_U6")
				(number "U6")
			)
			(pin bidirectional line
				(at 30.48 60.96 180)
				(length 5.08)
				(name "IO4_U7")
				(number "U7")
			)
			(pin bidirectional line
				(at 30.48 58.42 180)
				(length 5.08)
				(name "IO4_U8")
				(number "U8")
			)
			(pin bidirectional line
				(at 30.48 55.88 180)
				(length 5.08)
				(name "IO4_U13")
				(number "U13")
			)
			(pin bidirectional line
				(at 30.48 53.34 180)
				(length 5.08)
				(name "IO4_U14")
				(number "U14")
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 5.08)
				(name "IO4_U15")
				(number "U15")
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "IO4_U16")
				(number "U16")
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "IO4_V4")
				(number "V4")
			)
			(pin bidirectional line
				(at 30.48 43.18 180)
				(length 5.08)
				(name "IO4_V5")
				(number "V5")
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "IO4_V6")
				(number "V6")
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "IO4_V7")
				(number "V7")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "IO4_V14")
				(number "V14")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "IO4_V15")
				(number "V15")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "IO4_V16")
				(number "V16")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "IO4_V17")
				(number "V17")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "IO4_V18")
				(number "V18")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "IO4_W3")
				(number "W3")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "IO4_W4")
				(number "W4")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "IO4_W5")
				(number "W5")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "IO4_W6")
				(number "W6")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "IO4_W7")
				(number "W7")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "IO4_W8")
				(number "W8")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "IO4_W9")
				(number "W9")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "IO4_W10")
				(number "W10")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "IO4_W11")
				(number "W11")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "IO4_W12/DEV_OE")
				(number "W12")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "IO4_W13")
				(number "W13")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "IO4_W14")
				(number "W14")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "IO4_W15")
				(number "W15")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "IO4_W16")
				(number "W16")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "IO4_W17")
				(number "W17")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "IO4_W18")
				(number "W18")
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "IO4_Y1")
				(number "Y1")
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 5.08)
				(name "IO4_Y2")
				(number "Y2")
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "IO4_Y3")
				(number "Y3")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "IO4_Y4")
				(number "Y4")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "IO4_Y5")
				(number "Y5")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "IO4_Y6")
				(number "Y6")
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "IO4_Y7")
				(number "Y7")
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "IO4_Y8")
				(number "Y8")
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "IO4_Y9")
				(number "Y9")
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "IO4_Y10")
				(number "Y10")
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 5.08)
				(name "IO4_Y11")
				(number "Y11")
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "IO4_Y12")
				(number "Y12")
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "IO4_Y13/DEV_CLRn")
				(number "Y13")
			)
			(pin bidirectional line
				(at 30.48 -50.8 180)
				(length 5.08)
				(name "IO4_Y14")
				(number "Y14")
			)
			(pin bidirectional line
				(at 30.48 -53.34 180)
				(length 5.08)
				(name "IO4_Y15")
				(number "Y15")
			)
			(pin bidirectional line
				(at 30.48 -55.88 180)
				(length 5.08)
				(name "IO4_Y16")
				(number "Y16")
			)
			(pin bidirectional line
				(at 30.48 -58.42 180)
				(length 5.08)
				(name "IO4_Y17")
				(number "Y17")
			)
			(pin bidirectional line
				(at 30.48 -60.96 180)
				(length 5.08)
				(name "IO4_Y18")
				(number "Y18")
			)
			(pin bidirectional line
				(at 30.48 -63.5 180)
				(length 5.08)
				(name "IO4_Y19")
				(number "Y19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EPM1270T144"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 10.16 41.91 0)
		)
		(property "Value" "EPM1270T144"
			(at 12.7 -41.91 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at 12.7 -44.45 0)
		)
		(property "Datasheet" "https://www.altera.com/content/dam/altera-www/global/en_US/pdfs/literature/hb/max2/max2_mii5v1.pdf"
			(at 0 0 0)
		)
		(property "Description" "Altera MAX2 CPLD with 1270 LE"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "MAX2 TQFP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "EPM1270T144_1_1"
			(pin bidirectional line
				(at -27.94 38.1 0)
				(length 5.08)
				(name "IO1_1")
				(number "1")
			)
			(pin bidirectional line
				(at -27.94 35.56 0)
				(length 5.08)
				(name "IO1_2")
				(number "2")
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 5.08)
				(name "IO1_3")
				(number "3")
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 5.08)
				(name "IO1_4")
				(number "4")
			)
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 5.08)
				(name "IO1_5")
				(number "5")
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 5.08)
				(name "IO1_6")
				(number "6")
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 5.08)
				(name "IO1_7")
				(number "7")
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 5.08)
				(name "IO1_8")
				(number "8")
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 5.08)
				(name "IO1_11")
				(number "11")
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 5.08)
				(name "IO1_12")
				(number "12")
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 5.08)
				(name "IO1_13")
				(number "13")
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 5.08)
				(name "IO1_14")
				(number "14")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 5.08)
				(name "IO1_15")
				(number "15")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 5.08)
				(name "IO1_16")
				(number "16")
			)
			(pin bidirectional clock
				(at -27.94 2.54 0)
				(length 5.08)
				(name "IO1_18/GCLK0")
				(number "18")
			)
			(pin bidirectional clock
				(at -27.94 0 0)
				(length 5.08)
				(name "IO1_20/GCLK1")
				(number "20")
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 5.08)
				(name "IO1_21")
				(number "21")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 5.08)
				(name "IO1_22")
				(number "22")
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 5.08)
				(name "IO1_23")
				(number "23")
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 5.08)
				(name "IO1_24")
				(number "24")
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 5.08)
				(name "IO1_27")
				(number "27")
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 5.08)
				(name "IO1_28")
				(number "28")
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 5.08)
				(name "IO1_29")
				(number "29")
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 5.08)
				(name "IO1_30")
				(number "30")
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 5.08)
				(name "IO1_31")
				(number "31")
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 5.08)
				(name "IO1_32")
				(number "32")
			)
			(pin input line
				(at -27.94 -27.94 0)
				(length 5.08)
				(name "TMS")
				(number "33")
			)
			(pin input line
				(at -27.94 -30.48 0)
				(length 5.08)
				(name "TDI")
				(number "34")
			)
			(pin input clock
				(at -27.94 -33.02 0)
				(length 5.08)
				(name "TCK")
				(number "35")
			)
			(pin output line
				(at -27.94 -35.56 0)
				(length 5.08)
				(name "TDO")
				(number "36")
			)
			(pin power_in line
				(at -12.7 -45.72 90)
				(length 5.08)
				(name "GNDINT")
				(number "17")
			)
			(pin power_in line
				(at -10.16 45.72 270)
				(length 5.08)
				(name "VCCINT")
				(number "19")
			)
			(pin power_in line
				(at -10.16 -45.72 90)
				(length 5.08)
				(name "GNDINT")
				(number "54")
			)
			(pin power_in line
				(at -7.62 45.72 270)
				(length 5.08)
				(name "VCCINT")
				(number "56")
			)
			(pin power_in line
				(at -7.62 -45.72 90)
				(length 5.08)
				(name "GNDINT")
				(number "92")
			)
			(pin power_in line
				(at -5.08 45.72 270)
				(length 5.08)
				(name "VCCINT")
				(number "90")
			)
			(pin power_in line
				(at -5.08 -45.72 90)
				(length 5.08)
				(name "GNDINT")
				(number "128")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 5.08)
				(name "VCCINT")
				(number "126")
			)
			(pin power_in line
				(at -2.54 -45.72 90)
				(length 5.08)
				(name "GNDIO")
				(number "10")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 5.08)
				(name "VCCIO1")
				(number "9")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 5.08)
				(name "GNDIO")
				(number "26")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 5.08)
				(name "VCCIO1")
				(number "25")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 5.08)
				(name "GNDIO")
				(number "47")
			)
			(pin power_in line
				(at 5.08 45.72 270)
				(length 5.08)
				(name "VCCIO2")
				(number "116")
			)
			(pin power_in line
				(at 5.08 -45.72 90)
				(length 5.08)
				(name "GNDIO")
				(number "65")
			)
			(pin power_in line
				(at 7.62 45.72 270)
				(length 5.08)
				(name "VCCIO2")
				(number "136")
			)
			(pin power_in line
				(at 7.62 -45.72 90)
				(length 5.08)
				(name "GNDIO")
				(number "83")
			)
			(pin power_in line
				(at 10.16 -45.72 90)
				(length 5.08)
				(name "GNDIO")
				(number "99")
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 5.08)
				(name "IO2_109")
				(number "109")
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 5.08)
				(name "IO2_110")
				(number "110")
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 5.08)
				(name "IO2_111")
				(number "111")
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 5.08)
				(name "IO2_112")
				(number "112")
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 5.08)
				(name "IO2_113")
				(number "113")
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 5.08)
				(name "IO2_114")
				(number "114")
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 5.08)
				(name "IO2_117")
				(number "117")
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 5.08)
				(name "IO2_118")
				(number "118")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 5.08)
				(name "IO2_119")
				(number "119")
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 5.08)
				(name "IO2_120")
				(number "120")
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 5.08)
				(name "IO2_121")
				(number "121")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 5.08)
				(name "IO2_122")
				(number "122")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 5.08)
				(name "IO2_123")
				(number "123")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 5.08)
				(name "IO2_124")
				(number "124")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 5.08)
				(name "IO2_125")
				(number "125")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 5.08)
				(name "IO2_127")
				(number "127")
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 5.08)
				(name "IO2_129")
				(number "129")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 5.08)
				(name "IO2_130")
				(number "130")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 5.08)
				(name "IO2_131")
				(number "131")
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 5.08)
				(name "IO2_132")
				(number "132")
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 5.08)
				(name "IO2_133")
				(number "133")
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 5.08)
				(name "IO2_134")
				(number "134")
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 5.08)
				(name "IO2_137")
				(number "137")
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 5.08)
				(name "IO2_138")
				(number "138")
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 5.08)
				(name "IO2_139")
				(number "139")
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 5.08)
				(name "IO2_140")
				(number "140")
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 5.08)
				(name "IO2_141")
				(number "141")
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 5.08)
				(name "IO2_142")
				(number "142")
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 5.08)
				(name "IO2_143")
				(number "143")
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 5.08)
				(name "IO2_144")
				(number "144")
			)
		)
		(symbol "EPM1270T144_2_1"
			(pin bidirectional line
				(at -27.94 38.1 0)
				(length 5.08)
				(name "IO3_73")
				(number "73")
			)
			(pin bidirectional line
				(at -27.94 35.56 0)
				(length 5.08)
				(name "IO3_74")
				(number "74")
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 5.08)
				(name "IO3_75")
				(number "75")
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 5.08)
				(name "IO3_76")
				(number "76")
			)
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 5.08)
				(name "IO3_77")
				(number "77")
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 5.08)
				(name "IO3_78")
				(number "78")
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 5.08)
				(name "IO3_79")
				(number "79")
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 5.08)
				(name "IO3_80")
				(number "80")
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 5.08)
				(name "IO3_81")
				(number "81")
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 5.08)
				(name "IO3_84")
				(number "84")
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 5.08)
				(name "IO3_85")
				(number "85")
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 5.08)
				(name "IO3_86")
				(number "86")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 5.08)
				(name "IO3_87")
				(number "87")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 5.08)
				(name "IO3_88")
				(number "88")
			)
			(pin bidirectional clock
				(at -27.94 2.54 0)
				(length 5.08)
				(name "IO3_89/GCLK2")
				(number "89")
			)
			(pin bidirectional clock
				(at -27.94 0 0)
				(length 5.08)
				(name "IO3_91/GCLK3")
				(number "91")
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 5.08)
				(name "IO3_93")
				(number "93")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 5.08)
				(name "IO3_94")
				(number "94")
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 5.08)
				(name "IO3_95")
				(number "95")
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 5.08)
				(name "IO3_96")
				(number "96")
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 5.08)
				(name "IO3_97")
				(number "97")
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 5.08)
				(name "IO3_98")
				(number "98")
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 5.08)
				(name "IO3_101")
				(number "101")
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 5.08)
				(name "IO3_102")
				(number "102")
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 5.08)
				(name "IO3_103")
				(number "103")
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 5.08)
				(name "IO3_104")
				(number "104")
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 5.08)
				(name "IO3_105")
				(number "105")
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 5.08)
				(name "IO3_106")
				(number "106")
			)
			(pin bidirectional line
				(at -27.94 -33.02 0)
				(length 5.08)
				(name "IO3_107")
				(number "107")
			)
			(pin bidirectional line
				(at -27.94 -35.56 0)
				(length 5.08)
				(name "IO3_108")
				(number "108")
			)
			(pin power_in line
				(at -5.08 45.72 270)
				(length 5.08)
				(name "VCCIO3")
				(number "82")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 5.08)
				(name "VCCIO3")
				(number "100")
			)
			(pin power_in line
				(at -2.54 -45.72 90)
				(length 5.08)
				(name "GNDIO")
				(number "115")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 5.08)
				(name "VCCIO4")
				(number "46")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 5.08)
				(name "GNDIO")
				(number "135")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 5.08)
				(name "VCCIO4")
				(number "64")
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 5.08)
				(name "IO4_37")
				(number "37")
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 5.08)
				(name "IO4_38")
				(number "38")
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 5.08)
				(name "IO4_39")
				(number "39")
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 5.08)
				(name "IO4_40")
				(number "40")
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 5.08)
				(name "IO4_41")
				(number "41")
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 5.08)
				(name "IO4_42")
				(number "42")
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 5.08)
				(name "IO4_43")
				(number "43")
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 5.08)
				(name "IO4_44")
				(number "44")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 5.08)
				(name "IO4_45")
				(number "45")
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 5.08)
				(name "IO4_48")
				(number "48")
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 5.08)
				(name "IO4_49")
				(number "49")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 5.08)
				(name "IO4_50")
				(number "50")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 5.08)
				(name "IO4_51")
				(number "51")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 5.08)
				(name "IO4_52")
				(number "52")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 5.08)
				(name "IO4_53")
				(number "53")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 5.08)
				(name "IO4_55")
				(number "55")
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 5.08)
				(name "IO4_57")
				(number "57")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 5.08)
				(name "IO4_58")
				(number "58")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 5.08)
				(name "IO4_59")
				(number "59")
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 5.08)
				(name "IO4_60/DEV_OE")
				(number "60")
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 5.08)
				(name "IO4_61/DEV_CLRn")
				(number "61")
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 5.08)
				(name "IO4_62")
				(number "62")
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 5.08)
				(name "IO4_63")
				(number "63")
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 5.08)
				(name "IO4_66")
				(number "66")
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 5.08)
				(name "IO4_67")
				(number "67")
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 5.08)
				(name "IO4_68")
				(number "68")
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 5.08)
				(name "IO4_69")
				(number "69")
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 5.08)
				(name "IO4_70")
				(number "70")
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 5.08)
				(name "IO4_71")
				(number "71")
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 5.08)
				(name "IO4_72")
				(number "72")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EPM2210F256"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 20.32 69.85 0)
		)
		(property "Value" "EPM2210F256"
			(at 17.78 -69.85 0)
		)
		(property "Footprint" "Package_BGA:BGA-256_17.0x17.0mm_Layout16x16_P1.0mm_Ball0.5mm_Pad0.4mm_NSMD"
			(at 17.78 -72.39 0)
		)
		(property "Datasheet" "https://www.altera.com/content/dam/altera-www/global/en_US/pdfs/literature/hb/max2/max2_mii5v1.pdf"
			(at 0 0 0)
		)
		(property "Description" "Altera MAX2 CPLD with 2210 LE"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "MAX2 FBGA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*BGA*P1.0mm*"
			(at 0 0 0)
		)
		(symbol "EPM2210F256_1_1"
			(pin bidirectional line
				(at -35.56 66.04 0)
				(length 5.08)
				(name "IO1_C2")
				(number "C2")
			)
			(pin bidirectional line
				(at -35.56 63.5 0)
				(length 5.08)
				(name "IO1_C3")
				(number "C3")
			)
			(pin bidirectional line
				(at -35.56 60.96 0)
				(length 5.08)
				(name "IO1_D1")
				(number "D1")
			)
			(pin bidirectional line
				(at -35.56 58.42 0)
				(length 5.08)
				(name "IO1_D2")
				(number "D2")
			)
			(pin bidirectional line
				(at -35.56 55.88 0)
				(length 5.08)
				(name "IO1_D3")
				(number "D3")
			)
			(pin bidirectional line
				(at -35.56 53.34 0)
				(length 5.08)
				(name "IO1_E1")
				(number "E1")
			)
			(pin bidirectional line
				(at -35.56 50.8 0)
				(length 5.08)
				(name "IO1_E2")
				(number "E2")
			)
			(pin bidirectional line
				(at -35.56 48.26 0)
				(length 5.08)
				(name "IO1_E3")
				(number "E3")
			)
			(pin bidirectional line
				(at -35.56 45.72 0)
				(length 5.08)
				(name "IO1_E4")
				(number "E4")
			)
			(pin bidirectional line
				(at -35.56 43.18 0)
				(length 5.08)
				(name "IO1_E5")
				(number "E5")
			)
			(pin bidirectional line
				(at -35.56 40.64 0)
				(length 5.08)
				(name "IO1_F1")
				(number "F1")
			)
			(pin bidirectional line
				(at -35.56 38.1 0)
				(length 5.08)
				(name "IO1_F2")
				(number "F2")
			)
			(pin bidirectional line
				(at -35.56 35.56 0)
				(length 5.08)
				(name "IO1_F3")
				(number "F3")
			)
			(pin bidirectional line
				(at -35.56 33.02 0)
				(length 5.08)
				(name "IO1_F4")
				(number "F4")
			)
			(pin bidirectional line
				(at -35.56 30.48 0)
				(length 5.08)
				(name "IO1_F5")
				(number "F5")
			)
			(pin bidirectional line
				(at -35.56 27.94 0)
				(length 5.08)
				(name "IO1_F6")
				(number "F6")
			)
			(pin bidirectional line
				(at -35.56 25.4 0)
				(length 5.08)
				(name "IO1_G1")
				(number "G1")
			)
			(pin bidirectional line
				(at -35.56 22.86 0)
				(length 5.08)
				(name "IO1_G2")
				(number "G2")
			)
			(pin bidirectional line
				(at -35.56 20.32 0)
				(length 5.08)
				(name "IO1_G3")
				(number "G3")
			)
			(pin bidirectional line
				(at -35.56 17.78 0)
				(length 5.08)
				(name "IO1_G4")
				(number "G4")
			)
			(pin bidirectional line
				(at -35.56 15.24 0)
				(length 5.08)
				(name "IO1_G5")
				(number "G5")
			)
			(pin bidirectional line
				(at -35.56 12.7 0)
				(length 5.08)
				(name "IO1_H1")
				(number "H1")
			)
			(pin bidirectional line
				(at -35.56 10.16 0)
				(length 5.08)
				(name "IO1_H2")
				(number "H2")
			)
			(pin bidirectional line
				(at -35.56 7.62 0)
				(length 5.08)
				(name "IO1_H3")
				(number "H3")
			)
			(pin bidirectional line
				(at -35.56 5.08 0)
				(length 5.08)
				(name "IO1_H4")
				(number "H4")
			)
			(pin bidirectional clock
				(at -35.56 2.54 0)
				(length 5.08)
				(name "IO1_H5/GCLK0")
				(number "H5")
			)
			(pin bidirectional line
				(at -35.56 0 0)
				(length 5.08)
				(name "IO1_J1")
				(number "J1")
			)
			(pin bidirectional line
				(at -35.56 -2.54 0)
				(length 5.08)
				(name "IO1_J2")
				(number "J2")
			)
			(pin bidirectional line
				(at -35.56 -5.08 0)
				(length 5.08)
				(name "IO1_J3")
				(number "J3")
			)
			(pin bidirectional line
				(at -35.56 -7.62 0)
				(length 5.08)
				(name "IO1_J4")
				(number "J4")
			)
			(pin bidirectional clock
				(at -35.56 -10.16 0)
				(length 5.08)
				(name "IO1_J5/GCLK1")
				(number "J5")
			)
			(pin bidirectional line
				(at -35.56 -12.7 0)
				(length 5.08)
				(name "IO1_K1")
				(number "K1")
			)
			(pin bidirectional line
				(at -35.56 -15.24 0)
				(length 5.08)
				(name "IO1_K2")
				(number "K2")
			)
			(pin bidirectional line
				(at -35.56 -17.78 0)
				(length 5.08)
				(name "IO1_K3")
				(number "K3")
			)
			(pin bidirectional line
				(at -35.56 -20.32 0)
				(length 5.08)
				(name "IO1_K4")
				(number "K4")
			)
			(pin bidirectional line
				(at -35.56 -22.86 0)
				(length 5.08)
				(name "IO1_K5")
				(number "K5")
			)
			(pin bidirectional line
				(at -35.56 -25.4 0)
				(length 5.08)
				(name "IO1_L1")
				(number "L1")
			)
			(pin bidirectional line
				(at -35.56 -27.94 0)
				(length 5.08)
				(name "IO1_L2")
				(number "L2")
			)
			(pin bidirectional line
				(at -35.56 -30.48 0)
				(length 5.08)
				(name "IO1_L3")
				(number "L3")
			)
			(pin bidirectional line
				(at -35.56 -33.02 0)
				(length 5.08)
				(name "IO1_L4")
				(number "L4")
			)
			(pin bidirectional line
				(at -35.56 -35.56 0)
				(length 5.08)
				(name "IO1_L5")
				(number "L5")
			)
			(pin bidirectional line
				(at -35.56 -38.1 0)
				(length 5.08)
				(name "IO1_M1")
				(number "M1")
			)
			(pin bidirectional line
				(at -35.56 -40.64 0)
				(length 5.08)
				(name "IO1_M2")
				(number "M2")
			)
			(pin bidirectional line
				(at -35.56 -43.18 0)
				(length 5.08)
				(name "IO1_M3")
				(number "M3")
			)
			(pin bidirectional line
				(at -35.56 -45.72 0)
				(length 5.08)
				(name "IO1_M4")
				(number "M4")
			)
			(pin bidirectional line
				(at -35.56 -48.26 0)
				(length 5.08)
				(name "IO1_N1")
				(number "N1")
			)
			(pin bidirectional line
				(at -35.56 -50.8 0)
				(length 5.08)
				(name "IO1_N2")
				(number "N2")
			)
			(pin bidirectional line
				(at -35.56 -53.34 0)
				(length 5.08)
				(name "IO1_N3")
				(number "N3")
			)
			(pin bidirectional line
				(at -35.56 -55.88 0)
				(length 5.08)
				(name "IO1_P2")
				(number "P2")
			)
			(pin input line
				(at -35.56 -58.42 0)
				(length 5.08)
				(name "TMS")
				(number "N4")
			)
			(pin input line
				(at -35.56 -60.96 0)
				(length 5.08)
				(name "TDI")
				(number "L6")
			)
			(pin input clock
				(at -35.56 -63.5 0)
				(length 5.08)
				(name "TCK")
				(number "P3")
			)
			(pin output line
				(at -35.56 -66.04 0)
				(length 5.08)
				(name "TDO")
				(number "M5")
			)
			(pin power_in line
				(at -20.32 73.66 270)
				(length 5.08)
				(name "VCCINT")
				(number "F10")
			)
			(pin power_in line
				(at -17.78 73.66 270)
				(length 5.08)
				(name "VCCINT")
				(number "G11")
			)
			(pin power_in line
				(at -17.78 -73.66 90)
				(length 5.08)
				(name "GNDINT")
				(number "F7")
			)
			(pin power_in line
				(at -15.24 73.66 270)
				(length 5.08)
				(name "VCCINT")
				(number "H8")
			)
			(pin power_in line
				(at -15.24 -73.66 90)
				(length 5.08)
				(name "GNDINT")
				(number "G6")
			)
			(pin power_in line
				(at -12.7 73.66 270)
				(length 5.08)
				(name "VCCINT")
				(number "H10")
			)
			(pin power_in line
				(at -12.7 -73.66 90)
				(length 5.08)
				(name "GNDINT")
				(number "H7")
			)
			(pin power_in line
				(at -10.16 73.66 270)
				(length 5.08)
				(name "VCCINT")
				(number "J7")
			)
			(pin power_in line
				(at -10.16 -73.66 90)
				(length 5.08)
				(name "GNDINT")
				(number "H9")
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VCCINT")
				(number "J9")
			)
			(pin power_in line
				(at -7.62 -73.66 90)
				(length 5.08)
				(name "GNDINT")
				(number "J8")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VCCINT")
				(number "K6")
			)
			(pin power_in line
				(at -5.08 -73.66 90)
				(length 5.08)
				(name "GNDINT")
				(number "J10")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VCCINT")
				(number "L7")
			)
			(pin power_in line
				(at -2.54 -73.66 90)
				(length 5.08)
				(name "GNDINT")
				(number "K11")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VCCIO1")
				(number "C1")
			)
			(pin power_in line
				(at 0 -73.66 90)
				(length 5.08)
				(name "GNDINT")
				(number "L10")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VCCIO1")
				(number "H6")
			)
			(pin power_in line
				(at 2.54 -73.66 90)
				(length 5.08)
				(name "GNDIO")
				(number "A1")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VCCIO1")
				(number "J6")
			)
			(pin power_in line
				(at 5.08 -73.66 90)
				(length 5.08)
				(name "GNDIO")
				(number "A16")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VCCIO1")
				(number "P1")
			)
			(pin power_in line
				(at 7.62 -73.66 90)
				(length 5.08)
				(name "GNDIO")
				(number "B2")
			)
			(pin power_in line
				(at 10.16 73.66 270)
				(length 5.08)
				(name "VCCIO2")
				(number "A3")
			)
			(pin power_in line
				(at 10.16 -73.66 90)
				(length 5.08)
				(name "GNDIO")
				(number "B15")
			)
			(pin power_in line
				(at 12.7 73.66 270)
				(length 5.08)
				(name "VCCIO2")
				(number "A14")
			)
			(pin power_in line
				(at 12.7 -73.66 90)
				(length 5.08)
				(name "GNDIO")
				(number "G7")
			)
			(pin power_in line
				(at 15.24 73.66 270)
				(length 5.08)
				(name "VCCIO2")
				(number "F8")
			)
			(pin power_in line
				(at 15.24 -73.66 90)
				(length 5.08)
				(name "GNDIO")
				(number "G8")
			)
			(pin power_in line
				(at 17.78 73.66 270)
				(length 5.08)
				(name "VCCIO2")
				(number "F9")
			)
			(pin bidirectional line
				(at 35.56 66.04 180)
				(length 5.08)
				(name "IO2_A2")
				(number "A2")
			)
			(pin bidirectional line
				(at 35.56 63.5 180)
				(length 5.08)
				(name "IO2_A4")
				(number "A4")
			)
			(pin bidirectional line
				(at 35.56 60.96 180)
				(length 5.08)
				(name "IO2_A5")
				(number "A5")
			)
			(pin bidirectional line
				(at 35.56 58.42 180)
				(length 5.08)
				(name "IO2_A6")
				(number "A6")
			)
			(pin bidirectional line
				(at 35.56 55.88 180)
				(length 5.08)
				(name "IO2_A7")
				(number "A7")
			)
			(pin bidirectional line
				(at 35.56 53.34 180)
				(length 5.08)
				(name "IO2_A8")
				(number "A8")
			)
			(pin bidirectional line
				(at 35.56 50.8 180)
				(length 5.08)
				(name "IO2_A9")
				(number "A9")
			)
			(pin bidirectional line
				(at 35.56 48.26 180)
				(length 5.08)
				(name "IO2_A10")
				(number "A10")
			)
			(pin bidirectional line
				(at 35.56 45.72 180)
				(length 5.08)
				(name "IO2_A11")
				(number "A11")
			)
			(pin bidirectional line
				(at 35.56 43.18 180)
				(length 5.08)
				(name "IO2_A12")
				(number "A12")
			)
			(pin bidirectional line
				(at 35.56 40.64 180)
				(length 5.08)
				(name "IO2_A13")
				(number "A13")
			)
			(pin bidirectional line
				(at 35.56 38.1 180)
				(length 5.08)
				(name "IO2_A15")
				(number "A15")
			)
			(pin bidirectional line
				(at 35.56 35.56 180)
				(length 5.08)
				(name "IO2_B1")
				(number "B1")
			)
			(pin bidirectional line
				(at 35.56 33.02 180)
				(length 5.08)
				(name "IO2_B3")
				(number "B3")
			)
			(pin bidirectional line
				(at 35.56 30.48 180)
				(length 5.08)
				(name "IO2_B4")
				(number "B4")
			)
			(pin bidirectional line
				(at 35.56 27.94 180)
				(length 5.08)
				(name "IO2_B5")
				(number "B5")
			)
			(pin bidirectional line
				(at 35.56 25.4 180)
				(length 5.08)
				(name "IO2_B6")
				(number "B6")
			)
			(pin bidirectional line
				(at 35.56 22.86 180)
				(length 5.08)
				(name "IO2_B7")
				(number "B7")
			)
			(pin bidirectional line
				(at 35.56 20.32 180)
				(length 5.08)
				(name "IO2_B8")
				(number "B8")
			)
			(pin bidirectional line
				(at 35.56 17.78 180)
				(length 5.08)
				(name "IO2_B9")
				(number "B9")
			)
			(pin bidirectional line
				(at 35.56 15.24 180)
				(length 5.08)
				(name "IO2_B10")
				(number "B10")
			)
			(pin bidirectional line
				(at 35.56 12.7 180)
				(length 5.08)
				(name "IO2_B11")
				(number "B11")
			)
			(pin bidirectional line
				(at 35.56 10.16 180)
				(length 5.08)
				(name "IO2_B12")
				(number "B12")
			)
			(pin bidirectional line
				(at 35.56 7.62 180)
				(length 5.08)
				(name "IO2_B13")
				(number "B13")
			)
			(pin bidirectional line
				(at 35.56 5.08 180)
				(length 5.08)
				(name "IO2_B14")
				(number "B14")
			)
			(pin bidirectional line
				(at 35.56 2.54 180)
				(length 5.08)
				(name "IO2_B16")
				(number "B16")
			)
			(pin bidirectional line
				(at 35.56 0 180)
				(length 5.08)
				(name "IO2_C4")
				(number "C4")
			)
			(pin bidirectional line
				(at 35.56 -2.54 180)
				(length 5.08)
				(name "IO2_C5")
				(number "C5")
			)
			(pin bidirectional line
				(at 35.56 -5.08 180)
				(length 5.08)
				(name "IO2_C6")
				(number "C6")
			)
			(pin bidirectional line
				(at 35.56 -7.62 180)
				(length 5.08)
				(name "IO2_C7")
				(number "C7")
			)
			(pin bidirectional line
				(at 35.56 -10.16 180)
				(length 5.08)
				(name "IO2_C8")
				(number "C8")
			)
			(pin bidirectional line
				(at 35.56 -12.7 180)
				(length 5.08)
				(name "IO2_C9")
				(number "C9")
			)
			(pin bidirectional line
				(at 35.56 -15.24 180)
				(length 5.08)
				(name "IO2_C10")
				(number "C10")
			)
			(pin bidirectional line
				(at 35.56 -17.78 180)
				(length 5.08)
				(name "IO2_C11")
				(number "C11")
			)
			(pin bidirectional line
				(at 35.56 -20.32 180)
				(length 5.08)
				(name "IO2_C12")
				(number "C12")
			)
			(pin bidirectional line
				(at 35.56 -22.86 180)
				(length 5.08)
				(name "IO2_C13")
				(number "C13")
			)
			(pin bidirectional line
				(at 35.56 -25.4 180)
				(length 5.08)
				(name "IO2_D4")
				(number "D4")
			)
			(pin bidirectional line
				(at 35.56 -27.94 180)
				(length 5.08)
				(name "IO2_D5")
				(number "D5")
			)
			(pin bidirectional line
				(at 35.56 -30.48 180)
				(length 5.08)
				(name "IO2_D6")
				(number "D6")
			)
			(pin bidirectional line
				(at 35.56 -33.02 180)
				(length 5.08)
				(name "IO2_D7")
				(number "D7")
			)
			(pin bidirectional line
				(at 35.56 -35.56 180)
				(length 5.08)
				(name "IO2_D8")
				(number "D8")
			)
			(pin bidirectional line
				(at 35.56 -38.1 180)
				(length 5.08)
				(name "IO2_D9")
				(number "D9")
			)
			(pin bidirectional line
				(at 35.56 -40.64 180)
				(length 5.08)
				(name "IO2_D10")
				(number "D10")
			)
			(pin bidirectional line
				(at 35.56 -43.18 180)
				(length 5.08)
				(name "IO2_D11")
				(number "D11")
			)
			(pin bidirectional line
				(at 35.56 -45.72 180)
				(length 5.08)
				(name "IO2_D12")
				(number "D12")
			)
			(pin bidirectional line
				(at 35.56 -48.26 180)
				(length 5.08)
				(name "IO2_E6")
				(number "E6")
			)
			(pin bidirectional line
				(at 35.56 -50.8 180)
				(length 5.08)
				(name "IO2_E7")
				(number "E7")
			)
			(pin bidirectional line
				(at 35.56 -53.34 180)
				(length 5.08)
				(name "IO2_E8")
				(number "E8")
			)
			(pin bidirectional line
				(at 35.56 -55.88 180)
				(length 5.08)
				(name "IO2_E9")
				(number "E9")
			)
			(pin bidirectional line
				(at 35.56 -58.42 180)
				(length 5.08)
				(name "IO2_E10")
				(number "E10")
			)
			(pin bidirectional line
				(at 35.56 -60.96 180)
				(length 5.08)
				(name "IO2_E11")
				(number "E11")
			)
		)
		(symbol "EPM2210F256_2_1"
			(pin bidirectional line
				(at -35.56 66.04 0)
				(length 5.08)
				(name "IO3_C14")
				(number "C14")
			)
			(pin bidirectional line
				(at -35.56 63.5 0)
				(length 5.08)
				(name "IO3_C15")
				(number "C15")
			)
			(pin bidirectional line
				(at -35.56 60.96 0)
				(length 5.08)
				(name "IO3_D13")
				(number "D13")
			)
			(pin bidirectional line
				(at -35.56 58.42 0)
				(length 5.08)
				(name "IO3_D14")
				(number "D14")
			)
			(pin bidirectional line
				(at -35.56 55.88 0)
				(length 5.08)
				(name "IO3_D15")
				(number "D15")
			)
			(pin bidirectional line
				(at -35.56 53.34 0)
				(length 5.08)
				(name "IO3_D16")
				(number "D16")
			)
			(pin bidirectional line
				(at -35.56 50.8 0)
				(length 5.08)
				(name "IO3_E12")
				(number "E12")
			)
			(pin bidirectional line
				(at -35.56 48.26 0)
				(length 5.08)
				(name "IO3_E13")
				(number "E13")
			)
			(pin bidirectional line
				(at -35.56 45.72 0)
				(length 5.08)
				(name "IO3_E14")
				(number "E14")
			)
			(pin bidirectional line
				(at -35.56 43.18 0)
				(length 5.08)
				(name "IO3_E15")
				(number "E15")
			)
			(pin bidirectional line
				(at -35.56 40.64 0)
				(length 5.08)
				(name "IO3_E16")
				(number "E16")
			)
			(pin bidirectional line
				(at -35.56 38.1 0)
				(length 5.08)
				(name "IO3_F11")
				(number "F11")
			)
			(pin bidirectional line
				(at -35.56 35.56 0)
				(length 5.08)
				(name "IO3_F12")
				(number "F12")
			)
			(pin bidirectional line
				(at -35.56 33.02 0)
				(length 5.08)
				(name "IO3_F13")
				(number "F13")
			)
			(pin bidirectional line
				(at -35.56 30.48 0)
				(length 5.08)
				(name "IO3_F14")
				(number "F14")
			)
			(pin bidirectional line
				(at -35.56 27.94 0)
				(length 5.08)
				(name "IO3_F15")
				(number "F15")
			)
			(pin bidirectional line
				(at -35.56 25.4 0)
				(length 5.08)
				(name "IO3_F16")
				(number "F16")
			)
			(pin bidirectional line
				(at -35.56 22.86 0)
				(length 5.08)
				(name "IO3_G12")
				(number "G12")
			)
			(pin bidirectional line
				(at -35.56 20.32 0)
				(length 5.08)
				(name "IO3_G13")
				(number "G13")
			)
			(pin bidirectional line
				(at -35.56 17.78 0)
				(length 5.08)
				(name "IO3_G14")
				(number "G14")
			)
			(pin bidirectional line
				(at -35.56 15.24 0)
				(length 5.08)
				(name "IO3_G15")
				(number "G15")
			)
			(pin bidirectional line
				(at -35.56 12.7 0)
				(length 5.08)
				(name "IO3_G16")
				(number "G16")
			)
			(pin bidirectional clock
				(at -35.56 10.16 0)
				(length 5.08)
				(name "IO3_H12/GCLK3")
				(number "H12")
			)
			(pin bidirectional line
				(at -35.56 7.62 0)
				(length 5.08)
				(name "IO3_H13")
				(number "H13")
			)
			(pin bidirectional line
				(at -35.56 5.08 0)
				(length 5.08)
				(name "IO3_H14")
				(number "H14")
			)
			(pin bidirectional line
				(at -35.56 2.54 0)
				(length 5.08)
				(name "IO3_H15")
				(number "H15")
			)
			(pin bidirectional line
				(at -35.56 0 0)
				(length 5.08)
				(name "IO3_H16")
				(number "H16")
			)
			(pin bidirectional clock
				(at -35.56 -2.54 0)
				(length 5.08)
				(name "IO3_J12/GCLK2")
				(number "J12")
			)
			(pin bidirectional line
				(at -35.56 -5.08 0)
				(length 5.08)
				(name "IO3_J13")
				(number "J13")
			)
			(pin bidirectional line
				(at -35.56 -7.62 0)
				(length 5.08)
				(name "IO3_J14")
				(number "J14")
			)
			(pin bidirectional line
				(at -35.56 -10.16 0)
				(length 5.08)
				(name "IO3_J15")
				(number "J15")
			)
			(pin bidirectional line
				(at -35.56 -12.7 0)
				(length 5.08)
				(name "IO3_J16")
				(number "J16")
			)
			(pin bidirectional line
				(at -35.56 -15.24 0)
				(length 5.08)
				(name "IO3_K12")
				(number "K12")
			)
			(pin bidirectional line
				(at -35.56 -17.78 0)
				(length 5.08)
				(name "IO3_K13")
				(number "K13")
			)
			(pin bidirectional line
				(at -35.56 -20.32 0)
				(length 5.08)
				(name "IO3_K14")
				(number "K14")
			)
			(pin bidirectional line
				(at -35.56 -22.86 0)
				(length 5.08)
				(name "IO3_K15")
				(number "K15")
			)
			(pin bidirectional line
				(at -35.56 -25.4 0)
				(length 5.08)
				(name "IO3_K16")
				(number "K16")
			)
			(pin bidirectional line
				(at -35.56 -27.94 0)
				(length 5.08)
				(name "IO3_L11")
				(number "L11")
			)
			(pin bidirectional line
				(at -35.56 -30.48 0)
				(length 5.08)
				(name "IO3_L12")
				(number "L12")
			)
			(pin bidirectional line
				(at -35.56 -33.02 0)
				(length 5.08)
				(name "IO3_L13")
				(number "L13")
			)
			(pin bidirectional line
				(at -35.56 -35.56 0)
				(length 5.08)
				(name "IO3_L14")
				(number "L14")
			)
			(pin bidirectional line
				(at -35.56 -38.1 0)
				(length 5.08)
				(name "IO3_L15")
				(number "L15")
			)
			(pin bidirectional line
				(at -35.56 -40.64 0)
				(length 5.08)
				(name "IO3_L16")
				(number "L16")
			)
			(pin bidirectional line
				(at -35.56 -43.18 0)
				(length 5.08)
				(name "IO3_M13")
				(number "M13")
			)
			(pin bidirectional line
				(at -35.56 -45.72 0)
				(length 5.08)
				(name "IO3_M14")
				(number "M14")
			)
			(pin bidirectional line
				(at -35.56 -48.26 0)
				(length 5.08)
				(name "IO3_M15")
				(number "M15")
			)
			(pin bidirectional line
				(at -35.56 -50.8 0)
				(length 5.08)
				(name "IO3_M16")
				(number "M16")
			)
			(pin bidirectional line
				(at -35.56 -53.34 0)
				(length 5.08)
				(name "IO3_N13")
				(number "N13")
			)
			(pin bidirectional line
				(at -35.56 -55.88 0)
				(length 5.08)
				(name "IO3_N14")
				(number "N14")
			)
			(pin bidirectional line
				(at -35.56 -58.42 0)
				(length 5.08)
				(name "IO3_N15")
				(number "N15")
			)
			(pin bidirectional line
				(at -35.56 -60.96 0)
				(length 5.08)
				(name "IO3_N16")
				(number "N16")
			)
			(pin bidirectional line
				(at -35.56 -63.5 0)
				(length 5.08)
				(name "IO3_P14")
				(number "P14")
			)
			(pin bidirectional line
				(at -35.56 -66.04 0)
				(length 5.08)
				(name "IO3_P15")
				(number "P15")
			)
			(pin power_in line
				(at -12.7 -73.66 90)
				(length 5.08)
				(name "GNDIO")
				(number "G9")
			)
			(pin power_in line
				(at -10.16 73.66 270)
				(length 5.08)
				(name "VCCIO3")
				(number "C16")
			)
			(pin power_in line
				(at -10.16 -73.66 90)
				(length 5.08)
				(name "GNDIO")
				(number "G10")
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VCCIO3")
				(number "H11")
			)
			(pin power_in line
				(at -7.62 -73.66 90)
				(length 5.08)
				(name "GNDIO")
				(number "K7")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VCCIO3")
				(number "J11")
			)
			(pin power_in line
				(at -5.08 -73.66 90)
				(length 5.08)
				(name "GNDIO")
				(number "K8")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VCCIO3")
				(number "P16")
			)
			(pin power_in line
				(at -2.54 -73.66 90)
				(length 5.08)
				(name "GNDIO")
				(number "K9")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VCCIO4")
				(number "L8")
			)
			(pin power_in line
				(at 0 -73.66 90)
				(length 5.08)
				(name "GNDIO")
				(number "K10")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VCCIO4")
				(number "L9")
			)
			(pin power_in line
				(at 2.54 -73.66 90)
				(length 5.08)
				(name "GNDIO")
				(number "R2")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VCCIO4")
				(number "T3")
			)
			(pin power_in line
				(at 5.08 -73.66 90)
				(length 5.08)
				(name "GNDIO")
				(number "R15")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VCCIO4")
				(number "T14")
			)
			(pin power_in line
				(at 7.62 -73.66 90)
				(length 5.08)
				(name "GNDIO")
				(number "T1")
			)
			(pin power_in line
				(at 10.16 -73.66 90)
				(length 5.08)
				(name "GNDIO")
				(number "T16")
			)
			(pin bidirectional line
				(at 35.56 66.04 180)
				(length 5.08)
				(name "IO4_M6")
				(number "M6")
			)
			(pin bidirectional line
				(at 35.56 63.5 180)
				(length 5.08)
				(name "IO4_M7")
				(number "M7")
			)
			(pin bidirectional line
				(at 35.56 60.96 180)
				(length 5.08)
				(name "IO4_M8/DEV_OE")
				(number "M8")
			)
			(pin bidirectional line
				(at 35.56 58.42 180)
				(length 5.08)
				(name "IO4_M9/DEV_CLRn")
				(number "M9")
			)
			(pin bidirectional line
				(at 35.56 55.88 180)
				(length 5.08)
				(name "IO4_M10")
				(number "M10")
			)
			(pin bidirectional line
				(at 35.56 53.34 180)
				(length 5.08)
				(name "IO4_M11")
				(number "M11")
			)
			(pin bidirectional line
				(at 35.56 50.8 180)
				(length 5.08)
				(name "IO4_M12")
				(number "M12")
			)
			(pin bidirectional line
				(at 35.56 48.26 180)
				(length 5.08)
				(name "IO4_N5")
				(number "N5")
			)
			(pin bidirectional line
				(at 35.56 45.72 180)
				(length 5.08)
				(name "IO4_N6")
				(number "N6")
			)
			(pin bidirectional line
				(at 35.56 43.18 180)
				(length 5.08)
				(name "IO4_N7")
				(number "N7")
			)
			(pin bidirectional line
				(at 35.56 40.64 180)
				(length 5.08)
				(name "IO4_N8")
				(number "N8")
			)
			(pin bidirectional line
				(at 35.56 38.1 180)
				(length 5.08)
				(name "IO4_N9")
				(number "N9")
			)
			(pin bidirectional line
				(at 35.56 35.56 180)
				(length 5.08)
				(name "IO4_N10")
				(number "N10")
			)
			(pin bidirectional line
				(at 35.56 33.02 180)
				(length 5.08)
				(name "IO4_N11")
				(number "N11")
			)
			(pin bidirectional line
				(at 35.56 30.48 180)
				(length 5.08)
				(name "IO4_N12")
				(number "N12")
			)
			(pin bidirectional line
				(at 35.56 27.94 180)
				(length 5.08)
				(name "IO4_P4")
				(number "P4")
			)
			(pin bidirectional line
				(at 35.56 25.4 180)
				(length 5.08)
				(name "IO4_P5")
				(number "P5")
			)
			(pin bidirectional line
				(at 35.56 22.86 180)
				(length 5.08)
				(name "IO4_P6")
				(number "P6")
			)
			(pin bidirectional line
				(at 35.56 20.32 180)
				(length 5.08)
				(name "IO4_P7")
				(number "P7")
			)
			(pin bidirectional line
				(at 35.56 17.78 180)
				(length 5.08)
				(name "IO4_P8")
				(number "P8")
			)
			(pin bidirectional line
				(at 35.56 15.24 180)
				(length 5.08)
				(name "IO4_P9")
				(number "P9")
			)
			(pin bidirectional line
				(at 35.56 12.7 180)
				(length 5.08)
				(name "IO4_P10")
				(number "P10")
			)
			(pin bidirectional line
				(at 35.56 10.16 180)
				(length 5.08)
				(name "IO4_P11")
				(number "P11")
			)
			(pin bidirectional line
				(at 35.56 7.62 180)
				(length 5.08)
				(name "IO4_P12")
				(number "P12")
			)
			(pin bidirectional line
				(at 35.56 5.08 180)
				(length 5.08)
				(name "IO4_P13")
				(number "P13")
			)
			(pin bidirectional line
				(at 35.56 2.54 180)
				(length 5.08)
				(name "IO4_R1")
				(number "R1")
			)
			(pin bidirectional line
				(at 35.56 0 180)
				(length 5.08)
				(name "IO4_R3")
				(number "R3")
			)
			(pin bidirectional line
				(at 35.56 -2.54 180)
				(length 5.08)
				(name "IO4_R4")
				(number "R4")
			)
			(pin bidirectional line
				(at 35.56 -5.08 180)
				(length 5.08)
				(name "IO4_R5")
				(number "R5")
			)
			(pin bidirectional line
				(at 35.56 -7.62 180)
				(length 5.08)
				(name "IO4_R6")
				(number "R6")
			)
			(pin bidirectional line
				(at 35.56 -10.16 180)
				(length 5.08)
				(name "IO4_R7")
				(number "R7")
			)
			(pin bidirectional line
				(at 35.56 -12.7 180)
				(length 5.08)
				(name "IO4_R8")
				(number "R8")
			)
			(pin bidirectional line
				(at 35.56 -15.24 180)
				(length 5.08)
				(name "IO4_R9")
				(number "R9")
			)
			(pin bidirectional line
				(at 35.56 -17.78 180)
				(length 5.08)
				(name "IO4_R10")
				(number "R10")
			)
			(pin bidirectional line
				(at 35.56 -20.32 180)
				(length 5.08)
				(name "IO4_R11")
				(number "R11")
			)
			(pin bidirectional line
				(at 35.56 -22.86 180)
				(length 5.08)
				(name "IO4_R12")
				(number "R12")
			)
			(pin bidirectional line
				(at 35.56 -25.4 180)
				(length 5.08)
				(name "IO4_R13")
				(number "R13")
			)
			(pin bidirectional line
				(at 35.56 -27.94 180)
				(length 5.08)
				(name "IO4_R14")
				(number "R14")
			)
			(pin bidirectional line
				(at 35.56 -30.48 180)
				(length 5.08)
				(name "IO4_R16")
				(number "R16")
			)
			(pin bidirectional line
				(at 35.56 -33.02 180)
				(length 5.08)
				(name "IO4_T2")
				(number "T2")
			)
			(pin bidirectional line
				(at 35.56 -35.56 180)
				(length 5.08)
				(name "IO4_T4")
				(number "T4")
			)
			(pin bidirectional line
				(at 35.56 -38.1 180)
				(length 5.08)
				(name "IO4_T5")
				(number "T5")
			)
			(pin bidirectional line
				(at 35.56 -40.64 180)
				(length 5.08)
				(name "IO4_T6")
				(number "T6")
			)
			(pin bidirectional line
				(at 35.56 -43.18 180)
				(length 5.08)
				(name "IO4_T7")
				(number "T7")
			)
			(pin bidirectional line
				(at 35.56 -45.72 180)
				(length 5.08)
				(name "IO4_T8")
				(number "T8")
			)
			(pin bidirectional line
				(at 35.56 -48.26 180)
				(length 5.08)
				(name "IO4_T9")
				(number "T9")
			)
			(pin bidirectional line
				(at 35.56 -50.8 180)
				(length 5.08)
				(name "IO4_T10")
				(number "T10")
			)
			(pin bidirectional line
				(at 35.56 -53.34 180)
				(length 5.08)
				(name "IO4_T11")
				(number "T11")
			)
			(pin bidirectional line
				(at 35.56 -55.88 180)
				(length 5.08)
				(name "IO4_T12")
				(number "T12")
			)
			(pin bidirectional line
				(at 35.56 -58.42 180)
				(length 5.08)
				(name "IO4_T13")
				(number "T13")
			)
			(pin bidirectional line
				(at 35.56 -60.96 180)
				(length 5.08)
				(name "IO4_T15")
				(number "T15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EPM2210F324"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 20.32 95.25 0)
		)
		(property "Value" "EPM2210F324"
			(at 17.78 -95.25 0)
		)
		(property "Footprint" "Package_BGA:BGA-324_19.0x19.0mm_Layout18x18_P1.0mm_Ball0.5mm_Pad0.4mm_NSMD"
			(at 17.78 -97.79 0)
		)
		(property "Datasheet" "https://www.altera.com/content/dam/altera-www/global/en_US/pdfs/literature/hb/max2/max2_mii5v1.pdf"
			(at 0 0 0)
		)
		(property "Description" "Altera MAX2 CPLD with 2210 LE"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "MAX2 FBGA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*BGA*P1.0mm*"
			(at 0 0 0)
		)
		(symbol "EPM2210F324_1_1"
			(pin bidirectional line
				(at -35.56 91.44 0)
				(length 5.08)
				(name "IO1_C2")
				(number "C2")
			)
			(pin bidirectional line
				(at -35.56 88.9 0)
				(length 5.08)
				(name "IO1_C3")
				(number "C3")
			)
			(pin bidirectional line
				(at -35.56 86.36 0)
				(length 5.08)
				(name "IO1_D1")
				(number "D1")
			)
			(pin bidirectional line
				(at -35.56 83.82 0)
				(length 5.08)
				(name "IO1_D2")
				(number "D2")
			)
			(pin bidirectional line
				(at -35.56 81.28 0)
				(length 5.08)
				(name "IO1_D3")
				(number "D3")
			)
			(pin bidirectional line
				(at -35.56 78.74 0)
				(length 5.08)
				(name "IO1_D4")
				(number "D4")
			)
			(pin bidirectional line
				(at -35.56 76.2 0)
				(length 5.08)
				(name "IO1_E1")
				(number "E1")
			)
			(pin bidirectional line
				(at -35.56 73.66 0)
				(length 5.08)
				(name "IO1_E2")
				(number "E2")
			)
			(pin bidirectional line
				(at -35.56 71.12 0)
				(length 5.08)
				(name "IO1_E3")
				(number "E3")
			)
			(pin bidirectional line
				(at -35.56 68.58 0)
				(length 5.08)
				(name "IO1_E4")
				(number "E4")
			)
			(pin bidirectional line
				(at -35.56 66.04 0)
				(length 5.08)
				(name "IO1_E5")
				(number "E5")
			)
			(pin bidirectional line
				(at -35.56 63.5 0)
				(length 5.08)
				(name "IO1_F1")
				(number "F1")
			)
			(pin bidirectional line
				(at -35.56 60.96 0)
				(length 5.08)
				(name "IO1_F2")
				(number "F2")
			)
			(pin bidirectional line
				(at -35.56 58.42 0)
				(length 5.08)
				(name "IO1_F3")
				(number "F3")
			)
			(pin bidirectional line
				(at -35.56 55.88 0)
				(length 5.08)
				(name "IO1_F4")
				(number "F4")
			)
			(pin bidirectional line
				(at -35.56 53.34 0)
				(length 5.08)
				(name "IO1_F5")
				(number "F5")
			)
			(pin bidirectional line
				(at -35.56 50.8 0)
				(length 5.08)
				(name "IO1_F6")
				(number "F6")
			)
			(pin bidirectional line
				(at -35.56 48.26 0)
				(length 5.08)
				(name "IO1_G1")
				(number "G1")
			)
			(pin bidirectional line
				(at -35.56 45.72 0)
				(length 5.08)
				(name "IO1_G2")
				(number "G2")
			)
			(pin bidirectional line
				(at -35.56 43.18 0)
				(length 5.08)
				(name "IO1_G3")
				(number "G3")
			)
			(pin bidirectional line
				(at -35.56 40.64 0)
				(length 5.08)
				(name "IO1_G4")
				(number "G4")
			)
			(pin bidirectional line
				(at -35.56 38.1 0)
				(length 5.08)
				(name "IO1_G5")
				(number "G5")
			)
			(pin bidirectional line
				(at -35.56 35.56 0)
				(length 5.08)
				(name "IO1_G6")
				(number "G6")
			)
			(pin bidirectional line
				(at -35.56 33.02 0)
				(length 5.08)
				(name "IO1_G7")
				(number "G7")
			)
			(pin bidirectional line
				(at -35.56 30.48 0)
				(length 5.08)
				(name "IO1_H1")
				(number "H1")
			)
			(pin bidirectional line
				(at -35.56 27.94 0)
				(length 5.08)
				(name "IO1_H2")
				(number "H2")
			)
			(pin bidirectional line
				(at -35.56 25.4 0)
				(length 5.08)
				(name "IO1_H3")
				(number "H3")
			)
			(pin bidirectional line
				(at -35.56 22.86 0)
				(length 5.08)
				(name "IO1_H4")
				(number "H4")
			)
			(pin bidirectional line
				(at -35.56 20.32 0)
				(length 5.08)
				(name "IO1_H5")
				(number "H5")
			)
			(pin bidirectional line
				(at -35.56 17.78 0)
				(length 5.08)
				(name "IO1_H6")
				(number "H6")
			)
			(pin bidirectional line
				(at -35.56 15.24 0)
				(length 5.08)
				(name "IO1_J1")
				(number "J1")
			)
			(pin bidirectional line
				(at -35.56 12.7 0)
				(length 5.08)
				(name "IO1_J2")
				(number "J2")
			)
			(pin bidirectional line
				(at -35.56 10.16 0)
				(length 5.08)
				(name "IO1_J3")
				(number "J3")
			)
			(pin bidirectional line
				(at -35.56 7.62 0)
				(length 5.08)
				(name "IO1_J4")
				(number "J4")
			)
			(pin bidirectional line
				(at -35.56 5.08 0)
				(length 5.08)
				(name "IO1_J5")
				(number "J5")
			)
			(pin bidirectional clock
				(at -35.56 2.54 0)
				(length 5.08)
				(name "IO1_J6/GCLK0")
				(number "J6")
			)
			(pin bidirectional line
				(at -35.56 0 0)
				(length 5.08)
				(name "IO1_K1")
				(number "K1")
			)
			(pin bidirectional line
				(at -35.56 -2.54 0)
				(length 5.08)
				(name "IO1_K2")
				(number "K2")
			)
			(pin bidirectional line
				(at -35.56 -5.08 0)
				(length 5.08)
				(name "IO1_K3")
				(number "K3")
			)
			(pin bidirectional line
				(at -35.56 -7.62 0)
				(length 5.08)
				(name "IO1_K4")
				(number "K4")
			)
			(pin bidirectional line
				(at -35.56 -10.16 0)
				(length 5.08)
				(name "IO1_K5")
				(number "K5")
			)
			(pin bidirectional clock
				(at -35.56 -12.7 0)
				(length 5.08)
				(name "IO1_K6/GCLK1")
				(number "K6")
			)
			(pin bidirectional line
				(at -35.56 -15.24 0)
				(length 5.08)
				(name "IO1_L1")
				(number "L1")
			)
			(pin bidirectional line
				(at -35.56 -17.78 0)
				(length 5.08)
				(name "IO1_L2")
				(number "L2")
			)
			(pin bidirectional line
				(at -35.56 -20.32 0)
				(length 5.08)
				(name "IO1_L3")
				(number "L3")
			)
			(pin bidirectional line
				(at -35.56 -22.86 0)
				(length 5.08)
				(name "IO1_L4")
				(number "L4")
			)
			(pin bidirectional line
				(at -35.56 -25.4 0)
				(length 5.08)
				(name "IO1_L5")
				(number "L5")
			)
			(pin bidirectional line
				(at -35.56 -27.94 0)
				(length 5.08)
				(name "IO1_L6")
				(number "L6")
			)
			(pin bidirectional line
				(at -35.56 -30.48 0)
				(length 5.08)
				(name "IO1_M1")
				(number "M1")
			)
			(pin bidirectional line
				(at -35.56 -33.02 0)
				(length 5.08)
				(name "IO1_M2")
				(number "M2")
			)
			(pin bidirectional line
				(at -35.56 -35.56 0)
				(length 5.08)
				(name "IO1_M3")
				(number "M3")
			)
			(pin bidirectional line
				(at -35.56 -38.1 0)
				(length 5.08)
				(name "IO1_M4")
				(number "M4")
			)
			(pin bidirectional line
				(at -35.56 -40.64 0)
				(length 5.08)
				(name "IO1_M5")
				(number "M5")
			)
			(pin bidirectional line
				(at -35.56 -43.18 0)
				(length 5.08)
				(name "IO1_M6")
				(number "M6")
			)
			(pin bidirectional line
				(at -35.56 -45.72 0)
				(length 5.08)
				(name "IO1_N1")
				(number "N1")
			)
			(pin bidirectional line
				(at -35.56 -48.26 0)
				(length 5.08)
				(name "IO1_N2")
				(number "N2")
			)
			(pin bidirectional line
				(at -35.56 -50.8 0)
				(length 5.08)
				(name "IO1_N3")
				(number "N3")
			)
			(pin bidirectional line
				(at -35.56 -53.34 0)
				(length 5.08)
				(name "IO1_N4")
				(number "N4")
			)
			(pin bidirectional line
				(at -35.56 -55.88 0)
				(length 5.08)
				(name "IO1_N5")
				(number "N5")
			)
			(pin bidirectional line
				(at -35.56 -58.42 0)
				(length 5.08)
				(name "IO1_P1")
				(number "P1")
			)
			(pin bidirectional line
				(at -35.56 -60.96 0)
				(length 5.08)
				(name "IO1_P2")
				(number "P2")
			)
			(pin bidirectional line
				(at -35.56 -63.5 0)
				(length 5.08)
				(name "IO1_P3")
				(number "P3")
			)
			(pin bidirectional line
				(at -35.56 -66.04 0)
				(length 5.08)
				(name "IO1_P4")
				(number "P4")
			)
			(pin bidirectional line
				(at -35.56 -68.58 0)
				(length 5.08)
				(name "IO1_R1")
				(number "R1")
			)
			(pin bidirectional line
				(at -35.56 -71.12 0)
				(length 5.08)
				(name "IO1_R2")
				(number "R2")
			)
			(pin bidirectional line
				(at -35.56 -73.66 0)
				(length 5.08)
				(name "IO1_R3")
				(number "R3")
			)
			(pin bidirectional line
				(at -35.56 -76.2 0)
				(length 5.08)
				(name "IO1_T2")
				(number "T2")
			)
			(pin bidirectional line
				(at -35.56 -78.74 0)
				(length 5.08)
				(name "IO1_T3")
				(number "T3")
			)
			(pin input line
				(at -35.56 -81.28 0)
				(length 5.08)
				(name "TMS")
				(number "P5")
			)
			(pin input line
				(at -35.56 -83.82 0)
				(length 5.08)
				(name "TDI")
				(number "M7")
			)
			(pin input clock
				(at -35.56 -86.36 0)
				(length 5.08)
				(name "TCK")
				(number "R4")
			)
			(pin output line
				(at -35.56 -88.9 0)
				(length 5.08)
				(name "TDO")
				(number "N6")
			)
			(pin power_in line
				(at -20.32 99.06 270)
				(length 5.08)
				(name "VCCINT")
				(number "G11")
			)
			(pin power_in line
				(at -17.78 99.06 270)
				(length 5.08)
				(name "VCCINT")
				(number "H12")
			)
			(pin power_in line
				(at -17.78 -99.06 90)
				(length 5.08)
				(name "GNDINT")
				(number "G8")
			)
			(pin power_in line
				(at -15.24 99.06 270)
				(length 5.08)
				(name "VCCINT")
				(number "J9")
			)
			(pin power_in line
				(at -15.24 -99.06 90)
				(length 5.08)
				(name "GNDINT")
				(number "H7")
			)
			(pin power_in line
				(at -12.7 99.06 270)
				(length 5.08)
				(name "VCCINT")
				(number "J11")
			)
			(pin power_in line
				(at -12.7 -99.06 90)
				(length 5.08)
				(name "GNDINT")
				(number "J8")
			)
			(pin power_in line
				(at -10.16 99.06 270)
				(length 5.08)
				(name "VCCINT")
				(number "K8")
			)
			(pin power_in line
				(at -10.16 -99.06 90)
				(length 5.08)
				(name "GNDINT")
				(number "J10")
			)
			(pin power_in line
				(at -7.62 99.06 270)
				(length 5.08)
				(name "VCCINT")
				(number "K10")
			)
			(pin power_in line
				(at -7.62 -99.06 90)
				(length 5.08)
				(name "GNDINT")
				(number "K9")
			)
			(pin power_in line
				(at -5.08 99.06 270)
				(length 5.08)
				(name "VCCINT")
				(number "L7")
			)
			(pin power_in line
				(at -5.08 -99.06 90)
				(length 5.08)
				(name "GNDINT")
				(number "K11")
			)
			(pin power_in line
				(at -2.54 99.06 270)
				(length 5.08)
				(name "VCCINT")
				(number "M8")
			)
			(pin power_in line
				(at -2.54 -99.06 90)
				(length 5.08)
				(name "GNDINT")
				(number "L12")
			)
			(pin power_in line
				(at 0 99.06 270)
				(length 5.08)
				(name "VCCIO1")
				(number "C1")
			)
			(pin power_in line
				(at 0 -99.06 90)
				(length 5.08)
				(name "GNDINT")
				(number "M11")
			)
			(pin power_in line
				(at 2.54 99.06 270)
				(length 5.08)
				(name "VCCIO1")
				(number "J7")
			)
			(pin power_in line
				(at 2.54 -99.06 90)
				(length 5.08)
				(name "GNDIO")
				(number "A1")
			)
			(pin power_in line
				(at 5.08 99.06 270)
				(length 5.08)
				(name "VCCIO1")
				(number "K7")
			)
			(pin power_in line
				(at 5.08 -99.06 90)
				(length 5.08)
				(name "GNDIO")
				(number "A18")
			)
			(pin power_in line
				(at 7.62 99.06 270)
				(length 5.08)
				(name "VCCIO1")
				(number "T1")
			)
			(pin power_in line
				(at 7.62 -99.06 90)
				(length 5.08)
				(name "GNDIO")
				(number "B2")
			)
			(pin power_in line
				(at 10.16 99.06 270)
				(length 5.08)
				(name "VCCIO2")
				(number "A3")
			)
			(pin power_in line
				(at 10.16 -99.06 90)
				(length 5.08)
				(name "GNDIO")
				(number "B17")
			)
			(pin power_in line
				(at 12.7 99.06 270)
				(length 5.08)
				(name "VCCIO2")
				(number "A16")
			)
			(pin power_in line
				(at 12.7 -99.06 90)
				(length 5.08)
				(name "GNDIO")
				(number "H8")
			)
			(pin power_in line
				(at 15.24 99.06 270)
				(length 5.08)
				(name "VCCIO2")
				(number "G9")
			)
			(pin power_in line
				(at 15.24 -99.06 90)
				(length 5.08)
				(name "GNDIO")
				(number "H9")
			)
			(pin power_in line
				(at 17.78 99.06 270)
				(length 5.08)
				(name "VCCIO2")
				(number "G10")
			)
			(pin bidirectional line
				(at 35.56 91.44 180)
				(length 5.08)
				(name "IO2_A2")
				(number "A2")
			)
			(pin bidirectional line
				(at 35.56 88.9 180)
				(length 5.08)
				(name "IO2_A4")
				(number "A4")
			)
			(pin bidirectional line
				(at 35.56 86.36 180)
				(length 5.08)
				(name "IO2_A5")
				(number "A5")
			)
			(pin bidirectional line
				(at 35.56 83.82 180)
				(length 5.08)
				(name "IO2_A6")
				(number "A6")
			)
			(pin bidirectional line
				(at 35.56 81.28 180)
				(length 5.08)
				(name "IO2_A7")
				(number "A7")
			)
			(pin bidirectional line
				(at 35.56 78.74 180)
				(length 5.08)
				(name "IO2_A8")
				(number "A8")
			)
			(pin bidirectional line
				(at 35.56 76.2 180)
				(length 5.08)
				(name "IO2_A9")
				(number "A9")
			)
			(pin bidirectional line
				(at 35.56 73.66 180)
				(length 5.08)
				(name "IO2_A10")
				(number "A10")
			)
			(pin bidirectional line
				(at 35.56 71.12 180)
				(length 5.08)
				(name "IO2_A11")
				(number "A11")
			)
			(pin bidirectional line
				(at 35.56 68.58 180)
				(length 5.08)
				(name "IO2_A12")
				(number "A12")
			)
			(pin bidirectional line
				(at 35.56 66.04 180)
				(length 5.08)
				(name "IO2_A13")
				(number "A13")
			)
			(pin bidirectional line
				(at 35.56 63.5 180)
				(length 5.08)
				(name "IO2_A14")
				(number "A14")
			)
			(pin bidirectional line
				(at 35.56 60.96 180)
				(length 5.08)
				(name "IO2_A15")
				(number "A15")
			)
			(pin bidirectional line
				(at 35.56 58.42 180)
				(length 5.08)
				(name "IO2_A17")
				(number "A17")
			)
			(pin bidirectional line
				(at 35.56 55.88 180)
				(length 5.08)
				(name "IO2_B1")
				(number "B1")
			)
			(pin bidirectional line
				(at 35.56 53.34 180)
				(length 5.08)
				(name "IO2_B3")
				(number "B3")
			)
			(pin bidirectional line
				(at 35.56 50.8 180)
				(length 5.08)
				(name "IO2_B4")
				(number "B4")
			)
			(pin bidirectional line
				(at 35.56 48.26 180)
				(length 5.08)
				(name "IO2_B5")
				(number "B5")
			)
			(pin bidirectional line
				(at 35.56 45.72 180)
				(length 5.08)
				(name "IO2_B6")
				(number "B6")
			)
			(pin bidirectional line
				(at 35.56 43.18 180)
				(length 5.08)
				(name "IO2_B7")
				(number "B7")
			)
			(pin bidirectional line
				(at 35.56 40.64 180)
				(length 5.08)
				(name "IO2_B8")
				(number "B8")
			)
			(pin bidirectional line
				(at 35.56 38.1 180)
				(length 5.08)
				(name "IO2_B9")
				(number "B9")
			)
			(pin bidirectional line
				(at 35.56 35.56 180)
				(length 5.08)
				(name "IO2_B10")
				(number "B10")
			)
			(pin bidirectional line
				(at 35.56 33.02 180)
				(length 5.08)
				(name "IO2_B11")
				(number "B11")
			)
			(pin bidirectional line
				(at 35.56 30.48 180)
				(length 5.08)
				(name "IO2_B12")
				(number "B12")
			)
			(pin bidirectional line
				(at 35.56 27.94 180)
				(length 5.08)
				(name "IO2_B13")
				(number "B13")
			)
			(pin bidirectional line
				(at 35.56 25.4 180)
				(length 5.08)
				(name "IO2_B14")
				(number "B14")
			)
			(pin bidirectional line
				(at 35.56 22.86 180)
				(length 5.08)
				(name "IO2_B15")
				(number "B15")
			)
			(pin bidirectional line
				(at 35.56 20.32 180)
				(length 5.08)
				(name "IO2_B16")
				(number "B16")
			)
			(pin bidirectional line
				(at 35.56 17.78 180)
				(length 5.08)
				(name "IO2_B18")
				(number "B18")
			)
			(pin bidirectional line
				(at 35.56 15.24 180)
				(length 5.08)
				(name "IO2_C4")
				(number "C4")
			)
			(pin bidirectional line
				(at 35.56 12.7 180)
				(length 5.08)
				(name "IO2_C5")
				(number "C5")
			)
			(pin bidirectional line
				(at 35.56 10.16 180)
				(length 5.08)
				(name "IO2_C6")
				(number "C6")
			)
			(pin bidirectional line
				(at 35.56 7.62 180)
				(length 5.08)
				(name "IO2_C7")
				(number "C7")
			)
			(pin bidirectional line
				(at 35.56 5.08 180)
				(length 5.08)
				(name "IO2_C8")
				(number "C8")
			)
			(pin bidirectional line
				(at 35.56 2.54 180)
				(length 5.08)
				(name "IO2_C9")
				(number "C9")
			)
			(pin bidirectional line
				(at 35.56 0 180)
				(length 5.08)
				(name "IO2_C10")
				(number "C10")
			)
			(pin bidirectional line
				(at 35.56 -2.54 180)
				(length 5.08)
				(name "IO2_C11")
				(number "C11")
			)
			(pin bidirectional line
				(at 35.56 -5.08 180)
				(length 5.08)
				(name "IO2_C12")
				(number "C12")
			)
			(pin bidirectional line
				(at 35.56 -7.62 180)
				(length 5.08)
				(name "IO2_C13")
				(number "C13")
			)
			(pin bidirectional line
				(at 35.56 -10.16 180)
				(length 5.08)
				(name "IO2_C14")
				(number "C14")
			)
			(pin bidirectional line
				(at 35.56 -12.7 180)
				(length 5.08)
				(name "IO2_C15")
				(number "C15")
			)
			(pin bidirectional line
				(at 35.56 -15.24 180)
				(length 5.08)
				(name "IO2_D5")
				(number "D5")
			)
			(pin bidirectional line
				(at 35.56 -17.78 180)
				(length 5.08)
				(name "IO2_D6")
				(number "D6")
			)
			(pin bidirectional line
				(at 35.56 -20.32 180)
				(length 5.08)
				(name "IO2_D7")
				(number "D7")
			)
			(pin bidirectional line
				(at 35.56 -22.86 180)
				(length 5.08)
				(name "IO2_D8")
				(number "D8")
			)
			(pin bidirectional line
				(at 35.56 -25.4 180)
				(length 5.08)
				(name "IO2_D9")
				(number "D9")
			)
			(pin bidirectional line
				(at 35.56 -27.94 180)
				(length 5.08)
				(name "IO2_D10")
				(number "D10")
			)
			(pin bidirectional line
				(at 35.56 -30.48 180)
				(length 5.08)
				(name "IO2_D11")
				(number "D11")
			)
			(pin bidirectional line
				(at 35.56 -33.02 180)
				(length 5.08)
				(name "IO2_D12")
				(number "D12")
			)
			(pin bidirectional line
				(at 35.56 -35.56 180)
				(length 5.08)
				(name "IO2_D13")
				(number "D13")
			)
			(pin bidirectional line
				(at 35.56 -38.1 180)
				(length 5.08)
				(name "IO2_D14")
				(number "D14")
			)
			(pin bidirectional line
				(at 35.56 -40.64 180)
				(length 5.08)
				(name "IO2_E6")
				(number "E6")
			)
			(pin bidirectional line
				(at 35.56 -43.18 180)
				(length 5.08)
				(name "IO2_E7")
				(number "E7")
			)
			(pin bidirectional line
				(at 35.56 -45.72 180)
				(length 5.08)
				(name "IO2_E8")
				(number "E8")
			)
			(pin bidirectional line
				(at 35.56 -48.26 180)
				(length 5.08)
				(name "IO2_E9")
				(number "E9")
			)
			(pin bidirectional line
				(at 35.56 -50.8 180)
				(length 5.08)
				(name "IO2_E10")
				(number "E10")
			)
			(pin bidirectional line
				(at 35.56 -53.34 180)
				(length 5.08)
				(name "IO2_E11")
				(number "E11")
			)
			(pin bidirectional line
				(at 35.56 -55.88 180)
				(length 5.08)
				(name "IO2_E12")
				(number "E12")
			)
			(pin bidirectional line
				(at 35.56 -58.42 180)
				(length 5.08)
				(name "IO2_E13")
				(number "E13")
			)
			(pin bidirectional line
				(at 35.56 -60.96 180)
				(length 5.08)
				(name "IO2_F7")
				(number "F7")
			)
			(pin bidirectional line
				(at 35.56 -63.5 180)
				(length 5.08)
				(name "IO2_F8")
				(number "F8")
			)
			(pin bidirectional line
				(at 35.56 -66.04 180)
				(length 5.08)
				(name "IO2_F9")
				(number "F9")
			)
			(pin bidirectional line
				(at 35.56 -68.58 180)
				(length 5.08)
				(name "IO2_F10")
				(number "F10")
			)
			(pin bidirectional line
				(at 35.56 -71.12 180)
				(length 5.08)
				(name "IO2_F11")
				(number "F11")
			)
			(pin bidirectional line
				(at 35.56 -73.66 180)
				(length 5.08)
				(name "IO2_F12")
				(number "F12")
			)
		)
		(symbol "EPM2210F324_2_1"
			(pin bidirectional line
				(at -35.56 91.44 0)
				(length 5.08)
				(name "IO3_C16")
				(number "C16")
			)
			(pin bidirectional line
				(at -35.56 88.9 0)
				(length 5.08)
				(name "IO3_C17")
				(number "C17")
			)
			(pin bidirectional line
				(at -35.56 86.36 0)
				(length 5.08)
				(name "IO3_D15")
				(number "D15")
			)
			(pin bidirectional line
				(at -35.56 83.82 0)
				(length 5.08)
				(name "IO3_D16")
				(number "D16")
			)
			(pin bidirectional line
				(at -35.56 81.28 0)
				(length 5.08)
				(name "IO3_D17")
				(number "D17")
			)
			(pin bidirectional line
				(at -35.56 78.74 0)
				(length 5.08)
				(name "IO3_D18")
				(number "D18")
			)
			(pin bidirectional line
				(at -35.56 76.2 0)
				(length 5.08)
				(name "IO3_E14")
				(number "E14")
			)
			(pin bidirectional line
				(at -35.56 73.66 0)
				(length 5.08)
				(name "IO3_E15")
				(number "E15")
			)
			(pin bidirectional line
				(at -35.56 71.12 0)
				(length 5.08)
				(name "IO3_E16")
				(number "E16")
			)
			(pin bidirectional line
				(at -35.56 68.58 0)
				(length 5.08)
				(name "IO3_E17")
				(number "E17")
			)
			(pin bidirectional line
				(at -35.56 66.04 0)
				(length 5.08)
				(name "IO3_E18")
				(number "E18")
			)
			(pin bidirectional line
				(at -35.56 63.5 0)
				(length 5.08)
				(name "IO3_F13")
				(number "F13")
			)
			(pin bidirectional line
				(at -35.56 60.96 0)
				(length 5.08)
				(name "IO3_F14")
				(number "F14")
			)
			(pin bidirectional line
				(at -35.56 58.42 0)
				(length 5.08)
				(name "IO3_F15")
				(number "F15")
			)
			(pin bidirectional line
				(at -35.56 55.88 0)
				(length 5.08)
				(name "IO3_F16")
				(number "F16")
			)
			(pin bidirectional line
				(at -35.56 53.34 0)
				(length 5.08)
				(name "IO3_F17")
				(number "F17")
			)
			(pin bidirectional line
				(at -35.56 50.8 0)
				(length 5.08)
				(name "IO3_F18")
				(number "F18")
			)
			(pin bidirectional line
				(at -35.56 48.26 0)
				(length 5.08)
				(name "IO3_G12")
				(number "G12")
			)
			(pin bidirectional line
				(at -35.56 45.72 0)
				(length 5.08)
				(name "IO3_G13")
				(number "G13")
			)
			(pin bidirectional line
				(at -35.56 43.18 0)
				(length 5.08)
				(name "IO3_G14")
				(number "G14")
			)
			(pin bidirectional line
				(at -35.56 40.64 0)
				(length 5.08)
				(name "IO3_G15")
				(number "G15")
			)
			(pin bidirectional line
				(at -35.56 38.1 0)
				(length 5.08)
				(name "IO3_G16")
				(number "G16")
			)
			(pin bidirectional line
				(at -35.56 35.56 0)
				(length 5.08)
				(name "IO3_G17")
				(number "G17")
			)
			(pin bidirectional line
				(at -35.56 33.02 0)
				(length 5.08)
				(name "IO3_G18")
				(number "G18")
			)
			(pin bidirectional line
				(at -35.56 30.48 0)
				(length 5.08)
				(name "IO3_H13")
				(number "H13")
			)
			(pin bidirectional line
				(at -35.56 27.94 0)
				(length 5.08)
				(name "IO3_H14")
				(number "H14")
			)
			(pin bidirectional line
				(at -35.56 25.4 0)
				(length 5.08)
				(name "IO3_H15")
				(number "H15")
			)
			(pin bidirectional line
				(at -35.56 22.86 0)
				(length 5.08)
				(name "IO3_H16")
				(number "H16")
			)
			(pin bidirectional line
				(at -35.56 20.32 0)
				(length 5.08)
				(name "IO3_H17")
				(number "H17")
			)
			(pin bidirectional line
				(at -35.56 17.78 0)
				(length 5.08)
				(name "IO3_H18")
				(number "H18")
			)
			(pin bidirectional clock
				(at -35.56 15.24 0)
				(length 5.08)
				(name "IO3_J13/GCLK3")
				(number "J13")
			)
			(pin bidirectional line
				(at -35.56 12.7 0)
				(length 5.08)
				(name "IO3_J14")
				(number "J14")
			)
			(pin bidirectional line
				(at -35.56 10.16 0)
				(length 5.08)
				(name "IO3_J15")
				(number "J15")
			)
			(pin bidirectional line
				(at -35.56 7.62 0)
				(length 5.08)
				(name "IO3_J16")
				(number "J16")
			)
			(pin bidirectional line
				(at -35.56 5.08 0)
				(length 5.08)
				(name "IO3_J17")
				(number "J17")
			)
			(pin bidirectional line
				(at -35.56 2.54 0)
				(length 5.08)
				(name "IO3_J18")
				(number "J18")
			)
			(pin bidirectional clock
				(at -35.56 0 0)
				(length 5.08)
				(name "IO3_K13/GCLK2")
				(number "K13")
			)
			(pin bidirectional line
				(at -35.56 -2.54 0)
				(length 5.08)
				(name "IO3_K14")
				(number "K14")
			)
			(pin bidirectional line
				(at -35.56 -5.08 0)
				(length 5.08)
				(name "IO3_K15")
				(number "K15")
			)
			(pin bidirectional line
				(at -35.56 -7.62 0)
				(length 5.08)
				(name "IO3_K16")
				(number "K16")
			)
			(pin bidirectional line
				(at -35.56 -10.16 0)
				(length 5.08)
				(name "IO3_K17")
				(number "K17")
			)
			(pin bidirectional line
				(at -35.56 -12.7 0)
				(length 5.08)
				(name "IO3_K18")
				(number "K18")
			)
			(pin bidirectional line
				(at -35.56 -15.24 0)
				(length 5.08)
				(name "IO3_L13")
				(number "L13")
			)
			(pin bidirectional line
				(at -35.56 -17.78 0)
				(length 5.08)
				(name "IO3_L14")
				(number "L14")
			)
			(pin bidirectional line
				(at -35.56 -20.32 0)
				(length 5.08)
				(name "IO3_L15")
				(number "L15")
			)
			(pin bidirectional line
				(at -35.56 -22.86 0)
				(length 5.08)
				(name "IO3_L16")
				(number "L16")
			)
			(pin bidirectional line
				(at -35.56 -25.4 0)
				(length 5.08)
				(name "IO3_L17")
				(number "L17")
			)
			(pin bidirectional line
				(at -35.56 -27.94 0)
				(length 5.08)
				(name "IO3_L18")
				(number "L18")
			)
			(pin bidirectional line
				(at -35.56 -30.48 0)
				(length 5.08)
				(name "IO3_M12")
				(number "M12")
			)
			(pin bidirectional line
				(at -35.56 -33.02 0)
				(length 5.08)
				(name "IO3_M13")
				(number "M13")
			)
			(pin bidirectional line
				(at -35.56 -35.56 0)
				(length 5.08)
				(name "IO3_M14")
				(number "M14")
			)
			(pin bidirectional line
				(at -35.56 -38.1 0)
				(length 5.08)
				(name "IO3_M15")
				(number "M15")
			)
			(pin bidirectional line
				(at -35.56 -40.64 0)
				(length 5.08)
				(name "IO3_M16")
				(number "M16")
			)
			(pin bidirectional line
				(at -35.56 -43.18 0)
				(length 5.08)
				(name "IO3_M17")
				(number "M17")
			)
			(pin bidirectional line
				(at -35.56 -45.72 0)
				(length 5.08)
				(name "IO3_M18")
				(number "M18")
			)
			(pin bidirectional line
				(at -35.56 -48.26 0)
				(length 5.08)
				(name "IO3_N13")
				(number "N13")
			)
			(pin bidirectional line
				(at -35.56 -50.8 0)
				(length 5.08)
				(name "IO3_N14")
				(number "N14")
			)
			(pin bidirectional line
				(at -35.56 -53.34 0)
				(length 5.08)
				(name "IO3_N15")
				(number "N15")
			)
			(pin bidirectional line
				(at -35.56 -55.88 0)
				(length 5.08)
				(name "IO3_N16")
				(number "N16")
			)
			(pin bidirectional line
				(at -35.56 -58.42 0)
				(length 5.08)
				(name "IO3_N17")
				(number "N17")
			)
			(pin bidirectional line
				(at -35.56 -60.96 0)
				(length 5.08)
				(name "IO3_N18")
				(number "N18")
			)
			(pin bidirectional line
				(at -35.56 -63.5 0)
				(length 5.08)
				(name "IO3_P14")
				(number "P14")
			)
			(pin bidirectional line
				(at -35.56 -66.04 0)
				(length 5.08)
				(name "IO3_P15")
				(number "P15")
			)
			(pin bidirectional line
				(at -35.56 -68.58 0)
				(length 5.08)
				(name "IO3_P16")
				(number "P16")
			)
			(pin bidirectional line
				(at -35.56 -71.12 0)
				(length 5.08)
				(name "IO3_P17")
				(number "P17")
			)
			(pin bidirectional line
				(at -35.56 -73.66 0)
				(length 5.08)
				(name "IO3_P18")
				(number "P18")
			)
			(pin bidirectional line
				(at -35.56 -76.2 0)
				(length 5.08)
				(name "IO3_R15")
				(number "R15")
			)
			(pin bidirectional line
				(at -35.56 -78.74 0)
				(length 5.08)
				(name "IO3_R16")
				(number "R16")
			)
			(pin bidirectional line
				(at -35.56 -81.28 0)
				(length 5.08)
				(name "IO3_R17")
				(number "R17")
			)
			(pin bidirectional line
				(at -35.56 -83.82 0)
				(length 5.08)
				(name "IO3_R18")
				(number "R18")
			)
			(pin bidirectional line
				(at -35.56 -86.36 0)
				(length 5.08)
				(name "IO3_T16")
				(number "T16")
			)
			(pin bidirectional line
				(at -35.56 -88.9 0)
				(length 5.08)
				(name "IO3_T17")
				(number "T17")
			)
			(pin power_in line
				(at -12.7 -99.06 90)
				(length 5.08)
				(name "GNDIO")
				(number "H10")
			)
			(pin power_in line
				(at -10.16 99.06 270)
				(length 5.08)
				(name "VCCIO3")
				(number "C18")
			)
			(pin power_in line
				(at -10.16 -99.06 90)
				(length 5.08)
				(name "GNDIO")
				(number "H11")
			)
			(pin power_in line
				(at -7.62 99.06 270)
				(length 5.08)
				(name "VCCIO3")
				(number "J12")
			)
			(pin power_in line
				(at -7.62 -99.06 90)
				(length 5.08)
				(name "GNDIO")
				(number "L8")
			)
			(pin power_in line
				(at -5.08 99.06 270)
				(length 5.08)
				(name "VCCIO3")
				(number "K12")
			)
			(pin power_in line
				(at -5.08 -99.06 90)
				(length 5.08)
				(name "GNDIO")
				(number "L9")
			)
			(pin power_in line
				(at -2.54 99.06 270)
				(length 5.08)
				(name "VCCIO3")
				(number "T18")
			)
			(pin power_in line
				(at -2.54 -99.06 90)
				(length 5.08)
				(name "GNDIO")
				(number "L10")
			)
			(pin power_in line
				(at 0 99.06 270)
				(length 5.08)
				(name "VCCIO4")
				(number "M9")
			)
			(pin power_in line
				(at 0 -99.06 90)
				(length 5.08)
				(name "GNDIO")
				(number "L11")
			)
			(pin power_in line
				(at 2.54 99.06 270)
				(length 5.08)
				(name "VCCIO4")
				(number "M10")
			)
			(pin power_in line
				(at 2.54 -99.06 90)
				(length 5.08)
				(name "GNDIO")
				(number "U2")
			)
			(pin power_in line
				(at 5.08 99.06 270)
				(length 5.08)
				(name "VCCIO4")
				(number "V3")
			)
			(pin power_in line
				(at 5.08 -99.06 90)
				(length 5.08)
				(name "GNDIO")
				(number "U17")
			)
			(pin power_in line
				(at 7.62 99.06 270)
				(length 5.08)
				(name "VCCIO4")
				(number "V16")
			)
			(pin power_in line
				(at 7.62 -99.06 90)
				(length 5.08)
				(name "GNDIO")
				(number "V1")
			)
			(pin power_in line
				(at 10.16 -99.06 90)
				(length 5.08)
				(name "GNDIO")
				(number "V18")
			)
			(pin bidirectional line
				(at 35.56 91.44 180)
				(length 5.08)
				(name "IO4_N7")
				(number "N7")
			)
			(pin bidirectional line
				(at 35.56 88.9 180)
				(length 5.08)
				(name "IO4_N8")
				(number "N8")
			)
			(pin bidirectional line
				(at 35.56 86.36 180)
				(length 5.08)
				(name "IO4_N9/DEV_OE")
				(number "N9")
			)
			(pin bidirectional line
				(at 35.56 83.82 180)
				(length 5.08)
				(name "IO4_N10/DEV_CLRn")
				(number "N10")
			)
			(pin bidirectional line
				(at 35.56 81.28 180)
				(length 5.08)
				(name "IO4_N11")
				(number "N11")
			)
			(pin bidirectional line
				(at 35.56 78.74 180)
				(length 5.08)
				(name "IO4_N12")
				(number "N12")
			)
			(pin bidirectional line
				(at 35.56 76.2 180)
				(length 5.08)
				(name "IO4_P6")
				(number "P6")
			)
			(pin bidirectional line
				(at 35.56 73.66 180)
				(length 5.08)
				(name "IO4_P7")
				(number "P7")
			)
			(pin bidirectional line
				(at 35.56 71.12 180)
				(length 5.08)
				(name "IO4_P8")
				(number "P8")
			)
			(pin bidirectional line
				(at 35.56 68.58 180)
				(length 5.08)
				(name "IO4_P9")
				(number "P9")
			)
			(pin bidirectional line
				(at 35.56 66.04 180)
				(length 5.08)
				(name "IO4_P10")
				(number "P10")
			)
			(pin bidirectional line
				(at 35.56 63.5 180)
				(length 5.08)
				(name "IO4_P11")
				(number "P11")
			)
			(pin bidirectional line
				(at 35.56 60.96 180)
				(length 5.08)
				(name "IO4_P12")
				(number "P12")
			)
			(pin bidirectional line
				(at 35.56 58.42 180)
				(length 5.08)
				(name "IO4_P13")
				(number "P13")
			)
			(pin bidirectional line
				(at 35.56 55.88 180)
				(length 5.08)
				(name "IO4_R5")
				(number "R5")
			)
			(pin bidirectional line
				(at 35.56 53.34 180)
				(length 5.08)
				(name "IO4_R6")
				(number "R6")
			)
			(pin bidirectional line
				(at 35.56 50.8 180)
				(length 5.08)
				(name "IO4_R7")
				(number "R7")
			)
			(pin bidirectional line
				(at 35.56 48.26 180)
				(length 5.08)
				(name "IO4_R8")
				(number "R8")
			)
			(pin bidirectional line
				(at 35.56 45.72 180)
				(length 5.08)
				(name "IO4_R9")
				(number "R9")
			)
			(pin bidirectional line
				(at 35.56 43.18 180)
				(length 5.08)
				(name "IO4_R10")
				(number "R10")
			)
			(pin bidirectional line
				(at 35.56 40.64 180)
				(length 5.08)
				(name "IO4_R11")
				(number "R11")
			)
			(pin bidirectional line
				(at 35.56 38.1 180)
				(length 5.08)
				(name "IO4_R12")
				(number "R12")
			)
			(pin bidirectional line
				(at 35.56 35.56 180)
				(length 5.08)
				(name "IO4_R13")
				(number "R13")
			)
			(pin bidirectional line
				(at 35.56 33.02 180)
				(length 5.08)
				(name "IO4_R14")
				(number "R14")
			)
			(pin bidirectional line
				(at 35.56 30.48 180)
				(length 5.08)
				(name "IO4_T4")
				(number "T4")
			)
			(pin bidirectional line
				(at 35.56 27.94 180)
				(length 5.08)
				(name "IO4_T5")
				(number "T5")
			)
			(pin bidirectional line
				(at 35.56 25.4 180)
				(length 5.08)
				(name "IO4_T6")
				(number "T6")
			)
			(pin bidirectional line
				(at 35.56 22.86 180)
				(length 5.08)
				(name "IO4_T7")
				(number "T7")
			)
			(pin bidirectional line
				(at 35.56 20.32 180)
				(length 5.08)
				(name "IO4_T8")
				(number "T8")
			)
			(pin bidirectional line
				(at 35.56 17.78 180)
				(length 5.08)
				(name "IO4_T9")
				(number "T9")
			)
			(pin bidirectional line
				(at 35.56 15.24 180)
				(length 5.08)
				(name "IO4_T10")
				(number "T10")
			)
			(pin bidirectional line
				(at 35.56 12.7 180)
				(length 5.08)
				(name "IO4_T11")
				(number "T11")
			)
			(pin bidirectional line
				(at 35.56 10.16 180)
				(length 5.08)
				(name "IO4_T12")
				(number "T12")
			)
			(pin bidirectional line
				(at 35.56 7.62 180)
				(length 5.08)
				(name "IO4_T13")
				(number "T13")
			)
			(pin bidirectional line
				(at 35.56 5.08 180)
				(length 5.08)
				(name "IO4_T14")
				(number "T14")
			)
			(pin bidirectional line
				(at 35.56 2.54 180)
				(length 5.08)
				(name "IO4_T15")
				(number "T15")
			)
			(pin bidirectional line
				(at 35.56 0 180)
				(length 5.08)
				(name "IO4_U1")
				(number "U1")
			)
			(pin bidirectional line
				(at 35.56 -2.54 180)
				(length 5.08)
				(name "IO4_U3")
				(number "U3")
			)
			(pin bidirectional line
				(at 35.56 -5.08 180)
				(length 5.08)
				(name "IO4_U4")
				(number "U4")
			)
			(pin bidirectional line
				(at 35.56 -7.62 180)
				(length 5.08)
				(name "IO4_U5")
				(number "U5")
			)
			(pin bidirectional line
				(at 35.56 -10.16 180)
				(length 5.08)
				(name "IO4_U6")
				(number "U6")
			)
			(pin bidirectional line
				(at 35.56 -12.7 180)
				(length 5.08)
				(name "IO4_U7")
				(number "U7")
			)
			(pin bidirectional line
				(at 35.56 -15.24 180)
				(length 5.08)
				(name "IO4_U8")
				(number "U8")
			)
			(pin bidirectional line
				(at 35.56 -17.78 180)
				(length 5.08)
				(name "IO4_U9")
				(number "U9")
			)
			(pin bidirectional line
				(at 35.56 -20.32 180)
				(length 5.08)
				(name "IO4_U10")
				(number "U10")
			)
			(pin bidirectional line
				(at 35.56 -22.86 180)
				(length 5.08)
				(name "IO4_U11")
				(number "U11")
			)
			(pin bidirectional line
				(at 35.56 -25.4 180)
				(length 5.08)
				(name "IO4_U12")
				(number "U12")
			)
			(pin bidirectional line
				(at 35.56 -27.94 180)
				(length 5.08)
				(name "IO4_U13")
				(number "U13")
			)
			(pin bidirectional line
				(at 35.56 -30.48 180)
				(length 5.08)
				(name "IO4_U14")
				(number "U14")
			)
			(pin bidirectional line
				(at 35.56 -33.02 180)
				(length 5.08)
				(name "IO4_U15")
				(number "U15")
			)
			(pin bidirectional line
				(at 35.56 -35.56 180)
				(length 5.08)
				(name "IO4_U16")
				(number "U16")
			)
			(pin bidirectional line
				(at 35.56 -38.1 180)
				(length 5.08)
				(name "IO4_U18")
				(number "U18")
			)
			(pin bidirectional line
				(at 35.56 -40.64 180)
				(length 5.08)
				(name "IO4_V2")
				(number "V2")
			)
			(pin bidirectional line
				(at 35.56 -43.18 180)
				(length 5.08)
				(name "IO4_V4")
				(number "V4")
			)
			(pin bidirectional line
				(at 35.56 -45.72 180)
				(length 5.08)
				(name "IO4_V5")
				(number "V5")
			)
			(pin bidirectional line
				(at 35.56 -48.26 180)
				(length 5.08)
				(name "IO4_V6")
				(number "V6")
			)
			(pin bidirectional line
				(at 35.56 -50.8 180)
				(length 5.08)
				(name "IO4_V7")
				(number "V7")
			)
			(pin bidirectional line
				(at 35.56 -53.34 180)
				(length 5.08)
				(name "IO4_V8")
				(number "V8")
			)
			(pin bidirectional line
				(at 35.56 -55.88 180)
				(length 5.08)
				(name "IO4_V9")
				(number "V9")
			)
			(pin bidirectional line
				(at 35.56 -58.42 180)
				(length 5.08)
				(name "IO4_V10")
				(number "V10")
			)
			(pin bidirectional line
				(at 35.56 -60.96 180)
				(length 5.08)
				(name "IO4_V11")
				(number "V11")
			)
			(pin bidirectional line
				(at 35.56 -63.5 180)
				(length 5.08)
				(name "IO4_V12")
				(number "V12")
			)
			(pin bidirectional line
				(at 35.56 -66.04 180)
				(length 5.08)
				(name "IO4_V13")
				(number "V13")
			)
			(pin bidirectional line
				(at 35.56 -68.58 180)
				(length 5.08)
				(name "IO4_V14")
				(number "V14")
			)
			(pin bidirectional line
				(at 35.56 -71.12 180)
				(length 5.08)
				(name "IO4_V15")
				(number "V15")
			)
			(pin bidirectional line
				(at 35.56 -73.66 180)
				(length 5.08)
				(name "IO4_V17")
				(number "V17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EPM240F100"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 10.16 57.15 0)
		)
		(property "Value" "EPM240F100"
			(at 10.16 -57.15 0)
		)
		(property "Footprint" "Package_BGA:BGA-100_11.0x11.0mm_Layout10x10_P1.0mm_Ball0.5mm_Pad0.4mm_NSMD"
			(at 10.16 -59.69 0)
		)
		(property "Datasheet" "https://www.altera.com/content/dam/altera-www/global/en_US/pdfs/literature/hb/max2/max2_mii5v1.pdf"
			(at 0 0 0)
		)
		(property "Description" "Altera MAX2 CPLD with 240 LE"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "MAX2 FBGA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*BGA*P1.0mm*"
			(at 0 0 0)
		)
		(symbol "EPM240F100_1_1"
			(pin bidirectional line
				(at -25.4 53.34 0)
				(length 5.08)
				(name "IO1_B1")
				(number "B1")
			)
			(pin bidirectional line
				(at -25.4 50.8 0)
				(length 5.08)
				(name "IO1_C1")
				(number "C1")
			)
			(pin bidirectional line
				(at -25.4 48.26 0)
				(length 5.08)
				(name "IO1_C2")
				(number "C2")
			)
			(pin bidirectional line
				(at -25.4 45.72 0)
				(length 5.08)
				(name "IO1_D1")
				(number "D1")
			)
			(pin bidirectional line
				(at -25.4 43.18 0)
				(length 5.08)
				(name "IO1_D2")
				(number "D2")
			)
			(pin bidirectional line
				(at -25.4 40.64 0)
				(length 5.08)
				(name "IO1_D3")
				(number "D3")
			)
			(pin bidirectional clock
				(at -25.4 38.1 0)
				(length 5.08)
				(name "IO1_E1/GCLK1")
				(number "E1")
			)
			(pin bidirectional clock
				(at -25.4 35.56 0)
				(length 5.08)
				(name "IO1_E2/GCLK0")
				(number "E2")
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 5.08)
				(name "IO1_E3")
				(number "E3")
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 5.08)
				(name "IO1_F1")
				(number "F1")
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 5.08)
				(name "IO1_F2")
				(number "F2")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "IO1_F3")
				(number "F3")
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "IO1_G1")
				(number "G1")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "IO1_G2")
				(number "G2")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "IO1_G3")
				(number "G3")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "IO1_H1")
				(number "H1")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "IO1_H4")
				(number "H4")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "IO1_H5")
				(number "H5")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "IO1_H6")
				(number "H6")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "IO1_H7")
				(number "H7")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "IO1_H8")
				(number "H8")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "IO1_J3")
				(number "J3")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "IO1_J4")
				(number "J4")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "IO1_J5")
				(number "J5")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "IO1_J6")
				(number "J6")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "IO1_J7/DEV_OE")
				(number "J7")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "IO1_J8")
				(number "J8")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "IO1_J9")
				(number "J9")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "IO1_K1")
				(number "K1")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 5.08)
				(name "IO1_K2")
				(number "K2")
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "IO1_K3")
				(number "K3")
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "IO1_K4")
				(number "K4")
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 5.08)
				(name "IO1_K5")
				(number "K5")
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 5.08)
				(name "IO1_K6")
				(number "K6")
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 5.08)
				(name "IO1_K7")
				(number "K7")
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 5.08)
				(name "IO1_K8")
				(number "K8")
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 5.08)
				(name "IO1_K9/DEV_CLRn")
				(number "K9")
			)
			(pin bidirectional line
				(at -25.4 -40.64 0)
				(length 5.08)
				(name "IO1_K10")
				(number "K10")
			)
			(pin input line
				(at -25.4 -43.18 0)
				(length 5.08)
				(name "TMS")
				(number "J1")
			)
			(pin input line
				(at -25.4 -45.72 0)
				(length 5.08)
				(name "TDI")
				(number "H2")
			)
			(pin input clock
				(at -25.4 -48.26 0)
				(length 5.08)
				(name "TCK")
				(number "H3")
			)
			(pin output line
				(at -25.4 -50.8 0)
				(length 5.08)
				(name "TDO")
				(number "J2")
			)
			(pin power_in line
				(at -10.16 60.96 270)
				(length 5.08)
				(name "VCCINT")
				(number "F4")
			)
			(pin power_in line
				(at -10.16 -60.96 90)
				(length 5.08)
				(name "GNDINT")
				(number "F5")
			)
			(pin power_in line
				(at -7.62 60.96 270)
				(length 5.08)
				(name "VCCINT")
				(number "E7")
			)
			(pin power_in line
				(at -7.62 -60.96 90)
				(length 5.08)
				(name "GNDINT")
				(number "E6")
			)
			(pin power_in line
				(at -5.08 60.96 270)
				(length 5.08)
				(name "VCCIO1")
				(number "E4")
			)
			(pin power_in line
				(at -5.08 -60.96 90)
				(length 5.08)
				(name "GNDIO")
				(number "E5")
			)
			(pin power_in line
				(at -2.54 60.96 270)
				(length 5.08)
				(name "VCCIO1")
				(number "G4")
			)
			(pin power_in line
				(at -2.54 -60.96 90)
				(length 5.08)
				(name "GNDIO")
				(number "G5")
			)
			(pin power_in line
				(at 0 60.96 270)
				(length 5.08)
				(name "VCCIO1")
				(number "G6")
			)
			(pin power_in line
				(at 0 -60.96 90)
				(length 5.08)
				(name "GNDIO")
				(number "G7")
			)
			(pin power_in line
				(at 2.54 60.96 270)
				(length 5.08)
				(name "VCCIO2")
				(number "F7")
			)
			(pin power_in line
				(at 2.54 -60.96 90)
				(length 5.08)
				(name "GNDIO")
				(number "F6")
			)
			(pin power_in line
				(at 5.08 60.96 270)
				(length 5.08)
				(name "VCCIO2")
				(number "D6")
			)
			(pin power_in line
				(at 5.08 -60.96 90)
				(length 5.08)
				(name "GNDIO")
				(number "D7")
			)
			(pin power_in line
				(at 7.62 60.96 270)
				(length 5.08)
				(name "VCCIO2")
				(number "D4")
			)
			(pin power_in line
				(at 7.62 -60.96 90)
				(length 5.08)
				(name "GNDIO")
				(number "D5")
			)
			(pin bidirectional line
				(at 25.4 53.34 180)
				(length 5.08)
				(name "IO2_A1")
				(number "A1")
			)
			(pin bidirectional line
				(at 25.4 50.8 180)
				(length 5.08)
				(name "IO2_A2")
				(number "A2")
			)
			(pin bidirectional line
				(at 25.4 48.26 180)
				(length 5.08)
				(name "IO2_A3")
				(number "A3")
			)
			(pin bidirectional line
				(at 25.4 45.72 180)
				(length 5.08)
				(name "IO2_A4")
				(number "A4")
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 5.08)
				(name "IO2_A5")
				(number "A5")
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 5.08)
				(name "IO2_A6")
				(number "A6")
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 5.08)
				(name "IO2_A7")
				(number "A7")
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 5.08)
				(name "IO2_A8")
				(number "A8")
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 5.08)
				(name "IO2_A9")
				(number "A9")
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 5.08)
				(name "IO2_A10")
				(number "A10")
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 5.08)
				(name "IO2_B2")
				(number "B2")
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "IO2_B3")
				(number "B3")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 5.08)
				(name "IO2_B4")
				(number "B4")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "IO2_B5")
				(number "B5")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "IO2_B6")
				(number "B6")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "IO2_B7")
				(number "B7")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "IO2_B8")
				(number "B8")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "IO2_B9")
				(number "B9")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "IO2_B10")
				(number "B10")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "IO2_C3")
				(number "C3")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "IO2_C4")
				(number "C4")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "IO2_C5")
				(number "C5")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "IO2_C6")
				(number "C6")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "IO2_C7")
				(number "C7")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "IO2_C8")
				(number "C8")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "IO2_C9")
				(number "C9")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "IO2_C10")
				(number "C10")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "IO2_D8")
				(number "D8")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "IO2_D9")
				(number "D9")
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 5.08)
				(name "IO2_D10")
				(number "D10")
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "IO2_E8")
				(number "E8")
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "IO2_E9")
				(number "E9")
			)
			(pin bidirectional clock
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "IO2_E10/GCLK3")
				(number "E10")
			)
			(pin bidirectional clock
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "IO2_F8/GCLK2")
				(number "F8")
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 5.08)
				(name "IO2_F9")
				(number "F9")
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 5.08)
				(name "IO2_F10")
				(number "F10")
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 5.08)
				(name "IO2_G8")
				(number "G8")
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 5.08)
				(name "IO2_G9")
				(number "G9")
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 5.08)
				(name "IO2_G10")
				(number "G10")
			)
			(pin bidirectional line
				(at 25.4 -45.72 180)
				(length 5.08)
				(name "IO2_H9")
				(number "H9")
			)
			(pin bidirectional line
				(at 25.4 -48.26 180)
				(length 5.08)
				(name "IO2_H10")
				(number "H10")
			)
			(pin bidirectional line
				(at 25.4 -50.8 180)
				(length 5.08)
				(name "IO2_J10")
				(number "J10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EPM240M100"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 10.16 57.15 0)
		)
		(property "Value" "EPM240M100"
			(at 10.16 -57.15 0)
		)
		(property "Footprint" "Package_BGA:BGA-100_6.0x6.0mm_Layout11x11_P0.5mm_Ball0.3mm_Pad0.25mm_NSMD"
			(at 10.16 -59.69 0)
		)
		(property "Datasheet" "https://www.altera.com/content/dam/altera-www/global/en_US/pdfs/literature/hb/max2/max2_mii5v1.pdf"
			(at 0 0 0)
		)
		(property "Description" "Altera MAX2 CPLD with 240 LE"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "MAX2 MBGA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*BGA*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "EPM240M100_1_1"
			(pin bidirectional line
				(at -25.4 53.34 0)
				(length 5.08)
				(name "IO1_B1")
				(number "B1")
			)
			(pin bidirectional line
				(at -25.4 50.8 0)
				(length 5.08)
				(name "IO1_C1")
				(number "C1")
			)
			(pin bidirectional line
				(at -25.4 48.26 0)
				(length 5.08)
				(name "IO1_C2")
				(number "C2")
			)
			(pin bidirectional line
				(at -25.4 45.72 0)
				(length 5.08)
				(name "IO1_D1")
				(number "D1")
			)
			(pin bidirectional line
				(at -25.4 43.18 0)
				(length 5.08)
				(name "IO1_D2")
				(number "D2")
			)
			(pin bidirectional line
				(at -25.4 40.64 0)
				(length 5.08)
				(name "IO1_D3")
				(number "D3")
			)
			(pin bidirectional clock
				(at -25.4 38.1 0)
				(length 5.08)
				(name "IO1_E1/GCLK1")
				(number "E1")
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 5.08)
				(name "IO1_E2")
				(number "E2")
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 5.08)
				(name "IO1_F1")
				(number "F1")
			)
			(pin bidirectional clock
				(at -25.4 30.48 0)
				(length 5.08)
				(name "IO1_F2/GCLK0")
				(number "F2")
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 5.08)
				(name "IO1_F3")
				(number "F3")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "IO1_G1")
				(number "G1")
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "IO1_G2")
				(number "G2")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "IO1_H1")
				(number "H1")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "IO1_H2")
				(number "H2")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "IO1_H3")
				(number "H3")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "IO1_J5")
				(number "J5")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "IO1_J6")
				(number "J6")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "IO1_J7")
				(number "J7")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "IO1_K3")
				(number "K3")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "IO1_K4")
				(number "K4")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "IO1_K5")
				(number "K5")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "IO1_K6")
				(number "K6")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "IO1_K7")
				(number "K7")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "IO1_K8/DEV_CLRn")
				(number "K8")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "IO1_K9")
				(number "K9")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "IO1_K10")
				(number "K10")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "IO1_L1")
				(number "L1")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "IO1_L2")
				(number "L2")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 5.08)
				(name "IO1_L3")
				(number "L3")
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "IO1_L4")
				(number "L4")
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "IO1_L5")
				(number "L5")
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 5.08)
				(name "IO1_L6")
				(number "L6")
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 5.08)
				(name "IO1_L7")
				(number "L7")
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 5.08)
				(name "IO1_L8/DEV_OE")
				(number "L8")
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 5.08)
				(name "IO1_L9")
				(number "L9")
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 5.08)
				(name "IO1_L10")
				(number "L10")
			)
			(pin bidirectional line
				(at -25.4 -40.64 0)
				(length 5.08)
				(name "IO1_L11")
				(number "L11")
			)
			(pin input line
				(at -25.4 -43.18 0)
				(length 5.08)
				(name "TMS")
				(number "J1")
			)
			(pin input line
				(at -25.4 -45.72 0)
				(length 5.08)
				(name "TDI")
				(number "J2")
			)
			(pin input clock
				(at -25.4 -48.26 0)
				(length 5.08)
				(name "TCK")
				(number "K1")
			)
			(pin output line
				(at -25.4 -50.8 0)
				(length 5.08)
				(name "TDO")
				(number "K2")
			)
			(pin power_in line
				(at -10.16 60.96 270)
				(length 5.08)
				(name "VCCINT")
				(number "G3")
			)
			(pin power_in line
				(at -10.16 -60.96 90)
				(length 5.08)
				(name "GNDINT")
				(number "G4")
			)
			(pin power_in line
				(at -7.62 60.96 270)
				(length 5.08)
				(name "VCCINT")
				(number "E9")
			)
			(pin power_in line
				(at -7.62 -60.96 90)
				(length 5.08)
				(name "GNDINT")
				(number "E8")
			)
			(pin power_in line
				(at -5.08 60.96 270)
				(length 5.08)
				(name "VCCIO1")
				(number "E3")
			)
			(pin power_in line
				(at -5.08 -60.96 90)
				(length 5.08)
				(name "GNDIO")
				(number "E4")
			)
			(pin power_in line
				(at -2.54 60.96 270)
				(length 5.08)
				(name "VCCIO1")
				(number "J4")
			)
			(pin power_in line
				(at -2.54 -60.96 90)
				(length 5.08)
				(name "GNDIO")
				(number "H5")
			)
			(pin power_in line
				(at 0 60.96 270)
				(length 5.08)
				(name "VCCIO1")
				(number "J8")
			)
			(pin power_in line
				(at 0 -60.96 90)
				(length 5.08)
				(name "GNDIO")
				(number "H7")
			)
			(pin power_in line
				(at 2.54 60.96 270)
				(length 5.08)
				(name "VCCIO2")
				(number "G9")
			)
			(pin power_in line
				(at 2.54 -60.96 90)
				(length 5.08)
				(name "GNDIO")
				(number "G8")
			)
			(pin power_in line
				(at 5.08 60.96 270)
				(length 5.08)
				(name "VCCIO2")
				(number "C8")
			)
			(pin power_in line
				(at 5.08 -60.96 90)
				(length 5.08)
				(name "GNDIO")
				(number "D7")
			)
			(pin power_in line
				(at 7.62 60.96 270)
				(length 5.08)
				(name "VCCIO2")
				(number "C4")
			)
			(pin power_in line
				(at 7.62 -60.96 90)
				(length 5.08)
				(name "GNDIO")
				(number "D5")
			)
			(pin bidirectional line
				(at 25.4 53.34 180)
				(length 5.08)
				(name "IO2_A1")
				(number "A1")
			)
			(pin bidirectional line
				(at 25.4 50.8 180)
				(length 5.08)
				(name "IO2_A2")
				(number "A2")
			)
			(pin bidirectional line
				(at 25.4 48.26 180)
				(length 5.08)
				(name "IO2_A3")
				(number "A3")
			)
			(pin bidirectional line
				(at 25.4 45.72 180)
				(length 5.08)
				(name "IO2_A4")
				(number "A4")
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 5.08)
				(name "IO2_A5")
				(number "A5")
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 5.08)
				(name "IO2_A6")
				(number "A6")
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 5.08)
				(name "IO2_A7")
				(number "A7")
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 5.08)
				(name "IO2_A8")
				(number "A8")
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 5.08)
				(name "IO2_A9")
				(number "A9")
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 5.08)
				(name "IO2_A10")
				(number "A10")
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 5.08)
				(name "IO2_A11")
				(number "A11")
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "IO2_B2")
				(number "B2")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 5.08)
				(name "IO2_B3")
				(number "B3")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "IO2_B4")
				(number "B4")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "IO2_B5")
				(number "B5")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "IO2_B6")
				(number "B6")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "IO2_B7")
				(number "B7")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "IO2_B8")
				(number "B8")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "IO2_B9")
				(number "B9")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "IO2_B10")
				(number "B10")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "IO2_B11")
				(number "B11")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "IO2_C5")
				(number "C5")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "IO2_C6")
				(number "C6")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "IO2_C7")
				(number "C7")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "IO2_C10")
				(number "C10")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "IO2_C11")
				(number "C11")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "IO2_D9")
				(number "D9")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "IO2_D10")
				(number "D10")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "IO2_D11")
				(number "D11")
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 5.08)
				(name "IO2_E10")
				(number "E10")
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "IO2_E11")
				(number "E11")
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "IO2_F9")
				(number "F9")
			)
			(pin bidirectional clock
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "IO2_F10/GCLK2")
				(number "F10")
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "IO2_F11")
				(number "F11")
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 5.08)
				(name "IO2_G10")
				(number "G10")
			)
			(pin bidirectional clock
				(at 25.4 -35.56 180)
				(length 5.08)
				(name "IO2_G11/GCLK3")
				(number "G11")
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 5.08)
				(name "IO2_H9")
				(number "H9")
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 5.08)
				(name "IO2_H10")
				(number "H10")
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 5.08)
				(name "IO2_H11")
				(number "H11")
			)
			(pin bidirectional line
				(at 25.4 -45.72 180)
				(length 5.08)
				(name "IO2_J10")
				(number "J10")
			)
			(pin bidirectional line
				(at 25.4 -48.26 180)
				(length 5.08)
				(name "IO2_J11")
				(number "J11")
			)
			(pin bidirectional line
				(at 25.4 -50.8 180)
				(length 5.08)
				(name "IO2_K11")
				(number "K11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EPM240T100"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 10.16 57.15 0)
		)
		(property "Value" "EPM240T100"
			(at 10.16 -57.15 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at 10.16 -59.69 0)
		)
		(property "Datasheet" "https://www.altera.com/content/dam/altera-www/global/en_US/pdfs/literature/hb/max2/max2_mii5v1.pdf"
			(at 0 0 0)
		)
		(property "Description" "Altera MAX2 CPLD with 240 LE"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "MAX2 TQFP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "EPM240T100_1_1"
			(pin bidirectional line
				(at -25.4 53.34 0)
				(length 5.08)
				(name "IO1_2")
				(number "2")
			)
			(pin bidirectional line
				(at -25.4 50.8 0)
				(length 5.08)
				(name "IO1_3")
				(number "3")
			)
			(pin bidirectional line
				(at -25.4 48.26 0)
				(length 5.08)
				(name "IO1_4")
				(number "4")
			)
			(pin bidirectional line
				(at -25.4 45.72 0)
				(length 5.08)
				(name "IO1_5")
				(number "5")
			)
			(pin bidirectional line
				(at -25.4 43.18 0)
				(length 5.08)
				(name "IO1_6")
				(number "6")
			)
			(pin bidirectional line
				(at -25.4 40.64 0)
				(length 5.08)
				(name "IO1_7")
				(number "7")
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 5.08)
				(name "IO1_8")
				(number "8")
			)
			(pin bidirectional clock
				(at -25.4 35.56 0)
				(length 5.08)
				(name "IO1_12/GCLK0")
				(number "12")
			)
			(pin bidirectional clock
				(at -25.4 33.02 0)
				(length 5.08)
				(name "IO1_14/GCLK1")
				(number "14")
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 5.08)
				(name "IO1_15")
				(number "15")
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 5.08)
				(name "IO1_16")
				(number "16")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "IO1_17")
				(number "17")
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "IO1_18")
				(number "18")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "IO1_19")
				(number "19")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "IO1_20")
				(number "20")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "IO1_21")
				(number "21")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "IO1_26")
				(number "26")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "IO1_27")
				(number "27")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "IO1_28")
				(number "28")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "IO1_29")
				(number "29")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "IO1_30")
				(number "30")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "IO1_33")
				(number "33")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "IO1_34")
				(number "34")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "IO1_35")
				(number "35")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "IO1_36")
				(number "36")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "IO1_37")
				(number "37")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "IO1_38")
				(number "38")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "IO1_39")
				(number "39")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "IO1_40")
				(number "40")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 5.08)
				(name "IO1_41")
				(number "41")
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "IO1_42")
				(number "42")
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "IO1_43/DEV_OE")
				(number "43")
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 5.08)
				(name "IO1_44/DEV_CLRn")
				(number "44")
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 5.08)
				(name "IO1_47")
				(number "47")
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 5.08)
				(name "IO1_48")
				(number "48")
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 5.08)
				(name "IO1_49")
				(number "49")
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 5.08)
				(name "IO1_50")
				(number "50")
			)
			(pin bidirectional line
				(at -25.4 -40.64 0)
				(length 5.08)
				(name "IO1_51")
				(number "51")
			)
			(pin input line
				(at -25.4 -43.18 0)
				(length 5.08)
				(name "TMS")
				(number "22")
			)
			(pin input line
				(at -25.4 -45.72 0)
				(length 5.08)
				(name "TDI")
				(number "23")
			)
			(pin input clock
				(at -25.4 -48.26 0)
				(length 5.08)
				(name "TCK")
				(number "24")
			)
			(pin output line
				(at -25.4 -50.8 0)
				(length 5.08)
				(name "TDO")
				(number "25")
			)
			(pin power_in line
				(at -10.16 60.96 270)
				(length 5.08)
				(name "VCCINT")
				(number "13")
			)
			(pin power_in line
				(at -10.16 -60.96 90)
				(length 5.08)
				(name "GNDINT")
				(number "11")
			)
			(pin power_in line
				(at -7.62 60.96 270)
				(length 5.08)
				(name "VCCINT")
				(number "63")
			)
			(pin power_in line
				(at -7.62 -60.96 90)
				(length 5.08)
				(name "GNDINT")
				(number "65")
			)
			(pin power_in line
				(at -5.08 60.96 270)
				(length 5.08)
				(name "VCCIO1")
				(number "9")
			)
			(pin power_in line
				(at -5.08 -60.96 90)
				(length 5.08)
				(name "GNDIO")
				(number "10")
			)
			(pin power_in line
				(at -2.54 60.96 270)
				(length 5.08)
				(name "VCCIO1")
				(number "31")
			)
			(pin power_in line
				(at -2.54 -60.96 90)
				(length 5.08)
				(name "GNDIO")
				(number "32")
			)
			(pin power_in line
				(at 0 60.96 270)
				(length 5.08)
				(name "VCCIO1")
				(number "45")
			)
			(pin power_in line
				(at 0 -60.96 90)
				(length 5.08)
				(name "GNDIO")
				(number "46")
			)
			(pin power_in line
				(at 2.54 60.96 270)
				(length 5.08)
				(name "VCCIO2")
				(number "59")
			)
			(pin power_in line
				(at 2.54 -60.96 90)
				(length 5.08)
				(name "GNDIO")
				(number "60")
			)
			(pin power_in line
				(at 5.08 60.96 270)
				(length 5.08)
				(name "VCCIO2")
				(number "80")
			)
			(pin power_in line
				(at 5.08 -60.96 90)
				(length 5.08)
				(name "GNDIO")
				(number "79")
			)
			(pin power_in line
				(at 7.62 60.96 270)
				(length 5.08)
				(name "VCCIO2")
				(number "94")
			)
			(pin power_in line
				(at 7.62 -60.96 90)
				(length 5.08)
				(name "GNDIO")
				(number "93")
			)
			(pin bidirectional line
				(at 25.4 53.34 180)
				(length 5.08)
				(name "IO2_1")
				(number "1")
			)
			(pin bidirectional line
				(at 25.4 50.8 180)
				(length 5.08)
				(name "IO2_52")
				(number "52")
			)
			(pin bidirectional line
				(at 25.4 48.26 180)
				(length 5.08)
				(name "IO2_53")
				(number "53")
			)
			(pin bidirectional line
				(at 25.4 45.72 180)
				(length 5.08)
				(name "IO2_54")
				(number "54")
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 5.08)
				(name "IO2_55")
				(number "55")
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 5.08)
				(name "IO2_56")
				(number "56")
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 5.08)
				(name "IO2_57")
				(number "57")
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 5.08)
				(name "IO2_58")
				(number "58")
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 5.08)
				(name "IO2_61")
				(number "61")
			)
			(pin bidirectional clock
				(at 25.4 30.48 180)
				(length 5.08)
				(name "IO2_62/GCLK2")
				(number "62")
			)
			(pin bidirectional clock
				(at 25.4 27.94 180)
				(length 5.08)
				(name "IO2_64/GCLK3")
				(number "64")
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "IO2_66")
				(number "66")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 5.08)
				(name "IO2_67")
				(number "67")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "IO2_68")
				(number "68")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "IO2_69")
				(number "69")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "IO2_70")
				(number "70")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "IO2_71")
				(number "71")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "IO2_72")
				(number "72")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "IO2_73")
				(number "73")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "IO2_74")
				(number "74")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "IO2_75")
				(number "75")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "IO2_76")
				(number "76")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "IO2_77")
				(number "77")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "IO2_78")
				(number "78")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "IO2_81")
				(number "81")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "IO2_82")
				(number "82")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "IO2_83")
				(number "83")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "IO2_84")
				(number "84")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "IO2_85")
				(number "85")
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 5.08)
				(name "IO2_86")
				(number "86")
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "IO2_87")
				(number "87")
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "IO2_88")
				(number "88")
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "IO2_89")
				(number "89")
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "IO2_90")
				(number "90")
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 5.08)
				(name "IO2_91")
				(number "91")
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 5.08)
				(name "IO2_92")
				(number "92")
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 5.08)
				(name "IO2_95")
				(number "95")
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 5.08)
				(name "IO2_96")
				(number "96")
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 5.08)
				(name "IO2_97")
				(number "97")
			)
			(pin bidirectional line
				(at 25.4 -45.72 180)
				(length 5.08)
				(name "IO2_98")
				(number "98")
			)
			(pin bidirectional line
				(at 25.4 -48.26 180)
				(length 5.08)
				(name "IO2_99")
				(number "99")
			)
			(pin bidirectional line
				(at 25.4 -50.8 180)
				(length 5.08)
				(name "IO2_100")
				(number "100")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EPM240ZM100"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 10.16 57.15 0)
		)
		(property "Value" "EPM240ZM100"
			(at 10.16 -57.15 0)
		)
		(property "Footprint" "Package_BGA:BGA-100_6.0x6.0mm_Layout11x11_P0.5mm_Ball0.3mm_Pad0.25mm_NSMD"
			(at 10.16 -59.69 0)
		)
		(property "Datasheet" "https://www.altera.com/content/dam/altera-www/global/en_US/pdfs/literature/hb/max2/max2_mii5v1.pdf"
			(at 0 0 0)
		)
		(property "Description" "Altera Zero-Power MAX2 CPLD with 240 LE"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "MAX2 MBGA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*BGA*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "EPM240ZM100_1_1"
			(pin bidirectional line
				(at -25.4 53.34 0)
				(length 5.08)
				(name "IO1_B1")
				(number "B1")
			)
			(pin bidirectional line
				(at -25.4 50.8 0)
				(length 5.08)
				(name "IO1_C1")
				(number "C1")
			)
			(pin bidirectional line
				(at -25.4 48.26 0)
				(length 5.08)
				(name "IO1_C2")
				(number "C2")
			)
			(pin bidirectional line
				(at -25.4 45.72 0)
				(length 5.08)
				(name "IO1_D1")
				(number "D1")
			)
			(pin bidirectional line
				(at -25.4 43.18 0)
				(length 5.08)
				(name "IO1_D2")
				(number "D2")
			)
			(pin bidirectional line
				(at -25.4 40.64 0)
				(length 5.08)
				(name "IO1_D3")
				(number "D3")
			)
			(pin bidirectional clock
				(at -25.4 38.1 0)
				(length 5.08)
				(name "IO1_E1/GCLK1")
				(number "E1")
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 5.08)
				(name "IO1_E2")
				(number "E2")
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 5.08)
				(name "IO1_F1")
				(number "F1")
			)
			(pin bidirectional clock
				(at -25.4 30.48 0)
				(length 5.08)
				(name "IO1_F2/GCLK0")
				(number "F2")
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 5.08)
				(name "IO1_F3")
				(number "F3")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "IO1_G1")
				(number "G1")
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "IO1_G2")
				(number "G2")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "IO1_H1")
				(number "H1")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "IO1_H2")
				(number "H2")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "IO1_H3")
				(number "H3")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "IO1_J5")
				(number "J5")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "IO1_J6")
				(number "J6")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "IO1_J7")
				(number "J7")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "IO1_K3")
				(number "K3")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "IO1_K4")
				(number "K4")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "IO1_K5")
				(number "K5")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "IO1_K6")
				(number "K6")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "IO1_K7")
				(number "K7")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "IO1_K8/DEV_CLRn")
				(number "K8")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "IO1_K9")
				(number "K9")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "IO1_K10")
				(number "K10")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "IO1_L1")
				(number "L1")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "IO1_L2")
				(number "L2")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 5.08)
				(name "IO1_L3")
				(number "L3")
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "IO1_L4")
				(number "L4")
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "IO1_L5")
				(number "L5")
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 5.08)
				(name "IO1_L6")
				(number "L6")
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 5.08)
				(name "IO1_L7")
				(number "L7")
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 5.08)
				(name "IO1_L8/DEV_OE")
				(number "L8")
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 5.08)
				(name "IO1_L9")
				(number "L9")
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 5.08)
				(name "IO1_L10")
				(number "L10")
			)
			(pin bidirectional line
				(at -25.4 -40.64 0)
				(length 5.08)
				(name "IO1_L11")
				(number "L11")
			)
			(pin input line
				(at -25.4 -43.18 0)
				(length 5.08)
				(name "TMS")
				(number "J1")
			)
			(pin input line
				(at -25.4 -45.72 0)
				(length 5.08)
				(name "TDI")
				(number "J2")
			)
			(pin input clock
				(at -25.4 -48.26 0)
				(length 5.08)
				(name "TCK")
				(number "K1")
			)
			(pin output line
				(at -25.4 -50.8 0)
				(length 5.08)
				(name "TDO")
				(number "K2")
			)
			(pin power_in line
				(at -10.16 60.96 270)
				(length 5.08)
				(name "VCCINT")
				(number "G3")
			)
			(pin power_in line
				(at -10.16 -60.96 90)
				(length 5.08)
				(name "GND")
				(number "E4")
			)
			(pin power_in line
				(at -7.62 60.96 270)
				(length 5.08)
				(name "VCCINT")
				(number "E9")
			)
			(pin power_in line
				(at -7.62 -60.96 90)
				(length 5.08)
				(name "GND")
				(number "G4")
			)
			(pin power_in line
				(at -5.08 60.96 270)
				(length 5.08)
				(name "VCCIO1")
				(number "E3")
			)
			(pin power_in line
				(at -5.08 -60.96 90)
				(length 5.08)
				(name "GND")
				(number "H5")
			)
			(pin power_in line
				(at -2.54 60.96 270)
				(length 5.08)
				(name "VCCIO1")
				(number "J4")
			)
			(pin power_in line
				(at -2.54 -60.96 90)
				(length 5.08)
				(name "GND")
				(number "H7")
			)
			(pin power_in line
				(at 0 60.96 270)
				(length 5.08)
				(name "VCCIO1")
				(number "J8")
			)
			(pin power_in line
				(at 0 -60.96 90)
				(length 5.08)
				(name "GND")
				(number "G8")
			)
			(pin power_in line
				(at 2.54 60.96 270)
				(length 5.08)
				(name "VCCIO2")
				(number "G9")
			)
			(pin power_in line
				(at 2.54 -60.96 90)
				(length 5.08)
				(name "GND")
				(number "E8")
			)
			(pin power_in line
				(at 5.08 60.96 270)
				(length 5.08)
				(name "VCCIO2")
				(number "C8")
			)
			(pin power_in line
				(at 5.08 -60.96 90)
				(length 5.08)
				(name "GND")
				(number "D7")
			)
			(pin power_in line
				(at 7.62 60.96 270)
				(length 5.08)
				(name "VCCIO2")
				(number "C4")
			)
			(pin power_in line
				(at 7.62 -60.96 90)
				(length 5.08)
				(name "GND")
				(number "D5")
			)
			(pin bidirectional line
				(at 25.4 53.34 180)
				(length 5.08)
				(name "IO2_A1")
				(number "A1")
			)
			(pin bidirectional line
				(at 25.4 50.8 180)
				(length 5.08)
				(name "IO2_A2")
				(number "A2")
			)
			(pin bidirectional line
				(at 25.4 48.26 180)
				(length 5.08)
				(name "IO2_A3")
				(number "A3")
			)
			(pin bidirectional line
				(at 25.4 45.72 180)
				(length 5.08)
				(name "IO2_A4")
				(number "A4")
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 5.08)
				(name "IO2_A5")
				(number "A5")
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 5.08)
				(name "IO2_A6")
				(number "A6")
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 5.08)
				(name "IO2_A7")
				(number "A7")
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 5.08)
				(name "IO2_A8")
				(number "A8")
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 5.08)
				(name "IO2_A9")
				(number "A9")
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 5.08)
				(name "IO2_A10")
				(number "A10")
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 5.08)
				(name "IO2_A11")
				(number "A11")
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "IO2_B2")
				(number "B2")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 5.08)
				(name "IO2_B3")
				(number "B3")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "IO2_B4")
				(number "B4")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "IO2_B5")
				(number "B5")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "IO2_B6")
				(number "B6")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "IO2_B7")
				(number "B7")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "IO2_B8")
				(number "B8")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "IO2_B9")
				(number "B9")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "IO2_B10")
				(number "B10")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "IO2_B11")
				(number "B11")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "IO2_C5")
				(number "C5")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "IO2_C6")
				(number "C6")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "IO2_C7")
				(number "C7")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "IO2_C10")
				(number "C10")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "IO2_C11")
				(number "C11")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "IO2_D9")
				(number "D9")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "IO2_D10")
				(number "D10")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "IO2_D11")
				(number "D11")
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 5.08)
				(name "IO2_E10")
				(number "E10")
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "IO2_E11")
				(number "E11")
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "IO2_F9")
				(number "F9")
			)
			(pin bidirectional clock
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "IO2_F10/GCLK2")
				(number "F10")
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "IO2_F11")
				(number "F11")
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 5.08)
				(name "IO2_G10")
				(number "G10")
			)
			(pin bidirectional clock
				(at 25.4 -35.56 180)
				(length 5.08)
				(name "IO2_G11/GCLK3")
				(number "G11")
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 5.08)
				(name "IO2_H9")
				(number "H9")
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 5.08)
				(name "IO2_H10")
				(number "H10")
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 5.08)
				(name "IO2_H11")
				(number "H11")
			)
			(pin bidirectional line
				(at 25.4 -45.72 180)
				(length 5.08)
				(name "IO2_J10")
				(number "J10")
			)
			(pin bidirectional line
				(at 25.4 -48.26 180)
				(length 5.08)
				(name "IO2_J11")
				(number "J11")
			)
			(pin bidirectional line
				(at 25.4 -50.8 180)
				(length 5.08)
				(name "IO2_K11")
				(number "K11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EPM240ZM68"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 43.18 0)
		)
		(property "Value" "EPM240ZM68"
			(at 7.62 -43.18 0)
		)
		(property "Footprint" "Package_BGA:BGA-68_5.0x5.0mm_Layout9x9_P0.5mm_Ball0.3mm_Pad0.25mm_NSMD"
			(at 7.62 -45.72 0)
		)
		(property "Datasheet" "https://www.altera.com/content/dam/altera-www/global/en_US/pdfs/literature/hb/max2/max2_mii5v1.pdf"
			(at 0 0 0)
		)
		(property "Description" "Altera Zero-Power MAX2 CPLD with 240 LE"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "MAX2 MBGA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*BGA*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "EPM240ZM68_1_1"
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 3.81)
				(name "IO1_A1")
				(number "A1")
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 3.81)
				(name "IO1_B1")
				(number "B1")
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 3.81)
				(name "IO1_C1")
				(number "C1")
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 3.81)
				(name "IO1_C2")
				(number "C2")
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 3.81)
				(name "IO1_D1")
				(number "D1")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 3.81)
				(name "IO1_D2")
				(number "D2")
			)
			(pin bidirectional clock
				(at -25.4 22.86 0)
				(length 3.81)
				(name "IO1_E1/GCLK1")
				(number "E1")
			)
			(pin bidirectional clock
				(at -25.4 20.32 0)
				(length 3.81)
				(name "IO1_E2/GCLK0")
				(number "E2")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 3.81)
				(name "IO1_F1")
				(number "F1")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 3.81)
				(name "IO1_F2")
				(number "F2")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 3.81)
				(name "IO1_F3")
				(number "F3")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "IO1_G2")
				(number "G2")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 3.81)
				(name "IO1_G6")
				(number "G6")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 3.81)
				(name "IO1_H3")
				(number "H3")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 3.81)
				(name "IO1_H4")
				(number "H4")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 3.81)
				(name "IO1_H5")
				(number "H5")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 3.81)
				(name "IO1_H6")
				(number "H6")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "IO1_H7/DEV_CLRn")
				(number "H7")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 3.81)
				(name "IO1_H8")
				(number "H8")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 3.81)
				(name "IO1_J2")
				(number "J2")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 3.81)
				(name "IO1_J3")
				(number "J3")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 3.81)
				(name "IO1_J4")
				(number "J4")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 3.81)
				(name "IO1_J5")
				(number "J5")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 3.81)
				(name "IO1_J6/DEV_OE")
				(number "J6")
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 3.81)
				(name "IO1_J7")
				(number "J7")
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 3.81)
				(name "IO1_J8")
				(number "J8")
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 3.81)
				(name "IO1_J9")
				(number "J9")
			)
			(pin input line
				(at -25.4 -30.48 0)
				(length 3.81)
				(name "TMS")
				(number "G1")
			)
			(pin input line
				(at -25.4 -33.02 0)
				(length 3.81)
				(name "TDI")
				(number "H1")
			)
			(pin input clock
				(at -25.4 -35.56 0)
				(length 3.81)
				(name "TCK")
				(number "J1")
			)
			(pin output line
				(at -25.4 -38.1 0)
				(length 3.81)
				(name "TDO")
				(number "H2")
			)
			(pin power_in line
				(at -5.08 45.72 270)
				(length 3.81)
				(name "VCCINT")
				(number "D7")
			)
			(pin power_in line
				(at -5.08 -45.72 90)
				(length 3.81)
				(name "GND")
				(number "C5")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 3.81)
				(name "VCCIO1")
				(number "D3")
			)
			(pin power_in line
				(at -2.54 -45.72 90)
				(length 3.81)
				(name "GND")
				(number "E3")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 3.81)
				(name "VCCIO1")
				(number "G4")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 3.81)
				(name "GND")
				(number "E7")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 3.81)
				(name "VCCIO2")
				(number "C4")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 3.81)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at 5.08 45.72 270)
				(length 3.81)
				(name "VCCIO2")
				(number "F7")
			)
			(pin power_in line
				(at 5.08 -45.72 90)
				(length 3.81)
				(name "GND")
				(number "C6")
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 3.81)
				(name "IO2_A2")
				(number "A2")
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 3.81)
				(name "IO2_A3")
				(number "A3")
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 3.81)
				(name "IO2_A4")
				(number "A4")
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 3.81)
				(name "IO2_A5")
				(number "A5")
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 3.81)
				(name "IO2_A6")
				(number "A6")
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 3.81)
				(name "IO2_A7")
				(number "A7")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 3.81)
				(name "IO2_A8")
				(number "A8")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 3.81)
				(name "IO2_A9")
				(number "A9")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 3.81)
				(name "IO2_B2")
				(number "B2")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 3.81)
				(name "IO2_B3")
				(number "B3")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 3.81)
				(name "IO2_B4")
				(number "B4")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 3.81)
				(name "IO2_B5")
				(number "B5")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 3.81)
				(name "IO2_B6")
				(number "B6")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 3.81)
				(name "IO2_B7")
				(number "B7")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 3.81)
				(name "IO2_B8")
				(number "B8")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 3.81)
				(name "IO2_B9")
				(number "B9")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 3.81)
				(name "IO2_C8")
				(number "C8")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 3.81)
				(name "IO2_C9")
				(number "C9")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 3.81)
				(name "IO2_D8")
				(number "D8")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 3.81)
				(name "IO2_D9")
				(number "D9")
			)
			(pin bidirectional clock
				(at 25.4 -12.7 180)
				(length 3.81)
				(name "IO2_E8/GCLK3")
				(number "E8")
			)
			(pin bidirectional clock
				(at 25.4 -15.24 180)
				(length 3.81)
				(name "IO2_E9/GCLK2")
				(number "E9")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 3.81)
				(name "IO2_F8")
				(number "F8")
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 3.81)
				(name "IO2_F9")
				(number "F9")
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 3.81)
				(name "IO2_G8")
				(number "G8")
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 3.81)
				(name "IO2_G9")
				(number "G9")
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 3.81)
				(name "IO2_H9")
				(number "H9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EPM570F100"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 12.7 54.61 0)
		)
		(property "Value" "EPM570F100"
			(at 12.7 -54.61 0)
		)
		(property "Footprint" "Package_BGA:BGA-100_11.0x11.0mm_Layout10x10_P1.0mm_Ball0.5mm_Pad0.4mm_NSMD"
			(at 12.7 -57.15 0)
		)
		(property "Datasheet" "https://www.altera.com/content/dam/altera-www/global/en_US/pdfs/literature/hb/max2/max2_mii5v1.pdf"
			(at 0 0 0)
		)
		(property "Description" "Altera MAX2 CPLD with 570 LE"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "MAX2 FBGA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*BGA*P1.0mm*"
			(at 0 0 0)
		)
		(symbol "EPM570F100_1_1"
			(pin bidirectional line
				(at -27.94 50.8 0)
				(length 5.08)
				(name "IO1_B1")
				(number "B1")
			)
			(pin bidirectional line
				(at -27.94 48.26 0)
				(length 5.08)
				(name "IO1_C1")
				(number "C1")
			)
			(pin bidirectional line
				(at -27.94 45.72 0)
				(length 5.08)
				(name "IO1_C2")
				(number "C2")
			)
			(pin bidirectional line
				(at -27.94 43.18 0)
				(length 5.08)
				(name "IO1_D1")
				(number "D1")
			)
			(pin bidirectional line
				(at -27.94 40.64 0)
				(length 5.08)
				(name "IO1_D2")
				(number "D2")
			)
			(pin bidirectional line
				(at -27.94 38.1 0)
				(length 5.08)
				(name "IO1_D3")
				(number "D3")
			)
			(pin bidirectional clock
				(at -27.94 35.56 0)
				(length 5.08)
				(name "IO1_E1/GCLK1")
				(number "E1")
			)
			(pin bidirectional clock
				(at -27.94 33.02 0)
				(length 5.08)
				(name "IO1_E2/GCLK0")
				(number "E2")
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 5.08)
				(name "IO1_E3")
				(number "E3")
			)
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 5.08)
				(name "IO1_F1")
				(number "F1")
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 5.08)
				(name "IO1_F2")
				(number "F2")
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 5.08)
				(name "IO1_F3")
				(number "F3")
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 5.08)
				(name "IO1_G1")
				(number "G1")
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 5.08)
				(name "IO1_G2")
				(number "G2")
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 5.08)
				(name "IO1_G3")
				(number "G3")
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 5.08)
				(name "IO1_H1")
				(number "H1")
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 5.08)
				(name "IO1_H4")
				(number "H4")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 5.08)
				(name "IO1_H7")
				(number "H7")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 5.08)
				(name "IO1_H8")
				(number "H8")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 5.08)
				(name "IO1_J3")
				(number "J3")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 5.08)
				(name "IO1_J4")
				(number "J4")
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 5.08)
				(name "IO1_J5")
				(number "J5")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 5.08)
				(name "IO1_J6")
				(number "J6")
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 5.08)
				(name "IO1_J7/DEV_OE")
				(number "J7")
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 5.08)
				(name "IO1_J8")
				(number "J8")
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 5.08)
				(name "IO1_J9")
				(number "J9")
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 5.08)
				(name "IO1_K1")
				(number "K1")
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 5.08)
				(name "IO1_K2")
				(number "K2")
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 5.08)
				(name "IO1_K3")
				(number "K3")
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 5.08)
				(name "IO1_K4")
				(number "K4")
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 5.08)
				(name "IO1_K5")
				(number "K5")
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 5.08)
				(name "IO1_K6")
				(number "K6")
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 5.08)
				(name "IO1_K7")
				(number "K7")
			)
			(pin bidirectional line
				(at -27.94 -33.02 0)
				(length 5.08)
				(name "IO1_K8")
				(number "K8")
			)
			(pin bidirectional line
				(at -27.94 -35.56 0)
				(length 5.08)
				(name "IO1_K9/DEV_CLRn")
				(number "K9")
			)
			(pin bidirectional line
				(at -27.94 -38.1 0)
				(length 5.08)
				(name "IO1_K10")
				(number "K10")
			)
			(pin input line
				(at -27.94 -40.64 0)
				(length 5.08)
				(name "TMS")
				(number "J1")
			)
			(pin input line
				(at -27.94 -43.18 0)
				(length 5.08)
				(name "TDI")
				(number "H2")
			)
			(pin input clock
				(at -27.94 -45.72 0)
				(length 5.08)
				(name "TCK")
				(number "H3")
			)
			(pin output line
				(at -27.94 -48.26 0)
				(length 5.08)
				(name "TDO")
				(number "J2")
			)
			(pin power_in line
				(at -12.7 58.42 270)
				(length 5.08)
				(name "VCCINT")
				(number "F4")
			)
			(pin power_in line
				(at -12.7 -58.42 90)
				(length 5.08)
				(name "GNDINT")
				(number "F5")
			)
			(pin power_in line
				(at -10.16 58.42 270)
				(length 5.08)
				(name "VCCINT")
				(number "H6")
			)
			(pin power_in line
				(at -10.16 -58.42 90)
				(length 5.08)
				(name "GNDINT")
				(number "H5")
			)
			(pin power_in line
				(at -7.62 58.42 270)
				(length 5.08)
				(name "VCCINT")
				(number "E7")
			)
			(pin power_in line
				(at -7.62 -58.42 90)
				(length 5.08)
				(name "GNDINT")
				(number "E6")
			)
			(pin power_in line
				(at -5.08 58.42 270)
				(length 5.08)
				(name "VCCINT")
				(number "C6")
			)
			(pin power_in line
				(at -5.08 -58.42 90)
				(length 5.08)
				(name "GNDINT")
				(number "C5")
			)
			(pin power_in line
				(at -2.54 58.42 270)
				(length 5.08)
				(name "VCCIO1")
				(number "E4")
			)
			(pin power_in line
				(at -2.54 -58.42 90)
				(length 5.08)
				(name "GNDIO")
				(number "E5")
			)
			(pin power_in line
				(at 0 58.42 270)
				(length 5.08)
				(name "VCCIO1")
				(number "G4")
			)
			(pin power_in line
				(at 0 -58.42 90)
				(length 5.08)
				(name "GNDIO")
				(number "G5")
			)
			(pin power_in line
				(at 2.54 58.42 270)
				(length 5.08)
				(name "VCCIO1")
				(number "G6")
			)
			(pin power_in line
				(at 2.54 -58.42 90)
				(length 5.08)
				(name "GNDIO")
				(number "G7")
			)
			(pin power_in line
				(at 5.08 58.42 270)
				(length 5.08)
				(name "VCCIO2")
				(number "F7")
			)
			(pin power_in line
				(at 5.08 -58.42 90)
				(length 5.08)
				(name "GNDIO")
				(number "F6")
			)
			(pin power_in line
				(at 7.62 58.42 270)
				(length 5.08)
				(name "VCCIO2")
				(number "D6")
			)
			(pin power_in line
				(at 7.62 -58.42 90)
				(length 5.08)
				(name "GNDIO")
				(number "D7")
			)
			(pin power_in line
				(at 10.16 58.42 270)
				(length 5.08)
				(name "VCCIO2")
				(number "D4")
			)
			(pin power_in line
				(at 10.16 -58.42 90)
				(length 5.08)
				(name "GNDIO")
				(number "D5")
			)
			(pin bidirectional line
				(at 27.94 50.8 180)
				(length 5.08)
				(name "IO2_A1")
				(number "A1")
			)
			(pin bidirectional line
				(at 27.94 48.26 180)
				(length 5.08)
				(name "IO2_A2")
				(number "A2")
			)
			(pin bidirectional line
				(at 27.94 45.72 180)
				(length 5.08)
				(name "IO2_A3")
				(number "A3")
			)
			(pin bidirectional line
				(at 27.94 43.18 180)
				(length 5.08)
				(name "IO2_A4")
				(number "A4")
			)
			(pin bidirectional line
				(at 27.94 40.64 180)
				(length 5.08)
				(name "IO2_A5")
				(number "A5")
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 5.08)
				(name "IO2_A6")
				(number "A6")
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 5.08)
				(name "IO2_A7")
				(number "A7")
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 5.08)
				(name "IO2_A8")
				(number "A8")
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 5.08)
				(name "IO2_A9")
				(number "A9")
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 5.08)
				(name "IO2_A10")
				(number "A10")
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 5.08)
				(name "IO2_B2")
				(number "B2")
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 5.08)
				(name "IO2_B3")
				(number "B3")
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 5.08)
				(name "IO2_B4")
				(number "B4")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 5.08)
				(name "IO2_B5")
				(number "B5")
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 5.08)
				(name "IO2_B6")
				(number "B6")
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 5.08)
				(name "IO2_B7")
				(number "B7")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 5.08)
				(name "IO2_B8")
				(number "B8")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 5.08)
				(name "IO2_B9")
				(number "B9")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 5.08)
				(name "IO2_B10")
				(number "B10")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 5.08)
				(name "IO2_C3")
				(number "C3")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 5.08)
				(name "IO2_C4")
				(number "C4")
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 5.08)
				(name "IO2_C7")
				(number "C7")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 5.08)
				(name "IO2_C8")
				(number "C8")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 5.08)
				(name "IO2_C9")
				(number "C9")
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 5.08)
				(name "IO2_C10")
				(number "C10")
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 5.08)
				(name "IO2_D8")
				(number "D8")
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 5.08)
				(name "IO2_D9")
				(number "D9")
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 5.08)
				(name "IO2_D10")
				(number "D10")
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 5.08)
				(name "IO2_E8")
				(number "E8")
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 5.08)
				(name "IO2_E9")
				(number "E9")
			)
			(pin bidirectional clock
				(at 27.94 -25.4 180)
				(length 5.08)
				(name "IO2_E10/GCLK3")
				(number "E10")
			)
			(pin bidirectional clock
				(at 27.94 -27.94 180)
				(length 5.08)
				(name "IO2_F8/GCLK2")
				(number "F8")
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 5.08)
				(name "IO2_F9")
				(number "F9")
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 5.08)
				(name "IO2_F10")
				(number "F10")
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 5.08)
				(name "IO2_G8")
				(number "G8")
			)
			(pin bidirectional line
				(at 27.94 -38.1 180)
				(length 5.08)
				(name "IO2_G9")
				(number "G9")
			)
			(pin bidirectional line
				(at 27.94 -40.64 180)
				(length 5.08)
				(name "IO2_G10")
				(number "G10")
			)
			(pin bidirectional line
				(at 27.94 -43.18 180)
				(length 5.08)
				(name "IO2_H9")
				(number "H9")
			)
			(pin bidirectional line
				(at 27.94 -45.72 180)
				(length 5.08)
				(name "IO2_H10")
				(number "H10")
			)
			(pin bidirectional line
				(at 27.94 -48.26 180)
				(length 5.08)
				(name "IO2_J10")
				(number "J10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EPM570F256"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 25.4 107.95 0)
		)
		(property "Value" "EPM570F256"
			(at 25.4 -107.95 0)
		)
		(property "Footprint" "Package_BGA:BGA-256_17.0x17.0mm_Layout16x16_P1.0mm_Ball0.5mm_Pad0.4mm_NSMD"
			(at 25.4 -110.49 0)
		)
		(property "Datasheet" "https://www.altera.com/content/dam/altera-www/global/en_US/pdfs/literature/hb/max2/max2_mii5v1.pdf"
			(at 0 0 0)
		)
		(property "Description" "Altera MAX2 CPLD with 570 LE"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "MAX2 FBGA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*BGA*P1.0mm*"
			(at 0 0 0)
		)
		(symbol "EPM570F256_1_1"
			(pin bidirectional line
				(at -40.64 104.14 0)
				(length 5.08)
				(name "IO1_C2")
				(number "C2")
			)
			(pin bidirectional line
				(at -40.64 101.6 0)
				(length 5.08)
				(name "IO1_C3")
				(number "C3")
			)
			(pin bidirectional line
				(at -40.64 99.06 0)
				(length 5.08)
				(name "IO1_D1")
				(number "D1")
			)
			(pin bidirectional line
				(at -40.64 96.52 0)
				(length 5.08)
				(name "IO1_D2")
				(number "D2")
			)
			(pin bidirectional line
				(at -40.64 93.98 0)
				(length 5.08)
				(name "IO1_D3")
				(number "D3")
			)
			(pin bidirectional line
				(at -40.64 91.44 0)
				(length 5.08)
				(name "IO1_E1")
				(number "E1")
			)
			(pin bidirectional line
				(at -40.64 88.9 0)
				(length 5.08)
				(name "IO1_E2")
				(number "E2")
			)
			(pin bidirectional line
				(at -40.64 86.36 0)
				(length 5.08)
				(name "IO1_E3")
				(number "E3")
			)
			(pin bidirectional line
				(at -40.64 83.82 0)
				(length 5.08)
				(name "IO1_E4")
				(number "E4")
			)
			(pin bidirectional line
				(at -40.64 81.28 0)
				(length 5.08)
				(name "IO1_F1")
				(number "F1")
			)
			(pin bidirectional line
				(at -40.64 78.74 0)
				(length 5.08)
				(name "IO1_F2")
				(number "F2")
			)
			(pin bidirectional line
				(at -40.64 76.2 0)
				(length 5.08)
				(name "IO1_F3")
				(number "F3")
			)
			(pin bidirectional line
				(at -40.64 73.66 0)
				(length 5.08)
				(name "IO1_G1")
				(number "G1")
			)
			(pin bidirectional line
				(at -40.64 71.12 0)
				(length 5.08)
				(name "IO1_G2")
				(number "G2")
			)
			(pin bidirectional line
				(at -40.64 68.58 0)
				(length 5.08)
				(name "IO1_G3")
				(number "G3")
			)
			(pin bidirectional line
				(at -40.64 66.04 0)
				(length 5.08)
				(name "IO1_H1")
				(number "H1")
			)
			(pin bidirectional line
				(at -40.64 63.5 0)
				(length 5.08)
				(name "IO1_H2")
				(number "H2")
			)
			(pin bidirectional line
				(at -40.64 60.96 0)
				(length 5.08)
				(name "IO1_H3")
				(number "H3")
			)
			(pin bidirectional clock
				(at -40.64 58.42 0)
				(length 5.08)
				(name "IO1_H5/GCLK0")
				(number "H5")
			)
			(pin bidirectional line
				(at -40.64 55.88 0)
				(length 5.08)
				(name "IO1_J1")
				(number "J1")
			)
			(pin bidirectional line
				(at -40.64 53.34 0)
				(length 5.08)
				(name "IO1_J2")
				(number "J2")
			)
			(pin bidirectional line
				(at -40.64 50.8 0)
				(length 5.08)
				(name "IO1_J3")
				(number "J3")
			)
			(pin bidirectional clock
				(at -40.64 48.26 0)
				(length 5.08)
				(name "IO1_J5/GCLK1")
				(number "J5")
			)
			(pin bidirectional line
				(at -40.64 45.72 0)
				(length 5.08)
				(name "IO1_K1")
				(number "K1")
			)
			(pin bidirectional line
				(at -40.64 43.18 0)
				(length 5.08)
				(name "IO1_K2")
				(number "K2")
			)
			(pin bidirectional line
				(at -40.64 40.64 0)
				(length 5.08)
				(name "IO1_K3")
				(number "K3")
			)
			(pin bidirectional line
				(at -40.64 38.1 0)
				(length 5.08)
				(name "IO1_L1")
				(number "L1")
			)
			(pin bidirectional line
				(at -40.64 35.56 0)
				(length 5.08)
				(name "IO1_L2")
				(number "L2")
			)
			(pin bidirectional line
				(at -40.64 33.02 0)
				(length 5.08)
				(name "IO1_L3")
				(number "L3")
			)
			(pin bidirectional line
				(at -40.64 30.48 0)
				(length 5.08)
				(name "IO1_L4")
				(number "L4")
			)
			(pin bidirectional line
				(at -40.64 27.94 0)
				(length 5.08)
				(name "IO1_M1")
				(number "M1")
			)
			(pin bidirectional line
				(at -40.64 25.4 0)
				(length 5.08)
				(name "IO1_M2")
				(number "M2")
			)
			(pin bidirectional line
				(at -40.64 22.86 0)
				(length 5.08)
				(name "IO1_M3")
				(number "M3")
			)
			(pin bidirectional line
				(at -40.64 20.32 0)
				(length 5.08)
				(name "IO1_M4")
				(number "M4")
			)
			(pin bidirectional line
				(at -40.64 17.78 0)
				(length 5.08)
				(name "IO1_M8/DEV_OE")
				(number "M8")
			)
			(pin bidirectional line
				(at -40.64 15.24 0)
				(length 5.08)
				(name "IO1_M9/DEV_CLRn")
				(number "M9")
			)
			(pin bidirectional line
				(at -40.64 12.7 0)
				(length 5.08)
				(name "IO1_N1")
				(number "N1")
			)
			(pin bidirectional line
				(at -40.64 10.16 0)
				(length 5.08)
				(name "IO1_N2")
				(number "N2")
			)
			(pin bidirectional line
				(at -40.64 7.62 0)
				(length 5.08)
				(name "IO1_N3")
				(number "N3")
			)
			(pin bidirectional line
				(at -40.64 5.08 0)
				(length 5.08)
				(name "IO1_N5")
				(number "N5")
			)
			(pin bidirectional line
				(at -40.64 2.54 0)
				(length 5.08)
				(name "IO1_N12")
				(number "N12")
			)
			(pin bidirectional line
				(at -40.64 0 0)
				(length 5.08)
				(name "IO1_P2")
				(number "P2")
			)
			(pin bidirectional line
				(at -40.64 -2.54 0)
				(length 5.08)
				(name "IO1_P4")
				(number "P4")
			)
			(pin bidirectional line
				(at -40.64 -5.08 0)
				(length 5.08)
				(name "IO1_P5")
				(number "P5")
			)
			(pin bidirectional line
				(at -40.64 -7.62 0)
				(length 5.08)
				(name "IO1_P6")
				(number "P6")
			)
			(pin bidirectional line
				(at -40.64 -10.16 0)
				(length 5.08)
				(name "IO1_P7")
				(number "P7")
			)
			(pin bidirectional line
				(at -40.64 -12.7 0)
				(length 5.08)
				(name "IO1_P8")
				(number "P8")
			)
			(pin bidirectional line
				(at -40.64 -15.24 0)
				(length 5.08)
				(name "IO1_P9")
				(number "P9")
			)
			(pin bidirectional line
				(at -40.64 -17.78 0)
				(length 5.08)
				(name "IO1_P10")
				(number "P10")
			)
			(pin bidirectional line
				(at -40.64 -20.32 0)
				(length 5.08)
				(name "IO1_P11")
				(number "P11")
			)
			(pin bidirectional line
				(at -40.64 -22.86 0)
				(length 5.08)
				(name "IO1_P12")
				(number "P12")
			)
			(pin bidirectional line
				(at -40.64 -25.4 0)
				(length 5.08)
				(name "IO1_P13")
				(number "P13")
			)
			(pin bidirectional line
				(at -40.64 -27.94 0)
				(length 5.08)
				(name "IO1_R1")
				(number "R1")
			)
			(pin bidirectional line
				(at -40.64 -30.48 0)
				(length 5.08)
				(name "IO1_R3")
				(number "R3")
			)
			(pin bidirectional line
				(at -40.64 -33.02 0)
				(length 5.08)
				(name "IO1_R4")
				(number "R4")
			)
			(pin bidirectional line
				(at -40.64 -35.56 0)
				(length 5.08)
				(name "IO1_R5")
				(number "R5")
			)
			(pin bidirectional line
				(at -40.64 -38.1 0)
				(length 5.08)
				(name "IO1_R6")
				(number "R6")
			)
			(pin bidirectional line
				(at -40.64 -40.64 0)
				(length 5.08)
				(name "IO1_R7")
				(number "R7")
			)
			(pin bidirectional line
				(at -40.64 -43.18 0)
				(length 5.08)
				(name "IO1_R8")
				(number "R8")
			)
			(pin bidirectional line
				(at -40.64 -45.72 0)
				(length 5.08)
				(name "IO1_R9")
				(number "R9")
			)
			(pin bidirectional line
				(at -40.64 -48.26 0)
				(length 5.08)
				(name "IO1_R10")
				(number "R10")
			)
			(pin bidirectional line
				(at -40.64 -50.8 0)
				(length 5.08)
				(name "IO1_R11")
				(number "R11")
			)
			(pin bidirectional line
				(at -40.64 -53.34 0)
				(length 5.08)
				(name "IO1_R12")
				(number "R12")
			)
			(pin bidirectional line
				(at -40.64 -55.88 0)
				(length 5.08)
				(name "IO1_R13")
				(number "R13")
			)
			(pin bidirectional line
				(at -40.64 -58.42 0)
				(length 5.08)
				(name "IO1_R14")
				(number "R14")
			)
			(pin bidirectional line
				(at -40.64 -60.96 0)
				(length 5.08)
				(name "IO1_R16")
				(number "R16")
			)
			(pin bidirectional line
				(at -40.64 -63.5 0)
				(length 5.08)
				(name "IO1_T2")
				(number "T2")
			)
			(pin bidirectional line
				(at -40.64 -66.04 0)
				(length 5.08)
				(name "IO1_T4")
				(number "T4")
			)
			(pin bidirectional line
				(at -40.64 -68.58 0)
				(length 5.08)
				(name "IO1_T5")
				(number "T5")
			)
			(pin bidirectional line
				(at -40.64 -71.12 0)
				(length 5.08)
				(name "IO1_T6")
				(number "T6")
			)
			(pin bidirectional line
				(at -40.64 -73.66 0)
				(length 5.08)
				(name "IO1_T7")
				(number "T7")
			)
			(pin bidirectional line
				(at -40.64 -76.2 0)
				(length 5.08)
				(name "IO1_T8")
				(number "T8")
			)
			(pin bidirectional line
				(at -40.64 -78.74 0)
				(length 5.08)
				(name "IO1_T9")
				(number "T9")
			)
			(pin bidirectional line
				(at -40.64 -81.28 0)
				(length 5.08)
				(name "IO1_T10")
				(number "T10")
			)
			(pin bidirectional line
				(at -40.64 -83.82 0)
				(length 5.08)
				(name "IO1_T11")
				(number "T11")
			)
			(pin bidirectional line
				(at -40.64 -86.36 0)
				(length 5.08)
				(name "IO1_T12")
				(number "T12")
			)
			(pin bidirectional line
				(at -40.64 -88.9 0)
				(length 5.08)
				(name "IO1_T13")
				(number "T13")
			)
			(pin bidirectional line
				(at -40.64 -91.44 0)
				(length 5.08)
				(name "IO1_T15")
				(number "T15")
			)
			(pin input line
				(at -40.64 -93.98 0)
				(length 5.08)
				(name "TMS")
				(number "N4")
			)
			(pin input line
				(at -40.64 -96.52 0)
				(length 5.08)
				(name "TDI")
				(number "L6")
			)
			(pin input clock
				(at -40.64 -99.06 0)
				(length 5.08)
				(name "TCK")
				(number "P3")
			)
			(pin output line
				(at -40.64 -101.6 0)
				(length 5.08)
				(name "TDO")
				(number "M5")
			)
			(pin power_in line
				(at -25.4 111.76 270)
				(length 5.08)
				(name "VCCINT")
				(number "H8")
			)
			(pin power_in line
				(at -25.4 -111.76 90)
				(length 5.08)
				(name "GNDINT")
				(number "H7")
			)
			(pin power_in line
				(at -22.86 111.76 270)
				(length 5.08)
				(name "VCCINT")
				(number "H10")
			)
			(pin power_in line
				(at -22.86 -111.76 90)
				(length 5.08)
				(name "GNDINT")
				(number "H9")
			)
			(pin power_in line
				(at -20.32 111.76 270)
				(length 5.08)
				(name "VCCINT")
				(number "J7")
			)
			(pin power_in line
				(at -20.32 -111.76 90)
				(length 5.08)
				(name "GNDINT")
				(number "J8")
			)
			(pin power_in line
				(at -17.78 111.76 270)
				(length 5.08)
				(name "VCCINT")
				(number "J9")
			)
			(pin power_in line
				(at -17.78 -111.76 90)
				(length 5.08)
				(name "GNDINT")
				(number "J10")
			)
			(pin power_in line
				(at -15.24 111.76 270)
				(length 5.08)
				(name "VCCIO1")
				(number "C1")
			)
			(pin power_in line
				(at -15.24 -111.76 90)
				(length 5.08)
				(name "GNDIO")
				(number "A1")
			)
			(pin power_in line
				(at -12.7 111.76 270)
				(length 5.08)
				(name "VCCIO1")
				(number "H6")
			)
			(pin power_in line
				(at -12.7 -111.76 90)
				(length 5.08)
				(name "GNDIO")
				(number "A16")
			)
			(pin power_in line
				(at -10.16 111.76 270)
				(length 5.08)
				(name "VCCIO1")
				(number "J6")
			)
			(pin power_in line
				(at -10.16 -111.76 90)
				(length 5.08)
				(name "GNDIO")
				(number "B2")
			)
			(pin power_in line
				(at -7.62 111.76 270)
				(length 5.08)
				(name "VCCIO1")
				(number "P1")
			)
			(pin power_in line
				(at -7.62 -111.76 90)
				(length 5.08)
				(name "GNDIO")
				(number "B15")
			)
			(pin power_in line
				(at -5.08 111.76 270)
				(length 5.08)
				(name "VCCIO1")
				(number "T3")
			)
			(pin power_in line
				(at -5.08 -111.76 90)
				(length 5.08)
				(name "GNDIO")
				(number "G7")
			)
			(pin power_in line
				(at -2.54 111.76 270)
				(length 5.08)
				(name "VCCIO1")
				(number "L8")
			)
			(pin power_in line
				(at -2.54 -111.76 90)
				(length 5.08)
				(name "GNDIO")
				(number "G8")
			)
			(pin power_in line
				(at 0 111.76 270)
				(length 5.08)
				(name "VCCIO1")
				(number "L9")
			)
			(pin power_in line
				(at 0 -111.76 90)
				(length 5.08)
				(name "GNDIO")
				(number "G9")
			)
			(pin power_in line
				(at 2.54 111.76 270)
				(length 5.08)
				(name "VCCIO1")
				(number "T14")
			)
			(pin power_in line
				(at 2.54 -111.76 90)
				(length 5.08)
				(name "GNDIO")
				(number "G10")
			)
			(pin power_in line
				(at 5.08 111.76 270)
				(length 5.08)
				(name "VCCIO2")
				(number "P16")
			)
			(pin power_in line
				(at 5.08 -111.76 90)
				(length 5.08)
				(name "GNDIO")
				(number "K7")
			)
			(pin power_in line
				(at 7.62 111.76 270)
				(length 5.08)
				(name "VCCIO2")
				(number "J11")
			)
			(pin power_in line
				(at 7.62 -111.76 90)
				(length 5.08)
				(name "GNDIO")
				(number "K8")
			)
			(pin power_in line
				(at 10.16 111.76 270)
				(length 5.08)
				(name "VCCIO2")
				(number "H11")
			)
			(pin power_in line
				(at 10.16 -111.76 90)
				(length 5.08)
				(name "GNDIO")
				(number "K9")
			)
			(pin power_in line
				(at 12.7 111.76 270)
				(length 5.08)
				(name "VCCIO2")
				(number "C16")
			)
			(pin power_in line
				(at 12.7 -111.76 90)
				(length 5.08)
				(name "GNDIO")
				(number "K10")
			)
			(pin power_in line
				(at 15.24 111.76 270)
				(length 5.08)
				(name "VCCIO2")
				(number "A14")
			)
			(pin power_in line
				(at 15.24 -111.76 90)
				(length 5.08)
				(name "GNDIO")
				(number "R2")
			)
			(pin power_in line
				(at 17.78 111.76 270)
				(length 5.08)
				(name "VCCIO2")
				(number "F9")
			)
			(pin power_in line
				(at 17.78 -111.76 90)
				(length 5.08)
				(name "GNDIO")
				(number "R15")
			)
			(pin power_in line
				(at 20.32 111.76 270)
				(length 5.08)
				(name "VCCIO2")
				(number "F8")
			)
			(pin power_in line
				(at 20.32 -111.76 90)
				(length 5.08)
				(name "GNDIO")
				(number "T1")
			)
			(pin power_in line
				(at 22.86 111.76 270)
				(length 5.08)
				(name "VCCIO2")
				(number "A3")
			)
			(pin power_in line
				(at 22.86 -111.76 90)
				(length 5.08)
				(name "GNDIO")
				(number "T16")
			)
			(pin bidirectional line
				(at 40.64 104.14 180)
				(length 5.08)
				(name "IO2_A2")
				(number "A2")
			)
			(pin bidirectional line
				(at 40.64 101.6 180)
				(length 5.08)
				(name "IO2_A4")
				(number "A4")
			)
			(pin bidirectional line
				(at 40.64 99.06 180)
				(length 5.08)
				(name "IO2_A5")
				(number "A5")
			)
			(pin bidirectional line
				(at 40.64 96.52 180)
				(length 5.08)
				(name "IO2_A6")
				(number "A6")
			)
			(pin bidirectional line
				(at 40.64 93.98 180)
				(length 5.08)
				(name "IO2_A7")
				(number "A7")
			)
			(pin bidirectional line
				(at 40.64 91.44 180)
				(length 5.08)
				(name "IO2_A8")
				(number "A8")
			)
			(pin bidirectional line
				(at 40.64 88.9 180)
				(length 5.08)
				(name "IO2_A9")
				(number "A9")
			)
			(pin bidirectional line
				(at 40.64 86.36 180)
				(length 5.08)
				(name "IO2_A10")
				(number "A10")
			)
			(pin bidirectional line
				(at 40.64 83.82 180)
				(length 5.08)
				(name "IO2_A11")
				(number "A11")
			)
			(pin bidirectional line
				(at 40.64 81.28 180)
				(length 5.08)
				(name "IO2_A12")
				(number "A12")
			)
			(pin bidirectional line
				(at 40.64 78.74 180)
				(length 5.08)
				(name "IO2_A13")
				(number "A13")
			)
			(pin bidirectional line
				(at 40.64 76.2 180)
				(length 5.08)
				(name "IO2_A15")
				(number "A15")
			)
			(pin bidirectional line
				(at 40.64 73.66 180)
				(length 5.08)
				(name "IO2_B1")
				(number "B1")
			)
			(pin bidirectional line
				(at 40.64 71.12 180)
				(length 5.08)
				(name "IO2_B3")
				(number "B3")
			)
			(pin bidirectional line
				(at 40.64 68.58 180)
				(length 5.08)
				(name "IO2_B4")
				(number "B4")
			)
			(pin bidirectional line
				(at 40.64 66.04 180)
				(length 5.08)
				(name "IO2_B5")
				(number "B5")
			)
			(pin bidirectional line
				(at 40.64 63.5 180)
				(length 5.08)
				(name "IO2_B6")
				(number "B6")
			)
			(pin bidirectional line
				(at 40.64 60.96 180)
				(length 5.08)
				(name "IO2_B7")
				(number "B7")
			)
			(pin bidirectional line
				(at 40.64 58.42 180)
				(length 5.08)
				(name "IO2_B8")
				(number "B8")
			)
			(pin bidirectional line
				(at 40.64 55.88 180)
				(length 5.08)
				(name "IO2_B9")
				(number "B9")
			)
			(pin bidirectional line
				(at 40.64 53.34 180)
				(length 5.08)
				(name "IO2_B10")
				(number "B10")
			)
			(pin bidirectional line
				(at 40.64 50.8 180)
				(length 5.08)
				(name "IO2_B11")
				(number "B11")
			)
			(pin bidirectional line
				(at 40.64 48.26 180)
				(length 5.08)
				(name "IO2_B12")
				(number "B12")
			)
			(pin bidirectional line
				(at 40.64 45.72 180)
				(length 5.08)
				(name "IO2_B13")
				(number "B13")
			)
			(pin bidirectional line
				(at 40.64 43.18 180)
				(length 5.08)
				(name "IO2_B14")
				(number "B14")
			)
			(pin bidirectional line
				(at 40.64 40.64 180)
				(length 5.08)
				(name "IO2_B16")
				(number "B16")
			)
			(pin bidirectional line
				(at 40.64 38.1 180)
				(length 5.08)
				(name "IO2_C4")
				(number "C4")
			)
			(pin bidirectional line
				(at 40.64 35.56 180)
				(length 5.08)
				(name "IO2_C5")
				(number "C5")
			)
			(pin bidirectional line
				(at 40.64 33.02 180)
				(length 5.08)
				(name "IO2_C6")
				(number "C6")
			)
			(pin bidirectional line
				(at 40.64 30.48 180)
				(length 5.08)
				(name "IO2_C7")
				(number "C7")
			)
			(pin bidirectional line
				(at 40.64 27.94 180)
				(length 5.08)
				(name "IO2_C8")
				(number "C8")
			)
			(pin bidirectional line
				(at 40.64 25.4 180)
				(length 5.08)
				(name "IO2_C9")
				(number "C9")
			)
			(pin bidirectional line
				(at 40.64 22.86 180)
				(length 5.08)
				(name "IO2_C10")
				(number "C10")
			)
			(pin bidirectional line
				(at 40.64 20.32 180)
				(length 5.08)
				(name "IO2_C11")
				(number "C11")
			)
			(pin bidirectional line
				(at 40.64 17.78 180)
				(length 5.08)
				(name "IO2_C12")
				(number "C12")
			)
			(pin bidirectional line
				(at 40.64 15.24 180)
				(length 5.08)
				(name "IO2_C13")
				(number "C13")
			)
			(pin bidirectional line
				(at 40.64 12.7 180)
				(length 5.08)
				(name "IO2_C14")
				(number "C14")
			)
			(pin bidirectional line
				(at 40.64 10.16 180)
				(length 5.08)
				(name "IO2_C15")
				(number "C15")
			)
			(pin bidirectional line
				(at 40.64 7.62 180)
				(length 5.08)
				(name "IO2_D4")
				(number "D4")
			)
			(pin bidirectional line
				(at 40.64 5.08 180)
				(length 5.08)
				(name "IO2_D5")
				(number "D5")
			)
			(pin bidirectional line
				(at 40.64 2.54 180)
				(length 5.08)
				(name "IO2_D11")
				(number "D11")
			)
			(pin bidirectional line
				(at 40.64 0 180)
				(length 5.08)
				(name "IO2_D12")
				(number "D12")
			)
			(pin bidirectional line
				(at 40.64 -2.54 180)
				(length 5.08)
				(name "IO2_D13")
				(number "D13")
			)
			(pin bidirectional line
				(at 40.64 -5.08 180)
				(length 5.08)
				(name "IO2_D14")
				(number "D14")
			)
			(pin bidirectional line
				(at 40.64 -7.62 180)
				(length 5.08)
				(name "IO2_D15")
				(number "D15")
			)
			(pin bidirectional line
				(at 40.64 -10.16 180)
				(length 5.08)
				(name "IO2_D16")
				(number "D16")
			)
			(pin bidirectional line
				(at 40.64 -12.7 180)
				(length 5.08)
				(name "IO2_E13")
				(number "E13")
			)
			(pin bidirectional line
				(at 40.64 -15.24 180)
				(length 5.08)
				(name "IO2_E14")
				(number "E14")
			)
			(pin bidirectional line
				(at 40.64 -17.78 180)
				(length 5.08)
				(name "IO2_E15")
				(number "E15")
			)
			(pin bidirectional line
				(at 40.64 -20.32 180)
				(length 5.08)
				(name "IO2_E16")
				(number "E16")
			)
			(pin bidirectional line
				(at 40.64 -22.86 180)
				(length 5.08)
				(name "IO2_F13")
				(number "F13")
			)
			(pin bidirectional line
				(at 40.64 -25.4 180)
				(length 5.08)
				(name "IO2_F14")
				(number "F14")
			)
			(pin bidirectional line
				(at 40.64 -27.94 180)
				(length 5.08)
				(name "IO2_F15")
				(number "F15")
			)
			(pin bidirectional line
				(at 40.64 -30.48 180)
				(length 5.08)
				(name "IO2_F16")
				(number "F16")
			)
			(pin bidirectional line
				(at 40.64 -33.02 180)
				(length 5.08)
				(name "IO2_G14")
				(number "G14")
			)
			(pin bidirectional line
				(at 40.64 -35.56 180)
				(length 5.08)
				(name "IO2_G15")
				(number "G15")
			)
			(pin bidirectional line
				(at 40.64 -38.1 180)
				(length 5.08)
				(name "IO2_G16")
				(number "G16")
			)
			(pin bidirectional clock
				(at 40.64 -40.64 180)
				(length 5.08)
				(name "IO2_H12/GCLK3")
				(number "H12")
			)
			(pin bidirectional line
				(at 40.64 -43.18 180)
				(length 5.08)
				(name "IO2_H14")
				(number "H14")
			)
			(pin bidirectional line
				(at 40.64 -45.72 180)
				(length 5.08)
				(name "IO2_H15")
				(number "H15")
			)
			(pin bidirectional line
				(at 40.64 -48.26 180)
				(length 5.08)
				(name "IO2_H16")
				(number "H16")
			)
			(pin bidirectional clock
				(at 40.64 -50.8 180)
				(length 5.08)
				(name "IO2_J12/GCLK2")
				(number "J12")
			)
			(pin bidirectional line
				(at 40.64 -53.34 180)
				(length 5.08)
				(name "IO2_J14")
				(number "J14")
			)
			(pin bidirectional line
				(at 40.64 -55.88 180)
				(length 5.08)
				(name "IO2_J15")
				(number "J15")
			)
			(pin bidirectional line
				(at 40.64 -58.42 180)
				(length 5.08)
				(name "IO2_J16")
				(number "J16")
			)
			(pin bidirectional line
				(at 40.64 -60.96 180)
				(length 5.08)
				(name "IO2_K14")
				(number "K14")
			)
			(pin bidirectional line
				(at 40.64 -63.5 180)
				(length 5.08)
				(name "IO2_K15")
				(number "K15")
			)
			(pin bidirectional line
				(at 40.64 -66.04 180)
				(length 5.08)
				(name "IO2_K16")
				(number "K16")
			)
			(pin bidirectional line
				(at 40.64 -68.58 180)
				(length 5.08)
				(name "IO2_L13")
				(number "L13")
			)
			(pin bidirectional line
				(at 40.64 -71.12 180)
				(length 5.08)
				(name "IO2_L14")
				(number "L14")
			)
			(pin bidirectional line
				(at 40.64 -73.66 180)
				(length 5.08)
				(name "IO2_L15")
				(number "L15")
			)
			(pin bidirectional line
				(at 40.64 -76.2 180)
				(length 5.08)
				(name "IO2_L16")
				(number "L16")
			)
			(pin bidirectional line
				(at 40.64 -78.74 180)
				(length 5.08)
				(name "IO2_M13")
				(number "M13")
			)
			(pin bidirectional line
				(at 40.64 -81.28 180)
				(length 5.08)
				(name "IO2_M14")
				(number "M14")
			)
			(pin bidirectional line
				(at 40.64 -83.82 180)
				(length 5.08)
				(name "IO2_M15")
				(number "M15")
			)
			(pin bidirectional line
				(at 40.64 -86.36 180)
				(length 5.08)
				(name "IO2_M16")
				(number "M16")
			)
			(pin bidirectional line
				(at 40.64 -88.9 180)
				(length 5.08)
				(name "IO2_N13")
				(number "N13")
			)
			(pin bidirectional line
				(at 40.64 -91.44 180)
				(length 5.08)
				(name "IO2_N14")
				(number "N14")
			)
			(pin bidirectional line
				(at 40.64 -93.98 180)
				(length 5.08)
				(name "IO2_N15")
				(number "N15")
			)
			(pin bidirectional line
				(at 40.64 -96.52 180)
				(length 5.08)
				(name "IO2_N16")
				(number "N16")
			)
			(pin bidirectional line
				(at 40.64 -99.06 180)
				(length 5.08)
				(name "IO2_P14")
				(number "P14")
			)
			(pin bidirectional line
				(at 40.64 -101.6 180)
				(length 5.08)
				(name "IO2_P15")
				(number "P15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EPM570M100"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 12.7 54.61 0)
		)
		(property "Value" "EPM570M100"
			(at 12.7 -54.61 0)
		)
		(property "Footprint" "Package_BGA:BGA-100_6.0x6.0mm_Layout11x11_P0.5mm_Ball0.3mm_Pad0.25mm_NSMD"
			(at 12.7 -57.15 0)
		)
		(property "Datasheet" "https://www.altera.com/content/dam/altera-www/global/en_US/pdfs/literature/hb/max2/max2_mii5v1.pdf"
			(at 0 0 0)
		)
		(property "Description" "Altera MAX2 CPLD with 570 LE"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "MAX2 MBGA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*BGA*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "EPM570M100_1_1"
			(pin bidirectional line
				(at -27.94 50.8 0)
				(length 5.08)
				(name "IO1_B1")
				(number "B1")
			)
			(pin bidirectional line
				(at -27.94 48.26 0)
				(length 5.08)
				(name "IO1_C1")
				(number "C1")
			)
			(pin bidirectional line
				(at -27.94 45.72 0)
				(length 5.08)
				(name "IO1_C2")
				(number "C2")
			)
			(pin bidirectional line
				(at -27.94 43.18 0)
				(length 5.08)
				(name "IO1_D1")
				(number "D1")
			)
			(pin bidirectional line
				(at -27.94 40.64 0)
				(length 5.08)
				(name "IO1_D2")
				(number "D2")
			)
			(pin bidirectional line
				(at -27.94 38.1 0)
				(length 5.08)
				(name "IO1_D3")
				(number "D3")
			)
			(pin bidirectional clock
				(at -27.94 35.56 0)
				(length 5.08)
				(name "IO1_E1/GCLK1")
				(number "E1")
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 5.08)
				(name "IO1_E2")
				(number "E2")
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 5.08)
				(name "IO1_F1")
				(number "F1")
			)
			(pin bidirectional clock
				(at -27.94 27.94 0)
				(length 5.08)
				(name "IO1_F2/GCLK0")
				(number "F2")
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 5.08)
				(name "IO1_F3")
				(number "F3")
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 5.08)
				(name "IO1_G1")
				(number "G1")
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 5.08)
				(name "IO1_G2")
				(number "G2")
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 5.08)
				(name "IO1_H1")
				(number "H1")
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 5.08)
				(name "IO1_H2")
				(number "H2")
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 5.08)
				(name "IO1_H3")
				(number "H3")
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 5.08)
				(name "IO1_J6")
				(number "J6")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 5.08)
				(name "IO1_K3")
				(number "K3")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 5.08)
				(name "IO1_K4")
				(number "K4")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 5.08)
				(name "IO1_K5")
				(number "K5")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 5.08)
				(name "IO1_K6")
				(number "K6")
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 5.08)
				(name "IO1_K7")
				(number "K7")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 5.08)
				(name "IO1_K8/DEV_CLRn")
				(number "K8")
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 5.08)
				(name "IO1_K9")
				(number "K9")
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 5.08)
				(name "IO1_K10")
				(number "K10")
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 5.08)
				(name "IO1_L1")
				(number "L1")
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 5.08)
				(name "IO1_L2")
				(number "L2")
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 5.08)
				(name "IO1_L3")
				(number "L3")
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 5.08)
				(name "IO1_L4")
				(number "L4")
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 5.08)
				(name "IO1_L5")
				(number "L5")
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 5.08)
				(name "IO1_L6")
				(number "L6")
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 5.08)
				(name "IO1_L7")
				(number "L7")
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 5.08)
				(name "IO1_L8/DEV_OE")
				(number "L8")
			)
			(pin bidirectional line
				(at -27.94 -33.02 0)
				(length 5.08)
				(name "IO1_L9")
				(number "L9")
			)
			(pin bidirectional line
				(at -27.94 -35.56 0)
				(length 5.08)
				(name "IO1_L10")
				(number "L10")
			)
			(pin bidirectional line
				(at -27.94 -38.1 0)
				(length 5.08)
				(name "IO1_L11")
				(number "L11")
			)
			(pin input line
				(at -27.94 -40.64 0)
				(length 5.08)
				(name "TMS")
				(number "J1")
			)
			(pin input line
				(at -27.94 -43.18 0)
				(length 5.08)
				(name "TDI")
				(number "J2")
			)
			(pin input clock
				(at -27.94 -45.72 0)
				(length 5.08)
				(name "TCK")
				(number "K1")
			)
			(pin output line
				(at -27.94 -48.26 0)
				(length 5.08)
				(name "TDO")
				(number "K2")
			)
			(pin power_in line
				(at -12.7 58.42 270)
				(length 5.08)
				(name "VCCINT")
				(number "G3")
			)
			(pin power_in line
				(at -12.7 -58.42 90)
				(length 5.08)
				(name "GNDINT")
				(number "G4")
			)
			(pin power_in line
				(at -10.16 58.42 270)
				(length 5.08)
				(name "VCCINT")
				(number "J7")
			)
			(pin power_in line
				(at -10.16 -58.42 90)
				(length 5.08)
				(name "GNDINT")
				(number "J5")
			)
			(pin power_in line
				(at -7.62 58.42 270)
				(length 5.08)
				(name "VCCINT")
				(number "E9")
			)
			(pin power_in line
				(at -7.62 -58.42 90)
				(length 5.08)
				(name "GNDINT")
				(number "E8")
			)
			(pin power_in line
				(at -5.08 58.42 270)
				(length 5.08)
				(name "VCCINT")
				(number "C7")
			)
			(pin power_in line
				(at -5.08 -58.42 90)
				(length 5.08)
				(name "GNDINT")
				(number "C5")
			)
			(pin power_in line
				(at -2.54 58.42 270)
				(length 5.08)
				(name "VCCIO1")
				(number "E3")
			)
			(pin power_in line
				(at -2.54 -58.42 90)
				(length 5.08)
				(name "GNDIO")
				(number "E4")
			)
			(pin power_in line
				(at 0 58.42 270)
				(length 5.08)
				(name "VCCIO1")
				(number "J4")
			)
			(pin power_in line
				(at 0 -58.42 90)
				(length 5.08)
				(name "GNDIO")
				(number "H5")
			)
			(pin power_in line
				(at 2.54 58.42 270)
				(length 5.08)
				(name "VCCIO1")
				(number "J8")
			)
			(pin power_in line
				(at 2.54 -58.42 90)
				(length 5.08)
				(name "GNDIO")
				(number "H7")
			)
			(pin power_in line
				(at 5.08 58.42 270)
				(length 5.08)
				(name "VCCIO2")
				(number "G9")
			)
			(pin power_in line
				(at 5.08 -58.42 90)
				(length 5.08)
				(name "GNDIO")
				(number "G8")
			)
			(pin power_in line
				(at 7.62 58.42 270)
				(length 5.08)
				(name "VCCIO2")
				(number "C8")
			)
			(pin power_in line
				(at 7.62 -58.42 90)
				(length 5.08)
				(name "GNDIO")
				(number "D7")
			)
			(pin power_in line
				(at 10.16 58.42 270)
				(length 5.08)
				(name "VCCIO2")
				(number "C4")
			)
			(pin power_in line
				(at 10.16 -58.42 90)
				(length 5.08)
				(name "GNDIO")
				(number "D5")
			)
			(pin bidirectional line
				(at 27.94 50.8 180)
				(length 5.08)
				(name "IO2_A1")
				(number "A1")
			)
			(pin bidirectional line
				(at 27.94 48.26 180)
				(length 5.08)
				(name "IO2_A2")
				(number "A2")
			)
			(pin bidirectional line
				(at 27.94 45.72 180)
				(length 5.08)
				(name "IO2_A3")
				(number "A3")
			)
			(pin bidirectional line
				(at 27.94 43.18 180)
				(length 5.08)
				(name "IO2_A4")
				(number "A4")
			)
			(pin bidirectional line
				(at 27.94 40.64 180)
				(length 5.08)
				(name "IO2_A5")
				(number "A5")
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 5.08)
				(name "IO2_A6")
				(number "A6")
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 5.08)
				(name "IO2_A7")
				(number "A7")
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 5.08)
				(name "IO2_A8")
				(number "A8")
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 5.08)
				(name "IO2_A9")
				(number "A9")
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 5.08)
				(name "IO2_A10")
				(number "A10")
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 5.08)
				(name "IO2_A11")
				(number "A11")
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 5.08)
				(name "IO2_B2")
				(number "B2")
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 5.08)
				(name "IO2_B3")
				(number "B3")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 5.08)
				(name "IO2_B4")
				(number "B4")
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 5.08)
				(name "IO2_B5")
				(number "B5")
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 5.08)
				(name "IO2_B6")
				(number "B6")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 5.08)
				(name "IO2_B7")
				(number "B7")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 5.08)
				(name "IO2_B8")
				(number "B8")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 5.08)
				(name "IO2_B9")
				(number "B9")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 5.08)
				(name "IO2_B10")
				(number "B10")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 5.08)
				(name "IO2_B11")
				(number "B11")
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 5.08)
				(name "IO2_C6")
				(number "C6")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 5.08)
				(name "IO2_C10")
				(number "C10")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 5.08)
				(name "IO2_C11")
				(number "C11")
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 5.08)
				(name "IO2_D9")
				(number "D9")
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 5.08)
				(name "IO2_D10")
				(number "D10")
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 5.08)
				(name "IO2_D11")
				(number "D11")
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 5.08)
				(name "IO2_E10")
				(number "E10")
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 5.08)
				(name "IO2_E11")
				(number "E11")
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 5.08)
				(name "IO2_F9")
				(number "F9")
			)
			(pin bidirectional clock
				(at 27.94 -25.4 180)
				(length 5.08)
				(name "IO2_F10/GCLK2")
				(number "F10")
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 5.08)
				(name "IO2_F11")
				(number "F11")
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 5.08)
				(name "IO2_G10")
				(number "G10")
			)
			(pin bidirectional clock
				(at 27.94 -33.02 180)
				(length 5.08)
				(name "IO2_G11/GCLK3")
				(number "G11")
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 5.08)
				(name "IO2_H9")
				(number "H9")
			)
			(pin bidirectional line
				(at 27.94 -38.1 180)
				(length 5.08)
				(name "IO2_H10")
				(number "H10")
			)
			(pin bidirectional line
				(at 27.94 -40.64 180)
				(length 5.08)
				(name "IO2_H11")
				(number "H11")
			)
			(pin bidirectional line
				(at 27.94 -43.18 180)
				(length 5.08)
				(name "IO2_J10")
				(number "J10")
			)
			(pin bidirectional line
				(at 27.94 -45.72 180)
				(length 5.08)
				(name "IO2_J11")
				(number "J11")
			)
			(pin bidirectional line
				(at 27.94 -48.26 180)
				(length 5.08)
				(name "IO2_K11")
				(number "K11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EPM570M256"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 25.4 107.95 0)
		)
		(property "Value" "EPM570M256"
			(at 25.4 -107.95 0)
		)
		(property "Footprint" "Package_BGA:BGA-256_11.0x11.0mm_Layout20x20_P0.5mm_Ball0.3mm_Pad0.25mm_NSMD"
			(at 25.4 -110.49 0)
		)
		(property "Datasheet" "https://www.altera.com/content/dam/altera-www/global/en_US/pdfs/literature/hb/max2/max2_mii5v1.pdf"
			(at 0 0 0)
		)
		(property "Description" "Altera MAX2 CPLD with 570 LE"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "MAX2 MBGA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*BGA*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "EPM570M256_1_1"
			(pin bidirectional line
				(at -40.64 104.14 0)
				(length 5.08)
				(name "IO1_B1")
				(number "B1")
			)
			(pin bidirectional line
				(at -40.64 101.6 0)
				(length 5.08)
				(name "IO1_C1")
				(number "C1")
			)
			(pin bidirectional line
				(at -40.64 99.06 0)
				(length 5.08)
				(name "IO1_C2")
				(number "C2")
			)
			(pin bidirectional line
				(at -40.64 96.52 0)
				(length 5.08)
				(name "IO1_C3")
				(number "C3")
			)
			(pin bidirectional line
				(at -40.64 93.98 0)
				(length 5.08)
				(name "IO1_D1")
				(number "D1")
			)
			(pin bidirectional line
				(at -40.64 91.44 0)
				(length 5.08)
				(name "IO1_D2")
				(number "D2")
			)
			(pin bidirectional line
				(at -40.64 88.9 0)
				(length 5.08)
				(name "IO1_D3")
				(number "D3")
			)
			(pin bidirectional line
				(at -40.64 86.36 0)
				(length 5.08)
				(name "IO1_E1")
				(number "E1")
			)
			(pin bidirectional line
				(at -40.64 83.82 0)
				(length 5.08)
				(name "IO1_E2")
				(number "E2")
			)
			(pin bidirectional line
				(at -40.64 81.28 0)
				(length 5.08)
				(name "IO1_E3")
				(number "E3")
			)
			(pin bidirectional line
				(at -40.64 78.74 0)
				(length 5.08)
				(name "IO1_F1")
				(number "F1")
			)
			(pin bidirectional line
				(at -40.64 76.2 0)
				(length 5.08)
				(name "IO1_F2")
				(number "F2")
			)
			(pin bidirectional line
				(at -40.64 73.66 0)
				(length 5.08)
				(name "IO1_F3")
				(number "F3")
			)
			(pin bidirectional line
				(at -40.64 71.12 0)
				(length 5.08)
				(name "IO1_G1")
				(number "G1")
			)
			(pin bidirectional line
				(at -40.64 68.58 0)
				(length 5.08)
				(name "IO1_G2")
				(number "G2")
			)
			(pin bidirectional line
				(at -40.64 66.04 0)
				(length 5.08)
				(name "IO1_H1")
				(number "H1")
			)
			(pin bidirectional line
				(at -40.64 63.5 0)
				(length 5.08)
				(name "IO1_H2")
				(number "H2")
			)
			(pin bidirectional line
				(at -40.64 60.96 0)
				(length 5.08)
				(name "IO1_J1")
				(number "J1")
			)
			(pin bidirectional line
				(at -40.64 58.42 0)
				(length 5.08)
				(name "IO1_J2")
				(number "J2")
			)
			(pin bidirectional clock
				(at -40.64 55.88 0)
				(length 5.08)
				(name "IO1_K1/GCLK0")
				(number "K1")
			)
			(pin bidirectional clock
				(at -40.64 53.34 0)
				(length 5.08)
				(name "IO1_L1/GCLK1")
				(number "L1")
			)
			(pin bidirectional line
				(at -40.64 50.8 0)
				(length 5.08)
				(name "IO1_M1")
				(number "M1")
			)
			(pin bidirectional line
				(at -40.64 48.26 0)
				(length 5.08)
				(name "IO1_M2")
				(number "M2")
			)
			(pin bidirectional line
				(at -40.64 45.72 0)
				(length 5.08)
				(name "IO1_N1")
				(number "N1")
			)
			(pin bidirectional line
				(at -40.64 43.18 0)
				(length 5.08)
				(name "IO1_N2")
				(number "N2")
			)
			(pin bidirectional line
				(at -40.64 40.64 0)
				(length 5.08)
				(name "IO1_P1")
				(number "P1")
			)
			(pin bidirectional line
				(at -40.64 38.1 0)
				(length 5.08)
				(name "IO1_P2")
				(number "P2")
			)
			(pin bidirectional line
				(at -40.64 35.56 0)
				(length 5.08)
				(name "IO1_R1")
				(number "R1")
			)
			(pin bidirectional line
				(at -40.64 33.02 0)
				(length 5.08)
				(name "IO1_R2")
				(number "R2")
			)
			(pin bidirectional line
				(at -40.64 30.48 0)
				(length 5.08)
				(name "IO1_R3")
				(number "R3")
			)
			(pin bidirectional line
				(at -40.64 27.94 0)
				(length 5.08)
				(name "IO1_T1")
				(number "T1")
			)
			(pin bidirectional line
				(at -40.64 25.4 0)
				(length 5.08)
				(name "IO1_T2")
				(number "T2")
			)
			(pin bidirectional line
				(at -40.64 22.86 0)
				(length 5.08)
				(name "IO1_T4")
				(number "T4")
			)
			(pin bidirectional line
				(at -40.64 20.32 0)
				(length 5.08)
				(name "IO1_U1")
				(number "U1")
			)
			(pin bidirectional line
				(at -40.64 17.78 0)
				(length 5.08)
				(name "IO1_U3")
				(number "U3")
			)
			(pin bidirectional line
				(at -40.64 15.24 0)
				(length 5.08)
				(name "IO1_U4")
				(number "U4")
			)
			(pin bidirectional line
				(at -40.64 12.7 0)
				(length 5.08)
				(name "IO1_V1")
				(number "V1")
			)
			(pin bidirectional line
				(at -40.64 10.16 0)
				(length 5.08)
				(name "IO1_V3")
				(number "V3")
			)
			(pin bidirectional line
				(at -40.64 7.62 0)
				(length 5.08)
				(name "IO1_V4")
				(number "V4")
			)
			(pin bidirectional line
				(at -40.64 5.08 0)
				(length 5.08)
				(name "IO1_V5")
				(number "V5")
			)
			(pin bidirectional line
				(at -40.64 2.54 0)
				(length 5.08)
				(name "IO1_V6")
				(number "V6")
			)
			(pin bidirectional line
				(at -40.64 0 0)
				(length 5.08)
				(name "IO1_V16")
				(number "V16")
			)
			(pin bidirectional line
				(at -40.64 -2.54 0)
				(length 5.08)
				(name "IO1_V17")
				(number "V17")
			)
			(pin bidirectional line
				(at -40.64 -5.08 0)
				(length 5.08)
				(name "IO1_V18")
				(number "V18")
			)
			(pin bidirectional line
				(at -40.64 -7.62 0)
				(length 5.08)
				(name "IO1_W1")
				(number "W1")
			)
			(pin bidirectional line
				(at -40.64 -10.16 0)
				(length 5.08)
				(name "IO1_W3")
				(number "W3")
			)
			(pin bidirectional line
				(at -40.64 -12.7 0)
				(length 5.08)
				(name "IO1_W4")
				(number "W4")
			)
			(pin bidirectional line
				(at -40.64 -15.24 0)
				(length 5.08)
				(name "IO1_W5")
				(number "W5")
			)
			(pin bidirectional line
				(at -40.64 -17.78 0)
				(length 5.08)
				(name "IO1_W6")
				(number "W6")
			)
			(pin bidirectional line
				(at -40.64 -20.32 0)
				(length 5.08)
				(name "IO1_W7")
				(number "W7")
			)
			(pin bidirectional line
				(at -40.64 -22.86 0)
				(length 5.08)
				(name "IO1_W8")
				(number "W8")
			)
			(pin bidirectional line
				(at -40.64 -25.4 0)
				(length 5.08)
				(name "IO1_W11")
				(number "W11")
			)
			(pin bidirectional line
				(at -40.64 -27.94 0)
				(length 5.08)
				(name "IO1_W12/DEV_OE")
				(number "W12")
			)
			(pin bidirectional line
				(at -40.64 -30.48 0)
				(length 5.08)
				(name "IO1_W13")
				(number "W13")
			)
			(pin bidirectional line
				(at -40.64 -33.02 0)
				(length 5.08)
				(name "IO1_W14")
				(number "W14")
			)
			(pin bidirectional line
				(at -40.64 -35.56 0)
				(length 5.08)
				(name "IO1_W15")
				(number "W15")
			)
			(pin bidirectional line
				(at -40.64 -38.1 0)
				(length 5.08)
				(name "IO1_W16")
				(number "W16")
			)
			(pin bidirectional line
				(at -40.64 -40.64 0)
				(length 5.08)
				(name "IO1_W17")
				(number "W17")
			)
			(pin bidirectional line
				(at -40.64 -43.18 0)
				(length 5.08)
				(name "IO1_W18")
				(number "W18")
			)
			(pin bidirectional line
				(at -40.64 -45.72 0)
				(length 5.08)
				(name "IO1_Y1")
				(number "Y1")
			)
			(pin bidirectional line
				(at -40.64 -48.26 0)
				(length 5.08)
				(name "IO1_Y2")
				(number "Y2")
			)
			(pin bidirectional line
				(at -40.64 -50.8 0)
				(length 5.08)
				(name "IO1_Y3")
				(number "Y3")
			)
			(pin bidirectional line
				(at -40.64 -53.34 0)
				(length 5.08)
				(name "IO1_Y4")
				(number "Y4")
			)
			(pin bidirectional line
				(at -40.64 -55.88 0)
				(length 5.08)
				(name "IO1_Y5")
				(number "Y5")
			)
			(pin bidirectional line
				(at -40.64 -58.42 0)
				(length 5.08)
				(name "IO1_Y6")
				(number "Y6")
			)
			(pin bidirectional line
				(at -40.64 -60.96 0)
				(length 5.08)
				(name "IO1_Y7")
				(number "Y7")
			)
			(pin bidirectional line
				(at -40.64 -63.5 0)
				(length 5.08)
				(name "IO1_Y8")
				(number "Y8")
			)
			(pin bidirectional line
				(at -40.64 -66.04 0)
				(length 5.08)
				(name "IO1_Y9")
				(number "Y9")
			)
			(pin bidirectional line
				(at -40.64 -68.58 0)
				(length 5.08)
				(name "IO1_Y10")
				(number "Y10")
			)
			(pin bidirectional line
				(at -40.64 -71.12 0)
				(length 5.08)
				(name "IO1_Y11")
				(number "Y11")
			)
			(pin bidirectional line
				(at -40.64 -73.66 0)
				(length 5.08)
				(name "IO1_Y12")
				(number "Y12")
			)
			(pin bidirectional line
				(at -40.64 -76.2 0)
				(length 5.08)
				(name "IO1_Y13/DEV_CLRn")
				(number "Y13")
			)
			(pin bidirectional line
				(at -40.64 -78.74 0)
				(length 5.08)
				(name "IO1_Y14")
				(number "Y14")
			)
			(pin bidirectional line
				(at -40.64 -81.28 0)
				(length 5.08)
				(name "IO1_Y15")
				(number "Y15")
			)
			(pin bidirectional line
				(at -40.64 -83.82 0)
				(length 5.08)
				(name "IO1_Y16")
				(number "Y16")
			)
			(pin bidirectional line
				(at -40.64 -86.36 0)
				(length 5.08)
				(name "IO1_Y17")
				(number "Y17")
			)
			(pin bidirectional line
				(at -40.64 -88.9 0)
				(length 5.08)
				(name "IO1_Y18")
				(number "Y18")
			)
			(pin bidirectional line
				(at -40.64 -91.44 0)
				(length 5.08)
				(name "IO1_Y19")
				(number "Y19")
			)
			(pin input line
				(at -40.64 -93.98 0)
				(length 5.08)
				(name "TMS")
				(number "T3")
			)
			(pin input line
				(at -40.64 -96.52 0)
				(length 5.08)
				(name "TDI")
				(number "U2")
			)
			(pin input clock
				(at -40.64 -99.06 0)
				(length 5.08)
				(name "TCK")
				(number "W2")
			)
			(pin output line
				(at -40.64 -101.6 0)
				(length 5.08)
				(name "TDO")
				(number "V2")
			)
			(pin power_in line
				(at -25.4 111.76 270)
				(length 5.08)
				(name "VCCINT")
				(number "K4")
			)
			(pin power_in line
				(at -25.4 -111.76 90)
				(length 5.08)
				(name "GNDINT")
				(number "J4")
			)
			(pin power_in line
				(at -22.86 111.76 270)
				(length 5.08)
				(name "VCCINT")
				(number "U11")
			)
			(pin power_in line
				(at -22.86 -111.76 90)
				(length 5.08)
				(name "GNDINT")
				(number "U12")
			)
			(pin power_in line
				(at -20.32 111.76 270)
				(length 5.08)
				(name "VCCINT")
				(number "L17")
			)
			(pin power_in line
				(at -20.32 -111.76 90)
				(length 5.08)
				(name "GNDINT")
				(number "M17")
			)
			(pin power_in line
				(at -17.78 111.76 270)
				(length 5.08)
				(name "VCCINT")
				(number "D11")
			)
			(pin power_in line
				(at -17.78 -111.76 90)
				(length 5.08)
				(name "GNDINT")
				(number "D12")
			)
			(pin power_in line
				(at -15.24 111.76 270)
				(length 5.08)
				(name "VCCIO1")
				(number "K3")
			)
			(pin power_in line
				(at -15.24 -111.76 90)
				(length 5.08)
				(name "GNDIO")
				(number "H3")
			)
			(pin power_in line
				(at -12.7 111.76 270)
				(length 5.08)
				(name "VCCIO1")
				(number "L3")
			)
			(pin power_in line
				(at -12.7 -111.76 90)
				(length 5.08)
				(name "GNDIO")
				(number "J3")
			)
			(pin power_in line
				(at -10.16 111.76 270)
				(length 5.08)
				(name "VCCIO1")
				(number "L4")
			)
			(pin power_in line
				(at -10.16 -111.76 90)
				(length 5.08)
				(name "GNDIO")
				(number "M4")
			)
			(pin power_in line
				(at -7.62 111.76 270)
				(length 5.08)
				(name "VCCIO1")
				(number "M3")
			)
			(pin power_in line
				(at -7.62 -111.76 90)
				(length 5.08)
				(name "GNDIO")
				(number "N3")
			)
			(pin power_in line
				(at -5.08 111.76 270)
				(length 5.08)
				(name "VCCIO1")
				(number "U10")
			)
			(pin power_in line
				(at -5.08 -111.76 90)
				(length 5.08)
				(name "GNDIO")
				(number "U9")
			)
			(pin power_in line
				(at -2.54 111.76 270)
				(length 5.08)
				(name "VCCIO1")
				(number "V10")
			)
			(pin power_in line
				(at -2.54 -111.76 90)
				(length 5.08)
				(name "GNDIO")
				(number "V8")
			)
			(pin power_in line
				(at 0 111.76 270)
				(length 5.08)
				(name "VCCIO1")
				(number "V11")
			)
			(pin power_in line
				(at 0 -111.76 90)
				(length 5.08)
				(name "GNDIO")
				(number "V9")
			)
			(pin power_in line
				(at 2.54 111.76 270)
				(length 5.08)
				(name "VCCIO1")
				(number "V12")
			)
			(pin power_in line
				(at 2.54 -111.76 90)
				(length 5.08)
				(name "GNDIO")
				(number "V13")
			)
			(pin power_in line
				(at 5.08 111.76 270)
				(length 5.08)
				(name "VCCIO2")
				(number "J18")
			)
			(pin power_in line
				(at 5.08 -111.76 90)
				(length 5.08)
				(name "GNDIO")
				(number "H18")
			)
			(pin power_in line
				(at 7.62 111.76 270)
				(length 5.08)
				(name "VCCIO2")
				(number "K17")
			)
			(pin power_in line
				(at 7.62 -111.76 90)
				(length 5.08)
				(name "GNDIO")
				(number "J17")
			)
			(pin power_in line
				(at 10.16 111.76 270)
				(length 5.08)
				(name "VCCIO2")
				(number "K18")
			)
			(pin power_in line
				(at 10.16 -111.76 90)
				(length 5.08)
				(name "GNDIO")
				(number "N18")
			)
			(pin power_in line
				(at 12.7 111.76 270)
				(length 5.08)
				(name "VCCIO2")
				(number "L18")
			)
			(pin power_in line
				(at 12.7 -111.76 90)
				(length 5.08)
				(name "GNDIO")
				(number "C8")
			)
			(pin power_in line
				(at 15.24 111.76 270)
				(length 5.08)
				(name "VCCIO2")
				(number "C9")
			)
			(pin power_in line
				(at 15.24 -111.76 90)
				(length 5.08)
				(name "GNDIO")
				(number "D9")
			)
			(pin power_in line
				(at 17.78 111.76 270)
				(length 5.08)
				(name "VCCIO2")
				(number "C10")
			)
			(pin power_in line
				(at 17.78 -111.76 90)
				(length 5.08)
				(name "GNDIO")
				(number "C12")
			)
			(pin power_in line
				(at 20.32 111.76 270)
				(length 5.08)
				(name "VCCIO2")
				(number "D10")
			)
			(pin power_in line
				(at 20.32 -111.76 90)
				(length 5.08)
				(name "GNDIO")
				(number "C13")
			)
			(pin power_in line
				(at 22.86 111.76 270)
				(length 5.08)
				(name "VCCIO2")
				(number "C11")
			)
			(pin power_in line
				(at 22.86 -111.76 90)
				(length 5.08)
				(name "GNDIO")
				(number "M18")
			)
			(pin bidirectional line
				(at 40.64 104.14 180)
				(length 5.08)
				(name "IO2_A1")
				(number "A1")
			)
			(pin bidirectional line
				(at 40.64 101.6 180)
				(length 5.08)
				(name "IO2_A2")
				(number "A2")
			)
			(pin bidirectional line
				(at 40.64 99.06 180)
				(length 5.08)
				(name "IO2_A3")
				(number "A3")
			)
			(pin bidirectional line
				(at 40.64 96.52 180)
				(length 5.08)
				(name "IO2_A4")
				(number "A4")
			)
			(pin bidirectional line
				(at 40.64 93.98 180)
				(length 5.08)
				(name "IO2_A5")
				(number "A5")
			)
			(pin bidirectional line
				(at 40.64 91.44 180)
				(length 5.08)
				(name "IO2_A6")
				(number "A6")
			)
			(pin bidirectional line
				(at 40.64 88.9 180)
				(length 5.08)
				(name "IO2_A7")
				(number "A7")
			)
			(pin bidirectional line
				(at 40.64 86.36 180)
				(length 5.08)
				(name "IO2_A8")
				(number "A8")
			)
			(pin bidirectional line
				(at 40.64 83.82 180)
				(length 5.08)
				(name "IO2_A9")
				(number "A9")
			)
			(pin bidirectional line
				(at 40.64 81.28 180)
				(length 5.08)
				(name "IO2_A10")
				(number "A10")
			)
			(pin bidirectional line
				(at 40.64 78.74 180)
				(length 5.08)
				(name "IO2_A11")
				(number "A11")
			)
			(pin bidirectional line
				(at 40.64 76.2 180)
				(length 5.08)
				(name "IO2_A12")
				(number "A12")
			)
			(pin bidirectional line
				(at 40.64 73.66 180)
				(length 5.08)
				(name "IO2_A13")
				(number "A13")
			)
			(pin bidirectional line
				(at 40.64 71.12 180)
				(length 5.08)
				(name "IO2_A14")
				(number "A14")
			)
			(pin bidirectional line
				(at 40.64 68.58 180)
				(length 5.08)
				(name "IO2_A15")
				(number "A15")
			)
			(pin bidirectional line
				(at 40.64 66.04 180)
				(length 5.08)
				(name "IO2_A16")
				(number "A16")
			)
			(pin bidirectional line
				(at 40.64 63.5 180)
				(length 5.08)
				(name "IO2_A17")
				(number "A17")
			)
			(pin bidirectional line
				(at 40.64 60.96 180)
				(length 5.08)
				(name "IO2_A18")
				(number "A18")
			)
			(pin bidirectional line
				(at 40.64 58.42 180)
				(length 5.08)
				(name "IO2_A19")
				(number "A19")
			)
			(pin bidirectional line
				(at 40.64 55.88 180)
				(length 5.08)
				(name "IO2_A20")
				(number "A20")
			)
			(pin bidirectional line
				(at 40.64 53.34 180)
				(length 5.08)
				(name "IO2_B2")
				(number "B2")
			)
			(pin bidirectional line
				(at 40.64 50.8 180)
				(length 5.08)
				(name "IO2_B3")
				(number "B3")
			)
			(pin bidirectional line
				(at 40.64 48.26 180)
				(length 5.08)
				(name "IO2_B4")
				(number "B4")
			)
			(pin bidirectional line
				(at 40.64 45.72 180)
				(length 5.08)
				(name "IO2_B5")
				(number "B5")
			)
			(pin bidirectional line
				(at 40.64 43.18 180)
				(length 5.08)
				(name "IO2_B6")
				(number "B6")
			)
			(pin bidirectional line
				(at 40.64 40.64 180)
				(length 5.08)
				(name "IO2_B7")
				(number "B7")
			)
			(pin bidirectional line
				(at 40.64 38.1 180)
				(length 5.08)
				(name "IO2_B8")
				(number "B8")
			)
			(pin bidirectional line
				(at 40.64 35.56 180)
				(length 5.08)
				(name "IO2_B9")
				(number "B9")
			)
			(pin bidirectional line
				(at 40.64 33.02 180)
				(length 5.08)
				(name "IO2_B12")
				(number "B12")
			)
			(pin bidirectional line
				(at 40.64 30.48 180)
				(length 5.08)
				(name "IO2_B13")
				(number "B13")
			)
			(pin bidirectional line
				(at 40.64 27.94 180)
				(length 5.08)
				(name "IO2_B14")
				(number "B14")
			)
			(pin bidirectional line
				(at 40.64 25.4 180)
				(length 5.08)
				(name "IO2_B15")
				(number "B15")
			)
			(pin bidirectional line
				(at 40.64 22.86 180)
				(length 5.08)
				(name "IO2_B16")
				(number "B16")
			)
			(pin bidirectional line
				(at 40.64 20.32 180)
				(length 5.08)
				(name "IO2_B17")
				(number "B17")
			)
			(pin bidirectional line
				(at 40.64 17.78 180)
				(length 5.08)
				(name "IO2_B18")
				(number "B18")
			)
			(pin bidirectional line
				(at 40.64 15.24 180)
				(length 5.08)
				(name "IO2_B19")
				(number "B19")
			)
			(pin bidirectional line
				(at 40.64 12.7 180)
				(length 5.08)
				(name "IO2_B20")
				(number "B20")
			)
			(pin bidirectional line
				(at 40.64 10.16 180)
				(length 5.08)
				(name "IO2_C5")
				(number "C5")
			)
			(pin bidirectional line
				(at 40.64 7.62 180)
				(length 5.08)
				(name "IO2_C15")
				(number "C15")
			)
			(pin bidirectional line
				(at 40.64 5.08 180)
				(length 5.08)
				(name "IO2_C16")
				(number "C16")
			)
			(pin bidirectional line
				(at 40.64 2.54 180)
				(length 5.08)
				(name "IO2_C17")
				(number "C17")
			)
			(pin bidirectional line
				(at 40.64 0 180)
				(length 5.08)
				(name "IO2_C18")
				(number "C18")
			)
			(pin bidirectional line
				(at 40.64 -2.54 180)
				(length 5.08)
				(name "IO2_C19")
				(number "C19")
			)
			(pin bidirectional line
				(at 40.64 -5.08 180)
				(length 5.08)
				(name "IO2_C20")
				(number "C20")
			)
			(pin bidirectional line
				(at 40.64 -7.62 180)
				(length 5.08)
				(name "IO2_D18")
				(number "D18")
			)
			(pin bidirectional line
				(at 40.64 -10.16 180)
				(length 5.08)
				(name "IO2_D19")
				(number "D19")
			)
			(pin bidirectional line
				(at 40.64 -12.7 180)
				(length 5.08)
				(name "IO2_D20")
				(number "D20")
			)
			(pin bidirectional line
				(at 40.64 -15.24 180)
				(length 5.08)
				(name "IO2_E17")
				(number "E17")
			)
			(pin bidirectional line
				(at 40.64 -17.78 180)
				(length 5.08)
				(name "IO2_E18")
				(number "E18")
			)
			(pin bidirectional line
				(at 40.64 -20.32 180)
				(length 5.08)
				(name "IO2_E19")
				(number "E19")
			)
			(pin bidirectional line
				(at 40.64 -22.86 180)
				(length 5.08)
				(name "IO2_E20")
				(number "E20")
			)
			(pin bidirectional line
				(at 40.64 -25.4 180)
				(length 5.08)
				(name "IO2_F19")
				(number "F19")
			)
			(pin bidirectional line
				(at 40.64 -27.94 180)
				(length 5.08)
				(name "IO2_F20")
				(number "F20")
			)
			(pin bidirectional line
				(at 40.64 -30.48 180)
				(length 5.08)
				(name "IO2_G19")
				(number "G19")
			)
			(pin bidirectional line
				(at 40.64 -33.02 180)
				(length 5.08)
				(name "IO2_G20")
				(number "G20")
			)
			(pin bidirectional line
				(at 40.64 -35.56 180)
				(length 5.08)
				(name "IO2_H19")
				(number "H19")
			)
			(pin bidirectional line
				(at 40.64 -38.1 180)
				(length 5.08)
				(name "IO2_H20")
				(number "H20")
			)
			(pin bidirectional line
				(at 40.64 -40.64 180)
				(length 5.08)
				(name "IO2_J19")
				(number "J19")
			)
			(pin bidirectional line
				(at 40.64 -43.18 180)
				(length 5.08)
				(name "IO2_J20")
				(number "J20")
			)
			(pin bidirectional line
				(at 40.64 -45.72 180)
				(length 5.08)
				(name "IO2_K20")
				(number "K20")
			)
			(pin bidirectional clock
				(at 40.64 -48.26 180)
				(length 5.08)
				(name "IO2_L20/GCLK3")
				(number "L20")
			)
			(pin bidirectional line
				(at 40.64 -50.8 180)
				(length 5.08)
				(name "IO2_M19")
				(number "M19")
			)
			(pin bidirectional clock
				(at 40.64 -53.34 180)
				(length 5.08)
				(name "IO2_M20/GCLK2")
				(number "M20")
			)
			(pin bidirectional line
				(at 40.64 -55.88 180)
				(length 5.08)
				(name "IO2_N19")
				(number "N19")
			)
			(pin bidirectional line
				(at 40.64 -58.42 180)
				(length 5.08)
				(name "IO2_N20")
				(number "N20")
			)
			(pin bidirectional line
				(at 40.64 -60.96 180)
				(length 5.08)
				(name "IO2_P19")
				(number "P19")
			)
			(pin bidirectional line
				(at 40.64 -63.5 180)
				(length 5.08)
				(name "IO2_P20")
				(number "P20")
			)
			(pin bidirectional line
				(at 40.64 -66.04 180)
				(length 5.08)
				(name "IO2_R18")
				(number "R18")
			)
			(pin bidirectional line
				(at 40.64 -68.58 180)
				(length 5.08)
				(name "IO2_R19")
				(number "R19")
			)
			(pin bidirectional line
				(at 40.64 -71.12 180)
				(length 5.08)
				(name "IO2_R20")
				(number "R20")
			)
			(pin bidirectional line
				(at 40.64 -73.66 180)
				(length 5.08)
				(name "IO2_T18")
				(number "T18")
			)
			(pin bidirectional line
				(at 40.64 -76.2 180)
				(length 5.08)
				(name "IO2_T19")
				(number "T19")
			)
			(pin bidirectional line
				(at 40.64 -78.74 180)
				(length 5.08)
				(name "IO2_T20")
				(number "T20")
			)
			(pin bidirectional line
				(at 40.64 -81.28 180)
				(length 5.08)
				(name "IO2_U17")
				(number "U17")
			)
			(pin bidirectional line
				(at 40.64 -83.82 180)
				(length 5.08)
				(name "IO2_U18")
				(number "U18")
			)
			(pin bidirectional line
				(at 40.64 -86.36 180)
				(length 5.08)
				(name "IO2_U19")
				(number "U19")
			)
			(pin bidirectional line
				(at 40.64 -88.9 180)
				(length 5.08)
				(name "IO2_U20")
				(number "U20")
			)
			(pin bidirectional line
				(at 40.64 -91.44 180)
				(length 5.08)
				(name "IO2_V19")
				(number "V19")
			)
			(pin bidirectional line
				(at 40.64 -93.98 180)
				(length 5.08)
				(name "IO2_V20")
				(number "V20")
			)
			(pin bidirectional line
				(at 40.64 -96.52 180)
				(length 5.08)
				(name "IO2_W19")
				(number "W19")
			)
			(pin bidirectional line
				(at 40.64 -99.06 180)
				(length 5.08)
				(name "IO2_W20")
				(number "W20")
			)
			(pin bidirectional line
				(at 40.64 -101.6 180)
				(length 5.08)
				(name "IO2_Y20")
				(number "Y20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EPM570T100"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 12.7 54.61 0)
		)
		(property "Value" "EPM570T100"
			(at 12.7 -54.61 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at 12.7 -57.15 0)
		)
		(property "Datasheet" "https://www.altera.com/content/dam/altera-www/global/en_US/pdfs/literature/hb/max2/max2_mii5v1.pdf"
			(at 0 0 0)
		)
		(property "Description" "Altera MAX2 CPLD with 570 LE"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "MAX2 TQFP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "EPM570T100_1_1"
			(pin bidirectional line
				(at -27.94 50.8 0)
				(length 5.08)
				(name "IO1_2")
				(number "2")
			)
			(pin bidirectional line
				(at -27.94 48.26 0)
				(length 5.08)
				(name "IO1_3")
				(number "3")
			)
			(pin bidirectional line
				(at -27.94 45.72 0)
				(length 5.08)
				(name "IO1_4")
				(number "4")
			)
			(pin bidirectional line
				(at -27.94 43.18 0)
				(length 5.08)
				(name "IO1_5")
				(number "5")
			)
			(pin bidirectional line
				(at -27.94 40.64 0)
				(length 5.08)
				(name "IO1_6")
				(number "6")
			)
			(pin bidirectional line
				(at -27.94 38.1 0)
				(length 5.08)
				(name "IO1_7")
				(number "7")
			)
			(pin bidirectional line
				(at -27.94 35.56 0)
				(length 5.08)
				(name "IO1_8")
				(number "8")
			)
			(pin bidirectional clock
				(at -27.94 33.02 0)
				(length 5.08)
				(name "IO1_12/GCLK0")
				(number "12")
			)
			(pin bidirectional clock
				(at -27.94 30.48 0)
				(length 5.08)
				(name "IO1_14/GCLK1")
				(number "14")
			)
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 5.08)
				(name "IO1_15")
				(number "15")
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 5.08)
				(name "IO1_16")
				(number "16")
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 5.08)
				(name "IO1_17")
				(number "17")
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 5.08)
				(name "IO1_18")
				(number "18")
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 5.08)
				(name "IO1_19")
				(number "19")
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 5.08)
				(name "IO1_20")
				(number "20")
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 5.08)
				(name "IO1_21")
				(number "21")
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 5.08)
				(name "IO1_26")
				(number "26")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 5.08)
				(name "IO1_27")
				(number "27")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 5.08)
				(name "IO1_28")
				(number "28")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 5.08)
				(name "IO1_29")
				(number "29")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 5.08)
				(name "IO1_30")
				(number "30")
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 5.08)
				(name "IO1_33")
				(number "33")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 5.08)
				(name "IO1_34")
				(number "34")
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 5.08)
				(name "IO1_35")
				(number "35")
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 5.08)
				(name "IO1_36")
				(number "36")
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 5.08)
				(name "IO1_38")
				(number "38")
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 5.08)
				(name "IO1_40")
				(number "40")
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 5.08)
				(name "IO1_41")
				(number "41")
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 5.08)
				(name "IO1_42")
				(number "42")
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 5.08)
				(name "IO1_43/DEV_OE")
				(number "43")
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 5.08)
				(name "IO1_44/DEV_CLRn")
				(number "44")
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 5.08)
				(name "IO1_47")
				(number "47")
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 5.08)
				(name "IO1_48")
				(number "48")
			)
			(pin bidirectional line
				(at -27.94 -33.02 0)
				(length 5.08)
				(name "IO1_49")
				(number "49")
			)
			(pin bidirectional line
				(at -27.94 -35.56 0)
				(length 5.08)
				(name "IO1_50")
				(number "50")
			)
			(pin bidirectional line
				(at -27.94 -38.1 0)
				(length 5.08)
				(name "IO1_51")
				(number "51")
			)
			(pin input line
				(at -27.94 -40.64 0)
				(length 5.08)
				(name "TMS")
				(number "22")
			)
			(pin input line
				(at -27.94 -43.18 0)
				(length 5.08)
				(name "TDI")
				(number "23")
			)
			(pin input clock
				(at -27.94 -45.72 0)
				(length 5.08)
				(name "TCK")
				(number "24")
			)
			(pin output line
				(at -27.94 -48.26 0)
				(length 5.08)
				(name "TDO")
				(number "25")
			)
			(pin power_in line
				(at -12.7 58.42 270)
				(length 5.08)
				(name "VCCINT")
				(number "13")
			)
			(pin power_in line
				(at -12.7 -58.42 90)
				(length 5.08)
				(name "GNDINT")
				(number "11")
			)
			(pin power_in line
				(at -10.16 58.42 270)
				(length 5.08)
				(name "VCCINT")
				(number "39")
			)
			(pin power_in line
				(at -10.16 -58.42 90)
				(length 5.08)
				(name "GNDINT")
				(number "37")
			)
			(pin power_in line
				(at -7.62 58.42 270)
				(length 5.08)
				(name "VCCINT")
				(number "63")
			)
			(pin power_in line
				(at -7.62 -58.42 90)
				(length 5.08)
				(name "GNDINT")
				(number "65")
			)
			(pin power_in line
				(at -5.08 58.42 270)
				(length 5.08)
				(name "VCCINT")
				(number "88")
			)
			(pin power_in line
				(at -5.08 -58.42 90)
				(length 5.08)
				(name "GNDINT")
				(number "90")
			)
			(pin power_in line
				(at -2.54 58.42 270)
				(length 5.08)
				(name "VCCIO1")
				(number "9")
			)
			(pin power_in line
				(at -2.54 -58.42 90)
				(length 5.08)
				(name "GNDIO")
				(number "10")
			)
			(pin power_in line
				(at 0 58.42 270)
				(length 5.08)
				(name "VCCIO1")
				(number "31")
			)
			(pin power_in line
				(at 0 -58.42 90)
				(length 5.08)
				(name "GNDIO")
				(number "32")
			)
			(pin power_in line
				(at 2.54 58.42 270)
				(length 5.08)
				(name "VCCIO1")
				(number "45")
			)
			(pin power_in line
				(at 2.54 -58.42 90)
				(length 5.08)
				(name "GNDIO")
				(number "46")
			)
			(pin power_in line
				(at 5.08 58.42 270)
				(length 5.08)
				(name "VCCIO2")
				(number "59")
			)
			(pin power_in line
				(at 5.08 -58.42 90)
				(length 5.08)
				(name "GNDIO")
				(number "60")
			)
			(pin power_in line
				(at 7.62 58.42 270)
				(length 5.08)
				(name "VCCIO2")
				(number "80")
			)
			(pin power_in line
				(at 7.62 -58.42 90)
				(length 5.08)
				(name "GNDIO")
				(number "79")
			)
			(pin power_in line
				(at 10.16 58.42 270)
				(length 5.08)
				(name "VCCIO2")
				(number "94")
			)
			(pin power_in line
				(at 10.16 -58.42 90)
				(length 5.08)
				(name "GNDIO")
				(number "93")
			)
			(pin bidirectional line
				(at 27.94 50.8 180)
				(length 5.08)
				(name "IO2_1")
				(number "1")
			)
			(pin bidirectional line
				(at 27.94 48.26 180)
				(length 5.08)
				(name "IO2_52")
				(number "52")
			)
			(pin bidirectional line
				(at 27.94 45.72 180)
				(length 5.08)
				(name "IO2_53")
				(number "53")
			)
			(pin bidirectional line
				(at 27.94 43.18 180)
				(length 5.08)
				(name "IO2_54")
				(number "54")
			)
			(pin bidirectional line
				(at 27.94 40.64 180)
				(length 5.08)
				(name "IO2_55")
				(number "55")
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 5.08)
				(name "IO2_56")
				(number "56")
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 5.08)
				(name "IO2_57")
				(number "57")
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 5.08)
				(name "IO2_58")
				(number "58")
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 5.08)
				(name "IO2_61")
				(number "61")
			)
			(pin bidirectional clock
				(at 27.94 27.94 180)
				(length 5.08)
				(name "IO2_62/GCLK2")
				(number "62")
			)
			(pin bidirectional clock
				(at 27.94 25.4 180)
				(length 5.08)
				(name "IO2_64/GCLK3")
				(number "64")
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 5.08)
				(name "IO2_66")
				(number "66")
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 5.08)
				(name "IO2_67")
				(number "67")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 5.08)
				(name "IO2_68")
				(number "68")
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 5.08)
				(name "IO2_69")
				(number "69")
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 5.08)
				(name "IO2_70")
				(number "70")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 5.08)
				(name "IO2_71")
				(number "71")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 5.08)
				(name "IO2_72")
				(number "72")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 5.08)
				(name "IO2_73")
				(number "73")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 5.08)
				(name "IO2_74")
				(number "74")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 5.08)
				(name "IO2_75")
				(number "75")
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 5.08)
				(name "IO2_76")
				(number "76")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 5.08)
				(name "IO2_77")
				(number "77")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 5.08)
				(name "IO2_78")
				(number "78")
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 5.08)
				(name "IO2_81")
				(number "81")
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 5.08)
				(name "IO2_82")
				(number "82")
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 5.08)
				(name "IO2_83")
				(number "83")
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 5.08)
				(name "IO2_84")
				(number "84")
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 5.08)
				(name "IO2_85")
				(number "85")
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 5.08)
				(name "IO2_86")
				(number "86")
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 5.08)
				(name "IO2_87")
				(number "87")
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 5.08)
				(name "IO2_89")
				(number "89")
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 5.08)
				(name "IO2_91")
				(number "91")
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 5.08)
				(name "IO2_92")
				(number "92")
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 5.08)
				(name "IO2_95")
				(number "95")
			)
			(pin bidirectional line
				(at 27.94 -38.1 180)
				(length 5.08)
				(name "IO2_96")
				(number "96")
			)
			(pin bidirectional line
				(at 27.94 -40.64 180)
				(length 5.08)
				(name "IO2_97")
				(number "97")
			)
			(pin bidirectional line
				(at 27.94 -43.18 180)
				(length 5.08)
				(name "IO2_98")
				(number "98")
			)
			(pin bidirectional line
				(at 27.94 -45.72 180)
				(length 5.08)
				(name "IO2_99")
				(number "99")
			)
			(pin bidirectional line
				(at 27.94 -48.26 180)
				(length 5.08)
				(name "IO2_100")
				(number "100")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EPM570T144"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 15.24 80.01 0)
		)
		(property "Value" "EPM570T144"
			(at 15.24 -80.01 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at 15.24 -82.55 0)
		)
		(property "Datasheet" "https://www.altera.com/content/dam/altera-www/global/en_US/pdfs/literature/hb/max2/max2_mii5v1.pdf"
			(at 0 0 0)
		)
		(property "Description" "Altera MAX2 CPLD with 570 LE"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "MAX2 TQFP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "EPM570T144_1_1"
			(pin bidirectional line
				(at -30.48 76.2 0)
				(length 5.08)
				(name "IO1_1")
				(number "1")
			)
			(pin bidirectional line
				(at -30.48 73.66 0)
				(length 5.08)
				(name "IO1_2")
				(number "2")
			)
			(pin bidirectional line
				(at -30.48 71.12 0)
				(length 5.08)
				(name "IO1_3")
				(number "3")
			)
			(pin bidirectional line
				(at -30.48 68.58 0)
				(length 5.08)
				(name "IO1_4")
				(number "4")
			)
			(pin bidirectional line
				(at -30.48 66.04 0)
				(length 5.08)
				(name "IO1_5")
				(number "5")
			)
			(pin bidirectional line
				(at -30.48 63.5 0)
				(length 5.08)
				(name "IO1_6")
				(number "6")
			)
			(pin bidirectional line
				(at -30.48 60.96 0)
				(length 5.08)
				(name "IO1_7")
				(number "7")
			)
			(pin bidirectional line
				(at -30.48 58.42 0)
				(length 5.08)
				(name "IO1_8")
				(number "8")
			)
			(pin bidirectional line
				(at -30.48 55.88 0)
				(length 5.08)
				(name "IO1_11")
				(number "11")
			)
			(pin bidirectional line
				(at -30.48 53.34 0)
				(length 5.08)
				(name "IO1_12")
				(number "12")
			)
			(pin bidirectional line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "IO1_13")
				(number "13")
			)
			(pin bidirectional line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "IO1_14")
				(number "14")
			)
			(pin bidirectional line
				(at -30.48 45.72 0)
				(length 5.08)
				(name "IO1_15")
				(number "15")
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "IO1_16")
				(number "16")
			)
			(pin bidirectional clock
				(at -30.48 40.64 0)
				(length 5.08)
				(name "IO1_18/GCLK0")
				(number "18")
			)
			(pin bidirectional clock
				(at -30.48 38.1 0)
				(length 5.08)
				(name "IO1_20/GCLK1")
				(number "20")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "IO1_21")
				(number "21")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "IO1_22")
				(number "22")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "IO1_23")
				(number "23")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "IO1_24")
				(number "24")
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "IO1_27")
				(number "27")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "IO1_28")
				(number "28")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "IO1_29")
				(number "29")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "IO1_30")
				(number "30")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "IO1_31")
				(number "31")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "IO1_32")
				(number "32")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "IO1_37")
				(number "37")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "IO1_38")
				(number "38")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "IO1_39")
				(number "39")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "IO1_40")
				(number "40")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "IO1_41")
				(number "41")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "IO1_42")
				(number "42")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "IO1_43")
				(number "43")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "IO1_44")
				(number "44")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "IO1_45")
				(number "45")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "IO1_48")
				(number "48")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "IO1_49")
				(number "49")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "IO1_50")
				(number "50")
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "IO1_51")
				(number "51")
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "IO1_52")
				(number "52")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "IO1_53")
				(number "53")
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 5.08)
				(name "IO1_55")
				(number "55")
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "IO1_57")
				(number "57")
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "IO1_58")
				(number "58")
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "IO1_59")
				(number "59")
			)
			(pin bidirectional line
				(at -30.48 -38.1 0)
				(length 5.08)
				(name "IO1_60/DEV_OE")
				(number "60")
			)
			(pin bidirectional line
				(at -30.48 -40.64 0)
				(length 5.08)
				(name "IO1_61/DEV_CLRn")
				(number "61")
			)
			(pin bidirectional line
				(at -30.48 -43.18 0)
				(length 5.08)
				(name "IO1_62")
				(number "62")
			)
			(pin bidirectional line
				(at -30.48 -45.72 0)
				(length 5.08)
				(name "IO1_63")
				(number "63")
			)
			(pin bidirectional line
				(at -30.48 -48.26 0)
				(length 5.08)
				(name "IO1_66")
				(number "66")
			)
			(pin bidirectional line
				(at -30.48 -50.8 0)
				(length 5.08)
				(name "IO1_67")
				(number "67")
			)
			(pin bidirectional line
				(at -30.48 -53.34 0)
				(length 5.08)
				(name "IO1_68")
				(number "68")
			)
			(pin bidirectional line
				(at -30.48 -55.88 0)
				(length 5.08)
				(name "IO1_69")
				(number "69")
			)
			(pin bidirectional line
				(at -30.48 -58.42 0)
				(length 5.08)
				(name "IO1_70")
				(number "70")
			)
			(pin bidirectional line
				(at -30.48 -60.96 0)
				(length 5.08)
				(name "IO1_71")
				(number "71")
			)
			(pin bidirectional line
				(at -30.48 -63.5 0)
				(length 5.08)
				(name "IO1_72")
				(number "72")
			)
			(pin input line
				(at -30.48 -66.04 0)
				(length 5.08)
				(name "TMS")
				(number "33")
			)
			(pin input line
				(at -30.48 -68.58 0)
				(length 5.08)
				(name "TDI")
				(number "34")
			)
			(pin input clock
				(at -30.48 -71.12 0)
				(length 5.08)
				(name "TCK")
				(number "35")
			)
			(pin output line
				(at -30.48 -73.66 0)
				(length 5.08)
				(name "TDO")
				(number "36")
			)
			(pin power_in line
				(at -15.24 83.82 270)
				(length 5.08)
				(name "VCCINT")
				(number "19")
			)
			(pin power_in line
				(at -15.24 -83.82 90)
				(length 5.08)
				(name "GNDINT")
				(number "17")
			)
			(pin power_in line
				(at -12.7 83.82 270)
				(length 5.08)
				(name "VCCINT")
				(number "56")
			)
			(pin power_in line
				(at -12.7 -83.82 90)
				(length 5.08)
				(name "GNDINT")
				(number "54")
			)
			(pin power_in line
				(at -10.16 83.82 270)
				(length 5.08)
				(name "VCCINT")
				(number "90")
			)
			(pin power_in line
				(at -10.16 -83.82 90)
				(length 5.08)
				(name "GNDINT")
				(number "92")
			)
			(pin power_in line
				(at -7.62 83.82 270)
				(length 5.08)
				(name "VCCINT")
				(number "126")
			)
			(pin power_in line
				(at -7.62 -83.82 90)
				(length 5.08)
				(name "GNDINT")
				(number "128")
			)
			(pin power_in line
				(at -5.08 83.82 270)
				(length 5.08)
				(name "VCCIO1")
				(number "9")
			)
			(pin power_in line
				(at -5.08 -83.82 90)
				(length 5.08)
				(name "GNDIO")
				(number "10")
			)
			(pin power_in line
				(at -2.54 83.82 270)
				(length 5.08)
				(name "VCCIO1")
				(number "25")
			)
			(pin power_in line
				(at -2.54 -83.82 90)
				(length 5.08)
				(name "GNDIO")
				(number "26")
			)
			(pin power_in line
				(at 0 83.82 270)
				(length 5.08)
				(name "VCCIO1")
				(number "46")
			)
			(pin power_in line
				(at 0 -83.82 90)
				(length 5.08)
				(name "GNDIO")
				(number "47")
			)
			(pin power_in line
				(at 2.54 83.82 270)
				(length 5.08)
				(name "VCCIO1")
				(number "64")
			)
			(pin power_in line
				(at 2.54 -83.82 90)
				(length 5.08)
				(name "GNDIO")
				(number "65")
			)
			(pin power_in line
				(at 5.08 83.82 270)
				(length 5.08)
				(name "VCCIO2")
				(number "82")
			)
			(pin power_in line
				(at 5.08 -83.82 90)
				(length 5.08)
				(name "GNDIO")
				(number "83")
			)
			(pin power_in line
				(at 7.62 83.82 270)
				(length 5.08)
				(name "VCCIO2")
				(number "100")
			)
			(pin power_in line
				(at 7.62 -83.82 90)
				(length 5.08)
				(name "GNDIO")
				(number "99")
			)
			(pin power_in line
				(at 10.16 83.82 270)
				(length 5.08)
				(name "VCCIO2")
				(number "116")
			)
			(pin power_in line
				(at 10.16 -83.82 90)
				(length 5.08)
				(name "GNDIO")
				(number "115")
			)
			(pin power_in line
				(at 12.7 83.82 270)
				(length 5.08)
				(name "VCCIO2")
				(number "136")
			)
			(pin power_in line
				(at 12.7 -83.82 90)
				(length 5.08)
				(name "GNDIO")
				(number "135")
			)
			(pin bidirectional line
				(at 30.48 76.2 180)
				(length 5.08)
				(name "IO2_73")
				(number "73")
			)
			(pin bidirectional line
				(at 30.48 73.66 180)
				(length 5.08)
				(name "IO2_74")
				(number "74")
			)
			(pin bidirectional line
				(at 30.48 71.12 180)
				(length 5.08)
				(name "IO2_75")
				(number "75")
			)
			(pin bidirectional line
				(at 30.48 68.58 180)
				(length 5.08)
				(name "IO2_76")
				(number "76")
			)
			(pin bidirectional line
				(at 30.48 66.04 180)
				(length 5.08)
				(name "IO2_77")
				(number "77")
			)
			(pin bidirectional line
				(at 30.48 63.5 180)
				(length 5.08)
				(name "IO2_78")
				(number "78")
			)
			(pin bidirectional line
				(at 30.48 60.96 180)
				(length 5.08)
				(name "IO2_79")
				(number "79")
			)
			(pin bidirectional line
				(at 30.48 58.42 180)
				(length 5.08)
				(name "IO2_80")
				(number "80")
			)
			(pin bidirectional line
				(at 30.48 55.88 180)
				(length 5.08)
				(name "IO2_81")
				(number "81")
			)
			(pin bidirectional line
				(at 30.48 53.34 180)
				(length 5.08)
				(name "IO2_84")
				(number "84")
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 5.08)
				(name "IO2_85")
				(number "85")
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "IO2_86")
				(number "86")
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "IO2_87")
				(number "87")
			)
			(pin bidirectional line
				(at 30.48 43.18 180)
				(length 5.08)
				(name "IO2_88")
				(number "88")
			)
			(pin bidirectional clock
				(at 30.48 40.64 180)
				(length 5.08)
				(name "IO2_89/GCLK2")
				(number "89")
			)
			(pin bidirectional clock
				(at 30.48 38.1 180)
				(length 5.08)
				(name "IO2_91/GCLK3")
				(number "91")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "IO2_93")
				(number "93")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "IO2_94")
				(number "94")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "IO2_95")
				(number "95")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "IO2_96")
				(number "96")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "IO2_97")
				(number "97")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "IO2_98")
				(number "98")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "IO2_101")
				(number "101")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "IO2_102")
				(number "102")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "IO2_103")
				(number "103")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "IO2_104")
				(number "104")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "IO2_105")
				(number "105")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "IO2_106")
				(number "106")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "IO2_107")
				(number "107")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "IO2_108")
				(number "108")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "IO2_109")
				(number "109")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "IO2_110")
				(number "110")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "IO2_111")
				(number "111")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "IO2_112")
				(number "112")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "IO2_113")
				(number "113")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "IO2_114")
				(number "114")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "IO2_117")
				(number "117")
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "IO2_118")
				(number "118")
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 5.08)
				(name "IO2_119")
				(number "119")
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "IO2_120")
				(number "120")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "IO2_121")
				(number "121")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "IO2_122")
				(number "122")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "IO2_123")
				(number "123")
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "IO2_124")
				(number "124")
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "IO2_125")
				(number "125")
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "IO2_127")
				(number "127")
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "IO2_129")
				(number "129")
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 5.08)
				(name "IO2_130")
				(number "130")
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "IO2_131")
				(number "131")
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "IO2_132")
				(number "132")
			)
			(pin bidirectional line
				(at 30.48 -50.8 180)
				(length 5.08)
				(name "IO2_133")
				(number "133")
			)
			(pin bidirectional line
				(at 30.48 -53.34 180)
				(length 5.08)
				(name "IO2_134")
				(number "134")
			)
			(pin bidirectional line
				(at 30.48 -55.88 180)
				(length 5.08)
				(name "IO2_137")
				(number "137")
			)
			(pin bidirectional line
				(at 30.48 -58.42 180)
				(length 5.08)
				(name "IO2_138")
				(number "138")
			)
			(pin bidirectional line
				(at 30.48 -60.96 180)
				(length 5.08)
				(name "IO2_139")
				(number "139")
			)
			(pin bidirectional line
				(at 30.48 -63.5 180)
				(length 5.08)
				(name "IO2_140")
				(number "140")
			)
			(pin bidirectional line
				(at 30.48 -66.04 180)
				(length 5.08)
				(name "IO2_141")
				(number "141")
			)
			(pin bidirectional line
				(at 30.48 -68.58 180)
				(length 5.08)
				(name "IO2_142")
				(number "142")
			)
			(pin bidirectional line
				(at 30.48 -71.12 180)
				(length 5.08)
				(name "IO2_143")
				(number "143")
			)
			(pin bidirectional line
				(at 30.48 -73.66 180)
				(length 5.08)
				(name "IO2_144")
				(number "144")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EPM570ZM100"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 12.7 54.61 0)
		)
		(property "Value" "EPM570ZM100"
			(at 12.7 -54.61 0)
		)
		(property "Footprint" "Package_BGA:BGA-100_6.0x6.0mm_Layout11x11_P0.5mm_Ball0.3mm_Pad0.25mm_NSMD"
			(at 12.7 -57.15 0)
		)
		(property "Datasheet" "https://www.altera.com/content/dam/altera-www/global/en_US/pdfs/literature/hb/max2/max2_mii5v1.pdf"
			(at 0 0 0)
		)
		(property "Description" "Altera Zero-Power MAX2 CPLD with 570 LE"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "MAX2 MBGA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*BGA*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "EPM570ZM100_1_1"
			(pin bidirectional line
				(at -27.94 50.8 0)
				(length 5.08)
				(name "IO1_B1")
				(number "B1")
			)
			(pin bidirectional line
				(at -27.94 48.26 0)
				(length 5.08)
				(name "IO1_C1")
				(number "C1")
			)
			(pin bidirectional line
				(at -27.94 45.72 0)
				(length 5.08)
				(name "IO1_C2")
				(number "C2")
			)
			(pin bidirectional line
				(at -27.94 43.18 0)
				(length 5.08)
				(name "IO1_D1")
				(number "D1")
			)
			(pin bidirectional line
				(at -27.94 40.64 0)
				(length 5.08)
				(name "IO1_D2")
				(number "D2")
			)
			(pin bidirectional line
				(at -27.94 38.1 0)
				(length 5.08)
				(name "IO1_D3")
				(number "D3")
			)
			(pin bidirectional clock
				(at -27.94 35.56 0)
				(length 5.08)
				(name "IO1_E1/GCLK1")
				(number "E1")
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 5.08)
				(name "IO1_E2")
				(number "E2")
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 5.08)
				(name "IO1_F1")
				(number "F1")
			)
			(pin bidirectional clock
				(at -27.94 27.94 0)
				(length 5.08)
				(name "IO1_F2/GCLK0")
				(number "F2")
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 5.08)
				(name "IO1_F3")
				(number "F3")
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 5.08)
				(name "IO1_G1")
				(number "G1")
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 5.08)
				(name "IO1_G2")
				(number "G2")
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 5.08)
				(name "IO1_H1")
				(number "H1")
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 5.08)
				(name "IO1_H2")
				(number "H2")
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 5.08)
				(name "IO1_H3")
				(number "H3")
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 5.08)
				(name "IO1_J6")
				(number "J6")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 5.08)
				(name "IO1_K3")
				(number "K3")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 5.08)
				(name "IO1_K4")
				(number "K4")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 5.08)
				(name "IO1_K5")
				(number "K5")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 5.08)
				(name "IO1_K6")
				(number "K6")
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 5.08)
				(name "IO1_K7")
				(number "K7")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 5.08)
				(name "IO1_K8/DEV_CLRn")
				(number "K8")
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 5.08)
				(name "IO1_K9")
				(number "K9")
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 5.08)
				(name "IO1_K10")
				(number "K10")
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 5.08)
				(name "IO1_L1")
				(number "L1")
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 5.08)
				(name "IO1_L2")
				(number "L2")
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 5.08)
				(name "IO1_L3")
				(number "L3")
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 5.08)
				(name "IO1_L4")
				(number "L4")
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 5.08)
				(name "IO1_L5")
				(number "L5")
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 5.08)
				(name "IO1_L6")
				(number "L6")
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 5.08)
				(name "IO1_L7")
				(number "L7")
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 5.08)
				(name "IO1_L8/DEV_OE")
				(number "L8")
			)
			(pin bidirectional line
				(at -27.94 -33.02 0)
				(length 5.08)
				(name "IO1_L9")
				(number "L9")
			)
			(pin bidirectional line
				(at -27.94 -35.56 0)
				(length 5.08)
				(name "IO1_L10")
				(number "L10")
			)
			(pin bidirectional line
				(at -27.94 -38.1 0)
				(length 5.08)
				(name "IO1_L11")
				(number "L11")
			)
			(pin input line
				(at -27.94 -40.64 0)
				(length 5.08)
				(name "TMS")
				(number "J1")
			)
			(pin input line
				(at -27.94 -43.18 0)
				(length 5.08)
				(name "TDI")
				(number "J2")
			)
			(pin input clock
				(at -27.94 -45.72 0)
				(length 5.08)
				(name "TCK")
				(number "K1")
			)
			(pin output line
				(at -27.94 -48.26 0)
				(length 5.08)
				(name "TDO")
				(number "K2")
			)
			(pin power_in line
				(at -12.7 58.42 270)
				(length 5.08)
				(name "VCCINT")
				(number "G3")
			)
			(pin power_in line
				(at -12.7 -58.42 90)
				(length 5.08)
				(name "GND")
				(number "E4")
			)
			(pin power_in line
				(at -10.16 58.42 270)
				(length 5.08)
				(name "VCCINT")
				(number "J7")
			)
			(pin power_in line
				(at -10.16 -58.42 90)
				(length 5.08)
				(name "GND")
				(number "G4")
			)
			(pin power_in line
				(at -7.62 58.42 270)
				(length 5.08)
				(name "VCCINT")
				(number "E9")
			)
			(pin power_in line
				(at -7.62 -58.42 90)
				(length 5.08)
				(name "GND")
				(number "H5")
			)
			(pin power_in line
				(at -5.08 58.42 270)
				(length 5.08)
				(name "VCCINT")
				(number "C7")
			)
			(pin power_in line
				(at -5.08 -58.42 90)
				(length 5.08)
				(name "GND")
				(number "J5")
			)
			(pin power_in line
				(at -2.54 58.42 270)
				(length 5.08)
				(name "VCCIO1")
				(number "E3")
			)
			(pin power_in line
				(at -2.54 -58.42 90)
				(length 5.08)
				(name "GND")
				(number "H7")
			)
			(pin power_in line
				(at 0 58.42 270)
				(length 5.08)
				(name "VCCIO1")
				(number "J4")
			)
			(pin power_in line
				(at 0 -58.42 90)
				(length 5.08)
				(name "GND")
				(number "G8")
			)
			(pin power_in line
				(at 2.54 58.42 270)
				(length 5.08)
				(name "VCCIO1")
				(number "J8")
			)
			(pin power_in line
				(at 2.54 -58.42 90)
				(length 5.08)
				(name "GND")
				(number "E8")
			)
			(pin power_in line
				(at 5.08 58.42 270)
				(length 5.08)
				(name "VCCIO2")
				(number "G9")
			)
			(pin power_in line
				(at 5.08 -58.42 90)
				(length 5.08)
				(name "GND")
				(number "D7")
			)
			(pin power_in line
				(at 7.62 58.42 270)
				(length 5.08)
				(name "VCCIO2")
				(number "C8")
			)
			(pin power_in line
				(at 7.62 -58.42 90)
				(length 5.08)
				(name "GND")
				(number "C5")
			)
			(pin power_in line
				(at 10.16 58.42 270)
				(length 5.08)
				(name "VCCIO2")
				(number "C4")
			)
			(pin power_in line
				(at 10.16 -58.42 90)
				(length 5.08)
				(name "GND")
				(number "D5")
			)
			(pin bidirectional line
				(at 27.94 50.8 180)
				(length 5.08)
				(name "IO2_A1")
				(number "A1")
			)
			(pin bidirectional line
				(at 27.94 48.26 180)
				(length 5.08)
				(name "IO2_A2")
				(number "A2")
			)
			(pin bidirectional line
				(at 27.94 45.72 180)
				(length 5.08)
				(name "IO2_A3")
				(number "A3")
			)
			(pin bidirectional line
				(at 27.94 43.18 180)
				(length 5.08)
				(name "IO2_A4")
				(number "A4")
			)
			(pin bidirectional line
				(at 27.94 40.64 180)
				(length 5.08)
				(name "IO2_A5")
				(number "A5")
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 5.08)
				(name "IO2_A6")
				(number "A6")
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 5.08)
				(name "IO2_A7")
				(number "A7")
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 5.08)
				(name "IO2_A8")
				(number "A8")
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 5.08)
				(name "IO2_A9")
				(number "A9")
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 5.08)
				(name "IO2_A10")
				(number "A10")
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 5.08)
				(name "IO2_A11")
				(number "A11")
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 5.08)
				(name "IO2_B2")
				(number "B2")
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 5.08)
				(name "IO2_B3")
				(number "B3")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 5.08)
				(name "IO2_B4")
				(number "B4")
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 5.08)
				(name "IO2_B5")
				(number "B5")
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 5.08)
				(name "IO2_B6")
				(number "B6")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 5.08)
				(name "IO2_B7")
				(number "B7")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 5.08)
				(name "IO2_B8")
				(number "B8")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 5.08)
				(name "IO2_B9")
				(number "B9")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 5.08)
				(name "IO2_B10")
				(number "B10")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 5.08)
				(name "IO2_B11")
				(number "B11")
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 5.08)
				(name "IO2_C6")
				(number "C6")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 5.08)
				(name "IO2_C10")
				(number "C10")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 5.08)
				(name "IO2_C11")
				(number "C11")
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 5.08)
				(name "IO2_D9")
				(number "D9")
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 5.08)
				(name "IO2_D10")
				(number "D10")
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 5.08)
				(name "IO2_D11")
				(number "D11")
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 5.08)
				(name "IO2_E10")
				(number "E10")
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 5.08)
				(name "IO2_E11")
				(number "E11")
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 5.08)
				(name "IO2_F9")
				(number "F9")
			)
			(pin bidirectional clock
				(at 27.94 -25.4 180)
				(length 5.08)
				(name "IO2_F10/GCLK2")
				(number "F10")
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 5.08)
				(name "IO2_F11")
				(number "F11")
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 5.08)
				(name "IO2_G10")
				(number "G10")
			)
			(pin bidirectional clock
				(at 27.94 -33.02 180)
				(length 5.08)
				(name "IO2_G11/GCLK3")
				(number "G11")
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 5.08)
				(name "IO2_H9")
				(number "H9")
			)
			(pin bidirectional line
				(at 27.94 -38.1 180)
				(length 5.08)
				(name "IO2_H10")
				(number "H10")
			)
			(pin bidirectional line
				(at 27.94 -40.64 180)
				(length 5.08)
				(name "IO2_H11")
				(number "H11")
			)
			(pin bidirectional line
				(at 27.94 -43.18 180)
				(length 5.08)
				(name "IO2_J10")
				(number "J10")
			)
			(pin bidirectional line
				(at 27.94 -45.72 180)
				(length 5.08)
				(name "IO2_J11")
				(number "J11")
			)
			(pin bidirectional line
				(at 27.94 -48.26 180)
				(length 5.08)
				(name "IO2_K11")
				(number "K11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EPM570ZM144"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 15.24 80.01 0)
		)
		(property "Value" "EPM570ZM144"
			(at 15.24 -80.01 0)
		)
		(property "Footprint" "Package_BGA:BGA-144_7.0x7.0mm_Layout13x13_P0.5mm_Ball0.3mm_Pad0.25mm_NSMD"
			(at 15.24 -82.55 0)
		)
		(property "Datasheet" "https://www.altera.com/content/dam/altera-www/global/en_US/pdfs/literature/hb/max2/max2_mii5v1.pdf"
			(at 0 0 0)
		)
		(property "Description" "Altera Zero-Power MAX2 CPLD with 570 LE"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "MAX2 MBGA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*BGA*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "EPM570ZM144_1_1"
			(pin bidirectional line
				(at -30.48 76.2 0)
				(length 5.08)
				(name "IO1_A4")
				(number "A4")
			)
			(pin bidirectional line
				(at -30.48 73.66 0)
				(length 5.08)
				(name "IO1_A5")
				(number "A5")
			)
			(pin bidirectional line
				(at -30.48 71.12 0)
				(length 5.08)
				(name "IO1_A6")
				(number "A6")
			)
			(pin bidirectional line
				(at -30.48 68.58 0)
				(length 5.08)
				(name "IO1_A7")
				(number "A7")
			)
			(pin bidirectional clock
				(at -30.48 66.04 0)
				(length 5.08)
				(name "IO1_A8/GCLK0")
				(number "A8")
			)
			(pin bidirectional line
				(at -30.48 63.5 0)
				(length 5.08)
				(name "IO1_A9")
				(number "A9")
			)
			(pin bidirectional line
				(at -30.48 60.96 0)
				(length 5.08)
				(name "IO1_A10")
				(number "A10")
			)
			(pin bidirectional line
				(at -30.48 58.42 0)
				(length 5.08)
				(name "IO1_A11")
				(number "A11")
			)
			(pin bidirectional line
				(at -30.48 55.88 0)
				(length 5.08)
				(name "IO1_A12")
				(number "A12")
			)
			(pin bidirectional line
				(at -30.48 53.34 0)
				(length 5.08)
				(name "IO1_B1")
				(number "B1")
			)
			(pin bidirectional line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "IO1_B2")
				(number "B2")
			)
			(pin bidirectional line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "IO1_B4")
				(number "B4")
			)
			(pin bidirectional line
				(at -30.48 45.72 0)
				(length 5.08)
				(name "IO1_B5")
				(number "B5")
			)
			(pin bidirectional clock
				(at -30.48 43.18 0)
				(length 5.08)
				(name "IO1_B6/GCLK1")
				(number "B6")
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "IO1_B7")
				(number "B7")
			)
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "IO1_B8")
				(number "B8")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "IO1_B9")
				(number "B9")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "IO1_B10")
				(number "B10")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "IO1_B11")
				(number "B11")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "IO1_C1")
				(number "C1")
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "IO1_C2")
				(number "C2")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "IO1_C3")
				(number "C3")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "IO1_C4")
				(number "C4")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "IO1_C5")
				(number "C5")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "IO1_C9")
				(number "C9")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "IO1_C10")
				(number "C10")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "IO1_C11")
				(number "C11")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "IO1_D1")
				(number "D1")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "IO1_D2")
				(number "D2")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "IO1_D3")
				(number "D3")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "IO1_D4")
				(number "D4")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "IO1_D5")
				(number "D5")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "IO1_D9")
				(number "D9")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "IO1_D10")
				(number "D10")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "IO1_E1")
				(number "E1")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "IO1_E2")
				(number "E2")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "IO1_E3")
				(number "E3")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "IO1_E4")
				(number "E4")
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "IO1_F1")
				(number "F1")
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "IO1_F2")
				(number "F2")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "IO1_G1")
				(number "G1")
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 5.08)
				(name "IO1_G2")
				(number "G2")
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "IO1_H1")
				(number "H1")
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "IO1_H2")
				(number "H2")
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "IO1_J1")
				(number "J1")
			)
			(pin bidirectional line
				(at -30.48 -38.1 0)
				(length 5.08)
				(name "IO1_J2")
				(number "J2")
			)
			(pin bidirectional line
				(at -30.48 -40.64 0)
				(length 5.08)
				(name "IO1_J3")
				(number "J3")
			)
			(pin bidirectional line
				(at -30.48 -43.18 0)
				(length 5.08)
				(name "IO1_J4/DEV_OE")
				(number "J4")
			)
			(pin bidirectional line
				(at -30.48 -45.72 0)
				(length 5.08)
				(name "IO1_K1/DEV_CLRn")
				(number "K1")
			)
			(pin bidirectional line
				(at -30.48 -48.26 0)
				(length 5.08)
				(name "IO1_K2")
				(number "K2")
			)
			(pin bidirectional line
				(at -30.48 -50.8 0)
				(length 5.08)
				(name "IO1_K3")
				(number "K3")
			)
			(pin bidirectional line
				(at -30.48 -53.34 0)
				(length 5.08)
				(name "IO1_K4")
				(number "K4")
			)
			(pin bidirectional line
				(at -30.48 -55.88 0)
				(length 5.08)
				(name "IO1_L1")
				(number "L1")
			)
			(pin bidirectional line
				(at -30.48 -58.42 0)
				(length 5.08)
				(name "IO1_L2")
				(number "L2")
			)
			(pin bidirectional line
				(at -30.48 -60.96 0)
				(length 5.08)
				(name "IO1_M1")
				(number "M1")
			)
			(pin bidirectional line
				(at -30.48 -63.5 0)
				(length 5.08)
				(name "IO1_N1")
				(number "N1")
			)
			(pin input line
				(at -30.48 -66.04 0)
				(length 5.08)
				(name "TMS")
				(number "B3")
			)
			(pin input line
				(at -30.48 -68.58 0)
				(length 5.08)
				(name "TDI")
				(number "A3")
			)
			(pin input clock
				(at -30.48 -71.12 0)
				(length 5.08)
				(name "TCK")
				(number "A1")
			)
			(pin output line
				(at -30.48 -73.66 0)
				(length 5.08)
				(name "TDO")
				(number "A2")
			)
			(pin power_in line
				(at -15.24 83.82 270)
				(length 5.08)
				(name "VCCINT")
				(number "D7")
			)
			(pin power_in line
				(at -15.24 -83.82 90)
				(length 5.08)
				(name "GND")
				(number "C6")
			)
			(pin power_in line
				(at -12.7 83.82 270)
				(length 5.08)
				(name "VCCINT")
				(number "G4")
			)
			(pin power_in line
				(at -12.7 -83.82 90)
				(length 5.08)
				(name "GND")
				(number "C7")
			)
			(pin power_in line
				(at -10.16 83.82 270)
				(length 5.08)
				(name "VCCINT")
				(number "G10")
			)
			(pin power_in line
				(at -10.16 -83.82 90)
				(length 5.08)
				(name "GND")
				(number "C8")
			)
			(pin power_in line
				(at -7.62 83.82 270)
				(length 5.08)
				(name "VCCINT")
				(number "K7")
			)
			(pin power_in line
				(at -7.62 -83.82 90)
				(length 5.08)
				(name "GND")
				(number "F3")
			)
			(pin power_in line
				(at -5.08 83.82 270)
				(length 5.08)
				(name "VCCIO1")
				(number "D6")
			)
			(pin power_in line
				(at -5.08 -83.82 90)
				(length 5.08)
				(name "GND")
				(number "F11")
			)
			(pin power_in line
				(at -2.54 83.82 270)
				(length 5.08)
				(name "VCCIO1")
				(number "D8")
			)
			(pin power_in line
				(at -2.54 -83.82 90)
				(length 5.08)
				(name "GND")
				(number "G3")
			)
			(pin power_in line
				(at 0 83.82 270)
				(length 5.08)
				(name "VCCIO1")
				(number "F4")
			)
			(pin power_in line
				(at 0 -83.82 90)
				(length 5.08)
				(name "GND")
				(number "G11")
			)
			(pin power_in line
				(at 2.54 83.82 270)
				(length 5.08)
				(name "VCCIO1")
				(number "H4")
			)
			(pin power_in line
				(at 2.54 -83.82 90)
				(length 5.08)
				(name "GND")
				(number "H3")
			)
			(pin power_in line
				(at 5.08 83.82 270)
				(length 5.08)
				(name "VCCIO2")
				(number "F10")
			)
			(pin power_in line
				(at 5.08 -83.82 90)
				(length 5.08)
				(name "GND")
				(number "H11")
			)
			(pin power_in line
				(at 7.62 83.82 270)
				(length 5.08)
				(name "VCCIO2")
				(number "J10")
			)
			(pin power_in line
				(at 7.62 -83.82 90)
				(length 5.08)
				(name "GND")
				(number "L6")
			)
			(pin power_in line
				(at 10.16 83.82 270)
				(length 5.08)
				(name "VCCIO2")
				(number "K6")
			)
			(pin power_in line
				(at 10.16 -83.82 90)
				(length 5.08)
				(name "GND")
				(number "L7")
			)
			(pin power_in line
				(at 12.7 83.82 270)
				(length 5.08)
				(name "VCCIO2")
				(number "K8")
			)
			(pin power_in line
				(at 12.7 -83.82 90)
				(length 5.08)
				(name "GND")
				(number "L8")
			)
			(pin bidirectional line
				(at 30.48 76.2 180)
				(length 5.08)
				(name "IO2_A13")
				(number "A13")
			)
			(pin bidirectional line
				(at 30.48 73.66 180)
				(length 5.08)
				(name "IO2_B12")
				(number "B12")
			)
			(pin bidirectional line
				(at 30.48 71.12 180)
				(length 5.08)
				(name "IO2_B13")
				(number "B13")
			)
			(pin bidirectional line
				(at 30.48 68.58 180)
				(length 5.08)
				(name "IO2_C12")
				(number "C12")
			)
			(pin bidirectional line
				(at 30.48 66.04 180)
				(length 5.08)
				(name "IO2_C13")
				(number "C13")
			)
			(pin bidirectional line
				(at 30.48 63.5 180)
				(length 5.08)
				(name "IO2_D11")
				(number "D11")
			)
			(pin bidirectional line
				(at 30.48 60.96 180)
				(length 5.08)
				(name "IO2_D12")
				(number "D12")
			)
			(pin bidirectional line
				(at 30.48 58.42 180)
				(length 5.08)
				(name "IO2_D13")
				(number "D13")
			)
			(pin bidirectional line
				(at 30.48 55.88 180)
				(length 5.08)
				(name "IO2_E10")
				(number "E10")
			)
			(pin bidirectional line
				(at 30.48 53.34 180)
				(length 5.08)
				(name "IO2_E11")
				(number "E11")
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 5.08)
				(name "IO2_E12")
				(number "E12")
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "IO2_E13")
				(number "E13")
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "IO2_F12")
				(number "F12")
			)
			(pin bidirectional line
				(at 30.48 43.18 180)
				(length 5.08)
				(name "IO2_F13")
				(number "F13")
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "IO2_G12")
				(number "G12")
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "IO2_G13")
				(number "G13")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "IO2_H10")
				(number "H10")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "IO2_H12")
				(number "H12")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "IO2_H13")
				(number "H13")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "IO2_J11")
				(number "J11")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "IO2_J12")
				(number "J12")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "IO2_J13")
				(number "J13")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "IO2_K5")
				(number "K5")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "IO2_K9")
				(number "K9")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "IO2_K10")
				(number "K10")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "IO2_K11")
				(number "K11")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "IO2_K12")
				(number "K12")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "IO2_K13")
				(number "K13")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "IO2_L3")
				(number "L3")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "IO2_L4")
				(number "L4")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "IO2_L5")
				(number "L5")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "IO2_L9")
				(number "L9")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "IO2_L10")
				(number "L10")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "IO2_L11")
				(number "L11")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "IO2_L12")
				(number "L12")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "IO2_L13")
				(number "L13")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "IO2_M2")
				(number "M2")
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "IO2_M3")
				(number "M3")
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 5.08)
				(name "IO2_M4")
				(number "M4")
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "IO2_M5")
				(number "M5")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "IO2_M6")
				(number "M6")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "IO2_M7")
				(number "M7")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "IO2_M8")
				(number "M8")
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "IO2_M9")
				(number "M9")
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "IO2_M10")
				(number "M10")
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "IO2_M11")
				(number "M11")
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "IO2_M12")
				(number "M12")
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 5.08)
				(name "IO2_M13")
				(number "M13")
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "IO2_N2")
				(number "N2")
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "IO2_N3")
				(number "N3")
			)
			(pin bidirectional line
				(at 30.48 -50.8 180)
				(length 5.08)
				(name "IO2_N4")
				(number "N4")
			)
			(pin bidirectional line
				(at 30.48 -53.34 180)
				(length 5.08)
				(name "IO2_N5")
				(number "N5")
			)
			(pin bidirectional line
				(at 30.48 -55.88 180)
				(length 5.08)
				(name "IO2_N6")
				(number "N6")
			)
			(pin bidirectional clock
				(at 30.48 -58.42 180)
				(length 5.08)
				(name "IO2_N7/GCLK2")
				(number "N7")
			)
			(pin bidirectional clock
				(at 30.48 -60.96 180)
				(length 5.08)
				(name "IO2_N8/GCLK3")
				(number "N8")
			)
			(pin bidirectional line
				(at 30.48 -63.5 180)
				(length 5.08)
				(name "IO2_N9")
				(number "N9")
			)
			(pin bidirectional line
				(at 30.48 -66.04 180)
				(length 5.08)
				(name "IO2_N10")
				(number "N10")
			)
			(pin bidirectional line
				(at 30.48 -68.58 180)
				(length 5.08)
				(name "IO2_N11")
				(number "N11")
			)
			(pin bidirectional line
				(at 30.48 -71.12 180)
				(length 5.08)
				(name "IO2_N12")
				(number "N12")
			)
			(pin bidirectional line
				(at 30.48 -73.66 180)
				(length 5.08)
				(name "IO2_N13")
				(number "N13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EPM570ZM256"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 25.4 107.95 0)
		)
		(property "Value" "EPM570ZM256"
			(at 25.4 -107.95 0)
		)
		(property "Footprint" "Package_BGA:BGA-256_11.0x11.0mm_Layout20x20_P0.5mm_Ball0.3mm_Pad0.25mm_NSMD"
			(at 25.4 -110.49 0)
		)
		(property "Datasheet" "https://www.altera.com/content/dam/altera-www/global/en_US/pdfs/literature/hb/max2/max2_mii5v1.pdf"
			(at 0 0 0)
		)
		(property "Description" "Altera Zero-Power MAX2 CPLD with 570 LE"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "MAX2 MBGA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*BGA*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "EPM570ZM256_1_1"
			(pin bidirectional line
				(at -40.64 104.14 0)
				(length 5.08)
				(name "IO1_B1")
				(number "B1")
			)
			(pin bidirectional line
				(at -40.64 101.6 0)
				(length 5.08)
				(name "IO1_C1")
				(number "C1")
			)
			(pin bidirectional line
				(at -40.64 99.06 0)
				(length 5.08)
				(name "IO1_C2")
				(number "C2")
			)
			(pin bidirectional line
				(at -40.64 96.52 0)
				(length 5.08)
				(name "IO1_C3")
				(number "C3")
			)
			(pin bidirectional line
				(at -40.64 93.98 0)
				(length 5.08)
				(name "IO1_D1")
				(number "D1")
			)
			(pin bidirectional line
				(at -40.64 91.44 0)
				(length 5.08)
				(name "IO1_D2")
				(number "D2")
			)
			(pin bidirectional line
				(at -40.64 88.9 0)
				(length 5.08)
				(name "IO1_D3")
				(number "D3")
			)
			(pin bidirectional line
				(at -40.64 86.36 0)
				(length 5.08)
				(name "IO1_E1")
				(number "E1")
			)
			(pin bidirectional line
				(at -40.64 83.82 0)
				(length 5.08)
				(name "IO1_E2")
				(number "E2")
			)
			(pin bidirectional line
				(at -40.64 81.28 0)
				(length 5.08)
				(name "IO1_E3")
				(number "E3")
			)
			(pin bidirectional line
				(at -40.64 78.74 0)
				(length 5.08)
				(name "IO1_F1")
				(number "F1")
			)
			(pin bidirectional line
				(at -40.64 76.2 0)
				(length 5.08)
				(name "IO1_F2")
				(number "F2")
			)
			(pin bidirectional line
				(at -40.64 73.66 0)
				(length 5.08)
				(name "IO1_F3")
				(number "F3")
			)
			(pin bidirectional line
				(at -40.64 71.12 0)
				(length 5.08)
				(name "IO1_G1")
				(number "G1")
			)
			(pin bidirectional line
				(at -40.64 68.58 0)
				(length 5.08)
				(name "IO1_G2")
				(number "G2")
			)
			(pin bidirectional line
				(at -40.64 66.04 0)
				(length 5.08)
				(name "IO1_H1")
				(number "H1")
			)
			(pin bidirectional line
				(at -40.64 63.5 0)
				(length 5.08)
				(name "IO1_H2")
				(number "H2")
			)
			(pin bidirectional line
				(at -40.64 60.96 0)
				(length 5.08)
				(name "IO1_J1")
				(number "J1")
			)
			(pin bidirectional line
				(at -40.64 58.42 0)
				(length 5.08)
				(name "IO1_J2")
				(number "J2")
			)
			(pin bidirectional clock
				(at -40.64 55.88 0)
				(length 5.08)
				(name "IO1_K1/GCLK0")
				(number "K1")
			)
			(pin bidirectional clock
				(at -40.64 53.34 0)
				(length 5.08)
				(name "IO1_L1/GCLK1")
				(number "L1")
			)
			(pin bidirectional line
				(at -40.64 50.8 0)
				(length 5.08)
				(name "IO1_M1")
				(number "M1")
			)
			(pin bidirectional line
				(at -40.64 48.26 0)
				(length 5.08)
				(name "IO1_M2")
				(number "M2")
			)
			(pin bidirectional line
				(at -40.64 45.72 0)
				(length 5.08)
				(name "IO1_N1")
				(number "N1")
			)
			(pin bidirectional line
				(at -40.64 43.18 0)
				(length 5.08)
				(name "IO1_N2")
				(number "N2")
			)
			(pin bidirectional line
				(at -40.64 40.64 0)
				(length 5.08)
				(name "IO1_P1")
				(number "P1")
			)
			(pin bidirectional line
				(at -40.64 38.1 0)
				(length 5.08)
				(name "IO1_P2")
				(number "P2")
			)
			(pin bidirectional line
				(at -40.64 35.56 0)
				(length 5.08)
				(name "IO1_R1")
				(number "R1")
			)
			(pin bidirectional line
				(at -40.64 33.02 0)
				(length 5.08)
				(name "IO1_R2")
				(number "R2")
			)
			(pin bidirectional line
				(at -40.64 30.48 0)
				(length 5.08)
				(name "IO1_R3")
				(number "R3")
			)
			(pin bidirectional line
				(at -40.64 27.94 0)
				(length 5.08)
				(name "IO1_T1")
				(number "T1")
			)
			(pin bidirectional line
				(at -40.64 25.4 0)
				(length 5.08)
				(name "IO1_T2")
				(number "T2")
			)
			(pin bidirectional line
				(at -40.64 22.86 0)
				(length 5.08)
				(name "IO1_T4")
				(number "T4")
			)
			(pin bidirectional line
				(at -40.64 20.32 0)
				(length 5.08)
				(name "IO1_U1")
				(number "U1")
			)
			(pin bidirectional line
				(at -40.64 17.78 0)
				(length 5.08)
				(name "IO1_U3")
				(number "U3")
			)
			(pin bidirectional line
				(at -40.64 15.24 0)
				(length 5.08)
				(name "IO1_U4")
				(number "U4")
			)
			(pin bidirectional line
				(at -40.64 12.7 0)
				(length 5.08)
				(name "IO1_V1")
				(number "V1")
			)
			(pin bidirectional line
				(at -40.64 10.16 0)
				(length 5.08)
				(name "IO1_V3")
				(number "V3")
			)
			(pin bidirectional line
				(at -40.64 7.62 0)
				(length 5.08)
				(name "IO1_V4")
				(number "V4")
			)
			(pin bidirectional line
				(at -40.64 5.08 0)
				(length 5.08)
				(name "IO1_V5")
				(number "V5")
			)
			(pin bidirectional line
				(at -40.64 2.54 0)
				(length 5.08)
				(name "IO1_V6")
				(number "V6")
			)
			(pin bidirectional line
				(at -40.64 0 0)
				(length 5.08)
				(name "IO1_V16")
				(number "V16")
			)
			(pin bidirectional line
				(at -40.64 -2.54 0)
				(length 5.08)
				(name "IO1_V17")
				(number "V17")
			)
			(pin bidirectional line
				(at -40.64 -5.08 0)
				(length 5.08)
				(name "IO1_V18")
				(number "V18")
			)
			(pin bidirectional line
				(at -40.64 -7.62 0)
				(length 5.08)
				(name "IO1_W1")
				(number "W1")
			)
			(pin bidirectional line
				(at -40.64 -10.16 0)
				(length 5.08)
				(name "IO1_W3")
				(number "W3")
			)
			(pin bidirectional line
				(at -40.64 -12.7 0)
				(length 5.08)
				(name "IO1_W4")
				(number "W4")
			)
			(pin bidirectional line
				(at -40.64 -15.24 0)
				(length 5.08)
				(name "IO1_W5")
				(number "W5")
			)
			(pin bidirectional line
				(at -40.64 -17.78 0)
				(length 5.08)
				(name "IO1_W6")
				(number "W6")
			)
			(pin bidirectional line
				(at -40.64 -20.32 0)
				(length 5.08)
				(name "IO1_W7")
				(number "W7")
			)
			(pin bidirectional line
				(at -40.64 -22.86 0)
				(length 5.08)
				(name "IO1_W8")
				(number "W8")
			)
			(pin bidirectional line
				(at -40.64 -25.4 0)
				(length 5.08)
				(name "IO1_W11")
				(number "W11")
			)
			(pin bidirectional line
				(at -40.64 -27.94 0)
				(length 5.08)
				(name "IO1_W12/DEV_OE")
				(number "W12")
			)
			(pin bidirectional line
				(at -40.64 -30.48 0)
				(length 5.08)
				(name "IO1_W13")
				(number "W13")
			)
			(pin bidirectional line
				(at -40.64 -33.02 0)
				(length 5.08)
				(name "IO1_W14")
				(number "W14")
			)
			(pin bidirectional line
				(at -40.64 -35.56 0)
				(length 5.08)
				(name "IO1_W15")
				(number "W15")
			)
			(pin bidirectional line
				(at -40.64 -38.1 0)
				(length 5.08)
				(name "IO1_W16")
				(number "W16")
			)
			(pin bidirectional line
				(at -40.64 -40.64 0)
				(length 5.08)
				(name "IO1_W17")
				(number "W17")
			)
			(pin bidirectional line
				(at -40.64 -43.18 0)
				(length 5.08)
				(name "IO1_W18")
				(number "W18")
			)
			(pin bidirectional line
				(at -40.64 -45.72 0)
				(length 5.08)
				(name "IO1_Y1")
				(number "Y1")
			)
			(pin bidirectional line
				(at -40.64 -48.26 0)
				(length 5.08)
				(name "IO1_Y2")
				(number "Y2")
			)
			(pin bidirectional line
				(at -40.64 -50.8 0)
				(length 5.08)
				(name "IO1_Y3")
				(number "Y3")
			)
			(pin bidirectional line
				(at -40.64 -53.34 0)
				(length 5.08)
				(name "IO1_Y4")
				(number "Y4")
			)
			(pin bidirectional line
				(at -40.64 -55.88 0)
				(length 5.08)
				(name "IO1_Y5")
				(number "Y5")
			)
			(pin bidirectional line
				(at -40.64 -58.42 0)
				(length 5.08)
				(name "IO1_Y6")
				(number "Y6")
			)
			(pin bidirectional line
				(at -40.64 -60.96 0)
				(length 5.08)
				(name "IO1_Y7")
				(number "Y7")
			)
			(pin bidirectional line
				(at -40.64 -63.5 0)
				(length 5.08)
				(name "IO1_Y8")
				(number "Y8")
			)
			(pin bidirectional line
				(at -40.64 -66.04 0)
				(length 5.08)
				(name "IO1_Y9")
				(number "Y9")
			)
			(pin bidirectional line
				(at -40.64 -68.58 0)
				(length 5.08)
				(name "IO1_Y10")
				(number "Y10")
			)
			(pin bidirectional line
				(at -40.64 -71.12 0)
				(length 5.08)
				(name "IO1_Y11")
				(number "Y11")
			)
			(pin bidirectional line
				(at -40.64 -73.66 0)
				(length 5.08)
				(name "IO1_Y12")
				(number "Y12")
			)
			(pin bidirectional line
				(at -40.64 -76.2 0)
				(length 5.08)
				(name "IO1_Y13/DEV_CLRn")
				(number "Y13")
			)
			(pin bidirectional line
				(at -40.64 -78.74 0)
				(length 5.08)
				(name "IO1_Y14")
				(number "Y14")
			)
			(pin bidirectional line
				(at -40.64 -81.28 0)
				(length 5.08)
				(name "IO1_Y15")
				(number "Y15")
			)
			(pin bidirectional line
				(at -40.64 -83.82 0)
				(length 5.08)
				(name "IO1_Y16")
				(number "Y16")
			)
			(pin bidirectional line
				(at -40.64 -86.36 0)
				(length 5.08)
				(name "IO1_Y17")
				(number "Y17")
			)
			(pin bidirectional line
				(at -40.64 -88.9 0)
				(length 5.08)
				(name "IO1_Y18")
				(number "Y18")
			)
			(pin bidirectional line
				(at -40.64 -91.44 0)
				(length 5.08)
				(name "IO1_Y19")
				(number "Y19")
			)
			(pin input line
				(at -40.64 -93.98 0)
				(length 5.08)
				(name "TMS")
				(number "T3")
			)
			(pin input line
				(at -40.64 -96.52 0)
				(length 5.08)
				(name "TDI")
				(number "U2")
			)
			(pin input clock
				(at -40.64 -99.06 0)
				(length 5.08)
				(name "TCK")
				(number "W2")
			)
			(pin output line
				(at -40.64 -101.6 0)
				(length 5.08)
				(name "TDO")
				(number "V2")
			)
			(pin power_in line
				(at -25.4 111.76 270)
				(length 5.08)
				(name "VCCINT")
				(number "K4")
			)
			(pin power_in line
				(at -25.4 -111.76 90)
				(length 5.08)
				(name "GND")
				(number "J4")
			)
			(pin power_in line
				(at -22.86 111.76 270)
				(length 5.08)
				(name "VCCINT")
				(number "U11")
			)
			(pin power_in line
				(at -22.86 -111.76 90)
				(length 5.08)
				(name "GND")
				(number "U12")
			)
			(pin power_in line
				(at -20.32 111.76 270)
				(length 5.08)
				(name "VCCINT")
				(number "L17")
			)
			(pin power_in line
				(at -20.32 -111.76 90)
				(length 5.08)
				(name "GND")
				(number "M17")
			)
			(pin power_in line
				(at -17.78 111.76 270)
				(length 5.08)
				(name "VCCINT")
				(number "D11")
			)
			(pin power_in line
				(at -17.78 -111.76 90)
				(length 5.08)
				(name "GND")
				(number "D12")
			)
			(pin power_in line
				(at -15.24 111.76 270)
				(length 5.08)
				(name "VCCIO1")
				(number "K3")
			)
			(pin power_in line
				(at -15.24 -111.76 90)
				(length 5.08)
				(name "GND")
				(number "H3")
			)
			(pin power_in line
				(at -12.7 111.76 270)
				(length 5.08)
				(name "VCCIO1")
				(number "L3")
			)
			(pin power_in line
				(at -12.7 -111.76 90)
				(length 5.08)
				(name "GND")
				(number "J3")
			)
			(pin power_in line
				(at -10.16 111.76 270)
				(length 5.08)
				(name "VCCIO1")
				(number "L4")
			)
			(pin power_in line
				(at -10.16 -111.76 90)
				(length 5.08)
				(name "GND")
				(number "M4")
			)
			(pin power_in line
				(at -7.62 111.76 270)
				(length 5.08)
				(name "VCCIO1")
				(number "M3")
			)
			(pin power_in line
				(at -7.62 -111.76 90)
				(length 5.08)
				(name "GND")
				(number "N3")
			)
			(pin power_in line
				(at -5.08 111.76 270)
				(length 5.08)
				(name "VCCIO1")
				(number "U10")
			)
			(pin power_in line
				(at -5.08 -111.76 90)
				(length 5.08)
				(name "GND")
				(number "U9")
			)
			(pin power_in line
				(at -2.54 111.76 270)
				(length 5.08)
				(name "VCCIO1")
				(number "V10")
			)
			(pin power_in line
				(at -2.54 -111.76 90)
				(length 5.08)
				(name "GND")
				(number "V8")
			)
			(pin power_in line
				(at 0 111.76 270)
				(length 5.08)
				(name "VCCIO1")
				(number "V11")
			)
			(pin power_in line
				(at 0 -111.76 90)
				(length 5.08)
				(name "GND")
				(number "V9")
			)
			(pin power_in line
				(at 2.54 111.76 270)
				(length 5.08)
				(name "VCCIO1")
				(number "V12")
			)
			(pin power_in line
				(at 2.54 -111.76 90)
				(length 5.08)
				(name "GND")
				(number "V13")
			)
			(pin power_in line
				(at 5.08 111.76 270)
				(length 5.08)
				(name "VCCIO2")
				(number "J18")
			)
			(pin power_in line
				(at 5.08 -111.76 90)
				(length 5.08)
				(name "GND")
				(number "H18")
			)
			(pin power_in line
				(at 7.62 111.76 270)
				(length 5.08)
				(name "VCCIO2")
				(number "K17")
			)
			(pin power_in line
				(at 7.62 -111.76 90)
				(length 5.08)
				(name "GND")
				(number "J17")
			)
			(pin power_in line
				(at 10.16 111.76 270)
				(length 5.08)
				(name "VCCIO2")
				(number "K18")
			)
			(pin power_in line
				(at 10.16 -111.76 90)
				(length 5.08)
				(name "GND")
				(number "N18")
			)
			(pin power_in line
				(at 12.7 111.76 270)
				(length 5.08)
				(name "VCCIO2")
				(number "L18")
			)
			(pin power_in line
				(at 12.7 -111.76 90)
				(length 5.08)
				(name "GND")
				(number "C8")
			)
			(pin power_in line
				(at 15.24 111.76 270)
				(length 5.08)
				(name "VCCIO2")
				(number "C9")
			)
			(pin power_in line
				(at 15.24 -111.76 90)
				(length 5.08)
				(name "GND")
				(number "D9")
			)
			(pin power_in line
				(at 17.78 111.76 270)
				(length 5.08)
				(name "VCCIO2")
				(number "C10")
			)
			(pin power_in line
				(at 17.78 -111.76 90)
				(length 5.08)
				(name "GND")
				(number "C12")
			)
			(pin power_in line
				(at 20.32 111.76 270)
				(length 5.08)
				(name "VCCIO2")
				(number "D10")
			)
			(pin power_in line
				(at 20.32 -111.76 90)
				(length 5.08)
				(name "GND")
				(number "C13")
			)
			(pin power_in line
				(at 22.86 111.76 270)
				(length 5.08)
				(name "VCCIO2")
				(number "C11")
			)
			(pin power_in line
				(at 22.86 -111.76 90)
				(length 5.08)
				(name "GND")
				(number "M18")
			)
			(pin bidirectional line
				(at 40.64 104.14 180)
				(length 5.08)
				(name "IO2_A1")
				(number "A1")
			)
			(pin bidirectional line
				(at 40.64 101.6 180)
				(length 5.08)
				(name "IO2_A2")
				(number "A2")
			)
			(pin bidirectional line
				(at 40.64 99.06 180)
				(length 5.08)
				(name "IO2_A3")
				(number "A3")
			)
			(pin bidirectional line
				(at 40.64 96.52 180)
				(length 5.08)
				(name "IO2_A4")
				(number "A4")
			)
			(pin bidirectional line
				(at 40.64 93.98 180)
				(length 5.08)
				(name "IO2_A5")
				(number "A5")
			)
			(pin bidirectional line
				(at 40.64 91.44 180)
				(length 5.08)
				(name "IO2_A6")
				(number "A6")
			)
			(pin bidirectional line
				(at 40.64 88.9 180)
				(length 5.08)
				(name "IO2_A7")
				(number "A7")
			)
			(pin bidirectional line
				(at 40.64 86.36 180)
				(length 5.08)
				(name "IO2_A8")
				(number "A8")
			)
			(pin bidirectional line
				(at 40.64 83.82 180)
				(length 5.08)
				(name "IO2_A9")
				(number "A9")
			)
			(pin bidirectional line
				(at 40.64 81.28 180)
				(length 5.08)
				(name "IO2_A10")
				(number "A10")
			)
			(pin bidirectional line
				(at 40.64 78.74 180)
				(length 5.08)
				(name "IO2_A11")
				(number "A11")
			)
			(pin bidirectional line
				(at 40.64 76.2 180)
				(length 5.08)
				(name "IO2_A12")
				(number "A12")
			)
			(pin bidirectional line
				(at 40.64 73.66 180)
				(length 5.08)
				(name "IO2_A13")
				(number "A13")
			)
			(pin bidirectional line
				(at 40.64 71.12 180)
				(length 5.08)
				(name "IO2_A14")
				(number "A14")
			)
			(pin bidirectional line
				(at 40.64 68.58 180)
				(length 5.08)
				(name "IO2_A15")
				(number "A15")
			)
			(pin bidirectional line
				(at 40.64 66.04 180)
				(length 5.08)
				(name "IO2_A16")
				(number "A16")
			)
			(pin bidirectional line
				(at 40.64 63.5 180)
				(length 5.08)
				(name "IO2_A17")
				(number "A17")
			)
			(pin bidirectional line
				(at 40.64 60.96 180)
				(length 5.08)
				(name "IO2_A18")
				(number "A18")
			)
			(pin bidirectional line
				(at 40.64 58.42 180)
				(length 5.08)
				(name "IO2_A19")
				(number "A19")
			)
			(pin bidirectional line
				(at 40.64 55.88 180)
				(length 5.08)
				(name "IO2_A20")
				(number "A20")
			)
			(pin bidirectional line
				(at 40.64 53.34 180)
				(length 5.08)
				(name "IO2_B2")
				(number "B2")
			)
			(pin bidirectional line
				(at 40.64 50.8 180)
				(length 5.08)
				(name "IO2_B3")
				(number "B3")
			)
			(pin bidirectional line
				(at 40.64 48.26 180)
				(length 5.08)
				(name "IO2_B4")
				(number "B4")
			)
			(pin bidirectional line
				(at 40.64 45.72 180)
				(length 5.08)
				(name "IO2_B5")
				(number "B5")
			)
			(pin bidirectional line
				(at 40.64 43.18 180)
				(length 5.08)
				(name "IO2_B6")
				(number "B6")
			)
			(pin bidirectional line
				(at 40.64 40.64 180)
				(length 5.08)
				(name "IO2_B7")
				(number "B7")
			)
			(pin bidirectional line
				(at 40.64 38.1 180)
				(length 5.08)
				(name "IO2_B8")
				(number "B8")
			)
			(pin bidirectional line
				(at 40.64 35.56 180)
				(length 5.08)
				(name "IO2_B9")
				(number "B9")
			)
			(pin bidirectional line
				(at 40.64 33.02 180)
				(length 5.08)
				(name "IO2_B12")
				(number "B12")
			)
			(pin bidirectional line
				(at 40.64 30.48 180)
				(length 5.08)
				(name "IO2_B13")
				(number "B13")
			)
			(pin bidirectional line
				(at 40.64 27.94 180)
				(length 5.08)
				(name "IO2_B14")
				(number "B14")
			)
			(pin bidirectional line
				(at 40.64 25.4 180)
				(length 5.08)
				(name "IO2_B15")
				(number "B15")
			)
			(pin bidirectional line
				(at 40.64 22.86 180)
				(length 5.08)
				(name "IO2_B16")
				(number "B16")
			)
			(pin bidirectional line
				(at 40.64 20.32 180)
				(length 5.08)
				(name "IO2_B17")
				(number "B17")
			)
			(pin bidirectional line
				(at 40.64 17.78 180)
				(length 5.08)
				(name "IO2_B18")
				(number "B18")
			)
			(pin bidirectional line
				(at 40.64 15.24 180)
				(length 5.08)
				(name "IO2_B19")
				(number "B19")
			)
			(pin bidirectional line
				(at 40.64 12.7 180)
				(length 5.08)
				(name "IO2_B20")
				(number "B20")
			)
			(pin bidirectional line
				(at 40.64 10.16 180)
				(length 5.08)
				(name "IO2_C5")
				(number "C5")
			)
			(pin bidirectional line
				(at 40.64 7.62 180)
				(length 5.08)
				(name "IO2_C15")
				(number "C15")
			)
			(pin bidirectional line
				(at 40.64 5.08 180)
				(length 5.08)
				(name "IO2_C16")
				(number "C16")
			)
			(pin bidirectional line
				(at 40.64 2.54 180)
				(length 5.08)
				(name "IO2_C17")
				(number "C17")
			)
			(pin bidirectional line
				(at 40.64 0 180)
				(length 5.08)
				(name "IO2_C18")
				(number "C18")
			)
			(pin bidirectional line
				(at 40.64 -2.54 180)
				(length 5.08)
				(name "IO2_C19")
				(number "C19")
			)
			(pin bidirectional line
				(at 40.64 -5.08 180)
				(length 5.08)
				(name "IO2_C20")
				(number "C20")
			)
			(pin bidirectional line
				(at 40.64 -7.62 180)
				(length 5.08)
				(name "IO2_D18")
				(number "D18")
			)
			(pin bidirectional line
				(at 40.64 -10.16 180)
				(length 5.08)
				(name "IO2_D19")
				(number "D19")
			)
			(pin bidirectional line
				(at 40.64 -12.7 180)
				(length 5.08)
				(name "IO2_D20")
				(number "D20")
			)
			(pin bidirectional line
				(at 40.64 -15.24 180)
				(length 5.08)
				(name "IO2_E17")
				(number "E17")
			)
			(pin bidirectional line
				(at 40.64 -17.78 180)
				(length 5.08)
				(name "IO2_E18")
				(number "E18")
			)
			(pin bidirectional line
				(at 40.64 -20.32 180)
				(length 5.08)
				(name "IO2_E19")
				(number "E19")
			)
			(pin bidirectional line
				(at 40.64 -22.86 180)
				(length 5.08)
				(name "IO2_E20")
				(number "E20")
			)
			(pin bidirectional line
				(at 40.64 -25.4 180)
				(length 5.08)
				(name "IO2_F19")
				(number "F19")
			)
			(pin bidirectional line
				(at 40.64 -27.94 180)
				(length 5.08)
				(name "IO2_F20")
				(number "F20")
			)
			(pin bidirectional line
				(at 40.64 -30.48 180)
				(length 5.08)
				(name "IO2_G19")
				(number "G19")
			)
			(pin bidirectional line
				(at 40.64 -33.02 180)
				(length 5.08)
				(name "IO2_G20")
				(number "G20")
			)
			(pin bidirectional line
				(at 40.64 -35.56 180)
				(length 5.08)
				(name "IO2_H19")
				(number "H19")
			)
			(pin bidirectional line
				(at 40.64 -38.1 180)
				(length 5.08)
				(name "IO2_H20")
				(number "H20")
			)
			(pin bidirectional line
				(at 40.64 -40.64 180)
				(length 5.08)
				(name "IO2_J19")
				(number "J19")
			)
			(pin bidirectional line
				(at 40.64 -43.18 180)
				(length 5.08)
				(name "IO2_J20")
				(number "J20")
			)
			(pin bidirectional line
				(at 40.64 -45.72 180)
				(length 5.08)
				(name "IO2_K20")
				(number "K20")
			)
			(pin bidirectional clock
				(at 40.64 -48.26 180)
				(length 5.08)
				(name "IO2_L20/GCLK3")
				(number "L20")
			)
			(pin bidirectional line
				(at 40.64 -50.8 180)
				(length 5.08)
				(name "IO2_M19")
				(number "M19")
			)
			(pin bidirectional clock
				(at 40.64 -53.34 180)
				(length 5.08)
				(name "IO2_M20/GCLK2")
				(number "M20")
			)
			(pin bidirectional line
				(at 40.64 -55.88 180)
				(length 5.08)
				(name "IO2_N19")
				(number "N19")
			)
			(pin bidirectional line
				(at 40.64 -58.42 180)
				(length 5.08)
				(name "IO2_N20")
				(number "N20")
			)
			(pin bidirectional line
				(at 40.64 -60.96 180)
				(length 5.08)
				(name "IO2_P19")
				(number "P19")
			)
			(pin bidirectional line
				(at 40.64 -63.5 180)
				(length 5.08)
				(name "IO2_P20")
				(number "P20")
			)
			(pin bidirectional line
				(at 40.64 -66.04 180)
				(length 5.08)
				(name "IO2_R18")
				(number "R18")
			)
			(pin bidirectional line
				(at 40.64 -68.58 180)
				(length 5.08)
				(name "IO2_R19")
				(number "R19")
			)
			(pin bidirectional line
				(at 40.64 -71.12 180)
				(length 5.08)
				(name "IO2_R20")
				(number "R20")
			)
			(pin bidirectional line
				(at 40.64 -73.66 180)
				(length 5.08)
				(name "IO2_T18")
				(number "T18")
			)
			(pin bidirectional line
				(at 40.64 -76.2 180)
				(length 5.08)
				(name "IO2_T19")
				(number "T19")
			)
			(pin bidirectional line
				(at 40.64 -78.74 180)
				(length 5.08)
				(name "IO2_T20")
				(number "T20")
			)
			(pin bidirectional line
				(at 40.64 -81.28 180)
				(length 5.08)
				(name "IO2_U17")
				(number "U17")
			)
			(pin bidirectional line
				(at 40.64 -83.82 180)
				(length 5.08)
				(name "IO2_U18")
				(number "U18")
			)
			(pin bidirectional line
				(at 40.64 -86.36 180)
				(length 5.08)
				(name "IO2_U19")
				(number "U19")
			)
			(pin bidirectional line
				(at 40.64 -88.9 180)
				(length 5.08)
				(name "IO2_U20")
				(number "U20")
			)
			(pin bidirectional line
				(at 40.64 -91.44 180)
				(length 5.08)
				(name "IO2_V19")
				(number "V19")
			)
			(pin bidirectional line
				(at 40.64 -93.98 180)
				(length 5.08)
				(name "IO2_V20")
				(number "V20")
			)
			(pin bidirectional line
				(at 40.64 -96.52 180)
				(length 5.08)
				(name "IO2_W19")
				(number "W19")
			)
			(pin bidirectional line
				(at 40.64 -99.06 180)
				(length 5.08)
				(name "IO2_W20")
				(number "W20")
			)
			(pin bidirectional line
				(at 40.64 -101.6 180)
				(length 5.08)
				(name "IO2_Y20")
				(number "Y20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EP310"
		(extends "EP300")
		(property "Reference" "U"
			(at -2.54 17.145 0)
		)
		(property "Value" "EP310"
			(at -2.54 15.24 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at 1.27 -15.24 0)
		)
		(property "Datasheet" "https://www.usbid.com/assets/datasheets/A6/ep310%20-%20epld%20-%20altera.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "EPLD, 8 Macrocell, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "EPLD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
)
