(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "ATF1502AS-xAx44"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 24.13 0)
		)
		(property "Value" "ATF1502AS-xAx44"
			(at 12.7 24.13 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 36.83 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-0995-CPLD-ATF1502AS(L)-Datasheet.pdf"
			(at 0 36.83 0)
		)
		(property "Description" "Microchip CPLD, 32 Macrocell, 5 V, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "CPLD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ATF1502AS-xAx44_0_1")
		(symbol "ATF1502AS-xAx44_1_1"
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "I/O/TDI")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "I/O")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "I/O")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "I/O/PD1")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "I/O")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "I/O/TMS")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "I/O")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "I/O")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "I/O")
				(number "11")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "I/O")
				(number "12")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "I/O")
				(number "13")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "I/O")
				(number "14")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "I/O")
				(number "15")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "I/O")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "I/O/PD2")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "I/O")
				(number "20")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "I/O")
				(number "21")
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "I/O")
				(number "22")
			)
			(pin passive line
				(at 0 25.4 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "17")
			)
			(pin passive line
				(at 0 25.4 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "29")
			)
			(pin passive line
				(at 0 25.4 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "41")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VCC")
				(number "9")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "24")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "36")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "I/O")
				(number "44")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "I/O")
				(number "43")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "I/O")
				(number "42")
			)
			(pin input line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "I/OE2/GCLK2")
				(number "40")
			)
			(pin input line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "I/GCLR")
				(number "39")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "I/OE1/Vpp")
				(number "38")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "I/GCLK1")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "I/O/GCLK3")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "I/O")
				(number "34")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "I/O")
				(number "33")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "I/O/TDO")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "I/O")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "I/O")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "I/O")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "I/O")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "I/O/TCK")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "I/O")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "I/O")
				(number "23")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATF1502ASL-xAx44"
		(extends "ATF1502AS-xAx44")
		(property "Reference" "U"
			(at -12.7 24.13 0)
		)
		(property "Value" "ATF1502ASL-xAx44"
			(at 12.7 24.13 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 36.83 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-0995-CPLD-ATF1502AS(L)-Datasheet.pdf"
			(at 0 36.83 0)
		)
		(property "Description" "Microchip CPLD, 32 Macrocell, 5 V, Low Power, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "CPLD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATF1502ASV-xAx44"
		(extends "ATF1502AS-xAx44")
		(property "Reference" "U"
			(at -12.7 24.13 0)
		)
		(property "Value" "ATF1502ASV-xAx44"
			(at 12.7 24.13 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 36.83 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc1615.pdf"
			(at 0 36.83 0)
		)
		(property "Description" "Microchip CPLD, 32 Macrocell, 3.3 V, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "CPLD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATF1504AS-xAx44"
		(extends "ATF1502AS-xAx44")
		(property "Reference" "U"
			(at -12.7 24.13 0)
		)
		(property "Value" "ATF1504AS-xAx44"
			(at 12.7 24.13 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 36.83 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-0950-CPLD-ATF1504AS(L)-Datasheet.pdf"
			(at 0 36.83 0)
		)
		(property "Description" "Microchip CPLD, 64 Macrocell, 5 V, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "CPLD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATF1504ASL-xAx44"
		(extends "ATF1502AS-xAx44")
		(property "Reference" "U"
			(at -12.7 24.13 0)
		)
		(property "Value" "ATF1504ASL-xAx44"
			(at 12.7 24.13 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 36.83 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-0950-CPLD-ATF1504AS(L)-Datasheet.pdf"
			(at 0 36.83 0)
		)
		(property "Description" "Microchip CPLD, 64 Macrocell, 5 V, Low Power, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "CPLD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATF1504ASV-xAx44"
		(extends "ATF1502AS-xAx44")
		(property "Reference" "U"
			(at -12.7 24.13 0)
		)
		(property "Value" "ATF1504ASV-xAx44"
			(at 12.7 24.13 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 36.83 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATF1504ASV-ATF1504ASVL-Data-Sheet-20006185A.pdf"
			(at 0 36.83 0)
		)
		(property "Description" "Microchip CPLD, 64 Macrocell, 3.3 V, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "CPLD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATF1504ASVL-xAx44"
		(extends "ATF1502AS-xAx44")
		(property "Reference" "U"
			(at -12.7 24.13 0)
		)
		(property "Value" "ATF1504ASVL-xAx44"
			(at 12.7 24.13 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 36.83 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATF1504ASV-ATF1504ASVL-Data-Sheet-20006185A.pdf"
			(at 0 36.83 0)
		)
		(property "Description" "Microchip CPLD, 32 Macrocell, 3.3 V, Low Power, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "CPLD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
)
