(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "SLG46826G"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 16.51 0)
		)
		(property "Value" "SLG46826G"
			(at 6.35 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 0 -31.75 0)
		)
		(property "Datasheet" "https://www.renesas.com/in/en/document/dst/slg46826-datasheet"
			(at 0 -29.21 0)
		)
		(property "Description" "GreenPAK Programmable Mixed-Signal Matrix with In-System Programmability, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "cpld programmable logic low-cost renesas silego"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65*"
			(at 0 0 0)
		)
		(symbol "SLG46826G_1_1"
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "SDA")
				(number "12")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "SCL")
				(number "13")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IO0")
				(number "19")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "IO1")
				(number "18")
				(alternate "Vref_IN" input line)
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IO2")
				(number "17")
				(alternate "SLA_0" passive line)
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "IO3")
				(number "16")
				(alternate "SLA_1" passive line)
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "IO4")
				(number "15")
				(alternate "SLA_2" passive line)
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "IO5")
				(number "14")
				(alternate "SLA_3" passive line)
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 2.54)
				(name "V_{DD}")
				(number "20")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "V_{DD2}")
				(number "7")
			)
			(pin output line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "IO6")
				(number "11")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "IO7")
				(number "9")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "IO8")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "IO9")
				(number "6")
				(alternate "Vref_OUT1" output line)
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "IO10")
				(number "5")
				(alternate "Vref_OUT0" output line)
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "IO11")
				(number "4")
				(alternate "ACMP3L_IN" input line)
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "IO12")
				(number "3")
				(alternate "ACMP2L_IN" input line)
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "IO13")
				(number "2")
				(alternate "ACMP1H_IN" input line)
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "IO14")
				(number "1")
				(alternate "ACMP0H_IN" input line)
			)
		)
		(embedded_fonts no)
	)
)
