(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "XC7336"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -21.59 27.94 0)
		)
		(property "Value" "XC7336"
			(at -21.59 -27.94 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Xilinx CPLD, Obsolete"
			(at 0 0 0)
		)
		(symbol "XC7336_1_1"
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 3.81)
				(name "I/FI_A")
				(number "28")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 3.81)
				(name "I/FO/FI_1_1")
				(number "7")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 3.81)
				(name "I/FO_1_2")
				(number "8")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 3.81)
				(name "I/FO_1_3")
				(number "9")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 3.81)
				(name "I/FO_1_4")
				(number "11")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "I/FO_1_5")
				(number "12")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 3.81)
				(name "I/FO_1_6")
				(number "13")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 3.81)
				(name "I/FO_1_7")
				(number "14")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 3.81)
				(name "I/FO_1_8")
				(number "15")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 3.81)
				(name "I/FO_1_9")
				(number "16")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "I/FO_4_1")
				(number "27")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 3.81)
				(name "I/FO_4_2")
				(number "26")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 3.81)
				(name "I/FO_4_3")
				(number "25")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 3.81)
				(name "I/FO_4_4")
				(number "24")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 3.81)
				(name "I/FO_4_5")
				(number "22")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 3.81)
				(name "I/FO/FI_4_6")
				(number "20")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 3.81)
				(name "I/FO/FI_4_7")
				(number "19")
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 3.81)
				(name "I/FO/FI_4_8")
				(number "18")
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 3.81)
				(name "I/FO_4_9")
				(number "17")
			)
			(pin power_in line
				(at -2.54 30.48 270)
				(length 3.81)
				(name "VCCINT")
				(number "21")
			)
			(pin power_in line
				(at -2.54 -30.48 90)
				(length 3.81)
				(name "GND")
				(number "10")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 3.81)
				(name "VCCINT")
				(number "41")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 3.81)
				(name "GND")
				(number "23")
			)
			(pin power_in line
				(at 2.54 30.48 270)
				(length 3.81)
				(name "VCCIO")
				(number "32")
			)
			(pin power_in line
				(at 2.54 -30.48 90)
				(length 3.81)
				(name "GND")
				(number "31")
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 3.81)
				(name "I/FI_B")
				(number "42")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 3.81)
				(name "I/FO_2_9")
				(number "29")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 3.81)
				(name "I/FO_2_8")
				(number "30")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 3.81)
				(name "I/FO_2_7")
				(number "33")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 3.81)
				(name "I/FO_2_6")
				(number "34")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 3.81)
				(name "I/FO_2_5")
				(number "35")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 3.81)
				(name "I/FO_2_4")
				(number "36")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 3.81)
				(name "I/FO_2_3")
				(number "37")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 3.81)
				(name "I/FO_2_2")
				(number "38")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 3.81)
				(name "FO/FOE1_2_1")
				(number "39")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 3.81)
				(name "FO/FOE0_3_9")
				(number "40")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 3.81)
				(name "I/FO/FI_3_8")
				(number "43")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 3.81)
				(name "I/FO/FI_3_7")
				(number "44")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 3.81)
				(name "I/FO/FI/MR_3_6")
				(number "1")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 3.81)
				(name "I/FO/FI_3_5")
				(number "2")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 3.81)
				(name "I/FO/FI_3_4")
				(number "3")
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 3.81)
				(name "I/FO/FI_3_3")
				(number "4")
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 3.81)
				(name "FO/FCLK0_3_2")
				(number "5")
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 3.81)
				(name "FO/FCLK1_3_1")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC95108PC84"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -19.05 53.34 0)
		)
		(property "Value" "XC95108PC84"
			(at -19.05 -55.88 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "xilinx/xc95108.pdf"
			(at 0 0 0)
		)
		(property "Description" "Xilinx CPLD, Obsolete"
			(at 0 0 0)
		)
		(symbol "XC95108PC84_1_1"
			(pin input line
				(at -22.86 50.8 0)
				(length 3.81)
				(name "TDI")
				(number "28")
			)
			(pin input line
				(at -22.86 48.26 0)
				(length 3.81)
				(name "TMS")
				(number "29")
			)
			(pin input line
				(at -22.86 45.72 0)
				(length 3.81)
				(name "TCK")
				(number "30")
			)
			(pin output line
				(at -22.86 43.18 0)
				(length 3.81)
				(name "TDO")
				(number "59")
			)
			(pin bidirectional line
				(at -22.86 38.1 0)
				(length 3.81)
				(name "P1")
				(number "1")
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 3.81)
				(name "P2")
				(number "2")
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 3.81)
				(name "P3")
				(number "3")
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 3.81)
				(name "P4")
				(number "4")
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 3.81)
				(name "P5")
				(number "5")
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 3.81)
				(name "P6")
				(number "6")
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 3.81)
				(name "P7")
				(number "7")
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 3.81)
				(name "I/O/GCK1")
				(number "9")
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 3.81)
				(name "I/O/GCK2")
				(number "10")
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 3.81)
				(name "P11")
				(number "11")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 3.81)
				(name "I/O/GCK3")
				(number "12")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 3.81)
				(name "P13")
				(number "13")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 3.81)
				(name "P14")
				(number "14")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 3.81)
				(name "P15")
				(number "15")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 3.81)
				(name "P17")
				(number "17")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 3.81)
				(name "P18")
				(number "18")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 3.81)
				(name "P19")
				(number "19")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 3.81)
				(name "P20")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 3.81)
				(name "P21")
				(number "21")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 3.81)
				(name "P23")
				(number "23")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 3.81)
				(name "P24")
				(number "24")
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 3.81)
				(name "P25")
				(number "25")
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 3.81)
				(name "P26")
				(number "26")
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 3.81)
				(name "P31")
				(number "31")
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 3.81)
				(name "P32")
				(number "32")
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 3.81)
				(name "P33")
				(number "33")
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 3.81)
				(name "P34")
				(number "34")
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 3.81)
				(name "P35")
				(number "35")
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 3.81)
				(name "P36")
				(number "36")
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 3.81)
				(name "P37")
				(number "37")
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 3.81)
				(name "P39")
				(number "39")
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 3.81)
				(name "P40")
				(number "40")
			)
			(pin bidirectional line
				(at -22.86 -48.26 0)
				(length 3.81)
				(name "P41")
				(number "41")
			)
			(pin bidirectional line
				(at -22.86 -50.8 0)
				(length 3.81)
				(name "P43")
				(number "43")
			)
			(pin bidirectional line
				(at -22.86 -53.34 0)
				(length 3.81)
				(name "P44")
				(number "44")
			)
			(pin power_in line
				(at -5.08 55.88 270)
				(length 3.81)
				(name "VCC")
				(number "38")
			)
			(pin power_in line
				(at -5.08 -58.42 90)
				(length 3.81)
				(name "GND")
				(number "8")
			)
			(pin power_in line
				(at -2.54 55.88 270)
				(length 3.81)
				(name "VCC")
				(number "73")
			)
			(pin power_in line
				(at -2.54 -58.42 90)
				(length 3.81)
				(name "GND")
				(number "16")
			)
			(pin power_in line
				(at 0 55.88 270)
				(length 3.81)
				(name "VCC")
				(number "78")
			)
			(pin power_in line
				(at 0 -58.42 90)
				(length 3.81)
				(name "GND")
				(number "27")
			)
			(pin power_in line
				(at 2.54 55.88 270)
				(length 3.81)
				(name "VCCIO")
				(number "22")
			)
			(pin power_in line
				(at 2.54 -58.42 90)
				(length 3.81)
				(name "GND")
				(number "42")
			)
			(pin power_in line
				(at 5.08 55.88 270)
				(length 3.81)
				(name "VCCIO")
				(number "64")
			)
			(pin power_in line
				(at 5.08 -58.42 90)
				(length 3.81)
				(name "GND")
				(number "49")
			)
			(pin power_in line
				(at 7.62 -58.42 90)
				(length 3.81)
				(name "GND")
				(number "60")
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 3.81)
				(name "P84")
				(number "84")
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 3.81)
				(name "P83")
				(number "83")
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 3.81)
				(name "P82")
				(number "82")
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 3.81)
				(name "P81")
				(number "81")
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 3.81)
				(name "P80")
				(number "80")
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 3.81)
				(name "P79")
				(number "79")
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 3.81)
				(name "I/O/GTS2")
				(number "77")
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 3.81)
				(name "I/O/GTS1")
				(number "76")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 3.81)
				(name "P75")
				(number "75")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 3.81)
				(name "I/O/GSR")
				(number "74")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 3.81)
				(name "P72")
				(number "72")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 3.81)
				(name "P71")
				(number "71")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 3.81)
				(name "P70")
				(number "70")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "P69")
				(number "69")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "P68")
				(number "68")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 3.81)
				(name "P67")
				(number "67")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 3.81)
				(name "P66")
				(number "66")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 3.81)
				(name "P65")
				(number "65")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 3.81)
				(name "P63")
				(number "63")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 3.81)
				(name "P62")
				(number "62")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 3.81)
				(name "P61")
				(number "61")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 3.81)
				(name "P58")
				(number "58")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 3.81)
				(name "P57")
				(number "57")
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 3.81)
				(name "P56")
				(number "56")
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 3.81)
				(name "P55")
				(number "55")
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 3.81)
				(name "P54")
				(number "54")
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 3.81)
				(name "P53")
				(number "53")
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 3.81)
				(name "P52")
				(number "52")
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 3.81)
				(name "P51")
				(number "51")
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 3.81)
				(name "P50")
				(number "50")
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 3.81)
				(name "P48")
				(number "48")
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 3.81)
				(name "P47")
				(number "47")
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 3.81)
				(name "P46")
				(number "46")
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 3.81)
				(name "P45")
				(number "45")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC95108PQ100"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 59.69 0)
		)
		(property "Value" "XC95108PQ100"
			(at -20.32 -62.23 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "xilinx/xc95108.pdf"
			(at 0 0 0)
		)
		(property "Description" "Xilinx CPLD, Obsolete"
			(at 0 0 0)
		)
		(symbol "XC95108PQ100_1_1"
			(pin bidirectional line
				(at -25.4 55.88 0)
				(length 5.08)
				(name "P15")
				(number "15")
			)
			(pin bidirectional line
				(at -25.4 53.34 0)
				(length 5.08)
				(name "P16")
				(number "16")
			)
			(pin bidirectional line
				(at -25.4 50.8 0)
				(length 5.08)
				(name "P17")
				(number "17")
			)
			(pin bidirectional line
				(at -25.4 48.26 0)
				(length 5.08)
				(name "P18")
				(number "18")
			)
			(pin bidirectional line
				(at -25.4 45.72 0)
				(length 5.08)
				(name "P19")
				(number "19")
			)
			(pin bidirectional line
				(at -25.4 43.18 0)
				(length 5.08)
				(name "P20")
				(number "20")
			)
			(pin bidirectional line
				(at -25.4 40.64 0)
				(length 5.08)
				(name "P21")
				(number "21")
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 5.08)
				(name "P22")
				(number "22")
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 5.08)
				(name "P26")
				(number "26")
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 5.08)
				(name "P27")
				(number "27")
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 5.08)
				(name "P30")
				(number "30")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "P3")
				(number "3")
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "P4")
				(number "4")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "P8")
				(number "8")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "P9")
				(number "9")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "P10")
				(number "10")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "P11")
				(number "11")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "P12")
				(number "12")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "P13")
				(number "13")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "P14")
				(number "14")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "P98")
				(number "98")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "P99")
				(number "99")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "P31")
				(number "31")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "P32")
				(number "32")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "P34")
				(number "34")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "P35")
				(number "35")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "P36")
				(number "36")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "P37")
				(number "37")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 5.08)
				(name "P38")
				(number "38")
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "P39")
				(number "39")
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "P41")
				(number "41")
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 5.08)
				(name "P42")
				(number "42")
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 5.08)
				(name "P43")
				(number "43")
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 5.08)
				(name "P44")
				(number "44")
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 5.08)
				(name "P45")
				(number "45")
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 5.08)
				(name "P51")
				(number "51")
			)
			(pin bidirectional line
				(at -25.4 -43.18 0)
				(length 5.08)
				(name "I/O/GSR")
				(number "1")
			)
			(pin bidirectional line
				(at -25.4 -45.72 0)
				(length 5.08)
				(name "I/O/GTS1")
				(number "5")
			)
			(pin bidirectional line
				(at -25.4 -48.26 0)
				(length 5.08)
				(name "I/O/GTS2")
				(number "6")
			)
			(pin bidirectional line
				(at -25.4 -50.8 0)
				(length 5.08)
				(name "I/O/GCK1")
				(number "24")
			)
			(pin bidirectional line
				(at -25.4 -53.34 0)
				(length 5.08)
				(name "I/O/GCK2")
				(number "25")
			)
			(pin bidirectional line
				(at -25.4 -55.88 0)
				(length 5.08)
				(name "I/O/GCK3")
				(number "29")
			)
			(pin power_in line
				(at -7.62 63.5 270)
				(length 5.08)
				(name "VCC")
				(number "7")
			)
			(pin power_in line
				(at -7.62 -66.04 90)
				(length 5.08)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at -5.08 63.5 270)
				(length 5.08)
				(name "VCC")
				(number "59")
			)
			(pin power_in line
				(at -5.08 -66.04 90)
				(length 5.08)
				(name "GND")
				(number "23")
			)
			(pin power_in line
				(at -2.54 63.5 270)
				(length 5.08)
				(name "VCC")
				(number "100")
			)
			(pin power_in line
				(at -2.54 -66.04 90)
				(length 5.08)
				(name "GND")
				(number "33")
			)
			(pin power_in line
				(at 0 63.5 270)
				(length 5.08)
				(name "VCCIO")
				(number "28")
			)
			(pin power_in line
				(at 0 -66.04 90)
				(length 5.08)
				(name "GND")
				(number "46")
			)
			(pin power_in line
				(at 2.54 63.5 270)
				(length 5.08)
				(name "VCCIO")
				(number "40")
			)
			(pin power_in line
				(at 2.54 -66.04 90)
				(length 5.08)
				(name "GND")
				(number "64")
			)
			(pin power_in line
				(at 5.08 63.5 270)
				(length 5.08)
				(name "VCCIO")
				(number "53")
			)
			(pin power_in line
				(at 5.08 -66.04 90)
				(length 5.08)
				(name "GND")
				(number "71")
			)
			(pin power_in line
				(at 7.62 63.5 270)
				(length 5.08)
				(name "VCCIO")
				(number "90")
			)
			(pin power_in line
				(at 7.62 -66.04 90)
				(length 5.08)
				(name "GND")
				(number "77")
			)
			(pin power_in line
				(at 10.16 -66.04 90)
				(length 5.08)
				(name "GND")
				(number "86")
			)
			(pin input line
				(at 25.4 55.88 180)
				(length 5.08)
				(name "TDI")
				(number "47")
			)
			(pin input line
				(at 25.4 53.34 180)
				(length 5.08)
				(name "TMS")
				(number "49")
			)
			(pin input line
				(at 25.4 50.8 180)
				(length 5.08)
				(name "TCK")
				(number "50")
			)
			(pin output line
				(at 25.4 48.26 180)
				(length 5.08)
				(name "TDO")
				(number "85")
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 5.08)
				(name "P48")
				(number "48")
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 5.08)
				(name "P52")
				(number "52")
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 5.08)
				(name "P54")
				(number "54")
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 5.08)
				(name "P55")
				(number "55")
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 5.08)
				(name "P56")
				(number "56")
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 5.08)
				(name "P57")
				(number "57")
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 5.08)
				(name "P58")
				(number "58")
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "P60")
				(number "60")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 5.08)
				(name "P61")
				(number "61")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "P62")
				(number "62")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "P63")
				(number "63")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "P65")
				(number "65")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "P66")
				(number "66")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "P67")
				(number "67")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "P68")
				(number "68")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "P69")
				(number "69")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "P70")
				(number "70")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "P72")
				(number "72")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "P73")
				(number "73")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "P74")
				(number "74")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "P75")
				(number "75")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "P76")
				(number "76")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "P78")
				(number "78")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "P79")
				(number "79")
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 5.08)
				(name "P80")
				(number "80")
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "P81")
				(number "81")
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "P82")
				(number "82")
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "P83")
				(number "83")
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 5.08)
				(name "P84")
				(number "84")
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 5.08)
				(name "P87")
				(number "87")
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 5.08)
				(name "P88")
				(number "88")
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 5.08)
				(name "P89")
				(number "89")
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 5.08)
				(name "P91")
				(number "91")
			)
			(pin bidirectional line
				(at 25.4 -45.72 180)
				(length 5.08)
				(name "P92")
				(number "92")
			)
			(pin bidirectional line
				(at 25.4 -48.26 180)
				(length 5.08)
				(name "P93")
				(number "93")
			)
			(pin bidirectional line
				(at 25.4 -50.8 180)
				(length 5.08)
				(name "P94")
				(number "94")
			)
			(pin bidirectional line
				(at 25.4 -53.34 180)
				(length 5.08)
				(name "P95")
				(number "95")
			)
			(pin bidirectional line
				(at 25.4 -55.88 180)
				(length 5.08)
				(name "P96")
				(number "96")
			)
			(pin bidirectional line
				(at 25.4 -58.42 180)
				(length 5.08)
				(name "P97")
				(number "97")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC95144PQ100"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 59.69 0)
		)
		(property "Value" "XC95144PQ100"
			(at -20.32 -62.23 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Xilinx CPLD, Obsolete"
			(at 0 0 0)
		)
		(symbol "XC95144PQ100_1_1"
			(pin bidirectional line
				(at -25.4 55.88 0)
				(length 5.08)
				(name "P15")
				(number "15")
			)
			(pin bidirectional line
				(at -25.4 53.34 0)
				(length 5.08)
				(name "P16")
				(number "16")
			)
			(pin bidirectional line
				(at -25.4 50.8 0)
				(length 5.08)
				(name "P17")
				(number "17")
			)
			(pin bidirectional line
				(at -25.4 48.26 0)
				(length 5.08)
				(name "P18")
				(number "18")
			)
			(pin bidirectional line
				(at -25.4 45.72 0)
				(length 5.08)
				(name "P19")
				(number "19")
			)
			(pin bidirectional line
				(at -25.4 43.18 0)
				(length 5.08)
				(name "P20")
				(number "20")
			)
			(pin bidirectional line
				(at -25.4 40.64 0)
				(length 5.08)
				(name "P21")
				(number "21")
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 5.08)
				(name "P22")
				(number "22")
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 5.08)
				(name "P26")
				(number "26")
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 5.08)
				(name "P27")
				(number "27")
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 5.08)
				(name "P30")
				(number "30")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "I/O/GTS3")
				(number "3")
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "I/O/GTS4")
				(number "4")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "P8")
				(number "8")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "P9")
				(number "9")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "P10")
				(number "10")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "P11")
				(number "11")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "P12")
				(number "12")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "P13")
				(number "13")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "P14")
				(number "14")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "P98")
				(number "98")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "P99")
				(number "99")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "P31")
				(number "31")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "P32")
				(number "32")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "P34")
				(number "34")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "P35")
				(number "35")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "P36")
				(number "36")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "P37")
				(number "37")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 5.08)
				(name "P38")
				(number "38")
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "P39")
				(number "39")
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "P41")
				(number "41")
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 5.08)
				(name "P42")
				(number "42")
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 5.08)
				(name "P43")
				(number "43")
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 5.08)
				(name "P44")
				(number "44")
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 5.08)
				(name "P45")
				(number "45")
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 5.08)
				(name "P51")
				(number "51")
			)
			(pin bidirectional line
				(at -25.4 -43.18 0)
				(length 5.08)
				(name "I/O/GSR")
				(number "1")
			)
			(pin bidirectional line
				(at -25.4 -45.72 0)
				(length 5.08)
				(name "I/O/GTS1")
				(number "5")
			)
			(pin bidirectional line
				(at -25.4 -48.26 0)
				(length 5.08)
				(name "I/O/GTS2")
				(number "6")
			)
			(pin bidirectional line
				(at -25.4 -50.8 0)
				(length 5.08)
				(name "I/O/GCK1")
				(number "24")
			)
			(pin bidirectional line
				(at -25.4 -53.34 0)
				(length 5.08)
				(name "I/O/GCK2")
				(number "25")
			)
			(pin bidirectional line
				(at -25.4 -55.88 0)
				(length 5.08)
				(name "I/O/GCK3")
				(number "29")
			)
			(pin power_in line
				(at -7.62 63.5 270)
				(length 5.08)
				(name "VCC")
				(number "7")
			)
			(pin power_in line
				(at -7.62 -66.04 90)
				(length 5.08)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at -5.08 63.5 270)
				(length 5.08)
				(name "VCC")
				(number "59")
			)
			(pin power_in line
				(at -5.08 -66.04 90)
				(length 5.08)
				(name "GND")
				(number "23")
			)
			(pin power_in line
				(at -2.54 63.5 270)
				(length 5.08)
				(name "VCC")
				(number "100")
			)
			(pin power_in line
				(at -2.54 -66.04 90)
				(length 5.08)
				(name "GND")
				(number "33")
			)
			(pin power_in line
				(at 0 63.5 270)
				(length 5.08)
				(name "VCCIO")
				(number "28")
			)
			(pin power_in line
				(at 0 -66.04 90)
				(length 5.08)
				(name "GND")
				(number "46")
			)
			(pin power_in line
				(at 2.54 63.5 270)
				(length 5.08)
				(name "VCCIO")
				(number "40")
			)
			(pin power_in line
				(at 2.54 -66.04 90)
				(length 5.08)
				(name "GND")
				(number "64")
			)
			(pin power_in line
				(at 5.08 63.5 270)
				(length 5.08)
				(name "VCCIO")
				(number "53")
			)
			(pin power_in line
				(at 5.08 -66.04 90)
				(length 5.08)
				(name "GND")
				(number "71")
			)
			(pin power_in line
				(at 7.62 63.5 270)
				(length 5.08)
				(name "VCCIO")
				(number "90")
			)
			(pin power_in line
				(at 7.62 -66.04 90)
				(length 5.08)
				(name "GND")
				(number "77")
			)
			(pin power_in line
				(at 10.16 -66.04 90)
				(length 5.08)
				(name "GND")
				(number "86")
			)
			(pin input line
				(at 25.4 55.88 180)
				(length 5.08)
				(name "TDI")
				(number "47")
			)
			(pin input line
				(at 25.4 53.34 180)
				(length 5.08)
				(name "TMS")
				(number "49")
			)
			(pin input line
				(at 25.4 50.8 180)
				(length 5.08)
				(name "TCK")
				(number "50")
			)
			(pin output line
				(at 25.4 48.26 180)
				(length 5.08)
				(name "TDO")
				(number "85")
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 5.08)
				(name "P48")
				(number "48")
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 5.08)
				(name "P52")
				(number "52")
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 5.08)
				(name "P54")
				(number "54")
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 5.08)
				(name "P55")
				(number "55")
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 5.08)
				(name "P56")
				(number "56")
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 5.08)
				(name "P57")
				(number "57")
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 5.08)
				(name "P58")
				(number "58")
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "P60")
				(number "60")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 5.08)
				(name "P61")
				(number "61")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "P62")
				(number "62")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "P63")
				(number "63")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "P65")
				(number "65")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "P66")
				(number "66")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "P67")
				(number "67")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "P68")
				(number "68")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "P69")
				(number "69")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "P70")
				(number "70")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "P72")
				(number "72")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "P73")
				(number "73")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "P74")
				(number "74")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "P75")
				(number "75")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "P76")
				(number "76")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "P78")
				(number "78")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "P79")
				(number "79")
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 5.08)
				(name "P80")
				(number "80")
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "P81")
				(number "81")
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "P82")
				(number "82")
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "P83")
				(number "83")
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 5.08)
				(name "P84")
				(number "84")
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 5.08)
				(name "P87")
				(number "87")
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 5.08)
				(name "P88")
				(number "88")
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 5.08)
				(name "P89")
				(number "89")
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 5.08)
				(name "P91")
				(number "91")
			)
			(pin bidirectional line
				(at 25.4 -45.72 180)
				(length 5.08)
				(name "P92")
				(number "92")
			)
			(pin bidirectional line
				(at 25.4 -48.26 180)
				(length 5.08)
				(name "P93")
				(number "93")
			)
			(pin bidirectional line
				(at 25.4 -50.8 180)
				(length 5.08)
				(name "P94")
				(number "94")
			)
			(pin bidirectional line
				(at 25.4 -53.34 180)
				(length 5.08)
				(name "P95")
				(number "95")
			)
			(pin bidirectional line
				(at 25.4 -55.88 180)
				(length 5.08)
				(name "P96")
				(number "96")
			)
			(pin bidirectional line
				(at 25.4 -58.42 180)
				(length 5.08)
				(name "P97")
				(number "97")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC95144XL-TQ100"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 64.77 0)
		)
		(property "Value" "XC95144XL-TQ100"
			(at -20.32 -64.77 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.xilinx.com/support/documentation/data_sheets/ds056.pdf"
			(at 0 0 0)
		)
		(property "Description" "CPLD, 144 Macrocells, 3200 Usable Gates"
			(at 0 0 0)
		)
		(property "ki_keywords" "CPLD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "XC95144XL-TQ100_1_1"
			(pin bidirectional line
				(at -25.4 60.96 0)
				(length 5.08)
				(name "P11")
				(number "11")
			)
			(pin bidirectional line
				(at -25.4 58.42 0)
				(length 5.08)
				(name "P12")
				(number "12")
			)
			(pin bidirectional line
				(at -25.4 55.88 0)
				(length 5.08)
				(name "P13")
				(number "13")
			)
			(pin bidirectional line
				(at -25.4 53.34 0)
				(length 5.08)
				(name "P14")
				(number "14")
			)
			(pin bidirectional line
				(at -25.4 50.8 0)
				(length 5.08)
				(name "P15")
				(number "15")
			)
			(pin bidirectional line
				(at -25.4 48.26 0)
				(length 5.08)
				(name "P16")
				(number "16")
			)
			(pin bidirectional line
				(at -25.4 45.72 0)
				(length 5.08)
				(name "P17")
				(number "17")
			)
			(pin bidirectional line
				(at -25.4 43.18 0)
				(length 5.08)
				(name "P18")
				(number "18")
			)
			(pin bidirectional line
				(at -25.4 40.64 0)
				(length 5.08)
				(name "P19")
				(number "19")
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 5.08)
				(name "P20")
				(number "20")
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 5.08)
				(name "I/O/GCK1")
				(number "22")
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 5.08)
				(name "I/O/GSR")
				(number "99")
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 5.08)
				(name "I/O/GTS3")
				(number "1")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "I/O/GTS4")
				(number "2")
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "I/O/GTS1")
				(number "3")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "I/O/GTS2")
				(number "4")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "P6")
				(number "6")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "P7")
				(number "7")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "P8")
				(number "8")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "P9")
				(number "9")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "P10")
				(number "10")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "I/O/GCK2")
				(number "23")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "P24")
				(number "24")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "P25")
				(number "25")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "I/O/GCK3")
				(number "27")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "P28")
				(number "28")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "P29")
				(number "29")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "P30")
				(number "30")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "P32")
				(number "32")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "P33")
				(number "33")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 5.08)
				(name "P34")
				(number "34")
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "P87")
				(number "87")
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 5.08)
				(name "P89")
				(number "89")
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 5.08)
				(name "P90")
				(number "90")
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 5.08)
				(name "P91")
				(number "91")
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 5.08)
				(name "P92")
				(number "92")
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 5.08)
				(name "P93")
				(number "93")
			)
			(pin bidirectional line
				(at -25.4 -40.64 0)
				(length 5.08)
				(name "P94")
				(number "94")
			)
			(pin bidirectional line
				(at -25.4 -43.18 0)
				(length 5.08)
				(name "P95")
				(number "95")
			)
			(pin bidirectional line
				(at -25.4 -45.72 0)
				(length 5.08)
				(name "P96")
				(number "96")
			)
			(pin bidirectional line
				(at -25.4 -48.26 0)
				(length 5.08)
				(name "P97")
				(number "97")
			)
			(pin power_in line
				(at -7.62 68.58 270)
				(length 5.08)
				(name "VCCINT")
				(number "5")
			)
			(pin power_in line
				(at -7.62 -68.58 90)
				(length 5.08)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at -5.08 68.58 270)
				(length 5.08)
				(name "VCCINT")
				(number "57")
			)
			(pin power_in line
				(at -5.08 -68.58 90)
				(length 5.08)
				(name "GND")
				(number "31")
			)
			(pin power_in line
				(at -2.54 68.58 270)
				(length 5.08)
				(name "VCCINT")
				(number "98")
			)
			(pin power_in line
				(at -2.54 -68.58 90)
				(length 5.08)
				(name "GND")
				(number "44")
			)
			(pin power_in line
				(at 0 68.58 270)
				(length 5.08)
				(name "VCCIO")
				(number "26")
			)
			(pin power_in line
				(at 0 -68.58 90)
				(length 5.08)
				(name "GND")
				(number "62")
			)
			(pin power_in line
				(at 2.54 68.58 270)
				(length 5.08)
				(name "VCCIO")
				(number "38")
			)
			(pin power_in line
				(at 2.54 -68.58 90)
				(length 5.08)
				(name "GND")
				(number "69")
			)
			(pin power_in line
				(at 5.08 68.58 270)
				(length 5.08)
				(name "VCCIO")
				(number "51")
			)
			(pin power_in line
				(at 5.08 -68.58 90)
				(length 5.08)
				(name "GND")
				(number "75")
			)
			(pin power_in line
				(at 7.62 68.58 270)
				(length 5.08)
				(name "VCCIO")
				(number "88")
			)
			(pin power_in line
				(at 7.62 -68.58 90)
				(length 5.08)
				(name "GND")
				(number "84")
			)
			(pin power_in line
				(at 10.16 -68.58 90)
				(length 5.08)
				(name "GND")
				(number "100")
			)
			(pin bidirectional line
				(at 25.4 60.96 180)
				(length 5.08)
				(name "P35")
				(number "35")
			)
			(pin bidirectional line
				(at 25.4 58.42 180)
				(length 5.08)
				(name "P36")
				(number "36")
			)
			(pin bidirectional line
				(at 25.4 55.88 180)
				(length 5.08)
				(name "P37")
				(number "37")
			)
			(pin bidirectional line
				(at 25.4 53.34 180)
				(length 5.08)
				(name "P39")
				(number "39")
			)
			(pin bidirectional line
				(at 25.4 50.8 180)
				(length 5.08)
				(name "P40")
				(number "40")
			)
			(pin bidirectional line
				(at 25.4 48.26 180)
				(length 5.08)
				(name "P41")
				(number "41")
			)
			(pin bidirectional line
				(at 25.4 45.72 180)
				(length 5.08)
				(name "P42")
				(number "42")
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 5.08)
				(name "P43")
				(number "43")
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 5.08)
				(name "P46")
				(number "46")
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 5.08)
				(name "P49")
				(number "49")
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 5.08)
				(name "P74")
				(number "74")
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 5.08)
				(name "P76")
				(number "76")
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "P77")
				(number "77")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 5.08)
				(name "P78")
				(number "78")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "P79")
				(number "79")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "P80")
				(number "80")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "P81")
				(number "81")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "P82")
				(number "82")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "P85")
				(number "85")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "P86")
				(number "86")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "P50")
				(number "50")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "P52")
				(number "52")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "P53")
				(number "53")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "P54")
				(number "54")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "P55")
				(number "55")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "P56")
				(number "56")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "P58")
				(number "58")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "P59")
				(number "59")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "P60")
				(number "60")
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 5.08)
				(name "P61")
				(number "61")
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "P63")
				(number "63")
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "P64")
				(number "64")
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "P65")
				(number "65")
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 5.08)
				(name "P66")
				(number "66")
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 5.08)
				(name "P67")
				(number "67")
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 5.08)
				(name "P68")
				(number "68")
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 5.08)
				(name "P70")
				(number "70")
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 5.08)
				(name "P71")
				(number "71")
			)
			(pin bidirectional line
				(at 25.4 -45.72 180)
				(length 5.08)
				(name "P72")
				(number "72")
			)
			(pin bidirectional line
				(at 25.4 -48.26 180)
				(length 5.08)
				(name "P73")
				(number "73")
			)
			(pin input line
				(at 25.4 -53.34 180)
				(length 5.08)
				(name "TDI")
				(number "45")
			)
			(pin input line
				(at 25.4 -55.88 180)
				(length 5.08)
				(name "TMS")
				(number "47")
			)
			(pin input line
				(at 25.4 -58.42 180)
				(length 5.08)
				(name "TCK")
				(number "48")
			)
			(pin output line
				(at 25.4 -60.96 180)
				(length 5.08)
				(name "TDO")
				(number "83")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC95144XL-TQ144"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 85.09 0)
		)
		(property "Value" "XC95144XL-TQ144"
			(at -27.94 -85.09 0)
		)
		(property "Footprint" "Package_QFP:TQFP-144_20x20mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.xilinx.com/support/documentation/data_sheets/ds056.pdf"
			(at 0 0 0)
		)
		(property "Description" "CPLD, 144 Macrocells, 3200 Usable Gates"
			(at 0 0 0)
		)
		(property "ki_keywords" "CPLD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "XC95144XL-TQ144_1_1"
			(pin bidirectional line
				(at -33.02 81.28 0)
				(length 5.08)
				(name "P16")
				(number "16")
			)
			(pin bidirectional line
				(at -33.02 78.74 0)
				(length 5.08)
				(name "P17")
				(number "17")
			)
			(pin bidirectional line
				(at -33.02 76.2 0)
				(length 5.08)
				(name "P19")
				(number "19")
			)
			(pin bidirectional line
				(at -33.02 73.66 0)
				(length 5.08)
				(name "P20")
				(number "20")
			)
			(pin bidirectional line
				(at -33.02 71.12 0)
				(length 5.08)
				(name "P21")
				(number "21")
			)
			(pin bidirectional line
				(at -33.02 68.58 0)
				(length 5.08)
				(name "P22")
				(number "22")
			)
			(pin bidirectional line
				(at -33.02 66.04 0)
				(length 5.08)
				(name "P23")
				(number "23")
			)
			(pin bidirectional line
				(at -33.02 63.5 0)
				(length 5.08)
				(name "P24")
				(number "24")
			)
			(pin bidirectional line
				(at -33.02 60.96 0)
				(length 5.08)
				(name "P25")
				(number "25")
			)
			(pin bidirectional line
				(at -33.02 58.42 0)
				(length 5.08)
				(name "P26")
				(number "26")
			)
			(pin bidirectional line
				(at -33.02 55.88 0)
				(length 5.08)
				(name "P27")
				(number "27")
			)
			(pin bidirectional line
				(at -33.02 53.34 0)
				(length 5.08)
				(name "P28")
				(number "28")
			)
			(pin bidirectional line
				(at -33.02 50.8 0)
				(length 5.08)
				(name "I/O/GCK1")
				(number "30")
			)
			(pin bidirectional line
				(at -33.02 48.26 0)
				(length 5.08)
				(name "P31")
				(number "31")
			)
			(pin bidirectional line
				(at -33.02 45.72 0)
				(length 5.08)
				(name "P35")
				(number "35")
			)
			(pin bidirectional line
				(at -33.02 40.64 0)
				(length 5.08)
				(name "I/O/GTS3")
				(number "2")
			)
			(pin bidirectional line
				(at -33.02 38.1 0)
				(length 5.08)
				(name "I/O/GTS4")
				(number "3")
			)
			(pin bidirectional line
				(at -33.02 35.56 0)
				(length 5.08)
				(name "P4")
				(number "4")
			)
			(pin bidirectional line
				(at -33.02 33.02 0)
				(length 5.08)
				(name "I/O/GTS1")
				(number "5")
			)
			(pin bidirectional line
				(at -33.02 30.48 0)
				(length 5.08)
				(name "I/O/GTS2")
				(number "6")
			)
			(pin bidirectional line
				(at -33.02 27.94 0)
				(length 5.08)
				(name "P7")
				(number "7")
			)
			(pin bidirectional line
				(at -33.02 25.4 0)
				(length 5.08)
				(name "P9")
				(number "9")
			)
			(pin bidirectional line
				(at -33.02 22.86 0)
				(length 5.08)
				(name "P10")
				(number "10")
			)
			(pin bidirectional line
				(at -33.02 20.32 0)
				(length 5.08)
				(name "P11")
				(number "11")
			)
			(pin bidirectional line
				(at -33.02 17.78 0)
				(length 5.08)
				(name "P12")
				(number "12")
			)
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 5.08)
				(name "P13")
				(number "13")
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 5.08)
				(name "P14")
				(number "14")
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 5.08)
				(name "P15")
				(number "15")
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 5.08)
				(name "P142")
				(number "142")
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 5.08)
				(name "I/O/GSR")
				(number "143")
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 5.08)
				(name "I/O/GCK2")
				(number "32")
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 5.08)
				(name "P33")
				(number "33")
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 5.08)
				(name "P34")
				(number "34")
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 5.08)
				(name "I/O/GCK3")
				(number "38")
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 5.08)
				(name "P39")
				(number "39")
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 5.08)
				(name "P40")
				(number "40")
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 5.08)
				(name "P41")
				(number "41")
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 5.08)
				(name "P43")
				(number "43")
			)
			(pin bidirectional line
				(at -33.02 -20.32 0)
				(length 5.08)
				(name "P44")
				(number "44")
			)
			(pin bidirectional line
				(at -33.02 -22.86 0)
				(length 5.08)
				(name "P45")
				(number "45")
			)
			(pin bidirectional line
				(at -33.02 -25.4 0)
				(length 5.08)
				(name "P46")
				(number "46")
			)
			(pin bidirectional line
				(at -33.02 -27.94 0)
				(length 5.08)
				(name "P48")
				(number "48")
			)
			(pin bidirectional line
				(at -33.02 -30.48 0)
				(length 5.08)
				(name "P49")
				(number "49")
			)
			(pin bidirectional line
				(at -33.02 -33.02 0)
				(length 5.08)
				(name "P50")
				(number "50")
			)
			(pin bidirectional line
				(at -33.02 -35.56 0)
				(length 5.08)
				(name "P51")
				(number "51")
			)
			(pin bidirectional line
				(at -33.02 -40.64 0)
				(length 5.08)
				(name "P118")
				(number "118")
			)
			(pin bidirectional line
				(at -33.02 -43.18 0)
				(length 5.08)
				(name "P126")
				(number "126")
			)
			(pin bidirectional line
				(at -33.02 -45.72 0)
				(length 5.08)
				(name "P128")
				(number "128")
			)
			(pin bidirectional line
				(at -33.02 -48.26 0)
				(length 5.08)
				(name "P129")
				(number "129")
			)
			(pin bidirectional line
				(at -33.02 -50.8 0)
				(length 5.08)
				(name "P130")
				(number "130")
			)
			(pin bidirectional line
				(at -33.02 -53.34 0)
				(length 5.08)
				(name "P131")
				(number "131")
			)
			(pin bidirectional line
				(at -33.02 -55.88 0)
				(length 5.08)
				(name "P132")
				(number "132")
			)
			(pin bidirectional line
				(at -33.02 -58.42 0)
				(length 5.08)
				(name "P133")
				(number "133")
			)
			(pin bidirectional line
				(at -33.02 -60.96 0)
				(length 5.08)
				(name "P134")
				(number "134")
			)
			(pin bidirectional line
				(at -33.02 -63.5 0)
				(length 5.08)
				(name "P135")
				(number "135")
			)
			(pin bidirectional line
				(at -33.02 -66.04 0)
				(length 5.08)
				(name "P136")
				(number "136")
			)
			(pin bidirectional line
				(at -33.02 -68.58 0)
				(length 5.08)
				(name "P137")
				(number "137")
			)
			(pin bidirectional line
				(at -33.02 -71.12 0)
				(length 5.08)
				(name "P138")
				(number "138")
			)
			(pin bidirectional line
				(at -33.02 -73.66 0)
				(length 5.08)
				(name "P139")
				(number "139")
			)
			(pin bidirectional line
				(at -33.02 -76.2 0)
				(length 5.08)
				(name "P140")
				(number "140")
			)
			(pin power_in line
				(at -15.24 -88.9 90)
				(length 5.08)
				(name "GND")
				(number "18")
			)
			(pin power_in line
				(at -12.7 -88.9 90)
				(length 5.08)
				(name "GND")
				(number "29")
			)
			(pin power_in line
				(at -10.16 88.9 270)
				(length 5.08)
				(name "VCCINT")
				(number "8")
			)
			(pin power_in line
				(at -10.16 -88.9 90)
				(length 5.08)
				(name "GND")
				(number "36")
			)
			(pin power_in line
				(at -7.62 88.9 270)
				(length 5.08)
				(name "VCCINT")
				(number "42")
			)
			(pin power_in line
				(at -7.62 -88.9 90)
				(length 5.08)
				(name "GND")
				(number "47")
			)
			(pin power_in line
				(at -5.08 88.9 270)
				(length 5.08)
				(name "VCCINT")
				(number "84")
			)
			(pin power_in line
				(at -5.08 -88.9 90)
				(length 5.08)
				(name "GND")
				(number "62")
			)
			(pin power_in line
				(at -2.54 88.9 270)
				(length 5.08)
				(name "VCCINT")
				(number "141")
			)
			(pin power_in line
				(at -2.54 -88.9 90)
				(length 5.08)
				(name "GND")
				(number "72")
			)
			(pin power_in line
				(at 0 88.9 270)
				(length 5.08)
				(name "VCCIO")
				(number "1")
			)
			(pin power_in line
				(at 0 -88.9 90)
				(length 5.08)
				(name "GND")
				(number "89")
			)
			(pin power_in line
				(at 2.54 88.9 270)
				(length 5.08)
				(name "VCCIO")
				(number "37")
			)
			(pin power_in line
				(at 2.54 -88.9 90)
				(length 5.08)
				(name "GND")
				(number "90")
			)
			(pin power_in line
				(at 5.08 88.9 270)
				(length 5.08)
				(name "VCCIO")
				(number "55")
			)
			(pin power_in line
				(at 5.08 -88.9 90)
				(length 5.08)
				(name "GND")
				(number "99")
			)
			(pin power_in line
				(at 7.62 88.9 270)
				(length 5.08)
				(name "VCCIO")
				(number "73")
			)
			(pin power_in line
				(at 7.62 -88.9 90)
				(length 5.08)
				(name "GND")
				(number "108")
			)
			(pin power_in line
				(at 10.16 88.9 270)
				(length 5.08)
				(name "VCCIO")
				(number "109")
			)
			(pin power_in line
				(at 10.16 -88.9 90)
				(length 5.08)
				(name "GND")
				(number "114")
			)
			(pin power_in line
				(at 12.7 88.9 270)
				(length 5.08)
				(name "VCCIO")
				(number "127")
			)
			(pin power_in line
				(at 12.7 -88.9 90)
				(length 5.08)
				(name "GND")
				(number "123")
			)
			(pin power_in line
				(at 15.24 -88.9 90)
				(length 5.08)
				(name "GND")
				(number "144")
			)
			(pin bidirectional line
				(at 33.02 81.28 180)
				(length 5.08)
				(name "P52")
				(number "52")
			)
			(pin bidirectional line
				(at 33.02 78.74 180)
				(length 5.08)
				(name "P53")
				(number "53")
			)
			(pin bidirectional line
				(at 33.02 76.2 180)
				(length 5.08)
				(name "P54")
				(number "54")
			)
			(pin bidirectional line
				(at 33.02 73.66 180)
				(length 5.08)
				(name "P56")
				(number "56")
			)
			(pin bidirectional line
				(at 33.02 71.12 180)
				(length 5.08)
				(name "P57")
				(number "57")
			)
			(pin bidirectional line
				(at 33.02 68.58 180)
				(length 5.08)
				(name "P58")
				(number "58")
			)
			(pin bidirectional line
				(at 33.02 66.04 180)
				(length 5.08)
				(name "P59")
				(number "59")
			)
			(pin bidirectional line
				(at 33.02 63.5 180)
				(length 5.08)
				(name "P60")
				(number "60")
			)
			(pin bidirectional line
				(at 33.02 60.96 180)
				(length 5.08)
				(name "P61")
				(number "61")
			)
			(pin bidirectional line
				(at 33.02 58.42 180)
				(length 5.08)
				(name "P64")
				(number "64")
			)
			(pin bidirectional line
				(at 33.02 55.88 180)
				(length 5.08)
				(name "P66")
				(number "66")
			)
			(pin bidirectional line
				(at 33.02 53.34 180)
				(length 5.08)
				(name "P68")
				(number "68")
			)
			(pin bidirectional line
				(at 33.02 50.8 180)
				(length 5.08)
				(name "P69")
				(number "69")
			)
			(pin bidirectional line
				(at 33.02 48.26 180)
				(length 5.08)
				(name "P70")
				(number "70")
			)
			(pin bidirectional line
				(at 33.02 43.18 180)
				(length 5.08)
				(name "P106")
				(number "106")
			)
			(pin bidirectional line
				(at 33.02 40.64 180)
				(length 5.08)
				(name "P110")
				(number "110")
			)
			(pin bidirectional line
				(at 33.02 38.1 180)
				(length 5.08)
				(name "P111")
				(number "111")
			)
			(pin bidirectional line
				(at 33.02 35.56 180)
				(length 5.08)
				(name "P112")
				(number "112")
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 5.08)
				(name "P113")
				(number "113")
			)
			(pin bidirectional line
				(at 33.02 30.48 180)
				(length 5.08)
				(name "P115")
				(number "115")
			)
			(pin bidirectional line
				(at 33.02 27.94 180)
				(length 5.08)
				(name "P116")
				(number "116")
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 5.08)
				(name "P117")
				(number "117")
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 5.08)
				(name "P119")
				(number "119")
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 5.08)
				(name "P120")
				(number "120")
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 5.08)
				(name "P121")
				(number "121")
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 5.08)
				(name "P124")
				(number "124")
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 5.08)
				(name "P125")
				(number "125")
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 5.08)
				(name "P71")
				(number "71")
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 5.08)
				(name "P74")
				(number "74")
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 5.08)
				(name "P75")
				(number "75")
			)
			(pin bidirectional line
				(at 33.02 0 180)
				(length 5.08)
				(name "P76")
				(number "76")
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 5.08)
				(name "P77")
				(number "77")
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 5.08)
				(name "P78")
				(number "78")
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 5.08)
				(name "P79")
				(number "79")
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 5.08)
				(name "P80")
				(number "80")
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 5.08)
				(name "P81")
				(number "81")
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 5.08)
				(name "P82")
				(number "82")
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 5.08)
				(name "P83")
				(number "83")
			)
			(pin bidirectional line
				(at 33.02 -20.32 180)
				(length 5.08)
				(name "P85")
				(number "85")
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 5.08)
				(name "P86")
				(number "86")
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 5.08)
				(name "P87")
				(number "87")
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 5.08)
				(name "P88")
				(number "88")
			)
			(pin bidirectional line
				(at 33.02 -33.02 180)
				(length 5.08)
				(name "P91")
				(number "91")
			)
			(pin bidirectional line
				(at 33.02 -35.56 180)
				(length 5.08)
				(name "P92")
				(number "92")
			)
			(pin bidirectional line
				(at 33.02 -38.1 180)
				(length 5.08)
				(name "P93")
				(number "93")
			)
			(pin bidirectional line
				(at 33.02 -40.64 180)
				(length 5.08)
				(name "P94")
				(number "94")
			)
			(pin bidirectional line
				(at 33.02 -43.18 180)
				(length 5.08)
				(name "P95")
				(number "95")
			)
			(pin bidirectional line
				(at 33.02 -45.72 180)
				(length 5.08)
				(name "P96")
				(number "96")
			)
			(pin bidirectional line
				(at 33.02 -48.26 180)
				(length 5.08)
				(name "P97")
				(number "97")
			)
			(pin bidirectional line
				(at 33.02 -50.8 180)
				(length 5.08)
				(name "P98")
				(number "98")
			)
			(pin bidirectional line
				(at 33.02 -53.34 180)
				(length 5.08)
				(name "P100")
				(number "100")
			)
			(pin bidirectional line
				(at 33.02 -55.88 180)
				(length 5.08)
				(name "P101")
				(number "101")
			)
			(pin bidirectional line
				(at 33.02 -58.42 180)
				(length 5.08)
				(name "P102")
				(number "102")
			)
			(pin bidirectional line
				(at 33.02 -60.96 180)
				(length 5.08)
				(name "P103")
				(number "103")
			)
			(pin bidirectional line
				(at 33.02 -63.5 180)
				(length 5.08)
				(name "P104")
				(number "104")
			)
			(pin bidirectional line
				(at 33.02 -66.04 180)
				(length 5.08)
				(name "P105")
				(number "105")
			)
			(pin bidirectional line
				(at 33.02 -68.58 180)
				(length 5.08)
				(name "P107")
				(number "107")
			)
			(pin bidirectional line
				(at 33.02 -73.66 180)
				(length 5.08)
				(name "TCK")
				(number "67")
			)
			(pin bidirectional line
				(at 33.02 -76.2 180)
				(length 5.08)
				(name "TDI")
				(number "63")
			)
			(pin bidirectional line
				(at 33.02 -78.74 180)
				(length 5.08)
				(name "TDO")
				(number "122")
			)
			(pin bidirectional line
				(at 33.02 -81.28 180)
				(length 5.08)
				(name "TMS")
				(number "65")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC9536PC44"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 33.02 0)
		)
		(property "Value" "XC9536PC44"
			(at -13.97 -33.02 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "xilinx/xc9536.pdf"
			(at 0 0 0)
		)
		(property "Description" "Xilinx CPLD, Obsolete"
			(at 0 0 0)
		)
		(symbol "XC9536PC44_1_1"
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 3.81)
				(name "M1")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 3.81)
				(name "M2")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 3.81)
				(name "I/O/GCK1")
				(number "5")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 3.81)
				(name "M4")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 3.81)
				(name "I/O/GCK2")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 3.81)
				(name "I/O/GCK3")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "M6")
				(number "8")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "M8")
				(number "9")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "M9")
				(number "11")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "M10")
				(number "12")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "M11")
				(number "13")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "M12")
				(number "14")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 3.81)
				(name "M13")
				(number "18")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "M14")
				(number "19")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "M15")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "M16")
				(number "22")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 3.81)
				(name "M17")
				(number "24")
			)
			(pin power_in line
				(at -2.54 35.56 270)
				(length 3.81)
				(name "VCC")
				(number "21")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 3.81)
				(name "GND")
				(number "10")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 3.81)
				(name "VCC")
				(number "41")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 3.81)
				(name "GND")
				(number "23")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 3.81)
				(name "VCCIO")
				(number "32")
			)
			(pin power_in line
				(at 2.54 -35.56 90)
				(length 3.81)
				(name "GND")
				(number "31")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 3.81)
				(name "M1")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 3.81)
				(name "M2")
				(number "44")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 3.81)
				(name "M4")
				(number "43")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 3.81)
				(name "I/O/GTS1")
				(number "42")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 3.81)
				(name "I/O/GTS2")
				(number "40")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 3.81)
				(name "I/O/GSR")
				(number "39")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "M7")
				(number "38")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "M8")
				(number "37")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "M9")
				(number "36")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "M10")
				(number "35")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "M11")
				(number "34")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "M12")
				(number "33")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 3.81)
				(name "M13")
				(number "29")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "M14")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "M15")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "M16")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "M17")
				(number "25")
			)
			(pin input line
				(at 17.78 -22.86 180)
				(length 3.81)
				(name "TDI")
				(number "15")
			)
			(pin input line
				(at 17.78 -25.4 180)
				(length 3.81)
				(name "TMS")
				(number "16")
			)
			(pin input line
				(at 17.78 -27.94 180)
				(length 3.81)
				(name "TCK")
				(number "17")
			)
			(pin output line
				(at 17.78 -30.48 180)
				(length 3.81)
				(name "TDO")
				(number "30")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC9572XL-TQ100"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 64.77 0)
		)
		(property "Value" "XC9572XL-TQ100"
			(at -20.32 -67.31 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.xilinx.com/support/documentation/data_sheets/ds057.pdf"
			(at 0 0 0)
		)
		(property "Description" "CPLD, 72 Macrocells, 1600 Usable Gates"
			(at 0 0 0)
		)
		(property "ki_keywords" "CPLD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "XC9572XL-TQ100_1_1"
			(pin bidirectional line
				(at -25.4 43.18 0)
				(length 5.08)
				(name "P13")
				(number "13")
			)
			(pin bidirectional line
				(at -25.4 40.64 0)
				(length 5.08)
				(name "P14")
				(number "14")
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 5.08)
				(name "P15")
				(number "15")
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 5.08)
				(name "P16")
				(number "16")
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 5.08)
				(name "P17")
				(number "17")
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 5.08)
				(name "P18")
				(number "18")
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 5.08)
				(name "P20")
				(number "20")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "I/O/GCK1")
				(number "22")
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "I/O/GCK2")
				(number "23")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "P25")
				(number "25")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "I/O/GCK3")
				(number "27")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "P28")
				(number "28")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "P29")
				(number "29")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "P30")
				(number "30")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "P33")
				(number "33")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "P36")
				(number "36")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "P39")
				(number "39")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "P40")
				(number "40")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "I/O/GTS3")
				(number "1")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "I/O/GTS1")
				(number "3")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "I/O/GTS2")
				(number "4")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "P6")
				(number "6")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "P8")
				(number "8")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "P9")
				(number "9")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 5.08)
				(name "P10")
				(number "10")
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "P11")
				(number "11")
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "P12")
				(number "12")
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 5.08)
				(name "P87")
				(number "87")
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 5.08)
				(name "P91")
				(number "91")
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 5.08)
				(name "P92")
				(number "92")
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 5.08)
				(name "P93")
				(number "93")
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 5.08)
				(name "P94")
				(number "94")
			)
			(pin bidirectional line
				(at -25.4 -40.64 0)
				(length 5.08)
				(name "P95")
				(number "95")
			)
			(pin bidirectional line
				(at -25.4 -43.18 0)
				(length 5.08)
				(name "P96")
				(number "96")
			)
			(pin bidirectional line
				(at -25.4 -45.72 0)
				(length 5.08)
				(name "P97")
				(number "97")
			)
			(pin bidirectional line
				(at -25.4 -48.26 0)
				(length 5.08)
				(name "I/O/GSR")
				(number "99")
			)
			(pin no_connect line
				(at -20.32 60.96 0)
				(length 0)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -20.32 58.42 0)
				(length 0)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at -20.32 55.88 0)
				(length 0)
				(hide yes)
				(name "NC")
				(number "19")
			)
			(pin no_connect line
				(at -20.32 53.34 0)
				(length 0)
				(hide yes)
				(name "NC")
				(number "24")
			)
			(pin no_connect line
				(at -20.32 50.8 0)
				(length 0)
				(hide yes)
				(name "NC")
				(number "34")
			)
			(pin no_connect line
				(at -20.32 48.26 0)
				(length 0)
				(hide yes)
				(name "NC")
				(number "43")
			)
			(pin power_in line
				(at -7.62 68.58 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at -7.62 -71.12 90)
				(length 5.08)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at -5.08 68.58 270)
				(length 5.08)
				(name "VCC")
				(number "57")
			)
			(pin power_in line
				(at -5.08 -71.12 90)
				(length 5.08)
				(name "GND")
				(number "31")
			)
			(pin power_in line
				(at -2.54 68.58 270)
				(length 5.08)
				(name "VCC")
				(number "98")
			)
			(pin power_in line
				(at -2.54 -71.12 90)
				(length 5.08)
				(name "GND")
				(number "44")
			)
			(pin power_in line
				(at 0 68.58 270)
				(length 5.08)
				(name "VCCIO")
				(number "26")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "GND")
				(number "62")
			)
			(pin power_in line
				(at 2.54 68.58 270)
				(length 5.08)
				(name "VCCIO")
				(number "38")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "GND")
				(number "69")
			)
			(pin power_in line
				(at 5.08 68.58 270)
				(length 5.08)
				(name "VCCIO")
				(number "51")
			)
			(pin power_in line
				(at 5.08 -71.12 90)
				(length 5.08)
				(name "GND")
				(number "75")
			)
			(pin power_in line
				(at 7.62 68.58 270)
				(length 5.08)
				(name "VCCIO")
				(number "88")
			)
			(pin power_in line
				(at 7.62 -71.12 90)
				(length 5.08)
				(name "GND")
				(number "84")
			)
			(pin power_in line
				(at 10.16 -71.12 90)
				(length 5.08)
				(name "GND")
				(number "100")
			)
			(pin no_connect line
				(at 20.32 60.96 180)
				(length 0)
				(hide yes)
				(name "NC")
				(number "46")
			)
			(pin no_connect line
				(at 20.32 58.42 180)
				(length 0)
				(hide yes)
				(name "NC")
				(number "73")
			)
			(pin no_connect line
				(at 20.32 55.88 180)
				(length 0)
				(hide yes)
				(name "NC")
				(number "80")
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 5.08)
				(name "P32")
				(number "32")
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 5.08)
				(name "P35")
				(number "35")
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 5.08)
				(name "P37")
				(number "37")
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 5.08)
				(name "P41")
				(number "41")
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 5.08)
				(name "P42")
				(number "42")
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 5.08)
				(name "P49")
				(number "49")
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 5.08)
				(name "P50")
				(number "50")
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "P52")
				(number "52")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 5.08)
				(name "P53")
				(number "53")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "P54")
				(number "54")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "P55")
				(number "55")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "P56")
				(number "56")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "P58")
				(number "58")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "P59")
				(number "59")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "P60")
				(number "60")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "P61")
				(number "61")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "P63")
				(number "63")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "P64")
				(number "64")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "P65")
				(number "65")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "P66")
				(number "66")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "P67")
				(number "67")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "P68")
				(number "68")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "P70")
				(number "70")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "P71")
				(number "71")
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 5.08)
				(name "P72")
				(number "72")
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "P74")
				(number "74")
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "P76")
				(number "76")
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "P77")
				(number "77")
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "P78")
				(number "78")
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 5.08)
				(name "P79")
				(number "79")
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 5.08)
				(name "P81")
				(number "81")
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 5.08)
				(name "P82")
				(number "82")
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 5.08)
				(name "P85")
				(number "85")
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 5.08)
				(name "P86")
				(number "86")
			)
			(pin bidirectional line
				(at 25.4 -45.72 180)
				(length 5.08)
				(name "P89")
				(number "89")
			)
			(pin bidirectional line
				(at 25.4 -48.26 180)
				(length 5.08)
				(name "P90")
				(number "90")
			)
			(pin input line
				(at 25.4 -55.88 180)
				(length 5.08)
				(name "TDI")
				(number "45")
			)
			(pin input line
				(at 25.4 -58.42 180)
				(length 5.08)
				(name "TMS")
				(number "47")
			)
			(pin input line
				(at 25.4 -60.96 180)
				(length 5.08)
				(name "TCK")
				(number "48")
			)
			(pin output line
				(at 25.4 -63.5 180)
				(length 5.08)
				(name "TDO")
				(number "83")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC9572XL-VQ64"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -16.51 40.64 0)
		)
		(property "Value" "XC9572XL-VQ64"
			(at -16.51 -43.18 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_10x10mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.xilinx.com/support/documentation/data_sheets/ds057.pdf"
			(at 0 0 0)
		)
		(property "Description" "CPLD, 72 Macrocells, 1600 Usable Gates"
			(at 0 0 0)
		)
		(property "ki_keywords" "CPLD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "XC9572XL-VQ64_1_1"
			(pin bidirectional line
				(at -20.32 35.56 0)
				(length 3.81)
				(name "P8")
				(number "8")
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 3.81)
				(name "P9")
				(number "9")
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 3.81)
				(name "P10")
				(number "10")
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 3.81)
				(name "P11")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 3.81)
				(name "P12")
				(number "12")
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 3.81)
				(name "P13")
				(number "13")
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 3.81)
				(name "I/O/GCK1")
				(number "15")
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 3.81)
				(name "I/O/GCK2")
				(number "16")
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 3.81)
				(name "I/O/GCK3")
				(number "17")
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 3.81)
				(name "P18")
				(number "18")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 3.81)
				(name "P19")
				(number "19")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 3.81)
				(name "P20")
				(number "20")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "P23")
				(number "23")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 3.81)
				(name "P1")
				(number "1")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 3.81)
				(name "I/O/GTS2")
				(number "2")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "P4")
				(number "4")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 3.81)
				(name "I/O/GTS1")
				(number "5")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 3.81)
				(name "P6")
				(number "6")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 3.81)
				(name "P7")
				(number "7")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 3.81)
				(name "P58")
				(number "58")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 3.81)
				(name "P59")
				(number "59")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 3.81)
				(name "P60")
				(number "60")
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 3.81)
				(name "P61")
				(number "61")
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 3.81)
				(name "P62")
				(number "62")
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 3.81)
				(name "P63")
				(number "63")
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 3.81)
				(name "I/O/GSR")
				(number "64")
			)
			(pin power_in line
				(at -2.54 43.18 270)
				(length 3.81)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -45.72 90)
				(length 3.81)
				(name "GND")
				(number "14")
			)
			(pin power_in line
				(at 0 43.18 270)
				(length 3.81)
				(name "VCC")
				(number "37")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 3.81)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 2.54 43.18 270)
				(length 3.81)
				(name "VCCIO")
				(number "26")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 3.81)
				(name "GND")
				(number "41")
			)
			(pin power_in line
				(at 5.08 43.18 270)
				(length 3.81)
				(name "VCCIO")
				(number "55")
			)
			(pin power_in line
				(at 5.08 -45.72 90)
				(length 3.81)
				(name "GND")
				(number "54")
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 3.81)
				(name "P22")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 3.81)
				(name "P24")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 3.81)
				(name "P25")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 3.81)
				(name "P27")
				(number "27")
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 3.81)
				(name "P31")
				(number "31")
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 3.81)
				(name "P32")
				(number "32")
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 3.81)
				(name "P33")
				(number "33")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 3.81)
				(name "P34")
				(number "34")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 3.81)
				(name "P35")
				(number "35")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 3.81)
				(name "P36")
				(number "36")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 3.81)
				(name "P38")
				(number "38")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 3.81)
				(name "P39")
				(number "39")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "P40")
				(number "40")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "P42")
				(number "42")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 3.81)
				(name "P43")
				(number "43")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "P44")
				(number "44")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "P45")
				(number "45")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "P46")
				(number "46")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "P47")
				(number "47")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "P48")
				(number "48")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 3.81)
				(name "P49")
				(number "49")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 3.81)
				(name "P50")
				(number "50")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 3.81)
				(name "P51")
				(number "51")
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 3.81)
				(name "P52")
				(number "52")
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 3.81)
				(name "P56")
				(number "56")
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 3.81)
				(name "P57")
				(number "57")
			)
			(pin input line
				(at 20.32 -33.02 180)
				(length 3.81)
				(name "TDI")
				(number "28")
			)
			(pin input line
				(at 20.32 -35.56 180)
				(length 3.81)
				(name "TMS")
				(number "29")
			)
			(pin input line
				(at 20.32 -38.1 180)
				(length 3.81)
				(name "TCK")
				(number "30")
			)
			(pin output line
				(at 20.32 -40.64 180)
				(length 3.81)
				(name "TDO")
				(number "53")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XCR3064XL-VQ100"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -21.59 53.34 0)
		)
		(property "Value" "XCR3064XL-VQ100"
			(at -21.59 -53.34 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.xilinx.com/support/documentation/data_sheets/ds017.pdf"
			(at 0 0 0)
		)
		(property "Description" "Xilinx CoolRunner 64-Macrocell CPLD, 3.3V, VQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "CPLD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5*"
			(at 0 0 0)
		)
		(symbol "XCR3064XL-VQ100_1_1"
			(pin passive line
				(at -25.4 50.8 0)
				(length 3.81)
				(name "A8/TDO")
				(number "73")
			)
			(pin passive line
				(at -25.4 48.26 0)
				(length 3.81)
				(name "C0/TCK")
				(number "62")
			)
			(pin passive line
				(at -25.4 45.72 0)
				(length 3.81)
				(name "B8/TDI")
				(number "4")
			)
			(pin passive line
				(at -25.4 43.18 0)
				(length 3.81)
				(name "D0/TMS")
				(number "15")
			)
			(pin passive line
				(at -25.4 40.64 0)
				(length 3.81)
				(name "PORT_EN")
				(number "11")
			)
			(pin passive line
				(at -25.4 38.1 0)
				(length 3.81)
				(name "A0")
				(number "85")
			)
			(pin passive line
				(at -25.4 35.56 0)
				(length 3.81)
				(name "A1")
				(number "84")
			)
			(pin passive line
				(at -25.4 33.02 0)
				(length 3.81)
				(name "A2")
				(number "83")
			)
			(pin passive line
				(at -25.4 30.48 0)
				(length 3.81)
				(name "A3")
				(number "81")
			)
			(pin passive line
				(at -25.4 27.94 0)
				(length 3.81)
				(name "A4")
				(number "80")
			)
			(pin passive line
				(at -25.4 25.4 0)
				(length 3.81)
				(name "A5")
				(number "79")
			)
			(pin passive line
				(at -25.4 22.86 0)
				(length 3.81)
				(name "A6")
				(number "76")
			)
			(pin passive line
				(at -25.4 20.32 0)
				(length 3.81)
				(name "A7")
				(number "75")
			)
			(pin passive line
				(at -25.4 17.78 0)
				(length 3.81)
				(name "A9")
				(number "71")
			)
			(pin passive line
				(at -25.4 15.24 0)
				(length 3.81)
				(name "A10")
				(number "69")
			)
			(pin passive line
				(at -25.4 12.7 0)
				(length 3.81)
				(name "A11")
				(number "68")
			)
			(pin passive line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "A12")
				(number "67")
			)
			(pin passive line
				(at -25.4 7.62 0)
				(length 3.81)
				(name "A13")
				(number "65")
			)
			(pin passive line
				(at -25.4 5.08 0)
				(length 3.81)
				(name "A14")
				(number "64")
			)
			(pin passive line
				(at -25.4 2.54 0)
				(length 3.81)
				(name "A15")
				(number "63")
			)
			(pin passive line
				(at -25.4 -2.54 0)
				(length 3.81)
				(name "B0")
				(number "92")
			)
			(pin passive line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "B1")
				(number "93")
			)
			(pin passive line
				(at -25.4 -7.62 0)
				(length 3.81)
				(name "B2")
				(number "94")
			)
			(pin passive line
				(at -25.4 -10.16 0)
				(length 3.81)
				(name "B3")
				(number "96")
			)
			(pin passive line
				(at -25.4 -12.7 0)
				(length 3.81)
				(name "B4")
				(number "97")
			)
			(pin passive line
				(at -25.4 -15.24 0)
				(length 3.81)
				(name "B5")
				(number "98")
			)
			(pin passive line
				(at -25.4 -17.78 0)
				(length 3.81)
				(name "B6")
				(number "99")
			)
			(pin passive line
				(at -25.4 -20.32 0)
				(length 3.81)
				(name "B7")
				(number "100")
			)
			(pin passive line
				(at -25.4 -22.86 0)
				(length 3.81)
				(name "B9")
				(number "6")
			)
			(pin passive line
				(at -25.4 -25.4 0)
				(length 3.81)
				(name "B10")
				(number "8")
			)
			(pin passive line
				(at -25.4 -27.94 0)
				(length 3.81)
				(name "B11")
				(number "9")
			)
			(pin passive line
				(at -25.4 -30.48 0)
				(length 3.81)
				(name "B12")
				(number "10")
			)
			(pin passive line
				(at -25.4 -33.02 0)
				(length 3.81)
				(name "B13")
				(number "12")
			)
			(pin passive line
				(at -25.4 -35.56 0)
				(length 3.81)
				(name "B14")
				(number "13")
			)
			(pin passive line
				(at -25.4 -38.1 0)
				(length 3.81)
				(name "B15")
				(number "14")
			)
			(pin input line
				(at -25.4 -43.18 0)
				(length 3.81)
				(name "CLK0/IN0")
				(number "90")
			)
			(pin input line
				(at -25.4 -45.72 0)
				(length 3.81)
				(name "CLK1/IN1")
				(number "89")
			)
			(pin input line
				(at -25.4 -48.26 0)
				(length 3.81)
				(name "CLK2/IN2")
				(number "88")
			)
			(pin input line
				(at -25.4 -50.8 0)
				(length 3.81)
				(name "CLK3/IN3")
				(number "87")
			)
			(pin power_in line
				(at -7.62 55.88 270)
				(length 3.81)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at -7.62 -55.88 90)
				(length 3.81)
				(name "GND")
				(number "26")
			)
			(pin power_in line
				(at -5.08 55.88 270)
				(length 3.81)
				(name "VCC")
				(number "18")
			)
			(pin power_in line
				(at -5.08 -55.88 90)
				(length 3.81)
				(name "GND")
				(number "38")
			)
			(pin power_in line
				(at -2.54 55.88 270)
				(length 3.81)
				(name "VCC")
				(number "34")
			)
			(pin power_in line
				(at -2.54 -55.88 90)
				(length 3.81)
				(name "GND")
				(number "43")
			)
			(pin power_in line
				(at 0 55.88 270)
				(length 3.81)
				(name "VCC")
				(number "39")
			)
			(pin power_in line
				(at 0 -55.88 90)
				(length 3.81)
				(name "GND")
				(number "59")
			)
			(pin power_in line
				(at 2.54 55.88 270)
				(length 3.81)
				(name "VCC")
				(number "51")
			)
			(pin power_in line
				(at 2.54 -55.88 90)
				(length 3.81)
				(name "GND")
				(number "74")
			)
			(pin power_in line
				(at 5.08 55.88 270)
				(length 3.81)
				(name "VCC")
				(number "66")
			)
			(pin power_in line
				(at 5.08 -55.88 90)
				(length 3.81)
				(name "GND")
				(number "86")
			)
			(pin power_in line
				(at 7.62 55.88 270)
				(length 3.81)
				(name "VCC")
				(number "82")
			)
			(pin power_in line
				(at 7.62 -55.88 90)
				(length 3.81)
				(name "GND")
				(number "95")
			)
			(pin power_in line
				(at 10.16 55.88 270)
				(length 3.81)
				(name "VCC")
				(number "91")
			)
			(pin passive line
				(at 25.4 40.64 180)
				(length 3.81)
				(name "D15")
				(number "37")
			)
			(pin passive line
				(at 25.4 38.1 180)
				(length 3.81)
				(name "D14")
				(number "36")
			)
			(pin passive line
				(at 25.4 35.56 180)
				(length 3.81)
				(name "D13")
				(number "35")
			)
			(pin passive line
				(at 25.4 33.02 180)
				(length 3.81)
				(name "D12")
				(number "33")
			)
			(pin passive line
				(at 25.4 30.48 180)
				(length 3.81)
				(name "D11")
				(number "32")
			)
			(pin passive line
				(at 25.4 27.94 180)
				(length 3.81)
				(name "D10")
				(number "31")
			)
			(pin passive line
				(at 25.4 25.4 180)
				(length 3.81)
				(name "D9")
				(number "30")
			)
			(pin passive line
				(at 25.4 22.86 180)
				(length 3.81)
				(name "D8")
				(number "29")
			)
			(pin passive line
				(at 25.4 20.32 180)
				(length 3.81)
				(name "D7")
				(number "25")
			)
			(pin passive line
				(at 25.4 17.78 180)
				(length 3.81)
				(name "D6")
				(number "23")
			)
			(pin passive line
				(at 25.4 15.24 180)
				(length 3.81)
				(name "D5")
				(number "21")
			)
			(pin passive line
				(at 25.4 12.7 180)
				(length 3.81)
				(name "D4")
				(number "20")
			)
			(pin passive line
				(at 25.4 10.16 180)
				(length 3.81)
				(name "D3")
				(number "19")
			)
			(pin passive line
				(at 25.4 7.62 180)
				(length 3.81)
				(name "D2")
				(number "17")
			)
			(pin passive line
				(at 25.4 5.08 180)
				(length 3.81)
				(name "D1")
				(number "16")
			)
			(pin passive line
				(at 25.4 0 180)
				(length 3.81)
				(name "C15")
				(number "40")
			)
			(pin passive line
				(at 25.4 -2.54 180)
				(length 3.81)
				(name "C14")
				(number "41")
			)
			(pin passive line
				(at 25.4 -5.08 180)
				(length 3.81)
				(name "C13")
				(number "42")
			)
			(pin passive line
				(at 25.4 -7.62 180)
				(length 3.81)
				(name "C12")
				(number "44")
			)
			(pin passive line
				(at 25.4 -10.16 180)
				(length 3.81)
				(name "C11")
				(number "45")
			)
			(pin passive line
				(at 25.4 -12.7 180)
				(length 3.81)
				(name "C10")
				(number "46")
			)
			(pin passive line
				(at 25.4 -15.24 180)
				(length 3.81)
				(name "C9")
				(number "47")
			)
			(pin passive line
				(at 25.4 -17.78 180)
				(length 3.81)
				(name "C8")
				(number "48")
			)
			(pin passive line
				(at 25.4 -20.32 180)
				(length 3.81)
				(name "C7")
				(number "52")
			)
			(pin passive line
				(at 25.4 -22.86 180)
				(length 3.81)
				(name "C6")
				(number "54")
			)
			(pin passive line
				(at 25.4 -25.4 180)
				(length 3.81)
				(name "C5")
				(number "56")
			)
			(pin passive line
				(at 25.4 -27.94 180)
				(length 3.81)
				(name "C4")
				(number "57")
			)
			(pin passive line
				(at 25.4 -30.48 180)
				(length 3.81)
				(name "C3")
				(number "58")
			)
			(pin passive line
				(at 25.4 -33.02 180)
				(length 3.81)
				(name "C2")
				(number "60")
			)
			(pin passive line
				(at 25.4 -35.56 180)
				(length 3.81)
				(name "C1")
				(number "61")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XCR3064XL-VQ44"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -16.51 33.02 0)
		)
		(property "Value" "XCR3064XL-VQ44"
			(at -16.51 -33.02 0)
		)
		(property "Footprint" "Package_QFP:LQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.xilinx.com/support/documentation/data_sheets/ds017.pdf"
			(at 0 0 0)
		)
		(property "Description" "Xilinx CoolRunner 64-Macrocell CPLD, 3.3V, VQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "CPLD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "XCR3064XL-VQ44_1_1"
			(pin passive line
				(at -20.32 30.48 0)
				(length 3.81)
				(name "TDO")
				(number "32")
			)
			(pin passive line
				(at -20.32 27.94 0)
				(length 3.81)
				(name "TCK")
				(number "26")
			)
			(pin passive line
				(at -20.32 25.4 0)
				(length 3.81)
				(name "TDI")
				(number "1")
			)
			(pin passive line
				(at -20.32 22.86 0)
				(length 3.81)
				(name "TMS")
				(number "7")
			)
			(pin passive line
				(at -20.32 20.32 0)
				(length 3.81)
				(name "PORT_EN")
				(number "4")
			)
			(pin passive line
				(at -20.32 17.78 0)
				(length 3.81)
				(name "A0")
				(number "35")
			)
			(pin passive line
				(at -20.32 15.24 0)
				(length 3.81)
				(name "A1")
				(number "34")
			)
			(pin passive line
				(at -20.32 12.7 0)
				(length 3.81)
				(name "A7")
				(number "33")
			)
			(pin passive line
				(at -20.32 10.16 0)
				(length 3.81)
				(name "A9")
				(number "31")
			)
			(pin passive line
				(at -20.32 7.62 0)
				(length 3.81)
				(name "A10")
				(number "30")
			)
			(pin passive line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "A13")
				(number "28")
			)
			(pin passive line
				(at -20.32 2.54 0)
				(length 3.81)
				(name "A14")
				(number "27")
			)
			(pin passive line
				(at -20.32 -2.54 0)
				(length 3.81)
				(name "B0")
				(number "42")
			)
			(pin passive line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "B1")
				(number "43")
			)
			(pin passive line
				(at -20.32 -7.62 0)
				(length 3.81)
				(name "B2")
				(number "44")
			)
			(pin passive line
				(at -20.32 -10.16 0)
				(length 3.81)
				(name "B9")
				(number "2")
			)
			(pin passive line
				(at -20.32 -12.7 0)
				(length 3.81)
				(name "B10")
				(number "3")
			)
			(pin passive line
				(at -20.32 -15.24 0)
				(length 3.81)
				(name "B13")
				(number "5")
			)
			(pin passive line
				(at -20.32 -17.78 0)
				(length 3.81)
				(name "B14")
				(number "6")
			)
			(pin input line
				(at -20.32 -22.86 0)
				(length 3.81)
				(name "CLC0/IN0")
				(number "40")
			)
			(pin input line
				(at -20.32 -25.4 0)
				(length 3.81)
				(name "CLK1/IN1")
				(number "39")
			)
			(pin input line
				(at -20.32 -27.94 0)
				(length 3.81)
				(name "CLK2/IN2")
				(number "38")
			)
			(pin input line
				(at -20.32 -30.48 0)
				(length 3.81)
				(name "CLK3/IN3")
				(number "37")
			)
			(pin power_in line
				(at -2.54 35.56 270)
				(length 3.81)
				(name "VCC")
				(number "9")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 3.81)
				(name "GND")
				(number "16")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 3.81)
				(name "VCC")
				(number "17")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 3.81)
				(name "GND")
				(number "24")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 3.81)
				(name "VCC")
				(number "29")
			)
			(pin power_in line
				(at 2.54 -35.56 90)
				(length 3.81)
				(name "GND")
				(number "36")
			)
			(pin power_in line
				(at 5.08 35.56 270)
				(length 3.81)
				(name "VCC")
				(number "41")
			)
			(pin passive line
				(at 20.32 20.32 180)
				(length 3.81)
				(name "C1")
				(number "25")
			)
			(pin passive line
				(at 20.32 17.78 180)
				(length 3.81)
				(name "C3")
				(number "23")
			)
			(pin passive line
				(at 20.32 15.24 180)
				(length 3.81)
				(name "C8")
				(number "22")
			)
			(pin passive line
				(at 20.32 12.7 180)
				(length 3.81)
				(name "C9")
				(number "21")
			)
			(pin passive line
				(at 20.32 10.16 180)
				(length 3.81)
				(name "C10")
				(number "20")
			)
			(pin passive line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "C11")
				(number "19")
			)
			(pin passive line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "C12")
				(number "18")
			)
			(pin passive line
				(at 20.32 0 180)
				(length 3.81)
				(name "D1")
				(number "8")
			)
			(pin passive line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "D3")
				(number "10")
			)
			(pin passive line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "D4")
				(number "11")
			)
			(pin passive line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "D8")
				(number "12")
			)
			(pin passive line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "D9")
				(number "13")
			)
			(pin passive line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "D10")
				(number "14")
			)
			(pin passive line
				(at 20.32 -15.24 180)
				(length 3.81)
				(name "D11")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XCR3128XL-VQ100"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 67.31 0)
		)
		(property "Value" "XCR3128XL-VQ100"
			(at -20.32 -67.31 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.xilinx.com/support/documentation/data_sheets/ds016.pdf"
			(at 0 0 0)
		)
		(property "Description" "Xilinx CoolRunner 128-Macrocell CPLD, 3.3V, VQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "CPLD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5*"
			(at 0 0 0)
		)
		(symbol "XCR3128XL-VQ100_1_1"
			(pin passive line
				(at -25.4 63.5 0)
				(length 5.08)
				(name "A1/TDO")
				(number "73")
			)
			(pin passive line
				(at -25.4 60.96 0)
				(length 5.08)
				(name "C1/TCK")
				(number "62")
			)
			(pin passive line
				(at -25.4 58.42 0)
				(length 5.08)
				(name "F1/TDI")
				(number "4")
			)
			(pin passive line
				(at -25.4 55.88 0)
				(length 5.08)
				(name "H1/TMS")
				(number "15")
			)
			(pin passive line
				(at -25.4 53.34 0)
				(length 5.08)
				(name "PORT_EN")
				(number "11")
			)
			(pin passive line
				(at -25.4 50.8 0)
				(length 5.08)
				(name "A2")
				(number "72")
			)
			(pin passive line
				(at -25.4 48.26 0)
				(length 5.08)
				(name "A3")
				(number "71")
			)
			(pin passive line
				(at -25.4 45.72 0)
				(length 5.08)
				(name "A4")
				(number "70")
			)
			(pin passive line
				(at -25.4 43.18 0)
				(length 5.08)
				(name "A5")
				(number "69")
			)
			(pin passive line
				(at -25.4 40.64 0)
				(length 5.08)
				(name "A6")
				(number "68")
			)
			(pin passive line
				(at -25.4 38.1 0)
				(length 5.08)
				(name "A10")
				(number "67")
			)
			(pin passive line
				(at -25.4 35.56 0)
				(length 5.08)
				(name "A12")
				(number "65")
			)
			(pin passive line
				(at -25.4 33.02 0)
				(length 5.08)
				(name "A13")
				(number "64")
			)
			(pin passive line
				(at -25.4 30.48 0)
				(length 5.08)
				(name "A14")
				(number "63")
			)
			(pin passive line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "B0")
				(number "75")
			)
			(pin passive line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "B1")
				(number "76")
			)
			(pin passive line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "B2")
				(number "77")
			)
			(pin passive line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "B3")
				(number "78")
			)
			(pin passive line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "B4")
				(number "79")
			)
			(pin passive line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "B5")
				(number "80")
			)
			(pin passive line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "B6")
				(number "81")
			)
			(pin passive line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "B10")
				(number "83")
			)
			(pin passive line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "B11")
				(number "84")
			)
			(pin passive line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "B12")
				(number "85")
			)
			(pin passive line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "C2")
				(number "61")
			)
			(pin passive line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "C3")
				(number "60")
			)
			(pin passive line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "C5")
				(number "58")
			)
			(pin passive line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "C6")
				(number "57")
			)
			(pin passive line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "C10")
				(number "56")
			)
			(pin passive line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "C11")
				(number "55")
			)
			(pin passive line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "C12")
				(number "54")
			)
			(pin passive line
				(at -25.4 -20.32 0)
				(length 5.08)
				(name "C13")
				(number "53")
			)
			(pin passive line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "C14")
				(number "52")
			)
			(pin input line
				(at -25.4 -27.94 0)
				(length 5.08)
				(name "CLK0/IN0")
				(number "90")
			)
			(pin input line
				(at -25.4 -30.48 0)
				(length 5.08)
				(name "CLK1/IN1")
				(number "89")
			)
			(pin input line
				(at -25.4 -33.02 0)
				(length 5.08)
				(name "CLK2/IN2")
				(number "88")
			)
			(pin input line
				(at -25.4 -35.56 0)
				(length 5.08)
				(name "CLK3/IN3")
				(number "87")
			)
			(pin passive line
				(at -25.4 -40.64 0)
				(length 5.08)
				(name "D1")
				(number "40")
			)
			(pin passive line
				(at -25.4 -43.18 0)
				(length 5.08)
				(name "D2")
				(number "41")
			)
			(pin passive line
				(at -25.4 -45.72 0)
				(length 5.08)
				(name "D3")
				(number "42")
			)
			(pin passive line
				(at -25.4 -48.26 0)
				(length 5.08)
				(name "D4")
				(number "44")
			)
			(pin passive line
				(at -25.4 -50.8 0)
				(length 5.08)
				(name "D5")
				(number "45")
			)
			(pin passive line
				(at -25.4 -53.34 0)
				(length 5.08)
				(name "D6")
				(number "46")
			)
			(pin passive line
				(at -25.4 -55.88 0)
				(length 5.08)
				(name "D10")
				(number "47")
			)
			(pin passive line
				(at -25.4 -58.42 0)
				(length 5.08)
				(name "D11")
				(number "48")
			)
			(pin passive line
				(at -25.4 -60.96 0)
				(length 5.08)
				(name "D12")
				(number "49")
			)
			(pin passive line
				(at -25.4 -63.5 0)
				(length 5.08)
				(name "D13")
				(number "50")
			)
			(pin power_in line
				(at -7.62 71.12 270)
				(length 5.08)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at -7.62 -71.12 90)
				(length 5.08)
				(name "GND")
				(number "26")
			)
			(pin power_in line
				(at -5.08 71.12 270)
				(length 5.08)
				(name "VCC")
				(number "18")
			)
			(pin power_in line
				(at -5.08 -71.12 90)
				(length 5.08)
				(name "GND")
				(number "38")
			)
			(pin power_in line
				(at -2.54 71.12 270)
				(length 5.08)
				(name "VCC")
				(number "34")
			)
			(pin power_in line
				(at -2.54 -71.12 90)
				(length 5.08)
				(name "GND")
				(number "43")
			)
			(pin power_in line
				(at 0 71.12 270)
				(length 5.08)
				(name "VCC")
				(number "39")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "GND")
				(number "59")
			)
			(pin power_in line
				(at 2.54 71.12 270)
				(length 5.08)
				(name "VCC")
				(number "51")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "GND")
				(number "74")
			)
			(pin power_in line
				(at 5.08 71.12 270)
				(length 5.08)
				(name "VCC")
				(number "66")
			)
			(pin power_in line
				(at 5.08 -71.12 90)
				(length 5.08)
				(name "GND")
				(number "86")
			)
			(pin power_in line
				(at 7.62 71.12 270)
				(length 5.08)
				(name "VCC")
				(number "82")
			)
			(pin power_in line
				(at 7.62 -71.12 90)
				(length 5.08)
				(name "GND")
				(number "95")
			)
			(pin power_in line
				(at 10.16 71.12 270)
				(length 5.08)
				(name "VCC")
				(number "91")
			)
			(pin passive line
				(at 25.4 40.64 180)
				(length 5.08)
				(name "H14")
				(number "25")
			)
			(pin passive line
				(at 25.4 38.1 180)
				(length 5.08)
				(name "H13")
				(number "24")
			)
			(pin passive line
				(at 25.4 35.56 180)
				(length 5.08)
				(name "H12")
				(number "23")
			)
			(pin passive line
				(at 25.4 33.02 180)
				(length 5.08)
				(name "H11")
				(number "22")
			)
			(pin passive line
				(at 25.4 30.48 180)
				(length 5.08)
				(name "H10")
				(number "21")
			)
			(pin passive line
				(at 25.4 27.94 180)
				(length 5.08)
				(name "H6")
				(number "20")
			)
			(pin passive line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "H5")
				(number "19")
			)
			(pin passive line
				(at 25.4 22.86 180)
				(length 5.08)
				(name "H3")
				(number "17")
			)
			(pin passive line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "H2")
				(number "16")
			)
			(pin passive line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "G13")
				(number "27")
			)
			(pin passive line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "G12")
				(number "28")
			)
			(pin passive line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "G11")
				(number "29")
			)
			(pin passive line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "G10")
				(number "30")
			)
			(pin passive line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "G6")
				(number "31")
			)
			(pin passive line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "G5")
				(number "32")
			)
			(pin passive line
				(at 25.4 0 180)
				(length 5.08)
				(name "G4")
				(number "33")
			)
			(pin passive line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "G3")
				(number "35")
			)
			(pin passive line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "G2")
				(number "36")
			)
			(pin passive line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "G1")
				(number "37")
			)
			(pin passive line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "F15")
				(number "14")
			)
			(pin passive line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "F14")
				(number "13")
			)
			(pin passive line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "F13")
				(number "12")
			)
			(pin passive line
				(at 25.4 -20.32 180)
				(length 5.08)
				(name "F10")
				(number "10")
			)
			(pin passive line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "F6")
				(number "9")
			)
			(pin passive line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "F5")
				(number "8")
			)
			(pin passive line
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "F4")
				(number "7")
			)
			(pin passive line
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "F3")
				(number "6")
			)
			(pin passive line
				(at 25.4 -33.02 180)
				(length 5.08)
				(name "F2")
				(number "5")
			)
			(pin passive line
				(at 25.4 -38.1 180)
				(length 5.08)
				(name "E14")
				(number "92")
			)
			(pin passive line
				(at 25.4 -40.64 180)
				(length 5.08)
				(name "E13")
				(number "93")
			)
			(pin passive line
				(at 25.4 -43.18 180)
				(length 5.08)
				(name "E12")
				(number "94")
			)
			(pin passive line
				(at 25.4 -45.72 180)
				(length 5.08)
				(name "E6")
				(number "96")
			)
			(pin passive line
				(at 25.4 -48.26 180)
				(length 5.08)
				(name "E5")
				(number "97")
			)
			(pin passive line
				(at 25.4 -50.8 180)
				(length 5.08)
				(name "E4")
				(number "98")
			)
			(pin passive line
				(at 25.4 -53.34 180)
				(length 5.08)
				(name "E3")
				(number "99")
			)
			(pin passive line
				(at 25.4 -55.88 180)
				(length 5.08)
				(name "E2")
				(number "100")
			)
			(pin passive line
				(at 25.4 -58.42 180)
				(length 5.08)
				(name "E1")
				(number "1")
			)
			(pin passive line
				(at 25.4 -60.96 180)
				(length 5.08)
				(name "E0")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XCR3256XL-TQ144"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 87.63 0)
		)
		(property "Value" "XCR3256XL-TQ144"
			(at -25.4 -90.17 0)
		)
		(property "Footprint" "Package_QFP:TQFP-144_20x20mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.xilinx.com/support/documentation/data_sheets/ds013.pdf"
			(at 0 0 0)
		)
		(property "Description" "Xilinx CoolRunner 256-Macrocell CPLD, 3.3V, TQFP-144"
			(at 0 0 0)
		)
		(property "ki_keywords" "CPLD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*20x20mm*P0.5*"
			(at 0 0 0)
		)
		(symbol "XCR3256XL-TQ144_1_1"
			(pin passive line
				(at -30.48 83.82 0)
				(length 5.08)
				(name "A2/TDO")
				(number "104")
			)
			(pin passive line
				(at -30.48 81.28 0)
				(length 5.08)
				(name "E0/TCK")
				(number "89")
			)
			(pin passive line
				(at -30.48 78.74 0)
				(length 5.08)
				(name "J0/TDI")
				(number "4")
			)
			(pin passive line
				(at -30.48 76.2 0)
				(length 5.08)
				(name "N0/TMS")
				(number "20")
			)
			(pin passive line
				(at -30.48 73.66 0)
				(length 5.08)
				(name "PORT_EN")
				(number "13")
			)
			(pin passive line
				(at -30.48 68.58 0)
				(length 5.08)
				(name "A0")
				(number "106")
			)
			(pin passive line
				(at -30.48 66.04 0)
				(length 5.08)
				(name "A3")
				(number "103")
			)
			(pin passive line
				(at -30.48 63.5 0)
				(length 5.08)
				(name "A4")
				(number "102")
			)
			(pin passive line
				(at -30.48 60.96 0)
				(length 5.08)
				(name "A11")
				(number "101")
			)
			(pin passive line
				(at -30.48 58.42 0)
				(length 5.08)
				(name "A12")
				(number "100")
			)
			(pin passive line
				(at -30.48 55.88 0)
				(length 5.08)
				(name "A13")
				(number "99")
			)
			(pin passive line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "B0")
				(number "107")
			)
			(pin passive line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "B1")
				(number "108")
			)
			(pin passive line
				(at -30.48 45.72 0)
				(length 5.08)
				(name "B4")
				(number "109")
			)
			(pin passive line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "B11")
				(number "110")
			)
			(pin passive line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "B12")
				(number "111")
			)
			(pin passive line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "B14")
				(number "112")
			)
			(pin passive line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "B15")
				(number "113")
			)
			(pin passive line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "C0")
				(number "98")
			)
			(pin passive line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "C1")
				(number "97")
			)
			(pin passive line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "C2")
				(number "96")
			)
			(pin passive line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "C3")
				(number "94")
			)
			(pin passive line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "C4")
				(number "93")
			)
			(pin passive line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "C11")
				(number "92")
			)
			(pin passive line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "C13")
				(number "91")
			)
			(pin passive line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "C14")
				(number "90")
			)
			(pin input line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "CLK0/IN0")
				(number "128")
			)
			(pin input line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "CLK1/IN1")
				(number "127")
			)
			(pin input line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "CLK2/IN2")
				(number "126")
			)
			(pin input line
				(at -30.48 0 0)
				(length 5.08)
				(name "CLK3/IN3")
				(number "125")
			)
			(pin passive line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "D0")
				(number "114")
			)
			(pin passive line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "D1")
				(number "116")
			)
			(pin passive line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "D2")
				(number "117")
			)
			(pin passive line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "D4")
				(number "118")
			)
			(pin passive line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "D11")
				(number "119")
			)
			(pin passive line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "D12")
				(number "120")
			)
			(pin passive line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "D13")
				(number "121")
			)
			(pin passive line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "D15")
				(number "122")
			)
			(pin passive line
				(at -30.48 -27.94 0)
				(length 5.08)
				(name "E2")
				(number "88")
			)
			(pin passive line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "E3")
				(number "87")
			)
			(pin passive line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "E4")
				(number "86")
			)
			(pin passive line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "E13")
				(number "83")
			)
			(pin passive line
				(at -30.48 -38.1 0)
				(length 5.08)
				(name "E14")
				(number "82")
			)
			(pin passive line
				(at -30.48 -40.64 0)
				(length 5.08)
				(name "E11")
				(number "84")
			)
			(pin passive line
				(at -30.48 -43.18 0)
				(length 5.08)
				(name "F1")
				(number "55")
			)
			(pin passive line
				(at -30.48 -45.72 0)
				(length 5.08)
				(name "F2")
				(number "56")
			)
			(pin passive line
				(at -30.48 -48.26 0)
				(length 5.08)
				(name "F4")
				(number "60")
			)
			(pin passive line
				(at -30.48 -50.8 0)
				(length 5.08)
				(name "F11")
				(number "61")
			)
			(pin passive line
				(at -30.48 -53.34 0)
				(length 5.08)
				(name "F12")
				(number "62")
			)
			(pin passive line
				(at -30.48 -55.88 0)
				(length 5.08)
				(name "F13")
				(number "63")
			)
			(pin passive line
				(at -30.48 -58.42 0)
				(length 5.08)
				(name "F15")
				(number "65")
			)
			(pin input line
				(at -30.48 -60.96 0)
				(length 5.08)
				(name "G0")
				(number "81")
			)
			(pin passive line
				(at -30.48 -63.5 0)
				(length 5.08)
				(name "G2")
				(number "80")
			)
			(pin passive line
				(at -30.48 -66.04 0)
				(length 5.08)
				(name "G3")
				(number "79")
			)
			(pin passive line
				(at -30.48 -68.58 0)
				(length 5.08)
				(name "G4")
				(number "78")
			)
			(pin passive line
				(at -30.48 -71.12 0)
				(length 5.08)
				(name "G11")
				(number "77")
			)
			(pin passive line
				(at -30.48 -73.66 0)
				(length 5.08)
				(name "G13")
				(number "75")
			)
			(pin passive line
				(at -30.48 -76.2 0)
				(length 5.08)
				(name "G14")
				(number "74")
			)
			(pin passive line
				(at -30.48 -78.74 0)
				(length 5.08)
				(name "H0")
				(number "66")
			)
			(pin passive line
				(at -30.48 -81.28 0)
				(length 5.08)
				(name "H1")
				(number "67")
			)
			(pin passive line
				(at -30.48 -83.82 0)
				(length 5.08)
				(name "H2")
				(number "68")
			)
			(pin passive line
				(at -30.48 -86.36 0)
				(length 5.08)
				(name "H3")
				(number "69")
			)
			(pin power_in line
				(at -12.7 91.44 270)
				(length 5.08)
				(name "VCC")
				(number "24")
			)
			(pin power_in line
				(at -12.7 -93.98 90)
				(length 5.08)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at -10.16 91.44 270)
				(length 5.08)
				(name "VCC")
				(number "50")
			)
			(pin power_in line
				(at -10.16 -93.98 90)
				(length 5.08)
				(name "GND")
				(number "17")
			)
			(pin power_in line
				(at -7.62 91.44 270)
				(length 5.08)
				(name "VCC")
				(number "51")
			)
			(pin power_in line
				(at -7.62 -93.98 90)
				(length 5.08)
				(name "GND")
				(number "33")
			)
			(pin power_in line
				(at -5.08 91.44 270)
				(length 5.08)
				(name "VCC")
				(number "58")
			)
			(pin power_in line
				(at -5.08 -93.98 90)
				(length 5.08)
				(name "GND")
				(number "52")
			)
			(pin power_in line
				(at -2.54 91.44 270)
				(length 5.08)
				(name "VCC")
				(number "73")
			)
			(pin power_in line
				(at -2.54 -93.98 90)
				(length 5.08)
				(name "GND")
				(number "57")
			)
			(pin power_in line
				(at 0 91.44 270)
				(length 5.08)
				(name "VCC")
				(number "76")
			)
			(pin power_in line
				(at 0 -93.98 90)
				(length 5.08)
				(name "GND")
				(number "59")
			)
			(pin power_in line
				(at 2.54 91.44 270)
				(length 5.08)
				(name "VCC")
				(number "95")
			)
			(pin power_in line
				(at 2.54 -93.98 90)
				(length 5.08)
				(name "GND")
				(number "64")
			)
			(pin power_in line
				(at 5.08 91.44 270)
				(length 5.08)
				(name "VCC")
				(number "115")
			)
			(pin power_in line
				(at 5.08 -93.98 90)
				(length 5.08)
				(name "GND")
				(number "85")
			)
			(pin power_in line
				(at 7.62 91.44 270)
				(length 5.08)
				(name "VCC")
				(number "123")
			)
			(pin power_in line
				(at 7.62 -93.98 90)
				(length 5.08)
				(name "GND")
				(number "105")
			)
			(pin power_in line
				(at 10.16 91.44 270)
				(length 5.08)
				(name "VCC")
				(number "130")
			)
			(pin power_in line
				(at 10.16 -93.98 90)
				(length 5.08)
				(name "GND")
				(number "124")
			)
			(pin power_in line
				(at 12.7 91.44 270)
				(length 5.08)
				(name "VCC")
				(number "144")
			)
			(pin power_in line
				(at 12.7 -93.98 90)
				(length 5.08)
				(name "GND")
				(number "129")
			)
			(pin power_in line
				(at 15.24 -93.98 90)
				(length 5.08)
				(name "GND")
				(number "135")
			)
			(pin passive line
				(at 30.48 83.82 180)
				(length 5.08)
				(name "P15")
				(number "36")
			)
			(pin passive line
				(at 30.48 81.28 180)
				(length 5.08)
				(name "P14")
				(number "35")
			)
			(pin passive line
				(at 30.48 78.74 180)
				(length 5.08)
				(name "P13")
				(number "34")
			)
			(pin passive line
				(at 30.48 76.2 180)
				(length 5.08)
				(name "P11")
				(number "32")
			)
			(pin passive line
				(at 30.48 73.66 180)
				(length 5.08)
				(name "P4")
				(number "31")
			)
			(pin passive line
				(at 30.48 71.12 180)
				(length 5.08)
				(name "P3")
				(number "30")
			)
			(pin passive line
				(at 30.48 68.58 180)
				(length 5.08)
				(name "P2")
				(number "29")
			)
			(pin passive line
				(at 30.48 63.5 180)
				(length 5.08)
				(name "O15")
				(number "37")
			)
			(pin passive line
				(at 30.48 60.96 180)
				(length 5.08)
				(name "O13")
				(number "38")
			)
			(pin passive line
				(at 30.48 58.42 180)
				(length 5.08)
				(name "O12")
				(number "39")
			)
			(pin passive line
				(at 30.48 55.88 180)
				(length 5.08)
				(name "O4")
				(number "40")
			)
			(pin passive line
				(at 30.48 53.34 180)
				(length 5.08)
				(name "O3")
				(number "41")
			)
			(pin passive line
				(at 30.48 50.8 180)
				(length 5.08)
				(name "O2")
				(number "42")
			)
			(pin passive line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "O1")
				(number "43")
			)
			(pin passive line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "O0")
				(number "44")
			)
			(pin passive line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "N15")
				(number "28")
			)
			(pin passive line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "N14")
				(number "27")
			)
			(pin passive line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "N13")
				(number "26")
			)
			(pin passive line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "N11")
				(number "25")
			)
			(pin passive line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "N4")
				(number "23")
			)
			(pin passive line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "N3")
				(number "22")
			)
			(pin passive line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "N2")
				(number "21")
			)
			(pin passive line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "M15")
				(number "45")
			)
			(pin passive line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "M13")
				(number "46")
			)
			(pin passive line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "M12")
				(number "47")
			)
			(pin passive line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "M11")
				(number "48")
			)
			(pin passive line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "M4")
				(number "49")
			)
			(pin passive line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "M2")
				(number "53")
			)
			(pin passive line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "M1")
				(number "54")
			)
			(pin passive line
				(at 30.48 0 180)
				(length 5.08)
				(name "L14")
				(number "19")
			)
			(pin passive line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "L13")
				(number "18")
			)
			(pin passive line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "L11")
				(number "16")
			)
			(pin passive line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "L4")
				(number "15")
			)
			(pin passive line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "L3")
				(number "14")
			)
			(pin passive line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "L2")
				(number "12")
			)
			(pin passive line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "K15")
				(number "131")
			)
			(pin passive line
				(at 30.48 -20.32 180)
				(length 5.08)
				(name "K14")
				(number "132")
			)
			(pin passive line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "K13")
				(number "133")
			)
			(pin passive line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "K12")
				(number "134")
			)
			(pin passive line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "K11")
				(number "136")
			)
			(pin passive line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "K4")
				(number "137")
			)
			(pin passive line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "K2")
				(number "138")
			)
			(pin passive line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "J15")
				(number "11")
			)
			(pin passive line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "J14")
				(number "10")
			)
			(pin passive line
				(at 30.48 -43.18 180)
				(length 5.08)
				(name "J13")
				(number "9")
			)
			(pin passive line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "J11")
				(number "8")
			)
			(pin passive line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "J4")
				(number "7")
			)
			(pin passive line
				(at 30.48 -50.8 180)
				(length 5.08)
				(name "J3")
				(number "6")
			)
			(pin passive line
				(at 30.48 -53.34 180)
				(length 5.08)
				(name "J2")
				(number "5")
			)
			(pin passive line
				(at 30.48 -58.42 180)
				(length 5.08)
				(name "I15")
				(number "139")
			)
			(pin passive line
				(at 30.48 -60.96 180)
				(length 5.08)
				(name "I14")
				(number "140")
			)
			(pin passive line
				(at 30.48 -63.5 180)
				(length 5.08)
				(name "I13")
				(number "141")
			)
			(pin passive line
				(at 30.48 -66.04 180)
				(length 5.08)
				(name "I12")
				(number "142")
			)
			(pin passive line
				(at 30.48 -68.58 180)
				(length 5.08)
				(name "I4")
				(number "143")
			)
			(pin passive line
				(at 30.48 -71.12 180)
				(length 5.08)
				(name "I1")
				(number "1")
			)
			(pin passive line
				(at 30.48 -73.66 180)
				(length 5.08)
				(name "I0")
				(number "2")
			)
			(pin passive line
				(at 30.48 -78.74 180)
				(length 5.08)
				(name "H15")
				(number "72")
			)
			(pin passive line
				(at 30.48 -81.28 180)
				(length 5.08)
				(name "H13")
				(number "71")
			)
			(pin passive line
				(at 30.48 -83.82 180)
				(length 5.08)
				(name "H11")
				(number "70")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XCR3064-VQ100"
		(extends "XCR3064XL-VQ100")
		(property "Reference" "U"
			(at -21.59 53.34 0)
		)
		(property "Value" "XCR3064-VQ100"
			(at -21.59 -53.34 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.xilinx.com/support/documentation/data_sheets/ds017.pdf"
			(at 0 0 0)
		)
		(property "Description" "Xilinx CoolRunner 64-Macrocell CPLD, 3.3V, VQFP-100, Obsolete"
			(at 0 0 0)
		)
		(property "ki_keywords" "CPLD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5*"
			(at 0 0 0)
		)
	)
	(symbol "XCR3064-VQ44"
		(extends "XCR3064XL-VQ44")
		(property "Reference" "U"
			(at -16.51 33.02 0)
		)
		(property "Value" "XCR3064-VQ44"
			(at -16.51 -33.02 0)
		)
		(property "Footprint" "Package_QFP:LQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.xilinx.com/support/documentation/data_sheets/ds017.pdf"
			(at 0 0 0)
		)
		(property "Description" "Xilinx CoolRunner 64-Macrocell CPLD, 3.3V, VQFP-44, Obsolete"
			(at 0 0 0)
		)
		(property "ki_keywords" "CPLD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "XCR3128-VQ100"
		(extends "XCR3128XL-VQ100")
		(property "Reference" "U"
			(at -20.32 67.31 0)
		)
		(property "Value" "XCR3128-VQ100"
			(at -20.32 -67.31 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.xilinx.com/support/documentation/data_sheets/ds016.pdf"
			(at 0 0 0)
		)
		(property "Description" "Xilinx CoolRunner 128-Macrocell CPLD, 3.3V, VQFP-100, Obsolete"
			(at 0 0 0)
		)
		(property "ki_keywords" "CPLD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5*"
			(at 0 0 0)
		)
	)
	(symbol "XCR3256-TQ144"
		(extends "XCR3256XL-TQ144")
		(property "Reference" "U"
			(at -25.4 87.63 0)
		)
		(property "Value" "XCR3256-TQ144"
			(at -25.4 -90.17 0)
		)
		(property "Footprint" "Package_QFP:TQFP-144_20x20mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.xilinx.com/support/documentation/data_sheets/ds013.pdf"
			(at 0 0 0)
		)
		(property "Description" "Xilinx CoolRunner 256-Macrocell CPLD, 3.3V, TQFP-144, Obsolete"
			(at 0 0 0)
		)
		(property "ki_keywords" "CPLD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*20x20mm*P0.5*"
			(at 0 0 0)
		)
	)
)
