(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "CDP1802ACE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 34.29 0)
		)
		(property "Value" "CDP1802ACE"
			(at 3.81 34.29 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 48.26 0)
		)
		(property "Datasheet" "http://www.cosmacelf.com/publications/data-sheets/cdp1802.pdf"
			(at 0 50.8 0)
		)
		(property "Description" "8-bit, General Purpose, 5V, 3.2 MHz, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "CPU Processor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "CDP1802ACE_0_1")
		(symbol "CDP1802ACE_1_1"
			(pin input line
				(at -12.7 25.4 0)
				(length 2.54)
				(name "CLOCK")
				(number "1")
			)
			(pin output line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "~{XTAL}")
				(number "39")
			)
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "~{DMA_IN}")
				(number "38")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "~{DMA_OUT}")
				(number "37")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "~{INTERRUPT}")
				(number "36")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "~{EF1}")
				(number "24")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "~{EF2}")
				(number "23")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "~{EF3}")
				(number "22")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{EF4}")
				(number "21")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{CLEAR}")
				(number "3")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "~{WAIT}")
				(number "2")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "BUS0")
				(number "15")
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "BUS1")
				(number "14")
			)
			(pin bidirectional line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "BUS2")
				(number "13")
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "BUS3")
				(number "12")
			)
			(pin bidirectional line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "BUS4")
				(number "11")
			)
			(pin bidirectional line
				(at -12.7 -25.4 0)
				(length 2.54)
				(name "BUS5")
				(number "10")
			)
			(pin bidirectional line
				(at -12.7 -27.94 0)
				(length 2.54)
				(name "BUS6")
				(number "9")
			)
			(pin bidirectional line
				(at -12.7 -30.48 0)
				(length 2.54)
				(name "BUS7")
				(number "8")
			)
			(pin power_in line
				(at -2.54 35.56 270)
				(length 2.54)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "VSS")
				(number "20")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 2.54)
				(name "VDD")
				(number "40")
			)
			(pin output line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "Q")
				(number "4")
			)
			(pin output line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "SC0")
				(number "6")
			)
			(pin output line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "SC1")
				(number "5")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "TPA")
				(number "34")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "TPB")
				(number "33")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "N0")
				(number "19")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "N1")
				(number "18")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "N2")
				(number "17")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "~{MWR}")
				(number "35")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "~{MRD}")
				(number "7")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "MA0")
				(number "25")
			)
			(pin output line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "MA1")
				(number "26")
			)
			(pin output line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "MA2")
				(number "27")
			)
			(pin output line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "MA3")
				(number "28")
			)
			(pin output line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "MA4")
				(number "29")
			)
			(pin output line
				(at 12.7 -25.4 180)
				(length 2.54)
				(name "MA5")
				(number "30")
			)
			(pin output line
				(at 12.7 -27.94 180)
				(length 2.54)
				(name "MA6")
				(number "31")
			)
			(pin output line
				(at 12.7 -30.48 180)
				(length 2.54)
				(name "MA7")
				(number "32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "P4080-BGA1295"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 19.05 0)
		)
		(property "Value" "P4080-BGA1295"
			(at 1.27 16.51 0)
		)
		(property "Footprint" ""
			(at 1.27 3.81 0)
		)
		(property "Datasheet" "https://www.nxp.com/jp/products/microcontrollers-and-processors/power-architecture-processors/qoriq-platforms/p-series/qoriq-p4080-p4040-p4081-multicore-communications-processors:P4080?&tab=Documentation_Tab&linkline=Data-Sheet"
			(at 1.27 3.81 0)
		)
		(property "Description" "QorIQ P4080 Communications Processor, BGA-1295"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "Communications Processor"
			(at 0 0 0)
		)
		(symbol "P4080-BGA1295_1_1"
			(text "DDR SDRAM1"
				(at 1.27 26.67 900)
			)
			(pin bidirectional line
				(at -27.94 99.06 0)
				(length 7.62)
				(name "D1_MDQ0")
				(number "A17")
			)
			(pin bidirectional line
				(at -27.94 96.52 0)
				(length 7.62)
				(name "D1_MDQ1")
				(number "D17")
			)
			(pin bidirectional line
				(at -27.94 93.98 0)
				(length 7.62)
				(name "D1_MDQ2")
				(number "C14")
			)
			(pin bidirectional line
				(at -27.94 91.44 0)
				(length 7.62)
				(name "D1_MDQ3")
				(number "A14")
			)
			(pin bidirectional line
				(at -27.94 88.9 0)
				(length 7.62)
				(name "D1_MDQ4")
				(number "C17")
			)
			(pin bidirectional line
				(at -27.94 86.36 0)
				(length 7.62)
				(name "D1_MDQ5")
				(number "B17")
			)
			(pin bidirectional line
				(at -27.94 83.82 0)
				(length 7.62)
				(name "D1_MDQ6")
				(number "A15")
			)
			(pin bidirectional line
				(at -27.94 81.28 0)
				(length 7.62)
				(name "D1_MDQ7")
				(number "B15")
			)
			(pin bidirectional line
				(at -27.94 78.74 0)
				(length 7.62)
				(name "D1_MDQ8")
				(number "D15")
			)
			(pin bidirectional line
				(at -27.94 76.2 0)
				(length 7.62)
				(name "D1_MDQ9")
				(number "G15")
			)
			(pin bidirectional line
				(at -27.94 73.66 0)
				(length 7.62)
				(name "D1_MDQ10")
				(number "E12")
			)
			(pin bidirectional line
				(at -27.94 71.12 0)
				(length 7.62)
				(name "D1_MDQ11")
				(number "G12")
			)
			(pin bidirectional line
				(at -27.94 68.58 0)
				(length 7.62)
				(name "D1_MDQ12")
				(number "F16")
			)
			(pin bidirectional line
				(at -27.94 66.04 0)
				(length 7.62)
				(name "D1_MDQ13")
				(number "E15")
			)
			(pin bidirectional line
				(at -27.94 63.5 0)
				(length 7.62)
				(name "D1_MDQ14")
				(number "E13")
			)
			(pin bidirectional line
				(at -27.94 60.96 0)
				(length 7.62)
				(name "D1_MDQ15")
				(number "F13")
			)
			(pin bidirectional line
				(at -27.94 58.42 0)
				(length 7.62)
				(name "D1_MDQ16")
				(number "C8")
			)
			(pin bidirectional line
				(at -27.94 55.88 0)
				(length 7.62)
				(name "D1_MDQ17")
				(number "D12")
			)
			(pin bidirectional line
				(at -27.94 53.34 0)
				(length 7.62)
				(name "D1_MDQ18")
				(number "E9")
			)
			(pin bidirectional line
				(at -27.94 50.8 0)
				(length 7.62)
				(name "D1_MDQ19")
				(number "E10")
			)
			(pin bidirectional line
				(at -27.94 48.26 0)
				(length 7.62)
				(name "D1_MDQ20")
				(number "C11")
			)
			(pin bidirectional line
				(at -27.94 45.72 0)
				(length 7.62)
				(name "D1_MDQ21")
				(number "C10")
			)
			(pin bidirectional line
				(at -27.94 43.18 0)
				(length 7.62)
				(name "D1_MDQ22")
				(number "E6")
			)
			(pin bidirectional line
				(at -27.94 40.64 0)
				(length 7.62)
				(name "D1_MDQ23")
				(number "E7")
			)
			(pin bidirectional line
				(at -27.94 38.1 0)
				(length 7.62)
				(name "D1_MDQ24")
				(number "F7")
			)
			(pin bidirectional line
				(at -27.94 35.56 0)
				(length 7.62)
				(name "D1_MDQ25")
				(number "F11")
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 7.62)
				(name "D1_MDQ26")
				(number "H10")
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 7.62)
				(name "D1_MDQ27")
				(number "J10")
			)
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 7.62)
				(name "D1_MDQ28")
				(number "F10")
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 7.62)
				(name "D1_MDQ29")
				(number "F8")
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 7.62)
				(name "D1_MDQ30")
				(number "H7")
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 7.62)
				(name "D1_MDQ31")
				(number "H9")
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 7.62)
				(name "D1_MDQ32")
				(number "AC7")
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 7.62)
				(name "D1_MDQ33")
				(number "AC6")
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 7.62)
				(name "D1_MDQ34")
				(number "AF6")
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 7.62)
				(name "D1_MDQ35")
				(number "AF7")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 7.62)
				(name "D1_MDQ36")
				(number "AB5")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 7.62)
				(name "D1_MDQ37")
				(number "AB6")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 7.62)
				(name "D1_MDQ38")
				(number "AE5")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 7.62)
				(name "D1_MDQ39")
				(number "AE6")
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 7.62)
				(name "D1_MDQ40")
				(number "AG5")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 7.62)
				(name "D1_MDQ41")
				(number "AH9")
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 7.62)
				(name "D1_MDQ42")
				(number "AJ9")
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 7.62)
				(name "D1_MDQ43")
				(number "AJ10")
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 7.62)
				(name "D1_MDQ44")
				(number "AG8")
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 7.62)
				(name "D1_MDQ45")
				(number "AG7")
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 7.62)
				(name "D1_MDQ46")
				(number "AJ6")
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 7.62)
				(name "D1_MDQ47")
				(number "AJ7")
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 7.62)
				(name "D1_MDQ48")
				(number "AL9")
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 7.62)
				(name "D1_MDQ49")
				(number "AL8")
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 7.62)
				(name "D1_MDQ50")
				(number "AN10")
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 7.62)
				(name "D1_MDQ51")
				(number "AN11")
			)
			(pin bidirectional line
				(at -27.94 -33.02 0)
				(length 7.62)
				(name "D1_MDQ52")
				(number "AK8")
			)
			(pin bidirectional line
				(at -27.94 -35.56 0)
				(length 7.62)
				(name "D1_MDQ53")
				(number "AK7")
			)
			(pin bidirectional line
				(at -27.94 -38.1 0)
				(length 7.62)
				(name "D1_MDQ54")
				(number "AN7")
			)
			(pin bidirectional line
				(at -27.94 -40.64 0)
				(length 7.62)
				(name "D1_MDQ55")
				(number "AN8")
			)
			(pin bidirectional line
				(at -27.94 -43.18 0)
				(length 7.62)
				(name "D1_MDQ56")
				(number "AT9")
			)
			(pin bidirectional line
				(at -27.94 -45.72 0)
				(length 7.62)
				(name "D1_MDQ57")
				(number "AR10")
			)
			(pin bidirectional line
				(at -27.94 -48.26 0)
				(length 7.62)
				(name "D1_MDQ58")
				(number "AT13")
			)
			(pin bidirectional line
				(at -27.94 -50.8 0)
				(length 7.62)
				(name "D1_MDQ59")
				(number "AR13")
			)
			(pin bidirectional line
				(at -27.94 -53.34 0)
				(length 7.62)
				(name "D1_MDQ60")
				(number "AP9")
			)
			(pin bidirectional line
				(at -27.94 -55.88 0)
				(length 7.62)
				(name "D1_MDQ61")
				(number "AR9")
			)
			(pin bidirectional line
				(at -27.94 -58.42 0)
				(length 7.62)
				(name "D1_MDQ62")
				(number "AR12")
			)
			(pin bidirectional line
				(at -27.94 -60.96 0)
				(length 7.62)
				(name "D1_MDQ63")
				(number "AP12")
			)
			(pin bidirectional line
				(at -27.94 -64.77 0)
				(length 7.62)
				(name "D1_MECC0")
				(number "K9")
			)
			(pin bidirectional line
				(at -27.94 -67.31 0)
				(length 7.62)
				(name "D1_MECC1")
				(number "J5")
			)
			(pin bidirectional line
				(at -27.94 -69.85 0)
				(length 7.62)
				(name "D1_MECC2")
				(number "L10")
			)
			(pin bidirectional line
				(at -27.94 -72.39 0)
				(length 7.62)
				(name "D1_MECC3")
				(number "M10")
			)
			(pin bidirectional line
				(at -27.94 -74.93 0)
				(length 7.62)
				(name "D1_MECC4")
				(number "J8")
			)
			(pin bidirectional line
				(at -27.94 -77.47 0)
				(length 7.62)
				(name "D1_MECC5")
				(number "J7")
			)
			(pin bidirectional line
				(at -27.94 -80.01 0)
				(length 7.62)
				(name "D1_MECC6")
				(number "L7")
			)
			(pin bidirectional line
				(at -27.94 -82.55 0)
				(length 7.62)
				(name "D1_MECC7")
				(number "L9")
			)
			(pin input line
				(at -27.94 -86.36 0)
				(length 7.62)
				(name "/D1_MAPAR_ERR")
				(number "N8")
			)
			(pin output line
				(at -27.94 -88.9 0)
				(length 7.62)
				(name "D1_MAPAR_OUT")
				(number "Y7")
			)
			(pin bidirectional line
				(at -27.94 -92.71 0)
				(length 7.62)
				(name "D1_MDIC0")
				(number "T6")
			)
			(pin bidirectional line
				(at -27.94 -95.25 0)
				(length 7.62)
				(name "D1_MDIC1")
				(number "AA5")
			)
			(pin output line
				(at 30.48 99.06 180)
				(length 7.62)
				(name "D1_MBA0")
				(number "AA8")
			)
			(pin output line
				(at 30.48 96.52 180)
				(length 7.62)
				(name "D1_MBA1")
				(number "Y10")
			)
			(pin output line
				(at 30.48 93.98 180)
				(length 7.62)
				(name "D1_MBA2")
				(number "M8")
			)
			(pin output line
				(at 30.48 90.17 180)
				(length 7.62)
				(name "D1_MA0")
				(number "Y9")
			)
			(pin output line
				(at 30.48 87.63 180)
				(length 7.62)
				(name "D1_MA1")
				(number "U6")
			)
			(pin output line
				(at 30.48 85.09 180)
				(length 7.62)
				(name "D1_MA2")
				(number "U7")
			)
			(pin output line
				(at 30.48 82.55 180)
				(length 7.62)
				(name "D1_MA3")
				(number "U9")
			)
			(pin output line
				(at 30.48 80.01 180)
				(length 7.62)
				(name "D1_MA4")
				(number "U10")
			)
			(pin output line
				(at 30.48 77.47 180)
				(length 7.62)
				(name "D1_MA5")
				(number "T8")
			)
			(pin output line
				(at 30.48 74.93 180)
				(length 7.62)
				(name "D1_MA6")
				(number "T9")
			)
			(pin output line
				(at 30.48 72.39 180)
				(length 7.62)
				(name "D1_MA7")
				(number "R8")
			)
			(pin output line
				(at 30.48 69.85 180)
				(length 7.62)
				(name "D1_MA8")
				(number "R7")
			)
			(pin output line
				(at 30.48 67.31 180)
				(length 7.62)
				(name "D1_MA9")
				(number "P6")
			)
			(pin output line
				(at 30.48 64.77 180)
				(length 7.62)
				(name "D1_MA10")
				(number "AA7")
			)
			(pin output line
				(at 30.48 62.23 180)
				(length 7.62)
				(name "D1_MA11")
				(number "P7")
			)
			(pin output line
				(at 30.48 59.69 180)
				(length 7.62)
				(name "D1_MA12")
				(number "N6")
			)
			(pin output line
				(at 30.48 57.15 180)
				(length 7.62)
				(name "D1_MA13")
				(number "AE8")
			)
			(pin output line
				(at 30.48 54.61 180)
				(length 7.62)
				(name "D1_MA14")
				(number "M7")
			)
			(pin output line
				(at 30.48 52.07 180)
				(length 7.62)
				(name "D1_MA15")
				(number "L6")
			)
			(pin output line
				(at 30.48 48.26 180)
				(length 7.62)
				(name "/D1_MWE")
				(number "AB8")
			)
			(pin output line
				(at 30.48 45.72 180)
				(length 7.62)
				(name "/D1_MRAS")
				(number "AA10")
			)
			(pin output line
				(at 30.48 43.18 180)
				(length 7.62)
				(name "/D1_MCAS")
				(number "AC10")
			)
			(pin output line
				(at 30.48 39.37 180)
				(length 7.62)
				(name "/D1_MCS0")
				(number "AC9")
			)
			(pin output line
				(at 30.48 36.83 180)
				(length 7.62)
				(name "/D1_MCS1")
				(number "AE9")
			)
			(pin output line
				(at 30.48 34.29 180)
				(length 7.62)
				(name "/D1_MCS2")
				(number "AB9")
			)
			(pin output line
				(at 30.48 31.75 180)
				(length 7.62)
				(name "/D1_MCS3")
				(number "AF9")
			)
			(pin output line
				(at 30.48 27.94 180)
				(length 7.62)
				(name "D1_MCKE0")
				(number "P10")
			)
			(pin output line
				(at 30.48 25.4 180)
				(length 7.62)
				(name "D1_MCKE1")
				(number "R10")
			)
			(pin output line
				(at 30.48 22.86 180)
				(length 7.62)
				(name "D1_MCKE2")
				(number "P9")
			)
			(pin output line
				(at 30.48 20.32 180)
				(length 7.62)
				(name "D1_MCKE3")
				(number "N9")
			)
			(pin output line
				(at 30.48 16.51 180)
				(length 7.62)
				(name "D1_MCK0")
				(number "W6")
			)
			(pin output line
				(at 30.48 13.97 180)
				(length 7.62)
				(name "D1_MCK1")
				(number "V6")
			)
			(pin output line
				(at 30.48 11.43 180)
				(length 7.62)
				(name "D1_MCK2")
				(number "V8")
			)
			(pin output line
				(at 30.48 8.89 180)
				(length 7.62)
				(name "D1_MCK3")
				(number "W9")
			)
			(pin output line
				(at 30.48 6.35 180)
				(length 7.62)
				(name "D1_MCK4")
				(number "F1")
			)
			(pin output line
				(at 30.48 3.81 180)
				(length 7.62)
				(name "D1_MCK5")
				(number "AL1")
			)
			(pin output line
				(at 30.48 0 180)
				(length 7.62)
				(name "/D1_MCK0")
				(number "W5")
			)
			(pin output line
				(at 30.48 -2.54 180)
				(length 7.62)
				(name "/D1_MCK1")
				(number "V5")
			)
			(pin output line
				(at 30.48 -5.08 180)
				(length 7.62)
				(name "/D1_MCK2")
				(number "V9")
			)
			(pin output line
				(at 30.48 -7.62 180)
				(length 7.62)
				(name "/D1_MCK3")
				(number "W8")
			)
			(pin output line
				(at 30.48 -10.16 180)
				(length 7.62)
				(name "/D1_MCK4")
				(number "F2")
			)
			(pin output line
				(at 30.48 -12.7 180)
				(length 7.62)
				(name "/D1_MCK5")
				(number "AL2")
			)
			(pin output line
				(at 30.48 -16.51 180)
				(length 7.62)
				(name "D1_MODT0")
				(number "AD10")
			)
			(pin output line
				(at 30.48 -19.05 180)
				(length 7.62)
				(name "D1_MODT1")
				(number "AG10")
			)
			(pin output line
				(at 30.48 -21.59 180)
				(length 7.62)
				(name "D1_MODT2")
				(number "AD8")
			)
			(pin output line
				(at 30.48 -24.13 180)
				(length 7.62)
				(name "D1_MODT3")
				(number "AF10")
			)
			(pin output line
				(at 30.48 -27.94 180)
				(length 7.62)
				(name "D1_MDM0")
				(number "A16")
			)
			(pin output line
				(at 30.48 -30.48 180)
				(length 7.62)
				(name "D1_MDM1")
				(number "D14")
			)
			(pin output line
				(at 30.48 -33.02 180)
				(length 7.62)
				(name "D1_MDM2")
				(number "D11")
			)
			(pin output line
				(at 30.48 -35.56 180)
				(length 7.62)
				(name "D1_MDM3")
				(number "G11")
			)
			(pin output line
				(at 30.48 -38.1 180)
				(length 7.62)
				(name "D1_MDM4")
				(number "AD7")
			)
			(pin output line
				(at 30.48 -40.64 180)
				(length 7.62)
				(name "D1_MDM5")
				(number "AH8")
			)
			(pin output line
				(at 30.48 -43.18 180)
				(length 7.62)
				(name "D1_MDM6")
				(number "AL11")
			)
			(pin output line
				(at 30.48 -45.72 180)
				(length 7.62)
				(name "D1_MDM7")
				(number "AT10")
			)
			(pin output line
				(at 30.48 -48.26 180)
				(length 7.62)
				(name "D1_MDM8")
				(number "K8")
			)
			(pin bidirectional line
				(at 30.48 -52.07 180)
				(length 7.62)
				(name "D1_MDQS0")
				(number "C16")
			)
			(pin bidirectional line
				(at 30.48 -54.61 180)
				(length 7.62)
				(name "D1_MDQS1")
				(number "G14")
			)
			(pin bidirectional line
				(at 30.48 -57.15 180)
				(length 7.62)
				(name "D1_MDQS2")
				(number "D9")
			)
			(pin bidirectional line
				(at 30.48 -59.69 180)
				(length 7.62)
				(name "D1_MDQS3")
				(number "G9")
			)
			(pin bidirectional line
				(at 30.48 -62.23 180)
				(length 7.62)
				(name "D1_MDQS4")
				(number "AD5")
			)
			(pin bidirectional line
				(at 30.48 -64.77 180)
				(length 7.62)
				(name "D1_MDQS5")
				(number "AH6")
			)
			(pin bidirectional line
				(at 30.48 -67.31 180)
				(length 7.62)
				(name "D1_MDQS6")
				(number "AM10")
			)
			(pin bidirectional line
				(at 30.48 -69.85 180)
				(length 7.62)
				(name "D1_MDQS7")
				(number "AT12")
			)
			(pin bidirectional line
				(at 30.48 -72.39 180)
				(length 7.62)
				(name "D1_MDQS8")
				(number "K6")
			)
			(pin bidirectional line
				(at 30.48 -76.2 180)
				(length 7.62)
				(name "/D1_MDQS0")
				(number "B16")
			)
			(pin bidirectional line
				(at 30.48 -78.74 180)
				(length 7.62)
				(name "/D1_MDQS1")
				(number "F14")
			)
			(pin bidirectional line
				(at 30.48 -81.28 180)
				(length 7.62)
				(name "/D1_MDQS2")
				(number "D8")
			)
			(pin bidirectional line
				(at 30.48 -83.82 180)
				(length 7.62)
				(name "/D1_MDQS3")
				(number "G8")
			)
			(pin bidirectional line
				(at 30.48 -86.36 180)
				(length 7.62)
				(name "/D1_MDQS4")
				(number "AD4")
			)
			(pin bidirectional line
				(at 30.48 -88.9 180)
				(length 7.62)
				(name "/D1_MDQS5")
				(number "AH5")
			)
			(pin bidirectional line
				(at 30.48 -91.44 180)
				(length 7.62)
				(name "/D1_MDQS6")
				(number "AM9")
			)
			(pin bidirectional line
				(at 30.48 -93.98 180)
				(length 7.62)
				(name "/D1_MDQS7")
				(number "AT11")
			)
			(pin bidirectional line
				(at 30.48 -96.52 180)
				(length 7.62)
				(name "/D1_MDQS8")
				(number "K5")
			)
		)
		(symbol "P4080-BGA1295_2_1"
			(text "DDR SDRAM2"
				(at 1.27 26.67 900)
			)
			(pin bidirectional line
				(at -27.94 99.06 0)
				(length 7.62)
				(name "D2_MDQ0")
				(number "C13")
			)
			(pin bidirectional line
				(at -27.94 96.52 0)
				(length 7.62)
				(name "D2_MDQ1")
				(number "A12")
			)
			(pin bidirectional line
				(at -27.94 93.98 0)
				(length 7.62)
				(name "D2_MDQ2")
				(number "B9")
			)
			(pin bidirectional line
				(at -27.94 91.44 0)
				(length 7.62)
				(name "D2_MDQ3")
				(number "A8")
			)
			(pin bidirectional line
				(at -27.94 88.9 0)
				(length 7.62)
				(name "D2_MDQ4")
				(number "A13")
			)
			(pin bidirectional line
				(at -27.94 86.36 0)
				(length 7.62)
				(name "D2_MDQ5")
				(number "B13")
			)
			(pin bidirectional line
				(at -27.94 83.82 0)
				(length 7.62)
				(name "D2_MDQ6")
				(number "B10")
			)
			(pin bidirectional line
				(at -27.94 81.28 0)
				(length 7.62)
				(name "D2_MDQ7")
				(number "A9")
			)
			(pin bidirectional line
				(at -27.94 78.74 0)
				(length 7.62)
				(name "D2_MDQ8")
				(number "A7")
			)
			(pin bidirectional line
				(at -27.94 76.2 0)
				(length 7.62)
				(name "D2_MDQ9")
				(number "D6")
			)
			(pin bidirectional line
				(at -27.94 73.66 0)
				(length 7.62)
				(name "D2_MDQ10")
				(number "A4")
			)
			(pin bidirectional line
				(at -27.94 71.12 0)
				(length 7.62)
				(name "D2_MDQ11")
				(number "B4")
			)
			(pin bidirectional line
				(at -27.94 68.58 0)
				(length 7.62)
				(name "D2_MDQ12")
				(number "C7")
			)
			(pin bidirectional line
				(at -27.94 66.04 0)
				(length 7.62)
				(name "D2_MDQ13")
				(number "B7")
			)
			(pin bidirectional line
				(at -27.94 63.5 0)
				(length 7.62)
				(name "D2_MDQ14")
				(number "C5")
			)
			(pin bidirectional line
				(at -27.94 60.96 0)
				(length 7.62)
				(name "D2_MDQ15")
				(number "D5")
			)
			(pin bidirectional line
				(at -27.94 58.42 0)
				(length 7.62)
				(name "D2_MDQ16")
				(number "B1")
			)
			(pin bidirectional line
				(at -27.94 55.88 0)
				(length 7.62)
				(name "D2_MDQ17")
				(number "B3")
			)
			(pin bidirectional line
				(at -27.94 53.34 0)
				(length 7.62)
				(name "D2_MDQ18")
				(number "D3")
			)
			(pin bidirectional line
				(at -27.94 50.8 0)
				(length 7.62)
				(name "D2_MDQ19")
				(number "E1")
			)
			(pin bidirectional line
				(at -27.94 48.26 0)
				(length 7.62)
				(name "D2_MDQ20")
				(number "A3")
			)
			(pin bidirectional line
				(at -27.94 45.72 0)
				(length 7.62)
				(name "D2_MDQ21")
				(number "A2")
			)
			(pin bidirectional line
				(at -27.94 43.18 0)
				(length 7.62)
				(name "D2_MDQ22")
				(number "D1")
			)
			(pin bidirectional line
				(at -27.94 40.64 0)
				(length 7.62)
				(name "D2_MDQ23")
				(number "D2")
			)
			(pin bidirectional line
				(at -27.94 38.1 0)
				(length 7.62)
				(name "D2_MDQ24")
				(number "F4")
			)
			(pin bidirectional line
				(at -27.94 35.56 0)
				(length 7.62)
				(name "D2_MDQ25")
				(number "F5")
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 7.62)
				(name "D2_MDQ26")
				(number "H4")
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 7.62)
				(name "D2_MDQ27")
				(number "H6")
			)
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 7.62)
				(name "D2_MDQ28")
				(number "E4")
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 7.62)
				(name "D2_MDQ29")
				(number "E3")
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 7.62)
				(name "D2_MDQ30")
				(number "H3")
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 7.62)
				(name "D2_MDQ31")
				(number "H1")
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 7.62)
				(name "D2_MDQ32")
				(number "AG4")
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 7.62)
				(name "D2_MDQ33")
				(number "AG2")
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 7.62)
				(name "D2_MDQ34")
				(number "AJ3")
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 7.62)
				(name "D2_MDQ35")
				(number "AJ1")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 7.62)
				(name "D2_MDQ36")
				(number "AF4")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 7.62)
				(name "D2_MDQ37")
				(number "AF3")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 7.62)
				(name "D2_MDQ38")
				(number "AH1")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 7.62)
				(name "D2_MDQ39")
				(number "AJ4")
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 7.62)
				(name "D2_MDQ40")
				(number "AL6")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 7.62)
				(name "D2_MDQ41")
				(number "AL5")
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 7.62)
				(name "D2_MDQ42")
				(number "AN4")
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 7.62)
				(name "D2_MDQ43")
				(number "AN5")
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 7.62)
				(name "D2_MDQ44")
				(number "AK5")
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 7.62)
				(name "D2_MDQ45")
				(number "AK4")
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 7.62)
				(name "D2_MDQ46")
				(number "AM6")
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 7.62)
				(name "D2_MDQ47")
				(number "AM7")
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 7.62)
				(name "D2_MDQ48")
				(number "AN1")
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 7.62)
				(name "D2_MDQ49")
				(number "AP3")
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 7.62)
				(name "D2_MDQ50")
				(number "AT1")
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 7.62)
				(name "D2_MDQ51")
				(number "AT2")
			)
			(pin bidirectional line
				(at -27.94 -33.02 0)
				(length 7.62)
				(name "D2_MDQ52")
				(number "AM1")
			)
			(pin bidirectional line
				(at -27.94 -35.56 0)
				(length 7.62)
				(name "D2_MDQ53")
				(number "AN2")
			)
			(pin bidirectional line
				(at -27.94 -38.1 0)
				(length 7.62)
				(name "D2_MDQ54")
				(number "AR3")
			)
			(pin bidirectional line
				(at -27.94 -40.64 0)
				(length 7.62)
				(name "D2_MDQ55")
				(number "AT3")
			)
			(pin bidirectional line
				(at -27.94 -43.18 0)
				(length 7.62)
				(name "D2_MDQ56")
				(number "AP5")
			)
			(pin bidirectional line
				(at -27.94 -45.72 0)
				(length 7.62)
				(name "D2_MDQ57")
				(number "AT5")
			)
			(pin bidirectional line
				(at -27.94 -48.26 0)
				(length 7.62)
				(name "D2_MDQ58")
				(number "AP8")
			)
			(pin bidirectional line
				(at -27.94 -50.8 0)
				(length 7.62)
				(name "D2_MDQ59")
				(number "AT8")
			)
			(pin bidirectional line
				(at -27.94 -53.34 0)
				(length 7.62)
				(name "D2_MDQ60")
				(number "AR4")
			)
			(pin bidirectional line
				(at -27.94 -55.88 0)
				(length 7.62)
				(name "D2_MDQ61")
				(number "AT4")
			)
			(pin bidirectional line
				(at -27.94 -58.42 0)
				(length 7.62)
				(name "D2_MDQ62")
				(number "AR7")
			)
			(pin bidirectional line
				(at -27.94 -60.96 0)
				(length 7.62)
				(name "D2_MDQ63")
				(number "AT7")
			)
			(pin bidirectional line
				(at -27.94 -64.77 0)
				(length 7.62)
				(name "D2_MECC0")
				(number "J1")
			)
			(pin bidirectional line
				(at -27.94 -67.31 0)
				(length 7.62)
				(name "D2_MECC1")
				(number "K3")
			)
			(pin bidirectional line
				(at -27.94 -69.85 0)
				(length 7.62)
				(name "D2_MECC2")
				(number "M5")
			)
			(pin bidirectional line
				(at -27.94 -72.39 0)
				(length 7.62)
				(name "D2_MECC3")
				(number "N5")
			)
			(pin bidirectional line
				(at -27.94 -74.93 0)
				(length 7.62)
				(name "D2_MECC4")
				(number "J4")
			)
			(pin bidirectional line
				(at -27.94 -77.47 0)
				(length 7.62)
				(name "D2_MECC5")
				(number "J2")
			)
			(pin bidirectional line
				(at -27.94 -80.01 0)
				(length 7.62)
				(name "D2_MECC6")
				(number "L3")
			)
			(pin bidirectional line
				(at -27.94 -82.55 0)
				(length 7.62)
				(name "D2_MECC7")
				(number "L4")
			)
			(pin input line
				(at -27.94 -86.36 0)
				(length 7.62)
				(name "/D2_MAPA_ERR")
				(number "N2")
			)
			(pin output line
				(at -27.94 -88.9 0)
				(length 7.62)
				(name "D2_MAPAR_OUT")
				(number "Y1")
			)
			(pin bidirectional line
				(at -27.94 -92.71 0)
				(length 7.62)
				(name "D2_MDIC0")
				(number "AA4")
			)
			(pin bidirectional line
				(at -27.94 -95.25 0)
				(length 7.62)
				(name "D2_MDIC1")
				(number "Y6")
			)
			(pin output line
				(at 30.48 99.06 180)
				(length 7.62)
				(name "D2_MBA0")
				(number "AA3")
			)
			(pin output line
				(at 30.48 96.52 180)
				(length 7.62)
				(name "D2_MBA1")
				(number "AA1")
			)
			(pin output line
				(at 30.48 93.98 180)
				(length 7.62)
				(name "D2_MBA2")
				(number "M1")
			)
			(pin output line
				(at 30.48 90.17 180)
				(length 7.62)
				(name "D2_MA0")
				(number "Y4")
			)
			(pin output line
				(at 30.48 87.63 180)
				(length 7.62)
				(name "D2_MA1")
				(number "U1")
			)
			(pin output line
				(at 30.48 85.09 180)
				(length 7.62)
				(name "D2_MA2")
				(number "U4")
			)
			(pin output line
				(at 30.48 82.55 180)
				(length 7.62)
				(name "D2_MA3")
				(number "T1")
			)
			(pin output line
				(at 30.48 80.01 180)
				(length 7.62)
				(name "D2_MA4")
				(number "T2")
			)
			(pin output line
				(at 30.48 77.47 180)
				(length 7.62)
				(name "D2_MA5")
				(number "T3")
			)
			(pin output line
				(at 30.48 74.93 180)
				(length 7.62)
				(name "D2_MA6")
				(number "R1")
			)
			(pin output line
				(at 30.48 72.39 180)
				(length 7.62)
				(name "D2_MA7")
				(number "R4")
			)
			(pin output line
				(at 30.48 69.85 180)
				(length 7.62)
				(name "D2_MA8")
				(number "R2")
			)
			(pin output line
				(at 30.48 67.31 180)
				(length 7.62)
				(name "D2_MA9")
				(number "P1")
			)
			(pin output line
				(at 30.48 64.77 180)
				(length 7.62)
				(name "D2_MA10")
				(number "AA2")
			)
			(pin output line
				(at 30.48 62.23 180)
				(length 7.62)
				(name "D2_MA11")
				(number "P3")
			)
			(pin output line
				(at 30.48 59.69 180)
				(length 7.62)
				(name "D2_MA12")
				(number "N1")
			)
			(pin output line
				(at 30.48 57.15 180)
				(length 7.62)
				(name "D2_MA13")
				(number "AC4")
			)
			(pin output line
				(at 30.48 54.61 180)
				(length 7.62)
				(name "D2_MA14")
				(number "N3")
			)
			(pin output line
				(at 30.48 52.07 180)
				(length 7.62)
				(name "D2_MA15")
				(number "M2")
			)
			(pin output line
				(at 30.48 48.26 180)
				(length 7.62)
				(name "/D2_MWE")
				(number "AB2")
			)
			(pin output line
				(at 30.48 45.72 180)
				(length 7.62)
				(name "/D2_MRAS")
				(number "AB1")
			)
			(pin output line
				(at 30.48 43.18 180)
				(length 7.62)
				(name "/D2_MCAS")
				(number "AC3")
			)
			(pin output line
				(at 30.48 39.37 180)
				(length 7.62)
				(name "/D2_MCS0")
				(number "AC1")
			)
			(pin output line
				(at 30.48 36.83 180)
				(length 7.62)
				(name "/D2_MCS1")
				(number "AE1")
			)
			(pin output line
				(at 30.48 34.29 180)
				(length 7.62)
				(name "/D2_MCS2")
				(number "AB3")
			)
			(pin output line
				(at 30.48 31.75 180)
				(length 7.62)
				(name "/D2_MCS3")
				(number "AE2")
			)
			(pin output line
				(at 30.48 27.94 180)
				(length 7.62)
				(name "D2_MCKE0")
				(number "R5")
			)
			(pin output line
				(at 30.48 25.4 180)
				(length 7.62)
				(name "D2_MCKE1")
				(number "T5")
			)
			(pin output line
				(at 30.48 22.86 180)
				(length 7.62)
				(name "D2_MCKE2")
				(number "P4")
			)
			(pin output line
				(at 30.48 20.32 180)
				(length 7.62)
				(name "D2_MCKE3")
				(number "M4")
			)
			(pin output line
				(at 30.48 16.51 180)
				(length 7.62)
				(name "D2_MCK0")
				(number "W3")
			)
			(pin output line
				(at 30.48 13.97 180)
				(length 7.62)
				(name "D2_MCK1")
				(number "V3")
			)
			(pin output line
				(at 30.48 11.43 180)
				(length 7.62)
				(name "D2_MCK2")
				(number "V1")
			)
			(pin output line
				(at 30.48 8.89 180)
				(length 7.62)
				(name "D2_MCK3")
				(number "W2")
			)
			(pin output line
				(at 30.48 6.35 180)
				(length 7.62)
				(name "D2_MCK4")
				(number "G1")
			)
			(pin output line
				(at 30.48 3.81 180)
				(length 7.62)
				(name "D2_MCK5")
				(number "AK2")
			)
			(pin output line
				(at 30.48 0 180)
				(length 7.62)
				(name "/D2_MCK0")
				(number "W4")
			)
			(pin output line
				(at 30.48 -2.54 180)
				(length 7.62)
				(name "/D2_MCK1")
				(number "V4")
			)
			(pin output line
				(at 30.48 -5.08 180)
				(length 7.62)
				(name "/D2_MCK2")
				(number "V2")
			)
			(pin output line
				(at 30.48 -7.62 180)
				(length 7.62)
				(name "/D2_MCK3")
				(number "W1")
			)
			(pin output line
				(at 30.48 -10.16 180)
				(length 7.62)
				(name "/D2_MCK4")
				(number "G2")
			)
			(pin output line
				(at 30.48 -12.7 180)
				(length 7.62)
				(name "/D2_MCK5")
				(number "AK1")
			)
			(pin output line
				(at 30.48 -16.51 180)
				(length 7.62)
				(name "D2_MODT0")
				(number "AD2")
			)
			(pin output line
				(at 30.48 -19.05 180)
				(length 7.62)
				(name "D2_MODT1")
				(number "AF1")
			)
			(pin output line
				(at 30.48 -21.59 180)
				(length 7.62)
				(name "D2_MODT2")
				(number "AD1")
			)
			(pin output line
				(at 30.48 -24.13 180)
				(length 7.62)
				(name "D2_MODT3")
				(number "AE3")
			)
			(pin output line
				(at 30.48 -27.94 180)
				(length 7.62)
				(name "D2_MDM0")
				(number "B12")
			)
			(pin output line
				(at 30.48 -30.48 180)
				(length 7.62)
				(name "D2_MDM1")
				(number "B6")
			)
			(pin output line
				(at 30.48 -33.02 180)
				(length 7.62)
				(name "D2_MDM2")
				(number "C4")
			)
			(pin output line
				(at 30.48 -35.56 180)
				(length 7.62)
				(name "D2_MDM3")
				(number "G3")
			)
			(pin output line
				(at 30.48 -38.1 180)
				(length 7.62)
				(name "D2_MDM4")
				(number "AG1")
			)
			(pin output line
				(at 30.48 -40.64 180)
				(length 7.62)
				(name "D2_MDM5")
				(number "AL3")
			)
			(pin output line
				(at 30.48 -43.18 180)
				(length 7.62)
				(name "D2_MDM6")
				(number "AP2")
			)
			(pin output line
				(at 30.48 -45.72 180)
				(length 7.62)
				(name "D2_MDM7")
				(number "AP6")
			)
			(pin output line
				(at 30.48 -48.26 180)
				(length 7.62)
				(name "D2_MDM8")
				(number "K2")
			)
			(pin bidirectional line
				(at 30.48 -52.07 180)
				(length 7.62)
				(name "D2_MDQS0")
				(number "A10")
			)
			(pin bidirectional line
				(at 30.48 -54.61 180)
				(length 7.62)
				(name "D2_MDQS1")
				(number "A5")
			)
			(pin bidirectional line
				(at 30.48 -57.15 180)
				(length 7.62)
				(name "D2_MDQS2")
				(number "C2")
			)
			(pin bidirectional line
				(at 30.48 -59.69 180)
				(length 7.62)
				(name "D2_MDQS3")
				(number "G6")
			)
			(pin bidirectional line
				(at 30.48 -62.23 180)
				(length 7.62)
				(name "D2_MDQS4")
				(number "AH2")
			)
			(pin bidirectional line
				(at 30.48 -64.77 180)
				(length 7.62)
				(name "D2_MDQS5")
				(number "AM4")
			)
			(pin bidirectional line
				(at 30.48 -67.31 180)
				(length 7.62)
				(name "D2_MDQS6")
				(number "AR1")
			)
			(pin bidirectional line
				(at 30.48 -69.85 180)
				(length 7.62)
				(name "D2_MDQS7")
				(number "AR6")
			)
			(pin bidirectional line
				(at 30.48 -72.39 180)
				(length 7.62)
				(name "D2_MDQS8")
				(number "L1")
			)
			(pin bidirectional line
				(at 30.48 -76.2 180)
				(length 7.62)
				(name "/D2_MDQS0")
				(number "A11")
			)
			(pin bidirectional line
				(at 30.48 -78.74 180)
				(length 7.62)
				(name "/D2_MDQS1")
				(number "A6")
			)
			(pin bidirectional line
				(at 30.48 -81.28 180)
				(length 7.62)
				(name "/D2_MDQS2")
				(number "C1")
			)
			(pin bidirectional line
				(at 30.48 -83.82 180)
				(length 7.62)
				(name "/D2_MDQS3")
				(number "G5")
			)
			(pin bidirectional line
				(at 30.48 -86.36 180)
				(length 7.62)
				(name "/D2_MDQS4")
				(number "AH3")
			)
			(pin bidirectional line
				(at 30.48 -88.9 180)
				(length 7.62)
				(name "/D2_MDQS5")
				(number "AM3")
			)
			(pin bidirectional line
				(at 30.48 -91.44 180)
				(length 7.62)
				(name "/D2_MDQS6")
				(number "AP1")
			)
			(pin bidirectional line
				(at 30.48 -93.98 180)
				(length 7.62)
				(name "/D2_MDQS7")
				(number "AT6")
			)
			(pin bidirectional line
				(at 30.48 -96.52 180)
				(length 7.62)
				(name "/D2_MDQS8")
				(number "K1")
			)
		)
		(symbol "P4080-BGA1295_3_1"
			(text "PROG INTERRUPT"
				(at -13.97 -5.08 0)
			)
			(text "CONTROLLER"
				(at -13.97 -7.62 0)
			)
			(text "GENERAL-PURPOSE"
				(at -8.89 -64.77 0)
			)
			(text "INPUT/OUTPUT"
				(at -8.89 -68.58 0)
			)
			(text "LOCAL BUS CONTROLLER"
				(at 0 69.85 0)
			)
			(text "INTERFACE"
				(at 0 66.04 0)
			)
			(text "DMA"
				(at 0 7.62 0)
			)
			(pin bidirectional line
				(at -30.48 86.36 0)
				(length 7.62)
				(name "LAD0")
				(number "K26")
			)
			(pin bidirectional line
				(at -30.48 83.82 0)
				(length 7.62)
				(name "LAD1")
				(number "L26")
			)
			(pin bidirectional line
				(at -30.48 81.28 0)
				(length 7.62)
				(name "LAD2")
				(number "J26")
			)
			(pin bidirectional line
				(at -30.48 78.74 0)
				(length 7.62)
				(name "LAD3")
				(number "H25")
			)
			(pin bidirectional line
				(at -30.48 76.2 0)
				(length 7.62)
				(name "LAD4")
				(number "F25")
			)
			(pin bidirectional line
				(at -30.48 73.66 0)
				(length 7.62)
				(name "LAD5")
				(number "H24")
			)
			(pin bidirectional line
				(at -30.48 71.12 0)
				(length 7.62)
				(name "LAD6")
				(number "G24")
			)
			(pin bidirectional line
				(at -30.48 68.58 0)
				(length 7.62)
				(name "LAD7")
				(number "G23")
			)
			(pin bidirectional line
				(at -30.48 66.04 0)
				(length 7.62)
				(name "LAD8")
				(number "E23")
			)
			(pin bidirectional line
				(at -30.48 63.5 0)
				(length 7.62)
				(name "LAD9")
				(number "D23")
			)
			(pin bidirectional line
				(at -30.48 60.96 0)
				(length 7.62)
				(name "LAD10")
				(number "J22")
			)
			(pin bidirectional line
				(at -30.48 58.42 0)
				(length 7.62)
				(name "LAD11")
				(number "G22")
			)
			(pin bidirectional line
				(at -30.48 55.88 0)
				(length 7.62)
				(name "LAD12")
				(number "F19")
			)
			(pin bidirectional line
				(at -30.48 53.34 0)
				(length 7.62)
				(name "LAD13")
				(number "J18")
			)
			(pin bidirectional line
				(at -30.48 50.8 0)
				(length 7.62)
				(name "LAD14")
				(number "K18")
			)
			(pin bidirectional line
				(at -30.48 48.26 0)
				(length 7.62)
				(name "LAD15")
				(number "J17")
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 7.62)
				(name "LDP0")
				(number "J24")
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 7.62)
				(name "LDP1")
				(number "K23")
			)
			(pin output line
				(at -30.48 35.56 0)
				(length 7.62)
				(name "LGPL0")
				(number "B25")
			)
			(pin output line
				(at -30.48 33.02 0)
				(length 7.62)
				(name "LGPL1")
				(number "E25")
			)
			(pin output line
				(at -30.48 30.48 0)
				(length 7.62)
				(name "LGPL2")
				(number "D25")
			)
			(pin output line
				(at -30.48 27.94 0)
				(length 7.62)
				(name "LGPL3")
				(number "H26")
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 7.62)
				(name "LGPL4")
				(number "C25")
			)
			(pin output line
				(at -30.48 22.86 0)
				(length 7.62)
				(name "LGPL5")
				(number "E26")
			)
			(pin output line
				(at -30.48 16.51 0)
				(length 7.62)
				(name "LCLK0")
				(number "C24")
			)
			(pin output line
				(at -30.48 13.97 0)
				(length 7.62)
				(name "LCLK1")
				(number "C23")
			)
			(pin input line
				(at -30.48 -10.16 0)
				(length 7.62)
				(name "IRQ0")
				(number "AJ16")
			)
			(pin input line
				(at -30.48 -12.7 0)
				(length 7.62)
				(name "IRQ1")
				(number "AH16")
			)
			(pin input line
				(at -30.48 -15.24 0)
				(length 7.62)
				(name "IRQ2")
				(number "AK12")
			)
			(pin input line
				(at -30.48 -17.78 0)
				(length 7.62)
				(name "IRQ3/GPIO21")
				(number "AJ15")
			)
			(pin input line
				(at -30.48 -20.32 0)
				(length 7.62)
				(name "IRQ4/GPIO22")
				(number "AH17")
			)
			(pin input line
				(at -30.48 -22.86 0)
				(length 7.62)
				(name "IRQ5/GPIO23")
				(number "AJ13")
			)
			(pin input line
				(at -30.48 -25.4 0)
				(length 7.62)
				(name "IRQ6/GPIO24")
				(number "AG17")
			)
			(pin input line
				(at -30.48 -27.94 0)
				(length 7.62)
				(name "IRQ7/GPIO25")
				(number "AM13")
			)
			(pin input line
				(at -30.48 -30.48 0)
				(length 7.62)
				(name "IRQ8/GPIO26")
				(number "AG13")
			)
			(pin input line
				(at -30.48 -33.02 0)
				(length 7.62)
				(name "IRQ9/GPIO27")
				(number "AK11")
			)
			(pin input line
				(at -30.48 -38.1 0)
				(length 7.62)
				(name "IRQ11/GPIO29")
				(number "AL12")
			)
			(pin output line
				(at -30.48 -41.91 0)
				(length 7.62)
				(name "/IRQ_OUT/EVT9")
				(number "AK14")
			)
			(pin input line
				(at -30.48 -45.72 0)
				(length 7.62)
				(name "/TMP_DETECT")
				(number "AN19")
			)
			(pin output line
				(at 30.48 86.36 180)
				(length 7.62)
				(name "LA16")
				(number "J25")
			)
			(pin output line
				(at 30.48 83.82 180)
				(length 7.62)
				(name "LA17")
				(number "G25")
			)
			(pin output line
				(at 30.48 81.28 180)
				(length 7.62)
				(name "LA18")
				(number "H23")
			)
			(pin output line
				(at 30.48 78.74 180)
				(length 7.62)
				(name "LA19")
				(number "F22")
			)
			(pin output line
				(at 30.48 76.2 180)
				(length 7.62)
				(name "LA20")
				(number "H22")
			)
			(pin output line
				(at 30.48 73.66 180)
				(length 7.62)
				(name "LA21")
				(number "E21")
			)
			(pin output line
				(at 30.48 71.12 180)
				(length 7.62)
				(name "LA22")
				(number "F21")
			)
			(pin output line
				(at 30.48 68.58 180)
				(length 7.62)
				(name "LA23")
				(number "H21")
			)
			(pin output line
				(at 30.48 66.04 180)
				(length 7.62)
				(name "LA24")
				(number "K21")
			)
			(pin output line
				(at 30.48 63.5 180)
				(length 7.62)
				(name "LA25")
				(number "G20")
			)
			(pin output line
				(at 30.48 60.96 180)
				(length 7.62)
				(name "LA26")
				(number "J20")
			)
			(pin output line
				(at 30.48 58.42 180)
				(length 7.62)
				(name "LA27")
				(number "K20")
			)
			(pin output line
				(at 30.48 55.88 180)
				(length 7.62)
				(name "LA28")
				(number "G19")
			)
			(pin output line
				(at 30.48 53.34 180)
				(length 7.62)
				(name "LA29")
				(number "H19")
			)
			(pin output line
				(at 30.48 50.8 180)
				(length 7.62)
				(name "LA30")
				(number "J19")
			)
			(pin output line
				(at 30.48 48.26 180)
				(length 7.62)
				(name "LA31")
				(number "G18")
			)
			(pin output line
				(at 30.48 44.45 180)
				(length 7.62)
				(name "/LCS0")
				(number "D19")
			)
			(pin output line
				(at 30.48 41.91 180)
				(length 7.62)
				(name "/LCS1")
				(number "D20")
			)
			(pin output line
				(at 30.48 39.37 180)
				(length 7.62)
				(name "/LCS2")
				(number "E20")
			)
			(pin output line
				(at 30.48 36.83 180)
				(length 7.62)
				(name "/LCS3")
				(number "D21")
			)
			(pin output line
				(at 30.48 34.29 180)
				(length 7.62)
				(name "/LCS4")
				(number "D22")
			)
			(pin output line
				(at 30.48 31.75 180)
				(length 7.62)
				(name "/LCS5")
				(number "B23")
			)
			(pin output line
				(at 30.48 29.21 180)
				(length 7.62)
				(name "/LCS6")
				(number "F24")
			)
			(pin output line
				(at 30.48 26.67 180)
				(length 7.62)
				(name "/LCS7")
				(number "G26")
			)
			(pin output line
				(at 30.48 22.86 180)
				(length 7.62)
				(name "/LWE0")
				(number "D24")
			)
			(pin output line
				(at 30.48 20.32 180)
				(length 7.62)
				(name "/LWE1")
				(number "A24")
			)
			(pin output line
				(at 30.48 16.51 180)
				(length 7.62)
				(name "LBCTL")
				(number "C22")
			)
			(pin bidirectional line
				(at 30.48 13.97 180)
				(length 7.62)
				(name "LALE")
				(number "A23")
			)
			(pin output line
				(at 30.48 6.35 180)
				(length 7.62)
				(name "/DMA1_DDONE0")
				(number "AN21")
			)
			(pin output line
				(at 30.48 2.54 180)
				(length 7.62)
				(name "/DMA2_DACK0")
				(number "AG19")
			)
			(pin output line
				(at 30.48 0 180)
				(length 7.62)
				(name "/DMA2_DDONE0")
				(number "AP20")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 7.62)
				(name "GPIO0")
				(number "AL21")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 7.62)
				(name "GPIO1")
				(number "AK22")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 7.62)
				(name "GPIO2")
				(number "AM20")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 7.62)
				(name "GPIO3")
				(number "AN20")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 7.62)
				(name "GPIO4")
				(number "AH21")
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 7.62)
				(name "GPIO5")
				(number "AJ21")
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 7.62)
				(name "GPIO6")
				(number "AK21")
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 7.62)
				(name "GPIO7")
				(number "AG20")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 7.62)
				(name "GPIO8/UART1_SOUT")
				(number "AL22")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 7.62)
				(name "GPIO9/UART2_SOUT")
				(number "AJ22")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 7.62)
				(name "GPIO10/UART1_SIN")
				(number "AR23")
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 7.62)
				(name "GPIO11/UART2_SIN")
				(number "AN23")
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 7.62)
				(name "GPIO12/RTS/UART3_SOUT")
				(number "AM22")
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 7.62)
				(name "GPIO13/RTS/UART4_SOUT")
				(number "AK23")
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 7.62)
				(name "GPIO14/CTS/UART3_SIN")
				(number "AP22")
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 7.62)
				(name "GPIO15/CTS/UART4_SIN")
				(number "AH23")
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 7.62)
				(name "GPIO16/IIC3_SCL/SDHC_CD")
				(number "AK13")
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 7.62)
				(name "GPIO17/IIC3_SDA/SDHC_WP")
				(number "AM14")
			)
			(pin bidirectional line
				(at 30.48 -50.8 180)
				(length 7.62)
				(name "GPIO18/DMA1_DREQ0")
				(number "AP21")
			)
			(pin bidirectional line
				(at 30.48 -53.34 180)
				(length 7.62)
				(name "GPIO19/DMA1_DACK0")
				(number "AL19")
			)
			(pin bidirectional line
				(at 30.48 -55.88 180)
				(length 7.62)
				(name "GPIO20/DMA2_DREQ0/ALT_MDVAL")
				(number "AJ20")
			)
			(pin bidirectional line
				(at 30.48 -76.2 180)
				(length 7.62)
				(name "GPIO28/IRQ10")
				(number "AH14")
			)
			(pin bidirectional line
				(at 30.48 -81.28 180)
				(length 7.62)
				(name "GPIO30/TSEC_1588_ALARM_OUT2")
				(number "AK35")
			)
			(pin bidirectional line
				(at 30.48 -83.82 180)
				(length 7.62)
				(name "GPIO31/TSEC_1588_PULSE_OUT2")
				(number "AJ34")
			)
		)
		(symbol "P4080-BGA1295_4_1"
			(text "SERDES"
				(at 0 29.21 0)
			)
			(pin input line
				(at -27.94 55.88 0)
				(length 7.62)
				(name "SD_RX0")
				(number "C28")
			)
			(pin input line
				(at -27.94 53.34 0)
				(length 7.62)
				(name "SD_RX1")
				(number "A29")
			)
			(pin input line
				(at -27.94 50.8 0)
				(length 7.62)
				(name "SD_RX2")
				(number "C30")
			)
			(pin input line
				(at -27.94 48.26 0)
				(length 7.62)
				(name "SD_RX3")
				(number "A31")
			)
			(pin input line
				(at -27.94 45.72 0)
				(length 7.62)
				(name "SD_RX4")
				(number "D36")
			)
			(pin input line
				(at -27.94 43.18 0)
				(length 7.62)
				(name "SD_RX5")
				(number "F36")
			)
			(pin input line
				(at -27.94 40.64 0)
				(length 7.62)
				(name "SD_RX6")
				(number "H36")
			)
			(pin input line
				(at -27.94 38.1 0)
				(length 7.62)
				(name "SD_RX7")
				(number "K36")
			)
			(pin input line
				(at -27.94 35.56 0)
				(length 7.62)
				(name "SD_RX8")
				(number "L34")
			)
			(pin input line
				(at -27.94 33.02 0)
				(length 7.62)
				(name "SD_RX9")
				(number "M36")
			)
			(pin input line
				(at -27.94 30.48 0)
				(length 7.62)
				(name "SD_RX10")
				(number "P36")
			)
			(pin input line
				(at -27.94 27.94 0)
				(length 7.62)
				(name "SD_RX11")
				(number "T34")
			)
			(pin input line
				(at -27.94 25.4 0)
				(length 7.62)
				(name "SD_RX12")
				(number "W36")
			)
			(pin input line
				(at -27.94 22.86 0)
				(length 7.62)
				(name "SD_RX13")
				(number "Y34")
			)
			(pin input line
				(at -27.94 20.32 0)
				(length 7.62)
				(name "SD_RX14")
				(number "AA36")
			)
			(pin input line
				(at -27.94 17.78 0)
				(length 7.62)
				(name "SD_RX15")
				(number "AC36")
			)
			(pin input line
				(at -27.94 15.24 0)
				(length 7.62)
				(name "SD_RX16")
				(number "AF34")
			)
			(pin input line
				(at -27.94 12.7 0)
				(length 7.62)
				(name "SD_RX17")
				(number "AG36")
			)
			(pin input line
				(at -27.94 7.62 0)
				(length 7.62)
				(name "/SD_RX0")
				(number "D28")
			)
			(pin input line
				(at -27.94 5.08 0)
				(length 7.62)
				(name "/SD_RX1")
				(number "B29")
			)
			(pin input line
				(at -27.94 2.54 0)
				(length 7.62)
				(name "/SD_RX2")
				(number "D30")
			)
			(pin input line
				(at -27.94 0 0)
				(length 7.62)
				(name "/SD_RX3")
				(number "B31")
			)
			(pin input line
				(at -27.94 -2.54 0)
				(length 7.62)
				(name "/SD_RX4")
				(number "C36")
			)
			(pin input line
				(at -27.94 -5.08 0)
				(length 7.62)
				(name "/SD_RX5")
				(number "F35")
			)
			(pin input line
				(at -27.94 -7.62 0)
				(length 7.62)
				(name "/SD_RX6")
				(number "H35")
			)
			(pin input line
				(at -27.94 -10.16 0)
				(length 7.62)
				(name "/SD_RX7")
				(number "K35")
			)
			(pin input line
				(at -27.94 -12.7 0)
				(length 7.62)
				(name "/SD_RX8")
				(number "L33")
			)
			(pin input line
				(at -27.94 -15.24 0)
				(length 7.62)
				(name "/SD_RX9")
				(number "M35")
			)
			(pin input line
				(at -27.94 -17.78 0)
				(length 7.62)
				(name "/SD_RX10")
				(number "P35")
			)
			(pin input line
				(at -27.94 -20.32 0)
				(length 7.62)
				(name "/SD_RX11")
				(number "T33")
			)
			(pin input line
				(at -27.94 -22.86 0)
				(length 7.62)
				(name "/SD_RX12")
				(number "W35")
			)
			(pin input line
				(at -27.94 -25.4 0)
				(length 7.62)
				(name "/SD_RX13")
				(number "Y33")
			)
			(pin input line
				(at -27.94 -27.94 0)
				(length 7.62)
				(name "/SD_RX14")
				(number "AA35")
			)
			(pin input line
				(at -27.94 -30.48 0)
				(length 7.62)
				(name "/SD_RX15")
				(number "AC35")
			)
			(pin input line
				(at -27.94 -33.02 0)
				(length 7.62)
				(name "/SD_RX16")
				(number "AF33")
			)
			(pin input line
				(at -27.94 -35.56 0)
				(length 7.62)
				(name "/SD_RX17")
				(number "AG35")
			)
			(pin input line
				(at -27.94 -40.64 0)
				(length 7.62)
				(name "SD_REF_CLK1")
				(number "A35")
			)
			(pin input line
				(at -27.94 -43.18 0)
				(length 7.62)
				(name "/SD_REF_CLK1")
				(number "B35")
			)
			(pin input line
				(at -27.94 -45.72 0)
				(length 7.62)
				(name "SD_REF_CLK2")
				(number "V34")
			)
			(pin input line
				(at -27.94 -48.26 0)
				(length 7.62)
				(name "/SD_REF_CLK2")
				(number "V33")
			)
			(pin input line
				(at -27.94 -50.8 0)
				(length 7.62)
				(name "SD_REF_CLK3")
				(number "AC32")
			)
			(pin input line
				(at -27.94 -53.34 0)
				(length 7.62)
				(name "/SD_REF_CLK3")
				(number "AC31")
			)
			(pin output line
				(at 27.94 55.88 180)
				(length 7.62)
				(name "SD_TX0")
				(number "H28")
			)
			(pin output line
				(at 27.94 53.34 180)
				(length 7.62)
				(name "SD_TX1")
				(number "F29")
			)
			(pin output line
				(at 27.94 50.8 180)
				(length 7.62)
				(name "SD_TX2")
				(number "H30")
			)
			(pin output line
				(at 27.94 48.26 180)
				(length 7.62)
				(name "SD_TX3")
				(number "F31")
			)
			(pin output line
				(at 27.94 45.72 180)
				(length 7.62)
				(name "SD_TX4")
				(number "D34")
			)
			(pin output line
				(at 27.94 43.18 180)
				(length 7.62)
				(name "SD_TX5")
				(number "G33")
			)
			(pin output line
				(at 27.94 40.64 180)
				(length 7.62)
				(name "SD_TX6")
				(number "J33")
			)
			(pin output line
				(at 27.94 38.1 180)
				(length 7.62)
				(name "SD_TX7")
				(number "K31")
			)
			(pin output line
				(at 27.94 35.56 180)
				(length 7.62)
				(name "SD_TX8")
				(number "M31")
			)
			(pin output line
				(at 27.94 33.02 180)
				(length 7.62)
				(name "SD_TX9")
				(number "N33")
			)
			(pin output line
				(at 27.94 30.48 180)
				(length 7.62)
				(name "SD_TX10")
				(number "P31")
			)
			(pin output line
				(at 27.94 27.94 180)
				(length 7.62)
				(name "SD_TX11")
				(number "T30")
			)
			(pin output line
				(at 27.94 25.4 180)
				(length 7.62)
				(name "SD_TX12")
				(number "W31")
			)
			(pin output line
				(at 27.94 22.86 180)
				(length 7.62)
				(name "SD_TX13")
				(number "Y29")
			)
			(pin output line
				(at 27.94 20.32 180)
				(length 7.62)
				(name "SD_TX14")
				(number "AA31")
			)
			(pin output line
				(at 27.94 17.78 180)
				(length 7.62)
				(name "SD_TX15")
				(number "AB33")
			)
			(pin output line
				(at 27.94 15.24 180)
				(length 7.62)
				(name "SD_TX16")
				(number "AE31")
			)
			(pin output line
				(at 27.94 12.7 180)
				(length 7.62)
				(name "SD_TX17")
				(number "AG31")
			)
			(pin output line
				(at 27.94 7.62 180)
				(length 7.62)
				(name "/SD_TX0")
				(number "G28")
			)
			(pin output line
				(at 27.94 5.08 180)
				(length 7.62)
				(name "/SD_TX1")
				(number "E29")
			)
			(pin output line
				(at 27.94 2.54 180)
				(length 7.62)
				(name "/SD_TX2")
				(number "G30")
			)
			(pin output line
				(at 27.94 0 180)
				(length 7.62)
				(name "/SD_TX3")
				(number "E31")
			)
			(pin output line
				(at 27.94 -2.54 180)
				(length 7.62)
				(name "/SD_TX4")
				(number "E34")
			)
			(pin output line
				(at 27.94 -5.08 180)
				(length 7.62)
				(name "/SD_TX5")
				(number "F33")
			)
			(pin output line
				(at 27.94 -7.62 180)
				(length 7.62)
				(name "/SD_TX6")
				(number "J34")
			)
			(pin output line
				(at 27.94 -10.16 180)
				(length 7.62)
				(name "/SD_TX7")
				(number "K32")
			)
			(pin output line
				(at 27.94 -12.7 180)
				(length 7.62)
				(name "/SD_TX8")
				(number "M32")
			)
			(pin output line
				(at 27.94 -15.24 180)
				(length 7.62)
				(name "/SD_TX9")
				(number "N34")
			)
			(pin output line
				(at 27.94 -17.78 180)
				(length 7.62)
				(name "/SD_TX10")
				(number "P32")
			)
			(pin output line
				(at 27.94 -20.32 180)
				(length 7.62)
				(name "/SD_TX11")
				(number "T31")
			)
			(pin output line
				(at 27.94 -22.86 180)
				(length 7.62)
				(name "/SD_TX12")
				(number "W32")
			)
			(pin output line
				(at 27.94 -25.4 180)
				(length 7.62)
				(name "/SD_TX13")
				(number "Y30")
			)
			(pin output line
				(at 27.94 -27.94 180)
				(length 7.62)
				(name "/SD_TX14")
				(number "AA32")
			)
			(pin output line
				(at 27.94 -30.48 180)
				(length 7.62)
				(name "/SD_TX15")
				(number "AB34")
			)
			(pin output line
				(at 27.94 -33.02 180)
				(length 7.62)
				(name "/SD_TX16")
				(number "AE32")
			)
			(pin output line
				(at 27.94 -35.56 180)
				(length 7.62)
				(name "/SD_TX17")
				(number "AG32")
			)
		)
		(symbol "P4080-BGA1295_5_1"
			(text "POWER PINS SERDES"
				(at 0 39.37 900)
			)
			(pin power_in line
				(at -25.4 99.06 0)
				(length 7.62)
				(name "XVDD")
				(number "AA29")
			)
			(pin power_in line
				(at -25.4 96.52 0)
				(length 7.62)
				(name "XVDD")
				(number "AB30")
			)
			(pin power_in line
				(at -25.4 93.98 0)
				(length 7.62)
				(name "XVDD")
				(number "AB31")
			)
			(pin power_in line
				(at -25.4 91.44 0)
				(length 7.62)
				(name "XVDD")
				(number "AC33")
			)
			(pin power_in line
				(at -25.4 88.9 0)
				(length 7.62)
				(name "XVDD")
				(number "AD32")
			)
			(pin power_in line
				(at -25.4 86.36 0)
				(length 7.62)
				(name "XVDD")
				(number "AE30")
			)
			(pin power_in line
				(at -25.4 83.82 0)
				(length 7.62)
				(name "XVDD")
				(number "AF31")
			)
			(pin power_in line
				(at -25.4 81.28 0)
				(length 7.62)
				(name "XVDD")
				(number "E32")
			)
			(pin power_in line
				(at -25.4 78.74 0)
				(length 7.62)
				(name "XVDD")
				(number "E33")
			)
			(pin power_in line
				(at -25.4 76.2 0)
				(length 7.62)
				(name "XVDD")
				(number "F28")
			)
			(pin power_in line
				(at -25.4 73.66 0)
				(length 7.62)
				(name "XVDD")
				(number "F30")
			)
			(pin power_in line
				(at -25.4 71.12 0)
				(length 7.62)
				(name "XVDD")
				(number "G32")
			)
			(pin power_in line
				(at -25.4 68.58 0)
				(length 7.62)
				(name "XVDD")
				(number "H31")
			)
			(pin power_in line
				(at -25.4 66.04 0)
				(length 7.62)
				(name "XVDD")
				(number "H33")
			)
			(pin power_in line
				(at -25.4 63.5 0)
				(length 7.62)
				(name "XVDD")
				(number "J28")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 7.62)
				(name "XVDD")
				(number "J30")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 7.62)
				(name "XVDD")
				(number "J32")
			)
			(pin power_in line
				(at -25.4 55.88 0)
				(length 7.62)
				(name "XVDD")
				(number "K30")
			)
			(pin power_in line
				(at -25.4 53.34 0)
				(length 7.62)
				(name "XVDD")
				(number "L30")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 7.62)
				(name "XVDD")
				(number "L31")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 7.62)
				(name "XVDD")
				(number "M29")
			)
			(pin power_in line
				(at -25.4 45.72 0)
				(length 7.62)
				(name "XVDD")
				(number "N31")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 7.62)
				(name "XVDD")
				(number "P30")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 7.62)
				(name "XVDD")
				(number "P33")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 7.62)
				(name "XVDD")
				(number "R29")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 7.62)
				(name "XVDD")
				(number "R31")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 7.62)
				(name "XVDD")
				(number "T29")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 7.62)
				(name "XVDD")
				(number "T32")
			)
			(pin power_in line
				(at -25.4 27.94 0)
				(length 7.62)
				(name "XVDD")
				(number "U30")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 7.62)
				(name "XVDD")
				(number "V30")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 7.62)
				(name "XVDD")
				(number "V32")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 7.62)
				(name "XVDD")
				(number "W29")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 7.62)
				(name "XVDD")
				(number "Y31")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 7.62)
				(name "XVDD")
				(number "AH32")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 7.62)
				(name "SVDD")
				(number "A30")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 7.62)
				(name "SVDD")
				(number "A34")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 7.62)
				(name "SVDD")
				(number "AA33")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 7.62)
				(name "SVDD")
				(number "AB35")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 7.62)
				(name "SVDD")
				(number "AD36")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 7.62)
				(name "SVDD")
				(number "AE33")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 7.62)
				(name "SVDD")
				(number "AF35")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 7.62)
				(name "SVDD")
				(number "AG34")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 7.62)
				(name "SVDD")
				(number "B28")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 7.62)
				(name "SVDD")
				(number "B32")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 7.62)
				(name "SVDD")
				(number "B36")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 7.62)
				(name "SVDD")
				(number "C31")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 7.62)
				(name "SVDD")
				(number "C34")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 7.62)
				(name "SVDD")
				(number "C35")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 7.62)
				(name "SVDD")
				(number "D29")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 7.62)
				(name "SVDD")
				(number "E36")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 7.62)
				(name "SVDD")
				(number "F34")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 7.62)
				(name "SVDD")
				(number "G35")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 7.62)
				(name "SVDD")
				(number "J36")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 7.62)
				(name "SVDD")
				(number "K34")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 7.62)
				(name "SVDD")
				(number "L35")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 7.62)
				(name "SVDD")
				(number "M33")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 7.62)
				(name "SVDD")
				(number "N36")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 7.62)
				(name "SVDD")
				(number "R34")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 7.62)
				(name "SVDD")
				(number "R35")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 7.62)
				(name "SVDD")
				(number "U33")
			)
			(pin power_in line
				(at -25.4 -66.04 0)
				(length 7.62)
				(name "SVDD")
				(number "V35")
			)
			(pin power_in line
				(at -25.4 -68.58 0)
				(length 7.62)
				(name "SVDD")
				(number "W34")
			)
			(pin power_in line
				(at -25.4 -71.12 0)
				(length 7.62)
				(name "SVDD")
				(number "Y36")
			)
			(pin power_in line
				(at -25.4 -73.66 0)
				(length 7.62)
				(name "SVDD")
				(number "AH36")
			)
			(pin power_in line
				(at -25.4 -83.82 0)
				(length 7.62)
				(name "AVDD_SRDS1")
				(number "A33")
			)
			(pin power_in line
				(at -25.4 -86.36 0)
				(length 7.62)
				(name "AVDD_SRDS2")
				(number "U36")
			)
			(pin power_in line
				(at -25.4 -88.9 0)
				(length 7.62)
				(name "AVDD_SRDS3")
				(number "AE35")
			)
			(pin input line
				(at -25.4 -93.98 0)
				(length 7.62)
				(name "SD_IMP_CAL_TX")
				(number "AF30")
			)
			(pin input line
				(at -25.4 -96.52 0)
				(length 7.62)
				(name "SD_IMP_CAL_RX")
				(number "B27")
			)
			(pin power_in line
				(at 25.4 99.06 180)
				(length 7.62)
				(name "XGND")
				(number "AA30")
			)
			(pin power_in line
				(at 25.4 96.52 180)
				(length 7.62)
				(name "XGND")
				(number "AB32")
			)
			(pin power_in line
				(at 25.4 93.98 180)
				(length 7.62)
				(name "XGND")
				(number "AC30")
			)
			(pin power_in line
				(at 25.4 91.44 180)
				(length 7.62)
				(name "XGND")
				(number "AC34")
			)
			(pin power_in line
				(at 25.4 88.9 180)
				(length 7.62)
				(name "XGND")
				(number "AD30")
			)
			(pin power_in line
				(at 25.4 86.36 180)
				(length 7.62)
				(name "XGND")
				(number "AD31")
			)
			(pin power_in line
				(at 25.4 83.82 180)
				(length 7.62)
				(name "XGND")
				(number "AF32")
			)
			(pin power_in line
				(at 25.4 81.28 180)
				(length 7.62)
				(name "XGND")
				(number "AG30")
			)
			(pin power_in line
				(at 25.4 78.74 180)
				(length 7.62)
				(name "XGND")
				(number "D33")
			)
			(pin power_in line
				(at 25.4 76.2 180)
				(length 7.62)
				(name "XGND")
				(number "E28")
			)
			(pin power_in line
				(at 25.4 73.66 180)
				(length 7.62)
				(name "XGND")
				(number "E30")
			)
			(pin power_in line
				(at 25.4 71.12 180)
				(length 7.62)
				(name "XGND")
				(number "F32")
			)
			(pin power_in line
				(at 25.4 68.58 180)
				(length 7.62)
				(name "XGND")
				(number "G29")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 7.62)
				(name "XGND")
				(number "G31")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 7.62)
				(name "XGND")
				(number "H29")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 7.62)
				(name "XGND")
				(number "H32")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 7.62)
				(name "XGND")
				(number "H34")
			)
			(pin power_in line
				(at 25.4 55.88 180)
				(length 7.62)
				(name "XGND")
				(number "J29")
			)
			(pin power_in line
				(at 25.4 53.34 180)
				(length 7.62)
				(name "XGND")
				(number "J31")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 7.62)
				(name "XGND")
				(number "K28")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 7.62)
				(name "XGND")
				(number "K29")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 7.62)
				(name "XGND")
				(number "L29")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 7.62)
				(name "XGND")
				(number "L32")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 7.62)
				(name "XGND")
				(number "M30")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 7.62)
				(name "XGND")
				(number "N29")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 7.62)
				(name "XGND")
				(number "N30")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 7.62)
				(name "XGND")
				(number "N32")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 7.62)
				(name "XGND")
				(number "P29")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 7.62)
				(name "XGND")
				(number "P34")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 7.62)
				(name "XGND")
				(number "R30")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 7.62)
				(name "XGND")
				(number "R32")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 7.62)
				(name "XGND")
				(number "U29")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 7.62)
				(name "XGND")
				(number "U31")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 7.62)
				(name "XGND")
				(number "V29")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 7.62)
				(name "XGND")
				(number "V31")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 7.62)
				(name "XGND")
				(number "W30")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 7.62)
				(name "XGND")
				(number "Y32")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 7.62)
				(name "XGND")
				(number "AH31")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 7.62)
				(name "SGND")
				(number "A28")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 7.62)
				(name "SGND")
				(number "A32")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 7.62)
				(name "SGND")
				(number "A36")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 7.62)
				(name "SGND")
				(number "AA34")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 7.62)
				(name "SGND")
				(number "AB36")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 7.62)
				(name "SGND")
				(number "AD35")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 7.62)
				(name "SGND")
				(number "AE34")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 7.62)
				(name "SGND")
				(number "AF36")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 7.62)
				(name "SGND")
				(number "AG33")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 7.62)
				(name "SGND")
				(number "B30")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 7.62)
				(name "SGND")
				(number "B34")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 7.62)
				(name "SGND")
				(number "C29")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 7.62)
				(name "SGND")
				(number "C33")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 7.62)
				(name "SGND")
				(number "D31")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 7.62)
				(name "SGND")
				(number "D35")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 7.62)
				(name "SGND")
				(number "E35")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 7.62)
				(name "SGND")
				(number "G34")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 7.62)
				(name "SGND")
				(number "G36")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 7.62)
				(name "SGND")
				(number "J35")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 7.62)
				(name "SGND")
				(number "K33")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 7.62)
				(name "SGND")
				(number "L36")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 7.62)
				(name "SGND")
				(number "M34")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 7.62)
				(name "SGND")
				(number "N35")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 7.62)
				(name "SGND")
				(number "R33")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 7.62)
				(name "SGND")
				(number "R36")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 7.62)
				(name "SGND")
				(number "T35")
			)
			(pin power_in line
				(at 25.4 -66.04 180)
				(length 7.62)
				(name "SGND")
				(number "U34")
			)
			(pin power_in line
				(at 25.4 -68.58 180)
				(length 7.62)
				(name "SGND")
				(number "V36")
			)
			(pin power_in line
				(at 25.4 -71.12 180)
				(length 7.62)
				(name "SGND")
				(number "W33")
			)
			(pin power_in line
				(at 25.4 -73.66 180)
				(length 7.62)
				(name "SGND")
				(number "Y35")
			)
			(pin power_in line
				(at 25.4 -76.2 180)
				(length 7.62)
				(name "SGND")
				(number "AH35")
			)
			(pin power_in line
				(at 25.4 -78.74 180)
				(length 7.62)
				(name "SGND")
				(number "AH33")
			)
			(pin power_in line
				(at 25.4 -83.82 180)
				(length 7.62)
				(name "AGND_SRDS1")
				(number "B33")
			)
			(pin power_in line
				(at 25.4 -86.36 180)
				(length 7.62)
				(name "AGND_SRDS2")
				(number "T36")
			)
			(pin power_in line
				(at 25.4 -88.9 180)
				(length 7.62)
				(name "AGND_SRDS3")
				(number "AE36")
			)
		)
		(symbol "P4080-BGA1295_6_1"
			(text "USB1"
				(at -20.32 82.55 0)
			)
			(text "USB2"
				(at -20.32 58.42 0)
			)
			(text "CLOCK"
				(at -17.78 -63.5 0)
			)
			(text "JTAG"
				(at -17.78 -74.93 0)
			)
			(text "eSDHC"
				(at -15.24 41.91 0)
			)
			(text "I²C INTERFACE"
				(at -15.24 -3.81 0)
			)
			(text "SYSTEM"
				(at -12.7 -86.36 0)
			)
			(text "CONTROL"
				(at -12.7 -88.9 0)
			)
			(text "DEBUG"
				(at -1.27 -39.37 0)
			)
			(text "I/O VOLTAGE SELECT"
				(at 5.08 -69.85 0)
			)
			(text "IEEE 1588"
				(at 6.35 21.59 0)
			)
			(text "DUART"
				(at 6.35 -3.81 0)
			)
			(text "eSPI"
				(at 8.89 41.91 0)
			)
			(text "DFT"
				(at 8.89 -90.17 0)
			)
			(text "I/O VOLT.SELECT"
				(at 10.16 -77.47 0)
			)
			(text "PWR MANAGEMENT"
				(at 11.43 -63.5 0)
			)
			(pin output line
				(at -43.18 96.52 0)
				(length 7.62)
				(name "USB1_STP/EC1_TX_EN")
				(number "AR36")
			)
			(pin input line
				(at -43.18 91.44 0)
				(length 7.62)
				(name "USB1_NXT/EC1_RX_DV")
				(number "AM34")
			)
			(pin input line
				(at -43.18 88.9 0)
				(length 7.62)
				(name "USB1_DIR/EC1_RX_CLK")
				(number "AM36")
			)
			(pin input line
				(at -43.18 86.36 0)
				(length 7.62)
				(name "USB1_CLK/EC1_GTX_CLK")
				(number "AP35")
			)
			(pin output line
				(at -43.18 72.39 0)
				(length 7.62)
				(name "USB2_STP/EC2_TX_EN")
				(number "AR31")
			)
			(pin input line
				(at -43.18 67.31 0)
				(length 7.62)
				(name "USB2_NXT/EC2_RX_DV")
				(number "AR33")
			)
			(pin input line
				(at -43.18 64.77 0)
				(length 7.62)
				(name "USB2_DIR/EC2_RX_CLK")
				(number "AT33")
			)
			(pin input line
				(at -43.18 62.23 0)
				(length 7.62)
				(name "USB2_CLK/EC2_GTX_CLK")
				(number "AN31")
			)
			(pin bidirectional line
				(at -43.18 46.99 0)
				(length 7.62)
				(name "SDHC_CMD")
				(number "AG23")
			)
			(pin bidirectional line
				(at -43.18 44.45 0)
				(length 7.62)
				(name "SDHC_DAT0")
				(number "AP24")
			)
			(pin bidirectional line
				(at -43.18 41.91 0)
				(length 7.62)
				(name "SDHC_DAT1")
				(number "AT24")
			)
			(pin bidirectional line
				(at -43.18 39.37 0)
				(length 7.62)
				(name "SDHC_DAT2")
				(number "AM23")
			)
			(pin bidirectional line
				(at -43.18 36.83 0)
				(length 7.62)
				(name "SDHC_DAT3")
				(number "AG22")
			)
			(pin bidirectional line
				(at -43.18 34.29 0)
				(length 7.62)
				(name "SDHC_DAT4/SPI_CS0")
				(number "AN29")
			)
			(pin bidirectional line
				(at -43.18 31.75 0)
				(length 7.62)
				(name "SDHC_DAT5/SPI_CS1")
				(number "AJ28")
			)
			(pin bidirectional line
				(at -43.18 29.21 0)
				(length 7.62)
				(name "SDHC_DAT6/SPI_CS2")
				(number "AR29")
			)
			(pin bidirectional line
				(at -43.18 26.67 0)
				(length 7.62)
				(name "SDHC_DAT7/SPI_CS3")
				(number "AM29")
			)
			(pin output line
				(at -43.18 22.86 0)
				(length 7.62)
				(name "SDHC_CLK")
				(number "AL23")
			)
			(pin input line
				(at -43.18 10.16 0)
				(length 7.62)
				(name "TSEC_1588_CLK_IN")
				(number "AL35")
			)
			(pin input line
				(at -43.18 7.62 0)
				(length 7.62)
				(name "TSEC_1588_TRIG_IN1C")
				(number "AL36")
			)
			(pin input line
				(at -43.18 5.08 0)
				(length 7.62)
				(name "TSEC_1588_TRIG_IN2")
				(number "AK36")
			)
			(pin bidirectional line
				(at -43.18 -5.08 0)
				(length 7.62)
				(name "IIC1_SCL")
				(number "AH15")
			)
			(pin bidirectional line
				(at -43.18 -7.62 0)
				(length 7.62)
				(name "IIC1_SDA")
				(number "AN14")
			)
			(pin bidirectional line
				(at -43.18 -11.43 0)
				(length 7.62)
				(name "INC2_SCL")
				(number "AM15")
			)
			(pin bidirectional line
				(at -43.18 -13.97 0)
				(length 7.62)
				(name "INC2_SDA")
				(number "AL14")
			)
			(pin bidirectional line
				(at -43.18 -17.78 0)
				(length 7.62)
				(name "IIC3_SCL/GPIO16/SDHC_CD")
				(number "AK13")
			)
			(pin bidirectional line
				(at -43.18 -20.32 0)
				(length 7.62)
				(name "IIC3_SDA/GPIO17/SDHC_WP")
				(number "AM14")
			)
			(pin bidirectional line
				(at -43.18 -24.13 0)
				(length 7.62)
				(name "IIC4_SCL/EVT5")
				(number "AG14")
			)
			(pin bidirectional line
				(at -43.18 -26.67 0)
				(length 7.62)
				(name "IIC4_SDA/EVT6")
				(number "AL15")
			)
			(pin bidirectional line
				(at -43.18 -34.29 0)
				(length 7.62)
				(name "/EVT0")
				(number "AJ17")
			)
			(pin bidirectional line
				(at -43.18 -36.83 0)
				(length 7.62)
				(name "/EVT1")
				(number "AK17")
			)
			(pin bidirectional line
				(at -43.18 -39.37 0)
				(length 7.62)
				(name "/EVT2")
				(number "AN16")
			)
			(pin bidirectional line
				(at -43.18 -41.91 0)
				(length 7.62)
				(name "/EVT3")
				(number "AK16")
			)
			(pin bidirectional line
				(at -43.18 -44.45 0)
				(length 7.62)
				(name "/EVT4")
				(number "AM16")
			)
			(pin bidirectional line
				(at -43.18 -57.15 0)
				(length 7.62)
				(name "/EVT9/IRQ_OUT")
				(number "AK14")
			)
			(pin input line
				(at -43.18 -62.23 0)
				(length 7.62)
				(name "RTC")
				(number "AN24")
			)
			(pin input line
				(at -43.18 -64.77 0)
				(length 7.62)
				(name "SYSCLK")
				(number "AT23")
			)
			(pin input line
				(at -43.18 -69.85 0)
				(length 7.62)
				(name "TCK")
				(number "AR22")
			)
			(pin input line
				(at -43.18 -72.39 0)
				(length 7.62)
				(name "TDI")
				(number "AN17")
			)
			(pin output line
				(at -43.18 -74.93 0)
				(length 7.62)
				(name "TDO")
				(number "AP15")
			)
			(pin input line
				(at -43.18 -77.47 0)
				(length 7.62)
				(name "TMS")
				(number "AR20")
			)
			(pin input line
				(at -43.18 -80.01 0)
				(length 7.62)
				(name "/TRST")
				(number "AR19")
			)
			(pin input line
				(at -43.18 -83.82 0)
				(length 7.62)
				(name "/PORESET")
				(number "AP17")
			)
			(pin bidirectional line
				(at -43.18 -86.36 0)
				(length 7.62)
				(name "/HRESET")
				(number "AR17")
			)
			(pin output line
				(at -43.18 -88.9 0)
				(length 7.62)
				(name "/RESET_REQ")
				(number "AT16")
			)
			(pin output line
				(at -43.18 -91.44 0)
				(length 7.62)
				(name "/CKSTP_OUT")
				(number "AM19")
			)
			(pin bidirectional line
				(at 40.64 96.52 180)
				(length 7.62)
				(name "USB1_D0/EC1_RXD0")
				(number "AN36")
			)
			(pin bidirectional line
				(at 40.64 93.98 180)
				(length 7.62)
				(name "USB1_D0/EC1_RXD1")
				(number "AN35")
			)
			(pin bidirectional line
				(at 40.64 91.44 180)
				(length 7.62)
				(name "USB1_D2/EC1_RXD2")
				(number "AN34")
			)
			(pin bidirectional line
				(at 40.64 88.9 180)
				(length 7.62)
				(name "USB1_D3/EC1_RXD3")
				(number "AM33")
			)
			(pin bidirectional line
				(at 40.64 86.36 180)
				(length 7.62)
				(name "USB1_D4/EC1_TXD0")
				(number "AT35")
			)
			(pin bidirectional line
				(at 40.64 83.82 180)
				(length 7.62)
				(name "USB1_D5/EC1_TXD1")
				(number "AR34")
			)
			(pin bidirectional line
				(at 40.64 81.28 180)
				(length 7.62)
				(name "USB1_D6/EC1_TXD2")
				(number "AT34")
			)
			(pin bidirectional line
				(at 40.64 78.74 180)
				(length 7.62)
				(name "USB1_D7/EC1_TXD3")
				(number "AP36")
			)
			(pin bidirectional line
				(at 40.64 72.39 180)
				(length 7.62)
				(name "USB2_D0/EC2_RXD0")
				(number "AT32")
			)
			(pin bidirectional line
				(at 40.64 69.85 180)
				(length 7.62)
				(name "USB2_D1/EC2_RXD1")
				(number "AP32")
			)
			(pin bidirectional line
				(at 40.64 67.31 180)
				(length 7.62)
				(name "USB2_D2/EC2_RXD2")
				(number "AN32")
			)
			(pin bidirectional line
				(at 40.64 64.77 180)
				(length 7.62)
				(name "USB2_D3/EC2_RXD3")
				(number "AP33")
			)
			(pin bidirectional line
				(at 40.64 62.23 180)
				(length 7.62)
				(name "USB2_D4/EC2_TXD0")
				(number "AT30")
			)
			(pin bidirectional line
				(at 40.64 59.69 180)
				(length 7.62)
				(name "USB2_D5/EC2_TXD1")
				(number "AR30")
			)
			(pin bidirectional line
				(at 40.64 57.15 180)
				(length 7.62)
				(name "USB2_D6/EC2_TXD2")
				(number "AP30")
			)
			(pin bidirectional line
				(at 40.64 54.61 180)
				(length 7.62)
				(name "USB2_D7/EC2_TXD3")
				(number "AT31")
			)
			(pin bidirectional line
				(at 40.64 46.99 180)
				(length 7.62)
				(name "SPI_MOSI")
				(number "AT29")
			)
			(pin input line
				(at 40.64 44.45 180)
				(length 7.62)
				(name "SPI_MISO")
				(number "AH28")
			)
			(pin output line
				(at 40.64 40.64 180)
				(length 7.62)
				(name "SPI_CLK")
				(number "AK29")
			)
			(pin output line
				(at 40.64 19.05 180)
				(length 7.62)
				(name "TSEC_1588_CLK_OUT")
				(number "AM30")
			)
			(pin output line
				(at 40.64 15.24 180)
				(length 7.62)
				(name "TSEC_1588_ALARM_OUT1")
				(number "AJ36")
			)
			(pin output line
				(at 40.64 12.7 180)
				(length 7.62)
				(name "TSEC_1588_ALARM_OUT2/GPIO30")
				(number "AK35")
			)
			(pin output line
				(at 40.64 7.62 180)
				(length 7.62)
				(name "TSEC_1588_PULSE_OUT1")
				(number "AL30")
			)
			(pin output line
				(at 40.64 5.08 180)
				(length 7.62)
				(name "TSEC_1588_PULSE_OUT2/GPIO31")
				(number "AJ34")
			)
			(pin input line
				(at 40.64 -5.08 180)
				(length 7.62)
				(name "UART1_SIN/GPIO10")
				(number "AR23")
			)
			(pin input line
				(at 40.64 -7.62 180)
				(length 7.62)
				(name "UART2_SIN/GPIO11")
				(number "AN23")
			)
			(pin input line
				(at 40.64 -11.43 180)
				(length 7.62)
				(name "UART1_CTS/UART3_SIN/GPIO14")
				(number "AP22")
			)
			(pin input line
				(at 40.64 -13.97 180)
				(length 7.62)
				(name "UART2_CTS/UART4_SIN/GPIO15")
				(number "AH23")
			)
			(pin output line
				(at 40.64 -17.78 180)
				(length 7.62)
				(name "UART1_SDOUT/GPIO8")
				(number "AL22")
			)
			(pin output line
				(at 40.64 -20.32 180)
				(length 7.62)
				(name "UART2_SDOUT/GPIO9")
				(number "AJ22")
			)
			(pin output line
				(at 40.64 -24.13 180)
				(length 7.62)
				(name "UART1_RTS/UART3_SDOUT/GPIO12")
				(number "AM22")
			)
			(pin output line
				(at 40.64 -26.67 180)
				(length 7.62)
				(name "UART2_RTS/UART4_SDOUT/GPIO13")
				(number "AK23")
			)
			(pin output line
				(at 40.64 -34.29 180)
				(length 7.62)
				(name "MDVA")
				(number "AR15")
			)
			(pin output line
				(at 40.64 -38.1 180)
				(length 7.62)
				(name "MSRCID0")
				(number "AH20")
			)
			(pin output line
				(at 40.64 -40.64 180)
				(length 7.62)
				(name "MSRCID1")
				(number "AJ19")
			)
			(pin output line
				(at 40.64 -43.18 180)
				(length 7.62)
				(name "MSRCID2")
				(number "AH18")
			)
			(pin output line
				(at 40.64 -46.99 180)
				(length 7.62)
				(name "ALT_MDVAL/DMA2_DREQ0/GPIO20")
				(number "AJ20")
			)
			(pin output line
				(at 40.64 -49.53 180)
				(length 7.62)
				(name "ALT_MSRCID0/DMA2_DACK0/EVT7")
				(number "AG19")
			)
			(pin output line
				(at 40.64 -52.07 180)
				(length 7.62)
				(name "ALT_MSRCID1/DMA2_DDONE0/EVT8")
				(number "AP20")
			)
			(pin output line
				(at 40.64 -57.15 180)
				(length 7.62)
				(name "CLK_OUT")
				(number "AK20")
			)
			(pin output line
				(at 40.64 -63.5 180)
				(length 7.62)
				(name "ASLEEP")
				(number "AR21")
			)
			(pin input line
				(at 40.64 -72.39 180)
				(length 7.62)
				(name "IO_VSEL0")
				(number "AL18")
			)
			(pin input line
				(at 40.64 -74.93 180)
				(length 7.62)
				(name "IO_VSEL1")
				(number "AP18")
			)
			(pin input line
				(at 40.64 -77.47 180)
				(length 7.62)
				(name "IO_VSEL2")
				(number "AK18")
			)
			(pin input line
				(at 40.64 -80.01 180)
				(length 7.62)
				(name "IO_VSEL3")
				(number "AM18")
			)
			(pin input line
				(at 40.64 -82.55 180)
				(length 7.62)
				(name "IO_VSEL4")
				(number "AH19")
			)
			(pin input line
				(at 40.64 -88.9 180)
				(length 7.62)
				(name "/SCAN_MODE")
				(number "AL17")
			)
			(pin input line
				(at 40.64 -91.44 180)
				(length 7.62)
				(name "/TEST_SEL")
				(number "AT21")
			)
		)
		(symbol "P4080-BGA1295_7_1"
			(text "ETHERNET"
				(at 1.27 26.67 0)
			)
			(pin input line
				(at -33.02 25.4 0)
				(length 7.62)
				(name "EC_GTX_CLK125")
				(number "AK34")
			)
			(pin input line
				(at -33.02 22.86 0)
				(length 7.62)
				(name "EC_XTRNL_TX_STMP1")
				(number "AM31")
			)
			(pin input line
				(at -33.02 20.32 0)
				(length 7.62)
				(name "EC_XTRNL_RX_STMP1")
				(number "AK32")
			)
			(pin input line
				(at -33.02 17.78 0)
				(length 7.62)
				(name "EC_XTRNL_TX_STMP2")
				(number "AJ31")
			)
			(pin input line
				(at -33.02 15.24 0)
				(length 7.62)
				(name "EC_XTRNL_RX_STMP2")
				(number "AK31")
			)
			(pin input line
				(at -33.02 10.16 0)
				(length 7.62)
				(name "EC1_RX_CLK/USB1_DIR")
				(number "AM36")
			)
			(pin input line
				(at -33.02 7.62 0)
				(length 7.62)
				(name "EC1_RX_DV/USB1_NXT")
				(number "AM34")
			)
			(pin input line
				(at -33.02 2.54 0)
				(length 7.62)
				(name "EC1_RXD0/USB1_D0")
				(number "AN36")
			)
			(pin input line
				(at -33.02 0 0)
				(length 7.62)
				(name "EC1_RXD1/USB1_D1")
				(number "AN35")
			)
			(pin input line
				(at -33.02 -2.54 0)
				(length 7.62)
				(name "EC1_RXD2/USB1_D2")
				(number "AN34")
			)
			(pin input line
				(at -33.02 -5.08 0)
				(length 7.62)
				(name "EC1_RXD3/USB1_D3")
				(number "AM33")
			)
			(pin input line
				(at -33.02 -10.16 0)
				(length 7.62)
				(name "EC2_RX_CLK/USB2_DIR")
				(number "AT33")
			)
			(pin input line
				(at -33.02 -12.7 0)
				(length 7.62)
				(name "EC2_RX_DV/USB2_NXT")
				(number "AR33")
			)
			(pin input line
				(at -33.02 -17.78 0)
				(length 7.62)
				(name "EC2_RXD0/USB2_D0")
				(number "AT32")
			)
			(pin input line
				(at -33.02 -20.32 0)
				(length 7.62)
				(name "EC2_RXD1/USB2_D1")
				(number "AP32")
			)
			(pin input line
				(at -33.02 -22.86 0)
				(length 7.62)
				(name "EC2_RXD2/USB2_D2")
				(number "AN32")
			)
			(pin input line
				(at -33.02 -25.4 0)
				(length 7.62)
				(name "EC2_RXD3/USB2_D3")
				(number "AP33")
			)
			(pin output line
				(at 33.02 24.13 180)
				(length 7.62)
				(name "EMI1_MDC")
				(number "AJ33")
			)
			(pin bidirectional line
				(at 33.02 21.59 180)
				(length 7.62)
				(name "EMI1_MDIO")
				(number "AL32")
			)
			(pin output line
				(at 33.02 17.78 180)
				(length 7.62)
				(name "EMI2_MDC")
				(number "AK30")
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 7.62)
				(name "EMI2_MDIO")
				(number "AJ30")
			)
			(pin output line
				(at 33.02 10.16 180)
				(length 7.62)
				(name "EC1_GTX_CLK/USB1_CLK")
				(number "AP35")
			)
			(pin output line
				(at 33.02 7.62 180)
				(length 7.62)
				(name "EC1_TX_EN/USB1_STP")
				(number "AR36")
			)
			(pin output line
				(at 33.02 2.54 180)
				(length 7.62)
				(name "EC1_TXD0/USB1_D4")
				(number "AT35")
			)
			(pin output line
				(at 33.02 0 180)
				(length 7.62)
				(name "EC1_TXD1/USB1_D5")
				(number "AR34")
			)
			(pin output line
				(at 33.02 -2.54 180)
				(length 7.62)
				(name "EC1_TXD2/USB1_D6")
				(number "AT34")
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 7.62)
				(name "EC1_TXD3/USB1_D7")
				(number "AP36")
			)
			(pin output line
				(at 33.02 -10.16 180)
				(length 7.62)
				(name "EC2_GTX_CLK/USB2_CLK")
				(number "AN31")
			)
			(pin output line
				(at 33.02 -12.7 180)
				(length 7.62)
				(name "EC2_TX_EN/USB2_STP")
				(number "AR31")
			)
			(pin output line
				(at 33.02 -17.78 180)
				(length 7.62)
				(name "EC2_TXD0/USB2_D4")
				(number "AT30")
			)
			(pin output line
				(at 33.02 -20.32 180)
				(length 7.62)
				(name "EC2_TXD1/USB2_D5")
				(number "AR30")
			)
			(pin output line
				(at 33.02 -22.86 180)
				(length 7.62)
				(name "EC2_TXD2/USB2_D6")
				(number "AP30")
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 7.62)
				(name "EC2_TXD3/USB2_D7")
				(number "AT31")
			)
		)
		(symbol "P4080-BGA1295_8_1"
			(text "GND PINS"
				(at 0 26.67 0)
			)
			(pin power_in line
				(at -58.42 124.46 0)
				(length 7.62)
				(name "GND")
				(number "AK34")
			)
			(pin power_in line
				(at -58.42 121.92 0)
				(length 7.62)
				(name "GND")
				(number "L12")
			)
			(pin power_in line
				(at -58.42 119.38 0)
				(length 7.62)
				(name "GND")
				(number "AD27")
			)
			(pin power_in line
				(at -58.42 116.84 0)
				(length 7.62)
				(name "GND")
				(number "Y27")
			)
			(pin power_in line
				(at -58.42 114.3 0)
				(length 7.62)
				(name "GND")
				(number "V27")
			)
			(pin power_in line
				(at -58.42 111.76 0)
				(length 7.62)
				(name "GND")
				(number "T27")
			)
			(pin power_in line
				(at -58.42 109.22 0)
				(length 7.62)
				(name "GND")
				(number "M25")
			)
			(pin power_in line
				(at -58.42 106.68 0)
				(length 7.62)
				(name "GND")
				(number "P25")
			)
			(pin power_in line
				(at -58.42 104.14 0)
				(length 7.62)
				(name "GND")
				(number "T25")
			)
			(pin power_in line
				(at -58.42 101.6 0)
				(length 7.62)
				(name "GND")
				(number "V17")
			)
			(pin power_in line
				(at -58.42 99.06 0)
				(length 7.62)
				(name "GND")
				(number "P27")
			)
			(pin power_in line
				(at -58.42 96.52 0)
				(length 7.62)
				(name "GND")
				(number "Y25")
			)
			(pin power_in line
				(at -58.42 93.98 0)
				(length 7.62)
				(name "GND")
				(number "AB25")
			)
			(pin power_in line
				(at -58.42 91.44 0)
				(length 7.62)
				(name "GND")
				(number "AD25")
			)
			(pin power_in line
				(at -58.42 88.9 0)
				(length 7.62)
				(name "GND")
				(number "AF25")
			)
			(pin power_in line
				(at -58.42 86.36 0)
				(length 7.62)
				(name "GND")
				(number "AE24")
			)
			(pin power_in line
				(at -58.42 83.82 0)
				(length 7.62)
				(name "GND")
				(number "AC24")
			)
			(pin power_in line
				(at -58.42 81.28 0)
				(length 7.62)
				(name "GND")
				(number "AA24")
			)
			(pin power_in line
				(at -58.42 78.74 0)
				(length 7.62)
				(name "GND")
				(number "W24")
			)
			(pin power_in line
				(at -58.42 76.2 0)
				(length 7.62)
				(name "GND")
				(number "U24")
			)
			(pin power_in line
				(at -58.42 73.66 0)
				(length 7.62)
				(name "GND")
				(number "R24")
			)
			(pin power_in line
				(at -58.42 71.12 0)
				(length 7.62)
				(name "GND")
				(number "N24")
			)
			(pin power_in line
				(at -58.42 68.58 0)
				(length 7.62)
				(name "GND")
				(number "L24")
			)
			(pin power_in line
				(at -58.42 66.04 0)
				(length 7.62)
				(name "GND")
				(number "M23")
			)
			(pin power_in line
				(at -58.42 63.5 0)
				(length 7.62)
				(name "GND")
				(number "P23")
			)
			(pin power_in line
				(at -58.42 60.96 0)
				(length 7.62)
				(name "GND")
				(number "T23")
			)
			(pin power_in line
				(at -58.42 58.42 0)
				(length 7.62)
				(name "GND")
				(number "V23")
			)
			(pin power_in line
				(at -58.42 55.88 0)
				(length 7.62)
				(name "GND")
				(number "Y23")
			)
			(pin power_in line
				(at -58.42 53.34 0)
				(length 7.62)
				(name "GND")
				(number "AB23")
			)
			(pin power_in line
				(at -58.42 50.8 0)
				(length 7.62)
				(name "GND")
				(number "AD23")
			)
			(pin power_in line
				(at -58.42 48.26 0)
				(length 7.62)
				(name "GND")
				(number "AF23")
			)
			(pin power_in line
				(at -58.42 45.72 0)
				(length 7.62)
				(name "GND")
				(number "N22")
			)
			(pin power_in line
				(at -58.42 43.18 0)
				(length 7.62)
				(name "GND")
				(number "R22")
			)
			(pin power_in line
				(at -58.42 40.64 0)
				(length 7.62)
				(name "GND")
				(number "U22")
			)
			(pin power_in line
				(at -58.42 38.1 0)
				(length 7.62)
				(name "GND")
				(number "W22")
			)
			(pin power_in line
				(at -58.42 35.56 0)
				(length 7.62)
				(name "GND")
				(number "AA22")
			)
			(pin power_in line
				(at -58.42 33.02 0)
				(length 7.62)
				(name "GND")
				(number "AC22")
			)
			(pin power_in line
				(at -58.42 30.48 0)
				(length 7.62)
				(name "GND")
				(number "AE22")
			)
			(pin power_in line
				(at -58.42 27.94 0)
				(length 7.62)
				(name "GND")
				(number "M21")
			)
			(pin power_in line
				(at -58.42 25.4 0)
				(length 7.62)
				(name "GND")
				(number "P21")
			)
			(pin power_in line
				(at -58.42 22.86 0)
				(length 7.62)
				(name "GND")
				(number "T21")
			)
			(pin power_in line
				(at -58.42 20.32 0)
				(length 7.62)
				(name "GND")
				(number "V21")
			)
			(pin power_in line
				(at -58.42 17.78 0)
				(length 7.62)
				(name "GND")
				(number "Y21")
			)
			(pin power_in line
				(at -58.42 15.24 0)
				(length 7.62)
				(name "GND")
				(number "AB21")
			)
			(pin power_in line
				(at -58.42 12.7 0)
				(length 7.62)
				(name "GND")
				(number "AD21")
			)
			(pin power_in line
				(at -58.42 10.16 0)
				(length 7.62)
				(name "GND")
				(number "AF21")
			)
			(pin power_in line
				(at -58.42 7.62 0)
				(length 7.62)
				(name "GND")
				(number "W20")
			)
			(pin power_in line
				(at -58.42 5.08 0)
				(length 7.62)
				(name "GND")
				(number "AC20")
			)
			(pin power_in line
				(at -58.42 2.54 0)
				(length 7.62)
				(name "GND")
				(number "AA20")
			)
			(pin power_in line
				(at -58.42 0 0)
				(length 7.62)
				(name "GND")
				(number "AE20")
			)
			(pin power_in line
				(at -58.42 -2.54 0)
				(length 7.62)
				(name "GND")
				(number "U20")
			)
			(pin power_in line
				(at -58.42 -5.08 0)
				(length 7.62)
				(name "GND")
				(number "R20")
			)
			(pin power_in line
				(at -58.42 -7.62 0)
				(length 7.62)
				(name "GND")
				(number "N20")
			)
			(pin power_in line
				(at -58.42 -10.16 0)
				(length 7.62)
				(name "GND")
				(number "M19")
			)
			(pin power_in line
				(at -58.42 -12.7 0)
				(length 7.62)
				(name "GND")
				(number "P19")
			)
			(pin power_in line
				(at -58.42 -15.24 0)
				(length 7.62)
				(name "GND")
				(number "T19")
			)
			(pin power_in line
				(at -58.42 -17.78 0)
				(length 7.62)
				(name "GND")
				(number "V19")
			)
			(pin power_in line
				(at -58.42 -20.32 0)
				(length 7.62)
				(name "GND")
				(number "Y19")
			)
			(pin power_in line
				(at -58.42 -22.86 0)
				(length 7.62)
				(name "GND")
				(number "AB19")
			)
			(pin power_in line
				(at -58.42 -25.4 0)
				(length 7.62)
				(name "GND")
				(number "AD19")
			)
			(pin power_in line
				(at -58.42 -27.94 0)
				(length 7.62)
				(name "GND")
				(number "AF19")
			)
			(pin power_in line
				(at -58.42 -30.48 0)
				(length 7.62)
				(name "GND")
				(number "AE18")
			)
			(pin power_in line
				(at -58.42 -33.02 0)
				(length 7.62)
				(name "GND")
				(number "AA18")
			)
			(pin power_in line
				(at -58.42 -35.56 0)
				(length 7.62)
				(name "GND")
				(number "AC18")
			)
			(pin power_in line
				(at -58.42 -38.1 0)
				(length 7.62)
				(name "GND")
				(number "W18")
			)
			(pin power_in line
				(at -58.42 -40.64 0)
				(length 7.62)
				(name "GND")
				(number "AF17")
			)
			(pin power_in line
				(at -58.42 -43.18 0)
				(length 7.62)
				(name "GND")
				(number "AD17")
			)
			(pin power_in line
				(at -58.42 -45.72 0)
				(length 7.62)
				(name "GND")
				(number "AB17")
			)
			(pin power_in line
				(at -58.42 -48.26 0)
				(length 7.62)
				(name "GND")
				(number "Y17")
			)
			(pin power_in line
				(at -58.42 -50.8 0)
				(length 7.62)
				(name "GND")
				(number "U18")
			)
			(pin power_in line
				(at -58.42 -53.34 0)
				(length 7.62)
				(name "GND")
				(number "R18")
			)
			(pin power_in line
				(at -58.42 -55.88 0)
				(length 7.62)
				(name "GND")
				(number "N18")
			)
			(pin power_in line
				(at -58.42 -58.42 0)
				(length 7.62)
				(name "GND")
				(number "T17")
			)
			(pin power_in line
				(at -58.42 -60.96 0)
				(length 7.62)
				(name "GND")
				(number "P17")
			)
			(pin power_in line
				(at -58.42 -63.5 0)
				(length 7.62)
				(name "GND")
				(number "M17")
			)
			(pin power_in line
				(at -58.42 -66.04 0)
				(length 7.62)
				(name "GND")
				(number "N16")
			)
			(pin power_in line
				(at -58.42 -68.58 0)
				(length 7.62)
				(name "GND")
				(number "R16")
			)
			(pin power_in line
				(at -58.42 -71.12 0)
				(length 7.62)
				(name "GND")
				(number "U16")
			)
			(pin power_in line
				(at -58.42 -73.66 0)
				(length 7.62)
				(name "GND")
				(number "AE16")
			)
			(pin power_in line
				(at -58.42 -76.2 0)
				(length 7.62)
				(name "GND")
				(number "AA16")
			)
			(pin power_in line
				(at -58.42 -78.74 0)
				(length 7.62)
				(name "GND")
				(number "AC16")
			)
			(pin power_in line
				(at -58.42 -81.28 0)
				(length 7.62)
				(name "GND")
				(number "W16")
			)
			(pin power_in line
				(at -58.42 -83.82 0)
				(length 7.62)
				(name "GND")
				(number "AF15")
			)
			(pin power_in line
				(at -58.42 -86.36 0)
				(length 7.62)
				(name "GND")
				(number "AD15")
			)
			(pin power_in line
				(at -58.42 -88.9 0)
				(length 7.62)
				(name "GND")
				(number "AB15")
			)
			(pin power_in line
				(at -58.42 -91.44 0)
				(length 7.62)
				(name "GND")
				(number "Y15")
			)
			(pin power_in line
				(at -58.42 -93.98 0)
				(length 7.62)
				(name "GND")
				(number "V15")
			)
			(pin power_in line
				(at -58.42 -96.52 0)
				(length 7.62)
				(name "GND")
				(number "T15")
			)
			(pin power_in line
				(at -58.42 -99.06 0)
				(length 7.62)
				(name "GND")
				(number "P15")
			)
			(pin power_in line
				(at -58.42 -101.6 0)
				(length 7.62)
				(name "GND")
				(number "M15")
			)
			(pin power_in line
				(at -58.42 -104.14 0)
				(length 7.62)
				(name "GND")
				(number "L14")
			)
			(pin power_in line
				(at -58.42 -106.68 0)
				(length 7.62)
				(name "GND")
				(number "N14")
			)
			(pin power_in line
				(at -58.42 -109.22 0)
				(length 7.62)
				(name "GND")
				(number "R14")
			)
			(pin power_in line
				(at -58.42 -111.76 0)
				(length 7.62)
				(name "GND")
				(number "U14")
			)
			(pin power_in line
				(at -58.42 -114.3 0)
				(length 7.62)
				(name "GND")
				(number "W14")
			)
			(pin power_in line
				(at -58.42 -116.84 0)
				(length 7.62)
				(name "GND")
				(number "AA14")
			)
			(pin power_in line
				(at -58.42 -119.38 0)
				(length 7.62)
				(name "GND")
				(number "AC14")
			)
			(pin power_in line
				(at -58.42 -121.92 0)
				(length 7.62)
				(name "GND")
				(number "AE14")
			)
			(pin power_in line
				(at -43.18 134.62 270)
				(length 7.62)
				(name "GND")
				(number "C3")
			)
			(pin power_in line
				(at -40.64 134.62 270)
				(length 7.62)
				(name "GND")
				(number "B5")
			)
			(pin power_in line
				(at -38.1 134.62 270)
				(length 7.62)
				(name "GND")
				(number "F3")
			)
			(pin power_in line
				(at -35.56 134.62 270)
				(length 7.62)
				(name "GND")
				(number "E5")
			)
			(pin power_in line
				(at -33.02 134.62 270)
				(length 7.62)
				(name "GND")
				(number "D7")
			)
			(pin power_in line
				(at -30.48 134.62 270)
				(length 7.62)
				(name "GND")
				(number "C9")
			)
			(pin power_in line
				(at -27.94 134.62 270)
				(length 7.62)
				(name "GND")
				(number "B11")
			)
			(pin power_in line
				(at -25.4 134.62 270)
				(length 7.62)
				(name "GND")
				(number "J3")
			)
			(pin power_in line
				(at -22.86 134.62 270)
				(length 7.62)
				(name "GND")
				(number "H5")
			)
			(pin power_in line
				(at -20.32 134.62 270)
				(length 7.62)
				(name "GND")
				(number "G7")
			)
			(pin power_in line
				(at -17.78 134.62 270)
				(length 7.62)
				(name "GND")
				(number "F9")
			)
			(pin power_in line
				(at -15.24 134.62 270)
				(length 7.62)
				(name "GND")
				(number "E11")
			)
			(pin power_in line
				(at -12.7 134.62 270)
				(length 7.62)
				(name "GND")
				(number "D13")
			)
			(pin power_in line
				(at -10.16 134.62 270)
				(length 7.62)
				(name "GND")
				(number "C15")
			)
			(pin power_in line
				(at -7.62 134.62 270)
				(length 7.62)
				(name "GND")
				(number "K19")
			)
			(pin power_in line
				(at -5.08 134.62 270)
				(length 7.62)
				(name "GND")
				(number "B20")
			)
			(pin power_in line
				(at -2.54 134.62 270)
				(length 7.62)
				(name "GND")
				(number "B22")
			)
			(pin power_in line
				(at 0 134.62 270)
				(length 7.62)
				(name "GND")
				(number "E19")
			)
			(pin power_in line
				(at 2.54 134.62 270)
				(length 7.62)
				(name "GND")
				(number "L22")
			)
			(pin power_in line
				(at 5.08 134.62 270)
				(length 7.62)
				(name "GND")
				(number "J23")
			)
			(pin power_in line
				(at 7.62 134.62 270)
				(length 7.62)
				(name "GND")
				(number "A22")
			)
			(pin power_in line
				(at 10.16 134.62 270)
				(length 7.62)
				(name "GND")
				(number "L20")
			)
			(pin power_in line
				(at 12.7 134.62 270)
				(length 7.62)
				(name "GND")
				(number "A26")
			)
			(pin power_in line
				(at 15.24 134.62 270)
				(length 7.62)
				(name "GND")
				(number "A18")
			)
			(pin power_in line
				(at 17.78 134.62 270)
				(length 7.62)
				(name "GND")
				(number "E17")
			)
			(pin power_in line
				(at 20.32 134.62 270)
				(length 7.62)
				(name "GND")
				(number "F23")
			)
			(pin power_in line
				(at 22.86 134.62 270)
				(length 7.62)
				(name "GND")
				(number "J27")
			)
			(pin power_in line
				(at 25.4 134.62 270)
				(length 7.62)
				(name "GND")
				(number "F27")
			)
			(pin power_in line
				(at 27.94 134.62 270)
				(length 7.62)
				(name "GND")
				(number "G21")
			)
			(pin power_in line
				(at 30.48 134.62 270)
				(length 7.62)
				(name "GND")
				(number "K25")
			)
			(pin power_in line
				(at 33.02 134.62 270)
				(length 7.62)
				(name "GND")
				(number "B18")
			)
			(pin power_in line
				(at 35.56 134.62 270)
				(length 7.62)
				(name "GND")
				(number "L18")
			)
			(pin power_in line
				(at 38.1 134.62 270)
				(length 7.62)
				(name "GND")
				(number "J21")
			)
			(pin power_in line
				(at 40.64 134.62 270)
				(length 7.62)
				(name "GND")
				(number "M27")
			)
			(pin power_in line
				(at 43.18 134.62 270)
				(length 7.62)
				(name "GND")
				(number "G13")
			)
			(pin power_in line
				(at 58.42 124.46 180)
				(length 7.62)
				(name "GND")
				(number "F15")
			)
			(pin power_in line
				(at 58.42 121.92 180)
				(length 7.62)
				(name "GND")
				(number "H11")
			)
			(pin power_in line
				(at 58.42 119.38 180)
				(length 7.62)
				(name "GND")
				(number "J9")
			)
			(pin power_in line
				(at 58.42 116.84 180)
				(length 7.62)
				(name "GND")
				(number "K7")
			)
			(pin power_in line
				(at 58.42 114.3 180)
				(length 7.62)
				(name "GND")
				(number "L5")
			)
			(pin power_in line
				(at 58.42 111.76 180)
				(length 7.62)
				(name "GND")
				(number "M3")
			)
			(pin power_in line
				(at 58.42 109.22 180)
				(length 7.62)
				(name "GND")
				(number "R3")
			)
			(pin power_in line
				(at 58.42 106.68 180)
				(length 7.62)
				(name "GND")
				(number "P5")
			)
			(pin power_in line
				(at 58.42 104.14 180)
				(length 7.62)
				(name "GND")
				(number "N7")
			)
			(pin power_in line
				(at 58.42 101.6 180)
				(length 7.62)
				(name "GND")
				(number "M9")
			)
			(pin power_in line
				(at 58.42 99.06 180)
				(length 7.62)
				(name "GND")
				(number "V25")
			)
			(pin power_in line
				(at 58.42 96.52 180)
				(length 7.62)
				(name "GND")
				(number "R9")
			)
			(pin power_in line
				(at 58.42 93.98 180)
				(length 7.62)
				(name "GND")
				(number "T7")
			)
			(pin power_in line
				(at 58.42 91.44 180)
				(length 7.62)
				(name "GND")
				(number "U5")
			)
			(pin power_in line
				(at 58.42 88.9 180)
				(length 7.62)
				(name "GND")
				(number "U3")
			)
			(pin power_in line
				(at 58.42 86.36 180)
				(length 7.62)
				(name "GND")
				(number "Y3")
			)
			(pin power_in line
				(at 58.42 83.82 180)
				(length 7.62)
				(name "GND")
				(number "Y5")
			)
			(pin power_in line
				(at 58.42 81.28 180)
				(length 7.62)
				(name "GND")
				(number "W7")
			)
			(pin power_in line
				(at 58.42 78.74 180)
				(length 7.62)
				(name "GND")
				(number "V10")
			)
			(pin power_in line
				(at 58.42 76.2 180)
				(length 7.62)
				(name "GND")
				(number "AA9")
			)
			(pin power_in line
				(at 58.42 73.66 180)
				(length 7.62)
				(name "GND")
				(number "AB7")
			)
			(pin power_in line
				(at 58.42 71.12 180)
				(length 7.62)
				(name "GND")
				(number "AC5")
			)
			(pin power_in line
				(at 58.42 68.58 180)
				(length 7.62)
				(name "GND")
				(number "AD3")
			)
			(pin power_in line
				(at 58.42 66.04 180)
				(length 7.62)
				(name "GND")
				(number "AD9")
			)
			(pin power_in line
				(at 58.42 63.5 180)
				(length 7.62)
				(name "GND")
				(number "AE7")
			)
			(pin power_in line
				(at 58.42 60.96 180)
				(length 7.62)
				(name "GND")
				(number "AF5")
			)
			(pin power_in line
				(at 58.42 58.42 180)
				(length 7.62)
				(name "GND")
				(number "AG3")
			)
			(pin power_in line
				(at 58.42 55.88 180)
				(length 7.62)
				(name "GND")
				(number "AG9")
			)
			(pin power_in line
				(at 58.42 53.34 180)
				(length 7.62)
				(name "GND")
				(number "AH7")
			)
			(pin power_in line
				(at 58.42 50.8 180)
				(length 7.62)
				(name "GND")
				(number "AJ5")
			)
			(pin power_in line
				(at 58.42 48.26 180)
				(length 7.62)
				(name "GND")
				(number "AK3")
			)
			(pin power_in line
				(at 58.42 45.72 180)
				(length 7.62)
				(name "GND")
				(number "AN3")
			)
			(pin power_in line
				(at 58.42 43.18 180)
				(length 7.62)
				(name "GND")
				(number "AM5")
			)
			(pin power_in line
				(at 58.42 40.64 180)
				(length 7.62)
				(name "GND")
				(number "AL7")
			)
			(pin power_in line
				(at 58.42 38.1 180)
				(length 7.62)
				(name "GND")
				(number "AK9")
			)
			(pin power_in line
				(at 58.42 35.56 180)
				(length 7.62)
				(name "GND")
				(number "AJ11")
			)
			(pin power_in line
				(at 58.42 33.02 180)
				(length 7.62)
				(name "GND")
				(number "AH13")
			)
			(pin power_in line
				(at 58.42 30.48 180)
				(length 7.62)
				(name "GND")
				(number "AR5")
			)
			(pin power_in line
				(at 58.42 27.94 180)
				(length 7.62)
				(name "GND")
				(number "AP7")
			)
			(pin power_in line
				(at 58.42 25.4 180)
				(length 7.62)
				(name "GND")
				(number "AN9")
			)
			(pin power_in line
				(at 58.42 22.86 180)
				(length 7.62)
				(name "GND")
				(number "AM11")
			)
			(pin power_in line
				(at 58.42 20.32 180)
				(length 7.62)
				(name "GND")
				(number "AL13")
			)
			(pin power_in line
				(at 58.42 17.78 180)
				(length 7.62)
				(name "GND")
				(number "AK15")
			)
			(pin power_in line
				(at 58.42 15.24 180)
				(length 7.62)
				(name "GND")
				(number "AG18")
			)
			(pin power_in line
				(at 58.42 12.7 180)
				(length 7.62)
				(name "GND")
				(number "AR11")
			)
			(pin power_in line
				(at 58.42 10.16 180)
				(length 7.62)
				(name "GND")
				(number "AP13")
			)
			(pin power_in line
				(at 58.42 7.62 180)
				(length 7.62)
				(name "GND")
				(number "AN15")
			)
			(pin power_in line
				(at 58.42 5.08 180)
				(length 7.62)
				(name "GND")
				(number "AM17")
			)
			(pin power_in line
				(at 58.42 2.54 180)
				(length 7.62)
				(name "GND")
				(number "AK19")
			)
			(pin power_in line
				(at 58.42 0 180)
				(length 7.62)
				(name "GND")
				(number "AF13")
			)
			(pin power_in line
				(at 58.42 -2.54 180)
				(length 7.62)
				(name "GND")
				(number "AR18")
			)
			(pin power_in line
				(at 58.42 -5.08 180)
				(length 7.62)
				(name "GND")
				(number "AB27")
			)
			(pin power_in line
				(at 58.42 -7.62 180)
				(length 7.62)
				(name "GND")
				(number "AP19")
			)
			(pin power_in line
				(at 58.42 -10.16 180)
				(length 7.62)
				(name "GND")
				(number "AH22")
			)
			(pin power_in line
				(at 58.42 -12.7 180)
				(length 7.62)
				(name "GND")
				(number "AM21")
			)
			(pin power_in line
				(at 58.42 -15.24 180)
				(length 7.62)
				(name "GND")
				(number "AL29")
			)
			(pin power_in line
				(at 58.42 -17.78 180)
				(length 7.62)
				(name "GND")
				(number "AR16")
			)
			(pin power_in line
				(at 58.42 -20.32 180)
				(length 7.62)
				(name "GND")
				(number "AT22")
			)
			(pin power_in line
				(at 58.42 -22.86 180)
				(length 7.62)
				(name "GND")
				(number "AP23")
			)
			(pin power_in line
				(at 58.42 -25.4 180)
				(length 7.62)
				(name "GND")
				(number "AR32")
			)
			(pin power_in line
				(at 58.42 -27.94 180)
				(length 7.62)
				(name "GND")
				(number "AK28")
			)
			(pin power_in line
				(at 58.42 -30.48 180)
				(length 7.62)
				(name "GND")
				(number "AE27")
			)
			(pin power_in line
				(at 58.42 -33.02 180)
				(length 7.62)
				(name "GND")
				(number "L16")
			)
			(pin power_in line
				(at 58.42 -35.56 180)
				(length 7.62)
				(name "GND")
				(number "AP34")
			)
			(pin power_in line
				(at 58.42 -38.1 180)
				(length 7.62)
				(name "GND")
				(number "AJ32")
			)
			(pin power_in line
				(at 58.42 -40.64 180)
				(length 7.62)
				(name "GND")
				(number "AN30")
			)
			(pin power_in line
				(at 58.42 -43.18 180)
				(length 7.62)
				(name "GND")
				(number "AH34")
			)
			(pin power_in line
				(at 58.42 -45.72 180)
				(length 7.62)
				(name "GND")
				(number "AT36")
			)
			(pin power_in line
				(at 58.42 -48.26 180)
				(length 7.62)
				(name "GND")
				(number "AL34")
			)
			(pin power_in line
				(at 58.42 -50.8 180)
				(length 7.62)
				(name "GND")
				(number "AM32")
			)
			(pin power_in line
				(at 58.42 -53.34 180)
				(length 7.62)
				(name "GND")
				(number "AE26")
			)
			(pin power_in line
				(at 58.42 -55.88 180)
				(length 7.62)
				(name "GND")
				(number "AC26")
			)
			(pin power_in line
				(at 58.42 -58.42 180)
				(length 7.62)
				(name "GND")
				(number "AA26")
			)
			(pin power_in line
				(at 58.42 -60.96 180)
				(length 7.62)
				(name "GND")
				(number "W26")
			)
			(pin power_in line
				(at 58.42 -63.5 180)
				(length 7.62)
				(name "GND")
				(number "U26")
			)
			(pin power_in line
				(at 58.42 -66.04 180)
				(length 7.62)
				(name "GND")
				(number "R26")
			)
			(pin power_in line
				(at 58.42 -68.58 180)
				(length 7.62)
				(name "GND")
				(number "N26")
			)
			(pin power_in line
				(at 58.42 -71.12 180)
				(length 7.62)
				(name "GND")
				(number "M11")
			)
			(pin power_in line
				(at 58.42 -73.66 180)
				(length 7.62)
				(name "GND")
				(number "P11")
			)
			(pin power_in line
				(at 58.42 -76.2 180)
				(length 7.62)
				(name "GND")
				(number "T11")
			)
			(pin power_in line
				(at 58.42 -78.74 180)
				(length 7.62)
				(name "GND")
				(number "V11")
			)
			(pin power_in line
				(at 58.42 -81.28 180)
				(length 7.62)
				(name "GND")
				(number "Y11")
			)
			(pin power_in line
				(at 58.42 -83.82 180)
				(length 7.62)
				(name "GND")
				(number "AB11")
			)
			(pin power_in line
				(at 58.42 -86.36 180)
				(length 7.62)
				(name "GND")
				(number "AD11")
			)
			(pin power_in line
				(at 58.42 -88.9 180)
				(length 7.62)
				(name "GND")
				(number "AE12")
			)
			(pin power_in line
				(at 58.42 -91.44 180)
				(length 7.62)
				(name "GND")
				(number "AC12")
			)
			(pin power_in line
				(at 58.42 -93.98 180)
				(length 7.62)
				(name "GND")
				(number "AA12")
			)
			(pin power_in line
				(at 58.42 -96.52 180)
				(length 7.62)
				(name "GND")
				(number "W12")
			)
			(pin power_in line
				(at 58.42 -99.06 180)
				(length 7.62)
				(name "GND")
				(number "U12")
			)
			(pin power_in line
				(at 58.42 -101.6 180)
				(length 7.62)
				(name "GND")
				(number "R12")
			)
			(pin power_in line
				(at 58.42 -104.14 180)
				(length 7.62)
				(name "GND")
				(number "N12")
			)
			(pin power_in line
				(at 58.42 -106.68 180)
				(length 7.62)
				(name "GND")
				(number "M13")
			)
			(pin power_in line
				(at 58.42 -109.22 180)
				(length 7.62)
				(name "GND")
				(number "P13")
			)
			(pin power_in line
				(at 58.42 -111.76 180)
				(length 7.62)
				(name "GND")
				(number "T13")
			)
			(pin power_in line
				(at 58.42 -114.3 180)
				(length 7.62)
				(name "GND")
				(number "V13")
			)
			(pin power_in line
				(at 58.42 -116.84 180)
				(length 7.62)
				(name "GND")
				(number "Y13")
			)
			(pin power_in line
				(at 58.42 -119.38 180)
				(length 7.62)
				(name "GND")
				(number "AB13")
			)
			(pin power_in line
				(at 58.42 -121.92 180)
				(length 7.62)
				(name "GND")
				(number "AD13")
			)
		)
		(symbol "P4080-BGA1295_9_1"
			(text "POWER PINS"
				(at 0 36.83 900)
			)
			(pin power_in line
				(at -25.4 86.36 0)
				(length 7.62)
				(name "GVDD")
				(number "B2")
			)
			(pin power_in line
				(at -25.4 83.82 0)
				(length 7.62)
				(name "GVDD")
				(number "B8")
			)
			(pin power_in line
				(at -25.4 81.28 0)
				(length 7.62)
				(name "GVDD")
				(number "B14")
			)
			(pin power_in line
				(at -25.4 78.74 0)
				(length 7.62)
				(name "GVDD")
				(number "C18")
			)
			(pin power_in line
				(at -25.4 76.2 0)
				(length 7.62)
				(name "GVDD")
				(number "C12")
			)
			(pin power_in line
				(at -25.4 73.66 0)
				(length 7.62)
				(name "GVDD")
				(number "C6")
			)
			(pin power_in line
				(at -25.4 71.12 0)
				(length 7.62)
				(name "GVDD")
				(number "D4")
			)
			(pin power_in line
				(at -25.4 68.58 0)
				(length 7.62)
				(name "GVDD")
				(number "D10")
			)
			(pin power_in line
				(at -25.4 66.04 0)
				(length 7.62)
				(name "GVDD")
				(number "D16")
			)
			(pin power_in line
				(at -25.4 63.5 0)
				(length 7.62)
				(name "GVDD")
				(number "E14")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 7.62)
				(name "GVDD")
				(number "E8")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 7.62)
				(name "GVDD")
				(number "E2")
			)
			(pin power_in line
				(at -25.4 55.88 0)
				(length 7.62)
				(name "GVDD")
				(number "F6")
			)
			(pin power_in line
				(at -25.4 53.34 0)
				(length 7.62)
				(name "GVDD")
				(number "F12")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 7.62)
				(name "GVDD")
				(number "AR8")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 7.62)
				(name "GVDD")
				(number "G4")
			)
			(pin power_in line
				(at -25.4 45.72 0)
				(length 7.62)
				(name "GVDD")
				(number "G10")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 7.62)
				(name "GVDD")
				(number "G16")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 7.62)
				(name "GVDD")
				(number "H14")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 7.62)
				(name "GVDD")
				(number "H8")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 7.62)
				(name "GVDD")
				(number "H2")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 7.62)
				(name "GVDD")
				(number "J6")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 7.62)
				(name "GVDD")
				(number "K10")
			)
			(pin power_in line
				(at -25.4 27.94 0)
				(length 7.62)
				(name "GVDD")
				(number "K4")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 7.62)
				(name "GVDD")
				(number "L2")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 7.62)
				(name "GVDD")
				(number "L8")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 7.62)
				(name "GVDD")
				(number "M6")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 7.62)
				(name "GVDD")
				(number "N4")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 7.62)
				(name "GVDD")
				(number "N10")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 7.62)
				(name "GVDD")
				(number "P8")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 7.62)
				(name "GVDD")
				(number "P2")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 7.62)
				(name "GVDD")
				(number "R6")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 7.62)
				(name "GVDD")
				(number "T10")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 7.62)
				(name "GVDD")
				(number "T4")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 7.62)
				(name "GVDD")
				(number "J12")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 7.62)
				(name "GVDD")
				(number "U2")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 7.62)
				(name "GVDD")
				(number "U8")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 7.62)
				(name "GVDD")
				(number "V7")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 7.62)
				(name "GVDD")
				(number "AK10")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 7.62)
				(name "GVDD")
				(number "W10")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 7.62)
				(name "GVDD")
				(number "AA6")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 7.62)
				(name "GVDD")
				(number "AR2")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 7.62)
				(name "GVDD")
				(number "Y2")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 7.62)
				(name "GVDD")
				(number "Y8")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 7.62)
				(name "GVDD")
				(number "AC2")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 7.62)
				(name "GVDD")
				(number "AD6")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 7.62)
				(name "GVDD")
				(number "AE10")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 7.62)
				(name "GVDD")
				(number "AE4")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 7.62)
				(name "GVDD")
				(number "AF2")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 7.62)
				(name "GVDD")
				(number "AF8")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 7.62)
				(name "GVDD")
				(number "AB4")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 7.62)
				(name "GVDD")
				(number "AB10")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 7.62)
				(name "GVDD")
				(number "AC8")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 7.62)
				(name "GVDD")
				(number "AG6")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 7.62)
				(name "GVDD")
				(number "AH10")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 7.62)
				(name "GVDD")
				(number "AH4")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 7.62)
				(name "GVDD")
				(number "AJ2")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 7.62)
				(name "GVDD")
				(number "AJ8")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 7.62)
				(name "GVDD")
				(number "AR14")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 7.62)
				(name "GVDD")
				(number "AK6")
			)
			(pin power_in line
				(at -25.4 -66.04 0)
				(length 7.62)
				(name "GVDD")
				(number "AL4")
			)
			(pin power_in line
				(at -25.4 -68.58 0)
				(length 7.62)
				(name "GVDD")
				(number "AL10")
			)
			(pin power_in line
				(at -25.4 -71.12 0)
				(length 7.62)
				(name "GVDD")
				(number "AM2")
			)
			(pin power_in line
				(at -25.4 -73.66 0)
				(length 7.62)
				(name "GVDD")
				(number "AM8")
			)
			(pin power_in line
				(at -25.4 -76.2 0)
				(length 7.62)
				(name "GVDD")
				(number "AP10")
			)
			(pin power_in line
				(at -25.4 -78.74 0)
				(length 7.62)
				(name "GVDD")
				(number "AN12")
			)
			(pin power_in line
				(at -25.4 -81.28 0)
				(length 7.62)
				(name "GVDD")
				(number "AN6")
			)
			(pin power_in line
				(at -25.4 -83.82 0)
				(length 7.62)
				(name "GVDD")
				(number "AP4")
			)
			(pin power_in line
				(at 25.4 86.36 180)
				(length 7.62)
				(name "OVDD")
				(number "AN22")
			)
			(pin power_in line
				(at 25.4 83.82 180)
				(length 7.62)
				(name "OVDD")
				(number "AJ14")
			)
			(pin power_in line
				(at 25.4 81.28 180)
				(length 7.62)
				(name "OVDD")
				(number "AJ18")
			)
			(pin power_in line
				(at 25.4 78.74 180)
				(length 7.62)
				(name "OVDD")
				(number "AL16")
			)
			(pin power_in line
				(at 25.4 76.2 180)
				(length 7.62)
				(name "OVDD")
				(number "AJ12")
			)
			(pin power_in line
				(at 25.4 73.66 180)
				(length 7.62)
				(name "OVDD")
				(number "AN18")
			)
			(pin power_in line
				(at 25.4 71.12 180)
				(length 7.62)
				(name "OVDD")
				(number "AG21")
			)
			(pin power_in line
				(at 25.4 68.58 180)
				(length 7.62)
				(name "OVDD")
				(number "AL20")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 7.62)
				(name "OVDD")
				(number "AT15")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 7.62)
				(name "OVDD")
				(number "AJ23")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 7.62)
				(name "OVDD")
				(number "AP16")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 7.62)
				(name "OVDD")
				(number "AR24")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 7.62)
				(name "CVDD")
				(number "AJ29")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 7.62)
				(name "CVDD")
				(number "AP29")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 7.62)
				(name "BVDD")
				(number "B24")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 7.62)
				(name "BVDD")
				(number "K22")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 7.62)
				(name "BVDD")
				(number "F20")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 7.62)
				(name "BVDD")
				(number "F26")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 7.62)
				(name "BVDD")
				(number "E24")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 7.62)
				(name "BVDD")
				(number "E22")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 7.62)
				(name "BVDD")
				(number "K24")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 7.62)
				(name "BVDD")
				(number "H20")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 7.62)
				(name "BVDD")
				(number "H18")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 7.62)
				(name "LVDD")
				(number "AK33")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 7.62)
				(name "LVDD")
				(number "AP31")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 7.62)
				(name "LVDD")
				(number "AL31")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 7.62)
				(name "LVDD")
				(number "AN33")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 7.62)
				(name "LVDD")
				(number "AJ35")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 7.62)
				(name "LVDD")
				(number "AR35")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 7.62)
				(name "LVDD")
				(number "AM35")
			)
			(pin power_in line
				(at 25.4 -8.89 180)
				(length 7.62)
				(name "POVDD")
				(number "AT17")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 7.62)
				(name "AVDD_CC1")
				(number "A20")
			)
			(pin power_in line
				(at 25.4 -19.05 180)
				(length 7.62)
				(name "AVDD_CC2")
				(number "A21")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 7.62)
				(name "AVDD_CC3")
				(number "AT18")
			)
			(pin power_in line
				(at 25.4 -26.67 180)
				(length 7.62)
				(name "AVDD_CC4")
				(number "AT19")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 7.62)
				(name "AVDD_PLAT")
				(number "AT20")
			)
			(pin power_in line
				(at 25.4 -34.29 180)
				(length 7.62)
				(name "AVDD_DDR")
				(number "A19")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 7.62)
				(name "SENSEVDD_PL1")
				(number "AF11")
			)
			(pin power_in line
				(at 25.4 -44.45 180)
				(length 7.62)
				(name "SENSEGND_PL1")
				(number "AF12")
			)
			(pin power_in line
				(at 25.4 -52.07 180)
				(length 7.62)
				(name "SENSEVDD_PL2")
				(number "L27")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 7.62)
				(name "SENSEGND_PL2")
				(number "K27")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 7.62)
				(name "SENSEVDD_CA")
				(number "K16")
			)
			(pin power_in line
				(at 25.4 -67.31 180)
				(length 7.62)
				(name "SENSEGND_CA")
				(number "K17")
			)
			(pin power_in line
				(at 25.4 -74.93 180)
				(length 7.62)
				(name "SENSEVDD_CB")
				(number "AG15")
			)
			(pin power_in line
				(at 25.4 -78.74 180)
				(length 7.62)
				(name "SENSEGND_CB")
				(number "AG16")
			)
			(pin input line
				(at 25.4 -83.82 180)
				(length 7.62)
				(name "MVREF")
				(number "B19")
			)
		)
		(symbol "P4080-BGA1295_10_1"
			(text "POWER PINS"
				(at 0 39.37 900)
			)
			(pin power_in line
				(at -25.4 88.9 0)
				(length 7.62)
				(name "VDD_PL")
				(number "M26")
			)
			(pin power_in line
				(at -25.4 86.36 0)
				(length 7.62)
				(name "VDD_PL")
				(number "P26")
			)
			(pin power_in line
				(at -25.4 83.82 0)
				(length 7.62)
				(name "VDD_PL")
				(number "T26")
			)
			(pin power_in line
				(at -25.4 81.28 0)
				(length 7.62)
				(name "VDD_PL")
				(number "V26")
			)
			(pin power_in line
				(at -25.4 78.74 0)
				(length 7.62)
				(name "VDD_PL")
				(number "Y26")
			)
			(pin power_in line
				(at -25.4 76.2 0)
				(length 7.62)
				(name "VDD_PL")
				(number "AB26")
			)
			(pin power_in line
				(at -25.4 73.66 0)
				(length 7.62)
				(name "VDD_PL")
				(number "AD26")
			)
			(pin power_in line
				(at -25.4 71.12 0)
				(length 7.62)
				(name "VDD_PL")
				(number "N11")
			)
			(pin power_in line
				(at -25.4 68.58 0)
				(length 7.62)
				(name "VDD_PL")
				(number "R11")
			)
			(pin power_in line
				(at -25.4 66.04 0)
				(length 7.62)
				(name "VDD_PL")
				(number "W11")
			)
			(pin power_in line
				(at -25.4 63.5 0)
				(length 7.62)
				(name "VDD_PL")
				(number "AA11")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 7.62)
				(name "VDD_PL")
				(number "AE11")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 7.62)
				(name "VDD_PL")
				(number "M12")
			)
			(pin power_in line
				(at -25.4 55.88 0)
				(length 7.62)
				(name "VDD_PL")
				(number "P12")
			)
			(pin power_in line
				(at -25.4 53.34 0)
				(length 7.62)
				(name "VDD_PL")
				(number "T12")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 7.62)
				(name "VDD_PL")
				(number "V12")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 7.62)
				(name "VDD_PL")
				(number "Y12")
			)
			(pin power_in line
				(at -25.4 45.72 0)
				(length 7.62)
				(name "VDD_PL")
				(number "AB12")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 7.62)
				(name "VDD_PL")
				(number "AD12")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 7.62)
				(name "VDD_PL")
				(number "AE13")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 7.62)
				(name "VDD_PL")
				(number "AE15")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 7.62)
				(name "VDD_PL")
				(number "V16")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 7.62)
				(name "VDD_PL")
				(number "AE17")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 7.62)
				(name "VDD_PL")
				(number "L11")
			)
			(pin power_in line
				(at -25.4 27.94 0)
				(length 7.62)
				(name "VDD_PL")
				(number "AE19")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 7.62)
				(name "VDD_PL")
				(number "U11")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 7.62)
				(name "VDD_PL")
				(number "AC11")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 7.62)
				(name "VDD_PL")
				(number "V20")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 7.62)
				(name "VDD_PL")
				(number "AE21")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 7.62)
				(name "VDD_PL")
				(number "V22")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 7.62)
				(name "VDD_PL")
				(number "U13")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 7.62)
				(name "VDD_PL")
				(number "R27")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 7.62)
				(name "VDD_PL")
				(number "U23")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 7.62)
				(name "VDD_PL")
				(number "W23")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 7.62)
				(name "VDD_PL")
				(number "AA27")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 7.62)
				(name "VDD_PL")
				(number "AC27")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 7.62)
				(name "VDD_PL")
				(number "AE23")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 7.62)
				(name "VDD_PL")
				(number "M24")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 7.62)
				(name "VDD_PL")
				(number "P24")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 7.62)
				(name "VDD_PL")
				(number "T24")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 7.62)
				(name "VDD_PL")
				(number "V24")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 7.62)
				(name "VDD_PL")
				(number "Y24")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 7.62)
				(name "VDD_PL")
				(number "AB24")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 7.62)
				(name "VDD_PL")
				(number "AD24")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 7.62)
				(name "VDD_PL")
				(number "N25")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 7.62)
				(name "VDD_PL")
				(number "R25")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 7.62)
				(name "VDD_PL")
				(number "U25")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 7.62)
				(name "VDD_PL")
				(number "W25")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 7.62)
				(name "VDD_PL")
				(number "AA25")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 7.62)
				(name "VDD_CA")
				(number "T20")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 7.62)
				(name "VDD_CA")
				(number "P20")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 7.62)
				(name "VDD_CA")
				(number "R21")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 7.62)
				(name "VDD_CA")
				(number "R19")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 7.62)
				(name "VDD_CA")
				(number "P14")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 7.62)
				(name "VDD_CA")
				(number "N19")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 7.62)
				(name "VDD_CA")
				(number "M20")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 7.62)
				(name "VDD_CA")
				(number "N21")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 7.62)
				(name "VDD_CA")
				(number "M16")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 7.62)
				(name "VDD_CA")
				(number "N15")
			)
			(pin power_in line
				(at -25.4 -66.04 0)
				(length 7.62)
				(name "VDD_CA")
				(number "P16")
			)
			(pin power_in line
				(at -25.4 -68.58 0)
				(length 7.62)
				(name "VDD_CA")
				(number "T16")
			)
			(pin power_in line
				(at -25.4 -71.12 0)
				(length 7.62)
				(name "VDD_CA")
				(number "R17")
			)
			(pin power_in line
				(at -25.4 -73.66 0)
				(length 7.62)
				(name "VDD_CA")
				(number "T18")
			)
			(pin power_in line
				(at -25.4 -76.2 0)
				(length 7.62)
				(name "VDD_CA")
				(number "R15")
			)
			(pin power_in line
				(at -25.4 -78.74 0)
				(length 7.62)
				(name "VDD_CA")
				(number "N17")
			)
			(pin power_in line
				(at -25.4 -81.28 0)
				(length 7.62)
				(name "VDD_CA")
				(number "M18")
			)
			(pin power_in line
				(at -25.4 -83.82 0)
				(length 7.62)
				(name "VDD_CA")
				(number "P18")
			)
			(pin power_in line
				(at 25.4 86.36 180)
				(length 7.62)
				(name "VDD_PL")
				(number "Y14")
			)
			(pin power_in line
				(at 25.4 83.82 180)
				(length 7.62)
				(name "VDD_PL")
				(number "AD20")
			)
			(pin power_in line
				(at 25.4 81.28 180)
				(length 7.62)
				(name "VDD_PL")
				(number "AD18")
			)
			(pin power_in line
				(at 25.4 78.74 180)
				(length 7.62)
				(name "VDD_PL")
				(number "AD16")
			)
			(pin power_in line
				(at 25.4 76.2 180)
				(length 7.62)
				(name "VDD_PL")
				(number "AD14")
			)
			(pin power_in line
				(at 25.4 73.66 180)
				(length 7.62)
				(name "VDD_PL")
				(number "T14")
			)
			(pin power_in line
				(at 25.4 71.12 180)
				(length 7.62)
				(name "VDD_PL")
				(number "U19")
			)
			(pin power_in line
				(at 25.4 68.58 180)
				(length 7.62)
				(name "VDD_PL")
				(number "U17")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 7.62)
				(name "VDD_PL")
				(number "M14")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 7.62)
				(name "VDD_PL")
				(number "R13")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 7.62)
				(name "VDD_PL")
				(number "AA13")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 7.62)
				(name "VDD_PL")
				(number "AB22")
			)
			(pin power_in line
				(at 25.4 55.88 180)
				(length 7.62)
				(name "VDD_PL")
				(number "Y22")
			)
			(pin power_in line
				(at 25.4 53.34 180)
				(length 7.62)
				(name "VDD_PL")
				(number "T22")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 7.62)
				(name "VDD_PL")
				(number "P22")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 7.62)
				(name "VDD_PL")
				(number "AC13")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 7.62)
				(name "VDD_PL")
				(number "N13")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 7.62)
				(name "VDD_PL")
				(number "M22")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 7.62)
				(name "VDD_PL")
				(number "AD22")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 7.62)
				(name "VDD_PL")
				(number "AC21")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 7.62)
				(name "VDD_PL")
				(number "U15")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 7.62)
				(name "VDD_PL")
				(number "W21")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 7.62)
				(name "VDD_PL")
				(number "U21")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 7.62)
				(name "VDD_PL")
				(number "AC23")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 7.62)
				(name "VDD_PL")
				(number "AA23")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 7.62)
				(name "VDD_PL")
				(number "R23")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 7.62)
				(name "VDD_PL")
				(number "N23")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 7.62)
				(name "VDD_PL")
				(number "AF14")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 7.62)
				(name "VDD_PL")
				(number "L25")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 7.62)
				(name "VDD_PL")
				(number "L23")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 7.62)
				(name "VDD_PL")
				(number "L21")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 7.62)
				(name "VDD_PL")
				(number "L19")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 7.62)
				(name "VDD_PL")
				(number "L17")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 7.62)
				(name "VDD_PL")
				(number "L15")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 7.62)
				(name "VDD_PL")
				(number "L13")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 7.62)
				(name "VDD_PL")
				(number "V18")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 7.62)
				(name "VDD_PL")
				(number "V14")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 7.62)
				(name "VDD_PL")
				(number "AF18")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 7.62)
				(name "VDD_PL")
				(number "W13")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 7.62)
				(name "VDD_PL")
				(number "AF16")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 7.62)
				(name "VDD_PL")
				(number "AF20")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 7.62)
				(name "VDD_PL")
				(number "AF22")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 7.62)
				(name "VDD_PL")
				(number "AF24")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 7.62)
				(name "VDD_PL")
				(number "AE25")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 7.62)
				(name "VDD_PL")
				(number "W28")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 7.62)
				(name "VDD_PL")
				(number "U27")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 7.62)
				(name "VDD_PL")
				(number "N27")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 7.62)
				(name "VDD_PL")
				(number "AC25")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 7.62)
				(name "VDD_CB")
				(number "W15")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 7.62)
				(name "VDD_CB")
				(number "W19")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 7.62)
				(name "VDD_CB")
				(number "AA19")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 7.62)
				(name "VDD_CB")
				(number "Y20")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 7.62)
				(name "VDD_CB")
				(number "AB14")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 7.62)
				(name "VDD_CB")
				(number "AA21")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 7.62)
				(name "VDD_CB")
				(number "Y16")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 7.62)
				(name "VDD_CB")
				(number "AA15")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 7.62)
				(name "VDD_CB")
				(number "AC15")
			)
			(pin power_in line
				(at 25.4 -66.04 180)
				(length 7.62)
				(name "VDD_CB")
				(number "AA17")
			)
			(pin power_in line
				(at 25.4 -68.58 180)
				(length 7.62)
				(name "VDD_CB")
				(number "AC17")
			)
			(pin power_in line
				(at 25.4 -71.12 180)
				(length 7.62)
				(name "VDD_CB")
				(number "W17")
			)
			(pin power_in line
				(at 25.4 -73.66 180)
				(length 7.62)
				(name "VDD_CB")
				(number "Y18")
			)
			(pin power_in line
				(at 25.4 -76.2 180)
				(length 7.62)
				(name "VDD_CB")
				(number "AB18")
			)
			(pin power_in line
				(at 25.4 -78.74 180)
				(length 7.62)
				(name "VDD_CB")
				(number "AB16")
			)
			(pin power_in line
				(at 25.4 -81.28 180)
				(length 7.62)
				(name "VDD_CB")
				(number "AC19")
			)
			(pin power_in line
				(at 25.4 -83.82 180)
				(length 7.62)
				(name "VDD_CB")
				(number "AB20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Z80CPU"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 35.56 0)
		)
		(property "Value" "Z80CPU"
			(at 6.35 35.56 0)
		)
		(property "Footprint" ""
			(at 0 10.16 0)
		)
		(property "Datasheet" "www.zilog.com/manage_directlink.php?filepath=docs/z80/um0080"
			(at 0 10.16 0)
		)
		(property "Description" "8-bit General Purpose Microprocessor, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Z80 CPU uP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
		(symbol "Z80CPU_0_1")
		(symbol "Z80CPU_1_1"
			(pin input line
				(at -17.78 30.48 0)
				(length 3.81)
				(name "~{RESET}")
				(number "26")
			)
			(pin input clock
				(at -17.78 22.86 0)
				(length 3.81)
				(name "~{CLK}")
				(number "6")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "~{NMI}")
				(number "17")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "~{INT}")
				(number "16")
			)
			(pin output line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "~{M1}")
				(number "27")
			)
			(pin output line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "~{RFSH}")
				(number "28")
			)
			(pin input line
				(at -17.78 0 0)
				(length 3.81)
				(name "~{WAIT}")
				(number "24")
			)
			(pin output line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "~{HALT}")
				(number "18")
			)
			(pin output line
				(at -17.78 -12.7 0)
				(length 3.81)
				(name "~{RD}")
				(number "21")
			)
			(pin output line
				(at -17.78 -15.24 0)
				(length 3.81)
				(name "~{WR}")
				(number "22")
			)
			(pin output line
				(at -17.78 -17.78 0)
				(length 3.81)
				(name "~{MREQ}")
				(number "19")
			)
			(pin output line
				(at -17.78 -20.32 0)
				(length 3.81)
				(name "~{IORQ}")
				(number "20")
			)
			(pin input line
				(at -17.78 -27.94 0)
				(length 3.81)
				(name "~{BUSRQ}")
				(number "25")
			)
			(pin output line
				(at -17.78 -30.48 0)
				(length 3.81)
				(name "~{BUSACK}")
				(number "23")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 3.81)
				(name "VCC")
				(number "11")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 3.81)
				(name "GND")
				(number "29")
			)
			(pin output line
				(at 17.78 30.48 180)
				(length 3.81)
				(name "A0")
				(number "30")
			)
			(pin output line
				(at 17.78 27.94 180)
				(length 3.81)
				(name "A1")
				(number "31")
			)
			(pin output line
				(at 17.78 25.4 180)
				(length 3.81)
				(name "A2")
				(number "32")
			)
			(pin output line
				(at 17.78 22.86 180)
				(length 3.81)
				(name "A3")
				(number "33")
			)
			(pin output line
				(at 17.78 20.32 180)
				(length 3.81)
				(name "A4")
				(number "34")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 3.81)
				(name "A5")
				(number "35")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "A6")
				(number "36")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "A7")
				(number "37")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "A8")
				(number "38")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "A9")
				(number "39")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "A10")
				(number "40")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "A11")
				(number "1")
			)
			(pin output line
				(at 17.78 0 180)
				(length 3.81)
				(name "A12")
				(number "2")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "A13")
				(number "3")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "A14")
				(number "4")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "A15")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "D0")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "D1")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "D2")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 3.81)
				(name "D3")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 3.81)
				(name "D4")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 3.81)
				(name "D5")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 3.81)
				(name "D6")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 3.81)
				(name "D7")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CDP1802ACEX"
		(extends "CDP1802ACE")
		(property "Reference" "U"
			(at -10.16 34.29 0)
		)
		(property "Value" "CDP1802ACEX"
			(at 3.81 34.29 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 48.26 0)
		)
		(property "Datasheet" "http://www.cosmacelf.com/publications/data-sheets/cdp1802.pdf"
			(at 0 50.8 0)
		)
		(property "Description" "8-bit, General Purpose, 5V, 3.2 MHz, Burned-In, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "CPU Processor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "CDP1802BCE"
		(extends "CDP1802ACE")
		(property "Reference" "U"
			(at -10.16 34.29 0)
		)
		(property "Value" "CDP1802BCE"
			(at 3.81 34.29 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 48.26 0)
		)
		(property "Datasheet" "http://www.cosmacelf.com/publications/data-sheets/cdp1802.pdf"
			(at 0 50.8 0)
		)
		(property "Description" "8-bit, General Purpose, 5V, 5 MHz, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "CPU Processor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "CDP1802BCEX"
		(extends "CDP1802ACE")
		(property "Reference" "U"
			(at -10.16 34.29 0)
		)
		(property "Value" "CDP1802BCEX"
			(at 3.81 34.29 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 48.26 0)
		)
		(property "Datasheet" "http://www.cosmacelf.com/publications/data-sheets/cdp1802.pdf"
			(at 0 50.8 0)
		)
		(property "Description" "8-bit, General Purpose, 5V, 5 MHz, Burned-In, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "CPU Processor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
)
