(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "MC6800"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 34.29 0)
		)
		(property "Value" "MC6800"
			(at 10.16 34.29 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 -38.1 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheet/motorola/MC68A00L.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-Bit Microprocessing unit 1.0MHz, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "MC6800_0_1")
		(symbol "MC6800_1_1"
			(pin bidirectional line
				(at -12.7 30.48 0)
				(length 2.54)
				(name "D0")
				(number "33")
			)
			(pin bidirectional line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "D1")
				(number "32")
			)
			(pin bidirectional line
				(at -12.7 25.4 0)
				(length 2.54)
				(name "D2")
				(number "31")
			)
			(pin bidirectional line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "D3")
				(number "30")
			)
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "D4")
				(number "29")
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "D5")
				(number "28")
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "D6")
				(number "27")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "D7")
				(number "26")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "Phi1")
				(number "3")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "Phi2")
				(number "37")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "~{RESET}")
				(number "40")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{NMI}")
				(number "6")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{HALT}")
				(number "2")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{IRQ}")
				(number "4")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "TSC")
				(number "39")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "DBE")
				(number "36")
			)
			(pin no_connect line
				(at -10.16 -22.86 0)
				(length 2.54)
				(hide yes)
				(name "N.C.")
				(number "38")
			)
			(pin no_connect line
				(at -10.16 -25.4 0)
				(length 2.54)
				(hide yes)
				(name "N.C.")
				(number "35")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 2.54)
				(name "VSS")
				(number "1")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -35.56 90)
				(length 2.54)
				(name "VSS")
				(number "21")
			)
			(pin output line
				(at 12.7 30.48 180)
				(length 2.54)
				(name "A0")
				(number "9")
			)
			(pin output line
				(at 12.7 27.94 180)
				(length 2.54)
				(name "A1")
				(number "10")
			)
			(pin output line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "A2")
				(number "11")
			)
			(pin output line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "A3")
				(number "12")
			)
			(pin output line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "A4")
				(number "13")
			)
			(pin output line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "A5")
				(number "14")
			)
			(pin output line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "A6")
				(number "15")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "A7")
				(number "16")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "A8")
				(number "17")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "A9")
				(number "18")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "A10")
				(number "19")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "A11")
				(number "20")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "A12")
				(number "22")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "A13")
				(number "23")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "A14")
				(number "24")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "A15")
				(number "25")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "BA")
				(number "7")
			)
			(pin output line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "VMA")
				(number "5")
			)
			(pin output line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "R/~{W}")
				(number "34")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC6802"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 34.29 0)
		)
		(property "Value" "MC6802"
			(at 10.16 34.29 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 -38.1 0)
		)
		(property "Datasheet" "https://www.jameco.com/Jameco/Products/ProdDS/43502.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-Bit Microprocessing unit 1.0MHz, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "MC6802_0_1")
		(symbol "MC6802_1_1"
			(pin bidirectional line
				(at -12.7 30.48 0)
				(length 2.54)
				(name "D0")
				(number "33")
			)
			(pin bidirectional line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "D1")
				(number "32")
			)
			(pin bidirectional line
				(at -12.7 25.4 0)
				(length 2.54)
				(name "D2")
				(number "31")
			)
			(pin bidirectional line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "D3")
				(number "30")
			)
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "D4")
				(number "29")
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "D5")
				(number "28")
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "D6")
				(number "27")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "D7")
				(number "26")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "MR")
				(number "3")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "RE")
				(number "36")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "~{RESET}")
				(number "40")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{NMI}")
				(number "6")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{HALT}")
				(number "2")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{IRQ}")
				(number "4")
			)
			(pin passive line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "XTAL")
				(number "38")
			)
			(pin passive line
				(at -12.7 -25.4 0)
				(length 2.54)
				(name "EXTAL")
				(number "39")
			)
			(pin power_in line
				(at -2.54 35.56 270)
				(length 2.54)
				(name "VCC_STANDBY")
				(number "35")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "1")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "VSS")
				(number "21")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin output line
				(at 12.7 30.48 180)
				(length 2.54)
				(name "A0")
				(number "9")
			)
			(pin output line
				(at 12.7 27.94 180)
				(length 2.54)
				(name "A1")
				(number "10")
			)
			(pin output line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "A2")
				(number "11")
			)
			(pin output line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "A3")
				(number "12")
			)
			(pin output line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "A4")
				(number "13")
			)
			(pin output line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "A5")
				(number "14")
			)
			(pin output line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "A6")
				(number "15")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "A7")
				(number "16")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "A8")
				(number "17")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "A9")
				(number "18")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "A10")
				(number "19")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "A11")
				(number "20")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "A12")
				(number "22")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "A13")
				(number "23")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "A14")
				(number "24")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "A15")
				(number "25")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "BA")
				(number "7")
			)
			(pin output line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "VMA")
				(number "5")
			)
			(pin output line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "R/~{W}")
				(number "34")
			)
			(pin output line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "E")
				(number "37")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC6809"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 34.29 0)
		)
		(property "Value" "MC6809"
			(at 10.16 34.29 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 -38.1 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheet/motorola/MC68B09S.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-Bit Microprocessing unit 1.0MHz, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "MC6809_0_1")
		(symbol "MC6809_1_1"
			(pin bidirectional line
				(at -12.7 30.48 0)
				(length 2.54)
				(name "D0")
				(number "31")
			)
			(pin bidirectional line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "D1")
				(number "30")
			)
			(pin bidirectional line
				(at -12.7 25.4 0)
				(length 2.54)
				(name "D2")
				(number "29")
			)
			(pin bidirectional line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "D3")
				(number "28")
			)
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "D4")
				(number "27")
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "D5")
				(number "26")
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "D6")
				(number "25")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "D7")
				(number "24")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "~{RESET}")
				(number "37")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "~{NMI}")
				(number "2")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "~{IRQ}")
				(number "3")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{FIRQ}")
				(number "4")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "~{DMA/BREQ}")
				(number "33")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "~{HALT}")
				(number "40")
			)
			(pin input line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "MRDY")
				(number "36")
			)
			(pin input line
				(at -12.7 -25.4 0)
				(length 2.54)
				(name "XTAL")
				(number "39")
			)
			(pin input line
				(at -12.7 -27.94 0)
				(length 2.54)
				(name "EXTAL")
				(number "38")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VCC")
				(number "7")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "VSS")
				(number "1")
			)
			(pin output line
				(at 12.7 30.48 180)
				(length 2.54)
				(name "A0")
				(number "8")
			)
			(pin output line
				(at 12.7 27.94 180)
				(length 2.54)
				(name "A1")
				(number "9")
			)
			(pin output line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "A2")
				(number "10")
			)
			(pin output line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "A3")
				(number "11")
			)
			(pin output line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "A4")
				(number "12")
			)
			(pin output line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "A5")
				(number "13")
			)
			(pin output line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "A6")
				(number "14")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "A7")
				(number "15")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "A8")
				(number "16")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "A9")
				(number "17")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "A10")
				(number "18")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "A11")
				(number "19")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "A12")
				(number "20")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "A13")
				(number "21")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "A14")
				(number "22")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "A15")
				(number "23")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "R/~{W}")
				(number "32")
			)
			(pin output line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "BS")
				(number "5")
			)
			(pin output line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "BA")
				(number "6")
			)
			(pin output line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "E")
				(number "34")
			)
			(pin output line
				(at 12.7 -25.4 180)
				(length 2.54)
				(name "Q")
				(number "35")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC6809E"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 34.544 0)
		)
		(property "Value" "MC6809E"
			(at 10.16 34.544 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 -38.1 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheet/motorola/MC68B09S.pdf"
			(at -2.54 36.195 0)
		)
		(property "Description" "8-Bit Microprocessing unit 1.0MHz, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "MC6809E_0_1")
		(symbol "MC6809E_1_1"
			(pin bidirectional line
				(at -12.7 30.48 0)
				(length 2.54)
				(name "D0")
				(number "31")
			)
			(pin bidirectional line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "D1")
				(number "30")
			)
			(pin bidirectional line
				(at -12.7 25.4 0)
				(length 2.54)
				(name "D2")
				(number "29")
			)
			(pin bidirectional line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "D3")
				(number "28")
			)
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "D4")
				(number "27")
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "D5")
				(number "26")
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "D6")
				(number "25")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "D7")
				(number "24")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "~{RESET}")
				(number "37")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "~{NMI}")
				(number "2")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "~{IRQ}")
				(number "3")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{FIRQ}")
				(number "4")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "~{HALT}")
				(number "40")
			)
			(pin input line
				(at -12.7 -25.4 0)
				(length 2.54)
				(name "E")
				(number "34")
			)
			(pin input line
				(at -12.7 -27.94 0)
				(length 2.54)
				(name "Q")
				(number "35")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VCC")
				(number "7")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "VSS")
				(number "1")
			)
			(pin output line
				(at 12.7 30.48 180)
				(length 2.54)
				(name "A0")
				(number "8")
			)
			(pin output line
				(at 12.7 27.94 180)
				(length 2.54)
				(name "A1")
				(number "9")
			)
			(pin output line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "A2")
				(number "10")
			)
			(pin output line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "A3")
				(number "11")
			)
			(pin output line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "A4")
				(number "12")
			)
			(pin output line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "A5")
				(number "13")
			)
			(pin output line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "A6")
				(number "14")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "A7")
				(number "15")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "A8")
				(number "16")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "A9")
				(number "17")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "A10")
				(number "18")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "A11")
				(number "19")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "A12")
				(number "20")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "A13")
				(number "21")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "A14")
				(number "22")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "A15")
				(number "23")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "LIC")
				(number "38")
			)
			(pin output line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "AVMA")
				(number "36")
			)
			(pin output line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "R/~{W}")
				(number "32")
			)
			(pin output line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "TSC")
				(number "39")
			)
			(pin output line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "BA")
				(number "6")
			)
			(pin output line
				(at 12.7 -25.4 180)
				(length 2.54)
				(name "BS")
				(number "5")
			)
			(pin output line
				(at 12.7 -27.94 180)
				(length 2.54)
				(name "BUSY")
				(number "33")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC68A00"
		(extends "MC6800")
		(property "Reference" "U"
			(at -8.89 34.29 0)
		)
		(property "Value" "MC68A00"
			(at 10.16 34.29 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 -38.1 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheet/motorola/MC68A00L.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-Bit Microprocessing unit 1.5MHz, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC68A02"
		(extends "MC6802")
		(property "Reference" "U"
			(at -8.89 34.29 0)
		)
		(property "Value" "MC68A02"
			(at 10.16 34.29 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 -38.1 0)
		)
		(property "Datasheet" "https://www.jameco.com/Jameco/Products/ProdDS/43502.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-Bit Microprocessing unit 1.5MHz, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC68A09"
		(extends "MC6809")
		(property "Reference" "U"
			(at -7.62 34.29 0)
		)
		(property "Value" "MC68A09"
			(at 10.16 34.29 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 -38.1 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheet/motorola/MC68B09S.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-Bit Microprocessing unit 1.5MHz, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC68A09E"
		(extends "MC6809E")
		(property "Reference" "U"
			(at -7.62 34.544 0)
		)
		(property "Value" "MC68A09E"
			(at 10.16 34.544 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 -38.1 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheet/motorola/MC68B09S.pdf"
			(at -2.54 36.195 0)
		)
		(property "Description" "8-Bit Microprocessing unit 1.5MHz, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC68B00"
		(extends "MC6800")
		(property "Reference" "U"
			(at -8.89 34.29 0)
		)
		(property "Value" "MC68B00"
			(at 10.16 34.29 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 -38.1 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheet/motorola/MC68A00L.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-Bit Microprocessing unit 2.0MHz, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC68B02"
		(extends "MC6802")
		(property "Reference" "U"
			(at -8.89 34.29 0)
		)
		(property "Value" "MC68B02"
			(at 10.16 34.29 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 -38.1 0)
		)
		(property "Datasheet" "https://www.jameco.com/Jameco/Products/ProdDS/43502.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-Bit Microprocessing unit 2.0MHz, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC68B09"
		(extends "MC6809")
		(property "Reference" "U"
			(at -7.62 34.29 0)
		)
		(property "Value" "MC68B09"
			(at 10.16 34.29 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 -38.1 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheet/motorola/MC68B09S.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-Bit Microprocessing unit 2.0MHz, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC68B09E"
		(extends "MC6809E")
		(property "Reference" "U"
			(at -7.62 34.544 0)
		)
		(property "Value" "MC68B09E"
			(at 10.16 34.544 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 -38.1 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheet/motorola/MC68B09S.pdf"
			(at -2.54 36.195 0)
		)
		(property "Description" "8-Bit Microprocessing unit 2.0MHz, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
)
