(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "68000D"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "68000D"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/reference-manual/MC68000UM.pdf"
			(at 0 0 0)
		)
		(property "Description" "16/32-bit Microprocessor"
			(at 0 0 0)
		)
		(property "ki_keywords" "68000 Microprocessor CPU"
			(at 0 0 0)
		)
		(symbol "68000D_0_1")
		(symbol "68000D_1_1"
			(pin input clock
				(at -25.4 55.88 0)
				(length 7.62)
				(name "CLK")
				(number "15")
			)
			(pin input inverted
				(at -25.4 48.26 0)
				(length 7.62)
				(name "IPL0")
				(number "25")
			)
			(pin input inverted
				(at -25.4 45.72 0)
				(length 7.62)
				(name "IPL1")
				(number "24")
			)
			(pin input inverted
				(at -25.4 43.18 0)
				(length 7.62)
				(name "IPL2")
				(number "23")
			)
			(pin input inverted
				(at -25.4 38.1 0)
				(length 7.62)
				(name "BGACK")
				(number "12")
			)
			(pin output inverted
				(at -25.4 35.56 0)
				(length 7.62)
				(name "BG")
				(number "11")
			)
			(pin input inverted
				(at -25.4 33.02 0)
				(length 7.62)
				(name "BR")
				(number "13")
			)
			(pin output line
				(at -25.4 25.4 0)
				(length 7.62)
				(name "FC0")
				(number "28")
			)
			(pin output line
				(at -25.4 22.86 0)
				(length 7.62)
				(name "FC1")
				(number "27")
			)
			(pin output line
				(at -25.4 20.32 0)
				(length 7.62)
				(name "FC2")
				(number "26")
			)
			(pin output inverted
				(at -25.4 12.7 0)
				(length 7.62)
				(name "VMA")
				(number "19")
			)
			(pin output line
				(at -25.4 10.16 0)
				(length 7.62)
				(name "E")
				(number "20")
			)
			(pin input inverted
				(at -25.4 7.62 0)
				(length 7.62)
				(name "VPA")
				(number "21")
			)
			(pin input inverted
				(at -25.4 -15.24 0)
				(length 7.62)
				(name "BERR")
				(number "22")
			)
			(pin input inverted
				(at -25.4 -20.32 0)
				(length 7.62)
				(name "DTACK")
				(number "10")
			)
			(pin bidirectional inverted
				(at -25.4 -30.48 0)
				(length 7.62)
				(name "HALT")
				(number "17")
			)
			(pin bidirectional inverted
				(at -25.4 -33.02 0)
				(length 7.62)
				(name "RESET")
				(number "18")
			)
			(pin power_in line
				(at 0 60.96 270)
				(length 3.81)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -60.96 90)
				(length 3.81)
				(name "GND")
				(number "53")
			)
			(pin power_in line
				(at 2.54 60.96 270)
				(length 3.81)
				(name "VCC")
				(number "49")
			)
			(pin power_in line
				(at 2.54 -60.96 90)
				(length 3.81)
				(name "GND")
				(number "16")
			)
			(pin output line
				(at 25.4 55.88 180)
				(length 7.62)
				(name "A1")
				(number "29")
			)
			(pin output line
				(at 25.4 53.34 180)
				(length 7.62)
				(name "A2")
				(number "30")
			)
			(pin output line
				(at 25.4 50.8 180)
				(length 7.62)
				(name "A3")
				(number "31")
			)
			(pin output line
				(at 25.4 48.26 180)
				(length 7.62)
				(name "A4")
				(number "32")
			)
			(pin output line
				(at 25.4 45.72 180)
				(length 7.62)
				(name "A5")
				(number "33")
			)
			(pin output line
				(at 25.4 43.18 180)
				(length 7.62)
				(name "A6")
				(number "34")
			)
			(pin output line
				(at 25.4 40.64 180)
				(length 7.62)
				(name "A7")
				(number "35")
			)
			(pin output line
				(at 25.4 38.1 180)
				(length 7.62)
				(name "A8")
				(number "36")
			)
			(pin output line
				(at 25.4 35.56 180)
				(length 7.62)
				(name "A9")
				(number "37")
			)
			(pin output line
				(at 25.4 33.02 180)
				(length 7.62)
				(name "A10")
				(number "38")
			)
			(pin output line
				(at 25.4 30.48 180)
				(length 7.62)
				(name "A11")
				(number "39")
			)
			(pin output line
				(at 25.4 27.94 180)
				(length 7.62)
				(name "A12")
				(number "40")
			)
			(pin output line
				(at 25.4 25.4 180)
				(length 7.62)
				(name "A13")
				(number "41")
			)
			(pin output line
				(at 25.4 22.86 180)
				(length 7.62)
				(name "A14")
				(number "42")
			)
			(pin output line
				(at 25.4 20.32 180)
				(length 7.62)
				(name "A15")
				(number "43")
			)
			(pin output line
				(at 25.4 17.78 180)
				(length 7.62)
				(name "A16")
				(number "44")
			)
			(pin output line
				(at 25.4 15.24 180)
				(length 7.62)
				(name "A17")
				(number "45")
			)
			(pin output line
				(at 25.4 12.7 180)
				(length 7.62)
				(name "A18")
				(number "46")
			)
			(pin output line
				(at 25.4 10.16 180)
				(length 7.62)
				(name "A19")
				(number "47")
			)
			(pin output line
				(at 25.4 7.62 180)
				(length 7.62)
				(name "A20")
				(number "48")
			)
			(pin output line
				(at 25.4 5.08 180)
				(length 7.62)
				(name "A21")
				(number "50")
			)
			(pin output line
				(at 25.4 2.54 180)
				(length 7.62)
				(name "A22")
				(number "51")
			)
			(pin output line
				(at 25.4 0 180)
				(length 7.62)
				(name "A23")
				(number "52")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 7.62)
				(name "D0")
				(number "5")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 7.62)
				(name "D1")
				(number "4")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 7.62)
				(name "D2")
				(number "3")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 7.62)
				(name "D3")
				(number "2")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 7.62)
				(name "D4")
				(number "1")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 7.62)
				(name "D5")
				(number "64")
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 7.62)
				(name "D6")
				(number "63")
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 7.62)
				(name "D7")
				(number "62")
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 7.62)
				(name "D8")
				(number "61")
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 7.62)
				(name "D9")
				(number "60")
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 7.62)
				(name "D10")
				(number "59")
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 7.62)
				(name "D11")
				(number "58")
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 7.62)
				(name "D12")
				(number "57")
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 7.62)
				(name "D13")
				(number "56")
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 7.62)
				(name "D14")
				(number "55")
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 7.62)
				(name "D15")
				(number "54")
			)
			(pin output inverted
				(at 25.4 -48.26 180)
				(length 7.62)
				(name "AS")
				(number "6")
			)
			(pin output inverted
				(at 25.4 -50.8 180)
				(length 7.62)
				(name "UDS")
				(number "7")
			)
			(pin output inverted
				(at 25.4 -53.34 180)
				(length 7.62)
				(name "LDS")
				(number "8")
			)
			(pin output line
				(at 25.4 -55.88 180)
				(length 7.62)
				(name "R/W")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "68008D"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "68008D"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/reference-manual/MC68000UM.pdf"
			(at 0 0 0)
		)
		(property "Description" "16/32-bit Microprocessor, 8-bit databus"
			(at 0 0 0)
		)
		(property "ki_keywords" "68000 Microprocessor CPU"
			(at 0 0 0)
		)
		(symbol "68008D_0_1")
		(symbol "68008D_1_1"
			(pin input clock
				(at -22.86 38.1 0)
				(length 7.62)
				(name "CLK")
				(number "34")
			)
			(pin input inverted
				(at -22.86 35.56 0)
				(length 7.62)
				(name "VPA")
				(number "39")
			)
			(pin input inverted
				(at -22.86 30.48 0)
				(length 7.62)
				(name "IPL0/2")
				(number "42")
			)
			(pin input inverted
				(at -22.86 27.94 0)
				(length 7.62)
				(name "IPL1")
				(number "41")
			)
			(pin input inverted
				(at -22.86 17.78 0)
				(length 7.62)
				(name "BR")
				(number "33")
			)
			(pin input inverted
				(at -22.86 15.24 0)
				(length 7.62)
				(name "DTACK")
				(number "31")
			)
			(pin input inverted
				(at -22.86 12.7 0)
				(length 7.62)
				(name "BERR")
				(number "40")
			)
			(pin output line
				(at -22.86 7.62 0)
				(length 7.62)
				(name "FC0")
				(number "45")
			)
			(pin output line
				(at -22.86 5.08 0)
				(length 7.62)
				(name "FC1")
				(number "44")
			)
			(pin output line
				(at -22.86 2.54 0)
				(length 7.62)
				(name "FC2")
				(number "43")
			)
			(pin output inverted
				(at -22.86 -2.54 0)
				(length 7.62)
				(name "BG")
				(number "32")
			)
			(pin output line
				(at -22.86 -7.62 0)
				(length 7.62)
				(name "E")
				(number "38")
			)
			(pin bidirectional inverted
				(at -22.86 -27.94 0)
				(length 7.62)
				(name "HALT")
				(number "36")
			)
			(pin bidirectional inverted
				(at -22.86 -30.48 0)
				(length 7.62)
				(name "RESET")
				(number "37")
			)
			(pin tri_state inverted
				(at -22.86 -33.02 0)
				(length 7.62)
				(name "AS")
				(number "28")
			)
			(pin tri_state inverted
				(at -22.86 -35.56 0)
				(length 7.62)
				(name "DS")
				(number "29")
			)
			(pin tri_state line
				(at -22.86 -38.1 0)
				(length 7.62)
				(name "R/W")
				(number "30")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 3.81)
				(name "VCC")
				(number "13")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 3.81)
				(name "GND")
				(number "35")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 3.81)
				(name "GND")
				(number "15")
			)
			(pin tri_state line
				(at 22.86 38.1 180)
				(length 7.62)
				(name "A0")
				(number "46")
			)
			(pin tri_state line
				(at 22.86 35.56 180)
				(length 7.62)
				(name "A1")
				(number "47")
			)
			(pin tri_state line
				(at 22.86 33.02 180)
				(length 7.62)
				(name "A2")
				(number "48")
			)
			(pin tri_state line
				(at 22.86 30.48 180)
				(length 7.62)
				(name "A3")
				(number "1")
			)
			(pin tri_state line
				(at 22.86 27.94 180)
				(length 7.62)
				(name "A4")
				(number "2")
			)
			(pin tri_state line
				(at 22.86 25.4 180)
				(length 7.62)
				(name "A5")
				(number "3")
			)
			(pin tri_state line
				(at 22.86 22.86 180)
				(length 7.62)
				(name "A6")
				(number "4")
			)
			(pin tri_state line
				(at 22.86 20.32 180)
				(length 7.62)
				(name "A7")
				(number "5")
			)
			(pin tri_state line
				(at 22.86 17.78 180)
				(length 7.62)
				(name "A8")
				(number "6")
			)
			(pin tri_state line
				(at 22.86 15.24 180)
				(length 7.62)
				(name "A9")
				(number "7")
			)
			(pin tri_state line
				(at 22.86 12.7 180)
				(length 7.62)
				(name "A10")
				(number "8")
			)
			(pin tri_state line
				(at 22.86 10.16 180)
				(length 7.62)
				(name "A11")
				(number "9")
			)
			(pin tri_state line
				(at 22.86 7.62 180)
				(length 7.62)
				(name "A12")
				(number "10")
			)
			(pin tri_state line
				(at 22.86 5.08 180)
				(length 7.62)
				(name "A13")
				(number "11")
			)
			(pin tri_state line
				(at 22.86 2.54 180)
				(length 7.62)
				(name "A14")
				(number "12")
			)
			(pin tri_state line
				(at 22.86 0 180)
				(length 7.62)
				(name "A15")
				(number "14")
			)
			(pin tri_state line
				(at 22.86 -2.54 180)
				(length 7.62)
				(name "A16")
				(number "16")
			)
			(pin tri_state line
				(at 22.86 -5.08 180)
				(length 7.62)
				(name "A17")
				(number "17")
			)
			(pin tri_state line
				(at 22.86 -7.62 180)
				(length 7.62)
				(name "A18")
				(number "18")
			)
			(pin tri_state line
				(at 22.86 -10.16 180)
				(length 7.62)
				(name "A19")
				(number "19")
			)
			(pin tri_state line
				(at 22.86 -20.32 180)
				(length 7.62)
				(name "D0")
				(number "27")
			)
			(pin tri_state line
				(at 22.86 -22.86 180)
				(length 7.62)
				(name "D1")
				(number "26")
			)
			(pin tri_state line
				(at 22.86 -25.4 180)
				(length 7.62)
				(name "D2")
				(number "25")
			)
			(pin tri_state line
				(at 22.86 -27.94 180)
				(length 7.62)
				(name "D3")
				(number "24")
			)
			(pin tri_state line
				(at 22.86 -30.48 180)
				(length 7.62)
				(name "D4")
				(number "23")
			)
			(pin tri_state line
				(at 22.86 -33.02 180)
				(length 7.62)
				(name "D5")
				(number "22")
			)
			(pin tri_state line
				(at 22.86 -35.56 180)
				(length 7.62)
				(name "D6")
				(number "21")
			)
			(pin tri_state line
				(at 22.86 -38.1 180)
				(length 7.62)
				(name "D7")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC68000FN"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -16.51 59.69 0)
		)
		(property "Value" "MC68000FN"
			(at 12.7 -59.69 0)
		)
		(property "Footprint" "Package_LCC:PLCC-68"
			(at -19.05 57.15 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/reference-manual/MC68000UM.pdf"
			(at 0 0 0)
		)
		(property "Description" "Microprocessor, 16-bit bus"
			(at 0 0 0)
		)
		(property "ki_keywords" "MPRO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PLCC*"
			(at 0 0 0)
		)
		(symbol "MC68000FN_0_1")
		(symbol "MC68000FN_1_1"
			(pin input clock
				(at -25.4 55.88 0)
				(length 7.62)
				(name "CLK")
				(number "15")
			)
			(pin input inverted
				(at -25.4 48.26 0)
				(length 7.62)
				(name "IPL0")
				(number "27")
			)
			(pin input inverted
				(at -25.4 45.72 0)
				(length 7.62)
				(name "IPL1")
				(number "26")
			)
			(pin input inverted
				(at -25.4 43.18 0)
				(length 7.62)
				(name "IPL2")
				(number "25")
			)
			(pin input inverted
				(at -25.4 38.1 0)
				(length 7.62)
				(name "BGACK")
				(number "12")
			)
			(pin output inverted
				(at -25.4 35.56 0)
				(length 7.62)
				(name "BG")
				(number "11")
			)
			(pin input inverted
				(at -25.4 33.02 0)
				(length 7.62)
				(name "BR")
				(number "13")
			)
			(pin output line
				(at -25.4 25.4 0)
				(length 7.62)
				(name "FC0")
				(number "30")
			)
			(pin output line
				(at -25.4 22.86 0)
				(length 7.62)
				(name "FC1")
				(number "29")
			)
			(pin output line
				(at -25.4 20.32 0)
				(length 7.62)
				(name "FC2")
				(number "28")
			)
			(pin output inverted
				(at -25.4 12.7 0)
				(length 7.62)
				(name "VMA")
				(number "21")
			)
			(pin output line
				(at -25.4 10.16 0)
				(length 7.62)
				(name "E")
				(number "22")
			)
			(pin input inverted
				(at -25.4 7.62 0)
				(length 7.62)
				(name "VPA")
				(number "23")
			)
			(pin input inverted
				(at -25.4 -12.7 0)
				(length 7.62)
				(name "BERR")
				(number "24")
			)
			(pin input inverted
				(at -25.4 -17.78 0)
				(length 7.62)
				(name "DTACK")
				(number "10")
			)
			(pin bidirectional inverted
				(at -25.4 -30.48 0)
				(length 7.62)
				(name "HALT")
				(number "19")
			)
			(pin input inverted
				(at -25.4 -35.56 0)
				(length 7.62)
				(name "RESET")
				(number "20")
			)
			(pin no_connect line
				(at -17.78 -45.72 0)
				(length 0)
				(hide yes)
				(name "NC")
				(number "18")
			)
			(pin no_connect line
				(at -17.78 -48.26 0)
				(length 0)
				(hide yes)
				(name "NC")
				(number "31")
			)
			(pin power_in line
				(at -5.08 -66.04 90)
				(length 7.62)
				(name "GND")
				(number "57")
			)
			(pin power_in line
				(at -2.54 66.04 270)
				(length 7.62)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at -2.54 -66.04 90)
				(length 7.62)
				(name "GND")
				(number "56")
			)
			(pin power_in line
				(at 2.54 66.04 270)
				(length 7.62)
				(name "VCC")
				(number "52")
			)
			(pin power_in line
				(at 2.54 -66.04 90)
				(length 7.62)
				(name "GND")
				(number "16")
			)
			(pin power_in line
				(at 5.08 -66.04 90)
				(length 7.62)
				(name "GND")
				(number "17")
			)
			(pin output line
				(at 25.4 55.88 180)
				(length 7.62)
				(name "A1")
				(number "32")
			)
			(pin output line
				(at 25.4 53.34 180)
				(length 7.62)
				(name "A2")
				(number "33")
			)
			(pin output line
				(at 25.4 50.8 180)
				(length 7.62)
				(name "A3")
				(number "34")
			)
			(pin output line
				(at 25.4 48.26 180)
				(length 7.62)
				(name "A4")
				(number "35")
			)
			(pin output line
				(at 25.4 45.72 180)
				(length 7.62)
				(name "A5")
				(number "36")
			)
			(pin output line
				(at 25.4 43.18 180)
				(length 7.62)
				(name "A6")
				(number "37")
			)
			(pin output line
				(at 25.4 40.64 180)
				(length 7.62)
				(name "A7")
				(number "38")
			)
			(pin output line
				(at 25.4 38.1 180)
				(length 7.62)
				(name "A8")
				(number "39")
			)
			(pin output line
				(at 25.4 35.56 180)
				(length 7.62)
				(name "A9")
				(number "40")
			)
			(pin output line
				(at 25.4 33.02 180)
				(length 7.62)
				(name "A10")
				(number "41")
			)
			(pin output line
				(at 25.4 30.48 180)
				(length 7.62)
				(name "A11")
				(number "42")
			)
			(pin output line
				(at 25.4 27.94 180)
				(length 7.62)
				(name "A12")
				(number "43")
			)
			(pin output line
				(at 25.4 25.4 180)
				(length 7.62)
				(name "A13")
				(number "44")
			)
			(pin output line
				(at 25.4 22.86 180)
				(length 7.62)
				(name "A14")
				(number "45")
			)
			(pin output line
				(at 25.4 20.32 180)
				(length 7.62)
				(name "A15")
				(number "46")
			)
			(pin output line
				(at 25.4 17.78 180)
				(length 7.62)
				(name "A16")
				(number "47")
			)
			(pin output line
				(at 25.4 15.24 180)
				(length 7.62)
				(name "A17")
				(number "48")
			)
			(pin output line
				(at 25.4 12.7 180)
				(length 7.62)
				(name "A18")
				(number "49")
			)
			(pin output line
				(at 25.4 10.16 180)
				(length 7.62)
				(name "A19")
				(number "50")
			)
			(pin output line
				(at 25.4 7.62 180)
				(length 7.62)
				(name "A20")
				(number "51")
			)
			(pin output line
				(at 25.4 5.08 180)
				(length 7.62)
				(name "A21")
				(number "53")
			)
			(pin output line
				(at 25.4 2.54 180)
				(length 7.62)
				(name "A22")
				(number "54")
			)
			(pin output line
				(at 25.4 0 180)
				(length 7.62)
				(name "A23")
				(number "55")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 7.62)
				(name "D0")
				(number "5")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 7.62)
				(name "D1")
				(number "4")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 7.62)
				(name "D2")
				(number "3")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 7.62)
				(name "D3")
				(number "2")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 7.62)
				(name "D4")
				(number "1")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 7.62)
				(name "D5")
				(number "68")
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 7.62)
				(name "D6")
				(number "67")
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 7.62)
				(name "D7")
				(number "66")
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 7.62)
				(name "D8")
				(number "65")
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 7.62)
				(name "D9")
				(number "64")
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 7.62)
				(name "D10")
				(number "63")
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 7.62)
				(name "D11")
				(number "62")
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 7.62)
				(name "D12")
				(number "61")
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 7.62)
				(name "D13")
				(number "60")
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 7.62)
				(name "D14")
				(number "59")
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 7.62)
				(name "D15")
				(number "58")
			)
			(pin output inverted
				(at 25.4 -48.26 180)
				(length 7.62)
				(name "AS")
				(number "6")
			)
			(pin output inverted
				(at 25.4 -50.8 180)
				(length 7.62)
				(name "UDS")
				(number "7")
			)
			(pin output inverted
				(at 25.4 -53.34 180)
				(length 7.62)
				(name "LDS")
				(number "8")
			)
			(pin output line
				(at 25.4 -55.88 180)
				(length 7.62)
				(name "R/W")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC68332"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -24.13 85.09 0)
		)
		(property "Value" "MC68332"
			(at 21.336 85.09 0)
		)
		(property "Footprint" "Package_QFP:PQFP-132_24x24mm_P0.635mm"
			(at 0 -99.06 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheet/motorola/SPAKMC332AVFC20.pdf"
			(at 53.34 58.42 0)
		)
		(property "Description" "MCU 32 bit, PQFP-132"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU 32 bit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PQFP*24x24mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "MC68332_0_1")
		(symbol "MC68332_1_0"
			(pin power_in line
				(at -17.78 -88.9 90)
				(length 5.08)
				(name "VSS")
				(number "2")
			)
		)
		(symbol "MC68332_1_1"
			(pin input line
				(at -33.02 73.66 0)
				(length 7.62)
				(name "TP0")
				(number "16")
			)
			(pin input line
				(at -33.02 71.12 0)
				(length 7.62)
				(name "TP1")
				(number "15")
			)
			(pin input line
				(at -33.02 68.58 0)
				(length 7.62)
				(name "TP2")
				(number "14")
			)
			(pin input line
				(at -33.02 66.04 0)
				(length 7.62)
				(name "TP3")
				(number "13")
			)
			(pin input line
				(at -33.02 63.5 0)
				(length 7.62)
				(name "TP4")
				(number "12")
			)
			(pin input line
				(at -33.02 60.96 0)
				(length 7.62)
				(name "TP5")
				(number "11")
			)
			(pin input line
				(at -33.02 58.42 0)
				(length 7.62)
				(name "TP6")
				(number "10")
			)
			(pin input line
				(at -33.02 55.88 0)
				(length 7.62)
				(name "TP7")
				(number "9")
			)
			(pin input line
				(at -33.02 53.34 0)
				(length 7.62)
				(name "TP8")
				(number "6")
			)
			(pin input line
				(at -33.02 50.8 0)
				(length 7.62)
				(name "TP9")
				(number "5")
			)
			(pin input line
				(at -33.02 48.26 0)
				(length 7.62)
				(name "TP10")
				(number "4")
			)
			(pin input line
				(at -33.02 45.72 0)
				(length 7.62)
				(name "TP11")
				(number "3")
			)
			(pin input line
				(at -33.02 43.18 0)
				(length 7.62)
				(name "TP12")
				(number "132")
			)
			(pin input line
				(at -33.02 40.64 0)
				(length 7.62)
				(name "TP13")
				(number "131")
			)
			(pin input line
				(at -33.02 38.1 0)
				(length 7.62)
				(name "TP14")
				(number "130")
			)
			(pin input line
				(at -33.02 35.56 0)
				(length 7.62)
				(name "TP15")
				(number "129")
			)
			(pin input line
				(at -33.02 33.02 0)
				(length 7.62)
				(name "T2CLK")
				(number "128")
			)
			(pin input line
				(at -33.02 27.94 0)
				(length 7.62)
				(name "VSTBY")
				(number "19")
			)
			(pin input line
				(at -33.02 22.86 0)
				(length 7.62)
				(name "R/W")
				(number "79")
			)
			(pin input line
				(at -33.02 20.32 0)
				(length 7.62)
				(name "MODCK")
				(number "78")
			)
			(pin input line
				(at -33.02 17.78 0)
				(length 7.62)
				(name "IRQ1")
				(number "77")
			)
			(pin input line
				(at -33.02 15.24 0)
				(length 7.62)
				(name "IRQ2")
				(number "76")
			)
			(pin input line
				(at -33.02 12.7 0)
				(length 7.62)
				(name "IRQ3")
				(number "75")
			)
			(pin input line
				(at -33.02 10.16 0)
				(length 7.62)
				(name "IRQ4")
				(number "74")
			)
			(pin input line
				(at -33.02 7.62 0)
				(length 7.62)
				(name "IRQ5")
				(number "73")
			)
			(pin input line
				(at -33.02 5.08 0)
				(length 7.62)
				(name "IRQ6")
				(number "72")
			)
			(pin input line
				(at -33.02 2.54 0)
				(length 7.62)
				(name "IRQ7")
				(number "71")
			)
			(pin input line
				(at -33.02 -2.54 0)
				(length 7.62)
				(name "BERR")
				(number "70")
			)
			(pin input line
				(at -33.02 -5.08 0)
				(length 7.62)
				(name "HALT")
				(number "69")
			)
			(pin input line
				(at -33.02 -7.62 0)
				(length 7.62)
				(name "RESET")
				(number "68")
			)
			(pin output line
				(at -33.02 -10.16 0)
				(length 7.62)
				(name "CLKOUT")
				(number "66")
			)
			(pin input line
				(at -33.02 -12.7 0)
				(length 7.62)
				(name "XFC")
				(number "64")
			)
			(pin input line
				(at -33.02 -15.24 0)
				(length 7.62)
				(name "VDDSYN")
				(number "61")
			)
			(pin input line
				(at -33.02 -20.32 0)
				(length 7.62)
				(name "EXTAL")
				(number "62")
			)
			(pin output line
				(at -33.02 -22.86 0)
				(length 7.62)
				(name "XTAL")
				(number "60")
			)
			(pin output line
				(at -33.02 -27.94 0)
				(length 7.62)
				(name "FREEZE/QUOT")
				(number "58")
			)
			(pin input line
				(at -33.02 -30.48 0)
				(length 7.62)
				(name "TSTME/TSC")
				(number "57")
			)
			(pin input line
				(at -33.02 -33.02 0)
				(length 7.62)
				(name "BKPT/DSCLK")
				(number "56")
			)
			(pin input line
				(at -33.02 -35.56 0)
				(length 7.62)
				(name "IFETCH/DSI")
				(number "55")
			)
			(pin output line
				(at -33.02 -38.1 0)
				(length 7.62)
				(name "IPIPE/DSO")
				(number "54")
			)
			(pin input line
				(at -33.02 -43.18 0)
				(length 7.62)
				(name "RXD")
				(number "53")
			)
			(pin input line
				(at -33.02 -45.72 0)
				(length 7.62)
				(name "TXD")
				(number "52")
			)
			(pin input line
				(at -33.02 -48.26 0)
				(length 7.62)
				(name "PCS3")
				(number "49")
			)
			(pin input line
				(at -33.02 -50.8 0)
				(length 7.62)
				(name "PCS2")
				(number "48")
			)
			(pin input line
				(at -33.02 -53.34 0)
				(length 7.62)
				(name "PCS1")
				(number "47")
			)
			(pin input line
				(at -33.02 -55.88 0)
				(length 7.62)
				(name "PSCO/SS")
				(number "46")
			)
			(pin input line
				(at -33.02 -58.42 0)
				(length 7.62)
				(name "SCK")
				(number "45")
			)
			(pin input line
				(at -33.02 -60.96 0)
				(length 7.62)
				(name "MOSI")
				(number "44")
			)
			(pin input line
				(at -33.02 -63.5 0)
				(length 7.62)
				(name "MISO")
				(number "43")
			)
			(pin power_in line
				(at -15.24 88.9 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at -15.24 -88.9 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at -12.7 88.9 270)
				(length 5.08)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at -12.7 -88.9 90)
				(length 5.08)
				(name "VSS")
				(number "17")
			)
			(pin power_in line
				(at -10.16 88.9 270)
				(length 5.08)
				(name "VDD")
				(number "18")
			)
			(pin power_in line
				(at -10.16 -88.9 90)
				(length 5.08)
				(name "VSS")
				(number "29")
			)
			(pin power_in line
				(at -7.62 88.9 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -7.62 -88.9 90)
				(length 5.08)
				(name "VSS")
				(number "34")
			)
			(pin power_in line
				(at -5.08 88.9 270)
				(length 5.08)
				(name "VDD")
				(number "39")
			)
			(pin power_in line
				(at -5.08 -88.9 90)
				(length 5.08)
				(name "VSS")
				(number "40")
			)
			(pin power_in line
				(at -2.54 88.9 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at -2.54 -88.9 90)
				(length 5.08)
				(name "VSS")
				(number "51")
			)
			(pin power_in line
				(at 0 88.9 270)
				(length 5.08)
				(name "VDD")
				(number "63")
			)
			(pin power_in line
				(at 0 -88.9 90)
				(length 5.08)
				(name "VSS")
				(number "59")
			)
			(pin power_in line
				(at 2.54 88.9 270)
				(length 5.08)
				(name "VDD")
				(number "65")
			)
			(pin power_in line
				(at 2.54 -88.9 90)
				(length 5.08)
				(name "VSS")
				(number "67")
			)
			(pin power_in line
				(at 5.08 88.9 270)
				(length 5.08)
				(name "VDD")
				(number "84")
			)
			(pin power_in line
				(at 5.08 -88.9 90)
				(length 5.08)
				(name "VSS")
				(number "83")
			)
			(pin power_in line
				(at 7.62 88.9 270)
				(length 5.08)
				(name "VDD")
				(number "96")
			)
			(pin power_in line
				(at 7.62 -88.9 90)
				(length 5.08)
				(name "VSS")
				(number "95")
			)
			(pin power_in line
				(at 10.16 88.9 270)
				(length 5.08)
				(name "VDD")
				(number "107")
			)
			(pin power_in line
				(at 10.16 -88.9 90)
				(length 5.08)
				(name "VSS")
				(number "101")
			)
			(pin power_in line
				(at 12.7 88.9 270)
				(length 5.08)
				(name "VDD")
				(number "116")
			)
			(pin power_in line
				(at 12.7 -88.9 90)
				(length 5.08)
				(name "VSS")
				(number "106")
			)
			(pin power_in line
				(at 15.24 88.9 270)
				(length 5.08)
				(name "VDD")
				(number "126")
			)
			(pin power_in line
				(at 15.24 -88.9 90)
				(length 5.08)
				(name "VSS")
				(number "117")
			)
			(pin power_in line
				(at 17.78 -88.9 90)
				(length 5.08)
				(name "VSS")
				(number "127")
			)
			(pin output line
				(at 33.02 73.66 180)
				(length 7.62)
				(name "A23/CS10")
				(number "125")
			)
			(pin output line
				(at 33.02 71.12 180)
				(length 7.62)
				(name "A22/CS9")
				(number "124")
			)
			(pin output line
				(at 33.02 68.58 180)
				(length 7.62)
				(name "A21/CS8")
				(number "123")
			)
			(pin output line
				(at 33.02 66.04 180)
				(length 7.62)
				(name "A20/CS7")
				(number "122")
			)
			(pin output line
				(at 33.02 63.5 180)
				(length 7.62)
				(name "A19/CS6")
				(number "121")
			)
			(pin output line
				(at 33.02 60.96 180)
				(length 7.62)
				(name "FC2/CS5")
				(number "120")
			)
			(pin output line
				(at 33.02 58.42 180)
				(length 7.62)
				(name "FC1/CS4")
				(number "119")
			)
			(pin output line
				(at 33.02 55.88 180)
				(length 7.62)
				(name "FC0/CS3")
				(number "118")
			)
			(pin input line
				(at 33.02 53.34 180)
				(length 7.62)
				(name "BGACK/CS2")
				(number "115")
			)
			(pin output line
				(at 33.02 50.8 180)
				(length 7.62)
				(name "BG/CS1")
				(number "114")
			)
			(pin input line
				(at 33.02 48.26 180)
				(length 7.62)
				(name "BR/CS0")
				(number "113")
			)
			(pin output line
				(at 33.02 43.18 180)
				(length 7.62)
				(name "CSBOOT")
				(number "112")
			)
			(pin output line
				(at 33.02 38.1 180)
				(length 7.62)
				(name "A18")
				(number "42")
			)
			(pin output line
				(at 33.02 35.56 180)
				(length 7.62)
				(name "A17")
				(number "41")
			)
			(pin output line
				(at 33.02 33.02 180)
				(length 7.62)
				(name "A16")
				(number "38")
			)
			(pin output line
				(at 33.02 30.48 180)
				(length 7.62)
				(name "A15")
				(number "37")
			)
			(pin output line
				(at 33.02 27.94 180)
				(length 7.62)
				(name "A14")
				(number "36")
			)
			(pin output line
				(at 33.02 25.4 180)
				(length 7.62)
				(name "A13")
				(number "35")
			)
			(pin output line
				(at 33.02 22.86 180)
				(length 7.62)
				(name "A12")
				(number "33")
			)
			(pin output line
				(at 33.02 20.32 180)
				(length 7.62)
				(name "A11")
				(number "32")
			)
			(pin output line
				(at 33.02 17.78 180)
				(length 7.62)
				(name "A10")
				(number "31")
			)
			(pin output line
				(at 33.02 15.24 180)
				(length 7.62)
				(name "A9")
				(number "30")
			)
			(pin output line
				(at 33.02 12.7 180)
				(length 7.62)
				(name "A8")
				(number "27")
			)
			(pin output line
				(at 33.02 10.16 180)
				(length 7.62)
				(name "A7")
				(number "26")
			)
			(pin output line
				(at 33.02 7.62 180)
				(length 7.62)
				(name "A6")
				(number "25")
			)
			(pin output line
				(at 33.02 5.08 180)
				(length 7.62)
				(name "A5")
				(number "24")
			)
			(pin output line
				(at 33.02 2.54 180)
				(length 7.62)
				(name "A4")
				(number "23")
			)
			(pin output line
				(at 33.02 0 180)
				(length 7.62)
				(name "A3")
				(number "22")
			)
			(pin output line
				(at 33.02 -2.54 180)
				(length 7.62)
				(name "A2")
				(number "21")
			)
			(pin output line
				(at 33.02 -5.08 180)
				(length 7.62)
				(name "A1")
				(number "20")
			)
			(pin output line
				(at 33.02 -7.62 180)
				(length 7.62)
				(name "A0")
				(number "90")
			)
			(pin input line
				(at 33.02 -12.7 180)
				(length 7.62)
				(name "D0")
				(number "111")
			)
			(pin input line
				(at 33.02 -15.24 180)
				(length 7.62)
				(name "D1")
				(number "110")
			)
			(pin input line
				(at 33.02 -17.78 180)
				(length 7.62)
				(name "D2")
				(number "109")
			)
			(pin input line
				(at 33.02 -20.32 180)
				(length 7.62)
				(name "D3")
				(number "108")
			)
			(pin input line
				(at 33.02 -22.86 180)
				(length 7.62)
				(name "D4")
				(number "105")
			)
			(pin input line
				(at 33.02 -25.4 180)
				(length 7.62)
				(name "D5")
				(number "104")
			)
			(pin input line
				(at 33.02 -27.94 180)
				(length 7.62)
				(name "D6")
				(number "103")
			)
			(pin input line
				(at 33.02 -30.48 180)
				(length 7.62)
				(name "D7")
				(number "102")
			)
			(pin input line
				(at 33.02 -33.02 180)
				(length 7.62)
				(name "D8")
				(number "100")
			)
			(pin input line
				(at 33.02 -35.56 180)
				(length 7.62)
				(name "D9")
				(number "99")
			)
			(pin input line
				(at 33.02 -38.1 180)
				(length 7.62)
				(name "D10")
				(number "98")
			)
			(pin input line
				(at 33.02 -40.64 180)
				(length 7.62)
				(name "D11")
				(number "97")
			)
			(pin input line
				(at 33.02 -43.18 180)
				(length 7.62)
				(name "D12")
				(number "94")
			)
			(pin input line
				(at 33.02 -45.72 180)
				(length 7.62)
				(name "D13")
				(number "93")
			)
			(pin input line
				(at 33.02 -48.26 180)
				(length 7.62)
				(name "D14")
				(number "92")
			)
			(pin input line
				(at 33.02 -50.8 180)
				(length 7.62)
				(name "D15")
				(number "91")
			)
			(pin input line
				(at 33.02 -55.88 180)
				(length 7.62)
				(name "DSACK0")
				(number "89")
			)
			(pin input line
				(at 33.02 -58.42 180)
				(length 7.62)
				(name "DSACK1")
				(number "88")
			)
			(pin input line
				(at 33.02 -60.96 180)
				(length 7.62)
				(name "AVEC")
				(number "87")
			)
			(pin input line
				(at 33.02 -63.5 180)
				(length 7.62)
				(name "RMC")
				(number "86")
			)
			(pin input line
				(at 33.02 -66.04 180)
				(length 7.62)
				(name "DS")
				(number "85")
			)
			(pin input line
				(at 33.02 -68.58 180)
				(length 7.62)
				(name "AS")
				(number "82")
			)
			(pin input line
				(at 33.02 -71.12 180)
				(length 7.62)
				(name "SIZ0")
				(number "81")
			)
			(pin input line
				(at 33.02 -73.66 180)
				(length 7.62)
				(name "SIZ1")
				(number "80")
			)
		)
		(embedded_fonts no)
	)
	(symbol "68010D"
		(extends "68000D")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "68010D"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/reference-manual/MC68000UM.pdf"
			(at 0 0 0)
		)
		(property "Description" "16/32-bit Microprocessor"
			(at 0 0 0)
		)
		(property "ki_keywords" "68000 Microprocessor CPU"
			(at 0 0 0)
		)
	)
)
