(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "MCIMX6QP5EYM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 15.24 90.17 0)
		)
		(property "Value" "MCIMX6QP5EYM"
			(at -13.97 90.17 0)
		)
		(property "Footprint" "Package_BGA:BGA-624_21x21mm_Layout25x25_P0.8mm"
			(at -13.97 55.88 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/IMX6DQPCEC.pdf"
			(at -11.43 55.88 0)
		)
		(property "Description" "i.MX 6QuadPlus Application Processor for Consumer Products, BGA-624"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "Quad-Core ARM Cortex A9 SOC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "BGA*21x21mm*Layout25x25*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "MCIMX6QP5EYM_1_0"
			(text "Power Management"
				(at -1.27 -5.08 0)
			)
		)
		(symbol "MCIMX6QP5EYM_1_1"
			(pin power_in line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "VDD_ARM_IN")
				(number "H14")
			)
			(pin passive line
				(at -25.4 10.16 0)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM_IN")
				(number "J14")
			)
			(pin passive line
				(at -25.4 10.16 0)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM_IN")
				(number "K14")
			)
			(pin passive line
				(at -25.4 10.16 0)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM_IN")
				(number "L14")
			)
			(pin passive line
				(at -25.4 10.16 0)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM_IN")
				(number "M14")
			)
			(pin passive line
				(at -25.4 10.16 0)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM_IN")
				(number "N14")
			)
			(pin passive line
				(at -25.4 10.16 0)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM_IN")
				(number "P14")
			)
			(pin passive line
				(at -25.4 10.16 0)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM_IN")
				(number "R14")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "VDD_ARM23_IN")
				(number "K9")
			)
			(pin passive line
				(at -25.4 7.62 0)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM23_IN")
				(number "L9")
			)
			(pin passive line
				(at -25.4 7.62 0)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM23_IN")
				(number "M9")
			)
			(pin passive line
				(at -25.4 7.62 0)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM23_IN")
				(number "N9")
			)
			(pin passive line
				(at -25.4 7.62 0)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM23_IN")
				(number "P9")
			)
			(pin passive line
				(at -25.4 7.62 0)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM23_IN")
				(number "R9")
			)
			(pin passive line
				(at -25.4 7.62 0)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM23_IN")
				(number "T9")
			)
			(pin passive line
				(at -25.4 7.62 0)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM23_IN")
				(number "U9")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "VDD_SOC_IN")
				(number "H16")
			)
			(pin passive line
				(at -25.4 5.08 0)
				(length 5.08)
				(hide yes)
				(name "VDD_SOC_IN")
				(number "J16")
			)
			(pin passive line
				(at -25.4 5.08 0)
				(length 5.08)
				(hide yes)
				(name "VDD_SOC_IN")
				(number "K16")
			)
			(pin passive line
				(at -25.4 5.08 0)
				(length 5.08)
				(hide yes)
				(name "VDD_SOC_IN")
				(number "L16")
			)
			(pin passive line
				(at -25.4 5.08 0)
				(length 5.08)
				(hide yes)
				(name "VDD_SOC_IN")
				(number "M16")
			)
			(pin passive line
				(at -25.4 5.08 0)
				(length 5.08)
				(hide yes)
				(name "VDD_SOC_IN")
				(number "N16")
			)
			(pin passive line
				(at -25.4 5.08 0)
				(length 5.08)
				(hide yes)
				(name "VDD_SOC_IN")
				(number "P16")
			)
			(pin passive line
				(at -25.4 5.08 0)
				(length 5.08)
				(hide yes)
				(name "VDD_SOC_IN")
				(number "R16")
			)
			(pin passive line
				(at -25.4 5.08 0)
				(length 5.08)
				(hide yes)
				(name "VDD_SOC_IN")
				(number "T16")
			)
			(pin passive line
				(at -25.4 5.08 0)
				(length 5.08)
				(hide yes)
				(name "VDD_SOC_IN")
				(number "U16")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 5.08)
				(name "VDD_HIGH_IN")
				(number "H9")
			)
			(pin passive line
				(at -25.4 0 0)
				(length 5.08)
				(hide yes)
				(name "VDD_HIGH_IN")
				(number "J9")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "VDD_SNVS_IN")
				(number "G11")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 5.08)
				(name "GND")
				(number "A13")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "A25")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "A4")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "A8")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AA10")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AA13")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AA16")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AA19")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AA22")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AA7")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AB24")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AB3")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AD10")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AD13")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AD16")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AD19")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AD22")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AD4")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AD7")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AE1")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AE25")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "B4")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "C1")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "C10")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "C4")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "C6")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "D3")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "D6")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "D8")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "E5")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "E6")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "E7")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "F5")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "F6")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "F7")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "F8")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "G10")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "G19")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "G3")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "H12")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "H15")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "H18")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "H8")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "J12")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "J15")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "J18")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "J2")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "J8")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "K10")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "K12")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "K15")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "K18")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "K8")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L10")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L12")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L15")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L18")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L2")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L5")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L8")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "M10")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "M12")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "M15")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "M18")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "M8")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "N10")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "N15")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "N18")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "N8")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "P10")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "P12")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "P15")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "P18")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "P8")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "R12")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "R15")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "R17")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "R8")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "T11")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "T12")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "T15")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "T17")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "T19")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "T8")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U11")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U12")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U15")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U17")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U19")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U8")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V19")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V8")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W10")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W11")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W12")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W13")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W15")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W16")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W17")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W18")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W19")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W3")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W7")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W8")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W9")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "Y24")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "Y5")
			)
			(pin power_out line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "VDD_ARM_CAP")
				(number "H13")
			)
			(pin passive line
				(at 25.4 10.16 180)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM_CAP")
				(number "J13")
			)
			(pin passive line
				(at 25.4 10.16 180)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM_CAP")
				(number "K13")
			)
			(pin passive line
				(at 25.4 10.16 180)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM_CAP")
				(number "L13")
			)
			(pin passive line
				(at 25.4 10.16 180)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM_CAP")
				(number "M13")
			)
			(pin passive line
				(at 25.4 10.16 180)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM_CAP")
				(number "N13")
			)
			(pin passive line
				(at 25.4 10.16 180)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM_CAP")
				(number "P13")
			)
			(pin passive line
				(at 25.4 10.16 180)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM_CAP")
				(number "R13")
			)
			(pin power_out line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "VDD_ARM23_CAP")
				(number "H11")
			)
			(pin passive line
				(at 25.4 7.62 180)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM23_CAP")
				(number "J11")
			)
			(pin passive line
				(at 25.4 7.62 180)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM23_CAP")
				(number "K11")
			)
			(pin passive line
				(at 25.4 7.62 180)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM23_CAP")
				(number "L11")
			)
			(pin passive line
				(at 25.4 7.62 180)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM23_CAP")
				(number "M11")
			)
			(pin passive line
				(at 25.4 7.62 180)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM23_CAP")
				(number "N11")
			)
			(pin passive line
				(at 25.4 7.62 180)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM23_CAP")
				(number "P11")
			)
			(pin passive line
				(at 25.4 7.62 180)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM23_CAP")
				(number "R11")
			)
			(pin power_out line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "VDD_SOC_CAP")
				(number "R10")
			)
			(pin passive line
				(at 25.4 5.08 180)
				(length 5.08)
				(hide yes)
				(name "VDD_SOC_CAP")
				(number "T10")
			)
			(pin passive line
				(at 25.4 5.08 180)
				(length 5.08)
				(hide yes)
				(name "VDD_SOC_CAP")
				(number "T13")
			)
			(pin passive line
				(at 25.4 5.08 180)
				(length 5.08)
				(hide yes)
				(name "VDD_SOC_CAP")
				(number "T14")
			)
			(pin passive line
				(at 25.4 5.08 180)
				(length 5.08)
				(hide yes)
				(name "VDD_SOC_CAP")
				(number "U10")
			)
			(pin passive line
				(at 25.4 5.08 180)
				(length 5.08)
				(hide yes)
				(name "VDD_SOC_CAP")
				(number "U13")
			)
			(pin passive line
				(at 25.4 5.08 180)
				(length 5.08)
				(hide yes)
				(name "VDD_SOC_CAP")
				(number "U14")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "VDD_CACHE_CAP")
				(number "N12")
			)
			(pin power_out line
				(at 25.4 0 180)
				(length 5.08)
				(name "VDD_HIGH_CAP")
				(number "H10")
			)
			(pin passive line
				(at 25.4 0 180)
				(length 5.08)
				(hide yes)
				(name "VDD_HIGH_CAP")
				(number "J10")
			)
			(pin power_out line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "VDD_SNVS_CAP")
				(number "G9")
			)
			(pin power_out line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "VDD_PU_CAP")
				(number "H17")
			)
			(pin passive line
				(at 25.4 -5.08 180)
				(length 5.08)
				(hide yes)
				(name "VDD_PU_CAP")
				(number "J17")
			)
			(pin passive line
				(at 25.4 -5.08 180)
				(length 5.08)
				(hide yes)
				(name "VDD_PU_CAP")
				(number "K17")
			)
			(pin passive line
				(at 25.4 -5.08 180)
				(length 5.08)
				(hide yes)
				(name "VDD_PU_CAP")
				(number "L17")
			)
			(pin passive line
				(at 25.4 -5.08 180)
				(length 5.08)
				(hide yes)
				(name "VDD_PU_CAP")
				(number "M17")
			)
			(pin passive line
				(at 25.4 -5.08 180)
				(length 5.08)
				(hide yes)
				(name "VDD_PU_CAP")
				(number "N17")
			)
			(pin passive line
				(at 25.4 -5.08 180)
				(length 5.08)
				(hide yes)
				(name "VDD_PU_CAP")
				(number "P17")
			)
			(pin power_out line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "VDD_USB_CAP")
				(number "F9")
			)
			(pin power_out line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "NVCC_PLL_OUT")
				(number "E8")
			)
		)
		(symbol "MCIMX6QP5EYM_2_0"
			(text "Factory (NXP only)"
				(at -10.16 0 0)
			)
		)
		(symbol "MCIMX6QP5EYM_2_1"
			(pin passive line
				(at 0 10.16 270)
				(length 5.08)
				(name "VDD_FA")
				(number "B5")
			)
			(pin passive line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "FA_ANA")
				(number "A5")
			)
			(pin passive line
				(at 25.4 0 180)
				(length 5.08)
				(name "GPANAIO")
				(number "C8")
			)
			(pin passive line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "TEST_MODE")
				(number "E12")
			)
		)
		(symbol "MCIMX6QP5EYM_3_0"
			(text "Boot/Power Management"
				(at 1.27 -5.08 0)
			)
		)
		(symbol "MCIMX6QP5EYM_3_1"
			(text "VDD_SNVS_IN"
				(at 0 0 0)
			)
			(pin input line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "BOOT_MODE0")
				(number "C12")
			)
			(pin input line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "BOOT_MODE1")
				(number "F12")
			)
			(pin input line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "ONOFF")
				(number "D12")
			)
			(pin input line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "POR_B")
				(number "C11")
			)
			(pin output line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PMIC_ON_REQ")
				(number "D11")
			)
			(pin output line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "PMIC_STBY_REQ")
				(number "F11")
			)
			(pin input line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "TAMPER")
				(number "E11")
			)
		)
		(symbol "MCIMX6QP5EYM_4_0"
			(text "Clock"
				(at -16.51 11.43 0)
			)
			(text "MediaLB"
				(at 15.24 11.43 0)
			)
		)
		(symbol "MCIMX6QP5EYM_4_1"
			(text "VDD_HIGH_CAP"
				(at 0 0 0)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "CLK1_N")
				(number "C7")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "CLK1_P")
				(number "D7")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "CLK2_N")
				(number "C5")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "CLK2_P")
				(number "D5")
			)
			(pin input line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "MLB_CN")
				(number "A11")
			)
			(pin input line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "MLB_CP")
				(number "B11")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "MLB_DN")
				(number "B10")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "MLB_DP")
				(number "A10")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "MLB_SN")
				(number "A9")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "MLB_SP")
				(number "B9")
			)
		)
		(symbol "MCIMX6QP5EYM_5_0"
			(text "MIPI Camera"
				(at 0 0 0)
			)
		)
		(symbol "MCIMX6QP5EYM_5_1"
			(pin input line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "CSI_CLK0M")
				(number "F4")
			)
			(pin input line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "CSI_CLK0P")
				(number "F3")
			)
			(pin input line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "CSI_D0M")
				(number "E4")
			)
			(pin input line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "CSI_D0P")
				(number "E3")
			)
			(pin input line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "CSI_D1M")
				(number "D1")
			)
			(pin input line
				(at -25.4 0 0)
				(length 5.08)
				(name "CSI_D1P")
				(number "D2")
			)
			(pin input line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "CSI_D2M")
				(number "E1")
			)
			(pin input line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "CSI_D2P")
				(number "E2")
			)
			(pin input line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "CSI_D3M")
				(number "F2")
			)
			(pin input line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "CSI_D3P")
				(number "F1")
			)
			(pin passive line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "CSI_REXT")
				(number "D4")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 5.08)
				(name "NVCC_MIPI")
				(number "K7")
			)
			(pin output line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "DSI_CLK0M")
				(number "H3")
			)
			(pin output line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "DSI_CLK0P")
				(number "H4")
			)
			(pin output line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "DSI_D0M")
				(number "G2")
			)
			(pin output line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "DSI_D0P")
				(number "G1")
			)
			(pin output line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "DSI_D1M")
				(number "H2")
			)
			(pin output line
				(at 25.4 0 180)
				(length 5.08)
				(name "DSI_D1P")
				(number "H1")
			)
			(pin passive line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "DSI_REXT")
				(number "G4")
			)
		)
		(symbol "MCIMX6QP5EYM_6_0"
			(text "Camera"
				(at 0 0 0)
			)
		)
		(symbol "MCIMX6QP5EYM_6_1"
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "CSI0_MCLK")
				(number "P4")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "CSI0_PIXCLK")
				(number "P1")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "CSI0_DATA_EN")
				(number "P3")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "CSI0_VSYNC")
				(number "N2")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "CSI0_DAT4")
				(number "N1")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "CSI0_DAT5")
				(number "P2")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "CSI0_DAT6")
				(number "N4")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "CSI0_DAT7")
				(number "N3")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "CSI0_DAT8")
				(number "N6")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "CSI0_DAT9")
				(number "N5")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 5.08)
				(name "NVCC_CSI")
				(number "N7")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "CSI0_DAT10")
				(number "M1")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "CSI0_DAT11")
				(number "M3")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "CSI0_DAT12")
				(number "M2")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "CSI0_DAT13")
				(number "L1")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "CSI0_DAT14")
				(number "M4")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "CSI0_DAT15")
				(number "M5")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "CSI0_DAT16")
				(number "L4")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "CSI0_DAT17")
				(number "L3")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "CSI0_DAT18")
				(number "M6")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "CSI0_DAT19")
				(number "L6")
			)
		)
		(symbol "MCIMX6QP5EYM_7_0"
			(text "LCD Display"
				(at 0 0 0)
			)
		)
		(symbol "MCIMX6QP5EYM_7_1"
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "DI0_DISP_CLK")
				(number "N19")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "DI0_PIN15")
				(number "N21")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "DI0_PIN2")
				(number "N25")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "DI0_PIN3")
				(number "N20")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "DI0_PIN4")
				(number "P25")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "DISP0_DAT0")
				(number "P24")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "DISP0_DAT1")
				(number "P22")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "DISP0_DAT2")
				(number "P23")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "DISP0_DAT3")
				(number "P21")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "DISP0_DAT4")
				(number "P20")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "DISP0_DAT5")
				(number "R25")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "DISP0_DAT6")
				(number "R23")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "DISP0_DAT7")
				(number "R24")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "DISP0_DAT8")
				(number "R22")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "DISP0_DAT9")
				(number "T25")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 5.08)
				(name "NVCC_LCD")
				(number "P19")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "DISP0_DAT10")
				(number "R21")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "DISP0_DAT11")
				(number "T23")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "DISP0_DAT12")
				(number "T24")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "DISP0_DAT13")
				(number "R20")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "DISP0_DAT14")
				(number "U25")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "DISP0_DAT15")
				(number "T22")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "DISP0_DAT16")
				(number "T21")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "DISP0_DAT17")
				(number "U24")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "DISP0_DAT18")
				(number "V25")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "DISP0_DAT19")
				(number "U23")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "DISP0_DAT20")
				(number "U22")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "DISP0_DAT21")
				(number "T20")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "DISP0_DAT22")
				(number "V24")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "DISP0_DAT23")
				(number "W24")
			)
		)
		(symbol "MCIMX6QP5EYM_8_0"
			(text "External memory"
				(at 1.27 0 0)
			)
		)
		(symbol "MCIMX6QP5EYM_8_1"
			(pin bidirectional line
				(at -25.4 40.64 0)
				(length 5.08)
				(name "EIM_A16")
				(number "H25")
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 5.08)
				(name "EIM_A17")
				(number "G24")
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 5.08)
				(name "EIM_A18")
				(number "J22")
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 5.08)
				(name "EIM_A19")
				(number "G25")
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 5.08)
				(name "EIM_A20")
				(number "H22")
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 5.08)
				(name "EIM_A21")
				(number "H23")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "EIM_A22")
				(number "F24")
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "EIM_A23")
				(number "J21")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "EIM_A24")
				(number "F25")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "EIM_A25")
				(number "H19")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "EIM_EB0")
				(number "K21")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "EIM_EB1")
				(number "K23")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "EIM_EB2")
				(number "E22")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "EIM_EB3")
				(number "F23")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "EIM_BCLK")
				(number "N22")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "EIM_LBA")
				(number "K22")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "EIM_OE")
				(number "J24")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "EIM_RW")
				(number "K20")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "EIM_WAIT")
				(number "M25")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "EIM_CS0")
				(number "H24")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "EIM_CS1")
				(number "J23")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 5.08)
				(name "NVCC_EIM0")
				(number "K19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 5.08)
				(name "NVCC_EIM1")
				(number "L19")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 5.08)
				(name "NVCC_EIM2")
				(number "M19")
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 5.08)
				(name "EIM_DA0")
				(number "L20")
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 5.08)
				(name "EIM_DA1")
				(number "J25")
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 5.08)
				(name "EIM_DA2")
				(number "L21")
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 5.08)
				(name "EIM_DA3")
				(number "K24")
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 5.08)
				(name "EIM_DA4")
				(number "L22")
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 5.08)
				(name "EIM_DA5")
				(number "L23")
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "EIM_DA6")
				(number "K25")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 5.08)
				(name "EIM_DA7")
				(number "L25")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "EIM_DA8")
				(number "L24")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "EIM_DA9")
				(number "M21")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "EIM_DA10")
				(number "M22")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "EIM_DA11")
				(number "M20")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "EIM_DA12")
				(number "M24")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "EIM_DA13")
				(number "M23")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "EIM_DA14")
				(number "N23")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "EIM_DA15")
				(number "N24")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "EIM_D16")
				(number "C25")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "EIM_D17")
				(number "F21")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "EIM_D18")
				(number "D24")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "EIM_D19")
				(number "G21")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "EIM_D20")
				(number "G20")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "EIM_D21")
				(number "H20")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "EIM_D22")
				(number "E23")
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 5.08)
				(name "EIM_D23")
				(number "D25")
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "EIM_D24")
				(number "F22")
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "EIM_D25")
				(number "G22")
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "EIM_D26")
				(number "E24")
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "EIM_D27")
				(number "E25")
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 5.08)
				(name "EIM_D28")
				(number "G23")
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 5.08)
				(name "EIM_D29")
				(number "J19")
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 5.08)
				(name "EIM_D30")
				(number "J20")
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 5.08)
				(name "EIM_D31")
				(number "H21")
			)
		)
		(symbol "MCIMX6QP5EYM_9_0"
			(text "10/100-Mbit Ethernet"
				(at -2.54 -7.62 0)
			)
		)
		(symbol "MCIMX6QP5EYM_9_1"
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "ENET_RXD0")
				(number "W21")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "ENET_RXD1")
				(number "W22")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "ENET_CRS_DV")
				(number "U21")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "ENET_RX_ER")
				(number "W23")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "ENET_REF_CLK")
				(number "V22")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "NVCC_ENET")
				(number "R19")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "ENET_TXD0")
				(number "U20")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "ENET_TXD1")
				(number "W20")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "ENET_TX_EN")
				(number "V21")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "ENET_MDC")
				(number "V20")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "ENET_MDIO")
				(number "V23")
			)
		)
		(symbol "MCIMX6QP5EYM_10_0"
			(text "GPIO"
				(at 0 0 0)
			)
		)
		(symbol "MCIMX6QP5EYM_10_1"
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "GPIO_0")
				(number "T5")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "GPIO_1")
				(number "T4")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "GPIO_2")
				(number "T1")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "GPIO_3")
				(number "R7")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "GPIO_4")
				(number "R6")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "GPIO_5")
				(number "R4")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "GPIO_6")
				(number "T3")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "GPIO_7")
				(number "R3")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "GPIO_8")
				(number "R5")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "GPIO_9")
				(number "T2")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "GPIO_16")
				(number "R2")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "GPIO_17")
				(number "R1")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "GPIO_18")
				(number "P6")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "GPIO_19")
				(number "P5")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 5.08)
				(name "NVCC_GPIO")
				(number "P7")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "KEY_COL0")
				(number "W5")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "KEY_COL1")
				(number "U7")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "KEY_COL2")
				(number "W6")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "KEY_COL3")
				(number "U5")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "KEY_COL4")
				(number "T6")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "KEY_ROW0")
				(number "V6")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "KEY_ROW1")
				(number "U6")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "KEY_ROW2")
				(number "W4")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "KEY_ROW3")
				(number "T7")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "KEY_ROW4")
				(number "V5")
			)
		)
		(symbol "MCIMX6QP5EYM_11_0"
			(text "HDMI Display"
				(at 0 0 0)
			)
		)
		(symbol "MCIMX6QP5EYM_11_1"
			(pin input line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "HDMI_HPD")
				(number "K1")
			)
			(pin passive line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "HDMI_DDCCEC")
				(number "K2")
			)
			(pin passive line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "HDMI_REF")
				(number "J1")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 5.08)
				(name "HDMI_VP")
				(number "L7")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 5.08)
				(name "HDMI_VPH")
				(number "M7")
			)
			(pin output line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "HDMI_CLKM")
				(number "J5")
			)
			(pin output line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "HDMI_CLKP")
				(number "J6")
			)
			(pin output line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "HDMI_D0M")
				(number "K5")
			)
			(pin output line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "HDMI_D0P")
				(number "K6")
			)
			(pin output line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "HDMI_D1M")
				(number "J3")
			)
			(pin output line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "HDMI_D1P")
				(number "J4")
			)
			(pin output line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "HDMI_D2M")
				(number "K3")
			)
			(pin output line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "HDMI_D2P")
				(number "K4")
			)
		)
		(symbol "MCIMX6QP5EYM_12_0"
			(text "JTAG Debug"
				(at 0 -5.08 0)
			)
		)
		(symbol "MCIMX6QP5EYM_12_1"
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "NVCC_JTAG")
				(number "J7")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "JTAG_TMS")
				(number "C3")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "JTAG_TCK")
				(number "H5")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "JTAG_TDO")
				(number "G6")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "JTAG_TDI")
				(number "G5")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "JTAG_TRSTB")
				(number "C2")
			)
			(pin input line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "JTAG_MOD")
				(number "H6")
			)
		)
		(symbol "MCIMX6QP5EYM_13_0"
			(text "LVDS Display"
				(at 0 2.54 0)
			)
		)
		(symbol "MCIMX6QP5EYM_13_1"
			(pin output line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "LVDS0_CLK_N")
				(number "V4")
			)
			(pin output line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "LVDS0_CLK_P")
				(number "V3")
			)
			(pin output line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "LVDS0_TX0_N")
				(number "U2")
			)
			(pin output line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "LVDS0_TX0_P")
				(number "U1")
			)
			(pin output line
				(at -25.4 0 0)
				(length 5.08)
				(name "LVDS0_TX1_N")
				(number "U4")
			)
			(pin output line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "LVDS0_TX1_P")
				(number "U3")
			)
			(pin output line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "LVDS0_TX2_N")
				(number "V2")
			)
			(pin output line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "LVDS0_TX2_P")
				(number "V1")
			)
			(pin output line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "LVDS0_TX3_N")
				(number "W2")
			)
			(pin output line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "LVDS0_TX3_P")
				(number "W1")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 5.08)
				(name "NVCC_LVDS2P5")
				(number "V7")
			)
			(pin output line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "LVDS1_CLK_N")
				(number "Y3")
			)
			(pin output line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "LVDS1_CLK_P")
				(number "Y4")
			)
			(pin output line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "LVDS1_TX0_N")
				(number "Y1")
			)
			(pin output line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "LVDS1_TX0_P")
				(number "Y2")
			)
			(pin output line
				(at 25.4 0 180)
				(length 5.08)
				(name "LVDS1_TX1_N")
				(number "AA2")
			)
			(pin output line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "LVDS1_TX1_P")
				(number "AA1")
			)
			(pin output line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "LVDS1_TX2_N")
				(number "AB1")
			)
			(pin output line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "LVDS1_TX2_P")
				(number "AB2")
			)
			(pin output line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "LVDS1_TX3_N")
				(number "AA3")
			)
			(pin output line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "LVDS1_TX3_P")
				(number "AA4")
			)
		)
		(symbol "MCIMX6QP5EYM_14_0"
			(text "NAND Flash"
				(at -13.97 24.13 0)
			)
			(text "SD/MMC"
				(at 15.24 24.13 0)
			)
		)
		(symbol "MCIMX6QP5EYM_14_1"
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "NANDF_ALE")
				(number "A16")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "NANDF_CLE")
				(number "C15")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "NANDF_WP_B")
				(number "E15")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "NANDF_RB0")
				(number "B16")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "NANDF_CS0")
				(number "F15")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "NANDF_CS1")
				(number "C16")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "NANDF_CS2")
				(number "A17")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "NANDF_CS3")
				(number "D16")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "NANDF_D0")
				(number "A18")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "NANDF_D1")
				(number "C17")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "NANDF_D2")
				(number "F16")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "NANDF_D3")
				(number "D17")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "NANDF_D4")
				(number "A19")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "NANDF_D5")
				(number "B18")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 5.08)
				(name "NANDF_D6")
				(number "E17")
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "NANDF_D7")
				(number "C18")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 5.08)
				(name "NVCC_NANDF")
				(number "G15")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "SD4_CLK")
				(number "E16")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "SD4_CMD")
				(number "B17")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "SD4_DAT0")
				(number "D18")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "SD4_DAT1")
				(number "B19")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "SD4_DAT2")
				(number "F17")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "SD4_DAT3")
				(number "A20")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "SD4_DAT4")
				(number "E18")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "SD4_DAT5")
				(number "C19")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "SD4_DAT6")
				(number "B20")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "SD4_DAT7")
				(number "D19")
			)
		)
		(symbol "MCIMX6QP5EYM_15_0"
			(text "PCIe 2.0"
				(at 0 -5.08 0)
			)
		)
		(symbol "MCIMX6QP5EYM_15_1"
			(pin passive line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "PCIE_REXT")
				(number "A2")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 5.08)
				(name "PCIE_VPTX")
				(number "G8")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "PCIE_VP")
				(number "H7")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 5.08)
				(name "PCIE_VPH")
				(number "G7")
			)
			(pin input line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PCIE_RXM")
				(number "B1")
			)
			(pin input line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "PCIE_RXP")
				(number "B2")
			)
			(pin output line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "PCIE_TXM")
				(number "A3")
			)
			(pin output line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "PCIE_TXP")
				(number "B3")
			)
		)
		(symbol "MCIMX6QP5EYM_16_0"
			(text "HS USB2.0 Host"
				(at -11.43 6.35 0)
			)
			(text "HS USB2.0 OTG"
				(at 12.7 6.35 0)
			)
		)
		(symbol "MCIMX6QP5EYM_16_1"
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "USB_H1_DP")
				(number "E10")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "USB_H1_DN")
				(number "F10")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 5.08)
				(name "USB_H1_VBUS")
				(number "D10")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 5.08)
				(name "USB_OTG_VBUS")
				(number "E9")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "USB_OTG_DP")
				(number "A6")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "USB_OTG_DN")
				(number "B6")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "USB_OTG_CHD_B")
				(number "B8")
			)
		)
		(symbol "MCIMX6QP5EYM_17_0"
			(text "Gigabit Ethernet"
				(at 0 -5.08 0)
			)
		)
		(symbol "MCIMX6QP5EYM_17_1"
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "RGMII_RXC")
				(number "B25")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "RGMII_RX_CTL")
				(number "D22")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "RGMII_RD0")
				(number "C24")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "RGMII_RD1")
				(number "B23")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "RGMII_RD2")
				(number "B24")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "RGMII_RD3")
				(number "D23")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "NVCC_RGMII")
				(number "G18")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "RGMII_TXC")
				(number "D21")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "RGMII_TX_CTL")
				(number "C23")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "RGMII_TD0")
				(number "C22")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "RGMII_TD1")
				(number "F20")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "RGMII_TD2")
				(number "E21")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "RGMII_TD3")
				(number "A24")
			)
		)
		(symbol "MCIMX6QP5EYM_18_0"
			(text "SD/MMC"
				(at 0 -5.08 0)
			)
		)
		(symbol "MCIMX6QP5EYM_18_1"
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "NVCC_SD1")
				(number "G16")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "SD1_CLK")
				(number "D20")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "SD1_CMD")
				(number "B21")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "SD1_DAT0")
				(number "A21")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "SD1_DAT1")
				(number "C20")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "SD1_DAT2")
				(number "E19")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "SD1_DAT3")
				(number "F18")
			)
		)
		(symbol "MCIMX6QP5EYM_19_0"
			(text "SD/MMC"
				(at 0 -5.08 0)
			)
		)
		(symbol "MCIMX6QP5EYM_19_1"
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "NVCC_SD2")
				(number "G17")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "SD2_CLK")
				(number "C21")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "SD2_CMD")
				(number "F19")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "SD2_DAT0")
				(number "A22")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "SD2_DAT1")
				(number "E20")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "SD2_DAT2")
				(number "A23")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "SD2_DAT3")
				(number "B22")
			)
		)
		(symbol "MCIMX6QP5EYM_20_0"
			(text "SD/MMC"
				(at 0 0 0)
			)
		)
		(symbol "MCIMX6QP5EYM_20_1"
			(pin power_in line
				(at 0 22.86 270)
				(length 5.08)
				(name "NVCC_SD3")
				(number "G14")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "SD3_CLK")
				(number "D14")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "SD3_CMD")
				(number "B13")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "SD3_DAT0")
				(number "E14")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "SD3_DAT1")
				(number "F14")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "SD3_DAT2")
				(number "A15")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "SD3_DAT3")
				(number "B15")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "SD3_DAT4")
				(number "D13")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "SD3_DAT5")
				(number "C13")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "SD3_DAT6")
				(number "E13")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "SD3_DAT7")
				(number "F13")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "SD3_RST")
				(number "D15")
			)
		)
		(symbol "MCIMX6QP5EYM_21_0"
			(text "DDR3/DDR3L/LPDDR2"
				(at 0 -2.54 0)
			)
		)
		(symbol "MCIMX6QP5EYM_21_1"
			(pin bidirectional line
				(at -25.4 86.36 0)
				(length 5.08)
				(name "DRAM_D0")
				(number "AD2")
			)
			(pin bidirectional line
				(at -25.4 83.82 0)
				(length 5.08)
				(name "DRAM_D1")
				(number "AE2")
			)
			(pin bidirectional line
				(at -25.4 81.28 0)
				(length 5.08)
				(name "DRAM_D2")
				(number "AC4")
			)
			(pin bidirectional line
				(at -25.4 78.74 0)
				(length 5.08)
				(name "DRAM_D3")
				(number "AA5")
			)
			(pin bidirectional line
				(at -25.4 76.2 0)
				(length 5.08)
				(name "DRAM_D4")
				(number "AC1")
			)
			(pin bidirectional line
				(at -25.4 73.66 0)
				(length 5.08)
				(name "DRAM_D5")
				(number "AD1")
			)
			(pin bidirectional line
				(at -25.4 71.12 0)
				(length 5.08)
				(name "DRAM_D6")
				(number "AB4")
			)
			(pin bidirectional line
				(at -25.4 68.58 0)
				(length 5.08)
				(name "DRAM_D7")
				(number "AE4")
			)
			(pin bidirectional line
				(at -25.4 66.04 0)
				(length 5.08)
				(name "DRAM_SDQS0")
				(number "AE3")
			)
			(pin bidirectional line
				(at -25.4 63.5 0)
				(length 5.08)
				(name "DRAM_SDQS0_B")
				(number "AD3")
			)
			(pin output line
				(at -25.4 60.96 0)
				(length 5.08)
				(name "DRAM_DQM0")
				(number "AC3")
			)
			(pin bidirectional line
				(at -25.4 55.88 0)
				(length 5.08)
				(name "DRAM_D8")
				(number "AD5")
			)
			(pin bidirectional line
				(at -25.4 53.34 0)
				(length 5.08)
				(name "DRAM_D9")
				(number "AE5")
			)
			(pin bidirectional line
				(at -25.4 50.8 0)
				(length 5.08)
				(name "DRAM_D10")
				(number "AA6")
			)
			(pin bidirectional line
				(at -25.4 48.26 0)
				(length 5.08)
				(name "DRAM_D11")
				(number "AE7")
			)
			(pin bidirectional line
				(at -25.4 45.72 0)
				(length 5.08)
				(name "DRAM_D12")
				(number "AB5")
			)
			(pin bidirectional line
				(at -25.4 43.18 0)
				(length 5.08)
				(name "DRAM_D13")
				(number "AC5")
			)
			(pin bidirectional line
				(at -25.4 40.64 0)
				(length 5.08)
				(name "DRAM_D14")
				(number "AB6")
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 5.08)
				(name "DRAM_D15")
				(number "AC7")
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 5.08)
				(name "DRAM_SDQS1")
				(number "AD6")
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 5.08)
				(name "DRAM_SDQS1_B")
				(number "AE6")
			)
			(pin output line
				(at -25.4 30.48 0)
				(length 5.08)
				(name "DRAM_DQM1")
				(number "AC6")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "DRAM_D16")
				(number "AB7")
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "DRAM_D17")
				(number "AA8")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "DRAM_D18")
				(number "AB9")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "DRAM_D19")
				(number "Y9")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "DRAM_D20")
				(number "Y7")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "DRAM_D21")
				(number "Y8")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "DRAM_D22")
				(number "AC8")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "DRAM_D23")
				(number "AA9")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "DRAM_SDQS2")
				(number "AD8")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "DRAM_SDQS2_B")
				(number "AE8")
			)
			(pin output line
				(at -25.4 0 0)
				(length 5.08)
				(name "DRAM_DQM2")
				(number "AB8")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "DRAM_D24")
				(number "AE9")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "DRAM_D25")
				(number "Y10")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "DRAM_D26")
				(number "AE11")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "DRAM_D27")
				(number "AB11")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "DRAM_D28")
				(number "AC9")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "DRAM_D29")
				(number "AD9")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 5.08)
				(name "DRAM_D30")
				(number "AD11")
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "DRAM_D31")
				(number "AC11")
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "DRAM_SDQS3")
				(number "AC10")
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 5.08)
				(name "DRAM_SDQS3_B")
				(number "AB10")
			)
			(pin output line
				(at -25.4 -30.48 0)
				(length 5.08)
				(name "DRAM_DQM3")
				(number "AE10")
			)
			(pin output line
				(at -25.4 -38.1 0)
				(length 5.08)
				(name "DRAM_RAS")
				(number "AB15")
			)
			(pin output line
				(at -25.4 -40.64 0)
				(length 5.08)
				(name "DRAM_CAS")
				(number "AE16")
			)
			(pin output line
				(at -25.4 -43.18 0)
				(length 5.08)
				(name "DRAM_SDWE")
				(number "AB16")
			)
			(pin output line
				(at -25.4 -48.26 0)
				(length 5.08)
				(name "DRAM_SDCKE0")
				(number "Y11")
			)
			(pin output line
				(at -25.4 -50.8 0)
				(length 5.08)
				(name "DRAM_SDCKE1")
				(number "AA11")
			)
			(pin output line
				(at -25.4 -55.88 0)
				(length 5.08)
				(name "DRAM_SDODT0")
				(number "AC16")
			)
			(pin output line
				(at -25.4 -58.42 0)
				(length 5.08)
				(name "DRAM_SDODT1")
				(number "AB17")
			)
			(pin output line
				(at -25.4 -63.5 0)
				(length 5.08)
				(name "DRAM_SDCLK_0")
				(number "AD15")
			)
			(pin output line
				(at -25.4 -66.04 0)
				(length 5.08)
				(name "DRAM_SDCLK_0_B")
				(number "AE15")
			)
			(pin output line
				(at -25.4 -71.12 0)
				(length 5.08)
				(name "DRAM_SDCLK_1")
				(number "AD14")
			)
			(pin output line
				(at -25.4 -73.66 0)
				(length 5.08)
				(name "DRAM_SDCLK_1_B")
				(number "AE14")
			)
			(pin output line
				(at -25.4 -78.74 0)
				(length 5.08)
				(name "DRAM_RESET")
				(number "Y6")
			)
			(pin power_in line
				(at -25.4 -83.82 0)
				(length 5.08)
				(name "DRAM_VREF")
				(number "AC2")
			)
			(pin passive line
				(at -25.4 -88.9 0)
				(length 5.08)
				(name "ZQPAD")
				(number "AE17")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "NVCC_DRAM")
				(number "R18")
			)
			(pin passive line
				(at 0 93.98 270)
				(length 5.08)
				(hide yes)
				(name "NVCC_DRAM")
				(number "T18")
			)
			(pin passive line
				(at 0 93.98 270)
				(length 5.08)
				(hide yes)
				(name "NVCC_DRAM")
				(number "U18")
			)
			(pin passive line
				(at 0 93.98 270)
				(length 5.08)
				(hide yes)
				(name "NVCC_DRAM")
				(number "V10")
			)
			(pin passive line
				(at 0 93.98 270)
				(length 5.08)
				(hide yes)
				(name "NVCC_DRAM")
				(number "V11")
			)
			(pin passive line
				(at 0 93.98 270)
				(length 5.08)
				(hide yes)
				(name "NVCC_DRAM")
				(number "V12")
			)
			(pin passive line
				(at 0 93.98 270)
				(length 5.08)
				(hide yes)
				(name "NVCC_DRAM")
				(number "V13")
			)
			(pin passive line
				(at 0 93.98 270)
				(length 5.08)
				(hide yes)
				(name "NVCC_DRAM")
				(number "V14")
			)
			(pin passive line
				(at 0 93.98 270)
				(length 5.08)
				(hide yes)
				(name "NVCC_DRAM")
				(number "V15")
			)
			(pin passive line
				(at 0 93.98 270)
				(length 5.08)
				(hide yes)
				(name "NVCC_DRAM")
				(number "V16")
			)
			(pin passive line
				(at 0 93.98 270)
				(length 5.08)
				(hide yes)
				(name "NVCC_DRAM")
				(number "V17")
			)
			(pin passive line
				(at 0 93.98 270)
				(length 5.08)
				(hide yes)
				(name "NVCC_DRAM")
				(number "V18")
			)
			(pin passive line
				(at 0 93.98 270)
				(length 5.08)
				(hide yes)
				(name "NVCC_DRAM")
				(number "V9")
			)
			(pin bidirectional line
				(at 25.4 86.36 180)
				(length 5.08)
				(name "DRAM_D32")
				(number "AA17")
			)
			(pin bidirectional line
				(at 25.4 83.82 180)
				(length 5.08)
				(name "DRAM_D33")
				(number "AA18")
			)
			(pin bidirectional line
				(at 25.4 81.28 180)
				(length 5.08)
				(name "DRAM_D34")
				(number "AC18")
			)
			(pin bidirectional line
				(at 25.4 78.74 180)
				(length 5.08)
				(name "DRAM_D35")
				(number "AE19")
			)
			(pin bidirectional line
				(at 25.4 76.2 180)
				(length 5.08)
				(name "DRAM_D36")
				(number "Y17")
			)
			(pin bidirectional line
				(at 25.4 73.66 180)
				(length 5.08)
				(name "DRAM_D37")
				(number "Y18")
			)
			(pin bidirectional line
				(at 25.4 71.12 180)
				(length 5.08)
				(name "DRAM_D38")
				(number "AB19")
			)
			(pin bidirectional line
				(at 25.4 68.58 180)
				(length 5.08)
				(name "DRAM_D39")
				(number "AC19")
			)
			(pin bidirectional line
				(at 25.4 66.04 180)
				(length 5.08)
				(name "DRAM_SDQS4")
				(number "AD18")
			)
			(pin bidirectional line
				(at 25.4 63.5 180)
				(length 5.08)
				(name "DRAM_SDQS4_B")
				(number "AE18")
			)
			(pin output line
				(at 25.4 60.96 180)
				(length 5.08)
				(name "DRAM_DQM4")
				(number "AB18")
			)
			(pin bidirectional line
				(at 25.4 55.88 180)
				(length 5.08)
				(name "DRAM_D40")
				(number "Y19")
			)
			(pin bidirectional line
				(at 25.4 53.34 180)
				(length 5.08)
				(name "DRAM_D41")
				(number "AB20")
			)
			(pin bidirectional line
				(at 25.4 50.8 180)
				(length 5.08)
				(name "DRAM_D42")
				(number "AB21")
			)
			(pin bidirectional line
				(at 25.4 48.26 180)
				(length 5.08)
				(name "DRAM_D43")
				(number "AD21")
			)
			(pin bidirectional line
				(at 25.4 45.72 180)
				(length 5.08)
				(name "DRAM_D44")
				(number "Y20")
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 5.08)
				(name "DRAM_D45")
				(number "AA20")
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 5.08)
				(name "DRAM_D46")
				(number "AE21")
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 5.08)
				(name "DRAM_D47")
				(number "AC21")
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 5.08)
				(name "DRAM_SDQS5")
				(number "AD20")
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 5.08)
				(name "DRAM_SDQS5_B")
				(number "AE20")
			)
			(pin output line
				(at 25.4 30.48 180)
				(length 5.08)
				(name "DRAM_DQM5")
				(number "AC20")
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "DRAM_D48")
				(number "AC22")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 5.08)
				(name "DRAM_D49")
				(number "AE22")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "DRAM_D50")
				(number "AE24")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "DRAM_D51")
				(number "AC24")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "DRAM_D52")
				(number "AB22")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "DRAM_D53")
				(number "AC23")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "DRAM_D54")
				(number "AD25")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "DRAM_D55")
				(number "AC25")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "DRAM_SDQS6")
				(number "AD23")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "DRAM_SDQS6_B")
				(number "AE23")
			)
			(pin output line
				(at 25.4 0 180)
				(length 5.08)
				(name "DRAM_DQM6")
				(number "AD24")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "DRAM_D56")
				(number "AB25")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "DRAM_D57")
				(number "AA21")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "DRAM_D58")
				(number "Y25")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "DRAM_D59")
				(number "Y22")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "DRAM_D60")
				(number "AB23")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "DRAM_D61")
				(number "AA23")
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 5.08)
				(name "DRAM_D62")
				(number "Y23")
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "DRAM_D63")
				(number "W25")
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "DRAM_SDQS7")
				(number "AA25")
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "DRAM_SDQS7_B")
				(number "AA24")
			)
			(pin output line
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "DRAM_DQM7")
				(number "Y21")
			)
			(pin output line
				(at 25.4 -38.1 180)
				(length 5.08)
				(name "DRAM_A0")
				(number "AC14")
			)
			(pin output line
				(at 25.4 -40.64 180)
				(length 5.08)
				(name "DRAM_A1")
				(number "AB14")
			)
			(pin output line
				(at 25.4 -43.18 180)
				(length 5.08)
				(name "DRAM_A2")
				(number "AA14")
			)
			(pin output line
				(at 25.4 -45.72 180)
				(length 5.08)
				(name "DRAM_A3")
				(number "Y14")
			)
			(pin output line
				(at 25.4 -48.26 180)
				(length 5.08)
				(name "DRAM_A4")
				(number "W14")
			)
			(pin output line
				(at 25.4 -50.8 180)
				(length 5.08)
				(name "DRAM_A5")
				(number "AE13")
			)
			(pin output line
				(at 25.4 -53.34 180)
				(length 5.08)
				(name "DRAM_A6")
				(number "AC13")
			)
			(pin output line
				(at 25.4 -55.88 180)
				(length 5.08)
				(name "DRAM_A7")
				(number "Y13")
			)
			(pin output line
				(at 25.4 -58.42 180)
				(length 5.08)
				(name "DRAM_A8")
				(number "AB13")
			)
			(pin output line
				(at 25.4 -60.96 180)
				(length 5.08)
				(name "DRAM_A9")
				(number "AE12")
			)
			(pin output line
				(at 25.4 -63.5 180)
				(length 5.08)
				(name "DRAM_A10")
				(number "AA15")
			)
			(pin output line
				(at 25.4 -66.04 180)
				(length 5.08)
				(name "DRAM_A11")
				(number "AC12")
			)
			(pin output line
				(at 25.4 -68.58 180)
				(length 5.08)
				(name "DRAM_A12")
				(number "AD12")
			)
			(pin output line
				(at 25.4 -71.12 180)
				(length 5.08)
				(name "DRAM_A13")
				(number "AC17")
			)
			(pin output line
				(at 25.4 -73.66 180)
				(length 5.08)
				(name "DRAM_A14")
				(number "AA12")
			)
			(pin output line
				(at 25.4 -76.2 180)
				(length 5.08)
				(name "DRAM_A15")
				(number "Y12")
			)
			(pin output line
				(at 25.4 -81.28 180)
				(length 5.08)
				(name "DRAM_SDBA0")
				(number "AC15")
			)
			(pin output line
				(at 25.4 -83.82 180)
				(length 5.08)
				(name "DRAM_SDBA1")
				(number "Y15")
			)
			(pin output line
				(at 25.4 -86.36 180)
				(length 5.08)
				(name "DRAM_SDBA2")
				(number "AB12")
			)
			(pin output line
				(at 25.4 -91.44 180)
				(length 5.08)
				(name "DRAM_CS0")
				(number "Y16")
			)
			(pin output line
				(at 25.4 -93.98 180)
				(length 5.08)
				(name "DRAM_CS1")
				(number "AD17")
			)
		)
		(symbol "MCIMX6QP5EYM_22_0"
			(text "Crystal Oscillator"
				(at 0 1.27 0)
			)
		)
		(symbol "MCIMX6QP5EYM_22_1"
			(text "NVCC_PLL_OUT"
				(at 0 -2.54 0)
			)
			(pin input line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "XTALI")
				(number "A7")
			)
			(pin output line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "XTALO")
				(number "B7")
			)
		)
		(symbol "MCIMX6QP5EYM_23_0"
			(text "RTC"
				(at 0 1.27 0)
			)
		)
		(symbol "MCIMX6QP5EYM_23_1"
			(text "VDD_SNVS_CAP"
				(at 0 -2.54 0)
			)
			(pin input line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "RTC_XTALI")
				(number "D9")
			)
			(pin output line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "RTC_XTALO")
				(number "C9")
			)
		)
		(symbol "MCIMX6QP5EYM_24_0"
			(text "SATA"
				(at 0 -3.81 0)
			)
		)
		(symbol "MCIMX6QP5EYM_24_1"
			(pin passive line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "SATA_REXT")
				(number "C14")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 5.08)
				(name "SATA_VP")
				(number "G13")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 5.08)
				(name "SATA_VPH")
				(number "G12")
			)
			(pin input line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "SATA_RXM")
				(number "A14")
			)
			(pin input line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "SATA_RXP")
				(number "B14")
			)
			(pin output line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "SATA_TXM")
				(number "B12")
			)
			(pin output line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "SATA_TXP")
				(number "A12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCIMX6QP7CVT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 15.24 90.17 0)
		)
		(property "Value" "MCIMX6QP7CVT"
			(at -13.97 90.17 0)
		)
		(property "Footprint" "Package_BGA:BGA-624_21x21mm_Layout25x25_P0.8mm"
			(at -13.97 55.88 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/IMX6DQPIEC.pdf"
			(at -11.43 55.88 0)
		)
		(property "Description" "i.MX 6QuadPlus Application Processor for Industrial Products, BGA-624"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "Quad-Core ARM Cortex A9 SOC Industrial"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "BGA*21x21mm*Layout25x25*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "MCIMX6QP7CVT_1_0"
			(text "Power Management"
				(at -1.27 -5.08 0)
			)
		)
		(symbol "MCIMX6QP7CVT_1_1"
			(pin power_in line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "VDD_ARM_IN")
				(number "H14")
			)
			(pin passive line
				(at -25.4 10.16 0)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM_IN")
				(number "J14")
			)
			(pin passive line
				(at -25.4 10.16 0)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM_IN")
				(number "K14")
			)
			(pin passive line
				(at -25.4 10.16 0)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM_IN")
				(number "L14")
			)
			(pin passive line
				(at -25.4 10.16 0)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM_IN")
				(number "M14")
			)
			(pin passive line
				(at -25.4 10.16 0)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM_IN")
				(number "N14")
			)
			(pin passive line
				(at -25.4 10.16 0)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM_IN")
				(number "P14")
			)
			(pin passive line
				(at -25.4 10.16 0)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM_IN")
				(number "R14")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "VDD_ARM23_IN")
				(number "K9")
			)
			(pin passive line
				(at -25.4 7.62 0)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM23_IN")
				(number "L9")
			)
			(pin passive line
				(at -25.4 7.62 0)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM23_IN")
				(number "M9")
			)
			(pin passive line
				(at -25.4 7.62 0)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM23_IN")
				(number "N9")
			)
			(pin passive line
				(at -25.4 7.62 0)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM23_IN")
				(number "P9")
			)
			(pin passive line
				(at -25.4 7.62 0)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM23_IN")
				(number "R9")
			)
			(pin passive line
				(at -25.4 7.62 0)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM23_IN")
				(number "T9")
			)
			(pin passive line
				(at -25.4 7.62 0)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM23_IN")
				(number "U9")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "VDD_SOC_IN")
				(number "H16")
			)
			(pin passive line
				(at -25.4 5.08 0)
				(length 5.08)
				(hide yes)
				(name "VDD_SOC_IN")
				(number "J16")
			)
			(pin passive line
				(at -25.4 5.08 0)
				(length 5.08)
				(hide yes)
				(name "VDD_SOC_IN")
				(number "K16")
			)
			(pin passive line
				(at -25.4 5.08 0)
				(length 5.08)
				(hide yes)
				(name "VDD_SOC_IN")
				(number "L16")
			)
			(pin passive line
				(at -25.4 5.08 0)
				(length 5.08)
				(hide yes)
				(name "VDD_SOC_IN")
				(number "M16")
			)
			(pin passive line
				(at -25.4 5.08 0)
				(length 5.08)
				(hide yes)
				(name "VDD_SOC_IN")
				(number "N16")
			)
			(pin passive line
				(at -25.4 5.08 0)
				(length 5.08)
				(hide yes)
				(name "VDD_SOC_IN")
				(number "P16")
			)
			(pin passive line
				(at -25.4 5.08 0)
				(length 5.08)
				(hide yes)
				(name "VDD_SOC_IN")
				(number "R16")
			)
			(pin passive line
				(at -25.4 5.08 0)
				(length 5.08)
				(hide yes)
				(name "VDD_SOC_IN")
				(number "T16")
			)
			(pin passive line
				(at -25.4 5.08 0)
				(length 5.08)
				(hide yes)
				(name "VDD_SOC_IN")
				(number "U16")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 5.08)
				(name "VDD_HIGH_IN")
				(number "H9")
			)
			(pin passive line
				(at -25.4 0 0)
				(length 5.08)
				(hide yes)
				(name "VDD_HIGH_IN")
				(number "J9")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "VDD_SNVS_IN")
				(number "G11")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 5.08)
				(name "GND")
				(number "A13")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "A25")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "A4")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "A8")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AA10")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AA13")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AA16")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AA19")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AA22")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AA7")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AB24")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AB3")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AD10")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AD13")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AD16")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AD19")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AD22")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AD4")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AD7")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AE1")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AE25")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "B4")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "C1")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "C10")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "C4")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "C6")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "D3")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "D6")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "D8")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "E5")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "E6")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "E7")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "F5")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "F6")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "F7")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "F8")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "G10")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "G19")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "G3")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "H12")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "H15")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "H18")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "H8")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "J12")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "J15")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "J18")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "J2")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "J8")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "K10")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "K12")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "K15")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "K18")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "K8")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L10")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L12")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L15")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L18")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L2")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L5")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L8")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "M10")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "M12")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "M15")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "M18")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "M8")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "N10")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "N15")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "N18")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "N8")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "P10")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "P12")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "P15")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "P18")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "P8")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "R12")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "R15")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "R17")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "R8")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "T11")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "T12")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "T15")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "T17")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "T19")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "T8")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U11")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U12")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U15")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U17")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U19")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U8")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V19")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V8")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W10")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W11")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W12")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W13")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W15")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W16")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W17")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W18")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W19")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W3")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W7")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W8")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W9")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "Y24")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "Y5")
			)
			(pin power_out line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "VDD_ARM_CAP")
				(number "H13")
			)
			(pin passive line
				(at 25.4 10.16 180)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM_CAP")
				(number "J13")
			)
			(pin passive line
				(at 25.4 10.16 180)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM_CAP")
				(number "K13")
			)
			(pin passive line
				(at 25.4 10.16 180)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM_CAP")
				(number "L13")
			)
			(pin passive line
				(at 25.4 10.16 180)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM_CAP")
				(number "M13")
			)
			(pin passive line
				(at 25.4 10.16 180)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM_CAP")
				(number "N13")
			)
			(pin passive line
				(at 25.4 10.16 180)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM_CAP")
				(number "P13")
			)
			(pin passive line
				(at 25.4 10.16 180)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM_CAP")
				(number "R13")
			)
			(pin power_out line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "VDD_ARM23_CAP")
				(number "H11")
			)
			(pin passive line
				(at 25.4 7.62 180)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM23_CAP")
				(number "J11")
			)
			(pin passive line
				(at 25.4 7.62 180)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM23_CAP")
				(number "K11")
			)
			(pin passive line
				(at 25.4 7.62 180)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM23_CAP")
				(number "L11")
			)
			(pin passive line
				(at 25.4 7.62 180)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM23_CAP")
				(number "M11")
			)
			(pin passive line
				(at 25.4 7.62 180)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM23_CAP")
				(number "N11")
			)
			(pin passive line
				(at 25.4 7.62 180)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM23_CAP")
				(number "P11")
			)
			(pin passive line
				(at 25.4 7.62 180)
				(length 5.08)
				(hide yes)
				(name "VDD_ARM23_CAP")
				(number "R11")
			)
			(pin power_out line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "VDD_SOC_CAP")
				(number "R10")
			)
			(pin passive line
				(at 25.4 5.08 180)
				(length 5.08)
				(hide yes)
				(name "VDD_SOC_CAP")
				(number "T10")
			)
			(pin passive line
				(at 25.4 5.08 180)
				(length 5.08)
				(hide yes)
				(name "VDD_SOC_CAP")
				(number "T13")
			)
			(pin passive line
				(at 25.4 5.08 180)
				(length 5.08)
				(hide yes)
				(name "VDD_SOC_CAP")
				(number "T14")
			)
			(pin passive line
				(at 25.4 5.08 180)
				(length 5.08)
				(hide yes)
				(name "VDD_SOC_CAP")
				(number "U10")
			)
			(pin passive line
				(at 25.4 5.08 180)
				(length 5.08)
				(hide yes)
				(name "VDD_SOC_CAP")
				(number "U13")
			)
			(pin passive line
				(at 25.4 5.08 180)
				(length 5.08)
				(hide yes)
				(name "VDD_SOC_CAP")
				(number "U14")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "VDD_CACHE_CAP")
				(number "N12")
			)
			(pin power_out line
				(at 25.4 0 180)
				(length 5.08)
				(name "VDD_HIGH_CAP")
				(number "H10")
			)
			(pin passive line
				(at 25.4 0 180)
				(length 5.08)
				(hide yes)
				(name "VDD_HIGH_CAP")
				(number "J10")
			)
			(pin power_out line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "VDD_SNVS_CAP")
				(number "G9")
			)
			(pin power_out line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "VDD_PU_CAP")
				(number "H17")
			)
			(pin passive line
				(at 25.4 -5.08 180)
				(length 5.08)
				(hide yes)
				(name "VDD_PU_CAP")
				(number "J17")
			)
			(pin passive line
				(at 25.4 -5.08 180)
				(length 5.08)
				(hide yes)
				(name "VDD_PU_CAP")
				(number "K17")
			)
			(pin passive line
				(at 25.4 -5.08 180)
				(length 5.08)
				(hide yes)
				(name "VDD_PU_CAP")
				(number "L17")
			)
			(pin passive line
				(at 25.4 -5.08 180)
				(length 5.08)
				(hide yes)
				(name "VDD_PU_CAP")
				(number "M17")
			)
			(pin passive line
				(at 25.4 -5.08 180)
				(length 5.08)
				(hide yes)
				(name "VDD_PU_CAP")
				(number "N17")
			)
			(pin passive line
				(at 25.4 -5.08 180)
				(length 5.08)
				(hide yes)
				(name "VDD_PU_CAP")
				(number "P17")
			)
			(pin power_out line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "VDD_USB_CAP")
				(number "F9")
			)
			(pin power_out line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "NVCC_PLL_OUT")
				(number "E8")
			)
		)
		(symbol "MCIMX6QP7CVT_2_0"
			(text "Factory (NXP only)"
				(at -10.16 0 0)
			)
		)
		(symbol "MCIMX6QP7CVT_2_1"
			(pin passive line
				(at 0 10.16 270)
				(length 5.08)
				(name "VDD_FA")
				(number "B5")
			)
			(pin passive line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "FA_ANA")
				(number "A5")
			)
			(pin passive line
				(at 25.4 0 180)
				(length 5.08)
				(name "GPANAIO")
				(number "C8")
			)
			(pin passive line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "TEST_MODE")
				(number "E12")
			)
		)
		(symbol "MCIMX6QP7CVT_3_0"
			(text "Boot/Power Management"
				(at 1.27 -5.08 0)
			)
		)
		(symbol "MCIMX6QP7CVT_3_1"
			(text "VDD_SNVS_IN"
				(at 0 0 0)
			)
			(pin input line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "BOOT_MODE0")
				(number "C12")
			)
			(pin input line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "BOOT_MODE1")
				(number "F12")
			)
			(pin input line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "ONOFF")
				(number "D12")
			)
			(pin input line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "POR_B")
				(number "C11")
			)
			(pin output line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PMIC_ON_REQ")
				(number "D11")
			)
			(pin output line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "PMIC_STBY_REQ")
				(number "F11")
			)
			(pin input line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "TAMPER")
				(number "E11")
			)
		)
		(symbol "MCIMX6QP7CVT_4_0"
			(text "Clock"
				(at -16.51 11.43 0)
			)
		)
		(symbol "MCIMX6QP7CVT_4_1"
			(text "VDD_HIGH_CAP"
				(at 0 0 0)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "CLK1_N")
				(number "C7")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "CLK1_P")
				(number "D7")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "CLK2_N")
				(number "C5")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "CLK2_P")
				(number "D5")
			)
			(pin no_connect line
				(at 17.78 7.62 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "A11")
			)
			(pin no_connect line
				(at 17.78 5.08 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "B11")
			)
			(pin no_connect line
				(at 17.78 0 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "B10")
			)
			(pin no_connect line
				(at 17.78 -2.54 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "A10")
			)
			(pin no_connect line
				(at 17.78 -7.62 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "A9")
			)
			(pin no_connect line
				(at 17.78 -10.16 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "B9")
			)
		)
		(symbol "MCIMX6QP7CVT_5_0"
			(text "MIPI Camera"
				(at 0 0 0)
			)
		)
		(symbol "MCIMX6QP7CVT_5_1"
			(pin input line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "CSI_CLK0M")
				(number "F4")
			)
			(pin input line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "CSI_CLK0P")
				(number "F3")
			)
			(pin input line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "CSI_D0M")
				(number "E4")
			)
			(pin input line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "CSI_D0P")
				(number "E3")
			)
			(pin input line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "CSI_D1M")
				(number "D1")
			)
			(pin input line
				(at -25.4 0 0)
				(length 5.08)
				(name "CSI_D1P")
				(number "D2")
			)
			(pin input line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "CSI_D2M")
				(number "E1")
			)
			(pin input line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "CSI_D2P")
				(number "E2")
			)
			(pin input line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "CSI_D3M")
				(number "F2")
			)
			(pin input line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "CSI_D3P")
				(number "F1")
			)
			(pin passive line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "CSI_REXT")
				(number "D4")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 5.08)
				(name "NVCC_MIPI")
				(number "K7")
			)
			(pin output line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "DSI_CLK0M")
				(number "H3")
			)
			(pin output line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "DSI_CLK0P")
				(number "H4")
			)
			(pin output line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "DSI_D0M")
				(number "G2")
			)
			(pin output line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "DSI_D0P")
				(number "G1")
			)
			(pin output line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "DSI_D1M")
				(number "H2")
			)
			(pin output line
				(at 25.4 0 180)
				(length 5.08)
				(name "DSI_D1P")
				(number "H1")
			)
			(pin passive line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "DSI_REXT")
				(number "G4")
			)
		)
		(symbol "MCIMX6QP7CVT_6_0"
			(text "Camera"
				(at 0 0 0)
			)
		)
		(symbol "MCIMX6QP7CVT_6_1"
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "CSI0_MCLK")
				(number "P4")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "CSI0_PIXCLK")
				(number "P1")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "CSI0_DATA_EN")
				(number "P3")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "CSI0_VSYNC")
				(number "N2")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "CSI0_DAT4")
				(number "N1")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "CSI0_DAT5")
				(number "P2")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "CSI0_DAT6")
				(number "N4")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "CSI0_DAT7")
				(number "N3")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "CSI0_DAT8")
				(number "N6")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "CSI0_DAT9")
				(number "N5")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 5.08)
				(name "NVCC_CSI")
				(number "N7")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "CSI0_DAT10")
				(number "M1")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "CSI0_DAT11")
				(number "M3")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "CSI0_DAT12")
				(number "M2")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "CSI0_DAT13")
				(number "L1")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "CSI0_DAT14")
				(number "M4")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "CSI0_DAT15")
				(number "M5")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "CSI0_DAT16")
				(number "L4")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "CSI0_DAT17")
				(number "L3")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "CSI0_DAT18")
				(number "M6")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "CSI0_DAT19")
				(number "L6")
			)
		)
		(symbol "MCIMX6QP7CVT_7_0"
			(text "LCD Display"
				(at 0 0 0)
			)
		)
		(symbol "MCIMX6QP7CVT_7_1"
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "DI0_DISP_CLK")
				(number "N19")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "DI0_PIN15")
				(number "N21")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "DI0_PIN2")
				(number "N25")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "DI0_PIN3")
				(number "N20")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "DI0_PIN4")
				(number "P25")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "DISP0_DAT0")
				(number "P24")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "DISP0_DAT1")
				(number "P22")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "DISP0_DAT2")
				(number "P23")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "DISP0_DAT3")
				(number "P21")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "DISP0_DAT4")
				(number "P20")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "DISP0_DAT5")
				(number "R25")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "DISP0_DAT6")
				(number "R23")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "DISP0_DAT7")
				(number "R24")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "DISP0_DAT8")
				(number "R22")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "DISP0_DAT9")
				(number "T25")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 5.08)
				(name "NVCC_LCD")
				(number "P19")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "DISP0_DAT10")
				(number "R21")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "DISP0_DAT11")
				(number "T23")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "DISP0_DAT12")
				(number "T24")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "DISP0_DAT13")
				(number "R20")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "DISP0_DAT14")
				(number "U25")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "DISP0_DAT15")
				(number "T22")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "DISP0_DAT16")
				(number "T21")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "DISP0_DAT17")
				(number "U24")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "DISP0_DAT18")
				(number "V25")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "DISP0_DAT19")
				(number "U23")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "DISP0_DAT20")
				(number "U22")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "DISP0_DAT21")
				(number "T20")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "DISP0_DAT22")
				(number "V24")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "DISP0_DAT23")
				(number "W24")
			)
		)
		(symbol "MCIMX6QP7CVT_8_0"
			(text "External memory"
				(at 1.27 0 0)
			)
		)
		(symbol "MCIMX6QP7CVT_8_1"
			(pin bidirectional line
				(at -25.4 40.64 0)
				(length 5.08)
				(name "EIM_A16")
				(number "H25")
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 5.08)
				(name "EIM_A17")
				(number "G24")
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 5.08)
				(name "EIM_A18")
				(number "J22")
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 5.08)
				(name "EIM_A19")
				(number "G25")
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 5.08)
				(name "EIM_A20")
				(number "H22")
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 5.08)
				(name "EIM_A21")
				(number "H23")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "EIM_A22")
				(number "F24")
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "EIM_A23")
				(number "J21")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "EIM_A24")
				(number "F25")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "EIM_A25")
				(number "H19")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "EIM_EB0")
				(number "K21")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "EIM_EB1")
				(number "K23")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "EIM_EB2")
				(number "E22")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "EIM_EB3")
				(number "F23")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "EIM_BCLK")
				(number "N22")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "EIM_LBA")
				(number "K22")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "EIM_OE")
				(number "J24")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "EIM_RW")
				(number "K20")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "EIM_WAIT")
				(number "M25")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "EIM_CS0")
				(number "H24")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "EIM_CS1")
				(number "J23")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 5.08)
				(name "NVCC_EIM0")
				(number "K19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 5.08)
				(name "NVCC_EIM1")
				(number "L19")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 5.08)
				(name "NVCC_EIM2")
				(number "M19")
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 5.08)
				(name "EIM_DA0")
				(number "L20")
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 5.08)
				(name "EIM_DA1")
				(number "J25")
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 5.08)
				(name "EIM_DA2")
				(number "L21")
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 5.08)
				(name "EIM_DA3")
				(number "K24")
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 5.08)
				(name "EIM_DA4")
				(number "L22")
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 5.08)
				(name "EIM_DA5")
				(number "L23")
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "EIM_DA6")
				(number "K25")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 5.08)
				(name "EIM_DA7")
				(number "L25")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "EIM_DA8")
				(number "L24")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "EIM_DA9")
				(number "M21")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "EIM_DA10")
				(number "M22")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "EIM_DA11")
				(number "M20")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "EIM_DA12")
				(number "M24")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "EIM_DA13")
				(number "M23")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "EIM_DA14")
				(number "N23")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "EIM_DA15")
				(number "N24")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "EIM_D16")
				(number "C25")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "EIM_D17")
				(number "F21")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "EIM_D18")
				(number "D24")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "EIM_D19")
				(number "G21")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "EIM_D20")
				(number "G20")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "EIM_D21")
				(number "H20")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "EIM_D22")
				(number "E23")
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 5.08)
				(name "EIM_D23")
				(number "D25")
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "EIM_D24")
				(number "F22")
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "EIM_D25")
				(number "G22")
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "EIM_D26")
				(number "E24")
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "EIM_D27")
				(number "E25")
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 5.08)
				(name "EIM_D28")
				(number "G23")
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 5.08)
				(name "EIM_D29")
				(number "J19")
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 5.08)
				(name "EIM_D30")
				(number "J20")
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 5.08)
				(name "EIM_D31")
				(number "H21")
			)
		)
		(symbol "MCIMX6QP7CVT_9_0"
			(text "10/100-Mbit Ethernet"
				(at -2.54 -7.62 0)
			)
		)
		(symbol "MCIMX6QP7CVT_9_1"
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "ENET_RXD0")
				(number "W21")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "ENET_RXD1")
				(number "W22")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "ENET_CRS_DV")
				(number "U21")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "ENET_RX_ER")
				(number "W23")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "ENET_REF_CLK")
				(number "V22")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "NVCC_ENET")
				(number "R19")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "ENET_TXD0")
				(number "U20")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "ENET_TXD1")
				(number "W20")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "ENET_TX_EN")
				(number "V21")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "ENET_MDC")
				(number "V20")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "ENET_MDIO")
				(number "V23")
			)
		)
		(symbol "MCIMX6QP7CVT_10_0"
			(text "GPIO"
				(at 0 0 0)
			)
		)
		(symbol "MCIMX6QP7CVT_10_1"
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "GPIO_0")
				(number "T5")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "GPIO_1")
				(number "T4")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "GPIO_2")
				(number "T1")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "GPIO_3")
				(number "R7")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "GPIO_4")
				(number "R6")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "GPIO_5")
				(number "R4")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "GPIO_6")
				(number "T3")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "GPIO_7")
				(number "R3")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "GPIO_8")
				(number "R5")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "GPIO_9")
				(number "T2")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "GPIO_16")
				(number "R2")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "GPIO_17")
				(number "R1")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "GPIO_18")
				(number "P6")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "GPIO_19")
				(number "P5")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 5.08)
				(name "NVCC_GPIO")
				(number "P7")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "KEY_COL0")
				(number "W5")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "KEY_COL1")
				(number "U7")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "KEY_COL2")
				(number "W6")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "KEY_COL3")
				(number "U5")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "KEY_COL4")
				(number "T6")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "KEY_ROW0")
				(number "V6")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "KEY_ROW1")
				(number "U6")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "KEY_ROW2")
				(number "W4")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "KEY_ROW3")
				(number "T7")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "KEY_ROW4")
				(number "V5")
			)
		)
		(symbol "MCIMX6QP7CVT_11_0"
			(text "HDMI Display"
				(at 0 0 0)
			)
		)
		(symbol "MCIMX6QP7CVT_11_1"
			(pin input line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "HDMI_HPD")
				(number "K1")
			)
			(pin passive line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "HDMI_DDCCEC")
				(number "K2")
			)
			(pin passive line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "HDMI_REF")
				(number "J1")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 5.08)
				(name "HDMI_VP")
				(number "L7")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 5.08)
				(name "HDMI_VPH")
				(number "M7")
			)
			(pin output line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "HDMI_CLKM")
				(number "J5")
			)
			(pin output line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "HDMI_CLKP")
				(number "J6")
			)
			(pin output line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "HDMI_D0M")
				(number "K5")
			)
			(pin output line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "HDMI_D0P")
				(number "K6")
			)
			(pin output line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "HDMI_D1M")
				(number "J3")
			)
			(pin output line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "HDMI_D1P")
				(number "J4")
			)
			(pin output line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "HDMI_D2M")
				(number "K3")
			)
			(pin output line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "HDMI_D2P")
				(number "K4")
			)
		)
		(symbol "MCIMX6QP7CVT_12_0"
			(text "JTAG Debug"
				(at 0 -5.08 0)
			)
		)
		(symbol "MCIMX6QP7CVT_12_1"
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "NVCC_JTAG")
				(number "J7")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "JTAG_TMS")
				(number "C3")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "JTAG_TCK")
				(number "H5")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "JTAG_TDO")
				(number "G6")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "JTAG_TDI")
				(number "G5")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "JTAG_TRSTB")
				(number "C2")
			)
			(pin input line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "JTAG_MOD")
				(number "H6")
			)
		)
		(symbol "MCIMX6QP7CVT_13_0"
			(text "LVDS Display"
				(at 0 2.54 0)
			)
		)
		(symbol "MCIMX6QP7CVT_13_1"
			(pin output line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "LVDS0_CLK_N")
				(number "V4")
			)
			(pin output line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "LVDS0_CLK_P")
				(number "V3")
			)
			(pin output line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "LVDS0_TX0_N")
				(number "U2")
			)
			(pin output line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "LVDS0_TX0_P")
				(number "U1")
			)
			(pin output line
				(at -25.4 0 0)
				(length 5.08)
				(name "LVDS0_TX1_N")
				(number "U4")
			)
			(pin output line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "LVDS0_TX1_P")
				(number "U3")
			)
			(pin output line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "LVDS0_TX2_N")
				(number "V2")
			)
			(pin output line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "LVDS0_TX2_P")
				(number "V1")
			)
			(pin output line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "LVDS0_TX3_N")
				(number "W2")
			)
			(pin output line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "LVDS0_TX3_P")
				(number "W1")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 5.08)
				(name "NVCC_LVDS2P5")
				(number "V7")
			)
			(pin output line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "LVDS1_CLK_N")
				(number "Y3")
			)
			(pin output line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "LVDS1_CLK_P")
				(number "Y4")
			)
			(pin output line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "LVDS1_TX0_N")
				(number "Y1")
			)
			(pin output line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "LVDS1_TX0_P")
				(number "Y2")
			)
			(pin output line
				(at 25.4 0 180)
				(length 5.08)
				(name "LVDS1_TX1_N")
				(number "AA2")
			)
			(pin output line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "LVDS1_TX1_P")
				(number "AA1")
			)
			(pin output line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "LVDS1_TX2_N")
				(number "AB1")
			)
			(pin output line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "LVDS1_TX2_P")
				(number "AB2")
			)
			(pin output line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "LVDS1_TX3_N")
				(number "AA3")
			)
			(pin output line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "LVDS1_TX3_P")
				(number "AA4")
			)
		)
		(symbol "MCIMX6QP7CVT_14_0"
			(text "NAND Flash"
				(at -13.97 24.13 0)
			)
			(text "SD/MMC"
				(at 15.24 24.13 0)
			)
		)
		(symbol "MCIMX6QP7CVT_14_1"
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "NANDF_ALE")
				(number "A16")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "NANDF_CLE")
				(number "C15")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "NANDF_WP_B")
				(number "E15")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "NANDF_RB0")
				(number "B16")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "NANDF_CS0")
				(number "F15")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "NANDF_CS1")
				(number "C16")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "NANDF_CS2")
				(number "A17")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "NANDF_CS3")
				(number "D16")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "NANDF_D0")
				(number "A18")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "NANDF_D1")
				(number "C17")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "NANDF_D2")
				(number "F16")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "NANDF_D3")
				(number "D17")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "NANDF_D4")
				(number "A19")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "NANDF_D5")
				(number "B18")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 5.08)
				(name "NANDF_D6")
				(number "E17")
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "NANDF_D7")
				(number "C18")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 5.08)
				(name "NVCC_NANDF")
				(number "G15")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "SD4_CLK")
				(number "E16")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "SD4_CMD")
				(number "B17")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "SD4_DAT0")
				(number "D18")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "SD4_DAT1")
				(number "B19")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "SD4_DAT2")
				(number "F17")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "SD4_DAT3")
				(number "A20")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "SD4_DAT4")
				(number "E18")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "SD4_DAT5")
				(number "C19")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "SD4_DAT6")
				(number "B20")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "SD4_DAT7")
				(number "D19")
			)
		)
		(symbol "MCIMX6QP7CVT_15_0"
			(text "PCIe 2.0"
				(at 0 -5.08 0)
			)
		)
		(symbol "MCIMX6QP7CVT_15_1"
			(pin passive line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "PCIE_REXT")
				(number "A2")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 5.08)
				(name "PCIE_VPTX")
				(number "G8")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "PCIE_VP")
				(number "H7")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 5.08)
				(name "PCIE_VPH")
				(number "G7")
			)
			(pin input line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PCIE_RXM")
				(number "B1")
			)
			(pin input line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "PCIE_RXP")
				(number "B2")
			)
			(pin output line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "PCIE_TXM")
				(number "A3")
			)
			(pin output line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "PCIE_TXP")
				(number "B3")
			)
		)
		(symbol "MCIMX6QP7CVT_16_0"
			(text "HS USB2.0 Host"
				(at -11.43 6.35 0)
			)
			(text "HS USB2.0 OTG"
				(at 12.7 6.35 0)
			)
		)
		(symbol "MCIMX6QP7CVT_16_1"
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "USB_H1_DP")
				(number "E10")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "USB_H1_DN")
				(number "F10")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 5.08)
				(name "USB_H1_VBUS")
				(number "D10")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 5.08)
				(name "USB_OTG_VBUS")
				(number "E9")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "USB_OTG_DP")
				(number "A6")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "USB_OTG_DN")
				(number "B6")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "USB_OTG_CHD_B")
				(number "B8")
			)
		)
		(symbol "MCIMX6QP7CVT_17_0"
			(text "Gigabit Ethernet"
				(at 0 -5.08 0)
			)
		)
		(symbol "MCIMX6QP7CVT_17_1"
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "RGMII_RXC")
				(number "B25")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "RGMII_RX_CTL")
				(number "D22")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "RGMII_RD0")
				(number "C24")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "RGMII_RD1")
				(number "B23")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "RGMII_RD2")
				(number "B24")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "RGMII_RD3")
				(number "D23")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "NVCC_RGMII")
				(number "G18")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "RGMII_TXC")
				(number "D21")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "RGMII_TX_CTL")
				(number "C23")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "RGMII_TD0")
				(number "C22")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "RGMII_TD1")
				(number "F20")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "RGMII_TD2")
				(number "E21")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "RGMII_TD3")
				(number "A24")
			)
		)
		(symbol "MCIMX6QP7CVT_18_0"
			(text "SD/MMC"
				(at 0 -5.08 0)
			)
		)
		(symbol "MCIMX6QP7CVT_18_1"
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "NVCC_SD1")
				(number "G16")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "SD1_CLK")
				(number "D20")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "SD1_CMD")
				(number "B21")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "SD1_DAT0")
				(number "A21")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "SD1_DAT1")
				(number "C20")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "SD1_DAT2")
				(number "E19")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "SD1_DAT3")
				(number "F18")
			)
		)
		(symbol "MCIMX6QP7CVT_19_0"
			(text "SD/MMC"
				(at 0 -5.08 0)
			)
		)
		(symbol "MCIMX6QP7CVT_19_1"
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "NVCC_SD2")
				(number "G17")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "SD2_CLK")
				(number "C21")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "SD2_CMD")
				(number "F19")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "SD2_DAT0")
				(number "A22")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "SD2_DAT1")
				(number "E20")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "SD2_DAT2")
				(number "A23")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "SD2_DAT3")
				(number "B22")
			)
		)
		(symbol "MCIMX6QP7CVT_20_0"
			(text "SD/MMC"
				(at 0 0 0)
			)
		)
		(symbol "MCIMX6QP7CVT_20_1"
			(pin power_in line
				(at 0 22.86 270)
				(length 5.08)
				(name "NVCC_SD3")
				(number "G14")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "SD3_CLK")
				(number "D14")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "SD3_CMD")
				(number "B13")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "SD3_DAT0")
				(number "E14")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "SD3_DAT1")
				(number "F14")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "SD3_DAT2")
				(number "A15")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "SD3_DAT3")
				(number "B15")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "SD3_DAT4")
				(number "D13")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "SD3_DAT5")
				(number "C13")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "SD3_DAT6")
				(number "E13")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "SD3_DAT7")
				(number "F13")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "SD3_RST")
				(number "D15")
			)
		)
		(symbol "MCIMX6QP7CVT_21_0"
			(text "DDR3/DDR3L/LPDDR2"
				(at 0 -2.54 0)
			)
		)
		(symbol "MCIMX6QP7CVT_21_1"
			(pin bidirectional line
				(at -25.4 86.36 0)
				(length 5.08)
				(name "DRAM_D0")
				(number "AD2")
			)
			(pin bidirectional line
				(at -25.4 83.82 0)
				(length 5.08)
				(name "DRAM_D1")
				(number "AE2")
			)
			(pin bidirectional line
				(at -25.4 81.28 0)
				(length 5.08)
				(name "DRAM_D2")
				(number "AC4")
			)
			(pin bidirectional line
				(at -25.4 78.74 0)
				(length 5.08)
				(name "DRAM_D3")
				(number "AA5")
			)
			(pin bidirectional line
				(at -25.4 76.2 0)
				(length 5.08)
				(name "DRAM_D4")
				(number "AC1")
			)
			(pin bidirectional line
				(at -25.4 73.66 0)
				(length 5.08)
				(name "DRAM_D5")
				(number "AD1")
			)
			(pin bidirectional line
				(at -25.4 71.12 0)
				(length 5.08)
				(name "DRAM_D6")
				(number "AB4")
			)
			(pin bidirectional line
				(at -25.4 68.58 0)
				(length 5.08)
				(name "DRAM_D7")
				(number "AE4")
			)
			(pin bidirectional line
				(at -25.4 66.04 0)
				(length 5.08)
				(name "DRAM_SDQS0")
				(number "AE3")
			)
			(pin bidirectional line
				(at -25.4 63.5 0)
				(length 5.08)
				(name "DRAM_SDQS0_B")
				(number "AD3")
			)
			(pin output line
				(at -25.4 60.96 0)
				(length 5.08)
				(name "DRAM_DQM0")
				(number "AC3")
			)
			(pin bidirectional line
				(at -25.4 55.88 0)
				(length 5.08)
				(name "DRAM_D8")
				(number "AD5")
			)
			(pin bidirectional line
				(at -25.4 53.34 0)
				(length 5.08)
				(name "DRAM_D9")
				(number "AE5")
			)
			(pin bidirectional line
				(at -25.4 50.8 0)
				(length 5.08)
				(name "DRAM_D10")
				(number "AA6")
			)
			(pin bidirectional line
				(at -25.4 48.26 0)
				(length 5.08)
				(name "DRAM_D11")
				(number "AE7")
			)
			(pin bidirectional line
				(at -25.4 45.72 0)
				(length 5.08)
				(name "DRAM_D12")
				(number "AB5")
			)
			(pin bidirectional line
				(at -25.4 43.18 0)
				(length 5.08)
				(name "DRAM_D13")
				(number "AC5")
			)
			(pin bidirectional line
				(at -25.4 40.64 0)
				(length 5.08)
				(name "DRAM_D14")
				(number "AB6")
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 5.08)
				(name "DRAM_D15")
				(number "AC7")
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 5.08)
				(name "DRAM_SDQS1")
				(number "AD6")
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 5.08)
				(name "DRAM_SDQS1_B")
				(number "AE6")
			)
			(pin output line
				(at -25.4 30.48 0)
				(length 5.08)
				(name "DRAM_DQM1")
				(number "AC6")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "DRAM_D16")
				(number "AB7")
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "DRAM_D17")
				(number "AA8")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "DRAM_D18")
				(number "AB9")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "DRAM_D19")
				(number "Y9")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "DRAM_D20")
				(number "Y7")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "DRAM_D21")
				(number "Y8")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "DRAM_D22")
				(number "AC8")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "DRAM_D23")
				(number "AA9")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "DRAM_SDQS2")
				(number "AD8")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "DRAM_SDQS2_B")
				(number "AE8")
			)
			(pin output line
				(at -25.4 0 0)
				(length 5.08)
				(name "DRAM_DQM2")
				(number "AB8")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "DRAM_D24")
				(number "AE9")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "DRAM_D25")
				(number "Y10")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "DRAM_D26")
				(number "AE11")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "DRAM_D27")
				(number "AB11")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "DRAM_D28")
				(number "AC9")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "DRAM_D29")
				(number "AD9")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 5.08)
				(name "DRAM_D30")
				(number "AD11")
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "DRAM_D31")
				(number "AC11")
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "DRAM_SDQS3")
				(number "AC10")
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 5.08)
				(name "DRAM_SDQS3_B")
				(number "AB10")
			)
			(pin output line
				(at -25.4 -30.48 0)
				(length 5.08)
				(name "DRAM_DQM3")
				(number "AE10")
			)
			(pin output line
				(at -25.4 -38.1 0)
				(length 5.08)
				(name "DRAM_RAS")
				(number "AB15")
			)
			(pin output line
				(at -25.4 -40.64 0)
				(length 5.08)
				(name "DRAM_CAS")
				(number "AE16")
			)
			(pin output line
				(at -25.4 -43.18 0)
				(length 5.08)
				(name "DRAM_SDWE")
				(number "AB16")
			)
			(pin output line
				(at -25.4 -48.26 0)
				(length 5.08)
				(name "DRAM_SDCKE0")
				(number "Y11")
			)
			(pin output line
				(at -25.4 -50.8 0)
				(length 5.08)
				(name "DRAM_SDCKE1")
				(number "AA11")
			)
			(pin output line
				(at -25.4 -55.88 0)
				(length 5.08)
				(name "DRAM_SDODT0")
				(number "AC16")
			)
			(pin output line
				(at -25.4 -58.42 0)
				(length 5.08)
				(name "DRAM_SDODT1")
				(number "AB17")
			)
			(pin output line
				(at -25.4 -63.5 0)
				(length 5.08)
				(name "DRAM_SDCLK_0")
				(number "AD15")
			)
			(pin output line
				(at -25.4 -66.04 0)
				(length 5.08)
				(name "DRAM_SDCLK_0_B")
				(number "AE15")
			)
			(pin output line
				(at -25.4 -71.12 0)
				(length 5.08)
				(name "DRAM_SDCLK_1")
				(number "AD14")
			)
			(pin output line
				(at -25.4 -73.66 0)
				(length 5.08)
				(name "DRAM_SDCLK_1_B")
				(number "AE14")
			)
			(pin output line
				(at -25.4 -78.74 0)
				(length 5.08)
				(name "DRAM_RESET")
				(number "Y6")
			)
			(pin power_in line
				(at -25.4 -83.82 0)
				(length 5.08)
				(name "DRAM_VREF")
				(number "AC2")
			)
			(pin passive line
				(at -25.4 -88.9 0)
				(length 5.08)
				(name "ZQPAD")
				(number "AE17")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "NVCC_DRAM")
				(number "R18")
			)
			(pin passive line
				(at 0 93.98 270)
				(length 5.08)
				(hide yes)
				(name "NVCC_DRAM")
				(number "T18")
			)
			(pin passive line
				(at 0 93.98 270)
				(length 5.08)
				(hide yes)
				(name "NVCC_DRAM")
				(number "U18")
			)
			(pin passive line
				(at 0 93.98 270)
				(length 5.08)
				(hide yes)
				(name "NVCC_DRAM")
				(number "V10")
			)
			(pin passive line
				(at 0 93.98 270)
				(length 5.08)
				(hide yes)
				(name "NVCC_DRAM")
				(number "V11")
			)
			(pin passive line
				(at 0 93.98 270)
				(length 5.08)
				(hide yes)
				(name "NVCC_DRAM")
				(number "V12")
			)
			(pin passive line
				(at 0 93.98 270)
				(length 5.08)
				(hide yes)
				(name "NVCC_DRAM")
				(number "V13")
			)
			(pin passive line
				(at 0 93.98 270)
				(length 5.08)
				(hide yes)
				(name "NVCC_DRAM")
				(number "V14")
			)
			(pin passive line
				(at 0 93.98 270)
				(length 5.08)
				(hide yes)
				(name "NVCC_DRAM")
				(number "V15")
			)
			(pin passive line
				(at 0 93.98 270)
				(length 5.08)
				(hide yes)
				(name "NVCC_DRAM")
				(number "V16")
			)
			(pin passive line
				(at 0 93.98 270)
				(length 5.08)
				(hide yes)
				(name "NVCC_DRAM")
				(number "V17")
			)
			(pin passive line
				(at 0 93.98 270)
				(length 5.08)
				(hide yes)
				(name "NVCC_DRAM")
				(number "V18")
			)
			(pin passive line
				(at 0 93.98 270)
				(length 5.08)
				(hide yes)
				(name "NVCC_DRAM")
				(number "V9")
			)
			(pin bidirectional line
				(at 25.4 86.36 180)
				(length 5.08)
				(name "DRAM_D32")
				(number "AA17")
			)
			(pin bidirectional line
				(at 25.4 83.82 180)
				(length 5.08)
				(name "DRAM_D33")
				(number "AA18")
			)
			(pin bidirectional line
				(at 25.4 81.28 180)
				(length 5.08)
				(name "DRAM_D34")
				(number "AC18")
			)
			(pin bidirectional line
				(at 25.4 78.74 180)
				(length 5.08)
				(name "DRAM_D35")
				(number "AE19")
			)
			(pin bidirectional line
				(at 25.4 76.2 180)
				(length 5.08)
				(name "DRAM_D36")
				(number "Y17")
			)
			(pin bidirectional line
				(at 25.4 73.66 180)
				(length 5.08)
				(name "DRAM_D37")
				(number "Y18")
			)
			(pin bidirectional line
				(at 25.4 71.12 180)
				(length 5.08)
				(name "DRAM_D38")
				(number "AB19")
			)
			(pin bidirectional line
				(at 25.4 68.58 180)
				(length 5.08)
				(name "DRAM_D39")
				(number "AC19")
			)
			(pin bidirectional line
				(at 25.4 66.04 180)
				(length 5.08)
				(name "DRAM_SDQS4")
				(number "AD18")
			)
			(pin bidirectional line
				(at 25.4 63.5 180)
				(length 5.08)
				(name "DRAM_SDQS4_B")
				(number "AE18")
			)
			(pin output line
				(at 25.4 60.96 180)
				(length 5.08)
				(name "DRAM_DQM4")
				(number "AB18")
			)
			(pin bidirectional line
				(at 25.4 55.88 180)
				(length 5.08)
				(name "DRAM_D40")
				(number "Y19")
			)
			(pin bidirectional line
				(at 25.4 53.34 180)
				(length 5.08)
				(name "DRAM_D41")
				(number "AB20")
			)
			(pin bidirectional line
				(at 25.4 50.8 180)
				(length 5.08)
				(name "DRAM_D42")
				(number "AB21")
			)
			(pin bidirectional line
				(at 25.4 48.26 180)
				(length 5.08)
				(name "DRAM_D43")
				(number "AD21")
			)
			(pin bidirectional line
				(at 25.4 45.72 180)
				(length 5.08)
				(name "DRAM_D44")
				(number "Y20")
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 5.08)
				(name "DRAM_D45")
				(number "AA20")
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 5.08)
				(name "DRAM_D46")
				(number "AE21")
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 5.08)
				(name "DRAM_D47")
				(number "AC21")
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 5.08)
				(name "DRAM_SDQS5")
				(number "AD20")
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 5.08)
				(name "DRAM_SDQS5_B")
				(number "AE20")
			)
			(pin output line
				(at 25.4 30.48 180)
				(length 5.08)
				(name "DRAM_DQM5")
				(number "AC20")
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "DRAM_D48")
				(number "AC22")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 5.08)
				(name "DRAM_D49")
				(number "AE22")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "DRAM_D50")
				(number "AE24")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "DRAM_D51")
				(number "AC24")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "DRAM_D52")
				(number "AB22")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "DRAM_D53")
				(number "AC23")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "DRAM_D54")
				(number "AD25")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "DRAM_D55")
				(number "AC25")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "DRAM_SDQS6")
				(number "AD23")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "DRAM_SDQS6_B")
				(number "AE23")
			)
			(pin output line
				(at 25.4 0 180)
				(length 5.08)
				(name "DRAM_DQM6")
				(number "AD24")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "DRAM_D56")
				(number "AB25")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "DRAM_D57")
				(number "AA21")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "DRAM_D58")
				(number "Y25")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "DRAM_D59")
				(number "Y22")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "DRAM_D60")
				(number "AB23")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "DRAM_D61")
				(number "AA23")
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 5.08)
				(name "DRAM_D62")
				(number "Y23")
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "DRAM_D63")
				(number "W25")
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "DRAM_SDQS7")
				(number "AA25")
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "DRAM_SDQS7_B")
				(number "AA24")
			)
			(pin output line
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "DRAM_DQM7")
				(number "Y21")
			)
			(pin output line
				(at 25.4 -38.1 180)
				(length 5.08)
				(name "DRAM_A0")
				(number "AC14")
			)
			(pin output line
				(at 25.4 -40.64 180)
				(length 5.08)
				(name "DRAM_A1")
				(number "AB14")
			)
			(pin output line
				(at 25.4 -43.18 180)
				(length 5.08)
				(name "DRAM_A2")
				(number "AA14")
			)
			(pin output line
				(at 25.4 -45.72 180)
				(length 5.08)
				(name "DRAM_A3")
				(number "Y14")
			)
			(pin output line
				(at 25.4 -48.26 180)
				(length 5.08)
				(name "DRAM_A4")
				(number "W14")
			)
			(pin output line
				(at 25.4 -50.8 180)
				(length 5.08)
				(name "DRAM_A5")
				(number "AE13")
			)
			(pin output line
				(at 25.4 -53.34 180)
				(length 5.08)
				(name "DRAM_A6")
				(number "AC13")
			)
			(pin output line
				(at 25.4 -55.88 180)
				(length 5.08)
				(name "DRAM_A7")
				(number "Y13")
			)
			(pin output line
				(at 25.4 -58.42 180)
				(length 5.08)
				(name "DRAM_A8")
				(number "AB13")
			)
			(pin output line
				(at 25.4 -60.96 180)
				(length 5.08)
				(name "DRAM_A9")
				(number "AE12")
			)
			(pin output line
				(at 25.4 -63.5 180)
				(length 5.08)
				(name "DRAM_A10")
				(number "AA15")
			)
			(pin output line
				(at 25.4 -66.04 180)
				(length 5.08)
				(name "DRAM_A11")
				(number "AC12")
			)
			(pin output line
				(at 25.4 -68.58 180)
				(length 5.08)
				(name "DRAM_A12")
				(number "AD12")
			)
			(pin output line
				(at 25.4 -71.12 180)
				(length 5.08)
				(name "DRAM_A13")
				(number "AC17")
			)
			(pin output line
				(at 25.4 -73.66 180)
				(length 5.08)
				(name "DRAM_A14")
				(number "AA12")
			)
			(pin output line
				(at 25.4 -76.2 180)
				(length 5.08)
				(name "DRAM_A15")
				(number "Y12")
			)
			(pin output line
				(at 25.4 -81.28 180)
				(length 5.08)
				(name "DRAM_SDBA0")
				(number "AC15")
			)
			(pin output line
				(at 25.4 -83.82 180)
				(length 5.08)
				(name "DRAM_SDBA1")
				(number "Y15")
			)
			(pin output line
				(at 25.4 -86.36 180)
				(length 5.08)
				(name "DRAM_SDBA2")
				(number "AB12")
			)
			(pin output line
				(at 25.4 -91.44 180)
				(length 5.08)
				(name "DRAM_CS0")
				(number "Y16")
			)
			(pin output line
				(at 25.4 -93.98 180)
				(length 5.08)
				(name "DRAM_CS1")
				(number "AD17")
			)
		)
		(symbol "MCIMX6QP7CVT_22_0"
			(text "Crystal Oscillator"
				(at 0 1.27 0)
			)
		)
		(symbol "MCIMX6QP7CVT_22_1"
			(text "NVCC_PLL_OUT"
				(at 0 -2.54 0)
			)
			(pin input line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "XTALI")
				(number "A7")
			)
			(pin output line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "XTALO")
				(number "B7")
			)
		)
		(symbol "MCIMX6QP7CVT_23_0"
			(text "RTC"
				(at 0 1.27 0)
			)
		)
		(symbol "MCIMX6QP7CVT_23_1"
			(text "VDD_SNVS_CAP"
				(at 0 -2.54 0)
			)
			(pin input line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "RTC_XTALI")
				(number "D9")
			)
			(pin output line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "RTC_XTALO")
				(number "C9")
			)
		)
		(symbol "MCIMX6QP7CVT_24_0"
			(text "SATA"
				(at 0 -3.81 0)
			)
		)
		(symbol "MCIMX6QP7CVT_24_1"
			(pin passive line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "SATA_REXT")
				(number "C14")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 5.08)
				(name "SATA_VP")
				(number "G13")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 5.08)
				(name "SATA_VPH")
				(number "G12")
			)
			(pin input line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "SATA_RXM")
				(number "A14")
			)
			(pin input line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "SATA_RXP")
				(number "B14")
			)
			(pin output line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "SATA_TXM")
				(number "B12")
			)
			(pin output line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "SATA_TXP")
				(number "A12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCIMX6D4AVT"
		(extends "MCIMX6QP5EYM")
		(property "Reference" "U"
			(at 15.24 90.17 0)
		)
		(property "Value" "MCIMX6D4AVT"
			(at -13.97 90.17 0)
		)
		(property "Footprint" "Package_BGA:BGA-624_21x21mm_Layout25x25_P0.8mm"
			(at -13.97 55.88 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/IMX6DQAEC.pdf"
			(at -11.43 55.88 0)
		)
		(property "Description" "i.MX 6Dual Automotive and Infotainment Application Processor, BGA-624"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual-Core ARM Cortex A9 SOC Automotive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "BGA*21x21mm*Layout25x25*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCIMX6D5EYM"
		(extends "MCIMX6QP5EYM")
		(property "Reference" "U"
			(at 15.24 90.17 0)
		)
		(property "Value" "MCIMX6D5EYM"
			(at -13.97 90.17 0)
		)
		(property "Footprint" "Package_BGA:BGA-624_21x21mm_Layout25x25_P0.8mm"
			(at -13.97 55.88 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/IMX6DQCEC.pdf"
			(at -11.43 55.88 0)
		)
		(property "Description" "i.MX 6Dual Application Processor for Consumer Products, BGA-624"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual-Core ARM Cortex A9 SOC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "BGA*21x21mm*Layout25x25*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCIMX6D6AVT"
		(extends "MCIMX6QP5EYM")
		(property "Reference" "U"
			(at 15.24 90.17 0)
		)
		(property "Value" "MCIMX6D6AVT"
			(at -13.97 90.17 0)
		)
		(property "Footprint" "Package_BGA:BGA-624_21x21mm_Layout25x25_P0.8mm"
			(at -13.97 55.88 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/IMX6DQAEC.pdf"
			(at -11.43 55.88 0)
		)
		(property "Description" "i.MX 6Dual Automotive and Infotainment Application Processor, BGA-624"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual-Core ARM Cortex A9 SOC Automotive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "BGA*21x21mm*Layout25x25*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCIMX6D7CVT"
		(extends "MCIMX6QP7CVT")
		(property "Reference" "U"
			(at 15.24 90.17 0)
		)
		(property "Value" "MCIMX6D7CVT"
			(at -13.97 90.17 0)
		)
		(property "Footprint" "Package_BGA:BGA-624_21x21mm_Layout25x25_P0.8mm"
			(at -13.97 55.88 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/IMX6DQIEC.pdf"
			(at -11.43 55.88 0)
		)
		(property "Description" "i.MX 6Dual Application Processor for Industrial Products, BGA-624"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual-Core ARM Cortex A9 SOC Industrial"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "BGA*21x21mm*Layout25x25*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCIMX6DP4AVT"
		(extends "MCIMX6QP5EYM")
		(property "Reference" "U"
			(at 15.24 90.17 0)
		)
		(property "Value" "MCIMX6DP4AVT"
			(at -13.97 90.17 0)
		)
		(property "Footprint" "Package_BGA:BGA-624_21x21mm_Layout25x25_P0.8mm"
			(at -13.97 55.88 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/IMX6DQPAEC.pdf"
			(at -11.43 55.88 0)
		)
		(property "Description" "i.MX 6DualPlus Automotive and Infotainment Application Processor, BGA-624"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual-Core ARM Cortex A9 SOC Automotive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "BGA*21x21mm*Layout25x25*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCIMX6DP5EVT"
		(extends "MCIMX6QP5EYM")
		(property "Reference" "U"
			(at 15.24 90.17 0)
		)
		(property "Value" "MCIMX6DP5EVT"
			(at -13.97 90.17 0)
		)
		(property "Footprint" "Package_BGA:BGA-624_21x21mm_Layout25x25_P0.8mm"
			(at -13.97 55.88 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/IMX6DQPCEC.pdf"
			(at -11.43 55.88 0)
		)
		(property "Description" "i.MX 6DualPlus Application Processor for Consumer Products, BGA-624"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual-Core ARM Cortex A9 SOC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "BGA*21x21mm*Layout25x25*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCIMX6DP5EYM"
		(extends "MCIMX6QP5EYM")
		(property "Reference" "U"
			(at 15.24 90.17 0)
		)
		(property "Value" "MCIMX6DP5EYM"
			(at -13.97 90.17 0)
		)
		(property "Footprint" "Package_BGA:BGA-624_21x21mm_Layout25x25_P0.8mm"
			(at -13.97 55.88 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/IMX6DQPCEC.pdf"
			(at -11.43 55.88 0)
		)
		(property "Description" "i.MX 6DualPlus Application Processor for Consumer Products, BGA-624"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual-Core ARM Cortex A9 SOC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "BGA*21x21mm*Layout25x25*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCIMX6DP6AVT"
		(extends "MCIMX6QP5EYM")
		(property "Reference" "U"
			(at 15.24 90.17 0)
		)
		(property "Value" "MCIMX6DP6AVT"
			(at -13.97 90.17 0)
		)
		(property "Footprint" "Package_BGA:BGA-624_21x21mm_Layout25x25_P0.8mm"
			(at -13.97 55.88 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/IMX6DQPAEC.pdf"
			(at -11.43 55.88 0)
		)
		(property "Description" "i.MX 6DualPlus Automotive and Infotainment Application Processor, BGA-624"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual-Core ARM Cortex A9 SOC Automotive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "BGA*21x21mm*Layout25x25*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCIMX6DP7CVT"
		(extends "MCIMX6QP7CVT")
		(property "Reference" "U"
			(at 15.24 90.17 0)
		)
		(property "Value" "MCIMX6DP7CVT"
			(at -13.97 90.17 0)
		)
		(property "Footprint" "Package_BGA:BGA-624_21x21mm_Layout25x25_P0.8mm"
			(at -13.97 55.88 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/IMX6DQPIEC.pdf"
			(at -11.43 55.88 0)
		)
		(property "Description" "i.MX 6DualPlus Application Processor for Industrial Products, BGA-624"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual-Core ARM Cortex A9 SOC Industrial"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "BGA*21x21mm*Layout25x25*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCIMX6Q4AVT"
		(extends "MCIMX6QP5EYM")
		(property "Reference" "U"
			(at 15.24 90.17 0)
		)
		(property "Value" "MCIMX6Q4AVT"
			(at -13.97 90.17 0)
		)
		(property "Footprint" "Package_BGA:BGA-624_21x21mm_Layout25x25_P0.8mm"
			(at -13.97 55.88 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/IMX6DQAEC.pdf"
			(at -11.43 55.88 0)
		)
		(property "Description" "i.MX 6Quad Automotive and Infotainment Application Processor, BGA-624"
			(at 0 0 0)
		)
		(property "ki_keywords" "Quad-Core ARM Cortex A9 SOC Automotive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "BGA*21x21mm*Layout25x25*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCIMX6Q5EYM"
		(extends "MCIMX6QP5EYM")
		(property "Reference" "U"
			(at 15.24 90.17 0)
		)
		(property "Value" "MCIMX6Q5EYM"
			(at -13.97 90.17 0)
		)
		(property "Footprint" "Package_BGA:BGA-624_21x21mm_Layout25x25_P0.8mm"
			(at -13.97 55.88 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/IMX6DQCEC.pdf"
			(at -11.43 55.88 0)
		)
		(property "Description" "i.MX 6Quad Application Processor for Consumer Products, BGA-624"
			(at 0 0 0)
		)
		(property "ki_keywords" "Quad-Core ARM Cortex A9 SOC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "BGA*21x21mm*Layout25x25*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCIMX6Q6AVT"
		(extends "MCIMX6QP5EYM")
		(property "Reference" "U"
			(at 15.24 90.17 0)
		)
		(property "Value" "MCIMX6Q6AVT"
			(at -13.97 90.17 0)
		)
		(property "Footprint" "Package_BGA:BGA-624_21x21mm_Layout25x25_P0.8mm"
			(at -13.97 55.88 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/IMX6DQAEC.pdf"
			(at -11.43 55.88 0)
		)
		(property "Description" "i.MX 6Quad Automotive and Infotainment Application Processor, BGA-624"
			(at 0 0 0)
		)
		(property "ki_keywords" "Quad-Core ARM Cortex A9 SOC Automotive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "BGA*21x21mm*Layout25x25*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCIMX6Q7CVT"
		(extends "MCIMX6QP7CVT")
		(property "Reference" "U"
			(at 15.24 90.17 0)
		)
		(property "Value" "MCIMX6Q7CVT"
			(at -13.97 90.17 0)
		)
		(property "Footprint" "Package_BGA:BGA-624_21x21mm_Layout25x25_P0.8mm"
			(at -13.97 55.88 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/IMX6DQIEC.pdf"
			(at -11.43 55.88 0)
		)
		(property "Description" "i.MX 6Quad Application Processor for Industrial Products, BGA-624"
			(at 0 0 0)
		)
		(property "ki_keywords" "Quad-Core ARM Cortex A9 SOC Industrial"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "BGA*21x21mm*Layout25x25*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCIMX6QP4AVT"
		(extends "MCIMX6QP5EYM")
		(property "Reference" "U"
			(at 15.24 90.17 0)
		)
		(property "Value" "MCIMX6QP4AVT"
			(at -13.97 90.17 0)
		)
		(property "Footprint" "Package_BGA:BGA-624_21x21mm_Layout25x25_P0.8mm"
			(at -13.97 55.88 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/IMX6DQPAEC.pdf"
			(at -11.43 55.88 0)
		)
		(property "Description" "i.MX 6QuadPlus Automotive and Infotainment Application Processor, BGA-624"
			(at 0 0 0)
		)
		(property "ki_keywords" "Quad-Core ARM Cortex A9 SOC Automotive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "BGA*21x21mm*Layout25x25*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCIMX6QP5EVT"
		(extends "MCIMX6QP5EYM")
		(property "Reference" "U"
			(at 15.24 90.17 0)
		)
		(property "Value" "MCIMX6QP5EVT"
			(at -13.97 90.17 0)
		)
		(property "Footprint" "Package_BGA:BGA-624_21x21mm_Layout25x25_P0.8mm"
			(at -13.97 55.88 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/IMX6DQPCEC.pdf"
			(at -11.43 55.88 0)
		)
		(property "Description" "i.MX 6QuadPlus Application Processor for Consumer Products, BGA-624"
			(at 0 0 0)
		)
		(property "ki_keywords" "Quad-Core ARM Cortex A9 SOC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "BGA*21x21mm*Layout25x25*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCIMX6QP6AVT"
		(extends "MCIMX6QP5EYM")
		(property "Reference" "U"
			(at 15.24 90.17 0)
		)
		(property "Value" "MCIMX6QP6AVT"
			(at -13.97 90.17 0)
		)
		(property "Footprint" "Package_BGA:BGA-624_21x21mm_Layout25x25_P0.8mm"
			(at -13.97 55.88 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/IMX6DQPAEC.pdf"
			(at -11.43 55.88 0)
		)
		(property "Description" "i.MX 6QuadPlus Automotive and Infotainment Application Processor, BGA-624"
			(at 0 0 0)
		)
		(property "ki_keywords" "Quad-Core ARM Cortex A9 SOC Automotive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "BGA*21x21mm*Layout25x25*P0.8mm*"
			(at 0 0 0)
		)
	)
)
