(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "MPC8641D"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 1.27 0)
		)
		(property "Value" "MPC8641D"
			(at -2.54 -7.62 0)
		)
		(property "Footprint" ""
			(at -2.54 -2.54 0)
		)
		(property "Datasheet" ""
			(at -2.54 -2.54 0)
		)
		(property "Description" "Freescale PowerPC E600 core, package BGA1023 pins pitch 1mm"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "POWERPC"
			(at 0 0 0)
		)
		(symbol "MPC8641D_1_1"
			(text "DDR Memory Inter 2"
				(at 1.27 25.4 0)
			)
			(pin bidirectional line
				(at -33.02 104.14 0)
				(length 7.62)
				(name "D2_MDQ0")
				(number "A7")
			)
			(pin bidirectional line
				(at -33.02 101.6 0)
				(length 7.62)
				(name "D2_MDQ1")
				(number "B7")
			)
			(pin bidirectional line
				(at -33.02 99.06 0)
				(length 7.62)
				(name "D2_MDQ2")
				(number "C5")
			)
			(pin bidirectional line
				(at -33.02 96.52 0)
				(length 7.62)
				(name "D2_MDQ3")
				(number "D5")
			)
			(pin bidirectional line
				(at -33.02 93.98 0)
				(length 7.62)
				(name "D2_MDQ4")
				(number "C8")
			)
			(pin bidirectional line
				(at -33.02 91.44 0)
				(length 7.62)
				(name "D2_MDQ5")
				(number "D8")
			)
			(pin bidirectional line
				(at -33.02 88.9 0)
				(length 7.62)
				(name "D2_MDQ6")
				(number "D6")
			)
			(pin bidirectional line
				(at -33.02 86.36 0)
				(length 7.62)
				(name "D2_MDQ7")
				(number "A5")
			)
			(pin bidirectional line
				(at -33.02 83.82 0)
				(length 7.62)
				(name "D2_MDQ8")
				(number "C4")
			)
			(pin bidirectional line
				(at -33.02 81.28 0)
				(length 7.62)
				(name "D2_MDQ9")
				(number "A3")
			)
			(pin bidirectional line
				(at -33.02 78.74 0)
				(length 7.62)
				(name "D2_MDQ10")
				(number "D3")
			)
			(pin bidirectional line
				(at -33.02 76.2 0)
				(length 7.62)
				(name "D2_MDQ11")
				(number "D2")
			)
			(pin bidirectional line
				(at -33.02 73.66 0)
				(length 7.62)
				(name "D2_MDQ12")
				(number "A4")
			)
			(pin bidirectional line
				(at -33.02 71.12 0)
				(length 7.62)
				(name "D2_MDQ13")
				(number "B4")
			)
			(pin bidirectional line
				(at -33.02 68.58 0)
				(length 7.62)
				(name "D2_MDQ14")
				(number "C2")
			)
			(pin bidirectional line
				(at -33.02 66.04 0)
				(length 7.62)
				(name "D2_MDQ15")
				(number "C1")
			)
			(pin bidirectional line
				(at -33.02 63.5 0)
				(length 7.62)
				(name "D2_MDQ16")
				(number "E3")
			)
			(pin bidirectional line
				(at -33.02 60.96 0)
				(length 7.62)
				(name "D2_MDQ17")
				(number "E1")
			)
			(pin bidirectional line
				(at -33.02 58.42 0)
				(length 7.62)
				(name "D2_MDQ18")
				(number "H4")
			)
			(pin bidirectional line
				(at -33.02 55.88 0)
				(length 7.62)
				(name "D2_MDQ19")
				(number "G1")
			)
			(pin bidirectional line
				(at -33.02 53.34 0)
				(length 7.62)
				(name "D2_MDQ20")
				(number "D1")
			)
			(pin bidirectional line
				(at -33.02 50.8 0)
				(length 7.62)
				(name "D2_MDQ21")
				(number "E4")
			)
			(pin bidirectional line
				(at -33.02 48.26 0)
				(length 7.62)
				(name "D2_MDQ22")
				(number "G3")
			)
			(pin bidirectional line
				(at -33.02 45.72 0)
				(length 7.62)
				(name "D2_MDQ23")
				(number "G2")
			)
			(pin bidirectional line
				(at -33.02 43.18 0)
				(length 7.62)
				(name "D2_MDQ24")
				(number "J4")
			)
			(pin bidirectional line
				(at -33.02 40.64 0)
				(length 7.62)
				(name "D2_MDQ25")
				(number "J2")
			)
			(pin bidirectional line
				(at -33.02 38.1 0)
				(length 7.62)
				(name "D2_MDQ26")
				(number "L1")
			)
			(pin bidirectional line
				(at -33.02 35.56 0)
				(length 7.62)
				(name "D2_MDQ27")
				(number "L3")
			)
			(pin bidirectional line
				(at -33.02 33.02 0)
				(length 7.62)
				(name "D2_MDQ28")
				(number "H3")
			)
			(pin bidirectional line
				(at -33.02 30.48 0)
				(length 7.62)
				(name "D2_MDQ29")
				(number "H1")
			)
			(pin bidirectional line
				(at -33.02 27.94 0)
				(length 7.62)
				(name "D2_MDQ30")
				(number "K1")
			)
			(pin bidirectional line
				(at -33.02 25.4 0)
				(length 7.62)
				(name "D2_MDQ31")
				(number "L4")
			)
			(pin bidirectional line
				(at -33.02 22.86 0)
				(length 7.62)
				(name "D2_MDQ32")
				(number "AA4")
			)
			(pin bidirectional line
				(at -33.02 20.32 0)
				(length 7.62)
				(name "D2_MDQ33")
				(number "AA2")
			)
			(pin bidirectional line
				(at -33.02 17.78 0)
				(length 7.62)
				(name "D2_MDQ34")
				(number "AD1")
			)
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 7.62)
				(name "D2_MDQ35")
				(number "AD2")
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 7.62)
				(name "D2_MDQ36")
				(number "Y1")
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 7.62)
				(name "D2_MDQ37")
				(number "AA1")
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 7.62)
				(name "D2_MDQ38")
				(number "AC1")
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 7.62)
				(name "D2_MDQ39")
				(number "AC3")
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 7.62)
				(name "D2_MDQ40")
				(number "AD5")
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 7.62)
				(name "D2_MDQ41")
				(number "AE1")
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 7.62)
				(name "D2_MDQ42")
				(number "AG1")
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 7.62)
				(name "D2_MDQ43")
				(number "AG2")
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 7.62)
				(name "D2_MDQ44")
				(number "AC4")
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 7.62)
				(name "D2_MDQ45")
				(number "AD4")
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 7.62)
				(name "D2_MDQ46")
				(number "AF3")
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 7.62)
				(name "D2_MDQ47")
				(number "AF4")
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 7.62)
				(name "D2_MDQ48")
				(number "AH3")
			)
			(pin bidirectional line
				(at -33.02 -20.32 0)
				(length 7.62)
				(name "D2_MDQ49")
				(number "AJ1")
			)
			(pin bidirectional line
				(at -33.02 -22.86 0)
				(length 7.62)
				(name "D2_MDQ50")
				(number "AM1")
			)
			(pin bidirectional line
				(at -33.02 -25.4 0)
				(length 7.62)
				(name "D2_MDQ51")
				(number "AM3")
			)
			(pin bidirectional line
				(at -33.02 -27.94 0)
				(length 7.62)
				(name "D2_MDQ52")
				(number "AH1")
			)
			(pin bidirectional line
				(at -33.02 -30.48 0)
				(length 7.62)
				(name "D2_MDQ53")
				(number "AH2")
			)
			(pin bidirectional line
				(at -33.02 -33.02 0)
				(length 7.62)
				(name "D2_MDQ54")
				(number "AL2")
			)
			(pin bidirectional line
				(at -33.02 -35.56 0)
				(length 7.62)
				(name "D2_MDQ55")
				(number "AL3")
			)
			(pin bidirectional line
				(at -33.02 -38.1 0)
				(length 7.62)
				(name "D2_MDQ56")
				(number "AK5")
			)
			(pin bidirectional line
				(at -33.02 -40.64 0)
				(length 7.62)
				(name "D2_MDQ57")
				(number "AL5")
			)
			(pin bidirectional line
				(at -33.02 -43.18 0)
				(length 7.62)
				(name "D2_MDQ58")
				(number "AK7")
			)
			(pin bidirectional line
				(at -33.02 -45.72 0)
				(length 7.62)
				(name "D2_MDQ59")
				(number "AM7")
			)
			(pin bidirectional line
				(at -33.02 -48.26 0)
				(length 7.62)
				(name "D2_MDQ60")
				(number "AK4")
			)
			(pin bidirectional line
				(at -33.02 -50.8 0)
				(length 7.62)
				(name "D2_MDQ61")
				(number "AM4")
			)
			(pin bidirectional line
				(at -33.02 -53.34 0)
				(length 7.62)
				(name "D2_MDQ62")
				(number "AM6")
			)
			(pin bidirectional line
				(at -33.02 -55.88 0)
				(length 7.62)
				(name "D2_MDQ63")
				(number "AJ7")
			)
			(pin bidirectional line
				(at -33.02 -60.96 0)
				(length 7.62)
				(name "D2_MECC0")
				(number "H6")
			)
			(pin bidirectional line
				(at -33.02 -63.5 0)
				(length 7.62)
				(name "D2_MECC1")
				(number "J5")
			)
			(pin bidirectional line
				(at -33.02 -66.04 0)
				(length 7.62)
				(name "D2_MECC2")
				(number "M5")
			)
			(pin bidirectional line
				(at -33.02 -68.58 0)
				(length 7.62)
				(name "D2_MECC3")
				(number "M4")
			)
			(pin bidirectional line
				(at -33.02 -71.12 0)
				(length 7.62)
				(name "D2_MECC4")
				(number "G6")
			)
			(pin bidirectional line
				(at -33.02 -73.66 0)
				(length 7.62)
				(name "D2_MECC5")
				(number "H7")
			)
			(pin bidirectional line
				(at -33.02 -76.2 0)
				(length 7.62)
				(name "D2_MECC6")
				(number "M2")
			)
			(pin bidirectional line
				(at -33.02 -78.74 0)
				(length 7.62)
				(name "D2_MECC7")
				(number "M1")
			)
			(pin bidirectional line
				(at -33.02 -83.82 0)
				(length 7.62)
				(name "D2_MDQS0")
				(number "B6")
			)
			(pin bidirectional line
				(at -33.02 -86.36 0)
				(length 7.62)
				(name "D2_MDQS1")
				(number "B1")
			)
			(pin bidirectional line
				(at -33.02 -88.9 0)
				(length 7.62)
				(name "D2_MDQS2")
				(number "F1")
			)
			(pin bidirectional line
				(at -33.02 -91.44 0)
				(length 7.62)
				(name "D2_MDQS3")
				(number "K2")
			)
			(pin bidirectional line
				(at -33.02 -93.98 0)
				(length 7.62)
				(name "D2_MDQS4")
				(number "AB3")
			)
			(pin bidirectional line
				(at -33.02 -96.52 0)
				(length 7.62)
				(name "D2_MDQS5")
				(number "AF1")
			)
			(pin bidirectional line
				(at -33.02 -99.06 0)
				(length 7.62)
				(name "D2_MDQS6")
				(number "AL1")
			)
			(pin bidirectional line
				(at -33.02 -101.6 0)
				(length 7.62)
				(name "D2_MDQS7")
				(number "AL6")
			)
			(pin bidirectional line
				(at -33.02 -104.14 0)
				(length 7.62)
				(name "D2_MDQS8")
				(number "L6")
			)
			(pin output line
				(at 33.02 104.14 180)
				(length 7.62)
				(name "D2_MDM0")
				(number "C7")
			)
			(pin output line
				(at 33.02 101.6 180)
				(length 7.62)
				(name "D2_MDM1")
				(number "B3")
			)
			(pin output line
				(at 33.02 99.06 180)
				(length 7.62)
				(name "D2_MDM2")
				(number "F4")
			)
			(pin output line
				(at 33.02 96.52 180)
				(length 7.62)
				(name "D2_MDM3")
				(number "J1")
			)
			(pin output line
				(at 33.02 93.98 180)
				(length 7.62)
				(name "D2_MDM4")
				(number "AB1")
			)
			(pin output line
				(at 33.02 91.44 180)
				(length 7.62)
				(name "D2_MDM5")
				(number "AE2")
			)
			(pin output line
				(at 33.02 88.9 180)
				(length 7.62)
				(name "D2_MDM6")
				(number "AK1")
			)
			(pin output line
				(at 33.02 86.36 180)
				(length 7.62)
				(name "D2_MDM7")
				(number "AM5")
			)
			(pin output line
				(at 33.02 83.82 180)
				(length 7.62)
				(name "D2_MDM8")
				(number "K6")
			)
			(pin output line
				(at 33.02 78.74 180)
				(length 7.62)
				(name "D2_MBA0")
				(number "W5")
			)
			(pin output line
				(at 33.02 76.2 180)
				(length 7.62)
				(name "D2_MBA1")
				(number "V5")
			)
			(pin output line
				(at 33.02 73.66 180)
				(length 7.62)
				(name "D2_MBA2")
				(number "P3")
			)
			(pin output line
				(at 33.02 66.04 180)
				(length 7.62)
				(name "D2_MA0")
				(number "W1")
			)
			(pin output line
				(at 33.02 63.5 180)
				(length 7.62)
				(name "D2_MA1")
				(number "U4")
			)
			(pin output line
				(at 33.02 60.96 180)
				(length 7.62)
				(name "D2_MA2")
				(number "U3")
			)
			(pin output line
				(at 33.02 58.42 180)
				(length 7.62)
				(name "D2_MA3")
				(number "T1")
			)
			(pin output line
				(at 33.02 55.88 180)
				(length 7.62)
				(name "D2_MA4")
				(number "T2")
			)
			(pin output line
				(at 33.02 53.34 180)
				(length 7.62)
				(name "D2_MA5")
				(number "T3")
			)
			(pin output line
				(at 33.02 50.8 180)
				(length 7.62)
				(name "D2_MA6")
				(number "T5")
			)
			(pin output line
				(at 33.02 48.26 180)
				(length 7.62)
				(name "D2_MA7")
				(number "R2")
			)
			(pin output line
				(at 33.02 45.72 180)
				(length 7.62)
				(name "D2_MA8")
				(number "R1")
			)
			(pin output line
				(at 33.02 43.18 180)
				(length 7.62)
				(name "D2_MA9")
				(number "R5")
			)
			(pin output line
				(at 33.02 40.64 180)
				(length 7.62)
				(name "D2_MA10")
				(number "V4")
			)
			(pin output line
				(at 33.02 38.1 180)
				(length 7.62)
				(name "D2_MA11")
				(number "R4")
			)
			(pin output line
				(at 33.02 35.56 180)
				(length 7.62)
				(name "D2_MA12")
				(number "P1")
			)
			(pin output line
				(at 33.02 33.02 180)
				(length 7.62)
				(name "D2_MA13")
				(number "AH5")
			)
			(pin output line
				(at 33.02 30.48 180)
				(length 7.62)
				(name "D2_MA14")
				(number "P4")
			)
			(pin output line
				(at 33.02 27.94 180)
				(length 7.62)
				(name "D2_MA15")
				(number "N1")
			)
			(pin output line
				(at 33.02 22.86 180)
				(length 7.62)
				(name "/D2_MWE")
				(number "Y4")
			)
			(pin output line
				(at 33.02 20.32 180)
				(length 7.62)
				(name "/D2_MRAS")
				(number "W3")
			)
			(pin output line
				(at 33.02 17.78 180)
				(length 7.62)
				(name "/D2_MCAS")
				(number "AB5")
			)
			(pin output line
				(at 33.02 10.16 180)
				(length 7.62)
				(name "/D2_MCS0")
				(number "Y3")
			)
			(pin output line
				(at 33.02 7.62 180)
				(length 7.62)
				(name "/D2_MCS1")
				(number "AF6")
			)
			(pin output line
				(at 33.02 5.08 180)
				(length 7.62)
				(name "/D2_MCS2")
				(number "AA5")
			)
			(pin output line
				(at 33.02 2.54 180)
				(length 7.62)
				(name "/D2_MCS3")
				(number "AF7")
			)
			(pin output line
				(at 33.02 -2.54 180)
				(length 7.62)
				(name "D2_MCKE0")
				(number "N6")
			)
			(pin output line
				(at 33.02 -5.08 180)
				(length 7.62)
				(name "D2_MCKE1")
				(number "N5")
			)
			(pin output line
				(at 33.02 -7.62 180)
				(length 7.62)
				(name "D2_MCKE2")
				(number "N2")
			)
			(pin output line
				(at 33.02 -10.16 180)
				(length 7.62)
				(name "D2_MCKE3")
				(number "N3")
			)
			(pin output line
				(at 33.02 -17.78 180)
				(length 7.62)
				(name "D2_MCK0")
				(number "U1")
			)
			(pin output line
				(at 33.02 -20.32 180)
				(length 7.62)
				(name "D2_MCK1")
				(number "F5")
			)
			(pin output line
				(at 33.02 -22.86 180)
				(length 7.62)
				(name "D2_MCK2")
				(number "AJ3")
			)
			(pin output line
				(at 33.02 -25.4 180)
				(length 7.62)
				(name "D2_MCK3")
				(number "V2")
			)
			(pin output line
				(at 33.02 -27.94 180)
				(length 7.62)
				(name "D2_MCK4")
				(number "E7")
			)
			(pin output line
				(at 33.02 -30.48 180)
				(length 7.62)
				(name "D2_MCK5")
				(number "AG4")
			)
			(pin output line
				(at 33.02 -38.1 180)
				(length 7.62)
				(name "/D2_MCK0")
				(number "V1")
			)
			(pin output line
				(at 33.02 -40.64 180)
				(length 7.62)
				(name "/D2_MCK1")
				(number "G5")
			)
			(pin output line
				(at 33.02 -43.18 180)
				(length 7.62)
				(name "/D2_MCK2")
				(number "AJ4")
			)
			(pin output line
				(at 33.02 -45.72 180)
				(length 7.62)
				(name "/D2_MCK3")
				(number "W2")
			)
			(pin output line
				(at 33.02 -48.26 180)
				(length 7.62)
				(name "/D2_MCK4")
				(number "E6")
			)
			(pin output line
				(at 33.02 -50.8 180)
				(length 7.62)
				(name "/D2_MCK5")
				(number "AG5")
			)
			(pin output line
				(at 33.02 -55.88 180)
				(length 7.62)
				(name "D2_MODT0")
				(number "AE6")
			)
			(pin output line
				(at 33.02 -58.42 180)
				(length 7.62)
				(name "D2_MODT1")
				(number "AG7")
			)
			(pin output line
				(at 33.02 -60.96 180)
				(length 7.62)
				(name "D2_MODT2")
				(number "AE5")
			)
			(pin output line
				(at 33.02 -63.5 180)
				(length 7.62)
				(name "D2_MODT3")
				(number "AH6")
			)
			(pin output line
				(at 33.02 -68.58 180)
				(length 7.62)
				(name "D2_MVREF")
				(number "A18")
			)
			(pin bidirectional line
				(at 33.02 -73.66 180)
				(length 7.62)
				(name "/D2_MDQS0")
				(number "A6")
			)
			(pin bidirectional line
				(at 33.02 -76.2 180)
				(length 7.62)
				(name "/D2_MDQS1")
				(number "A2")
			)
			(pin bidirectional line
				(at 33.02 -78.74 180)
				(length 7.62)
				(name "/D2_MDQS2")
				(number "F2")
			)
			(pin bidirectional line
				(at 33.02 -81.28 180)
				(length 7.62)
				(name "/D2_MDQS3")
				(number "K3")
			)
			(pin bidirectional line
				(at 33.02 -83.82 180)
				(length 7.62)
				(name "/D2_MDQS4")
				(number "AB2")
			)
			(pin bidirectional line
				(at 33.02 -86.36 180)
				(length 7.62)
				(name "/D2_MDQS5")
				(number "AE3")
			)
			(pin bidirectional line
				(at 33.02 -88.9 180)
				(length 7.62)
				(name "/D2_MDQS6")
				(number "AK2")
			)
			(pin bidirectional line
				(at 33.02 -91.44 180)
				(length 7.62)
				(name "/D2_MDQS7")
				(number "AJ6")
			)
			(pin bidirectional line
				(at 33.02 -93.98 180)
				(length 7.62)
				(name "/D2_MDQS8")
				(number "K5")
			)
			(pin bidirectional line
				(at 33.02 -99.06 180)
				(length 7.62)
				(name "D2_MDIC0")
				(number "F8")
			)
			(pin bidirectional line
				(at 33.02 -101.6 180)
				(length 7.62)
				(name "D2_MDIC1")
				(number "F7")
			)
		)
		(symbol "MPC8641D_2_1"
			(text "SERDES1"
				(at 0 107.95 0)
			)
			(text "SERDES2"
				(at 0 48.26 0)
			)
			(text "eTSEC1"
				(at 0 11.43 0)
			)
			(text "eTSEC2"
				(at 0 -38.1 0)
			)
			(text "eTSEC3"
				(at 0 -74.93 0)
			)
			(text "eTSEC4"
				(at 0 -111.76 0)
			)
			(pin input line
				(at -27.94 135.89 0)
				(length 7.62)
				(name "SD1_RX0")
				(number "J32")
			)
			(pin input line
				(at -27.94 133.35 0)
				(length 7.62)
				(name "SD1_RX1")
				(number "K30")
			)
			(pin input line
				(at -27.94 130.81 0)
				(length 7.62)
				(name "SD1_RX2")
				(number "L32")
			)
			(pin input line
				(at -27.94 128.27 0)
				(length 7.62)
				(name "SD1_RX3")
				(number "M30")
			)
			(pin input line
				(at -27.94 125.73 0)
				(length 7.62)
				(name "SD1_RX4")
				(number "T30")
			)
			(pin input line
				(at -27.94 123.19 0)
				(length 7.62)
				(name "SD1_RX5")
				(number "U32")
			)
			(pin input line
				(at -27.94 120.65 0)
				(length 7.62)
				(name "SD1_RX6")
				(number "V30")
			)
			(pin input line
				(at -27.94 118.11 0)
				(length 7.62)
				(name "SD1_RX7")
				(number "W32")
			)
			(pin input line
				(at -27.94 113.03 0)
				(length 7.62)
				(name "/SD1_RX0")
				(number "J31")
			)
			(pin input line
				(at -27.94 110.49 0)
				(length 7.62)
				(name "/SD1_RX1")
				(number "K29")
			)
			(pin input line
				(at -27.94 107.95 0)
				(length 7.62)
				(name "/SD1_RX2")
				(number "L31")
			)
			(pin input line
				(at -27.94 105.41 0)
				(length 7.62)
				(name "/SD1_RX3")
				(number "M29")
			)
			(pin input line
				(at -27.94 102.87 0)
				(length 7.62)
				(name "/SD1_RX4")
				(number "T29")
			)
			(pin input line
				(at -27.94 100.33 0)
				(length 7.62)
				(name "/SD1_RX5")
				(number "U31")
			)
			(pin input line
				(at -27.94 97.79 0)
				(length 7.62)
				(name "/SD1_RX6")
				(number "V29")
			)
			(pin input line
				(at -27.94 95.25 0)
				(length 7.62)
				(name "/SD1_RX7")
				(number "W31")
			)
			(pin input clock
				(at -27.94 90.17 0)
				(length 7.62)
				(name "SD1_REF_CLK")
				(number "N32")
			)
			(pin input clock
				(at -27.94 87.63 0)
				(length 7.62)
				(name "/SD1_REF_CLK")
				(number "N31")
			)
			(pin input line
				(at -27.94 83.82 0)
				(length 7.62)
				(name "SD1_IMP_CAL_TX")
				(number "Y26")
			)
			(pin input line
				(at -27.94 81.28 0)
				(length 7.62)
				(name "SD1_IMP_CAL_RX")
				(number "J28")
			)
			(pin input line
				(at -27.94 76.2 0)
				(length 7.62)
				(name "SD2_RX0")
				(number "Y30")
			)
			(pin input line
				(at -27.94 73.66 0)
				(length 7.62)
				(name "SD2_RX1")
				(number "AA32")
			)
			(pin input line
				(at -27.94 71.12 0)
				(length 7.62)
				(name "SD2_RX2")
				(number "AB30")
			)
			(pin input line
				(at -27.94 68.58 0)
				(length 7.62)
				(name "SD2_RX3")
				(number "AC32")
			)
			(pin input line
				(at -27.94 66.04 0)
				(length 7.62)
				(name "SD2_RX4")
				(number "AH30")
			)
			(pin input line
				(at -27.94 63.5 0)
				(length 7.62)
				(name "SD2_RX5")
				(number "AJ32")
			)
			(pin input line
				(at -27.94 60.96 0)
				(length 7.62)
				(name "SD2_RX6")
				(number "AK30")
			)
			(pin input line
				(at -27.94 58.42 0)
				(length 7.62)
				(name "SD2_RX7")
				(number "AL32")
			)
			(pin input line
				(at -27.94 53.34 0)
				(length 7.62)
				(name "/SD2_RX0")
				(number "Y29")
			)
			(pin input line
				(at -27.94 50.8 0)
				(length 7.62)
				(name "/SD2_RX1")
				(number "AA31")
			)
			(pin input line
				(at -27.94 48.26 0)
				(length 7.62)
				(name "/SD2_RX2")
				(number "AB29")
			)
			(pin input line
				(at -27.94 45.72 0)
				(length 7.62)
				(name "/SD2_RX3")
				(number "AC31")
			)
			(pin input line
				(at -27.94 43.18 0)
				(length 7.62)
				(name "/SD2_RX4")
				(number "AH29")
			)
			(pin input line
				(at -27.94 40.64 0)
				(length 7.62)
				(name "/SD2_RX5")
				(number "AJ31")
			)
			(pin input line
				(at -27.94 38.1 0)
				(length 7.62)
				(name "/SD2_RX6")
				(number "AK29")
			)
			(pin input line
				(at -27.94 35.56 0)
				(length 7.62)
				(name "/SD2_RX7")
				(number "AL31")
			)
			(pin input clock
				(at -27.94 30.48 0)
				(length 7.62)
				(name "SD2_REF_CLK")
				(number "AE32")
			)
			(pin input clock
				(at -27.94 27.94 0)
				(length 7.62)
				(name "/SD2_REF_CLK")
				(number "AE31")
			)
			(pin input line
				(at -27.94 24.13 0)
				(length 7.62)
				(name "SD2_IMP_CAL_TX")
				(number "AM29")
			)
			(pin input line
				(at -27.94 21.59 0)
				(length 7.62)
				(name "SD2_IMP_CAL_RX")
				(number "AA26")
			)
			(pin input line
				(at -27.94 15.24 0)
				(length 7.62)
				(name "TSEC1_RXD0")
				(number "AL25")
			)
			(pin input line
				(at -27.94 12.7 0)
				(length 7.62)
				(name "TSEC1_RXD1")
				(number "AL24")
			)
			(pin input line
				(at -27.94 10.16 0)
				(length 7.62)
				(name "TSEC1_RXD2")
				(number "AK26")
			)
			(pin input line
				(at -27.94 7.62 0)
				(length 7.62)
				(name "TSEC1_RXD3")
				(number "AK25")
			)
			(pin input line
				(at -27.94 5.08 0)
				(length 7.62)
				(name "TSEC1_RXD4")
				(number "AM26")
			)
			(pin input line
				(at -27.94 2.54 0)
				(length 7.62)
				(name "TSEC1_RXD5")
				(number "AF26")
			)
			(pin input line
				(at -27.94 0 0)
				(length 7.62)
				(name "TSEC1_RXD6")
				(number "AH24")
			)
			(pin input line
				(at -27.94 -2.54 0)
				(length 7.62)
				(name "TSEC1_RXD7")
				(number "AG25")
			)
			(pin input line
				(at -27.94 -8.89 0)
				(length 7.62)
				(name "TSEC1_RX_DV")
				(number "AJ24")
			)
			(pin input line
				(at -27.94 -11.43 0)
				(length 7.62)
				(name "TSEC1_RX_ER")
				(number "AJ25")
			)
			(pin input line
				(at -27.94 -13.97 0)
				(length 7.62)
				(name "TSEC1_RX_CLK")
				(number "AK24")
			)
			(pin input line
				(at -27.94 -16.51 0)
				(length 7.62)
				(name "TSEC1_COL")
				(number "AM25")
			)
			(pin input line
				(at -27.94 -21.59 0)
				(length 7.62)
				(name "TSEC2_RXD0")
				(number "AL22")
			)
			(pin input line
				(at -27.94 -24.13 0)
				(length 7.62)
				(name "TSEC2_RXD1")
				(number "AK22")
			)
			(pin input line
				(at -27.94 -26.67 0)
				(length 7.62)
				(name "TSEC2_RXD2")
				(number "AM21")
			)
			(pin input line
				(at -27.94 -29.21 0)
				(length 7.62)
				(name "TSEC2_RXD3")
				(number "AH20")
			)
			(pin input line
				(at -27.94 -31.75 0)
				(length 7.62)
				(name "TSEC2_RXD4")
				(number "AG20")
			)
			(pin input line
				(at -27.94 -34.29 0)
				(length 7.62)
				(name "TSEC2_RXD5")
				(number "AF20")
			)
			(pin input line
				(at -27.94 -36.83 0)
				(length 7.62)
				(name "TSEC2_RXD6")
				(number "AF23")
			)
			(pin input line
				(at -27.94 -39.37 0)
				(length 7.62)
				(name "TSEC3_RXD7")
				(number "AF22")
			)
			(pin input line
				(at -27.94 -45.72 0)
				(length 7.62)
				(name "TSEC2_RX_DV")
				(number "AC19")
			)
			(pin input line
				(at -27.94 -48.26 0)
				(length 7.62)
				(name "TSEC2_RX_ER")
				(number "AD21")
			)
			(pin input line
				(at -27.94 -50.8 0)
				(length 7.62)
				(name "TSEC2_RX_CLK")
				(number "AM22")
			)
			(pin input line
				(at -27.94 -53.34 0)
				(length 7.62)
				(name "TSEC2_COL")
				(number "AE21")
			)
			(pin input line
				(at -27.94 -58.42 0)
				(length 7.62)
				(name "TSEC3_RXD0")
				(number "AJ17")
			)
			(pin input line
				(at -27.94 -60.96 0)
				(length 7.62)
				(name "TSEC3_RXD1")
				(number "AE16")
			)
			(pin input line
				(at -27.94 -63.5 0)
				(length 7.62)
				(name "TSEC3_RXD2")
				(number "AH16")
			)
			(pin input line
				(at -27.94 -66.04 0)
				(length 7.62)
				(name "TSEC3_RXD3")
				(number "AH14")
			)
			(pin input line
				(at -27.94 -68.58 0)
				(length 7.62)
				(name "TSEC3_RXD4")
				(number "AJ19")
			)
			(pin input line
				(at -27.94 -71.12 0)
				(length 7.62)
				(name "TSEC3_RXD5")
				(number "AH15")
			)
			(pin input line
				(at -27.94 -73.66 0)
				(length 7.62)
				(name "TSEC3_RXD6")
				(number "AG16")
			)
			(pin input line
				(at -27.94 -76.2 0)
				(length 7.62)
				(name "TSEC3_RXD7")
				(number "AE19")
			)
			(pin input line
				(at -27.94 -82.55 0)
				(length 7.62)
				(name "TSEC3_RX_DV")
				(number "AG15")
			)
			(pin input line
				(at -27.94 -85.09 0)
				(length 7.62)
				(name "TSEC3_RX_ER")
				(number "AF16")
			)
			(pin input line
				(at -27.94 -87.63 0)
				(length 7.62)
				(name "TSEC3_RX_CLK")
				(number "AJ18")
			)
			(pin input line
				(at -27.94 -90.17 0)
				(length 7.62)
				(name "TSEC3_COL")
				(number "AF15")
			)
			(pin input line
				(at -27.94 -95.25 0)
				(length 7.62)
				(name "TSEC4_RXD0")
				(number "AG14")
			)
			(pin input line
				(at -27.94 -97.79 0)
				(length 7.62)
				(name "TSEC4_RXD1")
				(number "AD13")
			)
			(pin input line
				(at -27.94 -100.33 0)
				(length 7.62)
				(name "TSEC4_RXD2")
				(number "AF13")
			)
			(pin input line
				(at -27.94 -102.87 0)
				(length 7.62)
				(name "TSEC4_RXD3")
				(number "AD14")
			)
			(pin input line
				(at -27.94 -105.41 0)
				(length 7.62)
				(name "TSEX4_RXD4")
				(number "AE14")
			)
			(pin input line
				(at -27.94 -107.95 0)
				(length 7.62)
				(name "TSEC4_RXD5")
				(number "AB15")
			)
			(pin input line
				(at -27.94 -110.49 0)
				(length 7.62)
				(name "TSEC4_RXD6")
				(number "AC14")
			)
			(pin input line
				(at -27.94 -113.03 0)
				(length 7.62)
				(name "TSEC4_RXD7")
				(number "AE17")
			)
			(pin input line
				(at -27.94 -119.38 0)
				(length 7.62)
				(name "TSEC4_RX_DV")
				(number "AC15")
			)
			(pin input line
				(at -27.94 -121.92 0)
				(length 7.62)
				(name "TSEC4_RX_ER")
				(number "AF14")
			)
			(pin input line
				(at -27.94 -124.46 0)
				(length 7.62)
				(name "TSEC4_RX_CLK")
				(number "AG13")
			)
			(pin input line
				(at -27.94 -127 0)
				(length 7.62)
				(name "TSEC4_COL")
				(number "AC13")
			)
			(pin input line
				(at -27.94 -132.08 0)
				(length 7.62)
				(name "EC1_GTX_CLK125")
				(number "AL23")
			)
			(pin input line
				(at -27.94 -135.89 0)
				(length 7.62)
				(name "EC2_GTX_CLK125")
				(number "AM23")
			)
			(pin output line
				(at 27.94 135.89 180)
				(length 7.62)
				(name "SD1_TX0")
				(number "L26")
			)
			(pin output line
				(at 27.94 133.35 180)
				(length 7.62)
				(name "SD1_TX1")
				(number "M24")
			)
			(pin output line
				(at 27.94 130.81 180)
				(length 7.62)
				(name "SD1_TX2")
				(number "N26")
			)
			(pin output line
				(at 27.94 128.27 180)
				(length 7.62)
				(name "SD1_TX3")
				(number "P24")
			)
			(pin output line
				(at 27.94 125.73 180)
				(length 7.62)
				(name "SD1_TX4")
				(number "R26")
			)
			(pin output line
				(at 27.94 123.19 180)
				(length 7.62)
				(name "SD1_TX5")
				(number "T24")
			)
			(pin output line
				(at 27.94 120.65 180)
				(length 7.62)
				(name "SD1_TX6")
				(number "U26")
			)
			(pin output line
				(at 27.94 118.11 180)
				(length 7.62)
				(name "SD1_TX7")
				(number "V24")
			)
			(pin output line
				(at 27.94 113.03 180)
				(length 7.62)
				(name "/SD1_TX0")
				(number "L27")
			)
			(pin output line
				(at 27.94 110.49 180)
				(length 7.62)
				(name "/SD1_TX1")
				(number "M25")
			)
			(pin output line
				(at 27.94 107.95 180)
				(length 7.62)
				(name "/SD1_TX2")
				(number "N27")
			)
			(pin output line
				(at 27.94 105.41 180)
				(length 7.62)
				(name "/SD1_TX3")
				(number "P25")
			)
			(pin output line
				(at 27.94 102.87 180)
				(length 7.62)
				(name "/SD1_TX4")
				(number "R27")
			)
			(pin output line
				(at 27.94 100.33 180)
				(length 7.62)
				(name "/SD1_TX5")
				(number "T25")
			)
			(pin output line
				(at 27.94 97.79 180)
				(length 7.62)
				(name "/SD1_TX6")
				(number "U27")
			)
			(pin output line
				(at 27.94 95.25 180)
				(length 7.62)
				(name "/SD1_TX7")
				(number "V25")
			)
			(pin output line
				(at 27.94 90.17 180)
				(length 7.62)
				(name "SD1_PLL_TPD")
				(number "U28")
			)
			(pin output line
				(at 27.94 87.63 180)
				(length 7.62)
				(name "SD1_PLL_TPA")
				(number "T28")
			)
			(pin output line
				(at 27.94 83.82 180)
				(length 7.62)
				(name "SD1_DLL_TPD")
				(number "N28")
			)
			(pin output line
				(at 27.94 81.28 180)
				(length 7.62)
				(name "SD1_DLL_TPA")
				(number "P31")
			)
			(pin output line
				(at 27.94 76.2 180)
				(length 7.62)
				(name "SD2_TX0")
				(number "Y24")
			)
			(pin output line
				(at 27.94 73.66 180)
				(length 7.62)
				(name "SD2_TX1")
				(number "AA27")
			)
			(pin output line
				(at 27.94 71.12 180)
				(length 7.62)
				(name "SD2_TX2")
				(number "AB25")
			)
			(pin output line
				(at 27.94 68.58 180)
				(length 7.62)
				(name "SD2_TX3")
				(number "AC27")
			)
			(pin output line
				(at 27.94 66.04 180)
				(length 7.62)
				(name "SD2_TX4")
				(number "AE27")
			)
			(pin output line
				(at 27.94 63.5 180)
				(length 7.62)
				(name "SD2_TX5")
				(number "AG27")
			)
			(pin output line
				(at 27.94 60.96 180)
				(length 7.62)
				(name "SD2_TX6")
				(number "AJ27")
			)
			(pin output line
				(at 27.94 58.42 180)
				(length 7.62)
				(name "SD2_TX7")
				(number "AL27")
			)
			(pin output line
				(at 27.94 53.34 180)
				(length 7.62)
				(name "/SD2_TX0")
				(number "Y25")
			)
			(pin output line
				(at 27.94 50.8 180)
				(length 7.62)
				(name "/SD2_TX1")
				(number "AA28")
			)
			(pin output line
				(at 27.94 48.26 180)
				(length 7.62)
				(name "/SD2_TX2")
				(number "AB26")
			)
			(pin output line
				(at 27.94 45.72 180)
				(length 7.62)
				(name "/SD2_TX3")
				(number "AC28")
			)
			(pin output line
				(at 27.94 43.18 180)
				(length 7.62)
				(name "/SD2_TX4")
				(number "AE28")
			)
			(pin output line
				(at 27.94 40.64 180)
				(length 7.62)
				(name "/SD2_TX5")
				(number "AG28")
			)
			(pin output line
				(at 27.94 38.1 180)
				(length 7.62)
				(name "/SD2_TX6")
				(number "AJ28")
			)
			(pin output line
				(at 27.94 35.56 180)
				(length 7.62)
				(name "/SD2_TX7")
				(number "AL28")
			)
			(pin output line
				(at 27.94 30.48 180)
				(length 7.62)
				(name "SD2_PLL_TPD")
				(number "AF29")
			)
			(pin output line
				(at 27.94 27.94 180)
				(length 7.62)
				(name "SD2_PLL_TPA")
				(number "AF31")
			)
			(pin output line
				(at 27.94 24.13 180)
				(length 7.62)
				(name "SD2_DLL_TPD")
				(number "AD29")
			)
			(pin output line
				(at 27.94 21.59 180)
				(length 7.62)
				(name "SD2_DLL_TPA")
				(number "AD30")
			)
			(pin output line
				(at 27.94 15.24 180)
				(length 7.62)
				(name "TSEC1_TXD0")
				(number "AF25")
			)
			(pin output line
				(at 27.94 12.7 180)
				(length 7.62)
				(name "TSEC1_TXD1")
				(number "AC23")
			)
			(pin output line
				(at 27.94 10.16 180)
				(length 7.62)
				(name "TSEC1_TXD2")
				(number "AG24")
			)
			(pin output line
				(at 27.94 7.62 180)
				(length 7.62)
				(name "TSEC1_TXD3")
				(number "AG23")
			)
			(pin output line
				(at 27.94 5.08 180)
				(length 7.62)
				(name "TSEC1_TXD4")
				(number "AE24")
			)
			(pin output line
				(at 27.94 2.54 180)
				(length 7.62)
				(name "TSEC1_TXD5")
				(number "AE23")
			)
			(pin output line
				(at 27.94 0 180)
				(length 7.62)
				(name "TSEC1_TXD6")
				(number "AE22")
			)
			(pin output line
				(at 27.94 -2.54 180)
				(length 7.62)
				(name "TSEC1_TXD7")
				(number "AD22")
			)
			(pin output line
				(at 27.94 -6.35 180)
				(length 7.62)
				(name "TSEC1_TX_EN")
				(number "AB22")
			)
			(pin output line
				(at 27.94 -8.89 180)
				(length 7.62)
				(name "TSEC1_TX_ER")
				(number "AH26")
			)
			(pin input line
				(at 27.94 -11.43 180)
				(length 7.62)
				(name "TSEC1_TX_CLK")
				(number "AC22")
			)
			(pin output line
				(at 27.94 -13.97 180)
				(length 7.62)
				(name "TSEC1_GTX_CLK")
				(number "AH25")
			)
			(pin bidirectional line
				(at 27.94 -16.51 180)
				(length 7.62)
				(name "TSEC1_CRS")
				(number "AM24")
			)
			(pin output line
				(at 27.94 -21.59 180)
				(length 7.62)
				(name "TSEC2_TXD0")
				(number "AB20")
			)
			(pin output line
				(at 27.94 -24.13 180)
				(length 7.62)
				(name "TSEC2_TXD1")
				(number "AJ23")
			)
			(pin output line
				(at 27.94 -26.67 180)
				(length 7.62)
				(name "TSEC2_TXD2")
				(number "AJ22")
			)
			(pin output line
				(at 27.94 -29.21 180)
				(length 7.62)
				(name "TSEC2_TXD3")
				(number "AD19")
			)
			(pin output line
				(at 27.94 -31.75 180)
				(length 7.62)
				(name "TSEC2_TXD4")
				(number "AH23")
			)
			(pin output line
				(at 27.94 -34.29 180)
				(length 7.62)
				(name "TSEC2_TXD5")
				(number "AH21")
			)
			(pin output line
				(at 27.94 -36.83 180)
				(length 7.62)
				(name "TSEC2_TXD6")
				(number "AG22")
			)
			(pin output line
				(at 27.94 -39.37 180)
				(length 7.62)
				(name "TSEC2_TXD7")
				(number "AG21")
			)
			(pin output line
				(at 27.94 -43.18 180)
				(length 7.62)
				(name "TSEC2_TX_EN")
				(number "AB21")
			)
			(pin output line
				(at 27.94 -45.72 180)
				(length 7.62)
				(name "TSEC2_TX_ER")
				(number "AB19")
			)
			(pin input line
				(at 27.94 -48.26 180)
				(length 7.62)
				(name "TSEC2_TX_CLK")
				(number "AC21")
			)
			(pin output line
				(at 27.94 -50.8 180)
				(length 7.62)
				(name "TSEC2_GTX_CLK")
				(number "AD20")
			)
			(pin bidirectional line
				(at 27.94 -53.34 180)
				(length 7.62)
				(name "TSEC2_CRS")
				(number "AE20")
			)
			(pin output line
				(at 27.94 -58.42 180)
				(length 7.62)
				(name "TSEC3_TXD0")
				(number "AL21")
			)
			(pin output line
				(at 27.94 -60.96 180)
				(length 7.62)
				(name "TSEC3_TXD1")
				(number "AJ21")
			)
			(pin output line
				(at 27.94 -63.5 180)
				(length 7.62)
				(name "TSEC3_TXD2")
				(number "AM20")
			)
			(pin output line
				(at 27.94 -66.04 180)
				(length 7.62)
				(name "TSEC3_TXD3")
				(number "AJ20")
			)
			(pin output line
				(at 27.94 -68.58 180)
				(length 7.62)
				(name "TSEC3_TXD4")
				(number "AM19")
			)
			(pin output line
				(at 27.94 -71.12 180)
				(length 7.62)
				(name "TSEC3_TXD5")
				(number "AK21")
			)
			(pin output line
				(at 27.94 -73.66 180)
				(length 7.62)
				(name "TSEC3_TXD6")
				(number "AL20")
			)
			(pin output line
				(at 27.94 -76.2 180)
				(length 7.62)
				(name "TSEC3_TXD7")
				(number "AL19")
			)
			(pin output line
				(at 27.94 -80.01 180)
				(length 7.62)
				(name "TSEC3_TX_EN")
				(number "AH19")
			)
			(pin output line
				(at 27.94 -82.55 180)
				(length 7.62)
				(name "TSEC3_TX_ER")
				(number "AH17")
			)
			(pin input line
				(at 27.94 -85.09 180)
				(length 7.62)
				(name "TSEC3_TX_CLK")
				(number "AH18")
			)
			(pin output line
				(at 27.94 -87.63 180)
				(length 7.62)
				(name "TSEC3_GTX_CLK")
				(number "AG19")
			)
			(pin bidirectional line
				(at 27.94 -90.17 180)
				(length 7.62)
				(name "TSEC3_CRS")
				(number "AE15")
			)
			(pin output line
				(at 27.94 -95.25 180)
				(length 7.62)
				(name "TSEC4_TXD0")
				(number "AC18")
			)
			(pin output line
				(at 27.94 -97.79 180)
				(length 7.62)
				(name "TSEC4_TXD1")
				(number "AC16")
			)
			(pin output line
				(at 27.94 -100.33 180)
				(length 7.62)
				(name "TSEC4_TXD2")
				(number "AD18")
			)
			(pin output line
				(at 27.94 -102.87 180)
				(length 7.62)
				(name "TSEC4_TXD3")
				(number "AD17")
			)
			(pin output line
				(at 27.94 -105.41 180)
				(length 7.62)
				(name "TSEC4_TXD4")
				(number "AD16")
			)
			(pin output line
				(at 27.94 -107.95 180)
				(length 7.62)
				(name "TSEC4_TXD5")
				(number "AB18")
			)
			(pin output line
				(at 27.94 -110.49 180)
				(length 7.62)
				(name "TSEC4_TXD6")
				(number "AB17")
			)
			(pin output line
				(at 27.94 -113.03 180)
				(length 7.62)
				(name "TSEC4_TXD7")
				(number "AB16")
			)
			(pin output line
				(at 27.94 -116.84 180)
				(length 7.62)
				(name "TSEC4_TX_EN")
				(number "AF17")
			)
			(pin output line
				(at 27.94 -119.38 180)
				(length 7.62)
				(name "TSEC4_TX_ER")
				(number "AF19")
			)
			(pin input line
				(at 27.94 -121.92 180)
				(length 7.62)
				(name "TSEC4_TX_CLK")
				(number "AF18")
			)
			(pin output line
				(at 27.94 -124.46 180)
				(length 7.62)
				(name "TSEC4_GTX_CLK")
				(number "AG17")
			)
			(pin bidirectional line
				(at 27.94 -127 180)
				(length 7.62)
				(name "TSEC4_CRS")
				(number "AB14")
			)
			(pin output line
				(at 27.94 -132.08 180)
				(length 7.62)
				(name "EC_MDC")
				(number "G31")
			)
			(pin bidirectional line
				(at 27.94 -135.89 180)
				(length 7.62)
				(name "EC_MDIO")
				(number "G32")
			)
		)
		(symbol "MPC8641D_3_1"
			(text "DUART"
				(at 0 128.27 0)
			)
			(text "LOCAL BUS"
				(at 0 54.61 0)
			)
			(text "IRQ/DMA"
				(at 0 -17.78 0)
			)
			(text "MISC."
				(at 0 -58.42 0)
			)
			(pin input line
				(at -27.94 132.08 0)
				(length 7.62)
				(name "UART_SIN0")
				(number "B32")
			)
			(pin input line
				(at -27.94 129.54 0)
				(length 7.62)
				(name "UART_SIN1")
				(number "C32")
			)
			(pin input line
				(at -27.94 125.73 0)
				(length 7.62)
				(name "/UART_CTS0")
				(number "A31")
			)
			(pin input line
				(at -27.94 123.19 0)
				(length 7.62)
				(name "/UART_CTS1")
				(number "B31")
			)
			(pin bidirectional line
				(at -27.94 118.11 0)
				(length 7.62)
				(name "LAD0")
				(number "A30")
			)
			(pin bidirectional line
				(at -27.94 115.57 0)
				(length 7.62)
				(name "LAD1")
				(number "E29")
			)
			(pin bidirectional line
				(at -27.94 113.03 0)
				(length 7.62)
				(name "LAD2")
				(number "C29")
			)
			(pin bidirectional line
				(at -27.94 110.49 0)
				(length 7.62)
				(name "LAD3")
				(number "D28")
			)
			(pin bidirectional line
				(at -27.94 107.95 0)
				(length 7.62)
				(name "LAD4")
				(number "D29")
			)
			(pin bidirectional line
				(at -27.94 105.41 0)
				(length 7.62)
				(name "LAD5")
				(number "H25")
			)
			(pin bidirectional line
				(at -27.94 102.87 0)
				(length 7.62)
				(name "LAD6")
				(number "B29")
			)
			(pin bidirectional line
				(at -27.94 100.33 0)
				(length 7.62)
				(name "LAD7")
				(number "A29")
			)
			(pin bidirectional line
				(at -27.94 97.79 0)
				(length 7.62)
				(name "LAD8")
				(number "C28")
			)
			(pin bidirectional line
				(at -27.94 95.25 0)
				(length 7.62)
				(name "LAD9")
				(number "L22")
			)
			(pin bidirectional line
				(at -27.94 92.71 0)
				(length 7.62)
				(name "LAD10")
				(number "M22")
			)
			(pin bidirectional line
				(at -27.94 90.17 0)
				(length 7.62)
				(name "LAD11")
				(number "A28")
			)
			(pin bidirectional line
				(at -27.94 87.63 0)
				(length 7.62)
				(name "LAD12")
				(number "C27")
			)
			(pin bidirectional line
				(at -27.94 85.09 0)
				(length 7.62)
				(name "LAD13")
				(number "H26")
			)
			(pin bidirectional line
				(at -27.94 82.55 0)
				(length 7.62)
				(name "LAD14")
				(number "G26")
			)
			(pin bidirectional line
				(at -27.94 80.01 0)
				(length 7.62)
				(name "LAD15")
				(number "B27")
			)
			(pin bidirectional line
				(at -27.94 77.47 0)
				(length 7.62)
				(name "LAD16")
				(number "B26")
			)
			(pin bidirectional line
				(at -27.94 74.93 0)
				(length 7.62)
				(name "LAD17")
				(number "A27")
			)
			(pin bidirectional line
				(at -27.94 72.39 0)
				(length 7.62)
				(name "LAD18")
				(number "E27")
			)
			(pin bidirectional line
				(at -27.94 69.85 0)
				(length 7.62)
				(name "LAD19")
				(number "G25")
			)
			(pin bidirectional line
				(at -27.94 67.31 0)
				(length 7.62)
				(name "LAD20")
				(number "D26")
			)
			(pin bidirectional line
				(at -27.94 64.77 0)
				(length 7.62)
				(name "LAD21")
				(number "E26")
			)
			(pin bidirectional line
				(at -27.94 62.23 0)
				(length 7.62)
				(name "LAD22")
				(number "G24")
			)
			(pin bidirectional line
				(at -27.94 59.69 0)
				(length 7.62)
				(name "LAD23")
				(number "F27")
			)
			(pin bidirectional line
				(at -27.94 57.15 0)
				(length 7.62)
				(name "LAD24")
				(number "A26")
			)
			(pin bidirectional line
				(at -27.94 54.61 0)
				(length 7.62)
				(name "LAD25")
				(number "A25")
			)
			(pin bidirectional line
				(at -27.94 52.07 0)
				(length 7.62)
				(name "LAD26")
				(number "C25")
			)
			(pin bidirectional line
				(at -27.94 49.53 0)
				(length 7.62)
				(name "LAD27")
				(number "H23")
			)
			(pin bidirectional line
				(at -27.94 46.99 0)
				(length 7.62)
				(name "LAD28")
				(number "K22")
			)
			(pin bidirectional line
				(at -27.94 44.45 0)
				(length 7.62)
				(name "LAD29")
				(number "D25")
			)
			(pin bidirectional line
				(at -27.94 41.91 0)
				(length 7.62)
				(name "LAD30")
				(number "F25")
			)
			(pin bidirectional line
				(at -27.94 39.37 0)
				(length 7.62)
				(name "LAD31")
				(number "H22")
			)
			(pin output line
				(at -27.94 34.29 0)
				(length 7.62)
				(name "LA27")
				(number "J21")
			)
			(pin output line
				(at -27.94 31.75 0)
				(length 7.62)
				(name "LA28")
				(number "K21")
			)
			(pin output line
				(at -27.94 29.21 0)
				(length 7.62)
				(name "LA29")
				(number "G22")
			)
			(pin output line
				(at -27.94 26.67 0)
				(length 7.62)
				(name "LA30")
				(number "F24")
			)
			(pin output line
				(at -27.94 24.13 0)
				(length 7.62)
				(name "LA31")
				(number "G21")
			)
			(pin bidirectional line
				(at -27.94 19.05 0)
				(length 7.62)
				(name "LDP0")
				(number "A24")
			)
			(pin bidirectional line
				(at -27.94 16.51 0)
				(length 7.62)
				(name "LDP1")
				(number "E24")
			)
			(pin bidirectional line
				(at -27.94 13.97 0)
				(length 7.62)
				(name "LDP2")
				(number "C24")
			)
			(pin bidirectional line
				(at -27.94 11.43 0)
				(length 7.62)
				(name "LDP3")
				(number "B24")
			)
			(pin input line
				(at -27.94 6.35 0)
				(length 7.62)
				(name "/MCP_0")
				(number "F17")
			)
			(pin input line
				(at -27.94 3.81 0)
				(length 7.62)
				(name "/MCP_1")
				(number "H17")
			)
			(pin input line
				(at -27.94 0 0)
				(length 7.62)
				(name "IRQ0")
				(number "G28")
			)
			(pin input line
				(at -27.94 -2.54 0)
				(length 7.62)
				(name "IRQ1")
				(number "G29")
			)
			(pin input line
				(at -27.94 -5.08 0)
				(length 7.62)
				(name "IRQ2")
				(number "H27")
			)
			(pin input line
				(at -27.94 -7.62 0)
				(length 7.62)
				(name "IRQ3")
				(number "J23")
			)
			(pin input line
				(at -27.94 -10.16 0)
				(length 7.62)
				(name "IRQ4")
				(number "M23")
			)
			(pin input line
				(at -27.94 -12.7 0)
				(length 7.62)
				(name "IRQ5")
				(number "J27")
			)
			(pin input line
				(at -27.94 -15.24 0)
				(length 7.62)
				(name "IRQ6")
				(number "F28")
			)
			(pin input line
				(at -27.94 -17.78 0)
				(length 7.62)
				(name "IRQ7")
				(number "J24")
			)
			(pin input line
				(at -27.94 -20.32 0)
				(length 7.62)
				(name "IRQ8")
				(number "L23")
			)
			(pin input line
				(at -27.94 -22.86 0)
				(length 7.62)
				(name "IRQ9/DMA_DREQ3")
				(number "B30")
			)
			(pin input line
				(at -27.94 -25.4 0)
				(length 7.62)
				(name "IRQ10/DMA_DACK3")
				(number "C30")
			)
			(pin input line
				(at -27.94 -27.94 0)
				(length 7.62)
				(name "IRQ11/DMA_DDONE3")
				(number "D30")
			)
			(pin bidirectional line
				(at -27.94 -33.02 0)
				(length 7.62)
				(name "IIC1_SDA")
				(number "A16")
			)
			(pin bidirectional line
				(at -27.94 -35.56 0)
				(length 7.62)
				(name "IIC1_SCL")
				(number "B17")
			)
			(pin bidirectional line
				(at -27.94 -39.37 0)
				(length 7.62)
				(name "IIC2_SDA")
				(number "A21")
			)
			(pin bidirectional line
				(at -27.94 -41.91 0)
				(length 7.62)
				(name "IIC2_SCL")
				(number "B21")
			)
			(pin bidirectional line
				(at -27.94 -45.72 0)
				(length 7.62)
				(name "/HRESET")
				(number "B18")
			)
			(pin input line
				(at -27.94 -48.26 0)
				(length 7.62)
				(name "/SRESET_0")
				(number "C20")
			)
			(pin input line
				(at -27.94 -50.8 0)
				(length 7.62)
				(name "/SRESET_1")
				(number "C21")
			)
			(pin input line
				(at -27.94 -54.61 0)
				(length 7.62)
				(name "SMI_0")
				(number "L15")
			)
			(pin input line
				(at -27.94 -57.15 0)
				(length 7.62)
				(name "SMI_1")
				(number "L16")
			)
			(pin input line
				(at -27.94 -60.96 0)
				(length 7.62)
				(name "/CKSTP_IN")
				(number "L18")
			)
			(pin input line
				(at -27.94 -64.77 0)
				(length 7.62)
				(name "TRIG_IN")
				(number "J14")
			)
			(pin input line
				(at -27.94 -69.85 0)
				(length 7.62)
				(name "TCK")
				(number "H18")
			)
			(pin input line
				(at -27.94 -72.39 0)
				(length 7.62)
				(name "TDI")
				(number "J18")
			)
			(pin output line
				(at -27.94 -74.93 0)
				(length 7.62)
				(name "TDO")
				(number "G18")
			)
			(pin input line
				(at -27.94 -77.47 0)
				(length 7.62)
				(name "TMS")
				(number "F18")
			)
			(pin input line
				(at -27.94 -80.01 0)
				(length 7.62)
				(name "/TRST")
				(number "A17")
			)
			(pin input line
				(at -27.94 -85.09 0)
				(length 7.62)
				(name "/LSSD_MODE")
				(number "C18")
			)
			(pin input line
				(at -27.94 -88.9 0)
				(length 7.62)
				(name "TEST_MODE0")
				(number "C16")
			)
			(pin input line
				(at -27.94 -91.44 0)
				(length 7.62)
				(name "TEST_MODE1")
				(number "E17")
			)
			(pin input line
				(at -27.94 -93.98 0)
				(length 7.62)
				(name "TEST_MODE2")
				(number "D18")
			)
			(pin input line
				(at -27.94 -96.52 0)
				(length 7.62)
				(name "TEST_MODE3")
				(number "D16")
			)
			(pin unspecified line
				(at -27.94 -101.6 0)
				(length 7.62)
				(name "SPARE")
				(number "J17")
			)
			(pin no_connect line
				(at -20.32 -106.68 0)
				(length 7.62)
				(hide yes)
				(name "NC")
				(number "K24")
			)
			(pin no_connect line
				(at -20.32 -109.22 0)
				(length 7.62)
				(hide yes)
				(name "NC")
				(number "K25")
			)
			(pin no_connect line
				(at -20.32 -111.76 0)
				(length 7.62)
				(hide yes)
				(name "NC")
				(number "P28")
			)
			(pin no_connect line
				(at -20.32 -114.3 0)
				(length 7.62)
				(hide yes)
				(name "NC")
				(number "P29")
			)
			(pin no_connect line
				(at -20.32 -116.84 0)
				(length 7.62)
				(hide yes)
				(name "NC")
				(number "W26")
			)
			(pin no_connect line
				(at -20.32 -119.38 0)
				(length 7.62)
				(hide yes)
				(name "NC")
				(number "W27")
			)
			(pin no_connect line
				(at -20.32 -121.92 0)
				(length 7.62)
				(hide yes)
				(name "NC")
				(number "AD25")
			)
			(pin no_connect line
				(at -20.32 -124.46 0)
				(length 7.62)
				(hide yes)
				(name "NC")
				(number "AD26")
			)
			(pin output line
				(at 27.94 132.08 180)
				(length 7.62)
				(name "UART_SOUT0")
				(number "D31")
			)
			(pin output line
				(at 27.94 129.54 180)
				(length 7.62)
				(name "UART_SOUT1")
				(number "A32")
			)
			(pin output line
				(at 27.94 125.73 180)
				(length 7.62)
				(name "/UART_RTS0")
				(number "C31")
			)
			(pin output line
				(at 27.94 123.19 180)
				(length 7.62)
				(name "/UART_RTS1")
				(number "E30")
			)
			(pin output line
				(at 27.94 118.11 180)
				(length 7.62)
				(name "/LCS0")
				(number "A22")
			)
			(pin output line
				(at 27.94 115.57 180)
				(length 7.62)
				(name "/LCS1")
				(number "C22")
			)
			(pin output line
				(at 27.94 113.03 180)
				(length 7.62)
				(name "/LCS3")
				(number "D23")
			)
			(pin output line
				(at 27.94 110.49 180)
				(length 7.62)
				(name "/LCS4")
				(number "E22")
			)
			(pin output line
				(at 27.94 107.95 180)
				(length 7.62)
				(name "/LCS5")
				(number "A23")
			)
			(pin output line
				(at 27.94 102.87 180)
				(length 7.62)
				(name "/LCS5/DMA_DREQ2")
				(number "B23")
			)
			(pin output line
				(at 27.94 100.33 180)
				(length 7.62)
				(name "/LCS6/DMA_DACK2")
				(number "E23")
			)
			(pin output line
				(at 27.94 97.79 180)
				(length 7.62)
				(name "/LCS7/DMA_DDONE2")
				(number "F23")
			)
			(pin output line
				(at 27.94 93.98 180)
				(length 7.62)
				(name "/LWE0/LBS0/LSDDQM0")
				(number "E21")
			)
			(pin output line
				(at 27.94 91.44 180)
				(length 7.62)
				(name "/LWE1/LBS1/LSDDQM1")
				(number "F21")
			)
			(pin output line
				(at 27.94 88.9 180)
				(length 7.62)
				(name "/LWE2/LBS2/LSDDQM2")
				(number "D22")
			)
			(pin output line
				(at 27.94 86.36 180)
				(length 7.62)
				(name "/LWE3/LBS3/LSDDQM3")
				(number "E20")
			)
			(pin output line
				(at 27.94 82.55 180)
				(length 7.62)
				(name "LBCTL")
				(number "D21")
			)
			(pin output line
				(at 27.94 80.01 180)
				(length 7.62)
				(name "LALE")
				(number "E19")
			)
			(pin output line
				(at 27.94 76.2 180)
				(length 7.62)
				(name "LGPL0/LSDA10")
				(number "F20")
			)
			(pin output line
				(at 27.94 73.66 180)
				(length 7.62)
				(name "LGPL1/LSDWE")
				(number "H20")
			)
			(pin output line
				(at 27.94 71.12 180)
				(length 7.62)
				(name "LGPL2/LOE/LSDRAS")
				(number "J20")
			)
			(pin output line
				(at 27.94 68.58 180)
				(length 7.62)
				(name "LGPL3/LSDCAS")
				(number "K20")
			)
			(pin bidirectional line
				(at 27.94 66.04 180)
				(length 7.62)
				(name "LGPL4/LGTA/LUPWAIT/LPBSE")
				(number "L21")
			)
			(pin output line
				(at 27.94 63.5 180)
				(length 7.62)
				(name "LGPL5")
				(number "J19")
			)
			(pin output line
				(at 27.94 59.69 180)
				(length 7.62)
				(name "LCKE")
				(number "H19")
			)
			(pin output line
				(at 27.94 57.15 180)
				(length 7.62)
				(name "LCLK0")
				(number "G19")
			)
			(pin output line
				(at 27.94 54.61 180)
				(length 7.62)
				(name "LCLK1")
				(number "L19")
			)
			(pin output line
				(at 27.94 52.07 180)
				(length 7.62)
				(name "LCLK2")
				(number "M20")
			)
			(pin input line
				(at 27.94 48.26 180)
				(length 7.62)
				(name "LSYNC_IN")
				(number "M19")
			)
			(pin input line
				(at 27.94 45.72 180)
				(length 7.62)
				(name "LSYNC_OUT")
				(number "D20")
			)
			(pin input line
				(at 27.94 3.81 180)
				(length 7.62)
				(name "DMA_DREQ0")
				(number "E31")
			)
			(pin input line
				(at 27.94 1.27 180)
				(length 7.62)
				(name "DMA_DREQ1")
				(number "E32")
			)
			(pin output line
				(at 27.94 -3.81 180)
				(length 7.62)
				(name "DMA_DACK0")
				(number "D32")
			)
			(pin output line
				(at 27.94 -6.35 180)
				(length 7.62)
				(name "DMA_DACK1")
				(number "F30")
			)
			(pin output line
				(at 27.94 -11.43 180)
				(length 7.62)
				(name "DMA_DDONE0")
				(number "F31")
			)
			(pin output line
				(at 27.94 -13.97 180)
				(length 7.62)
				(name "DMA_DDONE1")
				(number "F32")
			)
			(pin output line
				(at 27.94 -20.32 180)
				(length 7.62)
				(name "/IRQ_OUT")
				(number "J26")
			)
			(pin input line
				(at 27.94 -33.02 180)
				(length 7.62)
				(name "SYSCLK")
				(number "G16")
			)
			(pin output clock
				(at 27.94 -36.83 180)
				(length 7.62)
				(name "CLK_OUT")
				(number "B16")
			)
			(pin input line
				(at 27.94 -40.64 180)
				(length 7.62)
				(name "RTC")
				(number "K17")
			)
			(pin output line
				(at 27.94 -45.72 180)
				(length 7.62)
				(name "/HRESET_REQ")
				(number "K18")
			)
			(pin bidirectional line
				(at 27.94 -52.07 180)
				(length 7.62)
				(name "TEMP_ANODE")
				(number "AA11")
			)
			(pin bidirectional line
				(at 27.94 -54.61 180)
				(length 7.62)
				(name "TEMP_CATHODE")
				(number "Y11")
			)
			(pin output line
				(at 27.94 -60.96 180)
				(length 7.62)
				(name "/CKSTP_OUT")
				(number "L17")
			)
			(pin output line
				(at 27.94 -64.77 180)
				(length 7.62)
				(name "TRIG_OUT/READY")
				(number "J13")
			)
			(pin output line
				(at 27.94 -68.58 180)
				(length 7.62)
				(name "D1_MSRCID0/LB_SRCID0")
				(number "F15")
			)
			(pin output line
				(at 27.94 -71.12 180)
				(length 7.62)
				(name "D1_MSRCID1/LB_SRCID1")
				(number "K15")
			)
			(pin output line
				(at 27.94 -73.66 180)
				(length 7.62)
				(name "D1_MSRCID2/LB_SRCID2")
				(number "K14")
			)
			(pin output line
				(at 27.94 -76.2 180)
				(length 7.62)
				(name "D1_MSRCID3/LB_SRCID3")
				(number "H15")
			)
			(pin output line
				(at 27.94 -78.74 180)
				(length 7.62)
				(name "D1_MSRCID4/LB_SRCID4")
				(number "G15")
			)
			(pin output line
				(at 27.94 -81.28 180)
				(length 7.62)
				(name "D1_MDVAL/LB_DVAL")
				(number "J16")
			)
			(pin output line
				(at 27.94 -85.09 180)
				(length 7.62)
				(name "D2_MSRCID0")
				(number "E16")
			)
			(pin output line
				(at 27.94 -87.63 180)
				(length 7.62)
				(name "D2_MSRCID1")
				(number "C17")
			)
			(pin output line
				(at 27.94 -90.17 180)
				(length 7.62)
				(name "D2_MSRCID2")
				(number "F16")
			)
			(pin output line
				(at 27.94 -92.71 180)
				(length 7.62)
				(name "D2_MSRCID3")
				(number "H16")
			)
			(pin output line
				(at 27.94 -95.25 180)
				(length 7.62)
				(name "D2_MSRCID4")
				(number "K16")
			)
			(pin output line
				(at 27.94 -97.79 180)
				(length 7.62)
				(name "D2_MDVAL")
				(number "D19")
			)
			(pin output line
				(at 27.94 -101.6 180)
				(length 7.62)
				(name "ASLEEP")
				(number "C19")
			)
			(pin unspecified line
				(at 27.94 -106.68 180)
				(length 7.62)
				(name "RSVD")
				(number "H30")
			)
			(pin unspecified line
				(at 27.94 -109.22 180)
				(length 7.62)
				(name "RSVD")
				(number "R32")
			)
			(pin unspecified line
				(at 27.94 -111.76 180)
				(length 7.62)
				(name "RSVD")
				(number "V28")
			)
			(pin unspecified line
				(at 27.94 -114.3 180)
				(length 7.62)
				(name "RSVD")
				(number "AG32")
			)
			(pin unspecified line
				(at 27.94 -118.11 180)
				(length 7.62)
				(name "RSVD")
				(number "H29")
			)
			(pin unspecified line
				(at 27.94 -120.65 180)
				(length 7.62)
				(name "RSVD")
				(number "R31")
			)
			(pin unspecified line
				(at 27.94 -123.19 180)
				(length 7.62)
				(name "RSVD")
				(number "W28")
			)
			(pin unspecified line
				(at 27.94 -125.73 180)
				(length 7.62)
				(name "RSVD")
				(number "AG31")
			)
			(pin unspecified line
				(at 27.94 -129.54 180)
				(length 7.62)
				(name "RSVD")
				(number "AD24")
			)
			(pin unspecified line
				(at 27.94 -132.08 180)
				(length 7.62)
				(name "RSVD")
				(number "AG26")
			)
		)
		(symbol "MPC8641D_4_1"
			(text "CORE0 PWR"
				(at -5.08 44.45 900)
			)
			(text "PLAT PWR"
				(at -1.27 -8.89 0)
			)
			(text "GND"
				(at -1.27 -50.8 0)
			)
			(text "CORE1 PWR"
				(at 2.54 44.45 900)
			)
			(pin power_in line
				(at -30.48 83.82 0)
				(length 7.62)
				(name "AVDD_CORE0")
				(number "B20")
			)
			(pin power_in line
				(at -30.48 78.74 0)
				(length 7.62)
				(name "VDD_CORE0")
				(number "L12")
			)
			(pin power_in line
				(at -30.48 76.2 0)
				(length 7.62)
				(name "VDD_CORE0")
				(number "L13")
			)
			(pin power_in line
				(at -30.48 73.66 0)
				(length 7.62)
				(name "VDD_CORE0")
				(number "L14")
			)
			(pin power_in line
				(at -30.48 71.12 0)
				(length 7.62)
				(name "VDD_CORE0")
				(number "M13")
			)
			(pin power_in line
				(at -30.48 68.58 0)
				(length 7.62)
				(name "VDD_CORE0")
				(number "M15")
			)
			(pin power_in line
				(at -30.48 66.04 0)
				(length 7.62)
				(name "VDD_CORE0")
				(number "N12")
			)
			(pin power_in line
				(at -30.48 63.5 0)
				(length 7.62)
				(name "VDD_CORE0")
				(number "N14")
			)
			(pin power_in line
				(at -30.48 60.96 0)
				(length 7.62)
				(name "VDD_CORE0")
				(number "P11")
			)
			(pin power_in line
				(at -30.48 58.42 0)
				(length 7.62)
				(name "VDD_CORE0")
				(number "P13")
			)
			(pin power_in line
				(at -30.48 55.88 0)
				(length 7.62)
				(name "VDD_CORE0")
				(number "P15")
			)
			(pin power_in line
				(at -30.48 53.34 0)
				(length 7.62)
				(name "VDD_CORE0")
				(number "R12")
			)
			(pin power_in line
				(at -30.48 50.8 0)
				(length 7.62)
				(name "VDD_CORE0")
				(number "R14")
			)
			(pin power_in line
				(at -30.48 48.26 0)
				(length 7.62)
				(name "VDD_CORE0")
				(number "T11")
			)
			(pin power_in line
				(at -30.48 45.72 0)
				(length 7.62)
				(name "VDD_CORE0")
				(number "T13")
			)
			(pin power_in line
				(at -30.48 43.18 0)
				(length 7.62)
				(name "VDD_CORE0")
				(number "T15")
			)
			(pin power_in line
				(at -30.48 40.64 0)
				(length 7.62)
				(name "VDD_CORE0")
				(number "U12")
			)
			(pin power_in line
				(at -30.48 38.1 0)
				(length 7.62)
				(name "VDD_CORE0")
				(number "U14")
			)
			(pin power_in line
				(at -30.48 35.56 0)
				(length 7.62)
				(name "VDD_CORE0")
				(number "V11")
			)
			(pin power_in line
				(at -30.48 33.02 0)
				(length 7.62)
				(name "VDD_CORE0")
				(number "V13")
			)
			(pin power_in line
				(at -30.48 30.48 0)
				(length 7.62)
				(name "VDD_CORE0")
				(number "V15")
			)
			(pin power_in line
				(at -30.48 27.94 0)
				(length 7.62)
				(name "VDD_CORE0")
				(number "W12")
			)
			(pin power_in line
				(at -30.48 25.4 0)
				(length 7.62)
				(name "VDD_CORE0")
				(number "W14")
			)
			(pin power_in line
				(at -30.48 22.86 0)
				(length 7.62)
				(name "VDD_CORE0")
				(number "Y12")
			)
			(pin power_in line
				(at -30.48 20.32 0)
				(length 7.62)
				(name "VDD_CORE0")
				(number "Y13")
			)
			(pin power_in line
				(at -30.48 17.78 0)
				(length 7.62)
				(name "VDD_CORE0")
				(number "Y15")
			)
			(pin power_in line
				(at -30.48 15.24 0)
				(length 7.62)
				(name "VDD_CORE0")
				(number "AA12")
			)
			(pin power_in line
				(at -30.48 12.7 0)
				(length 7.62)
				(name "VDD_CORE0")
				(number "AA14")
			)
			(pin power_in line
				(at -30.48 10.16 0)
				(length 7.62)
				(name "VDD_CORE0")
				(number "AB13")
			)
			(pin power_in line
				(at -30.48 5.08 0)
				(length 7.62)
				(name "SENSEVDD_CORE0")
				(number "M14")
			)
			(pin power_in line
				(at -30.48 2.54 0)
				(length 7.62)
				(name "SENSEVSS_CORE0")
				(number "P14")
			)
			(pin power_in line
				(at -30.48 -2.54 0)
				(length 7.62)
				(name "VDD_PLAT")
				(number "M16")
			)
			(pin power_in line
				(at -30.48 -5.08 0)
				(length 7.62)
				(name "VDD_PLAT")
				(number "M17")
			)
			(pin power_in line
				(at -30.48 -7.62 0)
				(length 7.62)
				(name "VDD_PLAT")
				(number "M18")
			)
			(pin power_in line
				(at -30.48 -10.16 0)
				(length 7.62)
				(name "VDD_PLAT")
				(number "N20")
			)
			(pin power_in line
				(at -30.48 -12.7 0)
				(length 7.62)
				(name "VDD_PLAT")
				(number "N22")
			)
			(pin power_in line
				(at -30.48 -22.86 0)
				(length 7.62)
				(name "SGND")
				(number "H28")
			)
			(pin power_in line
				(at -30.48 -25.4 0)
				(length 7.62)
				(name "SGND")
				(number "H32")
			)
			(pin power_in line
				(at -30.48 -27.94 0)
				(length 7.62)
				(name "SGND")
				(number "J30")
			)
			(pin power_in line
				(at -30.48 -30.48 0)
				(length 7.62)
				(name "SGND")
				(number "K31")
			)
			(pin power_in line
				(at -30.48 -33.02 0)
				(length 7.62)
				(name "SGND")
				(number "L28")
			)
			(pin power_in line
				(at -30.48 -35.56 0)
				(length 7.62)
				(name "SGND")
				(number "L29")
			)
			(pin power_in line
				(at -30.48 -38.1 0)
				(length 7.62)
				(name "SGND")
				(number "M32")
			)
			(pin power_in line
				(at -30.48 -40.64 0)
				(length 7.62)
				(name "SGND")
				(number "N30")
			)
			(pin power_in line
				(at -30.48 -43.18 0)
				(length 7.62)
				(name "SGND")
				(number "R29")
			)
			(pin power_in line
				(at -30.48 -45.72 0)
				(length 7.62)
				(name "SGND")
				(number "T32")
			)
			(pin power_in line
				(at -30.48 -48.26 0)
				(length 7.62)
				(name "SGND")
				(number "U30")
			)
			(pin power_in line
				(at -30.48 -50.8 0)
				(length 7.62)
				(name "SGND")
				(number "V31")
			)
			(pin power_in line
				(at -30.48 -53.34 0)
				(length 7.62)
				(name "SGND")
				(number "W29")
			)
			(pin power_in line
				(at -30.48 -55.88 0)
				(length 7.62)
				(name "SGND")
				(number "Y32")
			)
			(pin power_in line
				(at -30.48 -58.42 0)
				(length 7.62)
				(name "SGND")
				(number "AA30")
			)
			(pin power_in line
				(at -30.48 -60.96 0)
				(length 7.62)
				(name "SGND")
				(number "AB31")
			)
			(pin power_in line
				(at -30.48 -63.5 0)
				(length 7.62)
				(name "SGND")
				(number "AC29")
			)
			(pin power_in line
				(at -30.48 -66.04 0)
				(length 7.62)
				(name "SGND")
				(number "AD32")
			)
			(pin power_in line
				(at -30.48 -68.58 0)
				(length 7.62)
				(name "SGND")
				(number "AE30")
			)
			(pin power_in line
				(at -30.48 -71.12 0)
				(length 7.62)
				(name "SGND")
				(number "AG29")
			)
			(pin power_in line
				(at -30.48 -73.66 0)
				(length 7.62)
				(name "SGND")
				(number "AH32")
			)
			(pin power_in line
				(at -30.48 -76.2 0)
				(length 7.62)
				(name "SGND")
				(number "AJ30")
			)
			(pin power_in line
				(at -30.48 -78.74 0)
				(length 7.62)
				(name "SGND")
				(number "AK31")
			)
			(pin power_in line
				(at -30.48 -81.28 0)
				(length 7.62)
				(name "SGND")
				(number "AL29")
			)
			(pin power_in line
				(at -30.48 -83.82 0)
				(length 7.62)
				(name "SGND")
				(number "AM32")
			)
			(pin power_in line
				(at 27.94 83.82 180)
				(length 7.62)
				(name "AVDD_CORE1")
				(number "A19")
			)
			(pin power_in line
				(at 27.94 78.74 180)
				(length 7.62)
				(name "VDD_CORE1")
				(number "R16")
			)
			(pin power_in line
				(at 27.94 76.2 180)
				(length 7.62)
				(name "VDD_CORE1")
				(number "R18")
			)
			(pin power_in line
				(at 27.94 73.66 180)
				(length 7.62)
				(name "VDD_CORE1")
				(number "R20")
			)
			(pin power_in line
				(at 27.94 71.12 180)
				(length 7.62)
				(name "VDD_CORE1")
				(number "T17")
			)
			(pin power_in line
				(at 27.94 68.58 180)
				(length 7.62)
				(name "VDD_CORE1")
				(number "T19")
			)
			(pin power_in line
				(at 27.94 66.04 180)
				(length 7.62)
				(name "VDD_CORE1")
				(number "T21")
			)
			(pin power_in line
				(at 27.94 63.5 180)
				(length 7.62)
				(name "VDD_CORE1")
				(number "T23")
			)
			(pin power_in line
				(at 27.94 60.96 180)
				(length 7.62)
				(name "VDD_CORE1")
				(number "U16")
			)
			(pin power_in line
				(at 27.94 58.42 180)
				(length 7.62)
				(name "VDD_CORE1")
				(number "U18")
			)
			(pin power_in line
				(at 27.94 55.88 180)
				(length 7.62)
				(name "VDD_CORE1")
				(number "U22")
			)
			(pin power_in line
				(at 27.94 53.34 180)
				(length 7.62)
				(name "VDD_CORE1")
				(number "V17")
			)
			(pin power_in line
				(at 27.94 50.8 180)
				(length 7.62)
				(name "VDD_CORE1")
				(number "V19")
			)
			(pin power_in line
				(at 27.94 48.26 180)
				(length 7.62)
				(name "VDD_CORE1")
				(number "V21")
			)
			(pin power_in line
				(at 27.94 45.72 180)
				(length 7.62)
				(name "VDD_CORE1")
				(number "V23")
			)
			(pin power_in line
				(at 27.94 43.18 180)
				(length 7.62)
				(name "VDD_CORE1")
				(number "W16")
			)
			(pin power_in line
				(at 27.94 40.64 180)
				(length 7.62)
				(name "VDD_CORE1")
				(number "W18")
			)
			(pin power_in line
				(at 27.94 38.1 180)
				(length 7.62)
				(name "VDD_CORE1")
				(number "W20")
			)
			(pin power_in line
				(at 27.94 35.56 180)
				(length 7.62)
				(name "VDD_CORE1")
				(number "W22")
			)
			(pin power_in line
				(at 27.94 33.02 180)
				(length 7.62)
				(name "VDD_CORE1")
				(number "Y17")
			)
			(pin power_in line
				(at 27.94 30.48 180)
				(length 7.62)
				(name "VDD_CORE1")
				(number "Y19")
			)
			(pin power_in line
				(at 27.94 27.94 180)
				(length 7.62)
				(name "VDD_CORE1")
				(number "Y21")
			)
			(pin power_in line
				(at 27.94 25.4 180)
				(length 7.62)
				(name "VDD_CORE1")
				(number "Y23")
			)
			(pin power_in line
				(at 27.94 22.86 180)
				(length 7.62)
				(name "VDD_CORE1")
				(number "AA16")
			)
			(pin power_in line
				(at 27.94 20.32 180)
				(length 7.62)
				(name "VDD_CORE1")
				(number "AA18")
			)
			(pin power_in line
				(at 27.94 17.78 180)
				(length 7.62)
				(name "VDD_CORE1")
				(number "AA20")
			)
			(pin power_in line
				(at 27.94 15.24 180)
				(length 7.62)
				(name "VDD_CORE1")
				(number "AA22")
			)
			(pin power_in line
				(at 27.94 12.7 180)
				(length 7.62)
				(name "VDD_CORE1")
				(number "AB23")
			)
			(pin power_in line
				(at 27.94 10.16 180)
				(length 7.62)
				(name "VDD_CORE1")
				(number "AC24")
			)
			(pin power_in line
				(at 27.94 5.08 180)
				(length 7.62)
				(name "SENSEVDD_CORE1")
				(number "U20")
			)
			(pin power_in line
				(at 27.94 2.54 180)
				(length 7.62)
				(name "SENSEVSS_CORE1")
				(number "V20")
			)
			(pin power_in line
				(at 27.94 -2.54 180)
				(length 7.62)
				(name "VDD_PLAT")
				(number "P17")
			)
			(pin power_in line
				(at 27.94 -5.08 180)
				(length 7.62)
				(name "VDD_PLAT")
				(number "P19")
			)
			(pin power_in line
				(at 27.94 -7.62 180)
				(length 7.62)
				(name "VDD_PLAT")
				(number "P21")
			)
			(pin power_in line
				(at 27.94 -10.16 180)
				(length 7.62)
				(name "VDD_PLAT")
				(number "P23")
			)
			(pin power_in line
				(at 27.94 -12.7 180)
				(length 7.62)
				(name "VDD_PLAT")
				(number "R22")
			)
			(pin power_in line
				(at 27.94 -16.51 180)
				(length 7.62)
				(name "VDD_PLAT/SENSEVDD_PLAT")
				(number "N18")
			)
			(pin power_in line
				(at 27.94 -22.86 180)
				(length 7.62)
				(name "XGND")
				(number "K27")
			)
			(pin power_in line
				(at 27.94 -25.4 180)
				(length 7.62)
				(name "XGND")
				(number "L25")
			)
			(pin power_in line
				(at 27.94 -27.94 180)
				(length 7.62)
				(name "XGND")
				(number "M26")
			)
			(pin power_in line
				(at 27.94 -30.48 180)
				(length 7.62)
				(name "XGND")
				(number "N24")
			)
			(pin power_in line
				(at 27.94 -33.02 180)
				(length 7.62)
				(name "XGND")
				(number "P27")
			)
			(pin power_in line
				(at 27.94 -35.56 180)
				(length 7.62)
				(name "XGND")
				(number "R25")
			)
			(pin power_in line
				(at 27.94 -38.1 180)
				(length 7.62)
				(name "XGND")
				(number "T26")
			)
			(pin power_in line
				(at 27.94 -40.64 180)
				(length 7.62)
				(name "XGND")
				(number "U24")
			)
			(pin power_in line
				(at 27.94 -43.18 180)
				(length 7.62)
				(name "XGND")
				(number "V27")
			)
			(pin power_in line
				(at 27.94 -45.72 180)
				(length 7.62)
				(name "XGND")
				(number "W25")
			)
			(pin power_in line
				(at 27.94 -48.26 180)
				(length 7.62)
				(name "XGND")
				(number "Y28")
			)
			(pin power_in line
				(at 27.94 -50.8 180)
				(length 7.62)
				(name "XGND")
				(number "AA24")
			)
			(pin power_in line
				(at 27.94 -53.34 180)
				(length 7.62)
				(name "XGND")
				(number "AB27")
			)
			(pin power_in line
				(at 27.94 -55.88 180)
				(length 7.62)
				(name "XGND")
				(number "AC25")
			)
			(pin power_in line
				(at 27.94 -58.42 180)
				(length 7.62)
				(name "XGND")
				(number "AD28")
			)
			(pin power_in line
				(at 27.94 -60.96 180)
				(length 7.62)
				(name "XGND")
				(number "AE26")
			)
			(pin power_in line
				(at 27.94 -63.5 180)
				(length 7.62)
				(name "XGND")
				(number "AF27")
			)
			(pin power_in line
				(at 27.94 -66.04 180)
				(length 7.62)
				(name "XGND")
				(number "AH28")
			)
			(pin power_in line
				(at 27.94 -68.58 180)
				(length 7.62)
				(name "XGND")
				(number "AJ26")
			)
			(pin power_in line
				(at 27.94 -71.12 180)
				(length 7.62)
				(name "XGND")
				(number "AK27")
			)
			(pin power_in line
				(at 27.94 -73.66 180)
				(length 7.62)
				(name "XGND")
				(number "AL26")
			)
			(pin power_in line
				(at 27.94 -76.2 180)
				(length 7.62)
				(name "XGND")
				(number "AM28")
			)
		)
		(symbol "MPC8641D_5_1"
			(text "eTSEC 1.2"
				(at -16.51 17.78 0)
			)
			(text "eTSEC 3.4"
				(at -16.51 -1.27 0)
			)
			(text "SERDES TCVR PWR"
				(at -8.89 -52.07 900)
			)
			(text "DDR SDRAM POWER 1"
				(at -6.35 60.96 900)
			)
			(text "I/O PWR"
				(at 2.54 12.7 0)
			)
			(text "SRDS1 PWR"
				(at 2.54 -41.91 900)
			)
			(text "SRDS2 PWR"
				(at 2.54 -83.82 900)
			)
			(text "DDR SDRAM POWER 2"
				(at 3.81 60.96 900)
			)
			(pin power_in line
				(at -30.48 99.06 0)
				(length 7.62)
				(name "D1_GVDD")
				(number "B11")
			)
			(pin power_in line
				(at -30.48 96.52 0)
				(length 7.62)
				(name "D1_GVDD")
				(number "B14")
			)
			(pin power_in line
				(at -30.48 93.98 0)
				(length 7.62)
				(name "D1_GVDD")
				(number "D10")
			)
			(pin power_in line
				(at -30.48 91.44 0)
				(length 7.62)
				(name "D1_GVDD")
				(number "D13")
			)
			(pin power_in line
				(at -30.48 88.9 0)
				(length 7.62)
				(name "D1_GVDD")
				(number "F9")
			)
			(pin power_in line
				(at -30.48 86.36 0)
				(length 7.62)
				(name "D1_GVDD")
				(number "F12")
			)
			(pin power_in line
				(at -30.48 83.82 0)
				(length 7.62)
				(name "D1_GVDD")
				(number "H8")
			)
			(pin power_in line
				(at -30.48 81.28 0)
				(length 7.62)
				(name "D1_GVDD")
				(number "H11")
			)
			(pin power_in line
				(at -30.48 78.74 0)
				(length 7.62)
				(name "D1_GVDD")
				(number "H14")
			)
			(pin power_in line
				(at -30.48 76.2 0)
				(length 7.62)
				(name "D1_GVDD")
				(number "K10")
			)
			(pin power_in line
				(at -30.48 73.66 0)
				(length 7.62)
				(name "D1_GVDD")
				(number "K13")
			)
			(pin power_in line
				(at -30.48 71.12 0)
				(length 7.62)
				(name "D1_GVDD")
				(number "L8")
			)
			(pin power_in line
				(at -30.48 68.58 0)
				(length 7.62)
				(name "D1_GVDD")
				(number "P8")
			)
			(pin power_in line
				(at -30.48 66.04 0)
				(length 7.62)
				(name "D1_GVDD")
				(number "R6")
			)
			(pin power_in line
				(at -30.48 63.5 0)
				(length 7.62)
				(name "D1_GVDD")
				(number "U8")
			)
			(pin power_in line
				(at -30.48 60.96 0)
				(length 7.62)
				(name "D1_GVDD")
				(number "V6")
			)
			(pin power_in line
				(at -30.48 58.42 0)
				(length 7.62)
				(name "D1_GVDD")
				(number "W10")
			)
			(pin power_in line
				(at -30.48 55.88 0)
				(length 7.62)
				(name "D1_GVDD")
				(number "Y8")
			)
			(pin power_in line
				(at -30.48 53.34 0)
				(length 7.62)
				(name "D1_GVDD")
				(number "AA6")
			)
			(pin power_in line
				(at -30.48 50.8 0)
				(length 7.62)
				(name "D1_GVDD")
				(number "AB10")
			)
			(pin power_in line
				(at -30.48 48.26 0)
				(length 7.62)
				(name "D1_GVDD")
				(number "AC8")
			)
			(pin power_in line
				(at -30.48 45.72 0)
				(length 7.62)
				(name "D1_GVDD")
				(number "AD12")
			)
			(pin power_in line
				(at -30.48 43.18 0)
				(length 7.62)
				(name "D1_GVDD")
				(number "AE10")
			)
			(pin power_in line
				(at -30.48 40.64 0)
				(length 7.62)
				(name "D1_GVDD")
				(number "AF8")
			)
			(pin power_in line
				(at -30.48 38.1 0)
				(length 7.62)
				(name "D1_GVDD")
				(number "AG12")
			)
			(pin power_in line
				(at -30.48 35.56 0)
				(length 7.62)
				(name "D1_GVDD")
				(number "AH10")
			)
			(pin power_in line
				(at -30.48 33.02 0)
				(length 7.62)
				(name "D1_GVDD")
				(number "AJ8")
			)
			(pin power_in line
				(at -30.48 30.48 0)
				(length 7.62)
				(name "D1_GVDD")
				(number "AJ14")
			)
			(pin power_in line
				(at -30.48 27.94 0)
				(length 7.62)
				(name "D1_GVDD")
				(number "AK12")
			)
			(pin power_in line
				(at -30.48 25.4 0)
				(length 7.62)
				(name "D1_GVDD")
				(number "AL10")
			)
			(pin power_in line
				(at -30.48 22.86 0)
				(length 7.62)
				(name "D1_GVDD")
				(number "AL16")
			)
			(pin power_in line
				(at -30.48 12.7 0)
				(length 7.62)
				(name "LVDD")
				(number "AC20")
			)
			(pin power_in line
				(at -30.48 10.16 0)
				(length 7.62)
				(name "LVDD")
				(number "AD23")
			)
			(pin power_in line
				(at -30.48 7.62 0)
				(length 7.62)
				(name "LVDD")
				(number "AH22")
			)
			(pin power_in line
				(at -30.48 -6.35 0)
				(length 7.62)
				(name "TVDD")
				(number "AC17")
			)
			(pin power_in line
				(at -30.48 -8.89 0)
				(length 7.62)
				(name "TVDD")
				(number "AG18")
			)
			(pin power_in line
				(at -30.48 -11.43 0)
				(length 7.62)
				(name "TVDD")
				(number "AK20")
			)
			(pin power_in line
				(at -30.48 -21.59 0)
				(length 7.62)
				(name "SVDD")
				(number "H31")
			)
			(pin power_in line
				(at -30.48 -24.13 0)
				(length 7.62)
				(name "SVDD")
				(number "J29")
			)
			(pin power_in line
				(at -30.48 -26.67 0)
				(length 7.62)
				(name "SVDD")
				(number "K28")
			)
			(pin power_in line
				(at -30.48 -29.21 0)
				(length 7.62)
				(name "SVDD")
				(number "K32")
			)
			(pin power_in line
				(at -30.48 -31.75 0)
				(length 7.62)
				(name "SVDD")
				(number "L30")
			)
			(pin power_in line
				(at -30.48 -34.29 0)
				(length 7.62)
				(name "SVDD")
				(number "M28")
			)
			(pin power_in line
				(at -30.48 -36.83 0)
				(length 7.62)
				(name "SVDD")
				(number "M31")
			)
			(pin power_in line
				(at -30.48 -39.37 0)
				(length 7.62)
				(name "SVDD")
				(number "N29")
			)
			(pin power_in line
				(at -30.48 -41.91 0)
				(length 7.62)
				(name "SVDD")
				(number "R30")
			)
			(pin power_in line
				(at -30.48 -44.45 0)
				(length 7.62)
				(name "SVDD")
				(number "T31")
			)
			(pin power_in line
				(at -30.48 -46.99 0)
				(length 7.62)
				(name "SVDD")
				(number "U29")
			)
			(pin power_in line
				(at -30.48 -49.53 0)
				(length 7.62)
				(name "SVDD")
				(number "V32")
			)
			(pin power_in line
				(at -30.48 -52.07 0)
				(length 7.62)
				(name "SVDD")
				(number "W30")
			)
			(pin power_in line
				(at -30.48 -54.61 0)
				(length 7.62)
				(name "SVDD")
				(number "Y31")
			)
			(pin power_in line
				(at -30.48 -57.15 0)
				(length 7.62)
				(name "SVDD")
				(number "AA29")
			)
			(pin power_in line
				(at -30.48 -59.69 0)
				(length 7.62)
				(name "SVDD")
				(number "AB32")
			)
			(pin power_in line
				(at -30.48 -62.23 0)
				(length 7.62)
				(name "SVDD")
				(number "AC30")
			)
			(pin power_in line
				(at -30.48 -64.77 0)
				(length 7.62)
				(name "SVDD")
				(number "AD31")
			)
			(pin power_in line
				(at -30.48 -67.31 0)
				(length 7.62)
				(name "SVDD")
				(number "AE29")
			)
			(pin power_in line
				(at -30.48 -69.85 0)
				(length 7.62)
				(name "SVDD")
				(number "AG30")
			)
			(pin power_in line
				(at -30.48 -72.39 0)
				(length 7.62)
				(name "SVDD")
				(number "AH31")
			)
			(pin power_in line
				(at -30.48 -74.93 0)
				(length 7.62)
				(name "SVDD")
				(number "AJ29")
			)
			(pin power_in line
				(at -30.48 -77.47 0)
				(length 7.62)
				(name "SVDD")
				(number "AK32")
			)
			(pin power_in line
				(at -30.48 -80.01 0)
				(length 7.62)
				(name "SVDD")
				(number "AL30")
			)
			(pin power_in line
				(at -30.48 -82.55 0)
				(length 7.62)
				(name "SVDD")
				(number "AM31")
			)
			(pin power_in line
				(at -30.48 -91.44 0)
				(length 7.62)
				(name "AVDD_PLAT")
				(number "B19")
			)
			(pin power_in line
				(at -30.48 -99.06 0)
				(length 7.62)
				(name "AVDD_LB")
				(number "A20")
			)
			(pin power_in line
				(at 27.94 99.06 180)
				(length 7.62)
				(name "D2_GVDD")
				(number "B2")
			)
			(pin power_in line
				(at 27.94 96.52 180)
				(length 7.62)
				(name "D2_GVDD")
				(number "B5")
			)
			(pin power_in line
				(at 27.94 93.98 180)
				(length 7.62)
				(name "D2_GVDD")
				(number "B8")
			)
			(pin power_in line
				(at 27.94 91.44 180)
				(length 7.62)
				(name "D2_GVDD")
				(number "D4")
			)
			(pin power_in line
				(at 27.94 88.9 180)
				(length 7.62)
				(name "D2_GVDD")
				(number "D7")
			)
			(pin power_in line
				(at 27.94 86.36 180)
				(length 7.62)
				(name "D2_GVDD")
				(number "E2")
			)
			(pin power_in line
				(at 27.94 83.82 180)
				(length 7.62)
				(name "D2_GVDD")
				(number "F6")
			)
			(pin power_in line
				(at 27.94 81.28 180)
				(length 7.62)
				(name "D2_GVDD")
				(number "G4")
			)
			(pin power_in line
				(at 27.94 78.74 180)
				(length 7.62)
				(name "D2_GVDD")
				(number "H2")
			)
			(pin power_in line
				(at 27.94 76.2 180)
				(length 7.62)
				(name "D2_GVDD")
				(number "J6")
			)
			(pin power_in line
				(at 27.94 73.66 180)
				(length 7.62)
				(name "D2_GVDD")
				(number "K4")
			)
			(pin power_in line
				(at 27.94 71.12 180)
				(length 7.62)
				(name "D2_GVDD")
				(number "L2")
			)
			(pin power_in line
				(at 27.94 68.58 180)
				(length 7.62)
				(name "D2_GVDD")
				(number "M6")
			)
			(pin power_in line
				(at 27.94 66.04 180)
				(length 7.62)
				(name "D2_GVDD")
				(number "N4")
			)
			(pin power_in line
				(at 27.94 63.5 180)
				(length 7.62)
				(name "D2_GVDD")
				(number "P2")
			)
			(pin power_in line
				(at 27.94 60.96 180)
				(length 7.62)
				(name "D2_GVDD")
				(number "T4")
			)
			(pin power_in line
				(at 27.94 58.42 180)
				(length 7.62)
				(name "D2_GVDD")
				(number "U2")
			)
			(pin power_in line
				(at 27.94 55.88 180)
				(length 7.62)
				(name "D2_GVDD")
				(number "W4")
			)
			(pin power_in line
				(at 27.94 53.34 180)
				(length 7.62)
				(name "D2_GVDD")
				(number "Y2")
			)
			(pin power_in line
				(at 27.94 50.8 180)
				(length 7.62)
				(name "D2_GVDD")
				(number "AB4")
			)
			(pin power_in line
				(at 27.94 48.26 180)
				(length 7.62)
				(name "D2_GVDD")
				(number "AC2")
			)
			(pin power_in line
				(at 27.94 45.72 180)
				(length 7.62)
				(name "D2_GVDD")
				(number "AD6")
			)
			(pin power_in line
				(at 27.94 43.18 180)
				(length 7.62)
				(name "D2_GVDD")
				(number "AE4")
			)
			(pin power_in line
				(at 27.94 40.64 180)
				(length 7.62)
				(name "D2_GVDD")
				(number "AF2")
			)
			(pin power_in line
				(at 27.94 38.1 180)
				(length 7.62)
				(name "D2_GVDD")
				(number "AG6")
			)
			(pin power_in line
				(at 27.94 35.56 180)
				(length 7.62)
				(name "D2_GVDD")
				(number "AH4")
			)
			(pin power_in line
				(at 27.94 33.02 180)
				(length 7.62)
				(name "D2_GVDD")
				(number "AJ2")
			)
			(pin power_in line
				(at 27.94 30.48 180)
				(length 7.62)
				(name "D2_GVDD")
				(number "AK6")
			)
			(pin power_in line
				(at 27.94 27.94 180)
				(length 7.62)
				(name "D2_GVDD")
				(number "AL4")
			)
			(pin power_in line
				(at 27.94 25.4 180)
				(length 7.62)
				(name "D2_GVDD")
				(number "AM2")
			)
			(pin power_in line
				(at 27.94 17.78 180)
				(length 7.62)
				(name "OVDD")
				(number "B22")
			)
			(pin power_in line
				(at 27.94 15.24 180)
				(length 7.62)
				(name "OVDD")
				(number "B25")
			)
			(pin power_in line
				(at 27.94 12.7 180)
				(length 7.62)
				(name "OVDD")
				(number "B28")
			)
			(pin power_in line
				(at 27.94 10.16 180)
				(length 7.62)
				(name "OVDD")
				(number "D17")
			)
			(pin power_in line
				(at 27.94 7.62 180)
				(length 7.62)
				(name "OVDD")
				(number "D24")
			)
			(pin power_in line
				(at 27.94 5.08 180)
				(length 7.62)
				(name "OVDD")
				(number "D27")
			)
			(pin power_in line
				(at 27.94 2.54 180)
				(length 7.62)
				(name "OVDD")
				(number "F19")
			)
			(pin power_in line
				(at 27.94 0 180)
				(length 7.62)
				(name "OVDD")
				(number "F22")
			)
			(pin power_in line
				(at 27.94 -2.54 180)
				(length 7.62)
				(name "OVDD")
				(number "F26")
			)
			(pin power_in line
				(at 27.94 -5.08 180)
				(length 7.62)
				(name "OVDD")
				(number "F29")
			)
			(pin power_in line
				(at 27.94 -7.62 180)
				(length 7.62)
				(name "OVDD")
				(number "G17")
			)
			(pin power_in line
				(at 27.94 -10.16 180)
				(length 7.62)
				(name "OVDD")
				(number "H21")
			)
			(pin power_in line
				(at 27.94 -12.7 180)
				(length 7.62)
				(name "OVDD")
				(number "H24")
			)
			(pin power_in line
				(at 27.94 -15.24 180)
				(length 7.62)
				(name "OVDD")
				(number "K19")
			)
			(pin power_in line
				(at 27.94 -17.78 180)
				(length 7.62)
				(name "OVDD")
				(number "K23")
			)
			(pin power_in line
				(at 27.94 -20.32 180)
				(length 7.62)
				(name "OVDD")
				(number "M21")
			)
			(pin power_in line
				(at 27.94 -22.86 180)
				(length 7.62)
				(name "OVDD")
				(number "AM30")
			)
			(pin power_in line
				(at 27.94 -30.48 180)
				(length 7.62)
				(name "XVDD_SRDS1")
				(number "K26")
			)
			(pin power_in line
				(at 27.94 -33.02 180)
				(length 7.62)
				(name "XVDD_SRDS1")
				(number "L24")
			)
			(pin power_in line
				(at 27.94 -35.56 180)
				(length 7.62)
				(name "XVDD_SRDS1")
				(number "M27")
			)
			(pin power_in line
				(at 27.94 -38.1 180)
				(length 7.62)
				(name "XVDD_SRDS1")
				(number "N25")
			)
			(pin power_in line
				(at 27.94 -40.64 180)
				(length 7.62)
				(name "XVDD_SRDS1")
				(number "P26")
			)
			(pin power_in line
				(at 27.94 -43.18 180)
				(length 7.62)
				(name "XVDD_SRDS1")
				(number "R24")
			)
			(pin power_in line
				(at 27.94 -45.72 180)
				(length 7.62)
				(name "XVDD_SRDS1")
				(number "R28")
			)
			(pin power_in line
				(at 27.94 -48.26 180)
				(length 7.62)
				(name "XVDD_SRDS1")
				(number "T27")
			)
			(pin power_in line
				(at 27.94 -50.8 180)
				(length 7.62)
				(name "XVDD_SRDS1")
				(number "U25")
			)
			(pin power_in line
				(at 27.94 -53.34 180)
				(length 7.62)
				(name "XVDD_SRDS1")
				(number "V26")
			)
			(pin power_in line
				(at 27.94 -58.42 180)
				(length 7.62)
				(name "AVDD_SRDS1")
				(number "P32")
			)
			(pin power_in line
				(at 27.94 -60.96 180)
				(length 7.62)
				(name "AGND_SRDS1")
				(number "P30")
			)
			(pin power_in line
				(at 27.94 -68.58 180)
				(length 7.62)
				(name "XVDD_SRDS2")
				(number "AA25")
			)
			(pin power_in line
				(at 27.94 -71.12 180)
				(length 7.62)
				(name "XVDD_SRDS2")
				(number "AB28")
			)
			(pin power_in line
				(at 27.94 -73.66 180)
				(length 7.62)
				(name "XVDD_SRDS2")
				(number "AC26")
			)
			(pin power_in line
				(at 27.94 -76.2 180)
				(length 7.62)
				(name "XVDD_SRDS2")
				(number "AD27")
			)
			(pin power_in line
				(at 27.94 -78.74 180)
				(length 7.62)
				(name "XVDD_SRDS2")
				(number "AE25")
			)
			(pin power_in line
				(at 27.94 -81.28 180)
				(length 7.62)
				(name "XVDD_SRDS2")
				(number "AF28")
			)
			(pin power_in line
				(at 27.94 -83.82 180)
				(length 7.62)
				(name "XVDD_SRDS2")
				(number "AH27")
			)
			(pin power_in line
				(at 27.94 -86.36 180)
				(length 7.62)
				(name "XVDD_SRDS2")
				(number "AK28")
			)
			(pin power_in line
				(at 27.94 -88.9 180)
				(length 7.62)
				(name "XVDD_SRDS2")
				(number "AM27")
			)
			(pin power_in line
				(at 27.94 -91.44 180)
				(length 7.62)
				(name "XVDD_SRDS2")
				(number "W24")
			)
			(pin power_in line
				(at 27.94 -93.98 180)
				(length 7.62)
				(name "XVDD_SRDS2")
				(number "Y27")
			)
			(pin power_in line
				(at 27.94 -99.06 180)
				(length 7.62)
				(name "AVDD_SRDS2")
				(number "AF32")
			)
			(pin power_in line
				(at 27.94 -101.6 180)
				(length 7.62)
				(name "AGND_SRDS2")
				(number "AF30")
			)
		)
		(symbol "MPC8641D_6_1"
			(text "GND"
				(at 0 17.78 0)
			)
			(pin power_in line
				(at -25.4 81.28 0)
				(length 7.62)
				(name "GND")
				(number "C3")
			)
			(pin power_in line
				(at -25.4 78.74 0)
				(length 7.62)
				(name "GND")
				(number "C6")
			)
			(pin power_in line
				(at -25.4 76.2 0)
				(length 7.62)
				(name "GND")
				(number "C9")
			)
			(pin power_in line
				(at -25.4 73.66 0)
				(length 7.62)
				(name "GND")
				(number "C12")
			)
			(pin power_in line
				(at -25.4 71.12 0)
				(length 7.62)
				(name "GND")
				(number "C15")
			)
			(pin power_in line
				(at -25.4 68.58 0)
				(length 7.62)
				(name "GND")
				(number "C23")
			)
			(pin power_in line
				(at -25.4 66.04 0)
				(length 7.62)
				(name "GND")
				(number "C26")
			)
			(pin power_in line
				(at -25.4 63.5 0)
				(length 7.62)
				(name "GND")
				(number "E5")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 7.62)
				(name "GND")
				(number "E8")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 7.62)
				(name "GND")
				(number "E11")
			)
			(pin power_in line
				(at -25.4 55.88 0)
				(length 7.62)
				(name "GND")
				(number "E14")
			)
			(pin power_in line
				(at -25.4 53.34 0)
				(length 7.62)
				(name "GND")
				(number "E18")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 7.62)
				(name "GND")
				(number "E25")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 7.62)
				(name "GND")
				(number "E28")
			)
			(pin power_in line
				(at -25.4 45.72 0)
				(length 7.62)
				(name "GND")
				(number "F3")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 7.62)
				(name "GND")
				(number "G7")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 7.62)
				(name "GND")
				(number "G10")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 7.62)
				(name "GND")
				(number "G13")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 7.62)
				(name "GND")
				(number "G20")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 7.62)
				(name "GND")
				(number "G23")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 7.62)
				(name "GND")
				(number "G27")
			)
			(pin power_in line
				(at -25.4 27.94 0)
				(length 7.62)
				(name "GND")
				(number "G30")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 7.62)
				(name "GND")
				(number "H5")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 7.62)
				(name "GND")
				(number "J3")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 7.62)
				(name "GND")
				(number "J9")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 7.62)
				(name "GND")
				(number "J12")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 7.62)
				(name "GND")
				(number "J15~")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 7.62)
				(name "GND")
				(number "J22")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 7.62)
				(name "GND")
				(number "J25")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 7.62)
				(name "GND")
				(number "K7")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 7.62)
				(name "GND")
				(number "L5")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 7.62)
				(name "GND")
				(number "L20")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 7.62)
				(name "GND")
				(number "M3")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 7.62)
				(name "GND")
				(number "M9")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 7.62)
				(name "GND")
				(number "M12")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 7.62)
				(name "GND")
				(number "N7")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 7.62)
				(name "GND")
				(number "N11")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 7.62)
				(name "GND")
				(number "N13")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 7.62)
				(name "GND")
				(number "N15")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 7.62)
				(name "GND")
				(number "N17")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 7.62)
				(name "GND")
				(number "N19")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 7.62)
				(name "GND")
				(number "N21")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 7.62)
				(name "GND")
				(number "N23")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 7.62)
				(name "GND")
				(number "P5")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 7.62)
				(name "GND")
				(number "P12")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 7.62)
				(name "GND")
				(number "P16")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 7.62)
				(name "GND")
				(number "P20")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 7.62)
				(name "GND")
				(number "P22")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 7.62)
				(name "GND")
				(number "R3")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 7.62)
				(name "GND")
				(number "R9")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 7.62)
				(name "GND")
				(number "R11")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 7.62)
				(name "GND")
				(number "R13")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 7.62)
				(name "GND")
				(number "R15")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 7.62)
				(name "GND")
				(number "R17")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 7.62)
				(name "GND")
				(number "R19")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 7.62)
				(name "GND")
				(number "R21")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 7.62)
				(name "GND")
				(number "R23")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 7.62)
				(name "GND")
				(number "T7")
			)
			(pin power_in line
				(at -25.4 -66.04 0)
				(length 7.62)
				(name "GND")
				(number "T12")
			)
			(pin power_in line
				(at -25.4 -68.58 0)
				(length 7.62)
				(name "GND")
				(number "T14")
			)
			(pin power_in line
				(at -25.4 -71.12 0)
				(length 7.62)
				(name "GND")
				(number "T16")
			)
			(pin power_in line
				(at -25.4 -73.66 0)
				(length 7.62)
				(name "GND")
				(number "T18")
			)
			(pin power_in line
				(at -25.4 -76.2 0)
				(length 7.62)
				(name "GND")
				(number "T20")
			)
			(pin power_in line
				(at -25.4 -78.74 0)
				(length 7.62)
				(name "GND")
				(number "T22")
			)
			(pin power_in line
				(at 25.4 81.28 180)
				(length 7.62)
				(name "GND")
				(number "U5")
			)
			(pin power_in line
				(at 25.4 78.74 180)
				(length 7.62)
				(name "GND")
				(number "U11")
			)
			(pin power_in line
				(at 25.4 76.2 180)
				(length 7.62)
				(name "GND")
				(number "U13")
			)
			(pin power_in line
				(at 25.4 73.66 180)
				(length 7.62)
				(name "GND")
				(number "U15")
			)
			(pin power_in line
				(at 25.4 71.12 180)
				(length 7.62)
				(name "GND")
				(number "U17")
			)
			(pin power_in line
				(at 25.4 68.58 180)
				(length 7.62)
				(name "GND")
				(number "U19")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 7.62)
				(name "GND")
				(number "U21")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 7.62)
				(name "GND")
				(number "U23")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 7.62)
				(name "GND")
				(number "V3")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 7.62)
				(name "GND")
				(number "V9")
			)
			(pin power_in line
				(at 25.4 55.88 180)
				(length 7.62)
				(name "GND")
				(number "V12")
			)
			(pin power_in line
				(at 25.4 53.34 180)
				(length 7.62)
				(name "GND")
				(number "V14")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 7.62)
				(name "GND")
				(number "V16")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 7.62)
				(name "GND")
				(number "V18")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 7.62)
				(name "GND")
				(number "V22")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 7.62)
				(name "GND")
				(number "W7")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 7.62)
				(name "GND")
				(number "W11")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 7.62)
				(name "GND")
				(number "W13")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 7.62)
				(name "GND")
				(number "W15")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 7.62)
				(name "GND")
				(number "W17")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 7.62)
				(name "GND")
				(number "W19")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 7.62)
				(name "GND")
				(number "W21")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 7.62)
				(name "GND")
				(number "W23")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 7.62)
				(name "GND")
				(number "Y5")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 7.62)
				(name "GND")
				(number "Y14")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 7.62)
				(name "GND")
				(number "Y16")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 7.62)
				(name "GND")
				(number "Y18")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 7.62)
				(name "GND")
				(number "Y20")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 7.62)
				(name "GND")
				(number "Y22")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 7.62)
				(name "GND")
				(number "AA3")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 7.62)
				(name "GND")
				(number "AA9")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 7.62)
				(name "GND")
				(number "AA13")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 7.62)
				(name "GND")
				(number "AA15")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 7.62)
				(name "GND")
				(number "AA17")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 7.62)
				(name "GND")
				(number "AA19")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 7.62)
				(name "GND")
				(number "AA21")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 7.62)
				(name "GND")
				(number "AA23")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 7.62)
				(name "GND")
				(number "AB7")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 7.62)
				(name "GND")
				(number "AB24")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 7.62)
				(name "GND")
				(number "AC5")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 7.62)
				(name "GND")
				(number "AC11")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 7.62)
				(name "GND")
				(number "AD3")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 7.62)
				(name "GND")
				(number "AD9")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 7.62)
				(name "GND")
				(number "AD15")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 7.62)
				(name "GND")
				(number "AE7")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 7.62)
				(name "GND")
				(number "AE13")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 7.62)
				(name "GND")
				(number "AE18")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 7.62)
				(name "GND")
				(number "AF5")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 7.62)
				(name "GND")
				(number "AF11")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 7.62)
				(name "GND")
				(number "AF21")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 7.62)
				(name "GND")
				(number "AF24")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 7.62)
				(name "GND")
				(number "AG3")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 7.62)
				(name "GND")
				(number "AG9")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 7.62)
				(name "GND")
				(number "AH7")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 7.62)
				(name "GND")
				(number "AH13")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 7.62)
				(name "GND")
				(number "AJ5")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 7.62)
				(name "GND")
				(number "AJ11")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 7.62)
				(name "GND")
				(number "AK3")
			)
			(pin power_in line
				(at 25.4 -66.04 180)
				(length 7.62)
				(name "GND")
				(number "AK9")
			)
			(pin power_in line
				(at 25.4 -68.58 180)
				(length 7.62)
				(name "GND")
				(number "AK15")
			)
			(pin power_in line
				(at 25.4 -71.12 180)
				(length 7.62)
				(name "GND")
				(number "AK19")
			)
			(pin power_in line
				(at 25.4 -73.66 180)
				(length 7.62)
				(name "GND")
				(number "AK23")
			)
			(pin power_in line
				(at 25.4 -76.2 180)
				(length 7.62)
				(name "GND")
				(number "AL7")
			)
			(pin power_in line
				(at 25.4 -78.74 180)
				(length 7.62)
				(name "GND")
				(number "AL13")
			)
			(pin power_in line
				(at 25.4 -83.82 180)
				(length 7.62)
				(name "GNDGND/SENSEVSS_PLAT")
				(number "P18")
			)
		)
		(symbol "MPC8641D_7_1"
			(text "DDR Memory Inter 1 "
				(at 2.54 24.13 0)
			)
			(pin bidirectional line
				(at -33.02 104.14 0)
				(length 7.62)
				(name "D1_MDQ0")
				(number "D15")
			)
			(pin bidirectional line
				(at -33.02 101.6 0)
				(length 7.62)
				(name "D1_MDQ1")
				(number "A14")
			)
			(pin bidirectional line
				(at -33.02 99.06 0)
				(length 7.62)
				(name "D1_MDQ2")
				(number "B12")
			)
			(pin bidirectional line
				(at -33.02 96.52 0)
				(length 7.62)
				(name "D1_MDQ3")
				(number "D12")
			)
			(pin bidirectional line
				(at -33.02 93.98 0)
				(length 7.62)
				(name "D1_MDQ4")
				(number "A15")
			)
			(pin bidirectional line
				(at -33.02 91.44 0)
				(length 7.62)
				(name "D1_MDQ5")
				(number "B15")
			)
			(pin bidirectional line
				(at -33.02 88.9 0)
				(length 7.62)
				(name "D1_MDQ6")
				(number "B13")
			)
			(pin bidirectional line
				(at -33.02 86.36 0)
				(length 7.62)
				(name "D1_MDQ7")
				(number "C13")
			)
			(pin bidirectional line
				(at -33.02 83.82 0)
				(length 7.62)
				(name "D1_MDQ8")
				(number "C11")
			)
			(pin bidirectional line
				(at -33.02 81.28 0)
				(length 7.62)
				(name "D1_MDQ9")
				(number "D11")
			)
			(pin bidirectional line
				(at -33.02 78.74 0)
				(length 7.62)
				(name "D1_MDQ10")
				(number "D9")
			)
			(pin bidirectional line
				(at -33.02 76.2 0)
				(length 7.62)
				(name "D1_MDQ11")
				(number "A8")
			)
			(pin bidirectional line
				(at -33.02 73.66 0)
				(length 7.62)
				(name "D1_MDQ12")
				(number "A12")
			)
			(pin bidirectional line
				(at -33.02 71.12 0)
				(length 7.62)
				(name "D1_MDQ13")
				(number "A11")
			)
			(pin bidirectional line
				(at -33.02 68.58 0)
				(length 7.62)
				(name "D1_MDQ14")
				(number "A9")
			)
			(pin bidirectional line
				(at -33.02 66.04 0)
				(length 7.62)
				(name "D1_MDQ15")
				(number "B9")
			)
			(pin bidirectional line
				(at -33.02 63.5 0)
				(length 7.62)
				(name "D1_MDQ16")
				(number "F11")
			)
			(pin bidirectional line
				(at -33.02 60.96 0)
				(length 7.62)
				(name "D1_MDQ17")
				(number "G12")
			)
			(pin bidirectional line
				(at -33.02 58.42 0)
				(length 7.62)
				(name "D1_MDQ18")
				(number "K11")
			)
			(pin bidirectional line
				(at -33.02 55.88 0)
				(length 7.62)
				(name "D1_MDQ19")
				(number "K12")
			)
			(pin bidirectional line
				(at -33.02 53.34 0)
				(length 7.62)
				(name "D1_MDQ20")
				(number "E10")
			)
			(pin bidirectional line
				(at -33.02 50.8 0)
				(length 7.62)
				(name "D1_MDQ21")
				(number "E9")
			)
			(pin bidirectional line
				(at -33.02 48.26 0)
				(length 7.62)
				(name "D1_MDQ22")
				(number "J11")
			)
			(pin bidirectional line
				(at -33.02 45.72 0)
				(length 7.62)
				(name "D1_MDQ23")
				(number "J10")
			)
			(pin bidirectional line
				(at -33.02 43.18 0)
				(length 7.62)
				(name "D1_MDQ24")
				(number "G8")
			)
			(pin bidirectional line
				(at -33.02 40.64 0)
				(length 7.62)
				(name "D1_MDQ25")
				(number "H10")
			)
			(pin bidirectional line
				(at -33.02 38.1 0)
				(length 7.62)
				(name "D1_MDQ26")
				(number "L9")
			)
			(pin bidirectional line
				(at -33.02 35.56 0)
				(length 7.62)
				(name "D1_MDQ27")
				(number "L7")
			)
			(pin bidirectional line
				(at -33.02 33.02 0)
				(length 7.62)
				(name "D1_MDQ28")
				(number "F10")
			)
			(pin bidirectional line
				(at -33.02 30.48 0)
				(length 7.62)
				(name "D1_MDQ29")
				(number "G9")
			)
			(pin bidirectional line
				(at -33.02 27.94 0)
				(length 7.62)
				(name "D1_MDQ30")
				(number "K9")
			)
			(pin bidirectional line
				(at -33.02 25.4 0)
				(length 7.62)
				(name "D1_MDQ31")
				(number "K8")
			)
			(pin bidirectional line
				(at -33.02 22.86 0)
				(length 7.62)
				(name "D1_MDQ32")
				(number "AC6")
			)
			(pin bidirectional line
				(at -33.02 20.32 0)
				(length 7.62)
				(name "D1_MDQ33")
				(number "AC7")
			)
			(pin bidirectional line
				(at -33.02 17.78 0)
				(length 7.62)
				(name "D1_MDQ34")
				(number "AG8")
			)
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 7.62)
				(name "D1_MDQ35")
				(number "AH9")
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 7.62)
				(name "D1_MDQ36")
				(number "AB6")
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 7.62)
				(name "D1_MDQ37")
				(number "AB8")
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 7.62)
				(name "D1_MDQ38")
				(number "AE9")
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 7.62)
				(name "D1_MDQ39")
				(number "AF9")
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 7.62)
				(name "D1_MDQ40")
				(number "AL8")
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 7.62)
				(name "D1_MDQ41")
				(number "AM8")
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 7.62)
				(name "D1_MDQ42")
				(number "AM10")
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 7.62)
				(name "D1_MDQ43")
				(number "AK11")
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 7.62)
				(name "D1_MDQ44")
				(number "AH8")
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 7.62)
				(name "D1_MDQ45")
				(number "AK8")
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 7.62)
				(name "D1_MDQ46")
				(number "AJ10")
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 7.62)
				(name "D1_MDQ47")
				(number "AK10")
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 7.62)
				(name "D1_MDQ48")
				(number "AL12")
			)
			(pin bidirectional line
				(at -33.02 -20.32 0)
				(length 7.62)
				(name "D1_MDQ49")
				(number "AJ12")
			)
			(pin bidirectional line
				(at -33.02 -22.86 0)
				(length 7.62)
				(name "D1_MDQ50")
				(number "AL14")
			)
			(pin bidirectional line
				(at -33.02 -25.4 0)
				(length 7.62)
				(name "D1_MDQ51")
				(number "AM14")
			)
			(pin bidirectional line
				(at -33.02 -27.94 0)
				(length 7.62)
				(name "D1_MDQ52")
				(number "AL11")
			)
			(pin bidirectional line
				(at -33.02 -30.48 0)
				(length 7.62)
				(name "D1_MDQ53")
				(number "AM11")
			)
			(pin bidirectional line
				(at -33.02 -33.02 0)
				(length 7.62)
				(name "D1_MDQ54")
				(number "AM13")
			)
			(pin bidirectional line
				(at -33.02 -35.56 0)
				(length 7.62)
				(name "D1_MDQ55")
				(number "AK14")
			)
			(pin bidirectional line
				(at -33.02 -38.1 0)
				(length 7.62)
				(name "D1_MDQ56")
				(number "AM15")
			)
			(pin bidirectional line
				(at -33.02 -40.64 0)
				(length 7.62)
				(name "D1_MDQ57")
				(number "AJ16")
			)
			(pin bidirectional line
				(at -33.02 -43.18 0)
				(length 7.62)
				(name "D1_MDQ58")
				(number "AK18")
			)
			(pin bidirectional line
				(at -33.02 -45.72 0)
				(length 7.62)
				(name "D1_MDQ59")
				(number "AL18")
			)
			(pin bidirectional line
				(at -33.02 -48.26 0)
				(length 7.62)
				(name "D1_MDQ60")
				(number "AJ15")
			)
			(pin bidirectional line
				(at -33.02 -50.8 0)
				(length 7.62)
				(name "D1_MDQ61")
				(number "AL15")
			)
			(pin bidirectional line
				(at -33.02 -53.34 0)
				(length 7.62)
				(name "D1_MDQ62")
				(number "AL17")
			)
			(pin bidirectional line
				(at -33.02 -55.88 0)
				(length 7.62)
				(name "D1_MDQ63")
				(number "AM17")
			)
			(pin bidirectional line
				(at -33.02 -60.96 0)
				(length 7.62)
				(name "D1_MECC0")
				(number "M8")
			)
			(pin bidirectional line
				(at -33.02 -63.5 0)
				(length 7.62)
				(name "D1_MECC1")
				(number "M7")
			)
			(pin bidirectional line
				(at -33.02 -66.04 0)
				(length 7.62)
				(name "D1_MECC2")
				(number "R8")
			)
			(pin bidirectional line
				(at -33.02 -68.58 0)
				(length 7.62)
				(name "D1_MECC3")
				(number "T10")
			)
			(pin bidirectional line
				(at -33.02 -71.12 0)
				(length 7.62)
				(name "D1_MECC4")
				(number "L11")
			)
			(pin bidirectional line
				(at -33.02 -73.66 0)
				(length 7.62)
				(name "D1_MECC5")
				(number "L10")
			)
			(pin bidirectional line
				(at -33.02 -76.2 0)
				(length 7.62)
				(name "D1_MECC6")
				(number "P9")
			)
			(pin bidirectional line
				(at -33.02 -78.74 0)
				(length 7.62)
				(name "D1_MECC7")
				(number "R10")
			)
			(pin bidirectional line
				(at -33.02 -83.82 0)
				(length 7.62)
				(name "D1_MDQS0")
				(number "A13")
			)
			(pin bidirectional line
				(at -33.02 -86.36 0)
				(length 7.62)
				(name "D1_MDQS1")
				(number "C10")
			)
			(pin bidirectional line
				(at -33.02 -88.9 0)
				(length 7.62)
				(name "D1_MDQS2")
				(number "H12")
			)
			(pin bidirectional line
				(at -33.02 -91.44 0)
				(length 7.62)
				(name "D1_MDQS3")
				(number "J7")
			)
			(pin bidirectional line
				(at -33.02 -93.98 0)
				(length 7.62)
				(name "D1_MDQS4")
				(number "AE8")
			)
			(pin bidirectional line
				(at -33.02 -96.52 0)
				(length 7.62)
				(name "D1_MDQS5")
				(number "AM9")
			)
			(pin bidirectional line
				(at -33.02 -99.06 0)
				(length 7.62)
				(name "D1_MDQS6")
				(number "AK13")
			)
			(pin bidirectional line
				(at -33.02 -101.6 0)
				(length 7.62)
				(name "D1_MDQS7")
				(number "AK17")
			)
			(pin bidirectional line
				(at -33.02 -104.14 0)
				(length 7.62)
				(name "D1_MDQS8")
				(number "N9")
			)
			(pin output line
				(at 33.02 104.14 180)
				(length 7.62)
				(name "D1_MDM0")
				(number "C14")
			)
			(pin output line
				(at 33.02 101.6 180)
				(length 7.62)
				(name "D1_MDM1")
				(number "A10")
			)
			(pin output line
				(at 33.02 99.06 180)
				(length 7.62)
				(name "D1_MDM2")
				(number "G11")
			)
			(pin output line
				(at 33.02 96.52 180)
				(length 7.62)
				(name "D1_MDM3")
				(number "H9")
			)
			(pin output line
				(at 33.02 93.98 180)
				(length 7.62)
				(name "D1_MDM4")
				(number "AD7")
			)
			(pin output line
				(at 33.02 91.44 180)
				(length 7.62)
				(name "D1_MDM5")
				(number "AJ9")
			)
			(pin output line
				(at 33.02 88.9 180)
				(length 7.62)
				(name "D1_MDM6")
				(number "AM12")
			)
			(pin output line
				(at 33.02 86.36 180)
				(length 7.62)
				(name "D1_MDM7")
				(number "AK16")
			)
			(pin output line
				(at 33.02 83.82 180)
				(length 7.62)
				(name "D1_MDM8")
				(number "N10")
			)
			(pin output line
				(at 33.02 77.47 180)
				(length 7.62)
				(name "D1_MBA0")
				(number "AA8")
			)
			(pin output line
				(at 33.02 74.93 180)
				(length 7.62)
				(name "D1_MBA1")
				(number "AA10")
			)
			(pin output line
				(at 33.02 72.39 180)
				(length 7.62)
				(name "D1_MBA2")
				(number "T9")
			)
			(pin output line
				(at 33.02 66.04 180)
				(length 7.62)
				(name "D1_MA0")
				(number "Y10")
			)
			(pin output line
				(at 33.02 63.5 180)
				(length 7.62)
				(name "D1_MA1")
				(number "W8")
			)
			(pin output line
				(at 33.02 60.96 180)
				(length 7.62)
				(name "D1_MA2")
				(number "W9")
			)
			(pin output line
				(at 33.02 58.42 180)
				(length 7.62)
				(name "D1_MA3")
				(number "V7")
			)
			(pin output line
				(at 33.02 55.88 180)
				(length 7.62)
				(name "D1_MA4")
				(number "V8")
			)
			(pin output line
				(at 33.02 53.34 180)
				(length 7.62)
				(name "D1_MA5")
				(number "U6")
			)
			(pin output line
				(at 33.02 50.8 180)
				(length 7.62)
				(name "D1_MA6")
				(number "V10")
			)
			(pin output line
				(at 33.02 48.26 180)
				(length 7.62)
				(name "D1_MA7")
				(number "U9")
			)
			(pin output line
				(at 33.02 45.72 180)
				(length 7.62)
				(name "D1_MA8")
				(number "U7")
			)
			(pin output line
				(at 33.02 43.18 180)
				(length 7.62)
				(name "D1_MA9")
				(number "U10")
			)
			(pin output line
				(at 33.02 40.64 180)
				(length 7.62)
				(name "D1_MA10")
				(number "Y9")
			)
			(pin output line
				(at 33.02 38.1 180)
				(length 7.62)
				(name "D1_MA11")
				(number "T6")
			)
			(pin output line
				(at 33.02 35.56 180)
				(length 7.62)
				(name "D1_MA12")
				(number "T8")
			)
			(pin output line
				(at 33.02 33.02 180)
				(length 7.62)
				(name "D1_MA13")
				(number "AE12")
			)
			(pin output line
				(at 33.02 30.48 180)
				(length 7.62)
				(name "D1_MA14")
				(number "R7")
			)
			(pin output line
				(at 33.02 27.94 180)
				(length 7.62)
				(name "D1_MA15")
				(number "P6")
			)
			(pin output line
				(at 33.02 21.59 180)
				(length 7.62)
				(name "/D1_MWE")
				(number "AB11")
			)
			(pin output line
				(at 33.02 19.05 180)
				(length 7.62)
				(name "/D1_MRAS")
				(number "AB12")
			)
			(pin output line
				(at 33.02 16.51 180)
				(length 7.62)
				(name "/D1_MCAS")
				(number "AC10")
			)
			(pin output line
				(at 33.02 10.16 180)
				(length 7.62)
				(name "/D1_MCS0")
				(number "AB9")
			)
			(pin output line
				(at 33.02 7.62 180)
				(length 7.62)
				(name "/D1_MCS1")
				(number "AD10")
			)
			(pin output line
				(at 33.02 5.08 180)
				(length 7.62)
				(name "/D1_MCS2")
				(number "AC12")
			)
			(pin output line
				(at 33.02 2.54 180)
				(length 7.62)
				(name "/D1_MCS3")
				(number "AD11")
			)
			(pin output line
				(at 33.02 -3.81 180)
				(length 7.62)
				(name "D1_MCKE0")
				(number "P7")
			)
			(pin output line
				(at 33.02 -6.35 180)
				(length 7.62)
				(name "D1_MCKE1")
				(number "M10")
			)
			(pin output line
				(at 33.02 -8.89 180)
				(length 7.62)
				(name "D1_MCKE2")
				(number "N8")
			)
			(pin output line
				(at 33.02 -11.43 180)
				(length 7.62)
				(name "D1_MCKE3")
				(number "M11")
			)
			(pin output line
				(at 33.02 -17.78 180)
				(length 7.62)
				(name "D1_MCK0")
				(number "W6")
			)
			(pin output line
				(at 33.02 -20.32 180)
				(length 7.62)
				(name "D1_MCK1")
				(number "E13")
			)
			(pin output line
				(at 33.02 -22.86 180)
				(length 7.62)
				(name "D1_MCK2")
				(number "AH11")
			)
			(pin output line
				(at 33.02 -25.4 180)
				(length 7.62)
				(name "D1_MCK3")
				(number "Y7")
			)
			(pin output line
				(at 33.02 -27.94 180)
				(length 7.62)
				(name "D1_MCK4")
				(number "F14")
			)
			(pin output line
				(at 33.02 -30.48 180)
				(length 7.62)
				(name "D1_MCK5")
				(number "AG10")
			)
			(pin output line
				(at 33.02 -36.83 180)
				(length 7.62)
				(name "/D1_MCK0")
				(number "Y6")
			)
			(pin output line
				(at 33.02 -39.37 180)
				(length 7.62)
				(name "/D1_MCK1")
				(number "E12")
			)
			(pin output line
				(at 33.02 -41.91 180)
				(length 7.62)
				(name "/D1_MCK2")
				(number "AH12")
			)
			(pin output line
				(at 33.02 -44.45 180)
				(length 7.62)
				(name "/D1_MCK3")
				(number "AA7")
			)
			(pin output line
				(at 33.02 -46.99 180)
				(length 7.62)
				(name "/D1_MCK4")
				(number "F13")
			)
			(pin output line
				(at 33.02 -49.53 180)
				(length 7.62)
				(name "/D1_MCK5")
				(number "AG11")
			)
			(pin output line
				(at 33.02 -55.88 180)
				(length 7.62)
				(name "D1_MODT0")
				(number "AC9")
			)
			(pin output line
				(at 33.02 -58.42 180)
				(length 7.62)
				(name "D1_MODT1")
				(number "AF12")
			)
			(pin output line
				(at 33.02 -60.96 180)
				(length 7.62)
				(name "D1_MODT2")
				(number "AE11")
			)
			(pin output line
				(at 33.02 -63.5 180)
				(length 7.62)
				(name "D1_MODT3")
				(number "AF10")
			)
			(pin output line
				(at 33.02 -68.58 180)
				(length 7.62)
				(name "D1_MVREF")
				(number "AM18")
			)
			(pin bidirectional line
				(at 33.02 -73.66 180)
				(length 7.62)
				(name "/D1_MDQS0")
				(number "D14")
			)
			(pin bidirectional line
				(at 33.02 -76.2 180)
				(length 7.62)
				(name "/D1_MDQS1")
				(number "B10")
			)
			(pin bidirectional line
				(at 33.02 -78.74 180)
				(length 7.62)
				(name "/D1_MDQS2")
				(number "H13")
			)
			(pin bidirectional line
				(at 33.02 -81.28 180)
				(length 7.62)
				(name "/D1_MDQS3")
				(number "J8")
			)
			(pin bidirectional line
				(at 33.02 -83.82 180)
				(length 7.62)
				(name "/D1_MDQS4")
				(number "AD8")
			)
			(pin bidirectional line
				(at 33.02 -86.36 180)
				(length 7.62)
				(name "/D1_MDQS5")
				(number "AL9")
			)
			(pin bidirectional line
				(at 33.02 -88.9 180)
				(length 7.62)
				(name "/D1_MDQS6")
				(number "AJ13")
			)
			(pin bidirectional line
				(at 33.02 -91.44 180)
				(length 7.62)
				(name "/D1_MDQS7")
				(number "AM16")
			)
			(pin bidirectional line
				(at 33.02 -93.98 180)
				(length 7.62)
				(name "/D1_MDQS8")
				(number "P10")
			)
			(pin bidirectional line
				(at 33.02 -100.33 180)
				(length 7.62)
				(name "D1_MDIC0")
				(number "E15")
			)
			(pin bidirectional line
				(at 33.02 -102.87 180)
				(length 7.62)
				(name "D1_MDIC1")
				(number "G14")
			)
		)
		(embedded_fonts no)
	)
)
