(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "AD8561"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "AD8561"
			(at 3.81 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ad8561.pdf"
			(at 0 0 0)
		)
		(property "Description" "Ultrafast 7 ns Single Supply Comparator, DIP-8/SOIC-8/TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "cmp complementary push-pull"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* TSSOP*4.4x3mm*P0.65mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "AD8561_0_1")
		(symbol "AD8561_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "3")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 5.08)
				(name "GND")
				(number "6")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 6.35)
				(name "LATCH")
				(number "5")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~{Q}")
				(number "8")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "Q")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADCMP350"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.175 5.08 0)
		)
		(property "Value" "ADCMP350"
			(at 3.175 -5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Analog_KS-4"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADCMP350_354_356.pdf"
			(at 3.81 5.08 0)
		)
		(property "Description" "Single-input comparator, internal 0.6V reference, Active-Low Open-Drain output, KS-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "cmp collector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Analog*KS?4*"
			(at 0 0 0)
		)
		(symbol "ADCMP350_0_1")
		(symbol "ADCMP350_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 3.81)
				(name "VCC")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "2")
			)
			(pin open_collector line
				(at 12.7 0 180)
				(length 5.08)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADCMP356"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.175 5.08 0)
		)
		(property "Value" "ADCMP356"
			(at 3.175 -5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Analog_KS-4"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADCMP350_354_356.pdf"
			(at 3.81 5.08 0)
		)
		(property "Description" "Single-input comparator, internal 0.6V reference, Active-High Push-Pull output, KS-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "cmp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Analog*KS?4*"
			(at 0 0 0)
		)
		(symbol "ADCMP356_0_1")
		(symbol "ADCMP356_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 3.81)
				(name "VCC")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM2901"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "LM2901"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at -1.27 2.54 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/lm2901.pdf"
			(at 1.27 5.08 0)
		)
		(property "Description" "Quad Differential Comparators, DIP-14/SOIC-14/TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "cmp open collector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* DIP*W7.62mm* TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LM2901_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(symbol "LM2901_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "7")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "6")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "LM2901_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "11")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "10")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "13")
			)
		)
		(symbol "LM2901_4_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "9")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "8")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(symbol "LM2901_5_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM2903"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "LM2903"
			(at 6.35 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm393.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Power, Low-Offset Voltage, Dual Comparators, DIP-8/SOIC-8/SOP-8/TSSOP-8/VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "cmp open collector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* SOP*5.28x5.23mm*P1.27mm* VSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LM2903_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "LM2903_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "6")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "LM2903_3_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM311"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "LM311"
			(at 3.81 3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/lm311.pdf"
			(at 0 0 0)
		)
		(property "Description" "Voltage Comparator, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "cmp open collector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "LM311_0_1")
		(symbol "LM311_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "3")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "BAL")
				(number "5")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 5.08)
				(name "GND")
				(number "1")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 6.35)
				(name "STRB")
				(number "6")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM319"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "LM319"
			(at 0 3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm319-n.pdf"
			(at 0 0 0)
		)
		(property "Description" "High Speed Dual Comparator, DIP-14/SOIC-14"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "cmp open collector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "LM319_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "5")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at 0 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 5.08)
				(name "GND")
				(number "3")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "12")
			)
		)
		(symbol "LM319_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "9")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "10")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin no_connect line
				(at 0 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "LM319_3_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "11")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM319H"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "LM319H"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-100-10"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm319-n.pdf"
			(at 0 0 0)
		)
		(property "Description" "High Speed Dual Comparator, TO-100-10"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "cmp open collector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?100*"
			(at 0 0 0)
		)
		(symbol "LM319H_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 5.08)
				(name "GND")
				(number "2")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "LM319H_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "8")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "9")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(symbol "LM319H_3_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "10")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM339"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "LM339"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at -1.27 2.54 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/lm139.pdf"
			(at 1.27 5.08 0)
		)
		(property "Description" "Quad Differential Comparators, SOIC-14/TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "cmp open collector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LM339_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(symbol "LM339_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "7")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "6")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "LM339_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "11")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "10")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "13")
			)
		)
		(symbol "LM339_4_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "9")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "8")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(symbol "LM339_5_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM397"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 5.08 0)
		)
		(property "Value" "LM397"
			(at 3.81 -5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -15.24 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm397.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Single General-Purpose Voltage Comparator with Open-Collector Output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single comparator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "LM397_0_1")
		(symbol "LM397_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "1")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "2")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LMH7324"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.905 5.715 0)
		)
		(property "Value" "LMH7324"
			(at 4.445 -5.08 0)
		)
		(property "Footprint" "Package_DFN_QFN:WQFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at -1.27 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmh7324.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad 700 ps High Speed Comparator with RSPECL Outputs, WQFN-32"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "cmp push-pull complementary"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WQFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LMH7324_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "30")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "31")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "VCCI")
				(number "32")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "VEE")
				(number "29")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "VEE")
				(number "4")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 5.08)
				(name "VCCO")
				(number "1")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "Q")
				(number "3")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~{Q}")
				(number "2")
			)
		)
		(symbol "LMH7324_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "11")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "10")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "VCCI")
				(number "9")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "VEE")
				(number "12")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "VEE")
				(number "5")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 5.08)
				(name "VCCO")
				(number "8")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "Q")
				(number "6")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~{Q}")
				(number "7")
			)
		)
		(symbol "LMH7324_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "14")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "15")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "VCCI")
				(number "16")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "VEE")
				(number "13")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "VEE")
				(number "20")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 5.08)
				(name "VCCO")
				(number "17")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "Q")
				(number "19")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~{Q}")
				(number "18")
			)
		)
		(symbol "LMH7324_4_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "27")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "26")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "VCCI")
				(number "25")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "VEE")
				(number "21")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "VEE")
				(number "28")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 5.08)
				(name "VCCO")
				(number "24")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "Q")
				(number "22")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~{Q}")
				(number "23")
			)
		)
		(symbol "LMH7324_5_1"
			(pin power_in line
				(at 0 -2.54 90)
				(length 2.54)
				(name "VEE/EP")
				(number "33")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LMV331"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 5.08 0)
		)
		(property "Value" "LMV331"
			(at 3.81 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 2.54 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmv331.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Single General-Purpose Low-Voltage Comparator, SOT-23-5/SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single comparator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* *SC?70*"
			(at 0 0 0)
		)
		(symbol "LMV331_0_1")
		(symbol "LMV331_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "3")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "2")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LMV393"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "LMV393"
			(at 6.35 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmv331.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual General-Purpose Low-Voltage Comparator, SOIC-8/TSSOP-8/VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "cmp open collector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* TSSOP*4.4x3mm*P0.65mm* VSSOP*3x3mm*P0.65mm* VSSOP*2.3x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LMV393_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "LMV393_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "6")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "LMV393_3_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LMV7271"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 5.08 0)
		)
		(property "Value" "LMV7271"
			(at 3.81 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 2.54 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmv7271.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Single, 1.8V Low Power, Rail-to-Rail Input, Push-Pull Output Comparator, SOT-23-5/SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "cmp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* *SC?70*"
			(at 0 0 0)
		)
		(symbol "LMV7271_0_1")
		(symbol "LMV7271_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "3")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LMV7272"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 6.35 0)
		)
		(property "Value" "LMV7272"
			(at 3.81 3.81 0)
		)
		(property "Footprint" "Package_BGA:Texas_DSBGA-8_1.5195x1.5195mm_Layout3x3_P0.5mm"
			(at -1.27 3.81 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmv7272.pdf"
			(at 1.27 6.35 0)
		)
		(property "Description" "Dual, 1.8V Low Power, Rail-to-Rail Input, Push-Pull Output Comparator, DSBGA-8"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "cmp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DSBGA*1.5195x1.5195*Layout3x3*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LMV7272_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "C1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "B1")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "A1")
			)
		)
		(symbol "LMV7272_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "C3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "B3")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "A3")
			)
		)
		(symbol "LMV7272_3_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "A2")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "C2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1016"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "LT1016"
			(at 3.81 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/lt1016.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single UltraFast Precision 10ns Comparator, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "cmp push-pull complementary latch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "LT1016_0_1")
		(symbol "LT1016_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "3")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 5.08)
				(name "GND")
				(number "6")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 6.35)
				(name "LATCH")
				(number "5")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~{Q}")
				(number "8")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "Q")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1711xMS8"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 7.62 0)
		)
		(property "Value" "LT1711xMS8"
			(at 8.89 5.08 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/171112f.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single ultrafast 4.5 ns rail-to-rail comparator, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "cmp latch push-pull complementary"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LT1711xMS8_0_1")
		(symbol "LT1711xMS8_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "3")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 5.08)
				(name "GND")
				(number "6")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 6.35)
				(name "LATCH")
				(number "5")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~{Q}")
				(number "8")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "Q")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC6752xMS8-2"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 -5.08 0)
		)
		(property "Value" "LTC6752xMS8-2"
			(at 3.81 -7.62 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 -9.525 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/6752fc.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single 280Mhz 2.9ns Comparator, Rail-to-Rail Inputs, CMOS Output, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single comparator high speed cmos"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LTC6752xMS8-2_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "3")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "VEE")
				(number "6")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 5.08)
				(name "VDD")
				(number "8")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "~{LE}")
				(number "5")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 6.35)
				(name "~{SHDN}")
				(number "4")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC6752xS5"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 -5.08 0)
		)
		(property "Value" "LTC6752xS5"
			(at 3.81 -7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/6752fc.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Single 280Mhz 2.9ns Comparator, Rail-to-Rail Inputs, CMOS Output, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single comparator high speed cmos"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23?5*"
			(at 0 0 0)
		)
		(symbol "LTC6752xS5_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "VEE")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC6752xSC6-1"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 -5.08 0)
		)
		(property "Value" "LTC6752xSC6-1"
			(at 3.81 -7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 -9.525 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/6752fc.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single 280Mhz 2.9ns Comparator, Rail-to-Rail Inputs, CMOS Output, SC-70"
			(at 0 0 0)
		)
		(property "ki_keywords" "single comparator high speed cmos"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
		(symbol "LTC6752xSC6-1_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "VCC")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "VEE")
				(number "2")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "~{LE}")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC6752xSC6-4"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 -5.08 0)
		)
		(property "Value" "LTC6752xSC6-4"
			(at 3.81 -7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 -9.525 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/6752fc.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single 280Mhz 2.9ns Comparator, Rail-to-Rail Inputs, CMOS Output, SC-70"
			(at 0 0 0)
		)
		(property "ki_keywords" "single comparator high speed cmos"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
		(symbol "LTC6752xSC6-4_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "VCC")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "VEE")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 5.08)
				(name "VDD")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC6752xUD-3"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 -5.08 0)
		)
		(property "Value" "LTC6752xUD-3"
			(at 3.81 -7.62 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-12-1EP_3x3mm_P0.5mm_EP1.65x1.65mm"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/6752fc.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Single 280Mhz 2.9ns Comparator, Rail-to-Rail Inputs, CMOS Output, QFN-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "single comparator high speed cmos"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC6752xUD-3_0_1")
		(symbol "LTC6752xUD-3_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "6")
			)
			(pin no_connect line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "VCC")
				(number "2")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "VEE")
				(number "13")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "VEE")
				(number "3")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "VEE")
				(number "9")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "~{LE}")
				(number "8")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 6.35)
				(name "~{SHDN}")
				(number "7")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "Q")
				(number "12")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~{Q}")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC6754xSC6"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 -7.62 0)
		)
		(property "Value" "LTC6754xSC6"
			(at 1.27 -5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/6754f.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single High Speed Rail-to-Rail Input Comparator with LVDS Compatible Outputs, SC-70-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "cmp r2r rtr push-pull complementary"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
		(symbol "LTC6754xSC6_0_1")
		(symbol "LTC6754xSC6_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "VEE")
				(number "2")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "Q")
				(number "1")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~{Q}")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC6754xUD"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 -7.62 0)
		)
		(property "Value" "LTC6754xUD"
			(at 1.27 -5.08 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-12-1EP_3x3mm_P0.5mm_EP1.65x1.65mm"
			(at 8.89 -15.24 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/6754f.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Single High Speed Rail-to-Rail Input Comparator with LVDS Compatible Outputs, QFN-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "cmp r2r rtr push-pull complementary"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC6754xUD_0_1")
		(symbol "LTC6754xUD_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "6")
			)
			(pin no_connect line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "VCCI")
				(number "2")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "VEE")
				(number "13")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "VEE")
				(number "3")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "VEE")
				(number "9")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 5.08)
				(name "VCCO")
				(number "1")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "~{LE}")
				(number "8")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 6.35)
				(name "~{SHDN}")
				(number "7")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "Q")
				(number "12")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~{Q}")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX941xPA"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "MAX941xPA"
			(at 3.81 3.81 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 2.54 0 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX941-MAX944.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "High-Speed, Low-Power, 3V/5V, Rail-to-Rail, Single-Supply Comparator, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single comparator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MAX941xPA_0_1")
		(symbol "MAX941xPA_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "3")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "6")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "~{LATCH}")
				(number "5")
			)
			(pin no_connect line
				(at 0 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 6.35)
				(name "~{SHDN}")
				(number "4")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX941xSA"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "MAX941xSA"
			(at 3.81 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 0 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX941-MAX944.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "High-Speed, Low-Power, 3V/5V, Rail-to-Rail, Single-Supply Comparator, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single comparator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MAX941xSA_0_1")
		(symbol "MAX941xSA_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "3")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "6")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "~{LATCH}")
				(number "5")
			)
			(pin no_connect line
				(at 0 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 6.35)
				(name "~{SHDN}")
				(number "4")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX941xUA"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "MAX941xUA"
			(at 3.81 3.81 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 2.54 0 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX941-MAX944.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "High-Speed, Low-Power, 3V/5V, Rail-to-Rail, Single-Supply Comparator, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single comparator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MAX941xUA_0_1")
		(symbol "MAX941xUA_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "3")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "6")
			)
			(pin input line
				(at 0 7.62 270)
				(length 5.08)
				(name "~{LATCH}")
				(number "5")
			)
			(pin no_connect line
				(at 0 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 6.35)
				(name "~{SHDN}")
				(number "4")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP6561-OT"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "MCP6561-OT"
			(at -1.27 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MCP6561-1R-1U-2-4-1.8V-Low-Power-Push-Pull-Output-Comparator-DS20002139E.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Single 1.8V Low-Power Push-Pull Output Comparator, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "cmp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MCP6561-OT_0_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "2")
			)
		)
		(symbol "MCP6561-OT_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP6561R"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "MCP6561R"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MCP6561-1R-1U-2-4-1.8V-Low-Power-Push-Pull-Output-Comparator-DS20002139E.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single 1.8V Low-Power Push-Pull Output Comparator, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "cmp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MCP6561R_0_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "5")
			)
		)
		(symbol "MCP6561R_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP6561U"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "MCP6561U"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MCP6561-1R-1U-2-4-1.8V-Low-Power-Push-Pull-Output-Comparator-DS20002139E.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single 1.8V Low-Power Push-Pull Output Comparator, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "cmp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MCP6561U_0_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "2")
			)
		)
		(symbol "MCP6561U_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "3")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP6561x-LT"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "MCP6561x-LT"
			(at -1.27 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MCP6561-1R-1U-2-4-1.8V-Low-Power-Push-Pull-Output-Comparator-DS20002139E.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single 1.8V Low-Power Push-Pull Output Comparator, SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "cmp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?353*"
			(at 0 0 0)
		)
		(symbol "MCP6561x-LT_0_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "2")
			)
		)
		(symbol "MCP6561x-LT_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP6562"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "MCP6562"
			(at 6.35 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MCP6561-1R-1U-2-4-1.8V-Low-Power-Push-Pull-Output-Comparator-DS20002139E.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual 1.8V Low-Power Push-Pull Output Comparator, SOIC-8/MSOP-8"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "cmp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP6562_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "MCP6562_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "MCP6562_3_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP6566"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "MCP6566"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MCP6566-6R-6U-7-9-1.8V-Low-Power-Open-Drain-Output-Comparator-DS20002143G.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single 1.8V Low-Power Open-Drain Output Comparator, SOT-23-5/SC-70"
			(at 0 0 0)
		)
		(property "ki_keywords" "cmp collector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* *SC*70*"
			(at 0 0 0)
		)
		(symbol "MCP6566_0_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "2")
			)
		)
		(symbol "MCP6566_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP6566R"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "MCP6566R"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MCP6566-6R-6U-7-9-1.8V-Low-Power-Open-Drain-Output-Comparator-DS20002143G.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single 1.8V Low-Power Open-Drain Output Comparator, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "cmp collector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MCP6566R_0_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "5")
			)
		)
		(symbol "MCP6566R_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP6566U"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "MCP6566U"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MCP6566-6R-6U-7-9-1.8V-Low-Power-Open-Drain-Output-Comparator-DS20002143G.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single 1.8V Low-Power Open-Drain Output Comparator, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "cmp collector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MCP6566U_0_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "2")
			)
		)
		(symbol "MCP6566U_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "3")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP6567"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "MCP6567"
			(at 6.35 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MCP6566-6R-6U-7-9-1.8V-Low-Power-Open-Drain-Output-Comparator-DS20002143G.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual 1.8V Low-Power Open-Drain Output Comparator, SOIC-8/MSOP-8"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "cmp collector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP6567_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "MCP6567_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "6")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "MCP6567_3_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP6569"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "MCP6569"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at -1.27 2.54 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MCP6566-6R-6U-7-9-1.8V-Low-Power-Open-Drain-Output-Comparator-DS20002143G.pdf"
			(at 1.27 5.08 0)
		)
		(property "Description" "Quad 1.8V Low-Power Open-Drain Output Comparator, SOIC-14/TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "cmp collector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP6569_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "MCP6569_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "6")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "MCP6569_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "10")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "9")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(symbol "MCP6569_4_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "12")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "13")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(symbol "MCP6569_5_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP65R41"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 3.81 0)
		)
		(property "Value" "MCP65R41"
			(at 6.35 -3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22269B.pdf"
			(at 0 0 0)
		)
		(property "Description" "3 μA Comparator with Integrated Reference Voltage, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "cmp reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MCP65R41_0_1")
		(symbol "MCP65R41_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "2")
			)
			(pin power_out line
				(at 0 7.62 270)
				(length 5.08)
				(name "Vref")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP65R46"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 3.81 0)
		)
		(property "Value" "MCP65R46"
			(at 6.35 -3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22269B.pdf"
			(at 13.97 24.13 0)
		)
		(property "Description" "3 μA Comparator with Integrated Reference Voltage, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "cmp reference open collector drain"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MCP65R46_0_1")
		(symbol "MCP65R46_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "2")
			)
			(pin power_out line
				(at 0 7.62 270)
				(length 5.08)
				(name "Vref")
				(number "5")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MIC845H"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 5.08 0)
		)
		(property "Value" "MIC845H"
			(at 7.62 -5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 -9.525 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic845.pdf"
			(at 3.81 5.08 0)
		)
		(property "Description" "Micro-Power Comparator / Battery Monitor, Active-High Push-Pull Output, SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single cmp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
		(symbol "MIC845H_0_1")
		(symbol "MIC845H_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin no_connect line
				(at -2.54 0 0)
				(length 2.54)
				(hide yes)
				(name "NIC")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 3.81)
				(name "V+")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MIC845N"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 5.08 0)
		)
		(property "Value" "MIC845N"
			(at 7.62 -5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 -9.525 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic845.pdf"
			(at 3.81 5.08 0)
		)
		(property "Description" "Micro-Power Comparator / Battery Monitor, Active-High Open-Drain Output, SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single cmp collector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
		(symbol "MIC845N_0_1")
		(symbol "MIC845N_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin no_connect line
				(at -2.54 0 0)
				(length 2.54)
				(hide yes)
				(name "NIC")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 3.81)
				(name "V+")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "2")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TL3116"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "TL3116"
			(at 3.81 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tl3116.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Ultra-Fast Low-Power Precision Comparators, SOIC-8/TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "cmp push-pull complementary"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TL3116_0_1")
		(symbol "TL3116_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "3")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 5.08)
				(name "GND")
				(number "6")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 6.35)
				(name "LATCH")
				(number "5")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~{Q}")
				(number "8")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "Q")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLV3501AID"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 -5.08 0)
		)
		(property "Value" "TLV3501AID"
			(at 3.81 -7.62 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -9.525 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv3501.pdf"
			(at 0 -11.43 0)
		)
		(property "Description" "High-Speed Comparator, 4.5-ns, Rail-to-Rail, Push-Pull CMOS Output, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single comparator high speed cmos"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm?P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TLV3501AID_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 5.08 180)
				(length 0)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -5.08 -5.08 180)
				(length 0)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "SHDN")
				(number "8")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLV3501AIDBV"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 -5.08 0)
		)
		(property "Value" "TLV3501AIDBV"
			(at 3.81 -7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -9.525 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv3501.pdf"
			(at 0 -11.43 0)
		)
		(property "Description" "High-Speed Comparator, 4.5-ns, Rail-to-Rail, Push-Pull CMOS Output, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "single comparator high speed cmos"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TLV3501AIDBV_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "1")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "2")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "SHDN")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADCMP354"
		(extends "ADCMP350")
		(property "Reference" "U"
			(at 3.175 5.08 0)
		)
		(property "Value" "ADCMP354"
			(at 3.175 -5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Analog_KS-4"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADCMP350_354_356.pdf"
			(at 3.81 5.08 0)
		)
		(property "Description" "Single-input comparator, internal 0.6V reference, Active-High Open-Drain output, KS-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "cmp collector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Analog*KS?4*"
			(at 0 0 0)
		)
	)
	(symbol "LM393"
		(extends "LM2903")
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "LM393"
			(at 6.35 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm393.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Power, Low-Offset Voltage, Dual Comparators, DIP-8/SOIC-8/TO-99-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "cmp open collector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* SOP*5.28x5.23mm*P1.27mm* VSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LMV339"
		(extends "LM339")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "LMV339"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at -1.27 2.54 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/lmv331.pdf"
			(at 1.27 5.08 0)
		)
		(property "Description" "Quad General-Purpose Low-Voltage Comparator, SOIC-14/TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "cmp open collector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LMV7219M5"
		(extends "MCP6561-OT")
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "LMV7219M5"
			(at -1.27 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lmv7219.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Single Low-Power High-Speed Push-Pull Output Comparator, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "cmp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LMV7219M7"
		(extends "MCP6561x-LT")
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "LMV7219M7"
			(at -1.27 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lmv7219.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Low-Power High-Speed Push-Pull Output Comparator, SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "cmp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?353*"
			(at 0 0 0)
		)
	)
	(symbol "LMV7275"
		(extends "LMV331")
		(property "Reference" "U"
			(at 1.27 5.08 0)
		)
		(property "Value" "LMV7275"
			(at 3.81 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 2.54 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmv7275.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Single, 1.8V Low Power, Rail-to-Rail Input, Open Collector Output Comparator, SOT-23-5/SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "cmp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* *SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "LP2901D"
		(extends "LM339")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "LP2901D"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at -1.27 2.54 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lp2901.pdf"
			(at 1.27 5.08 0)
		)
		(property "Description" "Quad Differential Comparators, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "cmp open collector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1011"
		(extends "LM311")
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "LT1011"
			(at 3.81 3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/lt1011.pdf"
			(at 0 0 0)
		)
		(property "Description" "Voltage Comparator, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "cmp open collector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1116"
		(extends "LT1016")
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "LT1116"
			(at 3.81 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1116fc.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single 12ns, Single Supply Ground-Sensing Comparator, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "cmp push-pull complementary latch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX9031AU"
		(extends "LMV7271")
		(property "Reference" "U"
			(at 1.27 5.715 0)
		)
		(property "Value" "MAX9031AU"
			(at 4.445 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX9030-MAX9034.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single, Rail to Rail, 2.5V - 5.5V Supply, 571mW, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "rail-rail"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX9031AX"
		(extends "LMV7271")
		(property "Reference" "U"
			(at 1.27 5.715 0)
		)
		(property "Value" "MAX9031AX"
			(at 4.445 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 0 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX9030-MAX9034.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single, Rail to Rail, 2.5V - 5.5V Supply, 247mW, SC70"
			(at 0 0 0)
		)
		(property "ki_keywords" "rail-rail"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "MIC845L"
		(extends "MIC845H")
		(property "Reference" "U"
			(at 3.81 5.08 0)
		)
		(property "Value" "MIC845L"
			(at 7.62 -5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 -9.525 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic845.pdf"
			(at 3.81 5.08 0)
		)
		(property "Description" "Micro-Power Comparator / Battery Monitor, Active-Low Push-Pull Output, SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single cmp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "TL331"
		(extends "LM397")
		(property "Reference" "U"
			(at 1.27 5.08 0)
		)
		(property "Value" "TL331"
			(at 3.81 -5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -15.24 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tl331.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Single Differential Comparator with Open-Collector Output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single comparator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV7031DBV"
		(extends "MCP6561-OT")
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "TLV7031DBV"
			(at -1.27 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv7031.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Single, 1.6V-6.5V, 315nA Quiescent, Push-Pull Output, Comparator, SOT-23-5/SC-70"
			(at 0 0 0)
		)
		(property "ki_keywords" "cmp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV7041DBV"
		(extends "MCP6566")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TLV7041DBV"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv7041.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "Single, 1.6V-6.5V, 315nA Quiescent, Open-Drain Output, Comparator, North-west pinout, SOT-23-5"
			(at 0 -10.16 0)
		)
		(property "ki_keywords" "cmp collector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV7041SDCK"
		(extends "MCP6566U")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TLV7041SDCK"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv7041.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "Single, 1.6V-6.5V, 315nA Quiescent, Open-Drain Output, Comparator, South-east pinout, SC-70"
			(at 0 -10.16 0)
		)
		(property "ki_keywords" "cmp collector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC*70*"
			(at 0 0 0)
		)
	)
	(symbol "TLV7041DCK"
		(extends "TLV7041DBV")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TLV7041DCK"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv7041.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "Single, 1.6V-6.5V, 315nA Quiescent, Open-Drain Output, Comparator, North-west pinout, SC-70"
			(at 0 -10.16 0)
		)
		(property "ki_keywords" "cmp collector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC*70*"
			(at 0 0 0)
		)
	)
)
